{"text_format":"1","workbook":"xlsx","n_sheets":22,"sheets":["Summary all Samples","Allom House and Barlow House","Avondale Park","Avondale Park Gardens","Bramley House","Camelford Walk","Darfield Way","Henry Dickens Estate","Kensington Memorial Park","Lancaster West Walkways","Markland House","Morland House","Portland Road Kitchen garden ","Robinson House","St Quintin Kitchen Garden","St. Quintin’s Roundabout","Tower Cordon","Treadgold House","Verity Close","Waynflete Square","West London Bowling Club","Whitstable House"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":138,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Summary all Samples","index":0,"n_rows":55,"n_cols":33,"rows_kept":55,"cut":false,"hidden":false,"merged":[[3,31,3,32],[4,31,4,32],[5,31,5,32],[1,31,1,32],[2,5,6,5],[2,6,6,6],[19,0,21,0],[23,0,24,0],[29,0,30,0],[53,0,53,1],[1,8,1,11],[8,0,13,0],[2,2,6,2],[2,3,6,3],[2,4,6,4]]}
[]
[null,null,null,null,null,null,null,"Location","Tower Cordon",null,null,null,"Lancaster West Walkways communal gardens","Communal garden at Treadgold House","Open space at Verity Close","Communal open space at Morland House","Communal open space at Allom House and Barlow House","Camelford Walk communal open space","Community kitchen garden at Portland Road","Community garden at Henry Dickens Estate","Avondale Park","Avondale Park Gardens","Bramley House communal garden","Communal open space at Whitstable House","St Quintin Community Kitchen Gardens","Communal open space at Markland House","Community garden areas along Darfield Way","Robinson House","Kensington Memorial Park (St Marks Park)","West London Bowling Club","St. Quintin’s Roundabout","Waynflete Square"]
[null,null,"Units","Method Detection Limit","GSC (human health residential scenario)","NBC","London Background (range min - max)","Sample identification","GTCS101","GTCS102","GTCS103","GTCS104","GTCS 1-05\nGTCS 1-06","GTCS 1-07\nGTCS 1-08","GTCS 1-09\nGTCS 1-10","GTCS 1-11\nGTCS 1-12","GTCS 1-13\nGTCS 1-14","GTCS 1-15\nGTCS 1-16","GTCS 1-17\nGTCS 1-18","GTCS 1-19\nGTCS 1-20","GTCS 1-21\nGTCS 1-22","GTCS 1-23\nGTCS 1-24","GTCS 1-25\nGTCS 1-26","GTCS 1-27\nGTCS 1-28","GTCS 1-29\nGTCS 1-30","GTCS 1-31\nGTCS 1-32","GTCS 1-33\nGTCS 1-34","GTCS 1-35\nGTCS 1-36","GTCS 1-37\nGTCS 1-38","GTCS 1-39\nGTCS 1-40","GTCS 1-41\nGTCS 1-42","GTCS 1-43\nto\nGTCS 1-59","GTCS 1-43\nto\nGTCS 1-51"]
[null,null,null,null,null,null,null,"Date","2019-04-10","2019-04-10","2019-04-10","2019-04-10","2019-06-06","2019-06-06","2019-06-06","2019-06-06T17:00:00","2019-06-07T09:00:00","2019-06-07T09:10:00","2019-06-05T10:40:00","2019-06-05T14:45:00","2019-06-05T12:30:00","2019-06-05T08:50:00","2019-06-05T16:20:00","2019-06-05T18:20:00","2019-06-06T15:30:00","2019-06-07T10:50:00","2019-06-04T09:30:00","2019-06-04T11:25:00","2019-06-04T13:30:00","2019-06-04T16:45:00","2019-06-04T14:45:00","2019-06-05"]
[null,null,null,null,null,null,null,"Sample Type","Normal","Normal","Normal","Normal","Normal","Normal","Normal","Normal","Normal","Normal","Normal","Normal","Normal","Normal","Normal","Normal","Normal","Normal","Normal","Normal","Normal","Normal","Normal","Normal"]
[null,null,null,null,null,null,null,"Field ID","GTCS101","GTCS102","GTCS103","GTCS104","GTCS 1-05A","GTCS 1-07A","GTCS 1-09A","GTCS 1-11A","GTCS 1-13A","GTCS 1-15A","GTCS 1-17A","GTCS 1-19A","GTCS 1-21A","GTCS 1-23 PRIMARY SAMPLE","GTCS 1-25A","GTCS 1-27A","GTCS 1-29A","GTCS 1-31A","GTCS 1-33A","GTCS 1-35A","GTCS 1-37A","GTCS 1-39 PRIMARY SAMPLE","GTCS 1-41 PRIMARY SAMPLE","GTCS 1-43A"]
[null,null,null,null,null,null,null,"Sample_Depth_Range","0-0.05","0-0.05","0-0.05","0-0.05","0-0.05","0-0.05","0-0.05","0-0.05","0-0.05","0-0.05","0-0.05","0-0.05","0-0.05","0-0.05","0-0.05","0-0.05","0-0.05","0-0.05","0-0.05","0-0.05","0-0.05","0-0.05","0-0.05","0-0.05","0.1-0.15"]
["Metals"]
[null,"Arsenic","mg/kg",0.5,"37#6",null,"1.2 - 160.90#9",null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","47.4* \n58.6*\n55.4*\n61.5*","N/A","N/A","N/A","N/A","N/A","92.9*","N/A","N/A","N/A","N/A","N/A","N/A","N/A","40.6*"]
[null,"Barium","mg/kg",1,"460#7",null,"143.50 - 3475.10#9",null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","991* \n945*\n948* \n944*","N/A","N/A","540\n613*\n564\n560*","N/A","N/A","475*\n535*\n607*\n575*","N/A","N/A","N/A","N/A","563","N/A","N/A","537*"]
[null,"Beryllium","mg/kg",0.5,"1.7#2",null,null,null,"N/A","N/A","N/A","N/A","N/A","1.8 \n2.1 \n2.3*\n2.6\n2.3","N/A","N/A","N/A","N/A","2.1 \n4* \n4.1* \n4.1*\n4*","N/A","N/A","N/A","N/A","N/A","2.2*\n1.9*\n2*\n1.8*","N/A","N/A","N/A","1.8","1.8*\n2.1*\n2.7\n1.8*\n2.2","1.9","1.8*","2.2*\n2\n2*"]
[null,"Cadmium","mg/kg",0.1,"22#6","2.1#8","0.00 - 165.20#9",null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","46.2*\n46.8*"]
[null,"Lead","mg/kg",5,"200#6","820#8","10.8 - 10,000#9",null,"N/A","N/A","N/A","N/A","N/A","500 \n473 \n516* \n442 \n587","N/A","N/A","N/A","280","492 \n1,785*\n1,780*\n1,528*\n1,519*","290\n434",1200,"2099\n2,621*\n2151\n2,539*\n659\n","262","439","980*\n1,083*\n1,111*\n1,597*\n",301,"N/A","312\n341*\n327*\n385*\n275","214","398*\n392*\n431\n393*\n1311","552\n556\n571\n564\n517","603*\n232\n318\n578\n257*\n298*\n222\n331\n422*\n330\n287\n484*\n274\n263","757*\n448*\n385\n429*\n334*"]
[null,"Zinc","mg/kg",5,"3,700#2",null,"0.00 - 10,095#9",null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","5,153*","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["VOCs"]
[null,"Chloromethane","ug/kg",3,"9.8#3",null,null,null,"N/A","N/A","N/A","N/A","N/A","N/A","12 \n10","17 \n20 \n14 \n21 \n14","N/A","11","26\n11\n14\n19","12\n21","N/A","16\n11\n18\n34\n","N/A","N/A","10\n12\n",12,"N/A","19","50\n36","12\n10\n13\n10\n27","27\n28\n30\n33","10\n10\n13\n12\n14\n10\n11","16"]
["SVOCs"]
[null,"Dibenzo[a,e]pyrene","ug/kg",100,"42#1",null,null,null," - "," - "," - "," - "," - "," - "," - "," - "," - "," - "," - "," - "," - "," - "," - "," - "," - "," - "," - "," - "," - "," - "," - ",6277," - "]
["PAH"]
[null,"Benzo(a) pyrene","mg/kg",0.01,"2.7#2","3.6#8","0.332 - 6.976#10",null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","4.52","N/A","7.43\n7.82\n7.68\n7.05\n5.75","N/A","N/A","2.87\n2.81\n3.18","N/A","N/A","3.97\n2.81","N/A","N/A","5.11\n5.04\n5.34\n4.88\n3.8","2.75\n5.55\n3.27\n4.54\n","8.61\n3.13\n6.93"]
[null,"Benzo(b)fluoranthene","mg/kg",0.01,"3.3#2",null,"0.272 - 4.141#10",null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","5.93","N/A","9.25\n10.06\n9.91\n9.05\n7.17","N/A","N/A","4.13\n3.69\n3.66\n4.53","N/A","N/A","5.09\n3.58","N/A","N/A","7.02\n6.83\n7.21\n6.65\n5.23","3.87\n7.34\n4.47\n6.397*\n6.03","11.28\n3.83\n9.33"]
[null,"Dibenz(a,h)anthracene","mg/kg",0.01,"0.28#2",null,"0.033 - 0.843#10",null,"N/A","N/A","N/A","N/A","0.5  \n0.29","0.33","N/A","N/A","N/A","0.29","0.33","0.67\n0.32","N/A","1.01\n1.49\n1.25\n1.31\n1.06","0.41","N/A","0.39\n0.42\n0.45\n0.6","N/A","N/A","0.71\n0.41\n0.47","N/A","0.37\n0.32","1\n0.8\n0.87\n0.79\n0.56","0.44\n0.96\n0.66\n0.36\n0.29\n0.74\n0.38\n0.37","1.51\n0.69\n1.44\n0.38\n0.34"]
["PCB (Dutch 7) congeners"]
[null,"PCB 118","ug/kg",5,"120#1",null,"0.1 - 76.5#10",null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","154*","N/A"]
[null,"Total PCB 7 Congeners","ug/kg",35,"200#5",null,"0.1 - 114.1#10",null," - "," - "," - "," - ","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","407","N/A"]
["PCB (WHO12) 12 congeners"]
[null,"Pentachlorobiphenyl, 2,3',4,4',5- (PCB-118)","ug/kg","various","120#1",null,"0.1 - 76.5#10",null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A",154,"N/A"]
[null,"Pentachlorobiphenyl, 3,3,4,4,5- (PCB 126)","ug/kg","various","0.036#1",null,"0.0002 - 0.156#11",null,"N/A","N/A","N/A","N/A","0.157","N/A","N/A","N/A","N/A","N/A","0.0387\n0.0633\n0.043\n0.0377","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","0.04\n0.169\n0.0462\n0.12","0.0497\n0.0856"]
["ESdat Calculated"]
[null,"Cresols Total","ug/kg",20,"180#3",null,null,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A",221,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A",313,"N/A"]
[null,"Benzo(a)pyrene (surrogate marker for PAH mixture)","mg/kg",0.01,"5.0#6",null,null,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","7.43\n7.82\n7.68\n7.05\n5.75","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","5.11\n5.04\n5.34","5.55","8.61\n6.93"]
["AECOM Calculated"]
[null,"Sum of PCDD/F +PCB12","ng/kg","Various","8700#4",null,null,null,"N/A","N/A","N/A","N/A",11309,"N/A","N/A",14761,"N/A","N/A","N/A","N/A","N/A","N/A",10444,"N/A","13098\n18758\n33961\n21417","N/A","N/A","N/A","N/A","N/A","N/A","10165\n69988\n18171\n11930\n16597\n63213\n12644\n279697\n95814\n","20610\n12518\n39446\n11069\n11187"]
[]
["Comments"]
["#1  USEPA RSL (May 2019)"]
["#2  LQM/CIEH S4ULs 2015"]
["#3  EIC/AGS/CL:AIRE 2010"]
["#4  EA SGV 2009"]
["#5  Dutch IV 2013"]
["#6  Defra C4SL 2014"]
["#7  AECOM (modified EIC GAC to include plant uptake route)"]
["#8  Johnson et al. 2012"]
["#9  London Earth"]
["#10  Vane"]
["#11  UKSHS"]
["GSC: Generic Screening Criteria"]
["(blank): No assessment criteria available"]
[" - : Not analysed"]
["N/A result was not above GSC"]
["* highest of two alternative values (obtained through different laboratory methods on same sample)"]
["Field_D: Field Duplicate"]
["HH: Human Health"]
["NAD: No Asbestos Detected"]
["Exceedance of HH Soil. Residential with Plant Uptake.  Sandy Loam.  TOC >=1.45 to <3.48%"]

{"sheet":"Allom House and Barlow House","index":1,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[[7,0,12,0],[18,0,20,0],[22,0,23,0],[28,0,29,0],[52,0,52,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6]]}
[]
[null,null,null,null,null,null,null,"Location","Communal open space at Allom House and Barlow House"]
[null,null,"Units","Method Detection Limit","GSC (human health residential scenario)","NBC","London Background (range min - max)","Sample identification","GTCS 1-13\nGTCS 1-14"]
[null,null,null,null,null,null,null,"Date","2019-06-07T09:00:00"]
[null,null,null,null,null,null,null,"Sample Type","Normal"]
[null,null,null,null,null,null,null,"Sample_Depth_Range","0-0.05"]
["Metals"]
[null,"Arsenic","mg/kg",0.5,"37#6",null,"1.2 - 160.90#9",null,"N/A"]
[null,"Barium","mg/kg",1,"460#7",null,"143.50 - 3475.10#9",null,"N/A"]
[null,"Beryllium","mg/kg",0.5,"1.7#2",null,null,null,"N/A"]
[null,"Cadmium","mg/kg",0.1,"22#6","2.1#8","0.00 - 165.20#9",null,"N/A"]
[null,"Lead","mg/kg",5,"200#6","820#8","10.8 - 10,000#9",null,"N/A"]
[null,"Zinc","mg/kg",5,"3,700#2",null,"0.00 - 10,095#9",null,"N/A"]
["VOCs"]
[null,"Chloromethane","ug/kg",3,"9.8#3",null,null,null,"N/A"]
["SVOCs"]
[null,"Dibenzo[a,e]pyrene","ug/kg",100,"42#1",null,null,null," - "]
["PAH"]
[null,"Benzo(a) pyrene","mg/kg",0.01,"2.7#2","3.6#8","0.332 - 6.976#10",null,"N/A"]
[null,"Benzo(b)fluoranthene","mg/kg",0.01,"3.3#2",null,"0.272 - 4.141#10",null,"N/A"]
[null,"Dibenz(a,h)anthracene","mg/kg",0.01,"0.28#2",null,"0.033 - 0.843#10",null,"N/A"]
["PCB (Dutch 7) congeners"]
[null,"PCB 118","ug/kg",5,"120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Total PCB 7 Congeners","ug/kg",35,"200#5",null,"0.1 - 114.1#10",null,"N/A"]
["PCB (WHO12) 12 congeners"]
[null,"Pentachlorobiphenyl, 2,3',4,4',5- (PCB-118)","ug/kg","Various","120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Pentachlorobiphenyl, 3,3,4,4,5- (PCB 126)","ug/kg",5,"0.036#1",null,"0.0002 - 0.156#11",null,"N/A"]
["ESdat Calculated"]
[null,"Cresols Total","ug/kg",20,"180#3",null,null,null,"N/A"]
[null,"Benzo(a)pyrene (surrogate marker for PAH mixture)","mg/kg",0.01,"5.0#6",null,null,null,"N/A"]
["AECOM Calculated"]
[null,"Sum of PCDD/F +PCB12","ng/kg","Various","8700#4",null,null,null,"N/A"]
[]
["Comments"]
["#1  USEPA RSL (May 2019)"]
["#2  LQM/CIEH S4ULs 2015"]
["#3  EIC/AGS/CL:AIRE 2010"]
["#4  EA SGV 2009"]
["#5  Dutch IV 2013"]
["#6  Defra C4SL 2014"]
["#7  AECOM (modified EIC GAC to include plant uptake route)"]
["#8  Johnson et al. 2012"]
["#9  London Earth"]
["#10  Vane"]
["#11  UKSHS"]
["GSC: Generic Screening Criteria"]
["(blank): No assessment criteria available"]
[" - : Not analysed"]
["N/A result was not above GSC"]
["* highest of two alternative values (obtained through different laboratory methods on same sample)"]
["Field_D: Field Duplicate"]
["HH: Human Health"]
["NAD: No Asbestos Detected"]
["Exceedance of HH Soil. Residential with Plant Uptake.  Sandy Loam.  TOC >=1.45 to <3.48%"]

{"sheet":"Avondale Park","index":2,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[[7,0,12,0],[18,0,20,0],[22,0,23,0],[28,0,29,0],[52,0,52,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6]]}
[]
[null,null,null,null,null,null,null,"Location","Avondale Park"]
[null,null,"Units","Method Detection Limit","GSC (human health residential scenario)","NBC","London Background (range min - max)","Sample identification","GTCS 1-21\nGTCS 1-22"]
[null,null,null,null,null,null,null,"Date","2019-06-05T12:30:00"]
[null,null,null,null,null,null,null,"Sample Type","Normal"]
[null,null,null,null,null,null,null,"Sample_Depth_Range","0-0.05"]
["Metals"]
[null,"Arsenic","mg/kg",0.5,"37#6",null,"1.2 - 160.90#9",null,"N/A"]
[null,"Barium","mg/kg",1,"460#7",null,"143.50 - 3475.10#9",null,"N/A"]
[null,"Beryllium","mg/kg",0.5,"1.7#2",null,null,null,"N/A"]
[null,"Cadmium","mg/kg",0.1,"22#6","2.1#8","0.00 - 165.20#9",null,"N/A"]
[null,"Lead","mg/kg",5,"200#6","820#8","10.8 - 10,000#9",null,1200]
[null,"Zinc","mg/kg",5,"3,700#2",null,"0.00 - 10,095#9",null,"N/A"]
["VOCs"]
[null,"Chloromethane","ug/kg",3,"9.8#3",null,null,null,"N/A"]
["SVOCs"]
[null,"Dibenzo[a,e]pyrene","ug/kg",100,"42#1",null,null,null," - "]
["PAH"]
[null,"Benzo(a) pyrene","mg/kg",0.01,"2.7#2","3.6#8","0.332 - 6.976#10",null,"N/A"]
[null,"Benzo(b)fluoranthene","mg/kg",0.01,"3.3#2",null,"0.272 - 4.141#10",null,"N/A"]
[null,"Dibenz(a,h)anthracene","mg/kg",0.01,"0.28#2",null,"0.033 - 0.843#10",null,"N/A"]
["PCB (Dutch 7) congeners"]
[null,"PCB 118","ug/kg",5,"120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Total PCB 7 Congeners","ug/kg",35,"200#5",null,"0.1 - 114.1#10",null,"N/A"]
["PCB (WHO12) 12 congeners"]
[null,"Pentachlorobiphenyl, 2,3',4,4',5- (PCB-118)","ug/kg","Various","120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Pentachlorobiphenyl, 3,3,4,4,5- (PCB 126)","ug/kg",5,"0.036#1",null,"0.0002 - 0.156#11",null,"N/A"]
["ESdat Calculated"]
[null,"Cresols Total","ug/kg",20,"180#3",null,null,null,"N/A"]
[null,"Benzo(a)pyrene (surrogate marker for PAH mixture)","mg/kg",0.01,"5.0#6",null,null,null,"N/A"]
["AECOM Calculated"]
[null,"Sum of PCDD/F +PCB12","ng/kg","Various","8700#4",null,null,null,"N/A"]
[]
["Comments"]
["#1  USEPA RSL (May 2019)"]
["#2  LQM/CIEH S4ULs 2015"]
["#3  EIC/AGS/CL:AIRE 2010"]
["#4  EA SGV 2009"]
["#5  Dutch IV 2013"]
["#6  Defra C4SL 2014"]
["#7  AECOM (modified EIC GAC to include plant uptake route)"]
["#8  Johnson et al. 2012"]
["#9  London Earth"]
["#10  Vane"]
["#11  UKSHS"]
["GSC: Generic Screening Criteria"]
["(blank): No assessment criteria available"]
[" - : Not analysed"]
["N/A result was not above GSC"]
["* highest of two alternative values (obtained through different laboratory methods on same sample)"]
["Field_D: Field Duplicate"]
["HH: Human Health"]
["NAD: No Asbestos Detected"]
["Exceedance of HH Soil. Residential with Plant Uptake.  Sandy Loam.  TOC >=1.45 to <3.48%"]

{"sheet":"Avondale Park Gardens","index":3,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[[7,0,12,0],[18,0,20,0],[22,0,23,0],[28,0,29,0],[52,0,52,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6]]}
[]
[null,null,null,null,null,null,null,"Location","Avondale Park Gardens"]
[null,null,"Units","Method Detection Limit","GSC (human health residential scenario)","NBC","London Background (range min - max)","Sample identification","GTCS 1-23\nGTCS 1-24"]
[null,null,null,null,null,null,null,"Date","2019-06-05T08:50:00"]
[null,null,null,null,null,null,null,"Sample Type","Normal"]
[null,null,null,null,null,null,null,"Sample_Depth_Range","0-0.05"]
["Metals"]
[null,"Arsenic","mg/kg",0.5,"37#6",null,"1.2 - 160.90#9",null,"N/A"]
[null,"Barium","mg/kg",1,"460#7",null,"143.50 - 3475.10#9",null,"540\n613*\n564\n560*"]
[null,"Beryllium","mg/kg",0.5,"1.7#2",null,null,null,"N/A"]
[null,"Cadmium","mg/kg",0.1,"22#6","2.1#8","0.00 - 165.20#9",null,"N/A"]
[null,"Lead","mg/kg",5,"200#6","820#8","10.8 - 10,000#9",null,"2099\n2,621*\n2151\n2,539*\n659\n"]
[null,"Zinc","mg/kg",5,"3,700#2",null,"0.00 - 10,095#9",null,"N/A"]
["VOCs"]
[null,"Chloromethane","ug/kg",3,"9.8#3",null,null,null,"16\n11\n18\n34\n"]
["SVOCs"]
[null,"Dibenzo[a,e]pyrene","ug/kg",100,"42#1",null,null,null," - "]
["PAH"]
[null,"Benzo(a) pyrene","mg/kg",0.01,"2.7#2","3.6#8","0.332 - 6.976#10",null,"7.43\n7.82\n7.68\n7.05\n5.75"]
[null,"Benzo(b)fluoranthene","mg/kg",0.01,"3.3#2",null,"0.272 - 4.141#10",null,"9.25\n10.06\n9.91\n9.05\n7.17"]
[null,"Dibenz(a,h)anthracene","mg/kg",0.01,"0.28#2",null,"0.033 - 0.843#10",null,"1.01\n1.49\n1.25\n1.31\n1.06"]
["PCB (Dutch 7) congeners"]
[null,"PCB 118","ug/kg",5,"120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Total PCB 7 Congeners","ug/kg",35,"200#5",null,"0.1 - 114.1#10",null,"N/A"]
["PCB (WHO12) 12 congeners"]
[null,"Pentachlorobiphenyl, 2,3',4,4',5- (PCB-118)","ug/kg","Various","120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Pentachlorobiphenyl, 3,3,4,4,5- (PCB 126)","ug/kg",5,"0.036#1",null,"0.0002 - 0.156#11",null,"N/A"]
["ESdat Calculated"]
[null,"Cresols Total","ug/kg",20,"180#3",null,null,null,"N/A"]
[null,"Benzo(a)pyrene (surrogate marker for PAH mixture)","mg/kg",0.01,"5.0#6",null,null,null,"7.43\n7.82\n7.68\n7.05\n5.75"]
["AECOM Calculated"]
[null,"Sum of PCDD/F +PCB12","ng/kg","Various","8700#4",null,null,null,"N/A"]
[]
["Comments"]
["#1  USEPA RSL (May 2019)"]
["#2  LQM/CIEH S4ULs 2015"]
["#3  EIC/AGS/CL:AIRE 2010"]
["#4  EA SGV 2009"]
["#5  Dutch IV 2013"]
["#6  Defra C4SL 2014"]
["#7  AECOM (modified EIC GAC to include plant uptake route)"]
["#8  Johnson et al. 2012"]
["#9  London Earth"]
["#10  Vane"]
["#11  UKSHS"]
["GSC: Generic Screening Criteria"]
["(blank): No assessment criteria available"]
[" - : Not analysed"]
["N/A result was not above GSC"]
["* highest of two alternative values (obtained through different laboratory methods on same sample)"]
["Field_D: Field Duplicate"]
["HH: Human Health"]
["NAD: No Asbestos Detected"]
["Exceedance of HH Soil. Residential with Plant Uptake.  Sandy Loam.  TOC >=1.45 to <3.48%"]

{"sheet":"Bramley House","index":4,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[[7,0,12,0],[18,0,20,0],[22,0,23,0],[28,0,29,0],[52,0,52,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6]]}
[]
[null,null,null,null,null,null,null,"Location","Bramley House communal garden"]
[null,null,"Units","Method Detection Limit","GSC (human health residential scenario)","NBC","London Background (range min - max)","Sample identification","GTCS 1-25\nGTCS 1-26"]
[null,null,null,null,null,null,null,"Date","2019-06-05T16:20:00"]
[null,null,null,null,null,null,null,"Sample Type","Normal"]
[null,null,null,null,null,null,null,"Sample_Depth_Range","0-0.05"]
["Metals"]
[null,"Arsenic","mg/kg",0.5,"37#6",null,"1.2 - 160.90#9",null,"N/A"]
[null,"Barium","mg/kg",1,"460#7",null,"143.50 - 3475.10#9",null,"N/A"]
[null,"Beryllium","mg/kg",0.5,"1.7#2",null,null,null,"N/A"]
[null,"Cadmium","mg/kg",0.1,"22#6","2.1#8","0.00 - 165.20#9",null,"N/A"]
[null,"Lead","mg/kg",5,"200#6","820#8","10.8 - 10,000#9",null,"262"]
[null,"Zinc","mg/kg",5,"3,700#2",null,"0.00 - 10,095#9",null,"N/A"]
["VOCs"]
[null,"Chloromethane","ug/kg",3,"9.8#3",null,null,null,"N/A"]
["SVOCs"]
[null,"Dibenzo[a,e]pyrene","ug/kg",100,"42#1",null,null,null," - "]
["PAH"]
[null,"Benzo(a) pyrene","mg/kg",0.01,"2.7#2","3.6#8","0.332 - 6.976#10",null,"N/A"]
[null,"Benzo(b)fluoranthene","mg/kg",0.01,"3.3#2",null,"0.272 - 4.141#10",null,"N/A"]
[null,"Dibenz(a,h)anthracene","mg/kg",0.01,"0.28#2",null,"0.033 - 0.843#10",null,"0.41"]
["PCB (Dutch 7) congeners"]
[null,"PCB 118","ug/kg",5,"120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Total PCB 7 Congeners","ug/kg",35,"200#5",null,"0.1 - 114.1#10",null,"N/A"]
["PCB (WHO12) 12 congeners"]
[null,"Pentachlorobiphenyl, 2,3',4,4',5- (PCB-118)","ug/kg","Various","120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Pentachlorobiphenyl, 3,3,4,4,5- (PCB 126)","ug/kg",5,"0.036#1",null,"0.0002 - 0.156#11",null,"N/A"]
["ESdat Calculated"]
[null,"Cresols Total","ug/kg",20,"180#3",null,null,null,221]
[null,"Benzo(a)pyrene (surrogate marker for PAH mixture)","mg/kg",0.01,"5.0#6",null,null,null,"N/A"]
["AECOM Calculated"]
[null,"Sum of PCDD/F +PCB12","ng/kg","Various","8700#4",null,null,null,10444]
[]
["Comments"]
["#1  USEPA RSL (May 2019)"]
["#2  LQM/CIEH S4ULs 2015"]
["#3  EIC/AGS/CL:AIRE 2010"]
["#4  EA SGV 2009"]
["#5  Dutch IV 2013"]
["#6  Defra C4SL 2014"]
["#7  AECOM (modified EIC GAC to include plant uptake route)"]
["#8  Johnson et al. 2012"]
["#9  London Earth"]
["#10  Vane"]
["#11  UKSHS"]
["GSC: Generic Screening Criteria"]
["(blank): No assessment criteria available"]
[" - : Not analysed"]
["N/A result was not above GSC"]
["* highest of two alternative values (obtained through different laboratory methods on same sample)"]
["Field_D: Field Duplicate"]
["HH: Human Health"]
["NAD: No Asbestos Detected"]
["Exceedance of HH Soil. Residential with Plant Uptake.  Sandy Loam.  TOC >=1.45 to <3.48%"]

{"sheet":"Camelford Walk","index":5,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[[7,0,12,0],[18,0,20,0],[22,0,23,0],[28,0,29,0],[52,0,52,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6]]}
[]
[null,null,null,null,null,null,null,"Location","Camelford Walk communal open space"]
[null,null,"Units","Method Detection Limit","GSC (human health residential scenario)","NBC","London Background (range min - max)","Sample identification","GTCS 1-15\nGTCS 1-16"]
[null,null,null,null,null,null,null,"Date","2019-06-07T09:10:00"]
[null,null,null,null,null,null,null,"Sample Type","Normal"]
[null,null,null,null,null,null,null,"Sample_Depth_Range","0-0.05"]
["Metals"]
[null,"Arsenic","mg/kg",0.5,"37#6",null,"1.2 - 160.90#9",null,"N/A"]
[null,"Barium","mg/kg",1,"460#7",null,"143.50 - 3475.10#9",null,"N/A"]
[null,"Beryllium","mg/kg",0.5,"1.7#2",null,null,null,"N/A"]
[null,"Cadmium","mg/kg",0.1,"22#6","2.1#8","0.00 - 165.20#9",null,"N/A"]
[null,"Lead","mg/kg",5,"200#6","820#8","10.8 - 10,000#9",null,"280"]
[null,"Zinc","mg/kg",5,"3,700#2",null,"0.00 - 10,095#9",null,"N/A"]
["VOCs"]
[null,"Chloromethane","ug/kg",3,"9.8#3",null,null,null,"11"]
["SVOCs"]
[null,"Dibenzo[a,e]pyrene","ug/kg",100,"42#1",null,null,null," - "]
["PAH"]
[null,"Benzo(a) pyrene","mg/kg",0.01,"2.7#2","3.6#8","0.332 - 6.976#10",null,"N/A"]
[null,"Benzo(b)fluoranthene","mg/kg",0.01,"3.3#2",null,"0.272 - 4.141#10",null,"N/A"]
[null,"Dibenz(a,h)anthracene","mg/kg",0.01,"0.28#2",null,"0.033 - 0.843#10",null,"0.29"]
["PCB (Dutch 7) congeners"]
[null,"PCB 118","ug/kg",5,"120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Total PCB 7 Congeners","ug/kg",35,"200#5",null,"0.1 - 114.1#10",null,"N/A"]
["PCB (WHO12) 12 congeners"]
[null,"Pentachlorobiphenyl, 2,3',4,4',5- (PCB-118)","ug/kg","Various","120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Pentachlorobiphenyl, 3,3,4,4,5- (PCB 126)","ug/kg",5,"0.036#1",null,"0.0002 - 0.156#11",null,"N/A"]
["ESdat Calculated"]
[null,"Cresols Total","ug/kg",20,"180#3",null,null,null,"N/A"]
[null,"Benzo(a)pyrene (surrogate marker for PAH mixture)","mg/kg",0.01,"5.0#6",null,null,null,"N/A"]
["AECOM Calculated"]
[null,"Sum of PCDD/F +PCB12","ng/kg","Various","8700#4",null,null,null,"N/A"]
[]
["Comments"]
["#1  USEPA RSL (May 2019)"]
["#2  LQM/CIEH S4ULs 2015"]
["#3  EIC/AGS/CL:AIRE 2010"]
["#4  EA SGV 2009"]
["#5  Dutch IV 2013"]
["#6  Defra C4SL 2014"]
["#7  AECOM (modified EIC GAC to include plant uptake route)"]
["#8  Johnson et al. 2012"]
["#9  London Earth"]
["#10  Vane"]
["#11  UKSHS"]
["GSC: Generic Screening Criteria"]
["(blank): No assessment criteria available"]
[" - : Not analysed"]
["N/A result was not above GSC"]
["* highest of two alternative values (obtained through different laboratory methods on same sample)"]
["Field_D: Field Duplicate"]
["HH: Human Health"]
["NAD: No Asbestos Detected"]
["Exceedance of HH Soil. Residential with Plant Uptake.  Sandy Loam.  TOC >=1.45 to <3.48%"]

{"sheet":"Darfield Way","index":6,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[[7,0,12,0],[18,0,20,0],[22,0,23,0],[28,0,29,0],[52,0,52,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6]]}
[]
[null,null,null,null,null,null,null,"Location","Community garden areas along Darfield Way"]
[null,null,"Units","Method Detection Limit","GSC (human health residential scenario)","NBC","London Background (range min - max)","Sample identification","GTCS 1-33\nGTCS 1-34"]
[null,null,null,null,null,null,null,"Date","2019-06-04T09:30:00"]
[null,null,null,null,null,null,null,"Sample Type","Normal"]
[null,null,null,null,null,null,null,"Sample_Depth_Range","0-0.05"]
["Metals"]
[null,"Arsenic","mg/kg",0.5,"37#6",null,"1.2 - 160.90#9",null,"N/A"]
[null,"Barium","mg/kg",1,"460#7",null,"143.50 - 3475.10#9",null,"N/A"]
[null,"Beryllium","mg/kg",0.5,"1.7#2",null,null,null,"N/A"]
[null,"Cadmium","mg/kg",0.1,"22#6","2.1#8","0.00 - 165.20#9",null,"N/A"]
[null,"Lead","mg/kg",5,"200#6","820#8","10.8 - 10,000#9",null,"N/A"]
[null,"Zinc","mg/kg",5,"3,700#2",null,"0.00 - 10,095#9",null,"N/A"]
["VOCs"]
[null,"Chloromethane","ug/kg",3,"9.8#3",null,null,null,"N/A"]
["SVOCs"]
[null,"Dibenzo[a,e]pyrene","ug/kg",100,"42#1",null,null,null," - "]
["PAH"]
[null,"Benzo(a) pyrene","mg/kg",0.01,"2.7#2","3.6#8","0.332 - 6.976#10",null,"N/A"]
[null,"Benzo(b)fluoranthene","mg/kg",0.01,"3.3#2",null,"0.272 - 4.141#10",null,"N/A"]
[null,"Dibenz(a,h)anthracene","mg/kg",0.01,"0.28#2",null,"0.033 - 0.843#10",null,"N/A"]
["PCB (Dutch 7) congeners"]
[null,"PCB 118","ug/kg",5,"120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Total PCB 7 Congeners","ug/kg",35,"200#5",null,"0.1 - 114.1#10",null,"N/A"]
["PCB (WHO12) 12 congeners"]
[null,"Pentachlorobiphenyl, 2,3',4,4',5- (PCB-118)","ug/kg","Various","120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Pentachlorobiphenyl, 3,3,4,4,5- (PCB 126)","ug/kg",5,"0.036#1",null,"0.0002 - 0.156#11",null,"N/A"]
["ESdat Calculated"]
[null,"Cresols Total","ug/kg",20,"180#3",null,null,null,"N/A"]
[null,"Benzo(a)pyrene (surrogate marker for PAH mixture)","mg/kg",0.01,"5.0#6",null,null,null,"N/A"]
["AECOM Calculated"]
[null,"Sum of PCDD/F +PCB12","ng/kg","Various","8700#4",null,null,null,"N/A"]
[]
["Comments"]
["#1  USEPA RSL (May 2019)"]
["#2  LQM/CIEH S4ULs 2015"]
["#3  EIC/AGS/CL:AIRE 2010"]
["#4  EA SGV 2009"]
["#5  Dutch IV 2013"]
["#6  Defra C4SL 2014"]
["#7  AECOM (modified EIC GAC to include plant uptake route)"]
["#8  Johnson et al. 2012"]
["#9  London Earth"]
["#10  Vane"]
["#11  UKSHS"]
["GSC: Generic Screening Criteria"]
["(blank): No assessment criteria available"]
[" - : Not analysed"]
["N/A result was not above GSC"]
["* highest of two alternative values (obtained through different laboratory methods on same sample)"]
["Field_D: Field Duplicate"]
["HH: Human Health"]
["NAD: No Asbestos Detected"]
["Exceedance of HH Soil. Residential with Plant Uptake.  Sandy Loam.  TOC >=1.45 to <3.48%"]

{"sheet":"Henry Dickens Estate","index":7,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[[7,0,12,0],[18,0,20,0],[22,0,23,0],[28,0,29,0],[52,0,52,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6]]}
[]
[null,null,null,null,null,null,null,"Location","Community garden at Henry Dickens Estate"]
[null,null,"Units","Method Detection Limit","GSC (human health residential scenario)","NBC","London Background (range min - max)","Sample identification","GTCS 1-19\nGTCS 1-20"]
[null,null,null,null,null,null,null,"Date","2019-06-05T14:45:00"]
[null,null,null,null,null,null,null,"Sample Type","Normal"]
[null,null,null,null,null,null,null,"Sample_Depth_Range","0-0.05"]
["Metals"]
[null,"Arsenic","mg/kg",0.5,"37#6",null,"1.2 - 160.90#9",null,"N/A"]
[null,"Barium","mg/kg",1,"460#7",null,"143.50 - 3475.10#9",null,"N/A"]
[null,"Beryllium","mg/kg",0.5,"1.7#2",null,null,null,"N/A"]
[null,"Cadmium","mg/kg",0.1,"22#6","2.1#8","0.00 - 165.20#9",null,"N/A"]
[null,"Lead","mg/kg",5,"200#6","820#8","10.8 - 10,000#9",null,"290\n434"]
[null,"Zinc","mg/kg",5,"3,700#2",null,"0.00 - 10,095#9",null,"N/A"]
["VOCs"]
[null,"Chloromethane","ug/kg",3,"9.8#3",null,null,null,"12\n21"]
["SVOCs"]
[null,"Dibenzo[a,e]pyrene","ug/kg",100,"42#1",null,null,null," - "]
["PAH"]
[null,"Benzo(a) pyrene","mg/kg",0.01,"2.7#2","3.6#8","0.332 - 6.976#10",null,"4.52"]
[null,"Benzo(b)fluoranthene","mg/kg",0.01,"3.3#2",null,"0.272 - 4.141#10",null,"5.93"]
[null,"Dibenz(a,h)anthracene","mg/kg",0.01,"0.28#2",null,"0.033 - 0.843#10",null,"0.67\n0.32"]
["PCB (Dutch 7) congeners"]
[null,"PCB 118","ug/kg",5,"120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Total PCB 7 Congeners","ug/kg",35,"200#5",null,"0.1 - 114.1#10",null,"N/A"]
["PCB (WHO12) 12 congeners"]
[null,"Pentachlorobiphenyl, 2,3',4,4',5- (PCB-118)","ug/kg","Various","120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Pentachlorobiphenyl, 3,3,4,4,5- (PCB 126)","ug/kg",5,"0.036#1",null,"0.0002 - 0.156#11",null,"N/A"]
["ESdat Calculated"]
[null,"Cresols Total","ug/kg",20,"180#3",null,null,null,"N/A"]
[null,"Benzo(a)pyrene (surrogate marker for PAH mixture)","mg/kg",0.01,"5.0#6",null,null,null,"N/A"]
["AECOM Calculated"]
[null,"Sum of PCDD/F +PCB12","ng/kg","Various","8700#4",null,null,null,"N/A"]
[]
["Comments"]
["#1  USEPA RSL (May 2019)"]
["#2  LQM/CIEH S4ULs 2015"]
["#3  EIC/AGS/CL:AIRE 2010"]
["#4  EA SGV 2009"]
["#5  Dutch IV 2013"]
["#6  Defra C4SL 2014"]
["#7  AECOM (modified EIC GAC to include plant uptake route)"]
["#8  Johnson et al. 2012"]
["#9  London Earth"]
["#10  Vane"]
["#11  UKSHS"]
["GSC: Generic Screening Criteria"]
["(blank): No assessment criteria available"]
[" - : Not analysed"]
["N/A result was not above GSC"]
["* highest of two alternative values (obtained through different laboratory methods on same sample)"]
["Field_D: Field Duplicate"]
["HH: Human Health"]
["NAD: No Asbestos Detected"]
["Exceedance of HH Soil. Residential with Plant Uptake.  Sandy Loam.  TOC >=1.45 to <3.48%"]

{"sheet":"Kensington Memorial Park","index":8,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[[7,0,12,0],[18,0,20,0],[22,0,23,0],[28,0,29,0],[52,0,52,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6]]}
[]
[null,null,null,null,null,null,null,"Location","Kensington Memorial Park (St Marks Park)"]
[null,null,"Units","Method Detection Limit","GSC (human health residential scenario)","NBC","London Background (range min - max)","Sample identification","GTCS 1-37\nGTCS 1-38"]
[null,null,null,null,null,null,null,"Date","2019-06-04T13:30:00"]
[null,null,null,null,null,null,null,"Sample Type","Normal"]
[null,null,null,null,null,null,null,"Sample_Depth_Range","0-0.05"]
["Metals"]
[null,"Arsenic","mg/kg",0.5,"37#6",null,"1.2 - 160.90#9",null,"N/A"]
[null,"Barium","mg/kg",1,"460#7",null,"143.50 - 3475.10#9",null,"N/A"]
[null,"Beryllium","mg/kg",0.5,"1.7#2",null,null,null,"1.8"]
[null,"Cadmium","mg/kg",0.1,"22#6","2.1#8","0.00 - 165.20#9",null,"N/A"]
[null,"Lead","mg/kg",5,"200#6","820#8","10.8 - 10,000#9",null,"214"]
[null,"Zinc","mg/kg",5,"3,700#2",null,"0.00 - 10,095#9",null,"N/A"]
["VOCs"]
[null,"Chloromethane","ug/kg",3,"9.8#3",null,null,null,"50\n36"]
["SVOCs"]
[null,"Dibenzo[a,e]pyrene","ug/kg",100,"42#1",null,null,null," - "]
["PAH"]
[null,"Benzo(a) pyrene","mg/kg",0.01,"2.7#2","3.6#8","0.332 - 6.976#10",null,"N/A"]
[null,"Benzo(b)fluoranthene","mg/kg",0.01,"3.3#2",null,"0.272 - 4.141#10",null,"N/A"]
[null,"Dibenz(a,h)anthracene","mg/kg",0.01,"0.28#2",null,"0.033 - 0.843#10",null,"N/A"]
["PCB (Dutch 7) congeners"]
[null,"PCB 118","ug/kg",5,"120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Total PCB 7 Congeners","ug/kg",35,"200#5",null,"0.1 - 114.1#10",null,"N/A"]
["PCB (WHO12) 12 congeners"]
[null,"Pentachlorobiphenyl, 2,3',4,4',5- (PCB-118)","ug/kg","Various","120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Pentachlorobiphenyl, 3,3,4,4,5- (PCB 126)","ug/kg",5,"0.036#1",null,"0.0002 - 0.156#11",null,"N/A"]
["ESdat Calculated"]
[null,"Cresols Total","ug/kg",20,"180#3",null,null,null,"N/A"]
[null,"Benzo(a)pyrene (surrogate marker for PAH mixture)","mg/kg",0.01,"5.0#6",null,null,null,"N/A"]
["AECOM Calculated"]
[null,"Sum of PCDD/F +PCB12","ng/kg","Various","8700#4",null,null,null,"N/A"]
[]
["Comments"]
["#1  USEPA RSL (May 2019)"]
["#2  LQM/CIEH S4ULs 2015"]
["#3  EIC/AGS/CL:AIRE 2010"]
["#4  EA SGV 2009"]
["#5  Dutch IV 2013"]
["#6  Defra C4SL 2014"]
["#7  AECOM (modified EIC GAC to include plant uptake route)"]
["#8  Johnson et al. 2012"]
["#9  London Earth"]
["#10  Vane"]
["#11  UKSHS"]
["GSC: Generic Screening Criteria"]
["(blank): No assessment criteria available"]
[" - : Not analysed"]
["N/A result was not above GSC"]
["* highest of two alternative values (obtained through different laboratory methods on same sample)"]
["Field_D: Field Duplicate"]
["HH: Human Health"]
["NAD: No Asbestos Detected"]
["Exceedance of HH Soil. Residential with Plant Uptake.  Sandy Loam.  TOC >=1.45 to <3.48%"]

{"sheet":"Lancaster West Walkways","index":9,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[[7,0,12,0],[18,0,20,0],[22,0,23,0],[28,0,29,0],[52,0,52,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6]]}
[]
[null,null,null,null,null,null,null,"Location","Lancaster West Walkways communal gardens"]
[null,null,"Units","Method Detection Limit","GSC (human health residential scenario)","NBC","London Background (range min - max)","Sample identification","GTCS 1-05\nGTCS 1-06"]
[null,null,null,null,null,null,null,"Date","2019-06-06"]
[null,null,null,null,null,null,null,"Sample Type","Normal"]
[null,null,null,null,null,null,null,"Sample_Depth_Range","0-0.05"]
["Metals"]
[null,"Arsenic","mg/kg",0.5,"37#6",null,"1.2 - 160.90#9",null,"N/A"]
[null,"Barium","mg/kg",1,"460#7",null,"143.50 - 3475.10#9",null,"N/A"]
[null,"Beryllium","mg/kg",0.5,"1.7#2",null,null,null,"N/A"]
[null,"Cadmium","mg/kg",0.1,"22#6","2.1#8","0.00 - 165.20#9",null,"N/A"]
[null,"Lead","mg/kg",5,"200#6","820#8","10.8 - 10,000#9",null,"N/A"]
[null,"Zinc","mg/kg",5,"3,700#2",null,"0.00 - 10,095#9",null,"N/A"]
["VOCs"]
[null,"Chloromethane","ug/kg",3,"9.8#3",null,null,null,"N/A"]
["SVOCs"]
[null,"Dibenzo[a,e]pyrene","ug/kg",100,"42#1",null,null,null," - "]
["PAH"]
[null,"Benzo(a) pyrene","mg/kg",0.01,"2.7#2","3.6#8","0.332 - 6.976#10",null,"N/A"]
[null,"Benzo(b)fluoranthene","mg/kg",0.01,"3.3#2",null,"0.272 - 4.141#10",null,"N/A"]
[null,"Dibenz(a,h)anthracene","mg/kg",0.01,"0.28#2",null,"0.033 - 0.843#10",null,"0.5  \n0.29"]
["PCB (Dutch 7) congeners"]
[null,"PCB 118","ug/kg",5,"120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Total PCB 7 Congeners","ug/kg",35,"200#5",null,"0.1 - 114.1#10",null,"N/A"]
["PCB (WHO12) 12 congeners"]
[null,"Pentachlorobiphenyl, 2,3',4,4',5- (PCB-118)","ug/kg","Various","120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Pentachlorobiphenyl, 3,3,4,4,5- (PCB 126)","ug/kg",5,"0.036#1",null,"0.0002 - 0.156#11",null,"0.157"]
["ESdat Calculated"]
[null,"Cresols Total","ug/kg",20,"180#3",null,null,null,"N/A"]
[null,"Benzo(a)pyrene (surrogate marker for PAH mixture)","mg/kg",0.01,"5.0#6",null,null,null,"N/A"]
["AECOM Calculated"]
[null,"Sum of PCDD/F +PCB12","ng/kg","Various","8700#4",null,null,null,11309]
[]
["Comments"]
["#1  USEPA RSL (May 2019)"]
["#2  LQM/CIEH S4ULs 2015"]
["#3  EIC/AGS/CL:AIRE 2010"]
["#4  EA SGV 2009"]
["#5  Dutch IV 2013"]
["#6  Defra C4SL 2014"]
["#7  AECOM (modified EIC GAC to include plant uptake route)"]
["#8  Johnson et al. 2012"]
["#9  London Earth"]
["#10  Vane"]
["#11  UKSHS"]
["GSC: Generic Screening Criteria"]
["(blank): No assessment criteria available"]
[" - : Not analysed"]
["N/A result was not above GSC"]
["* highest of two alternative values (obtained through different laboratory methods on same sample)"]
["Field_D: Field Duplicate"]
["HH: Human Health"]
["NAD: No Asbestos Detected"]
["Exceedance of HH Soil. Residential with Plant Uptake.  Sandy Loam.  TOC >=1.45 to <3.48%"]

{"sheet":"Markland House","index":10,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[[7,0,12,0],[18,0,20,0],[22,0,23,0],[28,0,29,0],[52,0,52,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6]]}
[]
[null,null,null,null,null,null,null,"Location","Communal open space at Markland House"]
[null,null,"Units","Method Detection Limit","GSC (human health residential scenario)","NBC","London Background (range min - max)","Sample identification","GTCS 1-31\nGTCS 1-32"]
[null,null,null,null,null,null,null,"Date","2019-06-07T10:50:00"]
[null,null,null,null,null,null,null,"Sample Type","Normal"]
[null,null,null,null,null,null,null,"Sample_Depth_Range","0-0.05"]
["Metals"]
[null,"Arsenic","mg/kg",0.5,"37#6",null,"1.2 - 160.90#9",null,"N/A"]
[null,"Barium","mg/kg",1,"460#7",null,"143.50 - 3475.10#9",null,"N/A"]
[null,"Beryllium","mg/kg",0.5,"1.7#2",null,null,null,"N/A"]
[null,"Cadmium","mg/kg",0.1,"22#6","2.1#8","0.00 - 165.20#9",null,"N/A"]
[null,"Lead","mg/kg",5,"200#6","820#8","10.8 - 10,000#9",null,301]
[null,"Zinc","mg/kg",5,"3,700#2",null,"0.00 - 10,095#9",null,"N/A"]
["VOCs"]
[null,"Chloromethane","ug/kg",3,"9.8#3",null,null,null,12]
["SVOCs"]
[null,"Dibenzo[a,e]pyrene","ug/kg",100,"42#1",null,null,null," - "]
["PAH"]
[null,"Benzo(a) pyrene","mg/kg",0.01,"2.7#2","3.6#8","0.332 - 6.976#10",null,"N/A"]
[null,"Benzo(b)fluoranthene","mg/kg",0.01,"3.3#2",null,"0.272 - 4.141#10",null,"N/A"]
[null,"Dibenz(a,h)anthracene","mg/kg",0.01,"0.28#2",null,"0.033 - 0.843#10",null,"N/A"]
["PCB (Dutch 7) congeners"]
[null,"PCB 118","ug/kg",5,"120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Total PCB 7 Congeners","ug/kg",35,"200#5",null,"0.1 - 114.1#10",null,"N/A"]
["PCB (WHO12) 12 congeners"]
[null,"Pentachlorobiphenyl, 2,3',4,4',5- (PCB-118)","ug/kg","Various","120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Pentachlorobiphenyl, 3,3,4,4,5- (PCB 126)","ug/kg",5,"0.036#1",null,"0.0002 - 0.156#11",null,"N/A"]
["ESdat Calculated"]
[null,"Cresols Total","ug/kg",20,"180#3",null,null,null,"N/A"]
[null,"Benzo(a)pyrene (surrogate marker for PAH mixture)","mg/kg",0.01,"5.0#6",null,null,null,"N/A"]
["AECOM Calculated"]
[null,"Sum of PCDD/F +PCB12","ng/kg","Various","8700#4",null,null,null,"N/A"]
[]
["Comments"]
["#1  USEPA RSL (May 2019)"]
["#2  LQM/CIEH S4ULs 2015"]
["#3  EIC/AGS/CL:AIRE 2010"]
["#4  EA SGV 2009"]
["#5  Dutch IV 2013"]
["#6  Defra C4SL 2014"]
["#7  AECOM (modified EIC GAC to include plant uptake route)"]
["#8  Johnson et al. 2012"]
["#9  London Earth"]
["#10  Vane"]
["#11  UKSHS"]
["GSC: Generic Screening Criteria"]
["(blank): No assessment criteria available"]
[" - : Not analysed"]
["N/A result was not above GSC"]
["* highest of two alternative values (obtained through different laboratory methods on same sample)"]
["Field_D: Field Duplicate"]
["HH: Human Health"]
["NAD: No Asbestos Detected"]
["Exceedance of HH Soil. Residential with Plant Uptake.  Sandy Loam.  TOC >=1.45 to <3.48%"]

{"sheet":"Morland House","index":11,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[[7,0,12,0],[18,0,20,0],[22,0,23,0],[28,0,29,0],[52,0,52,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6]]}
[]
[null,null,null,null,null,null,null,"Location","Communal open space at Morland House"]
[null,null,"Units","Method Detection Limit","GSC (human health residential scenario)","NBC","London Background (range min - max)","Sample identification","GTCS 1-11\nGTCS 1-12"]
[null,null,null,null,null,null,null,"Date","2019-06-06T17:00:00"]
[null,null,null,null,null,null,null,"Sample Type","Normal"]
[null,null,null,null,null,null,null,"Sample_Depth_Range","0-0.05"]
["Metals"]
[null,"Arsenic","mg/kg",0.5,"37#6",null,"1.2 - 160.90#9",null,"N/A"]
[null,"Barium","mg/kg",1,"460#7",null,"143.50 - 3475.10#9",null,"N/A"]
[null,"Beryllium","mg/kg",0.5,"1.7#2",null,null,null,"N/A"]
[null,"Cadmium","mg/kg",0.1,"22#6","2.1#8","0.00 - 165.20#9",null,"N/A"]
[null,"Lead","mg/kg",5,"200#6","820#8","10.8 - 10,000#9",null,"N/A"]
[null,"Zinc","mg/kg",5,"3,700#2",null,"0.00 - 10,095#9",null,"N/A"]
["VOCs"]
[null,"Chloromethane","ug/kg",3,"9.8#3",null,null,null,"17 \n20 \n14 \n21 \n14"]
["SVOCs"]
[null,"Dibenzo[a,e]pyrene","ug/kg",100,"42#1",null,null,null," - "]
["PAH"]
[null,"Benzo(a) pyrene","mg/kg",0.01,"2.7#2","3.6#8","0.332 - 6.976#10",null,"N/A"]
[null,"Benzo(b)fluoranthene","mg/kg",0.01,"3.3#2",null,"0.272 - 4.141#10",null,"N/A"]
[null,"Dibenz(a,h)anthracene","mg/kg",0.01,"0.28#2",null,"0.033 - 0.843#10",null,"N/A"]
["PCB (Dutch 7) congeners"]
[null,"PCB 118","ug/kg",5,"120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Total PCB 7 Congeners","ug/kg",35,"200#5",null,"0.1 - 114.1#10",null,"N/A"]
["PCB (WHO12) 12 congeners"]
[null,"Pentachlorobiphenyl, 2,3',4,4',5- (PCB-118)","ug/kg","Various","120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Pentachlorobiphenyl, 3,3,4,4,5- (PCB 126)","ug/kg",5,"0.036#1",null,"0.0002 - 0.156#11",null,"N/A"]
["ESdat Calculated"]
[null,"Cresols Total","ug/kg",20,"180#3",null,null,null,"N/A"]
[null,"Benzo(a)pyrene (surrogate marker for PAH mixture)","mg/kg",0.01,"5.0#6",null,null,null,"N/A"]
["AECOM Calculated"]
[null,"Sum of PCDD/F +PCB12","ng/kg","Various","8700#4",null,null,null,14761]
[]
["Comments"]
["#1  USEPA RSL (May 2019)"]
["#2  LQM/CIEH S4ULs 2015"]
["#3  EIC/AGS/CL:AIRE 2010"]
["#4  EA SGV 2009"]
["#5  Dutch IV 2013"]
["#6  Defra C4SL 2014"]
["#7  AECOM (modified EIC GAC to include plant uptake route)"]
["#8  Johnson et al. 2012"]
["#9  London Earth"]
["#10  Vane"]
["#11  UKSHS"]
["GSC: Generic Screening Criteria"]
["(blank): No assessment criteria available"]
[" - : Not analysed"]
["N/A result was not above GSC"]
["* highest of two alternative values (obtained through different laboratory methods on same sample)"]
["Field_D: Field Duplicate"]
["HH: Human Health"]
["NAD: No Asbestos Detected"]
["Exceedance of HH Soil. Residential with Plant Uptake.  Sandy Loam.  TOC >=1.45 to <3.48%"]

{"sheet":"Portland Road Kitchen garden ","index":12,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[[7,0,12,0],[18,0,20,0],[22,0,23,0],[28,0,29,0],[52,0,52,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6]]}
[]
[null,null,null,null,null,null,null,"Location","Community kitchen garden at Portland Road"]
[null,null,"Units","Method Detection Limit","GSC (human health residential scenario)","NBC","London Background (range min - max)","Sample identification","GTCS 1-17\nGTCS 1-18"]
[null,null,null,null,null,null,null,"Date","2019-06-05T10:40:00"]
[null,null,null,null,null,null,null,"Sample Type","Normal"]
[null,null,null,null,null,null,null,"Sample_Depth_Range","0-0.05"]
["Metals"]
[null,"Arsenic","mg/kg",0.5,"37#6",null,"1.2 - 160.90#9",null,"47.4* \n58.6*\n55.4*\n61.5*"]
[null,"Barium","mg/kg",1,"460#7",null,"143.50 - 3475.10#9",null,"991* \n945*\n948* \n944*"]
[null,"Beryllium","mg/kg",0.5,"1.7#2",null,null,null,"2.1 \n4* \n4.1* \n4.1*\n4*"]
[null,"Cadmium","mg/kg",0.1,"22#6","2.1#8","0.00 - 165.20#9",null,"N/A"]
[null,"Lead","mg/kg",5,"200#6","820#8","10.8 - 10,000#9",null,"492 \n1,785*\n1,780*\n1,528*\n1,519*"]
[null,"Zinc","mg/kg",5,"3,700#2",null,"0.00 - 10,095#9",null,"5,153*"]
["VOCs"]
[null,"Chloromethane","ug/kg",3,"9.8#3",null,null,null,"26\n11\n14\n19"]
["SVOCs"]
[null,"Dibenzo[a,e]pyrene","ug/kg",100,"42#1",null,null,null," - "]
["PAH"]
[null,"Benzo(a) pyrene","mg/kg",0.01,"2.7#2","3.6#8","0.332 - 6.976#10",null,"N/A"]
[null,"Benzo(b)fluoranthene","mg/kg",0.01,"3.3#2",null,"0.272 - 4.141#10",null,"N/A"]
[null,"Dibenz(a,h)anthracene","mg/kg",0.01,"0.28#2",null,"0.033 - 0.843#10",null,"0.33"]
["PCB (Dutch 7) congeners"]
[null,"PCB 118","ug/kg",5,"120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Total PCB 7 Congeners","ug/kg",35,"200#5",null,"0.1 - 114.1#10",null,"N/A"]
["PCB (WHO12) 12 congeners"]
[null,"Pentachlorobiphenyl, 2,3',4,4',5- (PCB-118)","ug/kg","Various","120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Pentachlorobiphenyl, 3,3,4,4,5- (PCB 126)","ug/kg",5,"0.036#1",null,"0.0002 - 0.156#11",null,"0.0387\n0.0633\n0.043\n0.0377"]
["ESdat Calculated"]
[null,"Cresols Total","ug/kg",20,"180#3",null,null,null,"N/A"]
[null,"Benzo(a)pyrene (surrogate marker for PAH mixture)","mg/kg",0.01,"5.0#6",null,null,null,"N/A"]
["AECOM Calculated"]
[null,"Sum of PCDD/F +PCB12","ng/kg","Various","8700#4",null,null,null,"N/A"]
[]
["Comments"]
["#1  USEPA RSL (May 2019)"]
["#2  LQM/CIEH S4ULs 2015"]
["#3  EIC/AGS/CL:AIRE 2010"]
["#4  EA SGV 2009"]
["#5  Dutch IV 2013"]
["#6  Defra C4SL 2014"]
["#7  AECOM (modified EIC GAC to include plant uptake route)"]
["#8  Johnson et al. 2012"]
["#9  London Earth"]
["#10  Vane"]
["#11  UKSHS"]
["GSC: Generic Screening Criteria"]
["(blank): No assessment criteria available"]
[" - : Not analysed"]
["N/A result was not above GSC"]
["* highest of two alternative values (obtained through different laboratory methods on same sample)"]
["Field_D: Field Duplicate"]
["HH: Human Health"]
["NAD: No Asbestos Detected"]
["Exceedance of HH Soil. Residential with Plant Uptake.  Sandy Loam.  TOC >=1.45 to <3.48%"]

{"sheet":"Robinson House","index":13,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[[7,0,12,0],[18,0,20,0],[22,0,23,0],[28,0,29,0],[52,0,52,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6]]}
[]
[null,null,null,null,null,null,null,"Location","Robinson House"]
[null,null,"Units","Method Detection Limit","GSC (human health residential scenario)","NBC","London Background (range min - max)","Sample identification","GTCS 1-35\nGTCS 1-36"]
[null,null,null,null,null,null,null,"Date","2019-06-04T11:25:00"]
[null,null,null,null,null,null,null,"Sample Type","Normal"]
[null,null,null,null,null,null,null,"Sample_Depth_Range","0-0.05"]
["Metals"]
[null,"Arsenic","mg/kg",0.5,"37#6",null,"1.2 - 160.90#9",null,"N/A"]
[null,"Barium","mg/kg",1,"460#7",null,"143.50 - 3475.10#9",null,"N/A"]
[null,"Beryllium","mg/kg",0.5,"1.7#2",null,null,null,"N/A"]
[null,"Cadmium","mg/kg",0.1,"22#6","2.1#8","0.00 - 165.20#9",null,"N/A"]
[null,"Lead","mg/kg",5,"200#6","820#8","10.8 - 10,000#9",null,"312\n341*\n327*\n385*\n275"]
[null,"Zinc","mg/kg",5,"3,700#2",null,"0.00 - 10,095#9",null,"N/A"]
["VOCs"]
[null,"Chloromethane","ug/kg",3,"9.8#3",null,null,null,"19"]
["SVOCs"]
[null,"Dibenzo[a,e]pyrene","ug/kg",100,"42#1",null,null,null," - "]
["PAH"]
[null,"Benzo(a) pyrene","mg/kg",0.01,"2.7#2","3.6#8","0.332 - 6.976#10",null,"3.97\n2.81"]
[null,"Benzo(b)fluoranthene","mg/kg",0.01,"3.3#2",null,"0.272 - 4.141#10",null,"5.09\n3.58"]
[null,"Dibenz(a,h)anthracene","mg/kg",0.01,"0.28#2",null,"0.033 - 0.843#10",null,"0.71\n0.41\n0.47"]
["PCB (Dutch 7) congeners"]
[null,"PCB 118","ug/kg",5,"120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Total PCB 7 Congeners","ug/kg",35,"200#5",null,"0.1 - 114.1#10",null,"N/A"]
["PCB (WHO12) 12 congeners"]
[null,"Pentachlorobiphenyl, 2,3',4,4',5- (PCB-118)","ug/kg","Various","120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Pentachlorobiphenyl, 3,3,4,4,5- (PCB 126)","ug/kg",5,"0.036#1",null,"0.0002 - 0.156#11",null,"N/A"]
["ESdat Calculated"]
[null,"Cresols Total","ug/kg",20,"180#3",null,null,null,"N/A"]
[null,"Benzo(a)pyrene (surrogate marker for PAH mixture)","mg/kg",0.01,"5.0#6",null,null,null,"N/A"]
["AECOM Calculated"]
[null,"Sum of PCDD/F +PCB12","ng/kg","Various","8700#4",null,null,null,"N/A"]
[]
["Comments"]
["#1  USEPA RSL (May 2019)"]
["#2  LQM/CIEH S4ULs 2015"]
["#3  EIC/AGS/CL:AIRE 2010"]
["#4  EA SGV 2009"]
["#5  Dutch IV 2013"]
["#6  Defra C4SL 2014"]
["#7  AECOM (modified EIC GAC to include plant uptake route)"]
["#8  Johnson et al. 2012"]
["#9  London Earth"]
["#10  Vane"]
["#11  UKSHS"]
["GSC: Generic Screening Criteria"]
["(blank): No assessment criteria available"]
[" - : Not analysed"]
["N/A result was not above GSC"]
["* highest of two alternative values (obtained through different laboratory methods on same sample)"]
["Field_D: Field Duplicate"]
["HH: Human Health"]
["NAD: No Asbestos Detected"]
["Exceedance of HH Soil. Residential with Plant Uptake.  Sandy Loam.  TOC >=1.45 to <3.48%"]

{"sheet":"St Quintin Kitchen Garden","index":14,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[[7,0,12,0],[18,0,20,0],[22,0,23,0],[28,0,29,0],[52,0,52,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6]]}
[]
[null,null,null,null,null,null,null,"Location","St Quintin Community Kitchen Gardens"]
[null,null,"Units","Method Detection Limit","GSC (human health residential scenario)","NBC","London Background (range min - max)","Sample identification","GTCS 1-29\nGTCS 1-30"]
[null,null,null,null,null,null,null,"Date","2019-06-06T15:30:00"]
[null,null,null,null,null,null,null,"Sample Type","Normal"]
[null,null,null,null,null,null,null,"Sample_Depth_Range","0-0.05"]
["Metals"]
[null,"Arsenic","mg/kg",0.5,"37#6",null,"1.2 - 160.90#9",null,"92.9*"]
[null,"Barium","mg/kg",1,"460#7",null,"143.50 - 3475.10#9",null,"475*\n535*\n607*\n575*"]
[null,"Beryllium","mg/kg",0.5,"1.7#2",null,null,null,"2.2*\n1.9*\n2*\n1.8*"]
[null,"Cadmium","mg/kg",0.1,"22#6","2.1#8","0.00 - 165.20#9",null,"N/A"]
[null,"Lead","mg/kg",5,"200#6","820#8","10.8 - 10,000#9",null,"980*\n1,083*\n1,111*\n1,597*\n"]
[null,"Zinc","mg/kg",5,"3,700#2",null,"0.00 - 10,095#9",null,"N/A"]
["VOCs"]
[null,"Chloromethane","ug/kg",3,"9.8#3",null,null,null,"10\n12\n"]
["SVOCs"]
[null,"Dibenzo[a,e]pyrene","ug/kg",100,"42#1",null,null,null," - "]
["PAH"]
[null,"Benzo(a) pyrene","mg/kg",0.01,"2.7#2","3.6#8","0.332 - 6.976#10",null,"2.87\n2.81\n3.18"]
[null,"Benzo(b)fluoranthene","mg/kg",0.01,"3.3#2",null,"0.272 - 4.141#10",null,"4.13\n3.69\n3.66\n4.53"]
[null,"Dibenz(a,h)anthracene","mg/kg",0.01,"0.28#2",null,"0.033 - 0.843#10",null,"0.39\n0.42\n0.45\n0.6"]
["PCB (Dutch 7) congeners"]
[null,"PCB 118","ug/kg",5,"120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Total PCB 7 Congeners","ug/kg",35,"200#5",null,"0.1 - 114.1#10",null,"N/A"]
["PCB (WHO12) 12 congeners"]
[null,"Pentachlorobiphenyl, 2,3',4,4',5- (PCB-118)","ug/kg","Various","120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Pentachlorobiphenyl, 3,3,4,4,5- (PCB 126)","ug/kg",5,"0.036#1",null,"0.0002 - 0.156#11",null,"N/A"]
["ESdat Calculated"]
[null,"Cresols Total","ug/kg",20,"180#3",null,null,null,"N/A"]
[null,"Benzo(a)pyrene (surrogate marker for PAH mixture)","mg/kg",0.01,"5.0#6",null,null,null,"N/A"]
["AECOM Calculated"]
[null,"Sum of PCDD/F +PCB12","ng/kg","Various","8700#4",null,null,null,"13098\n18758\n33961\n21417"]
[]
["Comments"]
["#1  USEPA RSL (May 2019)"]
["#2  LQM/CIEH S4ULs 2015"]
["#3  EIC/AGS/CL:AIRE 2010"]
["#4  EA SGV 2009"]
["#5  Dutch IV 2013"]
["#6  Defra C4SL 2014"]
["#7  AECOM (modified EIC GAC to include plant uptake route)"]
["#8  Johnson et al. 2012"]
["#9  London Earth"]
["#10  Vane"]
["#11  UKSHS"]
["GSC: Generic Screening Criteria"]
["(blank): No assessment criteria available"]
[" - : Not analysed"]
["N/A result was not above GSC"]
["* highest of two alternative values (obtained through different laboratory methods on same sample)"]
["Field_D: Field Duplicate"]
["HH: Human Health"]
["NAD: No Asbestos Detected"]
["Exceedance of HH Soil. Residential with Plant Uptake.  Sandy Loam.  TOC >=1.45 to <3.48%"]

{"sheet":"St. Quintin’s Roundabout","index":15,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[[7,0,12,0],[18,0,20,0],[22,0,23,0],[28,0,29,0],[52,0,52,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6]]}
[]
[null,null,null,null,null,null,null,"Location","St. Quintin’s Roundabout"]
[null,null,"Units","Method Detection Limit","GSC (human health residential scenario)","NBC","London Background (range min - max)","Sample identification","GTCS 1-41\nGTCS 1-42"]
[null,null,null,null,null,null,null,"Date","2019-06-04T14:45:00"]
[null,null,null,null,null,null,null,"Sample Type","Normal"]
[null,null,null,null,null,null,null,"Sample_Depth_Range","0-0.05"]
["Metals"]
[null,"Arsenic","mg/kg",0.5,"37#6",null,"1.2 - 160.90#9",null,"N/A"]
[null,"Barium","mg/kg",1,"460#7",null,"143.50 - 3475.10#9",null,"N/A"]
[null,"Beryllium","mg/kg",0.5,"1.7#2",null,null,null,"1.9"]
[null,"Cadmium","mg/kg",0.1,"22#6","2.1#8","0.00 - 165.20#9",null,"N/A"]
[null,"Lead","mg/kg",5,"200#6","820#8","10.8 - 10,000#9",null,"552\n556\n571\n564\n517"]
[null,"Zinc","mg/kg",5,"3,700#2",null,"0.00 - 10,095#9",null,"N/A"]
["VOCs"]
[null,"Chloromethane","ug/kg",3,"9.8#3",null,null,null,"27\n28\n30\n33"]
["SVOCs"]
[null,"Dibenzo[a,e]pyrene","ug/kg",100,"42#1",null,null,null," - "]
["PAH"]
[null,"Benzo(a) pyrene","mg/kg",0.01,"2.7#2","3.6#8","0.332 - 6.976#10",null,"5.11\n5.04\n5.34\n4.88\n3.8"]
[null,"Benzo(b)fluoranthene","mg/kg",0.01,"3.3#2",null,"0.272 - 4.141#10",null,"7.02\n6.83\n7.21\n6.65\n5.23"]
[null,"Dibenz(a,h)anthracene","mg/kg",0.01,"0.28#2",null,"0.033 - 0.843#10",null,"1\n0.8\n0.87\n0.79\n0.56"]
["PCB (Dutch 7) congeners"]
[null,"PCB 118","ug/kg",5,"120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Total PCB 7 Congeners","ug/kg",35,"200#5",null,"0.1 - 114.1#10",null,"N/A"]
["PCB (WHO12) 12 congeners"]
[null,"Pentachlorobiphenyl, 2,3',4,4',5- (PCB-118)","ug/kg","Various","120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Pentachlorobiphenyl, 3,3,4,4,5- (PCB 126)","ug/kg",5,"0.036#1",null,"0.0002 - 0.156#11",null,"N/A"]
["ESdat Calculated"]
[null,"Cresols Total","ug/kg",20,"180#3",null,null,null,"N/A"]
[null,"Benzo(a)pyrene (surrogate marker for PAH mixture)","mg/kg",0.01,"5.0#6",null,null,null,"5.11\n5.04\n5.34"]
["AECOM Calculated"]
[null,"Sum of PCDD/F +PCB12","ng/kg","Various","8700#4",null,null,null,"N/A"]
[]
["Comments"]
["#1  USEPA RSL (May 2019)"]
["#2  LQM/CIEH S4ULs 2015"]
["#3  EIC/AGS/CL:AIRE 2010"]
["#4  EA SGV 2009"]
["#5  Dutch IV 2013"]
["#6  Defra C4SL 2014"]
["#7  AECOM (modified EIC GAC to include plant uptake route)"]
["#8  Johnson et al. 2012"]
["#9  London Earth"]
["#10  Vane"]
["#11  UKSHS"]
["GSC: Generic Screening Criteria"]
["(blank): No assessment criteria available"]
[" - : Not analysed"]
["N/A result was not above GSC"]
["* highest of two alternative values (obtained through different laboratory methods on same sample)"]
["Field_D: Field Duplicate"]
["HH: Human Health"]
["NAD: No Asbestos Detected"]
["Exceedance of HH Soil. Residential with Plant Uptake.  Sandy Loam.  TOC >=1.45 to <3.48%"]

{"sheet":"Tower Cordon","index":16,"n_rows":54,"n_cols":12,"rows_kept":54,"cut":false,"hidden":false,"merged":[[7,0,12,0],[18,0,20,0],[22,0,23,0],[28,0,29,0],[52,0,52,1],[1,8,1,11],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6]]}
[]
[null,null,null,null,null,null,null,"Location","Tower Cordon"]
[null,null,"Units","Method Detection Limit","GSC (human health residential scenario)","NBC","London Background (range min - max)","Sample identification","GTCS101","GTCS102","GTCS103","GTCS104"]
[null,null,null,null,null,null,null,"Date","2019-04-10","2019-04-10","2019-04-10","2019-04-10"]
[null,null,null,null,null,null,null,"Sample Type","Normal","Normal","Normal","Normal"]
[null,null,null,null,null,null,null,"Sample_Depth_Range","0-0.05","0-0.05","0-0.05","0-0.05"]
["Metals"]
[null,"Arsenic","mg/kg",0.5,"37#6",null,"1.2 - 160.90#9",null,"N/A","N/A","N/A","N/A"]
[null,"Barium","mg/kg",1,"460#7",null,"143.50 - 3475.10#9",null,"N/A","N/A","N/A","N/A"]
[null,"Beryllium","mg/kg",0.5,"1.7#2",null,null,null,"N/A","N/A","N/A","N/A"]
[null,"Cadmium","mg/kg",0.1,"22#6","2.1#8","0.00 - 165.20#9",null,"N/A","N/A","N/A","N/A"]
[null,"Lead","mg/kg",5,"200#6","820#8","10.8 - 10,000#9",null,"N/A","N/A","N/A","N/A"]
[null,"Zinc","mg/kg",5,"3,700#2",null,"0.00 - 10,095#9",null,"N/A","N/A","N/A","N/A"]
["VOCs"]
[null,"Chloromethane","ug/kg",3,"9.8#3",null,null,null,"N/A","N/A","N/A","N/A"]
["SVOCs"]
[null,"Dibenzo[a,e]pyrene","ug/kg",100,"42#1",null,null,null," - "," - "," - "," - "]
["PAH"]
[null,"Benzo(a) pyrene","mg/kg",0.01,"2.7#2","3.6#8","0.332 - 6.976#10",null,"N/A","N/A","N/A","N/A"]
[null,"Benzo(b)fluoranthene","mg/kg",0.01,"3.3#2",null,"0.272 - 4.141#10",null,"N/A","N/A","N/A","N/A"]
[null,"Dibenz(a,h)anthracene","mg/kg",0.01,"0.28#2",null,"0.033 - 0.843#10",null,"N/A","N/A","N/A","N/A"]
["PCB (Dutch 7) congeners"]
[null,"PCB 118","ug/kg",5,"120#1",null,"0.1 - 76.5#10",null,"N/A","N/A","N/A","N/A"]
[null,"Total PCB 7 Congeners","ug/kg",35,"200#5",null,"0.1 - 114.1#10",null," - "," - "," - "," - "]
["PCB (WHO12) 12 congeners"]
[null,"Pentachlorobiphenyl, 2,3',4,4',5- (PCB-118)","ug/kg","Various","120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Pentachlorobiphenyl, 3,3,4,4,5- (PCB 126)","ug/kg",5,"0.036#1",null,"0.0002 - 0.156#11",null,"N/A","N/A","N/A","N/A"]
["ESdat Calculated"]
[null,"Cresols Total","ug/kg",20,"180#3",null,null,null,"N/A","N/A","N/A","N/A"]
[null,"Benzo(a)pyrene (surrogate marker for PAH mixture)","mg/kg",0.01,"5.0#6",null,null,null,"N/A","N/A","N/A","N/A"]
["AECOM Calculated"]
[null,"Sum of PCDD/F +PCB12","ng/kg","Various","8700#4",null,null,null,"N/A","N/A","N/A","N/A"]
[]
["Comments"]
["#1  USEPA RSL (May 2019)"]
["#2  LQM/CIEH S4ULs 2015"]
["#3  EIC/AGS/CL:AIRE 2010"]
["#4  EA SGV 2009"]
["#5  Dutch IV 2013"]
["#6  Defra C4SL 2014"]
["#7  AECOM (modified EIC GAC to include plant uptake route)"]
["#8  Johnson et al. 2012"]
["#9  London Earth"]
["#10  Vane"]
["#11  UKSHS"]
["GSC: Generic Screening Criteria"]
["(blank): No assessment criteria available"]
[" - : Not analysed"]
["N/A result was not above GSC"]
["* highest of two alternative values (obtained through different laboratory methods on same sample)"]
["Field_D: Field Duplicate"]
["HH: Human Health"]
["NAD: No Asbestos Detected"]
["Exceedance of HH Soil. Residential with Plant Uptake.  Sandy Loam.  TOC >=1.45 to <3.48%"]

{"sheet":"Treadgold House","index":17,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[[7,0,12,0],[18,0,20,0],[22,0,23,0],[28,0,29,0],[52,0,52,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6]]}
[]
[null,null,null,null,null,null,null,"Location","Communal garden at Treadgold House"]
[null,null,"Units","Method Detection Limit","GSC (human health residential scenario)","NBC","London Background (range min - max)","Sample identification","GTCS 1-07\nGTCS 1-08"]
[null,null,null,null,null,null,null,"Date","2019-06-06"]
[null,null,null,null,null,null,null,"Sample Type","Normal"]
[null,null,null,null,null,null,null,"Sample_Depth_Range","0-0.05"]
["Metals"]
[null,"Arsenic","mg/kg",0.5,"37#6",null,"1.2 - 160.90#9",null,"N/A"]
[null,"Barium","mg/kg",1,"460#7",null,"143.50 - 3475.10#9",null,"N/A"]
[null,"Beryllium","mg/kg",0.5,"1.7#2",null,null,null,"1.8 \n2.1 \n2.3*\n2.6\n2.3"]
[null,"Cadmium","mg/kg",0.1,"22#6","2.1#8","0.00 - 165.20#9",null,"N/A"]
[null,"Lead","mg/kg",5,"200#6","820#8","10.8 - 10,000#9",null,"500 \n473 \n516* \n442 \n587"]
[null,"Zinc","mg/kg",5,"3,700#2",null,"0.00 - 10,095#9",null,"N/A"]
["VOCs"]
[null,"Chloromethane","ug/kg",3,"9.8#3",null,null,null,"N/A"]
["SVOCs"]
[null,"Dibenzo[a,e]pyrene","ug/kg",100,"42#1",null,null,null," - "]
["PAH"]
[null,"Benzo(a) pyrene","mg/kg",0.01,"2.7#2","3.6#8","0.332 - 6.976#10",null,"N/A"]
[null,"Benzo(b)fluoranthene","mg/kg",0.01,"3.3#2",null,"0.272 - 4.141#10",null,"N/A"]
[null,"Dibenz(a,h)anthracene","mg/kg",0.01,"0.28#2",null,"0.033 - 0.843#10",null,"0.33"]
["PCB (Dutch 7) congeners"]
[null,"PCB 118","ug/kg",5,"120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Total PCB 7 Congeners","ug/kg",35,"200#5",null,"0.1 - 114.1#10",null,"N/A"]
["PCB (WHO12) 12 congeners"]
[null,"Pentachlorobiphenyl, 2,3',4,4',5- (PCB-118)","ug/kg","Various","120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Pentachlorobiphenyl, 3,3,4,4,5- (PCB 126)","ug/kg",5,"0.036#1",null,"0.0002 - 0.156#11",null,"N/A"]
["ESdat Calculated"]
[null,"Cresols Total","ug/kg",20,"180#3",null,null,null,"N/A"]
[null,"Benzo(a)pyrene (surrogate marker for PAH mixture)","mg/kg",0.01,"5.0#6",null,null,null,"N/A"]
["AECOM Calculated"]
[null,"Sum of PCDD/F +PCB12","ng/kg","Various","8700#4",null,null,null,"N/A"]
[]
["Comments"]
["#1  USEPA RSL (May 2019)"]
["#2  LQM/CIEH S4ULs 2015"]
["#3  EIC/AGS/CL:AIRE 2010"]
["#4  EA SGV 2009"]
["#5  Dutch IV 2013"]
["#6  Defra C4SL 2014"]
["#7  AECOM (modified EIC GAC to include plant uptake route)"]
["#8  Johnson et al. 2012"]
["#9  London Earth"]
["#10  Vane"]
["#11  UKSHS"]
["GSC: Generic Screening Criteria"]
["(blank): No assessment criteria available"]
[" - : Not analysed"]
["N/A result was not above GSC"]
["* highest of two alternative values (obtained through different laboratory methods on same sample)"]
["Field_D: Field Duplicate"]
["HH: Human Health"]
["NAD: No Asbestos Detected"]
["Exceedance of HH Soil. Residential with Plant Uptake.  Sandy Loam.  TOC >=1.45 to <3.48%"]

{"sheet":"Verity Close","index":18,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[[7,0,12,0],[18,0,20,0],[22,0,23,0],[28,0,29,0],[52,0,52,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6]]}
[]
[null,null,null,null,null,null,null,"Location","Open space at Verity Close"]
[null,null,"Units","Method Detection Limit","GSC (human health residential scenario)","NBC","London Background (range min - max)","Sample identification","GTCS 1-09\nGTCS 1-10"]
[null,null,null,null,null,null,null,"Date","2019-06-06"]
[null,null,null,null,null,null,null,"Sample Type","Normal"]
[null,null,null,null,null,null,null,"Sample_Depth_Range","0-0.05"]
["Metals"]
[null,"Arsenic","mg/kg",0.5,"37#6",null,"1.2 - 160.90#9",null,"N/A"]
[null,"Barium","mg/kg",1,"460#7",null,"143.50 - 3475.10#9",null,"N/A"]
[null,"Beryllium","mg/kg",0.5,"1.7#2",null,null,null,"N/A"]
[null,"Cadmium","mg/kg",0.1,"22#6","2.1#8","0.00 - 165.20#9",null,"N/A"]
[null,"Lead","mg/kg",5,"200#6","820#8","10.8 - 10,000#9",null,"N/A"]
[null,"Zinc","mg/kg",5,"3,700#2",null,"0.00 - 10,095#9",null,"N/A"]
["VOCs"]
[null,"Chloromethane","ug/kg",3,"9.8#3",null,null,null,"12 \n10"]
["SVOCs"]
[null,"Dibenzo[a,e]pyrene","ug/kg",100,"42#1",null,null,null," - "]
["PAH"]
[null,"Benzo(a) pyrene","mg/kg",0.01,"2.7#2","3.6#8","0.332 - 6.976#10",null,"N/A"]
[null,"Benzo(b)fluoranthene","mg/kg",0.01,"3.3#2",null,"0.272 - 4.141#10",null,"N/A"]
[null,"Dibenz(a,h)anthracene","mg/kg",0.01,"0.28#2",null,"0.033 - 0.843#10",null,"N/A"]
["PCB (Dutch 7) congeners"]
[null,"PCB 118","ug/kg",5,"120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Total PCB 7 Congeners","ug/kg",35,"200#5",null,"0.1 - 114.1#10",null,"N/A"]
["PCB (WHO12) 12 congeners"]
[null,"Pentachlorobiphenyl, 2,3',4,4',5- (PCB-118)","ug/kg","Various","120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Pentachlorobiphenyl, 3,3,4,4,5- (PCB 126)","ug/kg",5,"0.036#1",null,"0.0002 - 0.156#11",null,"N/A"]
["ESdat Calculated"]
[null,"Cresols Total","ug/kg",20,"180#3",null,null,null,"N/A"]
[null,"Benzo(a)pyrene (surrogate marker for PAH mixture)","mg/kg",0.01,"5.0#6",null,null,null,"N/A"]
["AECOM Calculated"]
[null,"Sum of PCDD/F +PCB12","ng/kg","Various","8700#4",null,null,null,"N/A"]
[]
["Comments"]
["#1  USEPA RSL (May 2019)"]
["#2  LQM/CIEH S4ULs 2015"]
["#3  EIC/AGS/CL:AIRE 2010"]
["#4  EA SGV 2009"]
["#5  Dutch IV 2013"]
["#6  Defra C4SL 2014"]
["#7  AECOM (modified EIC GAC to include plant uptake route)"]
["#8  Johnson et al. 2012"]
["#9  London Earth"]
["#10  Vane"]
["#11  UKSHS"]
["GSC: Generic Screening Criteria"]
["(blank): No assessment criteria available"]
[" - : Not analysed"]
["N/A result was not above GSC"]
["* highest of two alternative values (obtained through different laboratory methods on same sample)"]
["Field_D: Field Duplicate"]
["HH: Human Health"]
["NAD: No Asbestos Detected"]
["Exceedance of HH Soil. Residential with Plant Uptake.  Sandy Loam.  TOC >=1.45 to <3.48%"]

{"sheet":"Waynflete Square","index":19,"n_rows":54,"n_cols":10,"rows_kept":54,"cut":false,"hidden":false,"merged":[[7,0,12,0],[18,0,20,0],[22,0,23,0],[28,0,29,0],[52,0,52,1],[1,8,1,9],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6],[3,8,3,9],[4,8,4,9]]}
[]
[null,null,null,null,null,null,null,"Location","Waynflete Square"]
[null,null,"Units","Method Detection Limit","GSC (human health residential scenario)","NBC","London Background (range min - max)","Sample identification","GTCS 1-43\nto\nGTCS 1-59","GTCS 1-43\nto\nGTCS 1-51"]
[null,null,null,null,null,null,null,"Date","2019-06-05"]
[null,null,null,null,null,null,null,"Sample Type","Normal"]
[null,null,null,null,null,null,null,"Sample_Depth_Range","0-0.05","0.1-0.15"]
["Metals"]
[null,"Arsenic","mg/kg",0.5,"37#6",null,"1.2 - 160.90#9",null,"N/A","40.6*"]
[null,"Barium","mg/kg",1,"460#7",null,"143.50 - 3475.10#9",null,"N/A","537*"]
[null,"Beryllium","mg/kg",0.5,"1.7#2",null,null,null,"1.8*","2.2*\n2\n2*"]
[null,"Cadmium","mg/kg",0.1,"22#6","2.1#8","0.00 - 165.20#9",null,"N/A","46.2*\n46.8*"]
[null,"Lead","mg/kg",5,"200#6","820#8","10.8 - 10,000#9",null,"603*\n232\n318\n578\n257*\n298*\n222\n331\n422*\n330\n287\n484*\n274\n263","757*\n448*\n385\n429*\n334*"]
[null,"Zinc","mg/kg",5,"3,700#2",null,"0.00 - 10,095#9",null,"N/A","N/A"]
["VOCs"]
[null,"Chloromethane","ug/kg",3,"9.8#3",null,null,null,"10\n10\n13\n12\n14\n10\n11","16"]
["SVOCs"]
[null,"Dibenzo[a,e]pyrene","ug/kg",100,"42#1",null,null,null,6277," - "]
["PAH"]
[null,"Benzo(a) pyrene","mg/kg",0.01,"2.7#2","3.6#8","0.332 - 6.976#10",null,"2.75\n5.55\n3.27\n4.54\n","8.61\n3.13\n6.93"]
[null,"Benzo(b)fluoranthene","mg/kg",0.01,"3.3#2",null,"0.272 - 4.141#10",null,"3.87\n7.34\n4.47\n6.397*\n6.03","11.28\n3.83\n9.33"]
[null,"Dibenz(a,h)anthracene","mg/kg",0.01,"0.28#2",null,"0.033 - 0.843#10",null,"0.44\n0.96\n0.66\n0.36\n0.29\n0.74\n0.38\n0.37","1.51\n0.69\n1.44\n0.38\n0.34"]
["PCB (Dutch 7) congeners"]
[null,"PCB 118","ug/kg",5,"120#1",null,"0.1 - 76.5#10",null,"154*","N/A"]
[null,"Total PCB 7 Congeners","ug/kg",35,"200#5",null,"0.1 - 114.1#10",null,"407","N/A"]
["PCB (WHO12) 12 congeners"]
[null,"Pentachlorobiphenyl, 2,3',4,4',5- (PCB-118)","ug/kg","Various","120#1",null,"0.1 - 76.5#10",null,154,"N/A"]
[null,"Pentachlorobiphenyl, 3,3,4,4,5- (PCB 126)","ug/kg",5,"0.036#1",null,"0.0002 - 0.156#11",null,"0.04\n0.169\n0.0462\n0.12","0.0497\n0.0856"]
["ESdat Calculated"]
[null,"Cresols Total","ug/kg",20,"180#3",null,null,null,313,"N/A"]
[null,"Benzo(a)pyrene (surrogate marker for PAH mixture)","mg/kg",0.01,"5.0#6",null,null,null,"5.55","8.61\n6.93"]
["AECOM Calculated"]
[null,"Sum of PCDD/F +PCB12","ng/kg","Various","8700#4",null,null,null,"10165\n69988\n18171\n11930\n16597\n63213\n12644\n279697\n95814\n","20610\n12518\n39446\n11069\n11187"]
[]
["Comments"]
["#1  USEPA RSL (May 2019)"]
["#2  LQM/CIEH S4ULs 2015"]
["#3  EIC/AGS/CL:AIRE 2010"]
["#4  EA SGV 2009"]
["#5  Dutch IV 2013"]
["#6  Defra C4SL 2014"]
["#7  AECOM (modified EIC GAC to include plant uptake route)"]
["#8  Johnson et al. 2012"]
["#9  London Earth"]
["#10  Vane"]
["#11  UKSHS"]
["GSC: Generic Screening Criteria"]
["(blank): No assessment criteria available"]
[" - : Not analysed"]
["N/A result was not above GSC"]
["* highest of two alternative values (obtained through different laboratory methods on same sample)"]
["Field_D: Field Duplicate"]
["HH: Human Health"]
["NAD: No Asbestos Detected"]
["Exceedance of HH Soil. Residential with Plant Uptake.  Sandy Loam.  TOC >=1.45 to <3.48%"]

{"sheet":"West London Bowling Club","index":20,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[[7,0,12,0],[18,0,20,0],[22,0,23,0],[28,0,29,0],[52,0,52,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6]]}
[]
[null,null,null,null,null,null,null,"Location","West London Bowling Club"]
[null,null,"Units","Method Detection Limit","GSC (human health residential scenario)","NBC","London Background (range min - max)","Sample identification","GTCS 1-39\nGTCS 1-40"]
[null,null,null,null,null,null,null,"Date","2019-06-04T16:45:00"]
[null,null,null,null,null,null,null,"Sample Type","Normal"]
[null,null,null,null,null,null,null,"Sample_Depth_Range","0-0.05"]
["Metals"]
[null,"Arsenic","mg/kg",0.5,"37#6",null,"1.2 - 160.90#9",null,"N/A"]
[null,"Barium","mg/kg",1,"460#7",null,"143.50 - 3475.10#9",null,"563"]
[null,"Beryllium","mg/kg",0.5,"1.7#2",null,null,null,"1.8*\n2.1*\n2.7\n1.8*\n2.2"]
[null,"Cadmium","mg/kg",0.1,"22#6","2.1#8","0.00 - 165.20#9",null,"N/A"]
[null,"Lead","mg/kg",5,"200#6","820#8","10.8 - 10,000#9",null,"398*\n392*\n431\n393*\n1311"]
[null,"Zinc","mg/kg",5,"3,700#2",null,"0.00 - 10,095#9",null,"N/A"]
["VOCs"]
[null,"Chloromethane","ug/kg",3,"9.8#3",null,null,null,"12\n10\n13\n10\n27"]
["SVOCs"]
[null,"Dibenzo[a,e]pyrene","ug/kg",100,"42#1",null,null,null," - "]
["PAH"]
[null,"Benzo(a) pyrene","mg/kg",0.01,"2.7#2","3.6#8","0.332 - 6.976#10",null,"N/A"]
[null,"Benzo(b)fluoranthene","mg/kg",0.01,"3.3#2",null,"0.272 - 4.141#10",null,"N/A"]
[null,"Dibenz(a,h)anthracene","mg/kg",0.01,"0.28#2",null,"0.033 - 0.843#10",null,"0.37\n0.32"]
["PCB (Dutch 7) congeners"]
[null,"PCB 118","ug/kg",5,"120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Total PCB 7 Congeners","ug/kg",35,"200#5",null,"0.1 - 114.1#10",null,"N/A"]
["PCB (WHO12) 12 congeners"]
[null,"Pentachlorobiphenyl, 2,3',4,4',5- (PCB-118)","ug/kg","Various","120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Pentachlorobiphenyl, 3,3,4,4,5- (PCB 126)","ug/kg",5,"0.036#1",null,"0.0002 - 0.156#11",null,"N/A"]
["ESdat Calculated"]
[null,"Cresols Total","ug/kg",20,"180#3",null,null,null,"N/A"]
[null,"Benzo(a)pyrene (surrogate marker for PAH mixture)","mg/kg",0.01,"5.0#6",null,null,null,"N/A"]
["AECOM Calculated"]
[null,"Sum of PCDD/F +PCB12","ng/kg","Various","8700#4",null,null,null,"N/A"]
[]
["Comments"]
["#1  USEPA RSL (May 2019)"]
["#2  LQM/CIEH S4ULs 2015"]
["#3  EIC/AGS/CL:AIRE 2010"]
["#4  EA SGV 2009"]
["#5  Dutch IV 2013"]
["#6  Defra C4SL 2014"]
["#7  AECOM (modified EIC GAC to include plant uptake route)"]
["#8  Johnson et al. 2012"]
["#9  London Earth"]
["#10  Vane"]
["#11  UKSHS"]
["GSC: Generic Screening Criteria"]
["(blank): No assessment criteria available"]
[" - : Not analysed"]
["N/A result was not above GSC"]
["* highest of two alternative values (obtained through different laboratory methods on same sample)"]
["Field_D: Field Duplicate"]
["HH: Human Health"]
["NAD: No Asbestos Detected"]
["Exceedance of HH Soil. Residential with Plant Uptake.  Sandy Loam.  TOC >=1.45 to <3.48%"]

{"sheet":"Whitstable House","index":21,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[[7,0,12,0],[18,0,20,0],[22,0,23,0],[28,0,29,0],[52,0,52,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[2,6,5,6]]}
[]
[null,null,null,null,null,null,null,"Location","Communal open space at Whitstable House"]
[null,null,"Units","Method Detection Limit","GSC (human health residential scenario)","NBC","London Background (range min - max)","Sample identification","GTCS 1-27\nGTCS 1-28"]
[null,null,null,null,null,null,null,"Date","2019-06-05T18:20:00"]
[null,null,null,null,null,null,null,"Sample Type","Normal"]
[null,null,null,null,null,null,null,"Sample_Depth_Range","0-0.05"]
["Metals"]
[null,"Arsenic","mg/kg",0.5,"37#6",null,"1.2 - 160.90#9",null,"N/A"]
[null,"Barium","mg/kg",1,"460#7",null,"143.50 - 3475.10#9",null,"N/A"]
[null,"Beryllium","mg/kg",0.5,"1.7#2",null,null,null,"N/A"]
[null,"Cadmium","mg/kg",0.1,"22#6","2.1#8","0.00 - 165.20#9",null,"N/A"]
[null,"Lead","mg/kg",5,"200#6","820#8","10.8 - 10,000#9",null,"439"]
[null,"Zinc","mg/kg",5,"3,700#2",null,"0.00 - 10,095#9",null,"N/A"]
["VOCs"]
[null,"Chloromethane","ug/kg",3,"9.8#3",null,null,null,"N/A"]
["SVOCs"]
[null,"Dibenzo[a,e]pyrene","ug/kg",100,"42#1",null,null,null," - "]
["PAH"]
[null,"Benzo(a) pyrene","mg/kg",0.01,"2.7#2","3.6#8","0.332 - 6.976#10",null,"N/A"]
[null,"Benzo(b)fluoranthene","mg/kg",0.01,"3.3#2",null,"0.272 - 4.141#10",null,"N/A"]
[null,"Dibenz(a,h)anthracene","mg/kg",0.01,"0.28#2",null,"0.033 - 0.843#10",null,"N/A"]
["PCB (Dutch 7) congeners"]
[null,"PCB 118","ug/kg",5,"120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Total PCB 7 Congeners","ug/kg",35,"200#5",null,"0.1 - 114.1#10",null,"N/A"]
["PCB (WHO12) 12 congeners"]
[null,"Pentachlorobiphenyl, 2,3',4,4',5- (PCB-118)","ug/kg","Various","120#1",null,"0.1 - 76.5#10",null,"N/A"]
[null,"Pentachlorobiphenyl, 3,3,4,4,5- (PCB 126)","ug/kg",5,"0.036#1",null,"0.0002 - 0.156#11",null,"N/A"]
["ESdat Calculated"]
[null,"Cresols Total","ug/kg",20,"180#3",null,null,null,"N/A"]
[null,"Benzo(a)pyrene (surrogate marker for PAH mixture)","mg/kg",0.01,"5.0#6",null,null,null,"N/A"]
["AECOM Calculated"]
[null,"Sum of PCDD/F +PCB12","ng/kg","Various","8700#4",null,null,null,"N/A"]
[]
["Comments"]
["#1  USEPA RSL (May 2019)"]
["#2  LQM/CIEH S4ULs 2015"]
["#3  EIC/AGS/CL:AIRE 2010"]
["#4  EA SGV 2009"]
["#5  Dutch IV 2013"]
["#6  Defra C4SL 2014"]
["#7  AECOM (modified EIC GAC to include plant uptake route)"]
["#8  Johnson et al. 2012"]
["#9  London Earth"]
["#10  Vane"]
["#11  UKSHS"]
["GSC: Generic Screening Criteria"]
["(blank): No assessment criteria available"]
[" - : Not analysed"]
["N/A result was not above GSC"]
["* highest of two alternative values (obtained through different laboratory methods on same sample)"]
["Field_D: Field Duplicate"]
["HH: Human Health"]
["NAD: No Asbestos Detected"]
["Exceedance of HH Soil. Residential with Plant Uptake.  Sandy Loam.  TOC >=1.45 to <3.48%"]