|  |
| --- |
| Sprinkler Head Types |
| Sprinkler head - HI-FOG 1000 | HI-FOG 1000  | No action required  |
| Sprinkler head - HI-FOG 1900Single groove | HI-FOG 1900  | Action required |
| Sprinkler head - HI-FOG 2000 | HI-FOG 2000 | No action required This type should not be used in A1000 Assembly Body |
| Sprinkler head - HI-FOG 3000 | HI-FOG 3000  | No action required This type should not be used in A1000 Assembly Body |
| Assembly Body Types |
| Assembly body - A1000 | A1000 | Action requiredCover Plate over Assembly Body surface, held by the sprinkler - HI-FOG 1000 \ 1900 only |
| Assembly body - A1000 | A1000 | Action requiredCover Plate over Assembly Body surface, held by the sprinkler - HI-FOG 1000 \ 1900 only |
| Assembly body - A2000 | A2000 | No action requiredCover Plate over Assembly Body surface, held by the sprinkler – HI-FOG 2000 only |
| Assembly body - A2000 | A2000 | No action requiredCover Plate over Assembly Body surface, held by the sprinkler – HI-FOG 2000 only |
| Assembly body AB part 1Assembly body - AB part2Assembly body - AB part3 | AB | No action requiredClip Ring holds cover plate to the Assembly Body Optional Adaptor Ring to close gap between sprinkler and cover plate - multiple sprinkler types |
| Assembly body - C part1Assembly body - C part2 | C | No action requiredNarrow gap between cover plate and Assembly Body, plate snapped to the Assembly Body - multiple sprinkler types |