|  |  |  |
| --- | --- | --- |
| Sprinkler Head Types | | |
| Sprinkler head - HI-FOG 1000 | HI-FOG 1000 | No action required |
| Sprinkler head - HI-FOG 1900  Single groove | HI-FOG 1900 | Action required |
| Sprinkler head - HI-FOG 2000 | HI-FOG 2000 | No action required  This type should not be used in A1000 Assembly Body |
| Sprinkler head - HI-FOG 3000 | HI-FOG 3000 | No action required  This type should not be used in A1000 Assembly Body |
| Assembly Body Types | | |
| Assembly body - A1000 | A1000 | Action required  Cover Plate over Assembly Body surface, held by the sprinkler - HI-FOG 1000 \ 1900 only |
| Assembly body - A1000 | A1000 | Action required  Cover Plate over Assembly Body surface, held by the sprinkler - HI-FOG 1000 \ 1900 only |
| Assembly body - A2000 | A2000 | No action required  Cover Plate over Assembly Body surface, held by the sprinkler – HI-FOG 2000 only |
| Assembly body - A2000 | A2000 | No action required  Cover Plate over Assembly Body surface, held by the sprinkler – HI-FOG 2000 only |
| Assembly body AB part 1  Assembly body - AB part2  Assembly body - AB part3 | AB | No action required  Clip Ring holds cover plate to the Assembly Body  Optional Adaptor Ring to close gap between sprinkler and cover plate - multiple sprinkler types |
| Assembly body - C part1  Assembly body - C part2 | C | No action required  Narrow gap between cover plate and Assembly Body, plate snapped to the Assembly Body - multiple sprinkler types |