{"text_format":"1","workbook":"xlsx","n_sheets":14,"sheets":["Title and instructions","Secondary SoA","curriculum analysis (optional)","Existing Spaces","(Manual) ADS Template","(Manual) FFELib","(Manual) GenLib","(Manual) NotesLib","Individual Spaces","Project SoA","Prog Assums","Data Library","ADS Template","LOCK WORKBOOK"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":91,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Title and instructions","index":0,"n_rows":158,"n_cols":6,"rows_kept":158,"cut":false,"hidden":false,"merged":[]}
[]
[null,null,"Feasibility Study Appendix:"]
[null,null,"Schedule of Accommodation\n(SoA) tool (Secondary) version 8.3"]
[null,null,"December 2023"]
[]
[null,"DOCUMENT CONTROL"]
[]
[null,"Tool\nVersion","Amendments","Status","Date","Author"]
[null,7.4,"Area Data summary worksheets, Contractors ADS codes, ADS templates and FF&E library removed. Updated versions of these sheets now in SS1 School-specific SoA and ADS template v7.4.","n/a","2019-05-02","BWI"]
[null,8.1,"Version 7.4 revised to use new Uniclass names and codes and to incorporate changes to Annex 1A and 1B for the 2021 Output Specification. Rationalisation of some furnished space types, including food room and workshop 1 of 2.","n/a","2021-04-19","BWI"]
[null,"8.2\n(P01)","Amended to be accessible. Revised ADS codes to match SS1 of the 2021 Output Specification, as well as other corrections including all spaces listed on Individual spaces worksheet, updated curriculum models used to identify number of spaces. Additional plant room options added.","S2","2022-03-31","BWI"]
[null,"8.3\n(C01)","Plant spaces amended and number of blocks added. Additional rows added to allow for faith rooms, exams office and ablutions rooms if needed. Net capacity amended to match 2023 method. Other minor amendments including cell colours.","A","2023-12-15","BWI"]
[]
[null,"School-Specific Document "]
[null,"[Insert Project Code and Scheme Name here in title sheet]"]
[null,"Revision","Amendments","Status","Date","Author"]
[null,"P01","Employer's Representative to add amendments made to document (SoA tool Version: 8.3) here and rename file to make project specific.","S2","YYYY-MM-DD","ABC"]
[]
[]
[]
[null,"Contents"]
[null,"Worksheet","Description"]
[null,"Title and Instructions","Sheet sets out information about this resource information about the file (name, revision, status, document owner, document originator and revision history) and list of contents including descriptions. As well as instructions on how to use the document. "]
[null,"Secondary SoA","Tool create School-Specific Schedule of Accommodation (SoA) based on age range and number of pupil places - Tool Version 8.3"]
[null,"Existing Spaces","Sheet for identifying and recording all existing spaces in existing school buildings"]
[null,"Individual Spaces","Macro-created list of each individual space in the Secondary SoA"]
[null,"Project SoA","School-Specific Project Schedule of Accommodation (SoA) based on Individual spaces within the Works"]
[null,"Prog Assums","Sheet used for document calculations including drop-down lists"]
[null,"Data Library","Sheet used for document calculations, with data matching SS1"]
[]
[null,"Summary"]
[null,"This document is a tool to create a Schedule of Accommodation (SoA) for any secondary school, and a Project SoA for a related project"]
[null,"Review Date","Review dates for this document will be at 6-month intervals. "]
[null,"Who is this publication for?","This document is for technical professionals involved in the design and construction of school premises, to inform a School-specific Project SoA as part of the Employer’s Requirements of the DfE Construction Framework. It may also be used as the basis of similar documentation for other procurement routes."]
[null,"Uniclass Codes","This document captures Uniclass codes for the management of exchange of information. To access all codes and associated titles reference should be made to Refer to Uniclass | NBS (thenbs.com) for a description of Uniclass codes."]
[]
[null,"Notes"]
[null,"001","The Secondary SoA worksheet in this tool will create a Schedule of Accommodation (SoA) for any mainstream Secondary school that recommends the number type and size of spaces based on typical curriculum requirements, within the area ranges specified in BB103. Various adjustments can be made, using drop-down lists in any white cell, to suit the individual requirements of the school, as long as the total area of each category and the net capacity (in cell V5) are within the minimum and maximum range shown. The original recommendations remain unchanged in columns AI and AK."]
[null,"002","As set out in the instructions, the further worksheets offer options to list and check the existing spaces and to create a list of every individual space in the school. This can then be used to identify a Project SoA of all spaces in any project for new build, remodelling or refurbishment. This Project SoA can then be migrated to the School-specific SoA and ADS template in the Output Specification to provide the Employers Requirements for a projects, including Area Data Sheets."]
[null,"003","Use rows 17 to 21 to insert the name of the project and start a version log. More rows can be inserted below if needed."]
[null,"004","Where the school is to retain existing buildings, the appropriate designation should be chosen in cell AG8 and either:\n- use the minimum recommended sizes for new build projects, with the net and gross area at the minimum, and note the difference between this and the actual size of spaces, which may be smaller or larger (e.g. in column DV); or\n- match the sizes of the existing spaces in the SoA to their actual size, and note that the net and gross areas will be between the minimum and maximum recommended."]
[null,"005","This Secondary SoA tool will recommend possible areas for supplementary area where additionally resourced places for special educational needs (SEN) are identified, assuming that the SEN pupils will be taught in a specially resourced provision (SRP) or provide additional pupil places in a unit within the school. These recommendations are indicative, based on BB104."]
[null,"006","For all-age schools use two separate SoA tools, (the Secondary SoA and the Primary SoA) for the respective component parts of the school."]
[null,"007","The Technical Advisor should input the Scheme specific name into the Document Table (e.g., SRP1001-SchoolName) in cell B18. Subsequent Revisions to this template by the Employer’s Representative and Contractor should be recorded within the revisions table and follow the incremental revisioning as defined within National Annex of BS EN ISO 19650-2. "]
[]
[null,"Instructions"]
[null,null,"These instructions are colour coded to match the worksheet tabs in both this SoA tool and the SoA and ADS template, and cover the following steps:"]
[null,null,"This SoA tool covers items 1 to 4 from the red Secondary SoA to the green Project Brief. The SoA template in Annexe SS1 of School-Specific Brief covers the items 4 to 6."]
[null,"1.","Whether or not the options below are used, the first task is to Create the school specific SoA. "]
[null,"2.","Where several spaces or buildings are to be retained, the Existing Spaces and Secondary SoA worksheets can be used to Compare Existing Spaces"]
[null,"3.","Once the SoA has been finalised, the macro in the Individual Spaces worksheet can be used to Create the schedule of individual spaces "]
[null,"4.","If this version of the SoA is used as a contract document, the next 4 worksheets can be used to Create the Project SoA and Area Data summary worksheets, for architectural and M&E requirements as well as fittings, furniture and equipment (FF&E)."]
[null,"5.","The worksheets and the Contractors ADS codes in the School-specific SoA and ADS template offer the opportunity for the Contractor to complete SoA (at ITT and CP stages)"]
[null,"6.","If individual Area Data Sheets (ADSs) are required, the ADS template in the School-specific SoA and ADS can be used. This tool then has macros, with buttons on the top right of this sheet, to create ADSs for each space on the Project SoA. "]
[null,null,"The final 2 worksheets provide Programme Assumptions (including all drop down lists) and a data library of all generic requirements for all relevant space types. Like this title and instruction sheet, they are locked and for reference only."]
[]
[null,"1. Create the school specific SoA"]
[null,null,"The Secondary SoA worksheet will automatically list a typical ‘best practice’ set of teaching spaces, and their support spaces, based on the inserted number of places, age range, curriculum model and any supplementary SEN places. This can be adjusted to best suit the school's needs with various drop-down lists in column AG."]
[null,1.1000000000000001,"Create an initial SoA based on the age and number of pupil places.  In the ‘Secondary SoA’ worksheet:"]
[null,"1.1.1","Ensure the age range is correct. If the age range is not 11-16 or 11-18, fill in the ‘age range’ box by selecting from the drop-down menu (row 2, column K). "]
[null,"1.1.2","Identify pupil places. Fill in the number of pupil places per age range (rows 5 and 6, column K) to be accommodated (not the number on roll)."]
[null,null,"Column O, rows 5 and 6 are updated automatically; row 8, column K is updated automatically."]
[null,"1.1.3","Select the type of any additionally resourced SEN provision from the drop-down menu in row 12, column D, before filling in the number of additionally resourced SEN places (row 12, column K).\n\n"]
[null,null,"An indicative 'Supplementary Area' for any additionally resourced SEN places will be automatically allocated in column Y, under the related headings. If an SRP is chosen, the places are deemed to be included in the 'Total Mainstream Places', so the total supplementary area will be smaller than if a unit is chosen, when the pupil places will be additional and those pupils will be more likely to spend most of their time in a home-base classroom in the unit. The recommended areas are based on the minimum recommended in BB104 and should be tested in relation to the specific provision planned by the school. "]
[null,"1.1.4","Type of site and buildings: Select the area and type of site (row 4, column AD and AG) from the drop-down menus provided. Check the number of storeys (row 6, column AG), and select a different number from the drop down list if appropriate."]
[null,null,"The area of the site and number of split sites can have a minor effect on the net capacity in some cases. Buildings on confined sites may need to be multi-storey and this may require more circulation area. This will be allowed for if more than 2-storeys is chosen under the number of storeys."]
[]
[null,1.2,"Choose the right options to suit some school-specific requirements.  In the ‘Secondary SoA’ tab:"]
[null,"1.2.1","Identify retained buildings. From the corresponding drop-down menu (row 8, column AG), select if any buildings are to be retained or refurbished."]
[null,null,"If the selection includes retained or refurbished buildings, 'white' cells (i.e. with no colour fill) will appear where information can be entered in relation to existing spaces to be incorporated in the new school. The options for space types in the drop-down lists in column D (see 1.3) will also include additional spaces that may be found in existing school buildings. See also the second of the 'Notes' above."]
[null,null,"If retained spaces are to be incorporated in this SoA for the whole school, pick from the drop down list above and, for each type of space:"]
[null,null,"In column O, select from the drop down menus provided and, in column AA (Area of Retained Spaces), enter the corresponding area. "]
[null,null,"When 'retained' or 'refurb'ed' is chosen in column O, the area in columns S and Y will automatically be shown in column AA. When 'some retained' is chosen (for instance where some stores are in existing buildings and other would need to be new), the appropriate area should be inserted into column AA manually. "]
[null,null,"When existing space types are chosen from the drop down lists in column D, column 0 will automatically identify the space as 'retained', although it may still be amended to 'refurb'ed'. "]
[null,null,"If the number of retained spaces is small, this simple approach may be sufficient to identify the existing spaces. If the number of retained or refurbished spaces is more complex, see '2. Compare Existing Spaces' below."]
[null,"1.2.2","Select the type of curriculum from the drop-down menus provided in row 12, column AG, which most closely matches that of the school."]
[null,null,"This amends the number of rooms slightly, within the same total number, so for instance an academic curriculum will have more classrooms and science spaces recommended while a vocational curriculum will have more extra design technology spaces. The exact differences can be seen in hidden columns DG to DJ."]
[null,"1.2.3","Select options for classrooms, hall, science, dining and reception office(s) from the drop-down menus provided in rows 19, 31, 67 and 111, column AG."]
[null,null,"The classroom options will recommend different ways of providing these spaces. The default option of all 'standard except post-16' will suit new schools using the Standard Spaces in the 2021 Output Specification, while the alternative options may be more suitable for schools with existing larger or smaller classrooms: 'some extensive' will allow around 25% of the classrooms to be 'extensive' (as described in BB103) to allow for a wider range of activities or groups, at the expense of area in large spaces such as dining, while 'some variable' option allows a wider range of group sizes within a typical year cohort, providing a few rooms for up to 26 and a few for up to 34."]
[null,null,"The hall option allows for halls with or without bleacher seating, although bleacher seating is recommended in any school over 900 places, and this will be amended automatically based on the number of places. The bleacher seating store and capacity of the hall are also effected."]
[null,null,"The science option will recommend different ways of providing these spaces, including 3 specialist labs (for chemistry, biology and physics), suitable for schools with large sixth forms, or science studios shared between 2 larger general labs."]
[null,null,"The dining options allow for a range of dining scenarios, based on all pupils dining, with around a third eating traditional hot meals in about 20 minutes and two-thirds eating cold or 'grab and go' meals in 10 to 15 minutes. If a separate dining area is chosen, this may typically serve hot meals and some cold, while others go elsewhere (such as the hall) unless the net area is above the minimum recommended, or the school is larger than about 1350 pupils. Choosing to dine in the main hall or having a split lunch can allow more space in smaller schools, and will generally suggest a larger sports hall (up to 4 courts)."]
[null,null,"The number of reception desks in the general office relates to the public face, off the main entrance and the option of second desk for pupil access. If there is a separate office for finance and pupil services, this desk is assumed to be associated with that office."]
[]
[null,1.3,"Adjust the types of spaces, if necessary, to suit further school-specific requirements. "]
[null,null,"The schedule of teaching and learning spaces recommended by the tool is based on best practice and educational advice and typical teaching practice, and this will generally suit the requirements of most schools. In some cases, there may be more unusual options required by the school, such as photography or engineering, that need to be accommodated with specialist facilities. In such cases, and where the school wish to continue to offer the course, the appropriate spaces can be chosen from the drop-down list in column D. Spaces should generally be the standard size pre-set in the SoA, unless existing spaces are to be retained."]
[null,"1.3.1","Use ’curriculum analysis (optional)' sheet to confirm numbers of spaces in exceptional circumstances."]
[null,null,"The general principle is that the spaces required in the SoA tool will be assumed (at least at feasibility stage) to be what is appropriate for a school of the chosen age range and number of places, with the curriculum model chosen and the minor adjustments above. In exceptional cases, such as a vocational curriculum or where this does not match what the school feels it requires, a curriculum analysis can be used to check the SoA. In these cases, the appropriate skills are required, for instance from a Design Advisor, to ensure a complete analysis is achieved."]
[null,null,"If used, under 'current timetable' at the top of this sheet, the school should provide the information on their existing timetable and numbers on roll. Ensure that the number of 'periods in cycle', row 8 column AK, is correct."]
[null,null,"These figures will automatically be transferred to the ’11-18 CA (future linked)’ table lower down in this sheet, provided that the activities above have been completed."]
[null,null,"Then, in the 'future timetable' table at the bottom of this sheet, the pupil numbers (numbers in cohort for each year, in row 4) can be amended to match the planned number of pupil places and any planned curriculum changes."]
[null,null,"If the number of pupil places in Y7 is amended, for instance if the school is enlarging, the 11-16 figures will automatically be updated, and the other year groups will be updated to match."]
[null,null,"Check that the utilisation (bottom right, column AP) is within the range of utilisation factors assumed for the age range (top right, columns AR and AT). If this is not the case, the number and size of groups should be adjusted, ensuring they can realistically be delivered."]
[null,null,"Where the curriculum analysis has been used, the total number of places (row 8, column K) should match the curriculum analysis figures automatically transferred from the ’11-18 CA (future linked)’ table in 'curriculum analysis (optional)' spreadsheet."]
[]
[null,1.4,"Checks and balances.  In the ‘Secondary SoA’ tab:"]
[null,null,"The 'white' cells in columns S and U can be used to adjust the provision as necessary, to suit specific aspects of the school's pedagogy where the recommendation in columns AI and AK do not provide the spaces required by the school."]
[null,null,"Skill and judgement is needed to make the necessary adjustments so that the resulting SoA satisfies the school’s curriculum requirements, but stays within the recommended ranges in Building Bulletin 103 and does not become too specific to one style of management or organisation. Many space types are standard, as required in the Output Specification or Building Bulletin 103, and should not be adjusted (such as interview room off entrance and MI room), while some are more flexible and can be adjusted to suit the schools needs."]
[null,null,"It is particularly important that:"]
[null,"1.4.1","the total number of spaces for each subject-type (such as general teaching, science or art) should be the same or similar (+ or - one) as those in column AK;"]
[null,"1.4.2","the net capacity (row 5, column V) should match the number of mainstream places planned;"]
[null,"1.4.3","the total area of each category of space (different coloured) should be within the minimum and maximum range;"]
[null,"1.4.4","the spaces in the SoA should be coordinated with the space uses described in the School-specific Brief (SSB)."]
[]
[null,"Where several spaces or buildings are to be retained:"]
[null,"2. Compare Existing Spaces"]
[null,null,"The Existing Spaces sheet, linked to columns to the right of column EY, allows the spaces in the existing school buildings to be compared with the SoA tool recommendation for a new build school, to see what spaces are needed or where refurbishment or new build can be considered."]
[null,null,"To use this element of the tool effectively, you will need a detailed schedule of the current accommodation. This may be from cleaners' schedules or recent asbestos surveys, but would ideally be from a net capacity assessment and/or an Asset Management Plan, along with existing plans. A walk around the school will help assist if things have changed or the schedule is somewhat out of date."]
[null,2.1,"List the existing spaces. In the Existing Spaces sheet: "]
[null,"2.1.1","In column B and C, list each block or building, using EFA or other codes, and a letter to identify whether they are:\nS: Selected as a block to be upgraded or replaced due to its condition (e.g. in SRP, a 'Target' or 'Additional' block)\nU: Untouched, so to be kept but not due to be upgraded \nX: To be demolished, where the condition is such that this is the only option. "]
[null,"2.1.2","In columns G to N, in rows 25 down, insert the room number, block (using the names in the list above, from a drop-down list if preferred) and name of each space, and its net and non-net area. The number in column F will be allocated automatically."]
[null,null,"The net, or usable, area of the building is described in Building Bulletin 103 and will include classrooms, halls, offices and stores. Non-net area includes circulation, toilets and plant area. In some spaces, there may be 'essential access' to other spaces, so the total area of the space will include net and non-net area. This may be measured or estimated as:\n85% (for instance in corridors wider than 2.5m where there is room for lockers etc. at one side);\n50% (for instance in a shared resource or reception area with essential circulation through them);\n15% ( for instance in halls or classrooms with single circulation route through them)."]
[null,"2.1.3","In columns P to U, in rows 25 down, insert a number or symbol (e.g. '1') to indicate which category of space the spaces falls into. This can only be one type of net area, but may include non-net area as well (as above)."]
[null,"2.1.4","Click on the macro button 'Insert Block refs' at the top of column E, and the block reference in column AB will be inserted automatically, based on the block chosen in column G."]
[null,"2.1.5","Check the total areas and numbers of spaces in rows 4 to 12. This can give a useful indication as to whether the existing overall area of each category of space is within the minimum and maximum range recommended in the Building Bulletin 103 for the size and age range of school."]
[null,"2.1.6","Click on the macro button 'Sort Table' at the top of columns Q to T, and the spaces listed will be sorted automatically, based on the choices in columns P to AB, so that spaces in Selected (or successful) blocks are listed first, then Untouched (or unsuccessful), then demolished, each in order of the six categories of space. This allows them to be more easily compared to the master Secondary SoA (see 2.2)."]
[null,"2.1.7","Finally, click on the macro button 'Transfer Table' at the top of columns U to AB, and the spaces listed will be automatically listed in columns to the right of column EY on the master Secondary SoA sheet, ready to be compared."]
[]
[null,2.2000000000000002,"Compare existing spaces to SoA. In the Secondary SoA sheet:"]
[null,"2.2.1","In columns to the right of column EY, the existing spaces will be listed. Rows 2 to 6 indicate the space name, coloured to match the chosen category of space. Rows 6 to 13 indicate the room number and block, coloured to match whether the block is selected, or successful (S), untouched, or unsuccessful (U), or to be demolished (X). Row 15 sets whether the space is to be kept (untouched) , refurbished or remodelled. Initially, these should default to 'kept'."]
[null,"2.2.2","In the relevant 'white' cells in the columns to the right of column EY, insert the net area of the space, as shown in row 11, where the space matches a space type listed in the net area of the SoA in column D. And/or insert the non-net area, as shown in row 12, where the space matches a space type listed in the non-net areas of the SoA in column D. The area will automatically be taken away from the figure in row 11 or 12."]
[null,"2.2.3","The key at the top of columns EK to ET shows the colours that each cell may become, when compared to the SoA area. Green is within the area range that is recommended, while amber shows the area is 'restrictive' which can be acceptable for existing spaces but will restrict the types of activities that can be accommodated. for the group size. Red indicates that the space is too small and may be better identified as a smaller type of space, such as group room. These options are shown in column AD in the Prog Assums sheet."]
[null,"2.2.4","The pink areas of columns ER to EU show the total number of the spaces listed as 'kept' in row 2. The yellow areas of columns DS to DV then show the differences between the columns totals in columns DY to EU and the number and size of space recommended in the SoA."]
[null,"2.2.5","At this stage, if all the spaces, including those due for demolition, are identified to be kept, this gives a useful first analysis of the existing spaces. If the current school is the same capacity as that recommended in the SoA, there should be a very similar set of spaces. If some existing spaces are different to those on the SoA, it may be that some adjustment of the SoA is necessary (as 1.3 above)."]
[null,null,"When all data has been entered some issues can be considered, comparing the recommended SoA with the school under consideration, and the spaces of any Selected (or successful) blocks. These include:"]
[null,null,"a) Are the spaces in the successful blocks unique or are they duplicated elsewhere in the school?"]
[null,null,"b) Are any spaces under or over provided throughout the school?"]
[null,null,"c) Are spaces of the correct size? Too large, so they could be divided to make additional room? Or, too small that may require amalgamation?"]
[null,null,"d) Are individual blocks or the school sized differently from that expected?"]
[]
[null,2.2999999999999998,"Identify work required to each space. In the Secondary SoA sheet:"]
[null,null,"If the project involves a range of spaces that may be new, remodelled or refurbished, columns DY to EU can be usefully used to identify the work required in each space. This can then be transferred to the Individual Spaces sheet. it can also identify the spaces that are to be provided new in a project when these do not include all the spaces recommended - for instance if a sports hall is recommended but would need to be in a later phase. "]
[null,"2.3.1","If using this feature, delete any spaces that are to be demolished from the columns to the right of EY. Then use the drop-down options in row 2 to identify the work for each space as 'keep', 'refurb' or 'remodel' (where internal walls are to be altered). Ensure all spaces have their area included against a space in the SoA. Those spaces identified as 'keep' will remain totalled in the pink columns ER to EU. Those identified as 'refurb' will be totalled in the pink columns EK to EN. Those identified as 'remodel' will not automatically be totalled in the blue columns EE to EH, as they are likely to be different sizes when remodelled. However, the total remodelled area is collated in row 214, so it can be used as a check in column EH."]
[null,"2.3.2","Identify the number and size of spaces to be provided in new build in columns DY to EB, matching the area in the SoA but remembering that this may not include all space recommended in the SoA (as discussed above). Similarly, identify the number and size of spaces to be provided in remodelled area in columns EE to EH, matching the area in the SoA The total area to be remodelled should then be similar to that in cell EH214 if the remodelled spaces have been identified in column to the right of EY."]
[null,"2.3.3","The spaces listed in columns DY to EN should include all spaces on the SoA that are to be included in the project. Those in columns ER to EU will be those existing and untouched. The difference in the number of spaces should then generally be zero in column DU. The area may vary when it is existing. "]
[]
[null,"Once the SoA has been finalised: "]
[null,"3. Create the schedule of individual spaces "]
[null,3.1,"Prepare schedule of spaces. In the Individual Spaces sheet:"]
[null,"3.1.1","Once the SoA has been agreed, press the 'Generate' button located in cell A1. This will automatically produce a schedule of individual spaces, allocating unique code/ reference numbers to each space, based on the SoA in the Secondary SoA sheet."]
[null,"3.1.2","Column I allows the users to allocate room names and information associated with the proposed space as a record.  These are retained with the proposed space when further iterations of the Secondary SoA are created. If a space is removed then the associated information will be lost with it. "]
[null,"3.1.3","The following number allocation will be applied to the spaces listed:"]
[null,null,"Basic teaching areas",1000]
[null,null,"Large Spaces",2000]
[null,null,"Learning Resource Areas",3000]
[null,null,"Staff and Administration Areas",4000]
[null,null,"Storage (teaching and non-teaching)",5000]
[null,null,"Non-net areas",6000]
[null,null,"Unallocated",7000]
[null,"3.1.4","Column O should show whether the space has been designated as New, Remodel, Refurbish or Keep (as existing). if so, the schedule can be filtered to list the spaces in this order, and those in the first 3 of these designations will usually be the spaces within the project. These can be transferred to the Project SoA. The remainder will be as existing. However if there is no designation these spaces will still be shown as long as they are included in the Secondary SoA. There may also be spaces listed at the bottom of the schedule that are 'unallocated' because they are not included in the Secondary SoA but are listed in the existing spaces columns. These should not include any major spaces, but may include small offices or stores additional to the needs of the SoA."]
[null,null,"Note that any space that is not listed on the SoA will be deemed 'unallocated' and will be listed at the end. To ensure that any existing space is listed on the Individual Spaces, check that it is listed on the SoA with a number of spaces more than zero and a recommended area, before pressing the 'Generate' button.\nAlso note the Individual Spaces sheets automatically provide columns for Contractors to insert areas and comments (in columns K to M), but these can be ignored or deleted as the Contractor should use the Project SoA to insert the proposed areas and other information."]
[]
[null,"If the School-specific SoA and ADS is to be used as a contract document (Annex SS1 of the SSB):"]
[null,"4. Create the Project SoA and migrate to the School-specific SoA and SoA"]
[null,null,"The Project SoA provides the Employers Requirement schedule of accommodation required within the project. It is then replicated in the arch, M&E and FF&E area data summaries on the School-specific SoA and ADS (Annex SS1 of the SSB). This worksheets should therefore be completed on this SoA tool before migrating to the School-specific SoA and ADS template."]
[null,null,"When complete, the Project SoA should list every space required to be refurbished, remodelled or providing in new build, with no extra rows. It should include all circulation and plant areas, not automatically listed in the Individual Spaces. Where more rows are required, more can be copied and pasted as necessary."]
[null,null,"Ensure that the Project SoA to be migrated does not include any rows not required (with blanks in column D or marked #REF!), but does include the breakdown of plant and circulation area (including the correct number of stairs and lifts), the area of partition walls and the total net and gross area of new build. Amend or delete these rows as necessary to match the requirements of the project, and add more totals if there is refurbishment or remodelling, in the Project SoA before migrating to the School-specific SoA and ADS template."]
[null,4.0999999999999996,"Continue to create and amend the area data summary worksheets in the School-specific SoA and ADS template"]

{"sheet":"Secondary SoA","index":1,"n_rows":220,"n_cols":654,"rows_kept":220,"cut":false,"hidden":false,"merged":[]}
[null,null,null,"SCHEDULE OF ACCOMMODATION FOR ANY MAINSTREAM SECONDARY SCHOOL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Version 8.3 November 2023",null,null,null,null,null,"Technical notes (not for printing)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NET CAPACITY ASSESSMENT CALCULATIONS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,42,43,44,45,46,47,48,49,50,51,52,53,54,55,56,57,58,59,60,61,62,63,64,65,66,67,68,69,70,71,72,73,74,75,76,77,78,79,80,81,82,83,84,85,86,87,88,89,90,91,92,93,94,95,96,97,98,99,100,101,102,103,104,105,106,107,108,109,110,111,112,113,114,115,116,117,118,119,120,121,122,123,124,125,126,127,128,129,130,131,132,133,134,135,136,137,138,139,140,141,142,143,144,145,146,147,148,149,150,151,152,153,154,155,156,157,158,159,160,161,162,163,164,165,166,167,168,169,170,171,172,173,174,175,176,177,178,179,180,181,182,183,184,185,186,187,188,189,190,191,192,193,194,195,196,197,198,199,200,201,202,203,204,205,206,207,208,209,210,211,212,213,214,215,216,217,218,219,220,221,222,223,224,225,226,227,228,229,230,231,232,233,234,235,236,237,238,239,240,241,242,243,244,245,246,247,248,249,250,251,252,253,254,255,256,257,258,259,260,261,262,263,264,265,266,267,268,269,270,271,272,273,274,275,276,277,278,279,280,281,282,283,284,285,286,287,288,289,290,291,292,293,294,295,296,297,298,299,300,301,302,303,304,305,306,307,308,309,310,311,312,313,314,315,316,317,318,319,320,321,322,323,324,325,326,327,328,329,330,331,332,333,334,335,336,337,338,339,340,341,342,343,344,345,346,347,348,349,350,351,352,353,354,355,356,357,358,359,360,361,362,363,364,365,366,367,368,369,370,371,372,373,374,375,376,377,378,379,380,381,382,383,384,385,386,387,388,389,390,391,392,393,394,395,396,397,398,399,400,401,402,403,404,405,406,407,408,409,410,411,412,413,414,415,416,417,418,419,420,421,422,423,424,425,426,427,428,429,430,431,432,433,434,435,436,437,438,439,440,441,442,443,444,445,446,447,448,449,450,451,452,453,454,455,456,457,458,459,460,461,462,463,464,465,466,467,468,469,470,471,472,473,474,475,476,477,478,479,480,481,482,483,484,485,486,487,488,489,490,491,492,493,494,495,496,497,498,499,500]
[null,null,null,null,null,null,null,null,null,"age range","11-18",null,null,null,null,null,null,"school name",{"$f":"'Title and instructions'!B15","v":"[Insert Project Code and Scheme Name here in title sheet]"},null,null,null,null,null,null,null,null,null,null,null,null,"date",null,null," as a check, if new:",null,null,null,null,null,null,null,null,null,null,null,"years","places","group size",null,"yr groups","places/ yr",null,null,"contractor name",null,null,null,null,null,null,null,null,null,"Optional SoA by suite: identifying which spaces are in each suite of spaces",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAXA(1,ROUNDDOWN(K5/150,0))","v":6},"FE  11-16",null,null,null,1,1,1,1,1,1,1,1,null,null,null,null,null,{"$f":"IF(SUM(DU17:DU67)=0,\"OK: proposed basic teaching spaces sufficient\",IF(COUNTIF(DU17:DU67,\">0\")>0,\"NOTE: overprovision in proposed basic teaching spaces\",\"NOTE: proposed basic teaching spaces insufficient\"))","v":"NOTE: proposed basic teaching spaces insufficient"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KEY to formatting of existing spaces cells:",null,null,null,null,null,null,null,null,null,null,null,null,null,"Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep","Keep"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(O6=2,IF(K6>0,\"\",\"check age range and places\"),IF(O6=0,IF(K6>0,\"check age range and places\",\"\")))","v":""},null,null,null,"years",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(SUM(DU69:DU72)=0,\"OK: proposed large spaces sufficient\",IF(COUNTIF(DU69:DU72,\">0\")>0,\"NOTE: overprovision in proposed large spaces\",\"NOTE: proposed large spaces insufficient\"))","v":"NOTE: proposed large spaces insufficient"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Below Minimum Possible Area"]
[null,null,6,"FE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"     2023 net capacity",null,null,null,null,null,null,"site:","sufficient",null,null,null,null,"no. of blocks:",2,null,null,"net capacity",null,null,null,"site",{"$f":"VLOOKUP(AA4,'Prog Assums'!B6:D14,3,FALSE)","v":"OK"},null,null,null,null,"KS2",{"$f":"VLOOKUP(K$2,'Prog Assums'!E$5:J$17,3,FALSE)","v":0},{"$f":"IF(K4>0,(K4/(AS5+AS6+AY4))*AY4,0)","v":0},{"$f":"IF(AV4>0,ROUND(AZ4/ROUNDUP(AZ4/30,0),1),0)","v":0},{"$f":"IF(AV4>0,ROUND(AZ4/ROUNDUP(AZ4/30,0),1),0)","v":0},{"$f":"VLOOKUP(K2,'Prog Assums'!E6:K17,3,FALSE)","v":0},{"$f":"AV4/AY4","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,"Design SoA",null,null,null,null,null,null,null,{"$f":"BO15","v":"Mathematics"},null,{"$f":"BQ15","v":"English"},null,{"$f":"BS15","v":"MFL"},null,{"$f":"BU15","v":"Humanities"},null,{"$f":"BW15","v":"ICT and Business Studies"},null,{"$f":"BY15","v":"Science"},null,{"$f":"CA15","v":"DT/ Art"},null,{"$f":"CC15","v":"Perf arts, hall and dining"},null,{"$f":"CE15","v":"Sports/ PE"},null,{"$f":"CG15","v":"Admin"},null,{"$f":"CI15","v":"-"},null,{"$f":"CK15","v":"Balance"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAXA(1,ROUNDDOWN(K8/150,0))","v":7},"FE  total",null,{"$f":"IF(K4>0,1,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(SUM(DU76:DU94)=0,\"OK: proposed learning resource spaces sufficient\",IF(COUNTIF(DU76:DU94,\">0\")>0,\"NOTE: overprovision in proposed learning resource spaces\",\"NOTE: proposed learning resource spaces insufficient\"))","v":"NOTE: proposed learning resource spaces insufficient"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Between Restric-tive and Minimum"]
[{"$f":"C$6*C$4*(AU5+AU6)","v":900},null,"classes of",null,null,null,null,null,null,"11 to 16 places",{"$f":"A5","v":900},null,null,null,{"$f":"AY5+AY6","v":5},null,null,null,null,null,"for SoA below = ",{"$f":"IF(K8<V8,IF(K8>S8,K8,S8),V8)","v":1125},null,null,{"$f":"IF(V5<K8,\"WARNING: under capacity\",IF(V5>K8+10,\"NOTE: over capacity\",\"\"))","v":""},null,null,null,null,null,null,null,null,null,"for recommended",null,null,null,null,"sites",{"$f":"VLOOKUP(AA4,'Prog Assums'!B6:D14,2,FALSE)","v":1},null,null,null,null,"KS3",{"$f":"VLOOKUP(K$2,'Prog Assums'!E$5:J$17,4,FALSE)","v":3},{"$f":"IF(K5>0,(K5/(AY5+AY6))*AY5,0)","v":540},{"$f":"IF(AV5>0,ROUND(AZ5/ROUNDUP(AZ5/27,0),1),0)","v":25.7},{"$f":"IF(AV5>0,ROUND(AZ5/ROUND(AZ5/20,0),1),0)","v":20},{"$f":"VLOOKUP(K2,'Prog Assums'!E6:K17,4,FALSE)","v":3},{"$f":"AV5/AY5","v":180},null,null,null,null,null,null,"based on SoA by individual",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"utilisation factor",{"$f":"VLOOKUP(K2,'Prog Assums'!E6:L17,8,FALSE)","v":0.71},null,"2023 NCA of SoA",null,null,null,"2023 NCA of recom'd SoA",null,null,null,null,null,{"$f":"IF(K5>0,1,0)","v":1},null,{"$f":"IF(K5>0,1,0)","v":1},{"$f":"IF(K5>0,1,0)","v":1},{"$f":"IF(K5>0,1,0)","v":1},{"$f":"IF(K5>0,1,0)","v":1},{"$f":"IF($K$6>0,1,0)","v":1},{"$f":"IF($K$6>0,1,0)","v":1},1,1,null,null,null,null,null,{"$f":"IF(SUM(DU104:DU129)=0,\"OK: proposed staff and admin spaces sufficient\",IF(COUNTIF(DU104:DU129,\">0\")>0,\"NOTE: overprovision in proposed staff and admin spaces\",\"NOTE: proposed staff and admin spaces insufficient\"))","v":"NOTE: proposed staff and admin spaces insufficient"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Restrictive"]
[{"$f":"ROUND(C$6*C$4*A8*AU8,0)","v":225},null,30,null,null,null,null,null,null,"16 to 19 places",{"$f":"A6","v":225},null,null,null,{"$f":"AY8","v":2},null,null,null,null,null,"within a potential range of:",null,null,null,null,null,null,null,null,null,null,"number of storeys:",{"$f":"IF(K8<601,\"2-storey\",\"3-storey\")","v":"3-storey"},null,"SoA below:",null,{"$f":"IF(K8<AK8,IF(K8>AI8,K8,AI8),AK8)","v":1125},null,null,"storeys",{"$f":"VLOOKUP(AG6,'Prog Assums'!B18:C24,2,FALSE)","v":3},null,null,null,null,"KS4",{"$f":"VLOOKUP(K$2,'Prog Assums'!E$5:J$17,5,FALSE)","v":2},{"$f":"IF(K5>0,(K5/(AY5+AY6))*AY6,0)","v":360},{"$f":"IF(AV6>0,ROUND(AZ6/ROUND(AZ6/24,0),1),0)","v":22.5},{"$f":"IF(AV6>0,ROUND(AZ6/ROUND(AZ6/20,0),1),0)","v":20},{"$f":"VLOOKUP(K2,'Prog Assums'!E6:K17,5,FALSE)","v":2},{"$f":"AV6/AY6","v":180},null,null,null,null,null,null,"space showing area of",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(K8>200,IF(K6>0,1,0),0)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(SUM(DU132:DU164)=0,\"OK: proposed storage spaces sufficient\",IF(COUNTIF(DV132:DV164,\">0\")>0,\"NOTE: overprovision in proposed storage spaces\",\"NOTE: proposed storage spaces insufficient\"))","v":"NOTE: proposed storage spaces insufficient"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OK"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GT"]
[{"$f":"IF(O6>0,62.5%,0)","v":0.625},null,null,null,null,null,null,null,null,"Total Mainstream Places",{"$f":"K5+K6","v":1125},null,null,null,null,null,null,null,{"$f":"CV10","v":1093},null,"to",{"$f":"CT10","v":1215},null,null,null,null,null,null,null,null,null,"existing buildings to be:","some retained",null,{"$f":"CZ10","v":1093},"to",{"$f":"CX10","v":1215},null,null,"buildings",{"$f":"VLOOKUP(AG8,'Prog Assums'!B28:C33,2,FALSE)","v":"extg"},null,null,null,null,"KS5",{"$f":"VLOOKUP(K$2,'Prog Assums'!E$5:J$17,6,FALSE)","v":2},{"$f":"K6","v":225},{"$f":"IF(AV8>0,ROUND(AZ8/ROUND(AZ8/18,0),1),0)","v":18.8},{"$f":"IF(AV8>0,ROUND(AZ8/ROUND(AZ8/12,0),1),0)","v":12.5},{"$f":"VLOOKUP(K2,'Prog Assums'!E6:K17,6,FALSE)","v":2},{"$f":"AV8/AY8","v":112.5},null,null,null,null,null,null,"each space as designed",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"area of sites",{"$f":"AO4","v":"OK"},null,"net capacity ",null,null,null,"net capacity ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Extensive",null,null,null,null,null,null,null,null,null,null,null,"E.g. AA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"max",null,"min",null,"max",null,"min",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Above Maximum Possible Area",null,null,null,null,null,null,null,null,null,null,null,101]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AC168=\"OK\",AF166,AC168)","v":0},{"$f":"IF(AC168=\"OK\",\"float if rec'd net\",\"over rec'd net\")","v":"float if rec'd net"},null,null,null,{"$f":"IF(AC214=\"OK\",\"not\",AC214)","v":"not"},"over rec'd gross",null,"recommended",null,null,null,null,{"$f":"VLOOKUP(AG67,'Prog Assums'!B98:E103,2,FALSE)","v":"both"},null,null,null,null,null,null,null,null,"max percentage of curriculum that can be ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number of sites",{"$f":"AO5","v":1},null,{"$f":"MAXA(CT14,CU14)","v":1215},null,{"$f":"ROUNDDOWN(CT10*0.9,0)","v":1093},null,{"$f":"MAXA(CX14,CY14)","v":1215},null,{"$f":"ROUNDDOWN(CX10*0.9,0)","v":1093},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Block ref -","S"]
[null,null,null,"Additionally resourced places for:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"accommodated at frequency of use shown, ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Net Area -",{"$f":"56-SUM(INDIRECT(ADDRESS(ROW()+3, COLUMN())):INDIRECT(ADDRESS(ROW()+148, COLUMN())))","v":56}]
[null,null,null,"-",null,null,null,null,null,null,null,"SEN",null,null,null,null,{"$f":"IF(K8>1900,\"NOTE manual amendments needed for large schools\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"curriculum",null,null,"C: typical",null,null,null,null,null,null,{"$f":"IF(AO12=\"unit\",0,IF(AO12=\"SRP\",0,100))","v":100},{"$f":"IF(K14>0,VLOOKUP(D12,'Prog Assums'!B82:D94,3,FALSE),\"\")","v":0},null,null,null,null,null,null,null,"with average group size as listed to left",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"availability priority category","consequential unavailability ",null,null,"workplaces included",null,null,{"$f":"SUM(CU19:CU60)+SUM(CU64:CU67)+SUM(CU76:CU94)","v":1772},{"$f":"SUM(CU19:CU164)","v":1966},{"$f":"SUM(CV19:CV164)","v":397.5},{"$f":"IF(CR8=\"tight\",50)+(CR10*75)","v":75},{"$f":"SUM(CY19:CY60)+SUM(CY64:CY67)+SUM(CY76:CY94)","v":1772},{"$f":"SUM(CY19:CY164)","v":1966},{"$f":"SUM(CZ19:CZ164)","v":396},null,"recommended numbers",null,null,null,"11 to 16 spaces",null,null,null,"16 to 19 spaces",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Non Net Area -",{"$f":"-SUM(INDIRECT(ADDRESS(ROW()+151, COLUMN())):INDIRECT(ADDRESS(ROW()+170, COLUMN())))","v":0}]
[]
[null,null,null,null,null,null,null,null,null,"curriculum analysis data",{"$f":"IF('curriculum analysis (optional)'!AO73>0,\"linked\", \"manual\")","v":"manual"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"total x utilisation",null,null,{"$f":"ROUNDDOWN((CT12-60)*$CR5,0)","v":1215},{"$f":"ROUNDDOWN((CU12-$CW12)*0.7*$CR5,0)","v":939},null,null,{"$f":"ROUNDDOWN((CX12-60)*$CR5,0)","v":1215},{"$f":"ROUNDDOWN((CY12-$CW12)*0.7*$CR5,0)","v":939},null,null,"based on  'rule of thumb'",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Difference",null,null,null,null,null,"New Build Works",null,null,null,null,null,"Remodelling Works",null,null,null,null,null,"Refurbishment Works",null,null,null,null,null,null,"Keep (as existing)"]
["Parent ADS code",null,"Final ADS code","Space type",null,null,null,null,null,null,null,null,null,null,"existing or new (new if blank)",null,"max. group size",null,"average area of space (m2)",null,"TOTAL no. of spaces","TOTAL AREA (m2)","NON-NET AREA (m2) ",null,"SUPP AREA (m2)",null,"AREA OF RE-TAINED SPACES",null,null,null,null,null,null,null,"area of space (m2)",null,"no. of spaces (& total supp area)",null,null,"storage or prep req'd",null,"max group size","min for min group","max for max group","Total recom'd area (m2)","Total SEN area (m2)","space size code","likely average group size","max part of curriculum accommodated",null,null,null,null,null,"notes",null,"average area of space (m2)",null,"TOTAL no. of spaces","TOTAL AREA (incl supp)",null,"Area differ-ence","no. of spaces differ-ence",null,"Total",null,"Mathematics",null,"English",null,"MFL",null,"Humanities",null,"ICT and Business Studies",null,"Science",null,"DT/ Art",null,"Perf arts, hall and dining",null,"Sports/ PE",null,"Admin",null,{"$f":"D12","v":"-"},null,"Balance",null,null,null,null,null,"formula per work place","formula to be sub-tracted","work places per room","basic work places per room","total basic work places","total re-source work places","basic work place allow-ance","basic work places per room","total basic work places","total re-source work places","max group size","area","4 to 10 spaces","11 to 16 spaces","sixth form spaces",{"$f":"'Prog Assums'!B45","v":"A: vocational"},{"$f":"'Prog Assums'!B46","v":"B: music/ sports"},{"$f":"'Prog Assums'!B47","v":"C: typical"},{"$f":"'Prog Assums'!B48","v":"D: academic"},{"$f":"'Prog Assums'!B45","v":"A: vocational"},{"$f":"'Prog Assums'!B46","v":"B: music/ sports"},{"$f":"'Prog Assums'!B47","v":"C: typical"},{"$f":"'Prog Assums'!B48","v":"D: academic"},{"$f":"'Prog Assums'!AE4","v":"min possible area"},{"$f":"'Prog Assums'!AF4","v":"Min rec'd Area if restrictive (or 10%)"},{"$f":"'Prog Assums'!AG4","v":"Min rec'd Area if standard"},{"$f":"'Prog Assums'!AH4","v":"Min rec'd Area if extensive"},{"$f":"'Prog Assums'!AI4","v":"max possible area"},"average area of space (m2)",null,"TOTAL no. of spaces","TOTAL AREA  (m2)",null,null,"average area of space (m2)",null,"TOTAL no. of spaces","TOTAL AREA  (m2)",null,null,"average area of space (m2)",null,"TOTAL no. of spaces","TOTAL AREA  (m2)",null,null,"average area of space (m2)",null,"TOTAL no. of spaces","TOTAL AREA  (m2)",null,null,null,"average area of space (m2)",null,"TOTAL no. of spaces","TOTAL AREA  (m2)",null,null,null,"classroom"]
[]
[null,null,null,"Basic Teaching Area",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"area"]
[null,null,null,"General teaching spaces",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AW19+AW26+AW31+AW38+AW43+AW49+AW58","v":1.0167961904761906},"of curriculum indoors",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"DC20+DC21","v":0},{"$f":"HLOOKUP($AG$12,$DF$15:$DI$74,4,FALSE)","v":24},{"$f":"HLOOKUP($AG$12,$DJ$15:$DM$74,4,FALSE)","v":6},{"$f":"ROUNDUP(($K$5*3.5/150),0)","v":21},{"$f":"ROUNDUP(($K$5*4/150)-DG5,0)","v":23},{"$f":"ROUNDUP(($K$5*4/150),0)","v":24},{"$f":"ROUNDUP(($K$5*4/150)+DI5,0)","v":25},{"$f":"ROUNDUP(($K$6*3.5/150),0)","v":6},{"$f":"ROUNDUP(($K$6*4/150),0)","v":6},{"$f":"ROUNDUP(($K$6*4/150),0)","v":6},{"$f":"ROUNDUP(($K$6*4/150)+DM5,0)","v":7}]
[null,null,null,"Classrooms",null,null,null,null,null,null,{"$f":"'curriculum analysis (optional)'!AO110","v":0},null,null,null,null,null,null,null,null,null,{"$f":"U20+U21+U22+U23+U24","v":30},null,null,null,null,null,null,null,"classroom options",null,null,null,"all standard except post-16",null,null,null,{"$f":"AK20+AK21+AK22+AK23+AK24","v":30},null,null,null,null,null,null,null,null,null,null,{"$f":"((AW$4*AY$4)+(AV$5/AY$5/DA$2)+(AW$5*(AY$5-1))+(AW$6*AY$6)+(AW$8*AY$8))/(AY$4+AY$5+AY$6+AY$8)","v":23.428571428571427},{"$f":"(U19*AV19*0.9)/K$8","v":0.56228571428571428},"of curriculum @ 90% use",null,null,null,null,null,null,null,null,{"$f":"BG20+BG21+BG22+BG24","v":30},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(EA19,EG19,EM19,ET19)-U19","v":-30},null,null,null,null,null,{"$f":"SUM(EA20:EA24)","v":0},{"$f":"SUM(EB20:EB24)","v":0},null,null,null,null,{"$f":"SUM(EG20:EG24)","v":0},{"$f":"SUM(EH20:EH24)","v":0},null,null,null,null,{"$f":"SUM(EM20:EM24)","v":0},{"$f":"SUM(EN20:EN24)","v":0},null,null,null,null,null,{"$f":"SUM(ET20:ET24)","v":0},{"$f":"SUM(EU20:EU24)","v":0}]
[{"$f":"VLOOKUP($D20,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"CLA02"},null,{"$f":"VLOOKUP($D20,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"CLA02"},"Seminar rooms",null,null,null,null,null,null,null,null,{"$f":"IF(D20=\"\",\"\",_xlfn.XLOOKUP(D20,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Seminar room"},{"$f":"CONCATENATE(M20,S20)","v":"Seminar room41"},null,null,{"$f":"IF(S20>0,ROUND((S20-VLOOKUP(AU20,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU20,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":22},null,{"$f":"VLOOKUP(D20,'Prog Assums'!N$5:U$271,5,FALSE)","v":41},null,{"$f":"AK20","v":3},{"$f":"MAXA(0,(S20*U20)-Y20)","v":123},null,null,null,null,{"$f":"IF(O20=\"retained\",V20+Y20,IF(O20=\"refurb'ed\",V20+Y20,0))","v":0},null,{"$f":"IF(D20=\"-\",0,VLOOKUP(D20,'Prog Assums'!N$5:X$271,11,FALSE))","v":41},{"$f":"IF(D20=\"-\",\"\",\"m2 minimum size for 30 pupils\")","v":"m2 minimum size for 30 pupils"},null,null,null,null,{"$f":"IF(AK20>0,41,0)","v":41},null,{"$f":"DD20+DE20+DC20","v":3},null,null,{"$f":"IF(U20>0,VLOOKUP(D20,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":1},{"$f":"IF(O20=\"existing\",\"E\",\"\")","v":""},22,{"$f":"VLOOKUP(D20,'Prog Assums'!N$5:U$271,5,FALSE)","v":41},{"$f":"ROUNDUP(VLOOKUP(AU20,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP20*VLOOKUP(AU20,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":47},{"$f":"MAXA((AI20*AK20)-AT20,0)","v":123},null,"C",null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N20,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N20,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N20)","v":3},{"$f":"IF(ISERROR(BE20*BG20)=TRUE,\"\",BE20*BG20)","v":""},null,{"$f":"IF(ISERROR(BH20-Y20-V20)=TRUE,\"\",BH20-Y20-V20)","v":""},{"$f":"BG20-U20","v":0},null,{"$f":"SUM(BO20:CK20)","v":3},null,{"$f":"ROUNDUP($U20/3,0)","v":1},null,{"$f":"ROUNDUP($U20/3,0)","v":1},null,{"$f":"ROUND($U$20/3,0)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S20>0,VLOOKUP($D20,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"41m2 for 22"},{"$f":"IF($S20>0,VLOOKUP($D20,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"B"},null,null,{"$f":"IF(S20>90,2.5,1.5)","v":1.5},{"$f":"IF(S20>90,-20,4)","v":4},{"$f":"IF(U20=0,0,MAXA(1,ROUNDUP((S20/CQ20)-CR20,0)))","v":24},{"$f":"IF(CS20>14,IF(CS20<31,CS20,ROUNDDOWN(CS20/30,0)*30),0)","v":24},{"$f":"IF(S20>0,(V20/S20)*CT20,0)","v":72},{"$f":"IF(CS20>0,(V20/S20)*CS20,0)-CU20","v":0},{"$f":"IF(AK20=0,0,MAXA(1,ROUNDUP((AI20/CQ20)-CR20,0)))","v":24},{"$f":"IF(CW20>14,IF(CW20<31,CW20,ROUNDDOWN(CW20/30,0)*30),0)","v":24},{"$f":"IF(AK20>0,(AS20/AI20)*CX20,0)","v":72},{"$f":"IF(CW20>0,(AS20/AI20)*CW20,0)-CY20","v":0},20,null,null,null,{"$f":"ROUNDDOWN(DE18/2,0)","v":3},null,null,null,null,{"$f":"ROUNDDOWN(DJ18/2,0)","v":3},{"$f":"ROUNDDOWN(DK18/2,0)","v":3},3,3,{"$f":"VLOOKUP($C20,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":25},{"$f":"VLOOKUP($C20,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":36.9},{"$f":"IF(VLOOKUP($C20,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI20,VLOOKUP($C20,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":41},{"$f":"VLOOKUP($C20,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":46.8},{"$f":"VLOOKUP($C20,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":50},{"$f":"IF(ISERROR((SUM($EB20,$EH20,$EN20,$EU20)/SUM($EA20,$EG20,$EM20,$ET20)-$S20))=TRUE,0,IF($U20=0,0,(SUM($EB20,$EH20,$EN20,$EU20)/SUM($EA20,$EG20,$EM20,$ET20)-$S20)))","v":0},null,-3,{"$f":"SUM($EU20,$EN20,$EH20,$EB20)-$V20-$Y20","v":-123},null,null,0,null,null,{"$f":"EA20*DY20","v":0},null,null,0,null,0,{"$f":"EG20*EE20","v":0},null,null,{"$f":"IF(EN20>0,SUM(EN20/EM20),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY20:$YD20,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY20:$YD20)","v":0},null,null,null,{"$f":"IF(EU20>0,SUM(EU20/ET20),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY20:$YD20,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY20:$YD20)","v":0}]
[{"$f":"VLOOKUP($D21,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"CLA12"},null,{"$f":"VLOOKUP($D21,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"CLA12"},"Classrooms (general)",null,null,null,null,null,null,null,null,{"$f":"IF(D21=\"\",\"\",_xlfn.XLOOKUP(D21,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Classrooms (general)"},{"$f":"CONCATENATE(M21,S21)","v":"Classrooms (general)55"},null,null,{"$f":"IF(S21>0,ROUND((S21-VLOOKUP(AU21,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU21,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":30},null,{"$f":"VLOOKUP(D21,'Prog Assums'!N$5:U$271,5,FALSE)","v":55},null,{"$f":"AK21","v":27},{"$f":"MAXA(0,(S21*U21)-Y21)","v":1485},null,null,null,null,{"$f":"IF(O21=\"retained\",V21+Y21,IF(O21=\"refurb'ed\",V21+Y21,0))","v":0},null,{"$f":"IF(D21=\"-\",0,VLOOKUP(D21,'Prog Assums'!N$5:X$271,11,FALSE))","v":55},"m2 minimum size for 30 pupils",null,null,null,null,{"$f":"IF(AK21>0,55,0)","v":55},null,{"$f":"DD21+DE21+DC21-AK22-AK23","v":27},null,null,{"$f":"IF(U21>0,VLOOKUP(D21,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":1},{"$f":"IF(O21=\"existing\",\"E\",\"\")","v":""},30,{"$f":"VLOOKUP(D21,'Prog Assums'!N$5:U$271,5,FALSE)","v":55},{"$f":"ROUNDUP(VLOOKUP(AU21,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP21*VLOOKUP(AU21,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":62},{"$f":"MAXA((AI21*AK21)-AT21,0)","v":1485},null,"C",null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N21,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N21,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N21)","v":27},{"$f":"IF(ISERROR(BE21*BG21)=TRUE,\"\",BE21*BG21)","v":""},null,{"$f":"IF(ISERROR(BH21-Y21-V21)=TRUE,\"\",BH21-Y21-V21)","v":""},0,null,{"$f":"SUM(BO21:CK21)","v":27},null,{"$f":"ROUND(K8/150,0)+1-BO20","v":8},null,{"$f":"ROUND(K8/150,0)+1-BQ20","v":8},null,{"$f":"ROUNDDOWN((U19-BO21-BQ21)/2,0)-BS20","v":6},null,{"$f":"MAXA(0,U21-BO21-BQ21-BS21)","v":5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S21>0,VLOOKUP($D21,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"55m2 for 30"},{"$f":"IF($S21>0,VLOOKUP($D21,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"B"},null,null,{"$f":"IF(S21>90,2.5,1.5)","v":1.5},{"$f":"IF(S21>90,-20,4)","v":4},{"$f":"IF(U21=0,0,MAXA(1,ROUNDUP((S21/CQ21)-CR21,0)))","v":33},{"$f":"IF(CS21>14,IF(CS21<31,CS21,ROUNDDOWN(CS21/30,0)*30),0)","v":30},{"$f":"IF(S21>0,(V21/S21)*CT21,0)","v":810},{"$f":"IF(CS21>0,(V21/S21)*CS21,0)-CU21","v":81},{"$f":"IF(AK21=0,0,MAXA(1,ROUNDUP((AI21/CQ21)-CR21,0)))","v":33},{"$f":"IF(CW21>14,IF(CW21<31,CW21,ROUNDDOWN(CW21/30,0)*30),0)","v":30},{"$f":"IF(AK21>0,(AS21/AI21)*CX21,0)","v":810},{"$f":"IF(CW21>0,(AS21/AI21)*CW21,0)-CY21","v":81},30,null,null,{"$f":"DD18","v":24},{"$f":"DE18-DE20","v":3},{"$f":"DF18","v":21},{"$f":"DG18","v":23},24,25,{"$f":"DJ18-DJ20","v":3},{"$f":"DK18-DK20","v":3},3,4,{"$f":"VLOOKUP($C21,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":25},{"$f":"VLOOKUP($C21,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":49.5},{"$f":"IF(VLOOKUP($C21,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI21,VLOOKUP($C21,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":55},{"$f":"VLOOKUP($C21,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":62},{"$f":"VLOOKUP($C21,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":95},{"$f":"IF(ISERROR((SUM($EB21,$EH21,$EN21,$EU21)/SUM($EA21,$EG21,$EM21,$ET21)-$S21))=TRUE,0,IF($U21=0,0,(SUM($EB21,$EH21,$EN21,$EU21)/SUM($EA21,$EG21,$EM21,$ET21)-$S21)))","v":0},null,-27,{"$f":"SUM($EU21,$EN21,$EH21,$EB21)-$V21-$Y21","v":-1485},null,null,0,null,null,{"$f":"EA21*DY21","v":0},null,null,0,null,null,{"$f":"EG21*EE21","v":0},null,null,{"$f":"IF(EN21>0,SUM(EN21/EM21),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY21:$YD21,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY21:$YD21)","v":0},null,null,null,{"$f":"IF(EU21>0,SUM(EU21/ET21),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY21:$YD21,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY21:$YD21)","v":0}]
[{"$f":"VLOOKUP($D22,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D22,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},{"$f":"IF(AG19=\"some extensive\",\"Classrooms (extensive)\",IF(AG19=\"some variable\",\"Classrooms (larger group)\",\"-\"))","v":"-"},null,null,null,null,null,null,null,null,{"$f":"IF(D22=\"\",\"\",_xlfn.XLOOKUP(D22,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},{"$f":"CONCATENATE(M22,S22)","v":"-0"},{"$f":"IF(VLOOKUP(D22,'Prog Assums'!N$6:V$92,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S22>0,ROUND((S22-VLOOKUP(AU22,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU22,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":""},null,{"$f":"VLOOKUP(D22,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},null,0,0,null,null,null,null,0,null,{"$f":"IF(D22=\"-\",0,VLOOKUP(D22,'Prog Assums'!N$5:X$271,11,FALSE))","v":0},{"$f":"IF(D22=\"-\",\"\",\"m2 minimum size for 30 pupils\")","v":""},null,null,null,null,{"$f":"IF(AK22>0,62,0)","v":0},null,{"$f":"IF(AG$19=\"some extensive\",ROUND((DD$21+DE$21+DC$21)/4,0),IF(AG$19=\"some variable\",AK23,0))","v":0},null,null,{"$f":"IF(U22>0,VLOOKUP(D22,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",{"$f":"ROUNDDOWN((AQ22-VLOOKUP(AU22,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU22,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(D22,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},{"$f":"ROUNDUP(VLOOKUP(AU22,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP22*VLOOKUP(AU22,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":{"$error":"#DIV/0!"}},0,null,{"$f":"VLOOKUP(D22,'Prog Assums'!$N$6:$O$22,2,FALSE)","v":"-"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N22,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N22,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N22)","v":0},{"$f":"IF(ISERROR(BE22*BG22)=TRUE,\"\",BE22*BG22)","v":""},null,{"$f":"IF(ISERROR(BH22-Y22-V22)=TRUE,\"\",BH22-Y22-V22)","v":""},0,null,{"$f":"SUM(BO22:CK22)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S22>0,VLOOKUP($D22,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S22>0,VLOOKUP($D22,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"VLOOKUP(D22,'Prog Assums'!$N$6:$Q$229,3,0)","v":0},{"$f":"VLOOKUP(D22,'Prog Assums'!$N$6:$Q$229,4,0)","v":0},0,{"$f":"IF(CS22>14,IF(CS22<31,CS22,ROUNDDOWN(CS22/30,0)*30),0)","v":0},{"$f":"IF(S22>0,(V22/S22)*CT22,0)","v":0},{"$f":"IF(CS22>0,(V22/S22)*CS22,0)-CU22","v":0},{"$f":"IF(AK22=0,0,MAXA(1,ROUNDUP((AI22/CQ22)-CR22,0)))","v":0},{"$f":"IF(CW22>14,IF(CW22<31,CW22,ROUNDDOWN(CW22/30,0)*30),0)","v":0},{"$f":"IF(AK22>0,(AS22/AI22)*CX22,0)","v":0},{"$f":"IF(CW22>0,(AS22/AI22)*CW22,0)-CY22","v":0},30,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C22,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C22,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C22,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI22,VLOOKUP($C22,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C22,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C22,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},{"$f":"IF(ISERROR((SUM($EB22,$EH22,$EN22,$EU22)/SUM($EA22,$EG22,$EM22,$ET22)-$S22))=TRUE,0,IF($U22=0,0,(SUM($EB22,$EH22,$EN22,$EU22)/SUM($EA22,$EG22,$EM22,$ET22)-$S22)))","v":0},null,0,{"$f":"SUM($EU22,$EN22,$EH22,$EB22)-$V22-$Y22","v":0},null,null,0,null,null,{"$f":"EA22*DY22","v":0},null,null,0,null,null,{"$f":"EG22*EE22","v":0},null,null,{"$f":"IF(EN22>0,SUM(EN22/EM22),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY22:$YD22,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY22:$YD22)","v":0},null,null,null,{"$f":"IF(EU22>0,SUM(EU22/ET22),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY22:$YD22,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY22:$YD22)","v":0}]
[{"$f":"VLOOKUP($D23,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D23,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},{"$f":"IF(AG19=\"some variable\",\"Classrooms (smaller group)\",\"-\")","v":"-"},null,null,null,null,null,null,null,null,{"$f":"IF(D23=\"\",\"\",_xlfn.XLOOKUP(D23,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},{"$f":"CONCATENATE(M23,S23)","v":"-0"},{"$f":"IF(VLOOKUP(D23,'Prog Assums'!N$6:V$92,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S23>0,ROUND((S23-VLOOKUP(AU23,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU23,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":""},null,{"$f":"VLOOKUP(D23,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},null,{"$f":"AK23","v":0},{"$f":"MAXA(0,(S23*U23)-Y23)","v":0},null,null,null,null,0,null,{"$f":"IF(D23=\"-\",0,VLOOKUP(D23,'Prog Assums'!N$5:X$271,11,FALSE))","v":0},{"$f":"IF(D23=\"-\",\"\",\"m2 minimum size for 30 pupils\")","v":""},null,null,null,null,{"$f":"IF(AK23>0,48,0)","v":0},null,{"$f":"IF(AG$19=\"some variable\",ROUND((DD$21+DE$21+DC$21)/8,0),0)","v":0},null,null,{"$f":"IF(U23>0,VLOOKUP(D23,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",{"$f":"ROUNDDOWN((AQ23-VLOOKUP(AU23,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU23,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(D23,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},{"$f":"ROUNDUP(VLOOKUP(AU23,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP23*VLOOKUP(AU23,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":{"$error":"#DIV/0!"}},0,null,{"$f":"VLOOKUP(D23,'Prog Assums'!$N$6:$O$22,2,FALSE)","v":"-"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N23,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N23,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N23)","v":0},{"$f":"IF(ISERROR(BE23*BG23)=TRUE,\"\",BE23*BG23)","v":""},null,{"$f":"IF(ISERROR(BH23-Y23-V23)=TRUE,\"\",BH23-Y23-V23)","v":""},0,null,{"$f":"SUM(BO23:CK23)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S23>0,VLOOKUP($D23,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S23>0,VLOOKUP($D23,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"VLOOKUP(D23,'Prog Assums'!$N$6:$Q$229,3,0)","v":0},{"$f":"VLOOKUP(D23,'Prog Assums'!$N$6:$Q$229,4,0)","v":0},0,{"$f":"IF(CS23>14,IF(CS23<31,CS23,ROUNDDOWN(CS23/30,0)*30),0)","v":0},{"$f":"IF(S23>0,(V23/S23)*CT23,0)","v":0},{"$f":"IF(CS23>0,(V23/S23)*CS23,0)-CU23","v":0},0,{"$f":"IF(CW23>14,IF(CW23<31,CW23,ROUNDDOWN(CW23/30,0)*30),0)","v":0},{"$f":"IF(AK23>0,(AS23/AI23)*CX23,0)","v":0},{"$f":"IF(CW23>0,(AS23/AI23)*CW23,0)-CY23","v":0},31,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C23,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C23,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C23,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI23,VLOOKUP($C23,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C23,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C23,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},{"$f":"IF(ISERROR((SUM($EB23,$EH23,$EN23,$EU23)/SUM($EA23,$EG23,$EM23,$ET23)-$S23))=TRUE,0,IF($U23=0,0,(SUM($EB23,$EH23,$EN23,$EU23)/SUM($EA23,$EG23,$EM23,$ET23)-$S23)))","v":0},null,0,{"$f":"SUM($EU23,$EN23,$EH23,$EB23)-$V23-$Y23","v":0},null,null,0,null,0,{"$f":"EA23*DY23","v":0},null,null,0,null,0,{"$f":"EG23*EE23","v":0},null,null,{"$f":"IF(EN23>0,SUM(EN23/EM23),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY23:$YD23,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY23:$YD23)","v":0},null,null,null,{"$f":"IF(EU23>0,SUM(EU23/ET23),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY23:$YD23,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY23:$YD23)","v":0}]
[{"$f":"VLOOKUP($D24,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D24,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},{"$f":"IF(AO12=\"unit\",\"Secondary SEN classrooms (ambulant)\",\"-\")","v":"-"},null,null,null,null,null,null,null,null,{"$f":"IF(D24=\"\",\"\",_xlfn.XLOOKUP(D24,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},{"$f":"CONCATENATE(M24,S24)","v":"-0"},{"$f":"IF(VLOOKUP(D24,'Prog Assums'!N$6:V$92,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S24>0,ROUNDDOWN((S24-VLOOKUP(AU24,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU24,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":""},null,{"$f":"AI24","v":0},null,{"$f":"AK24","v":0},0,null,null,{"$f":"IF(D24=\"Secondary SEN classrooms (ambulant)\",S24*U24,0)","v":0},null,0,null,{"$f":"IF(D24=\"-\",0,VLOOKUP(D24,'Prog Assums'!N$5:X$271,11,FALSE))","v":0},"",null,null,null,null,{"$f":"IF(AO12=\"unit\",(ROUNDUP(DB24/7,0)*7)-1,0)","v":0},null,{"$f":"IF(AO12=\"unit\",ROUNDUP(K12/10,0),0)","v":0},null,null,{"$f":"IF(U24>0,VLOOKUP(D24,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",{"$f":"ROUNDDOWN((AQ24-VLOOKUP(AU24,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU24,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":{"$error":"#DIV/0!"}},{"$f":"DB24","v":0},{"$f":"AQ24+10","v":10},{"$f":"IF(K12>0,MAXA((AI24*AK24)-AT24,0),0)","v":0},{"$f":"AK24*AI24","v":0},{"$f":"VLOOKUP(D24,'Prog Assums'!$N$6:$O$22,2,FALSE)","v":"-"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N24,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N24,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N24)","v":0},{"$f":"IF(ISERROR(BE24*BG24)=TRUE,\"\",BE24*BG24)","v":""},null,{"$f":"IF(ISERROR(BH24-Y24-V24)=TRUE,\"\",BH24-Y24-V24)","v":""},0,null,{"$f":"SUM(BO24:CK24)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U24","v":0},null,null,null,{"$f":"IF($S24>0,VLOOKUP($D24,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S24>0,VLOOKUP($D24,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"VLOOKUP(D24,'Prog Assums'!$N$6:$Q$229,3,0)","v":0},{"$f":"VLOOKUP(D24,'Prog Assums'!$N$6:$Q$229,4,0)","v":0},0,{"$f":"IF(CS24>14,IF(CS24<31,CS24,ROUNDDOWN(CS24/30,0)*30),0)","v":0},{"$f":"IF(S24>0,(V24/S24)*CT24,0)","v":0},{"$f":"IF(CS24>0,(V24/S24)*CS24,0)-CU24","v":0},0,{"$f":"IF(CW24>14,IF(CW24<31,CW24,ROUNDDOWN(CW24/30,0)*30),0)","v":0},{"$f":"IF(AK24>0,(AS24/AI24)*CX24,0)","v":0},{"$f":"IF(CW24>0,(AS24/AI24)*CW24,0)-CY24","v":0},null,{"$f":"IF(AO12=\"unit\",ROUNDUP(K12*5.5,0)/AK24,0)","v":0},"SEN",null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C24,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C24,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C24,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI24,VLOOKUP($C24,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C24,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C24,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},{"$f":"IF(ISERROR((SUM($EB24,$EH24,$EN24,$EU24)/SUM($EA24,$EG24,$EM24,$ET24)-$S24))=TRUE,0,IF($U24=0,0,(SUM($EB24,$EH24,$EN24,$EU24)/SUM($EA24,$EG24,$EM24,$ET24)-$S24)))","v":0},null,0,{"$f":"SUM($EU24,$EN24,$EH24,$EB24)-$V24-$Y24","v":0},null,null,0,null,0,{"$f":"EA24*DY24","v":0},null,null,0,null,0,{"$f":"EG24*EE24","v":0},null,null,{"$f":"IF(EN24>0,SUM(EN24/EM24),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY24:$YD24,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY24:$YD24)","v":0},null,null,null,{"$f":"IF(EU24>0,SUM(EU24/ET24),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY24:$YD24,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY24:$YD24)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(ER25:FZ25)","v":0},null,null,null,null,null,null,{"$f":"SUM(EY25:GG25)","v":0}]
[null,null,null,"ICT/ business studies ",null,null,null,null,null,null,{"$f":"'curriculum analysis (optional)'!AO114","v":0},null,null,null,null,null,null,null,null,null,{"$f":"U27+U28+U29","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AK27+AK28+AK29","v":4},null,null,null,null,null,null,null,null,null,null,{"$f":"((AW$4*AY$4)+(AW$5*AY$5)+(AW$6*AY$6)+(AW$8*AY$8))/(AY$4+AY$5+AY$6+AY$8)","v":22.814285714285713},{"$f":"(U26*AV26*0.9)/K$8","v":7.3005714285714285E-2},"of curriculum @ 90% use",null,null,null,null,null,null,null,null,{"$f":"BG27+BG28+BG29","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(K12>0,ROUND(1+(K12/50),0),0)","v":0},{"$f":"SUM(DD27:DD30)","v":2},{"$f":"SUM(DE27:DE30)","v":2},{"$f":"MAXA(0,ROUNDDOWN($K$5/300,0))","v":3},{"$f":"MAXA(0,ROUNDDOWN($K$5/300,0))","v":3},{"$f":"MAXA(0,ROUNDDOWN($K$5/300,0)-DH5)","v":2},{"$f":"MAXA(0,ROUNDDOWN(($K$5/300),0))","v":3},{"$f":"MAXA(0,ROUNDDOWN($K$6/100,0))","v":2},{"$f":"MAXA(0,ROUNDDOWN($K$6/100,0))","v":2},{"$f":"MAXA(0,ROUNDDOWN($K$6/100,0))","v":2},{"$f":"MAXA(0,ROUNDDOWN($K$6/100,0)+DM5)","v":3},null,null,null,null,null,null,null,{"$f":"SUM(EA26,EG26,EM26,ET26)-U26","v":-4},null,null,null,null,null,{"$f":"SUM(EA27:EA29)","v":0},{"$f":"SUM(EB27:EB29)","v":0},null,null,null,null,{"$f":"SUM(EG27:EG29)","v":0},{"$f":"SUM(EH27:EH29)","v":0},null,null,null,null,{"$f":"SUM(EM27:EM29)","v":0},{"$f":"SUM(EN27:EN29)","v":0},null,null,null,null,null,{"$f":"SUM(ET27:ET29)","v":0},{"$f":"SUM(EU27:EU29)","v":0}]
[{"$f":"VLOOKUP($D27,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"CLA32"},null,{"$f":"VLOOKUP($D27,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"CLA32"},"ICT-rich classrooms",null,null,null,null,null,null,null,null,{"$f":"IF(D27=\"\",\"\",_xlfn.XLOOKUP(D27,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"ICT-rich classroom"},{"$f":"CONCATENATE(M27,S27)","v":"ICT-rich classroom69"},null,null,{"$f":"ROUNDDOWN((S27-VLOOKUP(AU27,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU27,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":33},null,{"$f":"VLOOKUP(D27,'Prog Assums'!N$5:U$271,5,FALSE)","v":69},null,{"$f":"AK27","v":3},207,null,null,null,null,0,null,{"$f":"IF(D27=\"-\",0,VLOOKUP(D27,'Prog Assums'!N$5:X$271,11,FALSE))","v":62},{"$f":"IF(D27=\"-\",\"\",\"m2 minimum size for 30 pupils\")","v":"m2 minimum size for 30 pupils"},null,null,null,null,{"$f":"IF(AK27>0,69,0)","v":69},null,{"$f":"DD27+DE27+DC27","v":3},null,null,{"$f":"IF(U27>0,VLOOKUP(D27,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0.5},"",{"$f":"ROUNDDOWN((AQ27-VLOOKUP(AU27,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU27,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":33},{"$f":"VLOOKUP(D27,'Prog Assums'!N$5:U$271,5,FALSE)","v":69},{"$f":"ROUNDUP(VLOOKUP(AU27,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP27*VLOOKUP(AU27,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":76},207,null,"D",null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N27,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N27,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N27)","v":3},{"$f":"IF(ISERROR(BE27*BG27)=TRUE,\"\",BE27*BG27)","v":""},null,{"$f":"IF(ISERROR(BH27-Y27-V27)=TRUE,\"\",BH27-Y27-V27)","v":""},0,null,{"$f":"SUM(BO27:CK27)","v":3},null,null,null,null,null,null,null,null,null,{"$f":"U27","v":3},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S27>0,VLOOKUP($D27,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"62m2 for 30"},{"$f":"IF($S27>0,VLOOKUP($D27,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"C"},null,null,{"$f":"VLOOKUP(D27,'Prog Assums'!$N$6:$Q$229,3,0)","v":2},{"$f":"VLOOKUP(D27,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},{"$f":"IF(S27=0,0,MAXA(1,ROUNDUP((S27/CQ27)-CR27,0)))","v":31},{"$f":"IF(CS27>14,IF(CS27<31,CS27,ROUNDDOWN(CS27/30,0)*30),0)","v":30},{"$f":"IF(S27>0,(V27/S27)*CT27,0)","v":90},{"$f":"IF(CS27>0,(V27/S27)*CS27,0)-CU27","v":3},{"$f":"IF(AK27=0,0,MAXA(1,ROUNDUP((AI27/CQ27)-CR27,0)))","v":31},{"$f":"IF(CW27>14,IF(CW27<31,CW27,ROUNDDOWN(CW27/30,0)*30),0)","v":30},{"$f":"IF(AK27>0,(AS27/AI27)*CX27,0)","v":90},{"$f":"IF(CW27>0,(AS27/AI27)*CW27,0)-CY27","v":3},null,null,null,{"$f":"HLOOKUP($AG$12,$DF$15:$DI$74,13,FALSE)","v":2},{"$f":"HLOOKUP($AG$12,$DJ$15:$DM$74,13,FALSE)","v":1},{"$f":"MAXA(DF26-DF28,0)","v":2},{"$f":"DG26","v":3},{"$f":"DH26","v":2},{"$f":"DI26","v":3},{"$f":"MAXA(DJ26-DJ28,0)","v":1},{"$f":"MAXA(DK26-DK28,0)","v":1},1,2,{"$f":"VLOOKUP($C27,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":45},{"$f":"VLOOKUP($C27,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":55},{"$f":"IF(VLOOKUP($C27,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI27,VLOOKUP($C27,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":62},{"$f":"VLOOKUP($C27,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":69},{"$f":"VLOOKUP($C27,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":125},{"$f":"IF(ISERROR((SUM($EB27,$EH27,$EN27,$EU27)/SUM($EA27,$EG27,$EM27,$ET27)-$S27))=TRUE,0,IF($U27=0,0,(SUM($EB27,$EH27,$EN27,$EU27)/SUM($EA27,$EG27,$EM27,$ET27)-$S27)))","v":0},null,{"$f":"SUM(EA27,EG27,EM27,ET27)-U27","v":-3},{"$f":"SUM($EU27,$EN27,$EH27,$EB27)-$V27-$Y27","v":-207},null,null,0,null,0,{"$f":"EA27*DY27","v":0},null,null,0,null,0,{"$f":"EG27*EE27","v":0},null,null,{"$f":"IF(EN27>0,SUM(EN27/EM27),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY27:$YD27,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY27:$YD27)","v":0},null,null,null,{"$f":"IF(EU27>0,SUM(EU27/ET27),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY27:$YD27,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY27:$YD27)","v":0}]
[{"$f":"VLOOKUP($D28,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"CLA32"},null,{"$f":"VLOOKUP($D28,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"CLA42"},{"$f":"IF(AK28>0,\"ICT-rich classrooms (business studies)\",\"-\")","v":"ICT-rich classrooms (business studies)"},null,null,null,null,null,null,null,null,{"$f":"IF(D28=\"\",\"\",_xlfn.XLOOKUP(D28,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"ICT-rich classroom (business studies)"},{"$f":"CONCATENATE(M28,S28)","v":"ICT-rich classroom (business studies)69"},{"$f":"IF(VLOOKUP(D28,'Prog Assums'!N$6:V$92,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S28>0,ROUNDDOWN((S28-VLOOKUP(AU28,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU28,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":33},null,{"$f":"VLOOKUP(D28,'Prog Assums'!N$5:U$271,5,FALSE)","v":69},null,{"$f":"AK28","v":1},69,null,null,null,null,0,null,{"$f":"IF(D28=\"-\",0,VLOOKUP(D28,'Prog Assums'!N$5:X$271,11,FALSE))","v":62},"m2 minimum size for 30 pupils",null,null,null,null,{"$f":"IF(AK28>0,69,0)","v":69},null,{"$f":"DD28+DE28+DC28","v":1},null,null,{"$f":"IF(U28>0,VLOOKUP(D28,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0.5},"",{"$f":"ROUNDDOWN((AQ28-VLOOKUP(AU28,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU28,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":33},{"$f":"VLOOKUP(D28,'Prog Assums'!N$5:U$271,5,FALSE)","v":69},{"$f":"ROUNDUP(VLOOKUP(AU28,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP28*VLOOKUP(AU28,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":76},69,null,{"$f":"VLOOKUP(D28,'Prog Assums'!$N$25:$O$34,2,FALSE)","v":"D"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N28,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N28,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N28)","v":1},{"$f":"IF(ISERROR(BE28*BG28)=TRUE,\"\",BE28*BG28)","v":""},null,{"$f":"IF(ISERROR(BH28-Y28-V28)=TRUE,\"\",BH28-Y28-V28)","v":""},0,null,{"$f":"SUM(BO28:CK28)","v":1},null,null,null,null,null,null,null,null,null,{"$f":"U28","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S28>0,VLOOKUP($D28,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"62m2 for 30"},{"$f":"IF($S28>0,VLOOKUP($D28,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"C"},null,null,{"$f":"VLOOKUP(D28,'Prog Assums'!$N$6:$Q$229,3,0)","v":2},{"$f":"VLOOKUP(D28,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},31,{"$f":"IF(CS28>14,IF(CS28<31,CS28,ROUNDDOWN(CS28/30,0)*30),0)","v":30},{"$f":"IF(S28>0,(V28/S28)*CT28,0)","v":30},{"$f":"IF(CS28>0,(V28/S28)*CS28,0)-CU28","v":1},31,30,30,1,30,null,null,{"$f":"HLOOKUP($AG$12,$DF$15:$DI$74,14,FALSE)","v":0},{"$f":"HLOOKUP($AG$12,$DJ$15:$DM$74,14,FALSE)","v":1},{"$f":"IF(DF26>0,DF5,0)","v":1},null,null,null,{"$f":"IF(DJ26>0,DJ5,0)","v":1},{"$f":"IF(DK26>0,DK5,0)","v":1},1,1,{"$f":"VLOOKUP($C28,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":45},{"$f":"VLOOKUP($C28,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":55},{"$f":"IF(VLOOKUP($C28,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI28,VLOOKUP($C28,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":62},{"$f":"VLOOKUP($C28,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":69},{"$f":"VLOOKUP($C28,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":125},{"$f":"IF(ISERROR((SUM($EB28,$EH28,$EN28,$EU28)/SUM($EA28,$EG28,$EM28,$ET28)-$S28))=TRUE,0,IF($U28=0,0,(SUM($EB28,$EH28,$EN28,$EU28)/SUM($EA28,$EG28,$EM28,$ET28)-$S28)))","v":0},null,{"$f":"SUM(EA28,EG28,EM28,ET28)-U28","v":-1},{"$f":"SUM($EU28,$EN28,$EH28,$EB28)-$V28-$Y28","v":-69},null,null,0,null,null,{"$f":"EA28*DY28","v":0},null,null,0,null,0,{"$f":"EG28*EE28","v":0},null,null,{"$f":"IF(EN28>0,SUM(EN28/EM28),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY28:$YD28,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY28:$YD28)","v":0},null,null,null,{"$f":"IF(EU28>0,SUM(EU28/ET28),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY28:$YD28,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY28:$YD28)","v":0}]
[{"$f":"VLOOKUP($D29,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D29,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},"-",null,null,null,null,null,null,null,null,{"$f":"IF(D29=\"\",\"\",_xlfn.XLOOKUP(D29,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},{"$f":"CONCATENATE(M29,S29)","v":"-0"},{"$f":"IF(VLOOKUP(D29,'Prog Assums'!N$6:V$92,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S29>0,ROUNDDOWN((S29-VLOOKUP(AU29,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU29,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":""},null,{"$f":"VLOOKUP(D29,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},null,{"$f":"AK29","v":0},0,null,null,null,null,0,null,{"$f":"IF(D29=\"-\",0,VLOOKUP(D29,'Prog Assums'!N$5:X$271,11,FALSE))","v":0},{"$f":"IF(D29=\"-\",\"\",\"m2 minimum size for 30 pupils\")","v":""},null,null,null,null,null,null,null,null,null,{"$f":"IF(U29>0,VLOOKUP(D29,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",{"$f":"ROUNDDOWN((AQ29-VLOOKUP(AU29,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU29,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(D29,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},{"$f":"ROUNDUP(VLOOKUP(AU29,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP29*VLOOKUP(AU29,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":{"$error":"#N/A"}},0,null,{"$f":"VLOOKUP(D29,'Prog Assums'!$N$25:$O$34,2,FALSE)","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N29,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N29,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N29)","v":0},{"$f":"IF(ISERROR(BE29*BG29)=TRUE,\"\",BE29*BG29)","v":""},null,{"$f":"IF(ISERROR(BH29-Y29-V29)=TRUE,\"\",BH29-Y29-V29)","v":""},0,null,{"$f":"SUM(BO29:CK29)","v":0},null,null,null,null,null,null,null,null,null,{"$f":"U29","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S29>0,VLOOKUP($D29,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S29>0,VLOOKUP($D29,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"VLOOKUP(D29,'Prog Assums'!$N$6:$Q$229,3,0)","v":0},{"$f":"VLOOKUP(D29,'Prog Assums'!$N$6:$Q$229,4,0)","v":0},0,{"$f":"IF(CS29>14,IF(CS29<31,CS29,ROUNDDOWN(CS29/30,0)*30),0)","v":0},{"$f":"IF(S29>0,(V29/S29)*CT29,0)","v":0},{"$f":"IF(CS29>0,(V29/S29)*CS29,0)-CU29","v":0},0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C29,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C29,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C29,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI29,VLOOKUP($C29,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C29,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C29,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},{"$f":"IF(ISERROR((SUM($EB29,$EH29,$EN29,$EU29)/SUM($EA29,$EG29,$EM29,$ET29)-$S29))=TRUE,0,IF($U29=0,0,(SUM($EB29,$EH29,$EN29,$EU29)/SUM($EA29,$EG29,$EM29,$ET29)-$S29)))","v":0},null,{"$f":"SUM(EA29,EG29,EM29,ET29)-U29","v":0},{"$f":"SUM($EU29,$EN29,$EH29,$EB29)-$V29-$Y29","v":0},null,null,0,null,0,{"$f":"EA29*DY29","v":0},null,null,0,null,0,{"$f":"EG29*EE29","v":0},null,null,{"$f":"IF(EN29>0,SUM(EN29/EM29),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY29:$YD29,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY29:$YD29)","v":0},null,null,null,{"$f":"IF(EU29>0,SUM(EU29/ET29),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY29:$YD29,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY29:$YD29)","v":0}]
[null,null,null,"Practical learning spaces"]
[null,null,null,"Science ",null,null,null,null,null,null,{"$f":"'curriculum analysis (optional)'!AO122","v":0},null,null,null,null,null,null,null,null,null,{"$f":"U32+U33+U34+U35+U36","v":10},null,null,null,null,null,null,null,"science options",null,null,null,"all standard labs + post-16",null,null,null,{"$f":"AK32+AK33+AK34+AK35+AK36","v":10},null,null,null,null,null,null,null,null,null,null,{"$f":"((AW$4*AY$4)+((AV$5/DA$2)*2/3)+(AW$5*(AY$5*1/3))+(AW$6*AY$6)+(AW$8*AY$8))/(AY$4+AY$5+AY$6+AY$8)","v":24.042857142857141},{"$f":"(U31*AV31*0.85)/K$8","v":0.18165714285714285},"of curriculum @ 85% use",null,null,null,null,null,null,null,null,{"$f":"BG32+BG33+BG34+BG36","v":10},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"DC32+DC33","v":0},{"$f":"SUM(DD32:DD35)","v":7},{"$f":"SUM(DE32:DE35)","v":3},{"$f":"ROUND($K$5/150,0)+IF(K8>800,DF5,0)","v":7},{"$f":"ROUND($K$5/150,0)","v":6},{"$f":"ROUND(($K$5/150),0)+DH5","v":7},{"$f":"ROUND(($K$5/150),0)+DI5","v":7},{"$f":"ROUND(($K$6/151),0)+DJ5","v":2},{"$f":"ROUND($K$6/150,0)","v":2},{"$f":"ROUND(($K$6/150),0)+DL5","v":3},{"$f":"ROUND($K$6/150,0)","v":2},null,null,null,null,null,null,null,{"$f":"SUM(EA31,EG31,EM31,ET31)-U31","v":-10},null,null,null,null,null,{"$f":"SUM(EA32:EA36)","v":0},{"$f":"SUM(EB32:EB36)","v":0},null,null,null,null,{"$f":"SUM(EG32:EG36)","v":0},{"$f":"SUM(EH32:EH36)","v":0},null,null,null,null,{"$f":"SUM(EM32:EM36)","v":0},{"$f":"SUM(EN32:EN36)","v":0},null,null,null,null,null,{"$f":"SUM(ET32:ET36)","v":0},{"$f":"SUM(EU32:EU36)","v":0}]
[{"$f":"VLOOKUP($D32,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"SCI02"},null,{"$f":"VLOOKUP($D32,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"SCI02"},"Science studios",null,null,null,null,null,null,null,null,{"$f":"IF(D32=\"\",\"\",_xlfn.XLOOKUP(D32,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Science studio"},{"$f":"CONCATENATE(M32,S32)","v":"Science studio69"},null,null,{"$f":"IF(S32>0,ROUNDDOWN((S32-VLOOKUP(AU32,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU32,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":30},null,{"$f":"VLOOKUP(D32,'Prog Assums'!N$5:U$271,5,FALSE)","v":69},null,{"$f":"AK32","v":0},0,null,null,null,null,0,null,{"$f":"IF(D32=\"-\",0,VLOOKUP(D32,'Prog Assums'!N$5:X$271,11,FALSE))","v":69},{"$f":"IF(D32=\"-\",\"\",\"m2 minimum size for 30 pupils\")","v":"m2 minimum size for 30 pupils"},null,null,null,null,{"$f":"IF(AK32>0,69,0)","v":0},null,{"$f":"IF(AG31=\"1 studio for every 2 spec labs\",ROUNDDOWN((DD31+DE31+DC31)*0.34,0),0)","v":0},null,null,{"$f":"IF(U32>0,VLOOKUP(D32,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",30,{"$f":"VLOOKUP(D32,'Prog Assums'!N$5:U$271,5,FALSE)","v":69},{"$f":"ROUNDUP(VLOOKUP(AU32,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP32*VLOOKUP(AU32,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":76},0,null,"E",null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N32,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N32,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N32)","v":0},{"$f":"IF(ISERROR(BE32*BG32)=TRUE,\"\",BE32*BG32)","v":""},null,{"$f":"IF(ISERROR(BH32-Y32-V32)=TRUE,\"\",BH32-Y32-V32)","v":""},0,null,{"$f":"SUM(BO32:CK32)","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"U32","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S32>0,VLOOKUP($D32,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"69m2 for 30"},{"$f":"IF($S32>0,VLOOKUP($D32,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"D"},null,null,{"$f":"VLOOKUP(D32,'Prog Assums'!$N$6:$Q$229,3,0)","v":2.5},{"$f":"VLOOKUP(D32,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},24,{"$f":"IF(CS32>14,IF(CS32<31,CS32,ROUNDDOWN(CS32/30,0)*30),0)","v":24},{"$f":"IF(S32>0,(V32/S32)*CT32,0)","v":0},{"$f":"IF(CS32>0,(V32/S32)*CS32,0)-CU32","v":0},{"$f":"IF(AK32=0,0,MAXA(1,ROUNDUP((AI32/CQ32)-CR32,0)))","v":0},{"$f":"IF(CW32>14,IF(CW32<31,CW32,ROUNDDOWN(CW32/30,0)*30),0)","v":0},{"$f":"IF(AK32>0,(AS32/AI32)*CX32,0)","v":0},{"$f":"IF(CW32>0,(AS32/AI32)*CW32,0)-CY32","v":0},30,null,null,{"$f":"HLOOKUP($AG$12,$DF$15:$DI$74,18,FALSE)","v":2},null,0,{"$f":"ROUNDDOWN(DG31/3,0)","v":2},{"$f":"ROUNDDOWN(DH31/3,0)","v":2},{"$f":"ROUNDDOWN(DI31/3,0)","v":2},null,null,null,null,{"$f":"VLOOKUP($C32,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":45},{"$f":"VLOOKUP($C32,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":62},{"$f":"IF(VLOOKUP($C32,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI32,VLOOKUP($C32,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":69},{"$f":"VLOOKUP($C32,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":76},{"$f":"VLOOKUP($C32,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":125},{"$f":"IF(ISERROR((SUM($EB32,$EH32,$EN32,$EU32)/SUM($EA32,$EG32,$EM32,$ET32)-$S32))=TRUE,0,IF($U32=0,0,(SUM($EB32,$EH32,$EN32,$EU32)/SUM($EA32,$EG32,$EM32,$ET32)-$S32)))","v":0},null,0,{"$f":"SUM($EU32,$EN32,$EH32,$EB32)-$V32-$Y32","v":0},null,null,0,null,0,{"$f":"EA32*DY32","v":0},null,null,0,null,0,{"$f":"EG32*EE32","v":0},null,null,{"$f":"IF(EN32>0,SUM(EN32/EM32),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY32:$YD32,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY32:$YD32)","v":0},null,null,null,{"$f":"IF(EU32>0,SUM(EU32/ET32),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY32:$YD32,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY32:$YD32)","v":0}]
[{"$f":"VLOOKUP($D33,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"SCI05"},null,{"$f":"VLOOKUP($D33,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"SCI05"},"Science laboratories",null,null,null,null,null,null,null,null,{"$f":"IF(D33=\"\",\"\",_xlfn.XLOOKUP(D33,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Science laboratory"},{"$f":"CONCATENATE(M33,S33)","v":"Science laboratory83"},null,null,{"$f":"IF(S33>0,ROUNDDOWN((S33-VLOOKUP(AU33,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU33,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":30},null,{"$f":"VLOOKUP(D33,'Prog Assums'!N$5:U$271,5,FALSE)","v":83},null,{"$f":"AK33","v":7},581,null,null,null,null,0,null,{"$f":"IF(D33=\"-\",0,VLOOKUP(D33,'Prog Assums'!N$5:X$271,11,FALSE))","v":83},{"$f":"IF(D33=\"-\",\"\",\"m2 minimum size for 30 pupils\")","v":"m2 minimum size for 30 pupils"},null,null,null,null,{"$f":"IF(AK33>0,83,0)","v":83},null,{"$f":"DD31+DE31+DC31-AK32-AK34-AK35-AK36","v":7},null,null,{"$f":"IF(U33>0,VLOOKUP(D33,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":10},"",30,{"$f":"VLOOKUP(D33,'Prog Assums'!N$5:U$271,5,FALSE)","v":83},{"$f":"ROUNDUP(VLOOKUP(AU33,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP33*VLOOKUP(AU33,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":97},581,null,"F",null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N33,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N33,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N33)","v":7},{"$f":"IF(ISERROR(BE33*BG33)=TRUE,\"\",BE33*BG33)","v":""},null,{"$f":"IF(ISERROR(BH33-Y33-V33)=TRUE,\"\",BH33-Y33-V33)","v":""},0,null,{"$f":"SUM(BO33:CK33)","v":7},null,null,null,null,null,null,null,null,null,null,null,{"$f":"U33","v":7},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S33>0,VLOOKUP($D33,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"90m2 for 30"},{"$f":"IF($S33>0,VLOOKUP($D33,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"E1"},null,null,{"$f":"VLOOKUP(D33,'Prog Assums'!$N$6:$Q$229,3,0)","v":2.5},{"$f":"VLOOKUP(D33,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},30,{"$f":"IF(CS33>14,IF(CS33<31,CS33,ROUNDDOWN(CS33/30,0)*30),0)","v":30},{"$f":"IF(S33>0,(V33/S33)*CT33,0)","v":210},{"$f":"IF(CS33>0,(V33/S33)*CS33,0)-CU33","v":0},30,30,210,0,30,null,null,{"$f":"HLOOKUP($AG$12,$DF$15:$DI$74,19,FALSE)","v":2},null,{"$f":"DF31-DF32","v":7},{"$f":"DG32","v":2},{"$f":"DH32","v":2},{"$f":"DI32","v":2},null,null,null,null,{"$f":"VLOOKUP($C33,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":45},{"$f":"VLOOKUP($C33,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":74.7},{"$f":"IF(VLOOKUP($C33,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI33,VLOOKUP($C33,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":83},{"$f":"VLOOKUP($C33,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":90},{"$f":"VLOOKUP($C33,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":90},{"$f":"IF(ISERROR((SUM($EB33,$EH33,$EN33,$EU33)/SUM($EA33,$EG33,$EM33,$ET33)-$S33))=TRUE,0,IF($U33=0,0,(SUM($EB33,$EH33,$EN33,$EU33)/SUM($EA33,$EG33,$EM33,$ET33)-$S33)))","v":0},null,-7,{"$f":"SUM($EU33,$EN33,$EH33,$EB33)-$V33-$Y33","v":-581},null,null,0,null,null,{"$f":"EA33*DY33","v":0},null,null,0,null,0,{"$f":"EG33*EE33","v":0},null,null,{"$f":"IF(EN33>0,SUM(EN33/EM33),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY33:$YD33,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY33:$YD33)","v":0},null,null,null,{"$f":"IF(EU33>0,SUM(EU33/ET33),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY33:$YD33,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY33:$YD33)","v":0}]
[{"$f":"VLOOKUP($D34,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"SCI05"},null,{"$f":"VLOOKUP($D34,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"SCI11"},{"$f":"IF(AG$31=\"3 specialist labs\",\"Science laboratories (chemistry)\",\"Science laboratories (specialist)\")","v":"Science laboratories (specialist)"},null,null,null,null,null,null,null,null,{"$f":"IF(D34=\"\",\"\",_xlfn.XLOOKUP(D34,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Science laboratory (specialist)"},{"$f":"CONCATENATE(M34,S34)","v":"Science laboratory (specialist)97"},{"$f":"IF(VLOOKUP(D34,'Prog Assums'!N$6:V$92,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S34>0,ROUNDDOWN((S34-VLOOKUP(AU34,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU34,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":32},null,{"$f":"VLOOKUP(D34,'Prog Assums'!N$5:U$271,5,FALSE)","v":97},null,{"$f":"AK34","v":3},291,null,null,null,null,0,null,{"$f":"IF(D34=\"-\",0,VLOOKUP(D34,'Prog Assums'!N$5:X$271,11,FALSE))","v":90},"m2 minimum size for 30 pupils",null,null,null,null,{"$f":"IF(AK$34>0,97,0)","v":97},null,{"$f":"IF(AG$31=\"1 studio for every 2 spec labs\",AK32*2,IF(AG31=\"3 specialist labs\",1,DE34))","v":3},null,null,{"$f":"IF(U34>0,VLOOKUP(D34,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":12},"",{"$f":"ROUNDDOWN((AQ34-VLOOKUP(AU34,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU34,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":32},{"$f":"VLOOKUP(D34,'Prog Assums'!N$5:U$271,5,FALSE)","v":97},{"$f":"ROUNDUP(VLOOKUP(AU34,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP34*VLOOKUP(AU34,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":103},291,null,{"$f":"VLOOKUP(D34,'Prog Assums'!$N$37:$O$48,2,FALSE)","v":"F1"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N34,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N34,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N34)","v":3},{"$f":"IF(ISERROR(BE34*BG34)=TRUE,\"\",BE34*BG34)","v":""},null,{"$f":"IF(ISERROR(BH34-Y34-V34)=TRUE,\"\",BH34-Y34-V34)","v":""},0,null,{"$f":"SUM(BO34:CK34)","v":3},null,null,null,null,null,null,null,null,null,null,null,{"$f":"U34","v":3},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S34>0,VLOOKUP($D34,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"90m2 for 30"},{"$f":"IF($S34>0,VLOOKUP($D34,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"F"},null,null,{"$f":"VLOOKUP(D34,'Prog Assums'!$N$6:$Q$229,3,0)","v":2.5},{"$f":"VLOOKUP(D34,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},35,{"$f":"IF(CS34>14,IF(CS34<31,CS34,ROUNDDOWN(CS34/30,0)*30),0)","v":30},{"$f":"IF(S34>0,(V34/S34)*CT34,0)","v":90},{"$f":"IF(CS34>0,(V34/S34)*CS34,0)-CU34","v":15},35,30,90,15,null,null,null,{"$f":"HLOOKUP($AG$12,$DF$15:$DI$74,20,FALSE)","v":3},{"$f":"HLOOKUP($AG$12,$DJ$15:$DM$74,20,FALSE)","v":3},null,{"$f":"DG31-DG32-DG33","v":2},{"$f":"DH31-DH32-DH33","v":3},{"$f":"DI31-DI32-DI33","v":3},{"$f":"DJ31","v":2},{"$f":"DK31","v":2},3,2,{"$f":"VLOOKUP($C34,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":45},{"$f":"VLOOKUP($C34,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":81},{"$f":"IF(VLOOKUP($C34,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI34,VLOOKUP($C34,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":90},{"$f":"VLOOKUP($C34,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":97},{"$f":"VLOOKUP($C34,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":150},{"$f":"IF(ISERROR((SUM($EB34,$EH34,$EN34,$EU34)/SUM($EA34,$EG34,$EM34,$ET34)-$S34))=TRUE,0,IF($U34=0,0,(SUM($EB34,$EH34,$EN34,$EU34)/SUM($EA34,$EG34,$EM34,$ET34)-$S34)))","v":0},null,-3,{"$f":"SUM($EU34,$EN34,$EH34,$EB34)-$V34-$Y34","v":-291},null,null,0,null,null,{"$f":"EA34*DY34","v":0},null,null,0,null,0,{"$f":"EG34*EE34","v":0},null,null,{"$f":"IF(EN34>0,SUM(EN34/EM34),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY34:$YD34,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY34:$YD34)","v":0},null,null,null,{"$f":"IF(EU34>0,SUM(EU34/ET34),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY34:$YD34,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY34:$YD34)","v":0}]
[{"$f":"VLOOKUP($D35,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D35,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},{"$f":"IF(AG$31=\"3 specialist labs\",\"Science laboratories (biology)\",\"-\")","v":"-"},null,null,null,null,null,null,null,null,{"$f":"IF(D35=\"\",\"\",_xlfn.XLOOKUP(D35,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},{"$f":"CONCATENATE(M35,S35)","v":"-0"},{"$f":"IF(VLOOKUP(D35,'Prog Assums'!N$6:V$92,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S35>0,ROUNDDOWN((S35-VLOOKUP(AU35,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU35,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":""},null,{"$f":"VLOOKUP(D35,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},null,{"$f":"AK35","v":0},0,null,null,null,null,0,null,{"$f":"IF(D35=\"-\",0,VLOOKUP(D35,'Prog Assums'!N$5:X$271,11,FALSE))","v":0},"",null,null,null,null,{"$f":"IF(AG$31=\"3 specialist labs\",90,0)","v":0},null,{"$f":"IF(AG$31=\"3 specialist labs\",1,0)","v":0},null,null,{"$f":"IF(U35>0,VLOOKUP(D35,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},null,{"$f":"ROUNDDOWN((AQ35-VLOOKUP(AU35,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU35,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(D35,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},{"$f":"ROUNDUP(VLOOKUP(AU35,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP35*VLOOKUP(AU35,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":{"$error":"#N/A"}},{"$f":"MAXA((AI35*AK35)-AT35,0)","v":0},null,{"$f":"VLOOKUP(D35,'Prog Assums'!$N$37:$O$48,2,FALSE)","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N35,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N35,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N35)","v":0},{"$f":"IF(ISERROR(BE35*BG35)=TRUE,\"\",BE35*BG35)","v":""},null,{"$f":"IF(ISERROR(BH35-Y35-V35)=TRUE,\"\",BH35-Y35-V35)","v":""},0,null,{"$f":"SUM(BO35:CK35)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S35>0,VLOOKUP($D35,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S35>0,VLOOKUP($D35,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"VLOOKUP(D35,'Prog Assums'!$N$6:$Q$229,3,0)","v":0},{"$f":"VLOOKUP(D35,'Prog Assums'!$N$6:$Q$229,4,0)","v":0},0,{"$f":"IF(CS35>14,IF(CS35<31,CS35,ROUNDDOWN(CS35/30,0)*30),0)","v":0},{"$f":"IF(S35>0,(V35/S35)*CT35,0)","v":0},{"$f":"IF(CS35>0,(V35/S35)*CS35,0)-CU35","v":0},0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C35,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C35,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C35,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI35,VLOOKUP($C35,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C35,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C35,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},{"$f":"IF(ISERROR((SUM($EB35,$EH35,$EN35,$EU35)/SUM($EA35,$EG35,$EM35,$ET35)-$S35))=TRUE,0,IF($U35=0,0,(SUM($EB35,$EH35,$EN35,$EU35)/SUM($EA35,$EG35,$EM35,$ET35)-$S35)))","v":0},null,0,{"$f":"SUM($EU35,$EN35,$EH35,$EB35)-$V35-$Y35","v":0},null,null,0,null,0,{"$f":"EA35*DY35","v":0},null,null,0,null,0,{"$f":"EG35*EE35","v":0},null,null,{"$f":"IF(EN35>0,SUM(EN35/EM35),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY35:$YD35,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY35:$YD35)","v":0},null,null,null,{"$f":"IF(EU35>0,SUM(EU35/ET35),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY35:$YD35,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY35:$YD35)","v":0}]
[{"$f":"VLOOKUP($D36,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D36,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},{"$f":"IF(AG$31=\"3 specialist labs\",\"Science laboratories (physics)\",\"-\")","v":"-"},null,null,null,null,null,null,null,null,{"$f":"IF(D36=\"\",\"\",_xlfn.XLOOKUP(D36,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},{"$f":"CONCATENATE(M36,S36)","v":"-0"},{"$f":"IF(VLOOKUP(D36,'Prog Assums'!N$6:V$92,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S36>0,ROUNDDOWN((S36-VLOOKUP(AU36,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU36,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":""},null,{"$f":"VLOOKUP(D36,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},null,{"$f":"AK36","v":0},0,null,null,null,null,0,null,{"$f":"IF(D36=\"-\",0,VLOOKUP(D36,'Prog Assums'!N$5:X$271,11,FALSE))","v":0},"",null,null,null,null,{"$f":"IF(AG$31=\"3 specialist labs\",90,0)","v":0},null,{"$f":"IF(AG$31=\"3 specialist labs\",1,0)","v":0},null,null,{"$f":"IF(U36>0,VLOOKUP(D36,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",{"$f":"ROUNDDOWN((AQ36-VLOOKUP(AU36,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU36,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(D36,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},{"$f":"ROUNDUP(VLOOKUP(AU36,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP36*VLOOKUP(AU36,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":{"$error":"#N/A"}},0,null,{"$f":"VLOOKUP(D36,'Prog Assums'!$N$37:$O$48,2,FALSE)","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N36,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N36,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N36)","v":0},{"$f":"IF(ISERROR(BE36*BG36)=TRUE,\"\",BE36*BG36)","v":""},null,{"$f":"IF(ISERROR(BH36-Y36-V36)=TRUE,\"\",BH36-Y36-V36)","v":""},0,null,{"$f":"SUM(BO36:CK36)","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"U36","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S36>0,VLOOKUP($D36,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S36>0,VLOOKUP($D36,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"VLOOKUP(D36,'Prog Assums'!$N$6:$Q$229,3,0)","v":0},{"$f":"VLOOKUP(D36,'Prog Assums'!$N$6:$Q$229,4,0)","v":0},0,{"$f":"IF(CS36>14,IF(CS36<31,CS36,ROUNDDOWN(CS36/30,0)*30),0)","v":0},{"$f":"IF(S36>0,(V36/S36)*CT36,0)","v":0},{"$f":"IF(CS36>0,(V36/S36)*CS36,0)-CU36","v":0},0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C36,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C36,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C36,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI36,VLOOKUP($C36,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C36,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C36,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},{"$f":"IF(ISERROR((SUM($EB36,$EH36,$EN36,$EU36)/SUM($EA36,$EG36,$EM36,$ET36)-$S36))=TRUE,0,IF($U36=0,0,(SUM($EB36,$EH36,$EN36,$EU36)/SUM($EA36,$EG36,$EM36,$ET36)-$S36)))","v":0},null,0,{"$f":"SUM($EU36,$EN36,$EH36,$EB36)-$V36-$Y36","v":0},null,null,0,null,0,{"$f":"EA36*DY36","v":0},null,null,0,null,0,{"$f":"EG36*EE36","v":0},null,null,{"$f":"IF(EN36>0,SUM(EN36/EM36),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY36:$YD36,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY36:$YD36)","v":0},null,null,null,{"$f":"IF(EU36>0,SUM(EU36/ET36),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY36:$YD36,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY36:$YD36)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(ER37:FZ37)","v":0},null,null,null,null,null,null,{"$f":"SUM(EY37:GG37)","v":0}]
[null,null,null,"Art",null,null,null,null,null,null,{"$f":"'curriculum analysis (optional)'!AO129","v":0},null,null,null,null,null,null,null,null,null,{"$f":"U39+U40+U41","v":3},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AK39+AK40+AK41","v":3},null,null,null,null,null,null,null,null,null,null,{"$f":"((AW$4*AY$4)+(AV$5/AY$5/DA$2)+(AW$5*(AY$5-1))+(AW$6*AY$6)+(AW$8*AY$8))/(AY$4+AY$5+AY$6+AY$8)","v":23.428571428571427},{"$f":"(U38*AV38*0.8)/K$8","v":4.9980952380952383E-2},"of curriculum @ 80% use",null,null,null,null,null,null,null,null,{"$f":"BG39+BG40+BG41","v":3},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"DC39+DC41","v":0},{"$f":"SUM(DD39:DD42)","v":2},{"$f":"SUM(DE39:DE42)","v":1},{"$f":"IF(ROUND($K$5/299,0)<2,DF5,ROUND($K$5/301,0))","v":3},{"$f":"IF(ROUND($K$5/301,0)<2,DG5,ROUND($K$5/301,0)-DG5)","v":2},{"$f":"IF(ROUND($K$5/301,0)<2,DH5,ROUND($K$5/301,0)-DH5)","v":2},{"$f":"IF(ROUND($K$5/301,0)<2,DI5,ROUND($K$5/301,0)-DI5)","v":2},{"$f":"IF(ROUND($K$6/301,0)<2,DJ5,ROUND($K$6/301,0))","v":1},{"$f":"IF(ROUND($K$6/301,0)<2,DK5,ROUND($K$6/301,0)+DK5)","v":1},{"$f":"IF(ROUND($K$6/301,0)<2,DL5,ROUND($K$6/301,0))","v":1},{"$f":"IF(ROUND($K$6/301,0)<2,DM5,ROUND($K$6/301,0)-DM5)","v":1},null,null,null,null,null,null,null,{"$f":"SUM(EA38,EG38,EM38,ET38)-U38","v":-3},null,null,null,null,null,{"$f":"SUM(EA39:EA41)","v":0},{"$f":"SUM(EB39:EB41)","v":0},null,null,null,null,{"$f":"SUM(EG39:EG41)","v":0},{"$f":"SUM(EH39:EH41)","v":0},null,null,null,null,{"$f":"SUM(EM39:EM41)","v":0},{"$f":"SUM(EN39:EN41)","v":0},null,null,null,null,null,{"$f":"SUM(ET39:ET41)","v":0},{"$f":"SUM(EU39:EU41)","v":0}]
[{"$f":"VLOOKUP($D39,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"DAT00"},null,{"$f":"VLOOKUP($D39,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"DAT02"},"Art rooms (general)",null,null,null,null,null,null,null,null,{"$f":"IF(D39=\"\",\"\",_xlfn.XLOOKUP(D39,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Art room (general)"},{"$f":"CONCATENATE(M39,S39)","v":"Art room (general)83"},null,null,{"$f":"ROUNDDOWN((S39-VLOOKUP(AU39,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU39,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":30},null,{"$f":"VLOOKUP(D39,'Prog Assums'!N$5:U$271,5,FALSE)","v":83},null,{"$f":"AK39","v":1},83,null,null,null,null,0,null,{"$f":"IF(D39=\"-\",0,VLOOKUP(D39,'Prog Assums'!N$5:X$271,11,FALSE))","v":83},{"$f":"IF(D39=\"-\",\"\",\"m2 minimum size for 30 pupils\")","v":"m2 minimum size for 30 pupils"},null,null,null,null,{"$f":"IF(AK39>0,83,0)","v":83},null,{"$f":"DD39+DE39+DC39","v":1},null,null,{"$f":"IF(U39>0,VLOOKUP(D39,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":10},"",{"$f":"ROUNDDOWN((AQ39-VLOOKUP(AU39,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU39,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":30},{"$f":"VLOOKUP(D39,'Prog Assums'!N$5:U$271,5,FALSE)","v":83},{"$f":"ROUNDUP(VLOOKUP(AU39,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP39*VLOOKUP(AU39,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":97},83,null,"F",null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N39,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N39,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N39)","v":1},{"$f":"IF(ISERROR(BE39*BG39)=TRUE,\"\",BE39*BG39)","v":""},null,{"$f":"IF(ISERROR(BH39-Y39-V39)=TRUE,\"\",BH39-Y39-V39)","v":""},0,null,{"$f":"SUM(BO39:CK39)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U39","v":1},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S39>0,VLOOKUP($D39,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"83m2 for 30"},{"$f":"IF($S39>0,VLOOKUP($D39,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"E1"},null,null,{"$f":"VLOOKUP(D39,'Prog Assums'!$N$6:$Q$229,3,0)","v":2.5},{"$f":"VLOOKUP(D39,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},30,{"$f":"IF(CS39>14,IF(CS39<31,CS39,ROUNDDOWN(CS39/30,0)*30),0)","v":30},{"$f":"IF(S39>0,(V39/S39)*CT39,0)","v":30},{"$f":"IF(CS39>0,(V39/S39)*CS39,0)-CU39","v":0},{"$f":"IF(AK39=0,0,MAXA(1,ROUNDUP((AI39/CQ39)-CR39,0)))","v":30},{"$f":"IF(CW39>14,IF(CW39<31,CW39,ROUNDDOWN(CW39/30,0)*30),0)","v":30},{"$f":"IF(AK39>0,(AS39/AI39)*CX39,0)","v":30},{"$f":"IF(CW39>0,(AS39/AI39)*CW39,0)-CY39","v":0},28,null,null,{"$f":"HLOOKUP($AG$12,$DF$15:$DI$74,25,FALSE)","v":1},{"$f":"HLOOKUP($AG$12,$DJ$15:$DM$74,25,FALSE)","v":0},{"$f":"IF(DF38>1,ROUND(DF38/2,0),0)","v":2},1,1,1,0,0,0,0,{"$f":"VLOOKUP($C39,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":45},{"$f":"VLOOKUP($C39,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":74.7},{"$f":"IF(VLOOKUP($C39,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI39,VLOOKUP($C39,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":83},{"$f":"VLOOKUP($C39,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":97},{"$f":"VLOOKUP($C39,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":104},{"$f":"IF(ISERROR((SUM($EB39,$EH39,$EN39,$EU39)/SUM($EA39,$EG39,$EM39,$ET39)-$S39))=TRUE,0,IF($U39=0,0,(SUM($EB39,$EH39,$EN39,$EU39)/SUM($EA39,$EG39,$EM39,$ET39)-$S39)))","v":0},null,{"$f":"SUM(EA39,EG39,EM39,ET39)-U39","v":-1},{"$f":"SUM($EU39,$EN39,$EH39,$EB39)-$V39-$Y39","v":-83},null,null,0,null,null,{"$f":"EA39*DY39","v":0},null,null,0,null,0,{"$f":"EG39*EE39","v":0},null,null,{"$f":"IF(EN39>0,SUM(EN39/EM39),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY39:$YD39,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY39:$YD39)","v":0},null,null,null,{"$f":"IF(EU39>0,SUM(EU39/ET39),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY39:$YD39,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY39:$YD39)","v":0}]
[{"$f":"VLOOKUP($D40,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"DAT00"},null,{"$f":"VLOOKUP($D40,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"DAT03"},"Art rooms (3D)",null,null,null,null,null,null,null,null,{"$f":"IF(D40=\"\",\"\",_xlfn.XLOOKUP(D40,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Art room (3D)"},"Art room (3D)97",{"$f":"IF(VLOOKUP(D40,'Prog Assums'!N$6:V$92,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S40>0,ROUNDDOWN((S40-VLOOKUP(AU40,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU40,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":30},null,{"$f":"VLOOKUP(D40,'Prog Assums'!N$5:U$271,5,FALSE)","v":97},null,{"$f":"AK40","v":2},194,null,null,null,null,0,null,{"$f":"IF(D40=\"-\",0,VLOOKUP(D40,'Prog Assums'!N$5:X$271,11,FALSE))","v":97},{"$f":"IF(D40=\"-\",\"\",\"m2 minimum size for 30 pupils\")","v":"m2 minimum size for 30 pupils"},null,null,null,null,{"$f":"IF(AK40>0,97,0)","v":97},null,{"$f":"DD40+DE40+DC40","v":2},null,null,{"$f":"IF(U40>0,VLOOKUP(D40,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":10},"",{"$f":"ROUNDDOWN((AQ40-VLOOKUP(AU40,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU40,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":30},{"$f":"VLOOKUP(D40,'Prog Assums'!N$5:U$271,5,FALSE)","v":97},{"$f":"ROUNDUP(VLOOKUP(AU40,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP40*VLOOKUP(AU40,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":116},194,null,{"$f":"VLOOKUP(D40,'Prog Assums'!$N$50:$O$62,2,FALSE)","v":"G"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N40,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N40,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N40)","v":2},{"$f":"IF(ISERROR(BE40*BG40)=TRUE,\"\",BE40*BG40)","v":""},null,{"$f":"IF(ISERROR(BH40-Y40-V40)=TRUE,\"\",BH40-Y40-V40)","v":""},0,null,{"$f":"SUM(BO40:CK40)","v":2},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U40","v":2},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S40>0,VLOOKUP($D40,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"97m2 for 30"},{"$f":"IF($S40>0,VLOOKUP($D40,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"F1"},null,null,{"$f":"VLOOKUP(D40,'Prog Assums'!$N$6:$Q$229,3,0)","v":2.5},{"$f":"VLOOKUP(D40,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},35,{"$f":"IF(CS40>14,IF(CS40<31,CS40,ROUNDDOWN(CS40/30,0)*30),0)","v":30},{"$f":"IF(S40>0,(V40/S40)*CT40,0)","v":60},{"$f":"IF(CS40>0,(V40/S40)*CS40,0)-CU40","v":10},35,30,60,10,30,null,null,{"$f":"HLOOKUP($AG$12,$DF$15:$DI$74,26,FALSE)","v":1},{"$f":"HLOOKUP($AG$12,$DJ$15:$DM$74,26,FALSE)","v":1},{"$f":"(DF38-DF41-DF39)*DF5","v":1},1,1,1,{"$f":"(DJ38-DJ41-DJ39)*DJ5","v":1},1,1,1,{"$f":"VLOOKUP($C40,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":45},{"$f":"VLOOKUP($C40,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":87.3},{"$f":"IF(VLOOKUP($C40,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI40,VLOOKUP($C40,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":97},{"$f":"VLOOKUP($C40,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":116},{"$f":"VLOOKUP($C40,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":150},{"$f":"IF(ISERROR((SUM($EB40,$EH40,$EN40,$EU40)/SUM($EA40,$EG40,$EM40,$ET40)-$S40))=TRUE,0,IF($U40=0,0,(SUM($EB40,$EH40,$EN40,$EU40)/SUM($EA40,$EG40,$EM40,$ET40)-$S40)))","v":0},null,{"$f":"SUM(EA40,EG40,EM40,ET40)-U40","v":-2},{"$f":"SUM($EU40,$EN40,$EH40,$EB40)-$V40-$Y40","v":-194},null,null,0,null,null,{"$f":"EA40*DY40","v":0},null,null,0,null,0,{"$f":"EG40*EE40","v":0},null,null,{"$f":"IF(EN40>0,SUM(EN40/EM40),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY40:$YD40,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY40:$YD40)","v":0},null,null,null,{"$f":"IF(EU40>0,SUM(EU40/ET40),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY40:$YD40,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY40:$YD40)","v":0}]
[{"$f":"VLOOKUP($D41,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D41,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},"-",null,null,null,null,null,null,null,null,{"$f":"IF(D41=\"\",\"\",_xlfn.XLOOKUP(D41,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},"-0",{"$f":"IF(VLOOKUP(D41,'Prog Assums'!N$6:V$92,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S41>0,ROUNDDOWN((S41-VLOOKUP(AU41,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU41,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":""},null,{"$f":"VLOOKUP(D41,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},null,null,0,null,null,null,null,0,null,{"$f":"IF(D41=\"-\",0,VLOOKUP(D41,'Prog Assums'!N$5:X$271,11,FALSE))","v":0},{"$f":"IF(D41=\"-\",\"\",\"m2 minimum size for 30 pupils\")","v":""},null,null,null,null,{"$f":"IF(AK41>0,104,0)","v":0},null,{"$f":"DD41+DE41+DC41","v":0},null,null,{"$f":"IF(U41>0,VLOOKUP(D41,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",{"$f":"ROUNDDOWN((AQ41-VLOOKUP(AU41,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU41,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(D41,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},{"$f":"ROUNDUP(VLOOKUP(AU41,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP41*VLOOKUP(AU41,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":{"$error":"#N/A"}},0,null,{"$f":"VLOOKUP(D41,'Prog Assums'!$N$50:$O$62,2,FALSE)","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N41,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N41,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N41)","v":0},{"$f":"IF(ISERROR(BE41*BG41)=TRUE,\"\",BE41*BG41)","v":""},null,{"$f":"IF(ISERROR(BH41-Y41-V41)=TRUE,\"\",BH41-Y41-V41)","v":""},0,null,{"$f":"SUM(BO41:CK41)","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"U41","v":0},null,{"$f":"U41","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S41>0,VLOOKUP($D41,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S41>0,VLOOKUP($D41,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"VLOOKUP(D41,'Prog Assums'!$N$6:$Q$229,3,0)","v":0},{"$f":"VLOOKUP(D41,'Prog Assums'!$N$6:$Q$229,4,0)","v":0},0,{"$f":"IF(CS41>14,IF(CS41<31,CS41,ROUNDDOWN(CS41/30,0)*30),0)","v":0},{"$f":"IF(S41>0,(V41/S41)*CT41,0)","v":0},{"$f":"IF(CS41>0,(V41/S41)*CS41,0)-CU41","v":0},0,0,0,0,28,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C41,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C41,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C41,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI41,VLOOKUP($C41,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C41,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C41,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},{"$f":"IF(ISERROR((SUM($EB41,$EH41,$EN41,$EU41)/SUM($EA41,$EG41,$EM41,$ET41)-$S41))=TRUE,0,IF($U41=0,0,(SUM($EB41,$EH41,$EN41,$EU41)/SUM($EA41,$EG41,$EM41,$ET41)-$S41)))","v":0},null,{"$f":"SUM(EA41,EG41,EM41,ET41)-U41","v":0},{"$f":"SUM($EU41,$EN41,$EH41,$EB41)-$V41-$Y41","v":0},null,null,0,null,0,{"$f":"EA41*DY41","v":0},null,null,0,null,0,{"$f":"EG41*EE41","v":0},null,null,{"$f":"IF(EN41>0,SUM(EN41/EM41),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY41:$YD41,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY41:$YD41)","v":0},null,null,null,{"$f":"IF(EU41>0,SUM(EU41/ET41),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY41:$YD41,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY41:$YD41)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(ER42:FZ42)","v":0},null,null,null,null,null,null,{"$f":"SUM(EY42:GG42)","v":0}]
[null,null,null,"Music and drama",null,null,null,null,null,null,{"$f":"'curriculum analysis (optional)'!AO136","v":0},null,null,"",null,null,null,null,null,null,{"$f":"U44+U46+U45+U47","v":2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AK44+AK45+AK46+AK47","v":2},null,null,null,null,null,null,null,null,null,null,{"$f":"((AW$4*AY$4)+(AV$5/AY$5/DA$2)+(AW$5*(AY$5-1))+(AW$6*AY$6)+(AW$8*AY$8))/(AY$4+AY$5+AY$6+AY$8)","v":23.428571428571427},{"$f":"(U43*AV43*0.8)/K$8","v":3.3320634920634924E-2},"of curriculum @ 80% use",null,null,null,null,null,null,null,null,{"$f":"BG44+BG46+BG45+BG47","v":2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ROUND(K$5/301,0)<2,DD5,ROUND(K$5/301,0)-1)","v":2},null,{"$f":"DC46+DC44+DC45+DC47+DC54","v":0},{"$f":"HLOOKUP($AG$12,$DF$15:$DI$74,29,FALSE)","v":2},{"$f":"HLOOKUP($AG$12,$DJ$15:$DM$74,29,FALSE)","v":0},{"$f":"MAXA($DA74-DF18-DF26-DF31-DF38-DF49-DF58,0)","v":1},{"$f":"MAXA($DA74-DG18-DG26-DG31-DG38-DG49-DG58,0)","v":2},{"$f":"MAXA($DA74-DH18-DH26-DH31-DH38-DH49-DH58,0)","v":2},{"$f":"MAXA($DA74-DI18-DI26-DI31-DI38-DI49-DI58,0)","v":1},{"$f":"MAXA($DB74-DJ18-DJ26-DJ31-DJ38-DJ49-DJ58,0)","v":1},{"$f":"MAXA($DB74-DK18-DK26-DK31-DK38-DK49-DK58,0)","v":1},{"$f":"MAXA($DB74-DL18-DL26-DL31-DL38-DL49-DL58,0)","v":0},{"$f":"MAXA($DB74-DM18-DM26-DM31-DM38-DM49-DM58,0)","v":0},null,null,null,null,null,null,null,{"$f":"SUM(EA43,EG43,EM43,ET43)-U43","v":-2},null,null,null,null,null,{"$f":"SUM(EA44:EA47)","v":0},{"$f":"SUM(EB44:EB47)","v":0},null,null,null,null,{"$f":"SUM(EG44:EG47)","v":0},{"$f":"SUM(EH44:EH47)","v":0},null,null,null,null,{"$f":"SUM(EM44:EM47)","v":0},{"$f":"SUM(EN44:EN47)","v":0},null,null,null,null,null,{"$f":"SUM(ET44:ET47)","v":0},{"$f":"SUM(EU44:EU47)","v":0}]
[{"$f":"VLOOKUP($D44,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"PER02"},null,{"$f":"VLOOKUP($D44,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"PER03"},"Music rooms (fitted, extensive)",null,null,null,null,null,null,null,null,{"$f":"IF(D44=\"\",\"\",_xlfn.XLOOKUP(D44,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Music room (fitted, extensive)"},"Music room (fitted, extensive)69",null,null,{"$f":"ROUNDDOWN((S44-VLOOKUP(AU44,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU44,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":33},null,{"$f":"VLOOKUP(D44,'Prog Assums'!N$5:U$271,5,FALSE)","v":69},null,{"$f":"AK44","v":1},69,null,null,null,null,0,null,{"$f":"IF(D44=\"-\",0,VLOOKUP(D44,'Prog Assums'!N$5:X$271,11,FALSE))","v":69},{"$f":"IF(D44=\"-\",\"\",\"m2 minimum size for 30 pupils\")","v":"m2 minimum size for 30 pupils"},null,null,null,null,{"$f":"IF(AK44>0,69,0)","v":69},null,{"$f":"DD44+DE44+DC44","v":1},null,null,{"$f":"IF(U44>0,VLOOKUP(D44,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":5},"",{"$f":"ROUNDDOWN((AQ44-VLOOKUP(AU44,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU44,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":33},{"$f":"VLOOKUP(D44,'Prog Assums'!N$5:U$271,5,FALSE)","v":69},{"$f":"ROUNDUP(VLOOKUP(AU44,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP44*VLOOKUP(AU44,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":76},69,null,"D",null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N44,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N44,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N44)","v":1},{"$f":"IF(ISERROR(BE44*BG44)=TRUE,\"\",BE44*BG44)","v":""},null,{"$f":"IF(ISERROR(BH44-Y44-V44)=TRUE,\"\",BH44-Y44-V44)","v":""},0,null,{"$f":"SUM(BO44:CK44)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U44","v":1},null,null,null,null,null,null,null,null,null,{"$f":"IF($S44>0,VLOOKUP($D44,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"69m2 for 30"},{"$f":"IF($S44>0,VLOOKUP($D44,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"C"},null,null,{"$f":"VLOOKUP(D44,'Prog Assums'!$N$6:$Q$229,3,0)","v":2},{"$f":"VLOOKUP(D44,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},31,{"$f":"IF(CS44>14,IF(CS44<31,CS44,ROUNDDOWN(CS44/30,0)*30),0)","v":30},{"$f":"IF(S44>0,(V44/S44)*CT44,0)","v":30},{"$f":"IF(CS44>0,(V44/S44)*CS44,0)-CU44","v":1},{"$f":"IF(AK44=0,0,MAXA(1,ROUNDUP((AI44/CQ44)-CR44,0)))","v":31},{"$f":"IF(CW44>14,IF(CW44<31,CW44,ROUNDDOWN(CW44/30,0)*30),0)","v":30},{"$f":"IF(AK44>0,(AS44/AI44)*CX44,0)","v":30},{"$f":"IF(CW44>0,(AS44/AI44)*CW44,0)-CY44","v":1},30,null,null,{"$f":"IF((DD43+DE43)>0,(DD43+DE43)-DD46-DD45,0)","v":1},null,{"$f":"IF(DF43>0,DF43-DF46-DF45,0)","v":0},1,1,0,1,1,0,0,{"$f":"VLOOKUP($C44,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":45},{"$f":"VLOOKUP($C44,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":55},{"$f":"IF(VLOOKUP($C44,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI44,VLOOKUP($C44,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":62},{"$f":"VLOOKUP($C44,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":69},{"$f":"VLOOKUP($C44,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":75},{"$f":"IF(ISERROR((SUM($EB44,$EH44,$EN44,$EU44)/SUM($EA44,$EG44,$EM44,$ET44)-$S44))=TRUE,0,IF($U44=0,0,(SUM($EB44,$EH44,$EN44,$EU44)/SUM($EA44,$EG44,$EM44,$ET44)-$S44)))","v":0},null,{"$f":"SUM(EA44,EG44,EM44,ET44)-U44","v":-1},{"$f":"SUM($EU44,$EN44,$EH44,$EB44)-$V44-$Y44","v":-69},null,null,0,null,null,{"$f":"EA44*DY44","v":0},null,null,0,null,0,{"$f":"EG44*EE44","v":0},null,null,{"$f":"IF(EN44>0,SUM(EN44/EM44),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY44:$YD44,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY44:$YD44)","v":0},null,null,null,{"$f":"IF(EU44>0,SUM(EU44/ET44),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY44:$YD44,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY44:$YD44)","v":0}]
[{"$f":"VLOOKUP($D45,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D45,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},{"$f":"IF(AK45>0,\"Music and drama classrooms\",\"-\")","v":"-"},null,null,null,null,null,null,null,null,{"$f":"IF(D45=\"\",\"\",_xlfn.XLOOKUP(D45,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},"-0",{"$f":"IF(VLOOKUP(D45,'Prog Assums'!N$6:V$92,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S45>0,ROUNDDOWN((S45-VLOOKUP(AU45,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU45,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":""},null,{"$f":"VLOOKUP(D45,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},null,{"$f":"AK45","v":0},0,null,null,null,null,0,null,{"$f":"IF(D45=\"-\",0,VLOOKUP(D45,'Prog Assums'!N$5:X$271,11,FALSE))","v":0},"",null,null,null,null,{"$f":"IF(AK45>0,83,0)","v":0},null,{"$f":"DD45+DE45+DC45","v":0},null,null,{"$f":"IF(U45>0,VLOOKUP(D45,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",{"$f":"ROUNDDOWN((AQ45-VLOOKUP(AU45,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU45,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(D45,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},{"$f":"ROUNDUP(VLOOKUP(AU45,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP45*VLOOKUP(AU45,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":{"$error":"#N/A"}},0,null,{"$f":"VLOOKUP(D45,'Prog Assums'!$N$50:$O$62,2,FALSE)","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N45,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N45,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N45)","v":0},{"$f":"IF(ISERROR(BE45*BG45)=TRUE,\"\",BE45*BG45)","v":""},null,{"$f":"IF(ISERROR(BH45-Y45-V45)=TRUE,\"\",BH45-Y45-V45)","v":""},0,null,{"$f":"SUM(BO45:CK45)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U45","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF($S45>0,VLOOKUP($D45,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S45>0,VLOOKUP($D45,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"VLOOKUP(D45,'Prog Assums'!$N$6:$Q$229,3,0)","v":0},{"$f":"VLOOKUP(D45,'Prog Assums'!$N$6:$Q$229,4,0)","v":0},0,{"$f":"IF(CS45>14,IF(CS45<31,CS45,ROUNDDOWN(CS45/30,0)*30),0)","v":0},{"$f":"IF(S45>0,(V45/S45)*CT45,0)","v":0},{"$f":"IF(CS45>0,(V45/S45)*CS45,0)-CU45","v":0},0,0,0,0,30,null,null,{"$f":"IF((DD43+DE43)=1,1,IF((DD43+DE43)>3,1,0))","v":0},null,{"$f":"IF(DF43=1,1,IF(DF43>3,1,0))","v":1},{"$f":"IF(DG43=1,1,IF(DG43>3,1,0))","v":0},0,1,{"$f":"IF(DJ43>1,1,0)","v":0},{"$f":"IF(DK43>1,1,0)","v":0},0,0,{"$f":"VLOOKUP($C45,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C45,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C45,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI45,VLOOKUP($C45,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C45,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C45,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},{"$f":"IF(ISERROR((SUM($EB45,$EH45,$EN45,$EU45)/SUM($EA45,$EG45,$EM45,$ET45)-$S45))=TRUE,0,IF($U45=0,0,(SUM($EB45,$EH45,$EN45,$EU45)/SUM($EA45,$EG45,$EM45,$ET45)-$S45)))","v":0},null,{"$f":"SUM(EA45,EG45,EM45,ET45)-U45","v":0},{"$f":"SUM($EU45,$EN45,$EH45,$EB45)-$V45-$Y45","v":0},null,null,0,null,null,{"$f":"EA45*DY45","v":0},null,null,0,null,0,{"$f":"EG45*EE45","v":0},null,null,{"$f":"IF(EN45>0,SUM(EN45/EM45),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY45:$YD45,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY45:$YD45)","v":0},null,null,null,{"$f":"IF(EU45>0,SUM(EU45/ET45),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY45:$YD45,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY45:$YD45)","v":0}]
[{"$f":"VLOOKUP($D46,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"PER15"},null,{"$f":"VLOOKUP($D46,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"PER15"},"Drama studios",null,null,null,null,null,null,null,null,{"$f":"IF(D46=\"\",\"\",_xlfn.XLOOKUP(D46,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Drama studio"},"Drama studio97",null,null,{"$f":"IF(S46>0,ROUNDDOWN((S46-VLOOKUP(AU46,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU46,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":35},null,{"$f":"VLOOKUP(D46,'Prog Assums'!N$5:U$271,5,FALSE)","v":97},null,{"$f":"AK46","v":1},97,null,null,null,null,0,null,{"$f":"IF(D46=\"-\",0,VLOOKUP(D46,'Prog Assums'!N$5:X$271,11,FALSE))","v":90},{"$f":"IF(D46=\"-\",\"\",\"m2 minimum size for 30 pupils\")","v":"m2 minimum size for 30 pupils"},null,null,null,null,{"$f":"IF(AK46>0,97,0)","v":97},null,{"$f":"DD46+DE46+DC46","v":1},null,null,{"$f":"IF(U46>0,VLOOKUP(D46,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":10},"",{"$f":"ROUNDDOWN((AQ46-VLOOKUP(AU46,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU46,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":35},{"$f":"VLOOKUP(D46,'Prog Assums'!N$5:U$271,5,FALSE)","v":97},{"$f":"ROUNDUP(VLOOKUP(AU46,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP46*VLOOKUP(AU46,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":112},97,null,"F",null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N46,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N46,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N46)","v":1},{"$f":"IF(ISERROR(BE46*BG46)=TRUE,\"\",BE46*BG46)","v":""},null,{"$f":"IF(ISERROR(BH46-Y46-V46)=TRUE,\"\",BH46-Y46-V46)","v":""},0,null,{"$f":"SUM(BO46:CK46)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U46","v":1},null,null,null,null,null,null,null,null,null,{"$f":"IF($S46>0,VLOOKUP($D46,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"90m2 for 30"},{"$f":"IF($S46>0,VLOOKUP($D46,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"E1"},null,null,{"$f":"VLOOKUP(D46,'Prog Assums'!$N$6:$Q$229,3,0)","v":12.5},{"$f":"VLOOKUP(D46,'Prog Assums'!$N$6:$Q$229,4,0)","v":-20},28,{"$f":"IF(CS46>14,IF(CS46<31,CS46,ROUNDDOWN(CS46/30,0)*30),0)","v":28},{"$f":"IF(S46>0,(V46/S46)*CT46,0)","v":28},{"$f":"IF(CS46>0,(V46/S46)*CS46,0)-CU46","v":0},28,28,28,0,28,null,null,{"$f":"IF((DD43+DE43)>1,1,0)","v":1},null,{"$f":"IF(DF43>1,1,0)","v":0},{"$f":"IF(DG43>1,1,0)","v":1},1,0,{"$f":"IF(DJ43>2,1,0)","v":0},{"$f":"IF(DK43>2,1,0)","v":0},0,0,{"$f":"VLOOKUP($C46,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":62},{"$f":"VLOOKUP($C46,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C46,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI46,VLOOKUP($C46,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":90},{"$f":"VLOOKUP($C46,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C46,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":150},{"$f":"IF(ISERROR((SUM($EB46,$EH46,$EN46,$EU46)/SUM($EA46,$EG46,$EM46,$ET46)-$S46))=TRUE,0,IF($U46=0,0,(SUM($EB46,$EH46,$EN46,$EU46)/SUM($EA46,$EG46,$EM46,$ET46)-$S46)))","v":0},null,{"$f":"SUM(EA46,EG46,EM46,ET46)-U46","v":-1},{"$f":"SUM($EU46,$EN46,$EH46,$EB46)-$V46-$Y46","v":-97},null,null,0,null,null,{"$f":"EA46*DY46","v":0},null,null,0,null,0,{"$f":"EG46*EE46","v":0},null,null,{"$f":"IF(EN46>0,SUM(EN46/EM46),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY46:$YD46,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY46:$YD46)","v":0},null,null,null,{"$f":"IF(EU46>0,SUM(EU46/ET46),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY46:$YD46,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY46:$YD46)","v":0}]
[{"$f":"VLOOKUP($D47,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D47,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},"-",null,null,null,null,null,null,null,null,{"$f":"IF(D47=\"\",\"\",_xlfn.XLOOKUP(D47,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},"-0",{"$f":"IF(VLOOKUP(D47,'Prog Assums'!N$6:V$92,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S47>0,ROUNDDOWN((S47-VLOOKUP(AU47,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU47,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":""},null,{"$f":"VLOOKUP(D47,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},null,{"$f":"AK47","v":0},0,null,null,null,null,0,null,{"$f":"IF(D47=\"-\",0,VLOOKUP(D47,'Prog Assums'!N$5:X$271,11,FALSE))","v":0},{"$f":"IF(D47=\"-\",\"\",\"m2 minimum size for 30 pupils\")","v":""},null,null,null,null,{"$f":"IF(AK47>0,83,0)","v":0},null,{"$f":"DD47+DE47+DC47","v":0},null,null,{"$f":"IF(U47>0,VLOOKUP(D47,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",{"$f":"ROUNDDOWN((AQ47-VLOOKUP(AU47,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU47,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(D47,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},{"$f":"ROUNDUP(VLOOKUP(AU47,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP47*VLOOKUP(AU47,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":{"$error":"#N/A"}},0,null,{"$f":"VLOOKUP(D47,'Prog Assums'!$N$50:$O$62,2,FALSE)","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N47,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N47,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N47)","v":0},{"$f":"IF(ISERROR(BE47*BG47)=TRUE,\"\",BE47*BG47)","v":""},null,{"$f":"IF(ISERROR(BH47-Y47-V47)=TRUE,\"\",BH47-Y47-V47)","v":""},0,null,{"$f":"SUM(BO47:CK47)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U47","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF($S47>0,VLOOKUP($D47,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S47>0,VLOOKUP($D47,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"VLOOKUP(D47,'Prog Assums'!$N$6:$Q$229,3,0)","v":0},{"$f":"VLOOKUP(D47,'Prog Assums'!$N$6:$Q$229,4,0)","v":0},0,{"$f":"IF(CS47>14,IF(CS47<31,CS47,ROUNDDOWN(CS47/30,0)*30),0)","v":0},{"$f":"IF(S47>0,(V47/S47)*CT47,0)","v":0},{"$f":"IF(CS47>0,(V47/S47)*CS47,0)-CU47","v":0},0,0,0,0,28,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C47,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C47,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C47,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI47,VLOOKUP($C47,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C47,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C47,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},{"$f":"IF(ISERROR((SUM($EB47,$EH47,$EN47,$EU47)/SUM($EA47,$EG47,$EM47,$ET47)-$S47))=TRUE,0,IF($U47=0,0,(SUM($EB47,$EH47,$EN47,$EU47)/SUM($EA47,$EG47,$EM47,$ET47)-$S47)))","v":0},null,{"$f":"SUM(EA47,EG47,EM47,ET47)-U47","v":0},{"$f":"SUM($EU47,$EN47,$EH47,$EB47)-$V47-$Y47","v":0},null,null,0,null,0,{"$f":"EA47*DY47","v":0},null,null,0,null,0,{"$f":"EG47*EE47","v":0},null,null,{"$f":"IF(EN47>0,SUM(EN47/EM47),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY47:$YD47,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY47:$YD47)","v":0},null,null,null,{"$f":"IF(EU47>0,SUM(EU47/ET47),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY47:$YD47,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY47:$YD47)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(ER48:FZ48)","v":0},null,null,null,null,null,null,{"$f":"SUM(EY48:GG48)","v":0}]
[null,null,null,"Design and technology",null,null,null,null,null,null,{"$f":"'curriculum analysis (optional)'!AO141","v":0},null,null,null,null,null,null,null,null,null,{"$f":"SUM(U50:U56)","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AK50:AK56)","v":4},null,null,null,null,null,null,null,null,null,null,{"$f":"((AX$4*AY$4)+(AX$5*AY$5)+(AX$6*AY$6)+(AX$8*AY$8))/(AY$4+AY$5+AY$6+AY$8)","v":17.857142857142858},{"$f":"(U49*AV49*0.8)/K$8","v":5.0793650793650794E-2},"of curriculum @ 80% use",null,null,null,null,null,null,null,null,{"$f":"BG56+BG54+BG55+BG53+BG52+BG50","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"DC56+DC54+DC53+DC52+DC50","v":0},{"$f":"HLOOKUP($AG$12,$DF$15:$DI$74,35,FALSE)","v":3},{"$f":"HLOOKUP($AG$12,$DJ$15:$DM$74,35,FALSE)","v":1},{"$f":"ROUND(($K$5/150),0)-DF5","v":5},{"$f":"ROUND(($K$5/300),0)","v":3},{"$f":"ROUND(($K$5/300),0)","v":3},{"$f":"ROUND(($K$5/300)-DI5,0)","v":2},{"$f":"ROUND(($K$6/150),0)-DJ5","v":1},{"$f":"ROUND(($K$6/300),0)","v":1},{"$f":"ROUND(($K$6/300),0)","v":1},1,null,null,null,null,null,null,null,{"$f":"SUM(EA49,EG49,EM49,ET49)-U49","v":-4},null,null,null,null,null,{"$f":"SUM(EA50:EA56)","v":0},{"$f":"SUM(EB50:EB56)","v":0},null,null,null,null,{"$f":"SUM(EG50:EG56)","v":0},{"$f":"SUM(EH50:EH56)","v":0},null,null,null,null,{"$f":"SUM(EM50:EM56)","v":0},{"$f":"SUM(EN50:EN56)","v":0},null,null,null,null,null,{"$f":"SUM(ET50:ET56)","v":0},{"$f":"SUM(EU50:EU56)","v":0}]
[{"$f":"VLOOKUP($D50,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"DAT43"},null,{"$f":"VLOOKUP($D50,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"DAT43"},"DT workshops",null,null,null,null,null,null,null,null,{"$f":"IF(D50=\"\",\"\",_xlfn.XLOOKUP(D50,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"DT workshop"},{"$f":"CONCATENATE(M50,S50)","v":"DT workshop111"},null,null,{"$f":"ROUNDDOWN((S50-VLOOKUP(AU50,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU50,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":28},null,{"$f":"VLOOKUP(D50,'Prog Assums'!N$5:U$271,5,FALSE)","v":111},null,{"$f":"AK50","v":1},111,null,null,null,null,0,null,{"$f":"IF(U50>1,97,104)","v":104},{"$f":"IF(AC50=104,\"m2 minimum for 24 if one space\",\"m2 minimum for 24 if 2 spaces\")","v":"m2 minimum for 24 if one space"},null,null,null,null,{"$f":"IF(AK50>0,111,0)","v":111},null,{"$f":"DD50+DE50+DC50","v":1},null,null,{"$f":"IF(U50>0,VLOOKUP(D50,'Prog Assums'!$N$6:$T$169,6,FALSE)+IF(U50>1,(U50-1)*VLOOKUP(D50,'Prog Assums'!$N$6:$T$169,7,FALSE),0),0)","v":34},"",{"$f":"ROUNDDOWN((AQ50-VLOOKUP(AU50,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU50,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":28},{"$f":"VLOOKUP(D50,'Prog Assums'!N$5:U$271,5,FALSE)","v":111},{"$f":"ROUNDUP(VLOOKUP(AU50,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP50*VLOOKUP(AU50,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":128},111,null,{"$f":"VLOOKUP(D50,'Prog Assums'!$N$63:$O$86,2,FALSE)","v":"H"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N50,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N50,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N50)","v":1},{"$f":"IF(ISERROR(BE50*BG50)=TRUE,\"\",BE50*BG50)","v":""},null,{"$f":"IF(ISERROR(BH50-Y50-V50)=TRUE,\"\",BH50-Y50-V50)","v":""},0,null,{"$f":"SUM(BO50:CK50)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U50","v":1},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S50>0,VLOOKUP($D50,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"104m2 for up to 24"},{"$f":"IF($S50>0,VLOOKUP($D50,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"G1"},null,null,{"$f":"VLOOKUP(D50,'Prog Assums'!$N$6:$Q$229,3,0)","v":3.5},{"$f":"VLOOKUP(D50,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},28,{"$f":"IF(CS50>14,IF(CS50<31,CS50,ROUNDDOWN(CS50/30,0)*30),0)","v":28},{"$f":"IF(S50>0,(V50/S50)*CT50,0)","v":28},{"$f":"IF(CS50>0,(V50/S50)*CS50,0)-CU50","v":0},{"$f":"IF(AK50=0,0,MAXA(1,ROUNDUP((AI50/CQ50)-CR50,0)))","v":28},{"$f":"IF(CW50>14,IF(CW50<31,CW50,ROUNDDOWN(CW50/30,0)*30),0)","v":28},{"$f":"IF(AK50>0,(AS50/AI50)*CX50,0)","v":28},{"$f":"IF(CW50>0,(AS50/AI50)*CW50,0)-CY50","v":0},20,null,null,{"$f":"IF(ROUND((DD49+DE49)*0.3,0)>0,1,0)","v":1},null,{"$f":"IF(ROUND(DF49*0.3,0)>0,1,1)","v":1},{"$f":"IF(ROUND(DG49*0.3,0)>0,1,0)","v":1},1,1,{"$f":"IF(ROUND(DJ49*0.3,0)>0,1,0)","v":0},{"$f":"IF(ROUND(DK49*0.3,0)>0,1,0)","v":0},{"$f":"IF(ROUND(DL49*0.3,0)>0,1,0)","v":0},{"$f":"IF(ROUND(DM49*0.3,0)>0,1,0)","v":0},{"$f":"VLOOKUP($C50,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":67},{"$f":"VLOOKUP($C50,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":85.4},{"$f":"IF(VLOOKUP($C50,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI50,VLOOKUP($C50,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":97},{"$f":"VLOOKUP($C50,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C50,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":150},{"$f":"IF(ISERROR((SUM($EB50,$EH50,$EN50,$EU50)/SUM($EA50,$EG50,$EM50,$ET50)-$S50))=TRUE,0,IF($U50=0,0,(SUM($EB50,$EH50,$EN50,$EU50)/SUM($EA50,$EG50,$EM50,$ET50)-$S50)))","v":0},null,-1,{"$f":"SUM($EU50,$EN50,$EH50,$EB50)-$V50-$Y50","v":-111},null,null,0,null,null,{"$f":"EA50*DY50","v":0},null,null,0,null,0,{"$f":"EG50*EE50","v":0},null,null,{"$f":"IF(EN50>0,SUM(EN50/EM50),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY50:$YD50,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY50:$YD50)","v":0},null,null,null,{"$f":"IF(EU50>0,SUM(EU50/ET50),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY50:$YD50,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY50:$YD50)","v":0}]
[{"$f":"VLOOKUP($D51,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D51,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},{"$f":"IF(AK51>0,\"DT workshops (2 of 2)\",\"-\")","v":"-"},null,null,null,null,null,null,null,null,{"$f":"IF(D51=\"\",\"\",_xlfn.XLOOKUP(D51,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},{"$f":"CONCATENATE(M51,S51)","v":"-0"},{"$f":"IF(VLOOKUP(D51,'Prog Assums'!N$6:V$92,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S51>0,ROUNDDOWN((S51-VLOOKUP(AU51,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU51,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":""},null,{"$f":"VLOOKUP(D51,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},null,{"$f":"AK51","v":0},{"$f":"MAXA(0,(S51*U51)-Y51)","v":0},null,null,null,null,{"$f":"IF(O51=\"retained\",V51+Y51,IF(O51=\"refurb'ed\",V51+Y51,0))","v":0},null,{"$f":"IF(D51=\"-\",0,VLOOKUP(D51,'Prog Assums'!N$5:X$271,11,FALSE))","v":0},{"$f":"IF(D51=\"-\",\"\",\"m2 minimum size for 24 pupils\")","v":""},null,null,null,null,{"$f":"IF(AK51>0,97,0)","v":0},null,0,null,null,{"$f":"IF(U51>0,VLOOKUP(D51,'Prog Assums'!$N$6:$T$169,6,FALSE)+IF(U51>1,(U51-1)*VLOOKUP(D51,'Prog Assums'!$N$6:$T$169,7,FALSE),0),0)","v":0},{"$f":"IF(O51=\"existing\",\"E\",\"\")","v":""},{"$f":"ROUNDDOWN((AQ51-VLOOKUP(AU51,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU51,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(D51,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},{"$f":"ROUNDUP(VLOOKUP(AU51,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP51*VLOOKUP(AU51,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":{"$error":"#N/A"}},{"$f":"MAXA((AI51*AK51)-AT51,0)","v":0},null,{"$f":"VLOOKUP(D51,'Prog Assums'!$N$65:$O$87,2,FALSE)","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N51,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N51,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N51)","v":0},{"$f":"IF(ISERROR(BE51*BG51)=TRUE,\"\",BE51*BG51)","v":""},null,{"$f":"IF(ISERROR(BH51-Y51-V51)=TRUE,\"\",BH51-Y51-V51)","v":""},{"$f":"BG51-U51","v":0},null,{"$f":"SUM(BO51:CK51)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U51","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP(D51,'Prog Assums'!$N$6:$Q$229,3,0)","v":0},{"$f":"VLOOKUP(D51,'Prog Assums'!$N$6:$Q$229,4,0)","v":0},0,{"$f":"IF(CS51>14,IF(CS51<31,CS51,ROUNDDOWN(CS51/30,0)*30),0)","v":0},{"$f":"IF(S51>0,(V51/S51)*CT51,0)","v":0},{"$f":"IF(CS51>0,(V51/S51)*CS51,0)-CU51","v":0},0,0,0,0,21,null,null,{"$f":"MINA(ROUND((DD49+DE49)*0.3,0)-DD50)","v":0},null,{"$f":"MINA(ROUND(DF49*0.3,0)-DF50)","v":1},{"$f":"MINA(ROUND(DG49*0.3,0)-DG50)","v":0},0,0,{"$f":"MINA(ROUND(DJ49*0.3,0)-DJ50)","v":0},{"$f":"MINA(ROUND(DK49*0.3,0)-DK50)","v":0},{"$f":"MINA(ROUND(DL49*0.3,0)-DL50)","v":0},{"$f":"MINA(ROUND(DM49*0.3,0)-DM50)","v":0},{"$f":"VLOOKUP($C51,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C51,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C51,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI51,VLOOKUP($C51,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C51,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C51,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},{"$f":"IF(ISERROR((SUM($EB51,$EH51,$EN51,$EU51)/SUM($EA51,$EG51,$EM51,$ET51)-$S51))=TRUE,0,IF($U51=0,0,(SUM($EB51,$EH51,$EN51,$EU51)/SUM($EA51,$EG51,$EM51,$ET51)-$S51)))","v":0},null,{"$f":"SUM(EA51,EG51,EM51,ET51)-U51","v":0},{"$f":"SUM($EU51,$EN51,$EH51,$EB51)-$V51-$Y51","v":0},null,null,0,null,0,{"$f":"EA51*DY51","v":0},null,null,0,null,0,{"$f":"EG51*EE51","v":0},null,null,{"$f":"IF(EN51>0,SUM(EN51/EM51),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY51:$YD51,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY51:$YD51)","v":0},null,null,null,{"$f":"IF(EU51>0,SUM(EU51/ET51),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY51:$YD51,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY51:$YD51)","v":0}]
[{"$f":"VLOOKUP($D52,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"DAT35"},null,{"$f":"VLOOKUP($D52,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"DAT35"},"Food rooms",null,null,null,null,null,null,null,null,{"$f":"IF(D52=\"\",\"\",_xlfn.XLOOKUP(D52,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Food room"},"Food room97",null,null,{"$f":"ROUNDDOWN((S52-VLOOKUP(AU52,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU52,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":24},null,{"$f":"VLOOKUP(D52,'Prog Assums'!N$5:U$271,5,FALSE)","v":97},null,1,97,null,null,null,null,0,null,{"$f":"IF(D52=\"-\",0,VLOOKUP(D52,'Prog Assums'!N$5:X$271,11,FALSE))","v":96},{"$f":"IF(D52=\"-\",\"\",\"m2 minimum size for 24 pupils\")","v":"m2 minimum size for 24 pupils"},null,null,null,null,{"$f":"IF(AK52>0,97,0)","v":97},null,1,null,null,{"$f":"IF(U52>0,VLOOKUP(D52,'Prog Assums'!$N$6:$T$169,6,FALSE)+IF(U52>1,(U52-1)*VLOOKUP(D52,'Prog Assums'!$N$6:$T$169,7,FALSE),0),0)","v":10},"",{"$f":"ROUNDDOWN((AQ52-VLOOKUP(AU52,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU52,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":24},{"$f":"VLOOKUP(D52,'Prog Assums'!N$5:U$271,5,FALSE)","v":97},{"$f":"ROUNDUP(VLOOKUP(AU52,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP52*VLOOKUP(AU52,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":112},97,null,{"$f":"VLOOKUP(D52,'Prog Assums'!$N$63:$O$86,2,FALSE)","v":"H"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N52,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N52,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N52)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U52","v":1},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S52>0,VLOOKUP($D52,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"97m2 for up to 24"},{"$f":"IF($S52>0,VLOOKUP($D52,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"G1"},null,null,{"$f":"VLOOKUP(D52,'Prog Assums'!$N$6:$Q$229,3,0)","v":3.5},{"$f":"VLOOKUP(D52,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},24,24,24,0,24,24,24,0,20,null,null,{"$f":"DD5","v":1},null,{"$f":"DF5","v":1},{"$f":"DG5","v":1},1,1,{"$f":"ROUNDDOWN(DJ49*0.3,0)","v":0},{"$f":"ROUNDDOWN(DK49*0.3,0)","v":0},0,0,{"$f":"VLOOKUP($C52,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":67},{"$f":"VLOOKUP($C52,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":85.4},{"$f":"IF(VLOOKUP($C52,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI52,VLOOKUP($C52,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":97},{"$f":"VLOOKUP($C52,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C52,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":150},0,null,-1,-97,null,null,0,null,null,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY52:$YD52,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY52:$YD52)","v":0}]
[{"$f":"VLOOKUP($D53,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D53,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},{"$f":"IF(AK53>0,\"Food rooms (2 of 2)\",\"-\")","v":"-"},null,null,null,null,null,null,null,null,{"$f":"IF(D53=\"\",\"\",_xlfn.XLOOKUP(D53,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},{"$f":"CONCATENATE(M53,S53)","v":"-0"},{"$f":"IF(VLOOKUP(D53,'Prog Assums'!N$6:V$92,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S53>0,ROUNDDOWN((S53-VLOOKUP(AU53,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU53,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":""},null,{"$f":"VLOOKUP(D53,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},null,{"$f":"AK53","v":0},{"$f":"MAXA(0,(S53*U53)-Y53)","v":0},null,null,null,null,{"$f":"IF(O53=\"retained\",V53+Y53,IF(O53=\"refurb'ed\",V53+Y53,0))","v":0},null,{"$f":"IF(D53=\"-\",0,VLOOKUP(D53,'Prog Assums'!N$5:X$271,11,FALSE))","v":0},{"$f":"IF(D53=\"-\",\"\",\"m2 minimum size for 24 pupils\")","v":""},null,null,null,null,0,null,0,null,null,{"$f":"IF(U53>0,VLOOKUP(D53,'Prog Assums'!$N$6:$T$169,6,FALSE)+IF(U53>1,(U53-1)*VLOOKUP(D53,'Prog Assums'!$N$6:$T$169,7,FALSE),0),0)","v":0},{"$f":"IF(O53=\"existing\",\"E\",\"\")","v":""},{"$f":"ROUNDDOWN((AQ53-VLOOKUP(AU53,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU53,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(D53,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},{"$f":"ROUNDUP(VLOOKUP(AU53,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP53*VLOOKUP(AU53,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":{"$error":"#N/A"}},{"$f":"MAXA((AI53*AK53)-AT53,0)","v":0},null,{"$f":"VLOOKUP(D53,'Prog Assums'!$N$65:$O$87,2,FALSE)","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N53,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N53,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N53)","v":0},{"$f":"IF(ISERROR(BE53*BG53)=TRUE,\"\",BE53*BG53)","v":""},null,{"$f":"IF(ISERROR(BH53-Y53-V53)=TRUE,\"\",BH53-Y53-V53)","v":""},{"$f":"BG53-U53","v":0},null,{"$f":"SUM(BO53:CK53)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U53","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S53>0,VLOOKUP($D53,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S53>0,VLOOKUP($D53,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"VLOOKUP(D53,'Prog Assums'!$N$6:$Q$229,3,0)","v":0},{"$f":"VLOOKUP(D53,'Prog Assums'!$N$6:$Q$229,4,0)","v":0},0,{"$f":"IF(CS53>14,IF(CS53<31,CS53,ROUNDDOWN(CS53/30,0)*30),0)","v":0},{"$f":"IF(S53>0,(V53/S53)*CT53,0)","v":0},{"$f":"IF(CS53>0,(V53/S53)*CS53,0)-CU53","v":0},0,0,0,0,20,null,null,{"$f":"IF((DD49+DE49)<6,0,1)","v":0},null,{"$f":"IF(DF49<6,0,1)","v":0},{"$f":"IF(DG49<6,0,1)","v":0},0,0,null,null,null,null,{"$f":"VLOOKUP($C53,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C53,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C53,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI53,VLOOKUP($C53,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C53,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C53,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},{"$f":"IF(ISERROR((SUM($EB53,$EH53,$EN53,$EU53)/SUM($EA53,$EG53,$EM53,$ET53)-$S53))=TRUE,0,IF($U53=0,0,(SUM($EB53,$EH53,$EN53,$EU53)/SUM($EA53,$EG53,$EM53,$ET53)-$S53)))","v":0},null,{"$f":"SUM(EA53,EG53,EM53,ET53)-U53","v":0},{"$f":"SUM($EU53,$EN53,$EH53,$EB53)-$V53-$Y53","v":0},null,null,0,null,0,{"$f":"EA53*DY53","v":0},null,null,0,null,0,{"$f":"EG53*EE53","v":0},null,null,{"$f":"IF(EN53>0,SUM(EN53/EM53),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY53:$YD53,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY53:$YD53)","v":0},null,null,null,{"$f":"IF(EU53>0,SUM(EU53/ET53),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY53:$YD53,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY53:$YD53)","v":0}]
[{"$f":"VLOOKUP($D54,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"DAT20"},null,{"$f":"VLOOKUP($D54,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"DAT22"},"DT studios (graphic products)",null,null,null,null,null,null,null,null,{"$f":"IF(D54=\"\",\"\",_xlfn.XLOOKUP(D54,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"DT studio (graphic products)"},"DT studio (graphic products)83",{"$f":"IF(VLOOKUP(D54,'Prog Assums'!N$6:V$92,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S54>0,ROUNDDOWN((S54-VLOOKUP(AU54,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU54,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":25},null,{"$f":"VLOOKUP(D54,'Prog Assums'!N$5:U$271,5,FALSE)","v":83},null,1,83,null,null,null,null,0,null,{"$f":"IF(D54=\"-\",0,VLOOKUP(D54,'Prog Assums'!N$5:X$271,11,FALSE))","v":83},{"$f":"IF(D54=\"-\",\"\",\"m2 minimum size for 24 pupils\")","v":"m2 minimum size for 24 pupils"},null,null,null,null,{"$f":"IF(AK54>0,83,0)","v":83},null,1,null,null,{"$f":"IF(U54>0,VLOOKUP(D54,'Prog Assums'!$N$6:$T$169,6,FALSE)+IF(U54>1,(U54-1)*VLOOKUP(D54,'Prog Assums'!$N$6:$T$169,7,FALSE),0),0)","v":5},"",{"$f":"ROUNDDOWN((AQ54-VLOOKUP(AU54,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU54,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":25},{"$f":"VLOOKUP(D54,'Prog Assums'!N$5:U$271,5,FALSE)","v":83},{"$f":"ROUNDUP(VLOOKUP(AU54,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP54*VLOOKUP(AU54,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":99},83,null,{"$f":"VLOOKUP(D54,'Prog Assums'!$N$65:$O$87,2,FALSE)","v":"G"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N54,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N54,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N54)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S54>0,VLOOKUP($D54,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"83m2 for up to 24"},{"$f":"IF($S54>0,VLOOKUP($D54,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"F1"},null,null,{"$f":"VLOOKUP(D54,'Prog Assums'!$N$6:$Q$229,3,0)","v":2.5},{"$f":"VLOOKUP(D54,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},30,30,30,0,30,30,30,0,20,null,null,{"$f":"IF((DD49+DE49)<7,IF((DD49+DE49)>2,DD5,0),2)","v":1},null,{"$f":"IF(DF49<7,IF(DF49>2,DF5,0),2)","v":1},{"$f":"IF(DG49<7,IF(DG49>2,DG5,0),2)","v":1},1,0,{"$f":"ROUND(DJ49*0.3,0)","v":0},{"$f":"ROUND(DK49*0.3,0)","v":0},0,0,{"$f":"VLOOKUP($C54,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":45},{"$f":"VLOOKUP($C54,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":74.7},{"$f":"IF(VLOOKUP($C54,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI54,VLOOKUP($C54,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":83},{"$f":"VLOOKUP($C54,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C54,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":150},0,null,-1,-83,null,null,0,null,null,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY54:$YD54,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY54:$YD54)","v":0}]
[{"$f":"VLOOKUP($D55,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"DAT20"},null,{"$f":"VLOOKUP($D55,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"DAT25"},"DT studios (textiles)",null,null,null,null,null,null,null,null,{"$f":"IF(D55=\"\",\"\",_xlfn.XLOOKUP(D55,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"DT studio (textiles)"},"DT studio (textiles)83",{"$f":"IF(VLOOKUP(D55,'Prog Assums'!N$6:V$92,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S55>0,ROUNDDOWN((S55-VLOOKUP(AU55,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU55,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":25},null,{"$f":"VLOOKUP(D55,'Prog Assums'!N$5:U$271,5,FALSE)","v":83},null,1,83,null,null,null,null,0,null,{"$f":"IF(D55=\"-\",0,VLOOKUP(D55,'Prog Assums'!N$5:X$271,11,FALSE))","v":83},"m2 minimum size for 24 pupils",null,null,null,null,{"$f":"IF(AK55>0,83,0)","v":83},null,1,null,null,{"$f":"IF(U55>0,VLOOKUP(D55,'Prog Assums'!$N$6:$T$169,6,FALSE)+IF(U55>1,(U55-1)*VLOOKUP(D55,'Prog Assums'!$N$6:$T$169,7,FALSE),0),0)","v":10},"",{"$f":"ROUNDDOWN((AQ55-VLOOKUP(AU55,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU55,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":25},{"$f":"VLOOKUP(D55,'Prog Assums'!N$5:U$271,5,FALSE)","v":83},{"$f":"ROUNDUP(VLOOKUP(AU55,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP55*VLOOKUP(AU55,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":99},83,null,{"$f":"VLOOKUP(D55,'Prog Assums'!$N$65:$O$87,2,FALSE)","v":"G"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N55,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N55,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N55)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S55>0,VLOOKUP($D55,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"83m2 for up to 24"},{"$f":"IF($S55>0,VLOOKUP($D55,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"F1"},null,null,{"$f":"VLOOKUP(D55,'Prog Assums'!$N$6:$Q$229,3,0)","v":2.5},{"$f":"VLOOKUP(D55,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},30,30,30,0,30,30,30,0,20,null,null,{"$f":"IF((DD49+DE49)>3,ROUND((DD49+DE49)/5,0),0)","v":1},null,{"$f":"IF(DF49>3,ROUND(DF49/5,0),0)","v":1},0,0,0,{"$f":"ROUNDDOWN(DJ49/4,0)","v":0},{"$f":"ROUNDDOWN(DK49/4,0)","v":0},0,0,{"$f":"VLOOKUP($C55,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":45},{"$f":"VLOOKUP($C55,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":74.7},{"$f":"IF(VLOOKUP($C55,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI55,VLOOKUP($C55,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":83},{"$f":"VLOOKUP($C55,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C55,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":150},0,null,-1,-83,null,null,0,null,null,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY55:$YD55,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY55:$YD55)","v":0}]
[{"$f":"VLOOKUP($D56,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D56,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},{"$f":"IF(AK56>0,\"DT studios (electronics & control)\",\"-\")","v":"-"},null,null,null,null,null,null,null,null,{"$f":"IF(D56=\"\",\"\",_xlfn.XLOOKUP(D56,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},"-0",{"$f":"IF(VLOOKUP(D56,'Prog Assums'!N$6:V$92,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S56>0,ROUNDDOWN((S56-VLOOKUP(AU56,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU56,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":""},null,{"$f":"VLOOKUP(D56,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},null,0,0,null,null,null,null,0,null,{"$f":"IF(D56=\"-\",0,VLOOKUP(D56,'Prog Assums'!N$5:X$271,11,FALSE))","v":0},"",null,null,null,null,{"$f":"IF(AK56>0,83,0)","v":0},null,0,null,null,{"$f":"IF(U56>0,VLOOKUP(D56,'Prog Assums'!$N$6:$T$169,6,FALSE)+IF(U56>1,(U56-1)*VLOOKUP(D56,'Prog Assums'!$N$6:$T$169,7,FALSE),0),0)","v":0},"",{"$f":"ROUNDDOWN((AQ56-VLOOKUP(AU56,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU56,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(D56,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},{"$f":"ROUNDUP(VLOOKUP(AU56,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP56*VLOOKUP(AU56,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":{"$error":"#N/A"}},0,null,{"$f":"VLOOKUP(D56,'Prog Assums'!$N$65:$O$87,2,FALSE)","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N56,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N56,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N56)","v":0},"",null,"",0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S56>0,VLOOKUP($D56,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S56>0,VLOOKUP($D56,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"VLOOKUP(D56,'Prog Assums'!$N$6:$Q$229,3,0)","v":0},{"$f":"VLOOKUP(D56,'Prog Assums'!$N$6:$Q$229,4,0)","v":0},0,0,0,0,0,0,0,0,20,null,null,{"$f":"MAXA(0,(DD49+DE49)-DD50-DD51-DD52-DD53-DD54-DD55)","v":0},null,{"$f":"MAXA(0,DF49-DF50-DF51-DF52-DF53-DF54-DF55)","v":0},{"$f":"MAXA(0,DG49-DG50-DG51-DG52-DG53-DG54-DG55)","v":0},0,0,{"$f":"MAXA(0,DJ49-DJ50-DJ51-DJ52-DJ53-DJ54-DJ55)","v":1},{"$f":"MAXA(0,DK49-DK50-DK51-DK52-DK53-DK54-DK55)","v":1},1,1,{"$f":"VLOOKUP($C56,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C56,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C56,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI56,VLOOKUP($C56,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C56,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C56,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},0,null,0,0,null,null,0,null,null,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY56:$YD56,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY56:$YD56)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S57>0,VLOOKUP($D57,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S57>0,VLOOKUP($D57,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(ER57:FZ57)","v":0},null,null,null,null,null,null,{"$f":"SUM(EY57:GG57)","v":0}]
[null,null,null,"PE basic teaching spaces",null,null,null,null,null,null,{"$f":"'curriculum analysis (optional)'!AO150","v":0},"All PE Spaces",null,null,null,null,null,null,null,null,{"$f":"U59+U60+U64+U65+U66+U67","v":3},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AK59+AK60+AK64+AK65+AK66+AK67","v":3},null,null,null,null,null,null,null,null,null,null,{"$f":"((AW$4*AY$4)+(AV5/DA2)+(AW$6*AY$6)+(AW$8*AY$8))/(AY$4+AY$5+AY$6+AY$8)","v":24.657142857142855},{"$f":"(U58*AV58)/K$8","v":6.5752380952380937E-2},"of curriculum in all indoor PE",null,null,null,null,null,null,null,null,{"$f":"BG59+BG60+BG64+BG65+BG66+BG67","v":3},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S58>0,VLOOKUP($D58,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S58>0,VLOOKUP($D58,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"DD59+DD64+DD65+DD66","v":3},null,{"$f":"DF59+DF64+DF65+DF66","v":3},4,3,3,0,0,0,0,null,null,null,null,null,"All PE Spaces",null,{"$f":"SUM(EA58,EG58,EM58,ET58)-U58","v":-3},null,null,null,null,null,{"$f":"SUM(EA59:EA67)","v":0},{"$f":"SUM(EB59+EB60)","v":0},null,null,null,null,{"$f":"SUM(EG59:EG67)","v":0},{"$f":"SUM(EH59+EH60)","v":0},null,null,null,null,{"$f":"SUM(EM59:EM67)","v":0},{"$f":"SUM(EN59+EN60)","v":0},null,null,null,null,null,{"$f":"SUM(ET59:ET67)","v":0},{"$f":"SUM(EU59+EU60)","v":0}]
[{"$f":"VLOOKUP($D59,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D59,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},{"$f":"IF(U59>0,\"Fitness rooms (exercise studio)\",\"-\")","v":"-"},null,null,null,null,null,null,null,null,{"$f":"IF(D59=\"\",\"\",_xlfn.XLOOKUP(D59,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},{"$f":"CONCATENATE(M59,S59)","v":"-0"},{"$f":"IF(VLOOKUP(D59,'Prog Assums'!N$6:V$92,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S59>0,ROUND((S59-VLOOKUP(AU59,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU59,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":""},null,{"$f":"VLOOKUP(D59,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},null,{"$f":"AK59","v":0},{"$f":"MAXA(0,(S59*U59)-Y59)","v":0},null,null,null,null,0,null,{"$f":"IF(D59=\"-\",0,VLOOKUP(D59,'Prog Assums'!N$5:X$271,11,FALSE))","v":0},{"$f":"IF(D59=\"-\",\"\",\"m2 minimum size for 30 pupils\")","v":""},null,null,null,null,{"$f":"IF(AK59>0,69,0)","v":0},null,{"$f":"DD59+DE59+DC59","v":0},null,null,{"$f":"IF(U59>0,VLOOKUP(D59,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",{"$f":"ROUNDDOWN((AQ59-VLOOKUP(AU59,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU59,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(D59,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},{"$f":"ROUNDUP(VLOOKUP(AU59,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP59*VLOOKUP(AU59,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":{"$error":"#DIV/0!"}},0,null,{"$f":"IF(D59=\"-\",\"-\",VLOOKUP(D59,'Prog Assums'!N90:Q92,2,FALSE))","v":"-"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N59,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N59,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N59)","v":0},{"$f":"IF(ISERROR(BE59*BG59)=TRUE,\"\",BE59*BG59)","v":""},null,{"$f":"IF(ISERROR(BH59-Y59-V59)=TRUE,\"\",BH59-Y59-V59)","v":""},0,null,{"$f":"SUM(BO59:CK59)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U59","v":0},null,null,null,null,null,null,null,{"$f":"IF($S59>0,VLOOKUP($D59,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S59>0,VLOOKUP($D59,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"VLOOKUP(D59,'Prog Assums'!$N$6:$Q$229,3,0)","v":0},{"$f":"VLOOKUP(D59,'Prog Assums'!$N$6:$Q$229,4,0)","v":0},0,{"$f":"IF(CS59>14,IF(CS59<31,CS59,ROUNDDOWN(CS59/30,0)*30),0)","v":0},{"$f":"IF(S59>0,(V59/S59)*CT59,0)","v":0},{"$f":"IF(CS59>0,(V59/S59)*CS59,0)-CU59","v":0},{"$f":"IF(AK59=0,0,MAXA(1,ROUNDUP((AI59/CQ59)-CR59,0)))","v":0},{"$f":"IF(CW59>14,IF(CW59<31,CW59,ROUNDDOWN(CW59/30,0)*30),0)","v":0},{"$f":"IF(AK59>0,(AS59/AI59)*CX59,0)","v":0},{"$f":"IF(CW59>0,(AS59/AI59)*CW59,0)-CY59","v":0},30,null,null,{"$f":"HLOOKUP(AG$12,$DF$15:$DI$74,45,FALSE)","v":0},null,null,1,null,null,null,null,null,null,{"$f":"VLOOKUP($C59,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C59,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C59,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI59,VLOOKUP($C59,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C59,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C59,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},{"$f":"IF(ISERROR((SUM($EB59,$EH59,$EN59,$EU59)/SUM($EA59,$EG59,$EM59,$ET59)-$S59))=TRUE,0,IF($U59=0,0,(SUM($EB59,$EH59,$EN59,$EU59)/SUM($EA59,$EG59,$EM59,$ET59)-$S59)))","v":0},null,{"$f":"SUM(EA59,EG59,EM59,ET59)-U59","v":0},{"$f":"SUM($EU59,$EN59,$EH59,$EB59)-$V59-$Y59","v":0},null,null,0,null,0,{"$f":"EA59*DY59","v":0},null,null,0,null,0,{"$f":"EG59*EE59","v":0},null,null,{"$f":"IF(EN59>0,SUM(EN59/EM59),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY59:$YD59,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY59:$YD59)","v":0},null,null,null,{"$f":"IF(EU59>0,SUM(EU59/ET59),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY59:$YD59,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY59:$YD59)","v":0}]
[{"$f":"VLOOKUP($D60,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D60,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},"-",null,null,null,null,null,null,null,null,{"$f":"IF(D60=\"\",\"\",_xlfn.XLOOKUP(D60,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},{"$f":"CONCATENATE(M60,S60)","v":"-0"},{"$f":"IF(VLOOKUP(D60,'Prog Assums'!N$6:V$92,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S60>0,ROUND((S60-VLOOKUP(AU60,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU60,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"\")","v":""},null,{"$f":"VLOOKUP(D60,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},null,{"$f":"AK60","v":0},{"$f":"MAXA(0,(S60*U60)-Y60)","v":0},null,null,null,null,0,null,{"$f":"IF(D60=\"-\",0,VLOOKUP(D60,'Prog Assums'!N$5:X$271,11,FALSE))","v":0},"",null,null,null,null,null,null,null,null,null,{"$f":"IF(U60>0,VLOOKUP(D60,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",{"$f":"ROUNDDOWN((AQ60-VLOOKUP(AU60,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU60,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(D60,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},{"$f":"ROUNDUP(VLOOKUP(AU60,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP60*VLOOKUP(AU60,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":{"$error":"#DIV/0!"}},0,null,{"$f":"IF(D60=\"-\",\"-\",VLOOKUP(D60,'Prog Assums'!N90:Q92,2,FALSE))","v":"-"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N60,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N60,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N60)","v":0},{"$f":"IF(ISERROR(BE60*BG60)=TRUE,\"\",BE60*BG60)","v":""},null,{"$f":"IF(ISERROR(BH60-Y60-V60)=TRUE,\"\",BH60-Y60-V60)","v":""},0,null,{"$f":"SUM(BO60:CK60)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U60","v":0},null,null,null,null,null,null,null,{"$f":"IF($S60>0,VLOOKUP($D60,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S60>0,VLOOKUP($D60,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"VLOOKUP(D60,'Prog Assums'!$N$6:$Q$229,3,0)","v":0},{"$f":"VLOOKUP(D60,'Prog Assums'!$N$6:$Q$229,4,0)","v":0},0,{"$f":"IF(CS60>14,IF(CS60<31,CS60,ROUNDDOWN(CS60/30,0)*30),0)","v":0},{"$f":"IF(S60>0,(V60/S60)*CT60,0)","v":0},{"$f":"IF(CS60>0,(V60/S60)*CS60,0)-CU60","v":0},0,0,0,0,25,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C60,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C60,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C60,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI60,VLOOKUP($C60,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C60,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C60,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},{"$f":"IF(ISERROR((SUM($EB60,$EH60,$EN60,$EU60)/SUM($EA60,$EG60,$EM60,$ET60)-$S60))=TRUE,0,IF($U60=0,0,(SUM($EB60,$EH60,$EN60,$EU60)/SUM($EA60,$EG60,$EM60,$ET60)-$S60)))","v":0},null,{"$f":"SUM(EA60,EG60,EM60,ET60)-U60","v":0},{"$f":"SUM($EU60,$EN60,$EH60,$EB60)-$V60-$Y60","v":0},null,null,0,null,0,{"$f":"EA60*DY60","v":0},null,null,0,null,0,{"$f":"EG60*EE60","v":0},null,null,{"$f":"IF(EN60>0,SUM(EN60/EM60),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY60:$YD60,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY60:$YD60)","v":0},null,null,null,{"$f":"IF(EU60>0,SUM(EU60/ET60),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY60:$YD60,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY60:$YD60)","v":0}]
[null,null,null,"TOTAL AREA ",null,null,null,null,null,null,null,"BB103 range",null,null,{"$f":"ROUND(IF(AR$8>0,0,0)+IF(K$6>0,0,0)+(K$4*2)+(K$5*2.9)+(K$6*3.2),0)","v":3330},"to",{"$f":"ROUND(IF(AR$8>0,100,150)+IF(K$5>0,100,0)+(K$4*2.2)+(K$5*3.2)+(K$6*3.5),0)","v":3918},null,null,null,null,{"$f":"SUM(V20:V60)","v":3573},null,null,{"$f":"SUM(Y20:Y60)","v":0},null,{"$f":"SUM(AA20:AA60)","v":0},null,{"$f":"IF(V61<O61,\"ERROR: total area for category is too low\",IF(V61>Q61,\"WARNING: total area for category is high\",\"OK: area within BB103 range\"))","v":"OK: area within BB103 range"},null,null,null,null,null,{"$f":"SUM(AS20:AS60)","v":3573},null,{"$f":"SUM(AT20:AT60)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(BH20:BH60)","v":0},null,{"$f":"BH61-Y61-V61","v":-3573},null,null,null,null,{"$f":"SUM(BO20:BO60)","v":9},null,{"$f":"SUM(BQ20:BQ60)","v":9},null,{"$f":"SUM(BS20:BS60)","v":7},null,{"$f":"SUM(BU20:BU60)","v":5},null,{"$f":"SUM(BW20:BW60)","v":4},null,{"$f":"SUM(BY20:BY60)","v":10},null,{"$f":"SUM(CA20:CA60)","v":7},null,{"$f":"SUM(CC20:CC60)","v":2},null,{"$f":"SUM(CE20:CE60)","v":0},null,{"$f":"SUM(CG20:CG60)","v":0},null,{"$f":"SUM(CI20:CI60)","v":0},null,{"$f":"SUM(CK20:CK60)","v":0},null,{"$f":"IF($S61>0,VLOOKUP($D61,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(EU61,EN61,EH61,EB61)-SUM(Y61,V61)","v":-3573},null,null,null,null,null,{"$f":"SUM(EB58,EB49,EB43,EB38,EB31,EB26,EB19)","v":0},null,null,null,null,null,{"$f":"SUM(EH58,EH49,EH43,EH38,EH31,EH26,EH19)","v":0},null,null,null,null,null,{"$f":"SUM(EN58,EN49,EN43,EN38,EN31,EN26,EN19)","v":0},null,null,null,null,null,null,{"$f":"SUM(EU58,EU49,EU43,EU38,EU31,EU26,EU19)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S62>0,VLOOKUP($D62,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S62>0,VLOOKUP($D62,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""}]
[null,null,null,"Large spaces: halls and indoor PE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"main hall options",null,null,null,{"$f":"IF(K8<900,\"hall including stage\",\"hall with bleacher seating\")","v":"hall with bleacher seating"},null,null,null,null,null,null,{"$f":"VLOOKUP(AG67,'Prog Assums'!B98:E103,3,FALSE)","v":2.6700000000000004},"sittings",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S63>0,VLOOKUP($D63,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S63>0,VLOOKUP($D63,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AN10=\"hall\",ROUND((AI64-2)*AN63,0)/(K8*0.95),1-AC69)","v":0.52044444444444449}]
[{"$f":"VLOOKUP($D64,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"HAL01"},null,{"$f":"VLOOKUP($D64,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"HAL03"},{"$f":"VLOOKUP(AG63,'Prog Assums'!B107:C108,2,FALSE)","v":"Assembly halls, secondary (with bleachers)"},null,null,null,null,null,null,null,null,{"$f":"D64","v":"Assembly halls, secondary (with bleachers)"},{"$f":"CONCATENATE(M64,S64)","v":"Assembly halls, secondary (with bleachers)197"},null,null,{"$f":"IF(S64>0,IF(D64=\"main hall (secondary, including stage)\",ROUNDUP((S64-45)/0.6,0),ROUNDUP((S64-25)/0.55,0)),0)","v":313},null,{"$f":"AI64","v":197},null,1,{"$f":"MAXA((S64*U64)-Y64,0)","v":197},null,null,null,null,{"$f":"IF(O64=\"retained\",V64+Y64,IF(O64=\"refurb'ed\",V64+Y64,0))","v":0},null,{"$f":"IF(AN10=\"hall\",ROUND((S64-2)*AN63,0)/(K8*0.95),MAXA(0,1-AC69))","v":0.52044444444444449},{"$f":"IF(AN10=\"hall\",\"of pupils incl 33% eating hot food\",\"of pupils eating cold food at lunch\")","v":"of pupils eating cold food at lunch"},null,null,null,null,{"$f":"IF(AN10=\"hall\",MAXA(AC68,DB64),DB64)","v":197},null,1,null,null,null,null,null,180,320,197,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N64,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N64,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N64)","v":1},{"$f":"IF(ISERROR(BE64*BG64)=TRUE,\"\",BE64*BG64)","v":""},null,{"$f":"IF(ISERROR(BH64-Y64-V64)=TRUE,\"\",BH64-Y64-V64)","v":""},{"$f":"BG64-U64","v":0},null,{"$f":"SUM(BO64:CK64)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,{"$f":"IF($S64>0,VLOOKUP($D64,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":0},{"$f":"IF($S64>0,VLOOKUP($D64,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"IF(S64<75,2.5,12.5)","v":12.5},{"$f":"IF(S64<75,4,-20)","v":-20},36,{"$f":"IF(CS64>14,IF(CS64<31,CS64,ROUNDDOWN(CS64/30,0)*30),0)","v":30},{"$f":"IF(S64>0,(V64/S64)*CT64,0)","v":30},{"$f":"IF(CS64>0,(V64/S64)*CS64,0)-CU64","v":6},{"$f":"IF(AK64=0,0,MAXA(1,ROUNDUP((AI64/CQ64)-CR64,0)))","v":36},{"$f":"IF(CW64>14,IF(CW64<31,CW64,ROUNDDOWN(CW64/30,0)*30),0)","v":30},{"$f":"IF(AK64>0,(AS64/AI64)*CX64,0)","v":30},{"$f":"IF(CW64>0,(AS64/AI64)*CW64,0)-CY64","v":6},null,{"$f":"VLOOKUP(DA2,'Prog Assums'!E58:I71,5,FALSE)","v":197},{"$f":"VLOOKUP(DA2+1,'Prog Assums'!E57:I71,5,FALSE)","v":226},1,{"$f":"IF(K7>0,\"add\",0)","v":0},1,1,1,1,null,null,null,null,{"$f":"VLOOKUP($C64,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":120},{"$f":"VLOOKUP($C64,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C64,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI64,VLOOKUP($C64,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":197},{"$f":"VLOOKUP($C64,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C64,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":600},{"$f":"IF(ISERROR((SUM($EB64,$EH64,$EN64,$EU64)/SUM($EA64,$EG64,$EM64,$ET64)-$S64))=TRUE,0,IF($U64=0,0,(SUM($EB64,$EH64,$EN64,$EU64)/SUM($EA64,$EG64,$EM64,$ET64)-$S64)))","v":0},null,{"$f":"SUM(EA64,EG64,EM64,ET64)-U64","v":-1},{"$f":"SUM($EU64,$EN64,$EH64,$EB64)-$V64-$Y64","v":-197},null,null,0,null,null,{"$f":"EA64*DY64","v":0},null,null,0,null,0,{"$f":"EG64*EE64","v":0},null,null,{"$f":"IF(EN64>0,SUM(EN64/EM64),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY64:$YD64,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY64:$YD64)","v":0},null,null,null,{"$f":"IF(EU64>0,SUM(EU64/ET64),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY64:$YD64,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY64:$YD64)","v":0}]
[{"$f":"VLOOKUP($D65,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"SPH00"},null,{"$f":"VLOOKUP($D65,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"SPH04"},{"$f":"AF65","v":"Sports halls, school (4-court)"},null,null,null,null,null,null,null,null,{"$f":"IF(D65=\"\",\"\",_xlfn.XLOOKUP(D65,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Sports hall, school (4-court)"},{"$f":"CONCATENATE(M65,S65)","v":"Sports hall, school (4-court)594"},{"$f":"IF(VLOOKUP(D65,'Prog Assums'!N$92:V$133,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S65>0,IF((S65-15)/1.75>(K5/O5),ROUNDUP((K5*1.033/O5),0),ROUNDDOWN((S65-15)/1.75,0)),0)","v":186},null,{"$f":"VLOOKUP(D65,'Prog Assums'!N$5:U$271,5,FALSE)","v":594},null,{"$f":"AK65","v":1},{"$f":"MAXA((S65*U65)-Y65,0)","v":594},null,null,{"$f":"IF((S65*U65)>594,(S65*U65)-594,0)","v":0},null,{"$f":"IF(O65=\"retained\",V65+Y65,IF(O65=\"refurb'ed\",V65+Y65,0))","v":0},null,"recommended:",null,null,{"$f":"VLOOKUP(AI65,'Prog Assums'!M119:N124,2)","v":"Sports halls, school (4-court)"},null,null,{"$f":"IF(K8>599,MAXA(504,DB65),DB65)","v":594},null,1,null,null,{"$f":"IF(U65>0,VLOOKUP(D65,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},{"$f":"IF(O65=\"existing\",\"E\",\"\")","v":""},null,{"$f":"VLOOKUP(D65,'Prog Assums'!N$5:U$271,5,FALSE)","v":594},900,594,null,null,{"$f":"DK65","v":0},null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N65,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N65,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N65)","v":1},{"$f":"IF(ISERROR(BE65*BG65)=TRUE,\"\",BE65*BG65)","v":""},null,{"$f":"IF(ISERROR(BH65-Y65-V65)=TRUE,\"\",BH65-Y65-V65)","v":""},0,null,{"$f":"SUM(BO65:CK65)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U65","v":1},null,null,null,null,null,null,null,{"$f":"IF($S65>0,VLOOKUP($D65,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"594m2"},{"$f":"IF($S65>0,VLOOKUP($D65,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"IF(S65<75,2.5,12.5)","v":12.5},{"$f":"IF(S65<75,4,-20)","v":-20},68,{"$f":"IF(CS65>14,IF(CS65<31,CS65,ROUNDDOWN(CS65/30,0)*30),0)","v":60},{"$f":"IF(S65>0,(V65/S65)*CT65,0)","v":60},{"$f":"IF(CS65>0,(V65/S65)*CS65,0)-CU65","v":8},68,60,60,8,60,{"$f":"VLOOKUP(DA2+DC65,'Prog Assums'!E58:I71,4,FALSE)","v":594},{"$f":"IF(VLOOKUP(AG67,'Prog Assums'!B98:G103,6,FALSE)=\"space\",0,1)","v":0},1,null,1,1,1,1,null,null,null,null,{"$f":"VLOOKUP($C65,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":594},{"$f":"VLOOKUP($C65,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C65,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI65,VLOOKUP($C65,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":594},{"$f":"VLOOKUP($C65,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C65,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":690},{"$f":"IF(ISERROR((SUM($EB65,$EH65,$EN65,$EU65)/SUM($EA65,$EG65,$EM65,$ET65)-$S65))=TRUE,0,IF($U65=0,0,(SUM($EB65,$EH65,$EN65,$EU65)/SUM($EA65,$EG65,$EM65,$ET65)-$S65)))","v":0},null,{"$f":"SUM(EA65,EG65,EM65,ET65)-U65","v":-1},{"$f":"SUM($EU65,$EN65,$EH65,$EB65)-$V65-$Y65","v":-594},null,null,0,null,null,{"$f":"EA65*DY65","v":0},null,null,0,null,0,{"$f":"EG65*EE65","v":0},null,null,{"$f":"IF(EN65>0,SUM(EN65/EM65),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY65:$YD65,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY65:$YD65)","v":0},null,null,null,{"$f":"IF(EU65>0,SUM(EU65/ET65),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY65:$YD65,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY65:$YD65)","v":0}]
[{"$f":"VLOOKUP($D66,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"ACT05"},null,{"$f":"VLOOKUP($D66,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"ACT07"},{"$f":"AF66","v":"Activity studios (10 x 15)"},null,null,null,null,null,null,null,null,{"$f":"IF(D66=\"\",\"\",_xlfn.XLOOKUP(D66,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Activity studio (10 x 15)"},{"$f":"CONCATENATE(M66,S66)","v":"Activity studio (10 x 15)150"},{"$f":"IF(VLOOKUP(D66,'Prog Assums'!N$92:V$133,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S66>0,CT66,0)","v":30},null,{"$f":"VLOOKUP(D66,'Prog Assums'!N$5:U$271,5,FALSE)","v":150},null,{"$f":"AK66","v":1},{"$f":"MAXA((S66*U66)-Y66,0)","v":150},null,null,{"$f":"IF(D66=\"swimming pool (existing)\",S66,0)","v":0},null,0,null,{"$f":"IF(AK66>0,\"recommended:\",\"\")","v":"recommended:"},null,null,{"$f":"IF(AK66>0,IF(K8>1100,IF(K8>1750,\"Activity studios, 1-court\",\"Activity studios (10 x 15)\"),\"Activity studios (10 x 12)\"),\"-\")","v":"Activity studios (10 x 15)"},null,null,{"$f":"VLOOKUP('Secondary SoA'!AF66,'Prog Assums'!N103:R116,5,FALSE)","v":150},null,{"$f":"DD66","v":1},null,null,{"$f":"IF(U66>0,VLOOKUP(D66,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",null,144,180,150,null,null,{"$f":"DK66","v":0},null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N66,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N66,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N66)","v":1},{"$f":"IF(ISERROR(BE66*BG66)=TRUE,\"\",BE66*BG66)","v":""},null,{"$f":"IF(ISERROR(BH66-Y66-V66)=TRUE,\"\",BH66-Y66-V66)","v":""},0,null,{"$f":"SUM(BO66:CK66)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U66","v":1},null,null,null,null,null,null,null,{"$f":"IF($S66>0,VLOOKUP($D66,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"150m2 for 30"},{"$f":"IF($S66>0,VLOOKUP($D66,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,12.5,-20,32,{"$f":"IF(CS66>14,IF(CS66<31,CS66,ROUNDDOWN(CS66/30,0)*30),0)","v":30},{"$f":"IF(S66>0,(V66/S66)*CT66,0)","v":30},{"$f":"IF(CS66>0,(V66/S66)*CS66,0)-CU66","v":2},32,30,30,2,30,{"$f":"VLOOKUP('Secondary SoA'!DA2,'Prog Assums'!E58:I71,3,FALSE)","v":120},null,{"$f":"HLOOKUP(AG$12,$DF$15:$DI$74,52,FALSE)","v":1},null,{"$f":"IF($K7+$K8>801,IF($K7+$K8>1600,2,1),0)","v":1},{"$f":"IF($K8>675,IF($K8>1600,2,1),0)","v":1},{"$f":"IF($K8>675,IF($K8>1600,2,1),0)","v":1},{"$f":"IF($K7+$K8>901,IF($K8>1600,2,1),0)","v":1},null,null,null,null,{"$f":"VLOOKUP($C66,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":150},{"$f":"VLOOKUP($C66,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C66,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI66,VLOOKUP($C66,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":150},{"$f":"VLOOKUP($C66,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C66,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":180},{"$f":"IF(ISERROR((SUM($EB66,$EH66,$EN66,$EU66)/SUM($EA66,$EG66,$EM66,$ET66)-$S66))=TRUE,0,IF($U66=0,0,(SUM($EB66,$EH66,$EN66,$EU66)/SUM($EA66,$EG66,$EM66,$ET66)-$S66)))","v":0},null,{"$f":"SUM(EA66,EG66,EM66,ET66)-U66","v":-1},{"$f":"SUM($EU66,$EN66,$EH66,$EB66)-$V66-$Y66","v":-150},null,null,0,null,null,{"$f":"EA66*DY66","v":0},null,null,0,null,0,{"$f":"EG66*EE66","v":0},null,null,{"$f":"IF(EN66>0,SUM(EN66/EM66),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY66:$YD66,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY66:$YD66)","v":0},null,null,null,{"$f":"IF(EU66>0,SUM(EU66/ET66),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY66:$YD66,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY66:$YD66)","v":0}]
[{"$f":"VLOOKUP($D67,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D67,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},"-",null,null,null,null,null,null,null,null,{"$f":"IF(D67=\"\",\"\",_xlfn.XLOOKUP(D67,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},{"$f":"CONCATENATE(M67,S67)","v":"-0"},{"$f":"IF(VLOOKUP(D67,'Prog Assums'!N$92:V$133,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S67>0,CT67,0)","v":0},null,{"$f":"VLOOKUP(D67,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},null,null,{"$f":"MAXA((S67*U67)-Y67,0)","v":0},null,null,{"$f":"IF(D67=\"swimming pool (existing)\",S67,0)","v":0},null,0,null,"dining",null,null,null,"40 mins in dining area and hall",null,null,null,null,null,null,{"$f":"IF(U67>0,VLOOKUP(D67,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",null,null,null,0,null,null,{"$f":"IF(#REF!>1,DK67,0)","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N67,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N67,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N67)","v":0},{"$f":"IF(ISERROR(BE67*BG67)=TRUE,\"\",BE67*BG67)","v":""},null,{"$f":"IF(ISERROR(BH67-Y67-V67)=TRUE,\"\",BH67-Y67-V67)","v":""},0,null,{"$f":"SUM(BO67:CK67)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U67","v":0},null,null,null,null,null,null,null,{"$f":"IF($S67>0,VLOOKUP($D67,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S67>0,VLOOKUP($D67,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,2.5,4,0,{"$f":"IF(CS67>14,IF(CS67<31,CS67,ROUNDDOWN(CS67/30,0)*30),0)","v":0},{"$f":"IF(S67>0,(V67/S67)*CT67,0)","v":0},{"$f":"IF(CS67>0,(V67/S67)*CS67,0)-CU67","v":0},0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C67,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C67,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C67,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI67,VLOOKUP($C67,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C67,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C67,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},{"$f":"IF(ISERROR((SUM($EB67,$EH67,$EN67,$EU67)/SUM($EA67,$EG67,$EM67,$ET67)-$S67))=TRUE,0,IF($U67=0,0,(SUM($EB67,$EH67,$EN67,$EU67)/SUM($EA67,$EG67,$EM67,$ET67)-$S67)))","v":0},null,{"$f":"SUM(EA67,EG67,EM67,ET67)-U67","v":0},{"$f":"SUM($EU67,$EN67,$EH67,$EB67)-$V67-$Y67","v":0},null,null,0,null,null,{"$f":"EA67*DY67","v":0},null,null,0,null,0,{"$f":"EG67*EE67","v":0},null,null,{"$f":"IF(EN67>0,SUM(EN67/EM67),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY67:$YD67,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY67:$YD67)","v":0},null,null,null,{"$f":"IF(EU67>0,SUM(EU67/ET67),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY67:$YD67,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY67:$YD67)","v":0}]
[null,null,null,"Dining and Social Areas",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ROUNDUP(K8*(0.95/AN63),0)+10","v":411},"m2 min. recom'd for all pupils dining ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AC68*0.4","v":164.4},"needed for 1/3 of pupils to eat hot meals",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S68>0,VLOOKUP($D68,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S68>0,VLOOKUP($D68,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""}]
[{"$f":"VLOOKUP($D69,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"DIN01"},null,{"$f":"VLOOKUP($D69,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"DIN01"},{"$f":"VLOOKUP(AG67,'Prog Assums'!B98:E103,4,FALSE)","v":"Dining halls"},null,null,null,null,null,null,null,null,{"$f":"IF(D69=\"\",\"\",_xlfn.XLOOKUP(D69,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Dining hall"},{"$f":"CONCATENATE(M69,S69)","v":"Dining hall214"},null,null,{"$f":"IF(S69>0,ROUND((S69-2)/0.95,0),0)","v":223},null,{"$f":"AI69","v":214},null,{"$f":"AK69","v":1},{"$f":"MAXA((S69*U69)-Y69,0)","v":214},null,null,null,null,0,null,{"$f":"IF(AN10=\"hall\",\"\",IF(V69>AU68,0.34+ROUND((V69-AU68)/(0.95/ROUNDUP(AN63,0)),0)/K8,0))","v":0.47955555555555557},{"$f":"IF(D69=\"Dining halls\",IF(V69>AU68,\"of pupils incl 33% eating hot food\",\"too small for 1/3 of pupils to eat hot food\"),\"for pupil access to servery\")","v":"of pupils incl 33% eating hot food"},null,null,null,null,{"$f":"IF(AN10=\"hall\",20,ROUND(MAXA(0,O73-AS64-AS65-AS66-AS70,5+IF(AI70>1,0,(K8*0.2)),MINA(AC68,O168-AI61-AI95-AI130-AI165-AS64-AS65-AS66-AS70,Q73-AS64-AS65-AS66-AS70)),0))","v":214},null,{"$f":"IF(AI69>0,1,0)","v":1},null,null,{"$f":"IF(U69>0,VLOOKUP(D69,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",null,{"$f":"5+ROUND((K5+K6)*0.25,0)","v":286},{"$f":"10+ROUND((K5+K6)*0.35,0)","v":404},214,null,{"$f":"AC68*0.6","v":246.6},"needed for 2/3 of pupils to eat cold meals",null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N69,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N69,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N69)","v":0},{"$f":"IF(ISERROR(BE69*BG69)=TRUE,\"\",BE69*BG69)","v":""},null,{"$f":"IF(ISERROR(BH69-Y69-V69)=TRUE,\"\",BH69-Y69-V69)","v":""},-1,null,{"$f":"SUM(BO69:CK69)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U69","v":1},null,null,null,null,null,null,null,null,null,{"$f":"IF($S69>0,VLOOKUP($D69,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":0},{"$f":"IF($S69>0,VLOOKUP($D69,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"IF(D69=\"Dining halls\",IF(S69<75,2.5,12.5),IF(S70>90,2.5,1.5))","v":12.5},{"$f":"IF(D69=\"Dining halls\",IF(S69<75,4,-20),IF(S70>90,-20,4))","v":-20},38,{"$f":"IF(CS69>14,IF(CS69<31,CS69,ROUNDDOWN(CS69/30,0)*30),0)","v":30},{"$f":"IF(S69>0,(V69/S69)*CT69,0)","v":30},{"$f":"IF(CS69>0,(V69/S69)*CS69,0)-CU69","v":8},{"$f":"IF(AK69=0,0,MAXA(1,ROUNDUP((AI69/CQ69)-CR69,0)))","v":38},{"$f":"IF(CW69>14,IF(CW69<31,CW69,ROUNDDOWN(CW69/30,0)*30),0)","v":30},{"$f":"IF(AK69>0,(AS69/AI69)*CX69,0)","v":30},{"$f":"IF(CW69>0,(AS69/AI69)*CW69,0)-CY69","v":8},"N/4",{"$f":"70+ROUND(K8*0.2,0)-DB70","v":256},null,{"$f":"IF(AN10=\"hall\",\"\",IF(AI69>AU68,0.33+ROUND((AI69-AU68)/(0.95/ROUNDUP(AN63,0)),0)/K8,0))","v":0.46955555555555556},"add",null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C69,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":12},{"$f":"VLOOKUP($C69,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C69,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI69,VLOOKUP($C69,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":214},{"$f":"VLOOKUP($C69,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C69,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":600},{"$f":"IF(ISERROR((SUM($EB69,$EH69,$EN69,$EU69)/SUM($EA69,$EG69,$EM69,$ET69)-$S69))=TRUE,0,IF($U69=0,0,(SUM($EB69,$EH69,$EN69,$EU69)/SUM($EA69,$EG69,$EM69,$ET69)-$S69)))","v":0},null,{"$f":"SUM(EA69,EG69,EM69,ET69)-U69","v":-1},{"$f":"SUM($EU69,$EN69,$EH69,$EB69)-$V69-$Y69","v":-214},null,null,0,null,null,{"$f":"EA69*DY69","v":0},null,null,0,null,0,{"$f":"EG69*EE69","v":0},null,null,{"$f":"IF(EN69>0,SUM(EN69/EM69),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY69:$YD69,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY69:$YD69)","v":0},null,null,null,{"$f":"IF(EU69>0,SUM(EU69/ET69),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY69:$YD69,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY69:$YD69)","v":0}]
[{"$f":"VLOOKUP($D70,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"DIN02"},null,{"$f":"VLOOKUP($D70,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"DIN02"},"Informal dining spaces",null,null,null,null,null,null,null,null,{"$f":"IF(D70=\"\",\"\",_xlfn.XLOOKUP(D70,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Informal dining space"},{"$f":"CONCATENATE(M70,S70)","v":"Informal dining space111"},{"$f":"IF(VLOOKUP(D70,'Prog Assums'!N$92:V$133,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S70>0,ROUND((S70-VLOOKUP(AU70,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU70,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":99},null,{"$f":"AI70","v":111},null,{"$f":"AK70","v":1},{"$f":"MAXA((S70*U70)-Y70,0)","v":111},null,null,null,null,0,null,{"$f":"IF(AK70>0,\"recommended:\",\"\")","v":"recommended:"},null,null,{"$f":"IF(AK70>0,\"Social spaces (sixth form)\",\"-\")","v":"Social spaces (sixth form)"},null,null,{"$f":"IF(K6>0,41+ROUND((K6*0.3)/7,0)*7,0)","v":111},null,{"$f":"IF(K6>0,1,0)","v":1},null,null,{"$f":"IF(U70>0,VLOOKUP(D70,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",null,0,null,111,null,{"$f":"VLOOKUP(D70,'Prog Assums'!$N$92:$O$99,2,FALSE)","v":"A"},{"$f":"IF(AD70>1,DK70,0)","v":0},null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N70,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N70,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N70)","v":1},{"$f":"IF(ISERROR(BE70*BG70)=TRUE,\"\",BE70*BG70)","v":""},null,{"$f":"IF(ISERROR(BH70-Y70-V70)=TRUE,\"\",BH70-Y70-V70)","v":""},0,null,{"$f":"SUM(BO70:CK70)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U70","v":1},null,{"$f":"IF($S70>0,VLOOKUP($D70,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":0},{"$f":"IF($S70>0,VLOOKUP($D70,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"IF(S70>90,2.5,1.5)","v":2.5},{"$f":"IF(S70>90,-20,4)","v":-20},65,{"$f":"IF(CS70>14,IF(CS70<31,CS70,ROUNDDOWN(CS70/30,0)*30),0)","v":60},{"$f":"IF(S70>0,(V70/S70)*CT70,0)","v":60},{"$f":"IF(CS70>0,(V70/S70)*CS70,0)-CU70","v":5},65,60,60,5,null,{"$f":"20+ROUND(K8/60,0)","v":39},null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C70,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":12},{"$f":"VLOOKUP($C70,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C70,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI70,VLOOKUP($C70,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":55},{"$f":"VLOOKUP($C70,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C70,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":600},{"$f":"IF(ISERROR((SUM($EB70,$EH70,$EN70,$EU70)/SUM($EA70,$EG70,$EM70,$ET70)-$S70))=TRUE,0,IF($U70=0,0,(SUM($EB70,$EH70,$EN70,$EU70)/SUM($EA70,$EG70,$EM70,$ET70)-$S70)))","v":0},null,{"$f":"SUM(EA70,EG70,EM70,ET70)-U70","v":-1},{"$f":"SUM($EU70,$EN70,$EH70,$EB70)-$V70-$Y70","v":-111},null,null,0,null,null,{"$f":"EA70*DY70","v":0},null,null,0,null,0,{"$f":"EG70*EE70","v":0},null,null,{"$f":"IF(EN70>0,SUM(EN70/EM70),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY70:$YD70,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY70:$YD70)","v":0},null,null,null,{"$f":"IF(EU70>0,SUM(EU70/ET70),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY70:$YD70,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY70:$YD70)","v":0}]
[{"$f":"VLOOKUP($D71,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D71,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},"-",null,null,null,null,null,null,null,null,{"$f":"IF(D71=\"\",\"\",_xlfn.XLOOKUP(D71,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},{"$f":"CONCATENATE(M71,S71)","v":"-"},{"$f":"IF(VLOOKUP(D71,'Prog Assums'!N$92:V$133,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S71>0,ROUND((S71-VLOOKUP(AU71,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU71,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":"-"},null,null,null,null,{"$f":"MAXA((S71*U71)-Y71,0)","v":0},null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(U71>0,VLOOKUP(D71,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",null,null,null,0,null,{"$f":"VLOOKUP(D71,'Prog Assums'!$N$92:$O$99,2,FALSE)","v":"-"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N71,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N71,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N71)","v":0},{"$f":"IF(ISERROR(BE71*BG71)=TRUE,\"\",BE71*BG71)","v":""},null,{"$f":"IF(ISERROR(BH71-Y71-V71)=TRUE,\"\",BH71-Y71-V71)","v":""},0,null,{"$f":"SUM(BO71:CK71)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U71","v":0},null,{"$f":"IF($S71>0,VLOOKUP($D71,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S71>0,VLOOKUP($D71,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"IF(S71>90,2.5,1.5)","v":1.5},{"$f":"IF(S71>90,-20,4)","v":4},0,{"$f":"IF(CS71>14,IF(CS71<31,CS71,ROUNDDOWN(CS71/30,0)*30),0)","v":0},{"$f":"IF(S71>0,(V71/S71)*CT71,0)","v":0},{"$f":"IF(CS71>0,(V71/S71)*CS71,0)-CU71","v":0},0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C71,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C71,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C71,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI71,VLOOKUP($C71,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C71,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C71,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},{"$f":"IF(ISERROR((SUM($EB71,$EH71,$EN71,$EU71)/SUM($EA71,$EG71,$EM71,$ET71)-$S71))=TRUE,0,IF($U71=0,0,(SUM($EB71,$EH71,$EN71,$EU71)/SUM($EA71,$EG71,$EM71,$ET71)-$S71)))","v":0},null,{"$f":"SUM(EA71,EG71,EM71,ET71)-U71","v":0},{"$f":"SUM($EU71,$EN71,$EH71,$EB71)-$V71-$Y71","v":0},null,null,0,null,0,{"$f":"EA71*DY71","v":0},null,null,0,null,0,{"$f":"EG71*EE71","v":0},null,null,{"$f":"IF(EN71>0,SUM(EN71/EM71),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY71:$YD71,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY71:$YD71)","v":0},null,null,null,{"$f":"IF(EU71>0,SUM(EU71/ET71),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY71:$YD71,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY71:$YD71)","v":0}]
[{"$f":"VLOOKUP($D72,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D72,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},"-",null,null,null,null,null,null,null,null,{"$f":"IF(D72=\"\",\"\",_xlfn.XLOOKUP(D72,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},{"$f":"CONCATENATE(M72,S72)","v":"-"},{"$f":"IF(VLOOKUP(D72,'Prog Assums'!N$92:V$133,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S72>0,ROUND((S72-VLOOKUP(AU72,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU72,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":"-"},null,null,null,null,{"$f":"MAXA((S72*U72)-Y72,0)","v":0},null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(U72>0,VLOOKUP(D72,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",null,{"$f":"IF(K6>0,50+ROUND(K6*0.3,0),0)","v":118},null,0,null,{"$f":"VLOOKUP(D72,'Prog Assums'!$N$92:$O$99,2,FALSE)","v":"-"},{"$f":"IF(AD72>1,DK72,0)","v":0},null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N72,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N72,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N72)","v":0},{"$f":"IF(ISERROR(BE72*BG72)=TRUE,\"\",BE72*BG72)","v":""},null,{"$f":"IF(ISERROR(BH72-Y72-V72)=TRUE,\"\",BH72-Y72-V72)","v":""},0,null,{"$f":"SUM(BO72:CK72)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,{"$f":"IF($S72>0,VLOOKUP($D72,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S72>0,VLOOKUP($D72,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,1.5,4,0,{"$f":"IF(CS72>14,IF(CS72<31,CS72,ROUNDDOWN(CS72/30,0)*30),0)","v":0},{"$f":"IF(S72>0,(V72/S72)*CT72,0)","v":0},{"$f":"IF(CS72>0,(V72/S72)*CS72,0)-CU72","v":0},0,0,0,0,null,{"$f":"IF(K6>0,50+ROUND(K6*0.3,0),0)","v":118},null,null,{"$f":"IF(K$6>0,1,0)","v":1},null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C72,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C72,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C72,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI72,VLOOKUP($C72,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C72,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C72,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},{"$f":"IF(ISERROR((SUM($EB72,$EH72,$EN72,$EU72)/SUM($EA72,$EG72,$EM72,$ET72)-$S72))=TRUE,0,IF($U72=0,0,(SUM($EB72,$EH72,$EN72,$EU72)/SUM($EA72,$EG72,$EM72,$ET72)-$S72)))","v":0},null,{"$f":"SUM(EA72,EG72,EM72,ET72)-U72","v":0},{"$f":"SUM($EU72,$EN72,$EH72,$EB72)-$V72-$Y72","v":0},null,null,0,null,0,{"$f":"EA72*DY72","v":0},null,null,0,null,0,{"$f":"EG72*EE72","v":0},null,null,{"$f":"IF(EN72>0,SUM(EN72/EM72),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY72:$YD72,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY72:$YD72)","v":0},null,null,null,{"$f":"IF(EU72>0,SUM(EU72/ET72),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY72:$YD72,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY72:$YD72)","v":0}]
[null,null,null,"TOTAL AREA ",null,null,null,null,null,null,null,"BB103 range","BB103 range","BB103 range",{"$f":"ROUND(IF(K$4>0,200,300)+IF(K$6>0,75,0)+(K$4*0.3)+((K$5+K$6)*0.6),0)","v":1050},"to",{"$f":"ROUND(IF(K$4>0,450,600)+IF(K$6>0,50,0)+(K$4*0.35)+(K5*0.7)+(K6*0.8),0)","v":1460},null,null,null,null,{"$f":"SUM(V64:V72)","v":1266},null,null,{"$f":"SUM(Y64:Y72)","v":0},null,{"$f":"SUM(AA64:AA72)","v":0},null,{"$f":"IF(V73<O73,\"ERROR: total area for category is too low\",IF(V73>Q73,\"WARNING: total area for category is high\",\"OK: area within BB103 range\"))","v":"OK: area within BB103 range"},null,null,null,null,null,{"$f":"SUM(AS64:AS72)","v":1266},null,{"$f":"SUM(AT64:AT72)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(BH64:BH72)","v":0},null,{"$f":"BH73-Y73-V73","v":-1266},null,null,null,null,{"$f":"SUM(BO64:BO72)","v":0},null,{"$f":"SUM(BQ64:BQ72)","v":0},null,{"$f":"SUM(BS64:BS72)","v":0},null,{"$f":"SUM(BU64:BU72)","v":0},null,{"$f":"SUM(BW64:BW72)","v":0},null,{"$f":"SUM(BY64:BY72)","v":0},null,{"$f":"SUM(CA64:CA72)","v":0},null,{"$f":"SUM(CC64:CC72)","v":2},null,{"$f":"SUM(CE64:CE72)","v":2},null,{"$f":"SUM(CG64:CG72)","v":0},null,{"$f":"SUM(CI64:CI72)","v":0},null,{"$f":"SUM(CK64:CK72)","v":1},null,{"$f":"IF($S73>0,VLOOKUP($D73,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S73>0,VLOOKUP($D73,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(EU73,EN73,EH73,EB73)-SUM(Y73,V73)","v":-1266},null,null,null,null,null,{"$f":"SUM(EB63:EB72)","v":0},null,null,null,null,null,{"$f":"SUM(EH63:EH72)","v":0},null,null,null,null,null,{"$f":"SUM(EN63:EN72)","v":0},null,null,null,null,null,null,{"$f":"SUM(EU63:EU72)","v":0}]
[null,null,null,"Total timetabled spaces",null,null,null,null,null,null,{"$f":"IF(K19+K26+K31+K38+K43+K49+K58>0,K19+K26+K31+K38+K43+K49+K58,\"\")","v":""},null,null,null,null,null,null,null,null,null,{"$f":"U19+U26+U31+U38+U43+U49+U58","v":56},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AK19+AK26+AK31+AK38+AK43+AK49+AK58","v":56},null,null,null,null,null,null,null,null,{"$f":"ROUND(K8*7/150,0)+1","v":54},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BG19+BG26+BG31+BG38+BG43+BG49+BG58","v":56},null,null,null,{"$f":"BG74-U74","v":0},null,{"$f":"SUM(BO74:CK74)","v":56},null,{"$f":"SUM(BO61:BO67)","v":9},null,{"$f":"SUM(BQ61:BQ67)","v":9},null,{"$f":"SUM(BS61:BS67)","v":7},null,{"$f":"SUM(BU61:BU67)","v":5},null,{"$f":"SUM(BW61:BW67)","v":4},null,{"$f":"SUM(BY61:BY67)","v":10},null,{"$f":"SUM(CA61:CA67)","v":7},null,{"$f":"SUM(CC61:CC67)","v":3},null,{"$f":"SUM(CE61:CE67)","v":2},null,{"$f":"SUM(CG61:CG67)","v":0},null,{"$f":"SUM(CI61:CI67)","v":0},null,{"$f":"SUM(CK61:CK67)","v":0},null,{"$f":"IF($S74>0,VLOOKUP($D74,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S74>0,VLOOKUP($D74,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ROUND(K5*7/150,0)+IF(K5>450,1,0)","v":43},{"$f":"IF(K6>0,ROUND(K6*8/150,0)+IF(K6<75,2,1),0)","v":13},{"$f":"DD20+DD27+DD32+DD59+DD50+DD44+DD64+DD65+DD66","v":9},{"$f":"DD18+DD26+DD31+DD38+DD43+DD49+DD58","v":43},13,43,43,43,43,13,13,13,14,null,null,null,null,null,null,null,{"$f":"SUM(EA74,EG74,EM74,ET74)-U74","v":-56},null,null,null,null,null,{"$f":"SUM(EA58+EA49+EA43+EA38+EA31+EA26+EA19)","v":0},null,null,null,null,null,{"$f":"SUM(EG58+EG49+EG43+EG38+EG31+EG26+EG19)","v":0},null,null,null,null,null,{"$f":"SUM(EM58+EM49+EM43+EM38+EM31+EM26+EM19)","v":0},null,null,null,null,null,null,{"$f":"SUM(ET58+ET49+ET43+ET38+ET31+ET26+ET19)","v":0}]
[null,null,null,"Learning Resource Areas",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S75>0,VLOOKUP($D75,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S75>0,VLOOKUP($D75,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""}]
[{"$f":"VLOOKUP($D76,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"LIB05"},null,{"$f":"VLOOKUP($D76,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"LIB05"},"Library resource centres (LRC)",null,null,null,null,null,null,null,null,{"$f":"IF(D76=\"\",\"\",_xlfn.XLOOKUP(D76,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Library resource centre (LRC)"},{"$f":"CONCATENATE(M76,S76)","v":"Library resource centre (LRC)146"},null,null,{"$f":"ROUNDDOWN((S76-VLOOKUP(AU76,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU76,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":55},null,{"$f":"AI76","v":146},null,{"$f":"AK76","v":1},{"$f":"MAXA((S76*U76)-Y76,0)","v":146},null,null,null,null,{"$f":"IF(O76=\"retained\",V76+Y76,IF(O76=\"refurb'ed\",V76+Y76,0))","v":0},null,{"$f":"ROUND(9+(K8*0.12),0)","v":144},"m2 minimum recommended",null,null,null,null,{"$f":"MAXA((ROUNDUP(AC76/7,0)*7)-1,O95-SUM(AS77:AS94))","v":146},null,1,null,null,{"$f":"IF(U76>0,VLOOKUP(D76,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",null,{"$f":"20+(K8*0.1)","v":132.5},{"$f":"50+(K8*0.15)","v":218.75},146,null,"F",null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N76,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N76,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N76)","v":1},{"$f":"IF(ISERROR(BE76*BG76)=TRUE,\"\",BE76*BG76)","v":""},null,{"$f":"IF(ISERROR(BH76-Y76-V76)=TRUE,\"\",BH76-Y76-V76)","v":""},{"$f":"BG76-U76","v":0},null,{"$f":"SUM(BO76:CK76)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U76","v":1},null,{"$f":"IF($S76>0,VLOOKUP($D76,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"[41m2]"},{"$f":"IF($S76>0,VLOOKUP($D76,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"IF(S76>120,3,2)","v":3},{"$f":"IF(S76>120,-16,4)","v":-16},65,{"$f":"IF(CS76>14,IF(CS76<31,CS76,ROUNDDOWN(CS76/30,0)*30),0)","v":60},{"$f":"IF(S76>0,(V76/S76)*CT76,0)","v":60},{"$f":"IF(CS76>0,(V76/S76)*CS76,0)-CU76","v":5},{"$f":"IF(AK76=0,0,MAXA(1,ROUNDUP((AI76/CQ76)-CR76,0)))","v":65},{"$f":"IF(CW76>14,IF(CW76<31,CW76,ROUNDDOWN(CW76/30,0)*30),0)","v":60},{"$f":"IF(AK76>0,(AS76/AI76)*CX76,0)","v":60},{"$f":"IF(CW76>0,(AS76/AI76)*CW76,0)-CY76","v":5},"N/10",{"$f":"ROUND(9+($K8*0.12),0)","v":144},null,null,"add",null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C76,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":12},{"$f":"VLOOKUP($C76,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C76,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI76,VLOOKUP($C76,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":146},{"$f":"VLOOKUP($C76,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C76,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":250},{"$f":"IF(ISERROR((SUM($EB76,$EH76,$EN76,$EU76)/SUM($EA76,$EG76,$EM76,$ET76)-$S76))=TRUE,0,IF($U76=0,0,(SUM($EB76,$EH76,$EN76,$EU76)/SUM($EA76,$EG76,$EM76,$ET76)-$S76)))","v":0},null,{"$f":"SUM(EA76,EG76,EM76,ET76)-U76","v":-1},{"$f":"SUM($EU76,$EN76,$EH76,$EB76)-$V76-$Y76","v":-146},null,null,0,null,null,{"$f":"EA76*DY76","v":0},null,null,0,null,0,{"$f":"EG76*EE76","v":0},null,null,{"$f":"IF(EN76>0,SUM(EN76/EM76),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY76:$YD76,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY76:$YD76)","v":0},null,null,null,{"$f":"IF(EU76>0,SUM(EU76/ET76),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY76:$YD76,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY76:$YD76)","v":0}]
[{"$f":"VLOOKUP($D77,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"LIB07"},null,{"$f":"VLOOKUP($D77,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"LIB06"},{"$f":"IF(K6>0,\"Study spaces, rooms (sixth form)\",\"-\")","v":"Study spaces, rooms (sixth form)"},null,null,null,null,null,null,null,null,{"$f":"IF(D77=\"\",\"\",_xlfn.XLOOKUP(D77,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Study space, room (sixth form)"},{"$f":"CONCATENATE(M77,S77)","v":"Study space, room (sixth form)69"},{"$f":"IF(VLOOKUP(D77,'Prog Assums'!N$128:V$174,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S77>0,ROUNDDOWN((S77-VLOOKUP(AU77,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU77,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":41},null,{"$f":"AI77","v":69},null,{"$f":"AK77","v":1},{"$f":"MAXA((S77*U77)-Y77,0)","v":69},null,null,null,null,{"$f":"IF(O77=\"retained\",V77+Y77,IF(O77=\"refurb'ed\",V77+Y77,0))","v":0},null,{"$f":"IF(K6>0,ROUND(20+(K6*0.2),0),0)","v":65},{"$f":"IF(K6>0,\"m2 minimum recommended\",\"options for further study areas\")","v":"m2 minimum recommended"},null,null,null,null,{"$f":"IF(K6>0,-DE6+ROUNDUP((AC77+1)/7,0)*7,0)","v":69},null,{"$f":"DE77","v":1},null,null,{"$f":"IF(U77>0,VLOOKUP(D77,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",null,{"$f":"ROUNDDOWN(VLOOKUP(AU77,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP77*VLOOKUP(AU77,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":2},{"$f":"ROUNDUP(VLOOKUP(AU77,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP77*VLOOKUP(AU77,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":4},69,null,{"$f":"VLOOKUP(D77,'Prog Assums'!$N$132:$O$172,2,FALSE)","v":"B"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N77,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N77,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N77)","v":1},{"$f":"IF(ISERROR(BE77*BG77)=TRUE,\"\",BE77*BG77)","v":""},null,{"$f":"IF(ISERROR(BH77-Y77-V77)=TRUE,\"\",BH77-Y77-V77)","v":""},0,null,{"$f":"SUM(BO77:CK77)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U77","v":1},null,{"$f":"IF($S77>0,VLOOKUP($D77,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"9m2 for up to 4"},{"$f":"IF($S77>0,VLOOKUP($D77,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"IF(S77>120,3,2)","v":2},{"$f":"IF(S77>120,-16,4)","v":4},31,{"$f":"IF(CS77>14,IF(CS77<31,CS77,ROUNDDOWN(CS77/30,0)*30),0)","v":30},{"$f":"IF(S77>0,(V77/S77)*CT77,0)","v":30},{"$f":"IF(CS77>0,(V77/S77)*CS77,0)-CU77","v":1},31,30,30,1,{"$f":"ROUND(K6/5,0)","v":45},{"$f":"ROUND(($DE6*25)+($K6*0.2),0)","v":70},null,null,{"$f":"DE6","v":1},null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C77,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":12},{"$f":"VLOOKUP($C77,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C77,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI77,VLOOKUP($C77,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":69},{"$f":"VLOOKUP($C77,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C77,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":250},{"$f":"IF(ISERROR((SUM($EB77,$EH77,$EN77,$EU77)/SUM($EA77,$EG77,$EM77,$ET77)-$S77))=TRUE,0,IF($U77=0,0,(SUM($EB77,$EH77,$EN77,$EU77)/SUM($EA77,$EG77,$EM77,$ET77)-$S77)))","v":0},null,{"$f":"SUM(EA77,EG77,EM77,ET77)-U77","v":-1},{"$f":"SUM($EU77,$EN77,$EH77,$EB77)-$V77-$Y77","v":-69},null,null,0,null,0,{"$f":"EA77*DY77","v":0},null,null,0,null,0,{"$f":"EG77*EE77","v":0},null,null,{"$f":"IF(EN77>0,SUM(EN77/EM77),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY77:$YD77,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY77:$YD77)","v":0},null,null,null,{"$f":"IF(EU77>0,SUM(EU77/ET77),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY77:$YD77,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY77:$YD77)","v":0}]
[{"$f":"VLOOKUP($D78,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D78,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},"-",null,null,null,null,null,null,null,null,{"$f":"IF(D78=\"\",\"\",_xlfn.XLOOKUP(D78,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},{"$f":"CONCATENATE(M78,S78)","v":"-"},{"$f":"IF(VLOOKUP(D78,'Prog Assums'!N$128:V$174,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S78>0,ROUNDDOWN((S78-VLOOKUP(AU78,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU78,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":"-"},null,null,null,null,{"$f":"MAXA((S78*U78)-Y78,0)","v":0},null,null,null,null,{"$f":"IF(O78=\"retained\",V78+Y78,IF(O78=\"refurb'ed\",V78+Y78,0))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(U78>0,VLOOKUP(D78,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},{"$f":"IF(O78=\"existing\",\"E\",\"\")","v":""},null,{"$f":"ROUNDDOWN(VLOOKUP(AU78,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP78*VLOOKUP(AU78,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":{"$error":"#N/A"}},{"$f":"ROUNDUP(VLOOKUP(AU78,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP78*VLOOKUP(AU78,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":{"$error":"#N/A"}},{"$f":"MAXA((AI78*AK78)-AT78,0)","v":0},null,{"$f":"VLOOKUP(D78,'Prog Assums'!$N$132:$O$172,2,FALSE)","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N78,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N78,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N78)","v":0},{"$f":"IF(ISERROR(BE78*BG78)=TRUE,\"\",BE78*BG78)","v":""},null,{"$f":"IF(ISERROR(BH78-Y78-V78)=TRUE,\"\",BH78-Y78-V78)","v":""},{"$f":"BG78-U78","v":0},null,{"$f":"SUM(BO78:CK78)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U78","v":0},null,{"$f":"IF($S78>0,VLOOKUP($D78,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S78>0,VLOOKUP($D78,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"IF(S78>120,3,2)","v":2},{"$f":"IF(S78>120,-16,4)","v":4},{"$f":"IF(S78=0,0,MAXA(1,ROUNDUP((S78/CQ78)-CR78,0)))","v":0},{"$f":"IF(CS78>14,IF(CS78<31,CS78,ROUNDDOWN(CS78/30,0)*30),0)","v":0},{"$f":"IF(S78>0,(V78/S78)*CT78,0)","v":0},{"$f":"IF(CS78>0,(V78/S78)*CS78,0)-CU78","v":0},{"$f":"IF(AK78=0,0,MAXA(1,ROUNDUP((AI78/CQ78)-CR78,0)))","v":0},{"$f":"IF(CW78>14,IF(CW78<31,CW78,ROUNDDOWN(CW78/30,0)*30),0)","v":0},{"$f":"IF(AK78>0,(AS78/AI78)*CX78,0)","v":0},{"$f":"IF(CW78>0,(AS78/AI78)*CW78,0)-CY78","v":0},{"$f":"ROUND(K6/5,0)","v":45},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C78,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C78,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C78,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI78,VLOOKUP($C78,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C78,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C78,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},{"$f":"IF(ISERROR((SUM($EB78,$EH78,$EN78,$EU78)/SUM($EA78,$EG78,$EM78,$ET78)-$S78))=TRUE,0,IF($U78=0,0,(SUM($EB78,$EH78,$EN78,$EU78)/SUM($EA78,$EG78,$EM78,$ET78)-$S78)))","v":0},null,{"$f":"SUM(EA78,EG78,EM78,ET78)-U78","v":0},{"$f":"SUM($EU78,$EN78,$EH78,$EB78)-$V78-$Y78","v":0},null,null,0,null,0,{"$f":"EA78*DY78","v":0},null,null,0,null,0,{"$f":"EG78*EE78","v":0},null,null,{"$f":"IF(EN78>0,SUM(EN78/EM78),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY78:$YD78,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY78:$YD78)","v":0},null,null,null,{"$f":"IF(EU78>0,SUM(EU78/ET78),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY78:$YD78,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY78:$YD78)","v":0}]
[{"$f":"VLOOKUP($D79,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D79,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},"-",null,null,null,null,null,null,null,null,{"$f":"IF(D79=\"\",\"\",_xlfn.XLOOKUP(D79,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},{"$f":"CONCATENATE(M79,S79)","v":"-"},{"$f":"IF(VLOOKUP(D79,'Prog Assums'!N$128:V$174,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S79>0,ROUNDDOWN((S79-VLOOKUP(AU79,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU79,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":"-"},null,null,null,null,{"$f":"MAXA((S79*U79)-Y79,0)","v":0},null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(U79>0,VLOOKUP(D79,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",null,{"$f":"ROUNDDOWN(VLOOKUP(AU79,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP79*VLOOKUP(AU79,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":{"$error":"#N/A"}},{"$f":"ROUNDUP(VLOOKUP(AU79,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP79*VLOOKUP(AU79,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":{"$error":"#N/A"}},0,null,{"$f":"VLOOKUP(D79,'Prog Assums'!$N$132:$O$172,2,FALSE)","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N79,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N79,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N79)","v":0},{"$f":"IF(ISERROR(BE79*BG79)=TRUE,\"\",BE79*BG79)","v":""},null,{"$f":"IF(ISERROR(BH79-Y79-V79)=TRUE,\"\",BH79-Y79-V79)","v":""},0,null,{"$f":"SUM(BO79:CK79)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U79","v":0},null,{"$f":"IF($S79>0,VLOOKUP($D79,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S79>0,VLOOKUP($D79,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,2,4,0,{"$f":"IF(CS79>14,IF(CS79<31,CS79,ROUNDDOWN(CS79/30,0)*30),0)","v":0},{"$f":"IF(S79>0,(V79/S79)*CT79,0)","v":0},{"$f":"IF(CS79>0,(V79/S79)*CS79,0)-CU79","v":0},0,0,0,0,{"$f":"ROUND(K7/5,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C79,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C79,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C79,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI79,VLOOKUP($C79,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C79,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C79,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},{"$f":"IF(ISERROR((SUM($EB79,$EH79,$EN79,$EU79)/SUM($EA79,$EG79,$EM79,$ET79)-$S79))=TRUE,0,IF($U79=0,0,(SUM($EB79,$EH79,$EN79,$EU79)/SUM($EA79,$EG79,$EM79,$ET79)-$S79)))","v":0},null,{"$f":"SUM(EA79,EG79,EM79,ET79)-U79","v":0},{"$f":"SUM($EU79,$EN79,$EH79,$EB79)-$V79-$Y79","v":0},null,null,0,null,0,{"$f":"EA79*DY79","v":0},null,null,0,null,0,{"$f":"EG79*EE79","v":0},null,null,{"$f":"IF(EN79>0,SUM(EN79/EM79),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY79:$YD79,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY79:$YD79)","v":0},null,null,null,{"$f":"IF(EU79>0,SUM(EU79/ET79),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY79:$YD79,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY79:$YD79)","v":0}]
[null,null,null,"Creative art",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S80>0,VLOOKUP($D80,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S80>0,VLOOKUP($D80,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""}]
[{"$f":"VLOOKUP($D81,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"RES21"},null,{"$f":"VLOOKUP($D81,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"RES21"},"Heavy practical resource (kiln)",null,null,null,null,null,null,null,null,{"$f":"IF(D81=\"\",\"\",_xlfn.XLOOKUP(D81,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Heavy practical resource (kiln)"},{"$f":"CONCATENATE(M81,S81)","v":"Heavy practical resource (kiln)4"},null,null,"-",null,{"$f":"VLOOKUP(D81,'Prog Assums'!N$5:U$271,5,FALSE)","v":4},null,{"$f":"AK81","v":1},{"$f":"MAXA((S81*U81)-Y81,0)","v":4},null,null,null,null,0,null,4,"m2 minimum in new build",null,null,null,null,{"$f":"IF(AK81>0,4,0)","v":4},null,{"$f":"IF(AK40+AK41>0,1,0)","v":1},null,null,{"$f":"IF(U81>0,VLOOKUP(D81,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",null,4,8,4,null,{"$f":"VLOOKUP(D81,'Prog Assums'!$N$132:$O$172,2,FALSE)","v":"-"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N81,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N81,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N81)","v":1},{"$f":"IF(ISERROR(BE81*BG81)=TRUE,\"\",BE81*BG81)","v":""},null,{"$f":"IF(ISERROR(BH81-Y81-V81)=TRUE,\"\",BH81-Y81-V81)","v":""},0,null,{"$f":"SUM(BO81:CK81)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U81","v":1},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S81>0,VLOOKUP($D81,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"4m2"},{"$f":"IF($S81>0,VLOOKUP($D81,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"-"},null,null,{"$f":"VLOOKUP(D81,'Prog Assums'!$N$6:$Q$229,3,0)","v":3.5},{"$f":"VLOOKUP(D81,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},1,{"$f":"IF(CS81>14,IF(CS81<31,CS81,ROUNDDOWN(CS81/30,0)*30),0)","v":0},{"$f":"IF(S81>0,(V81/S81)*CT81,0)","v":0},{"$f":"IF(CS81>0,(V81/S81)*CS81,0)-CU81","v":1},{"$f":"IF(AK81=0,0,MAXA(1,ROUNDUP((AI81/CQ81)-CR81,0)))","v":1},{"$f":"IF(CW81>14,IF(CW81<31,CW81,ROUNDDOWN(CW81/30,0)*30),0)","v":0},{"$f":"IF(AK81>0,(AS81/AI81)*CX81,0)","v":0},{"$f":"IF(CW81>0,(AS81/AI81)*CW81,0)-CY81","v":1},1,4,null,{"$f":"HLOOKUP(AG$12,$DF$15:$DI$165,66,FALSE)","v":0},null,{"$f":"IF(DF42>0,1,0)","v":0},0,0,0,0,0,0,0,{"$f":"VLOOKUP($C81,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":4},{"$f":"VLOOKUP($C81,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C81,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI81,VLOOKUP($C81,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":4},{"$f":"VLOOKUP($C81,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C81,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},{"$f":"IF(ISERROR((SUM($EB81,$EH81,$EN81,$EU81)/SUM($EA81,$EG81,$EM81,$ET81)-$S81))=TRUE,0,IF($U81=0,0,(SUM($EB81,$EH81,$EN81,$EU81)/SUM($EA81,$EG81,$EM81,$ET81)-$S81)))","v":0},null,{"$f":"SUM(EA81,EG81,EM81,ET81)-U81","v":-1},{"$f":"SUM($EU81,$EN81,$EH81,$EB81)-$V81-$Y81","v":-4},null,null,0,null,0,{"$f":"EA81*DY81","v":0},null,null,0,null,0,{"$f":"EG81*EE81","v":0},null,null,{"$f":"IF(EN81>0,SUM(EN81/EM81),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY81:$YD81,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY81:$YD81)","v":0},null,null,null,{"$f":"IF(EU81>0,SUM(EU81/ET81),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY81:$YD81,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY81:$YD81)","v":0}]
[{"$f":"VLOOKUP($D82,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"RES12"},null,{"$f":"VLOOKUP($D82,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"RES12"},"Music practice rooms",null,null,null,null,null,null,null,null,{"$f":"IF(D82=\"\",\"\",_xlfn.XLOOKUP(D82,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Music practice room"},"Music practice room8",null,null,{"$f":"IF(S82>0,ROUNDDOWN((S82-VLOOKUP(AU82,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU82,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":3},null,{"$f":"VLOOKUP(D82,'Prog Assums'!N$5:U$271,5,FALSE)","v":8},null,{"$f":"(3*(U44+U45))-IF((U44+U45)>0,U83,0)","v":1},8,null,null,null,null,0,null,8,"m2 standard size",null,null,null,null,{"$f":"IF(AK82>0,8,0)","v":8},null,{"$f":"(3*(AK44+AK45))-IF((AK44+AK45)>0,AK83,0)","v":1},null,null,{"$f":"IF(U82>0,VLOOKUP(D82,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",{"$f":"VLOOKUP(D82,'Prog Assums'!N$139:T$210,7, FALSE)","v":3},{"$f":"ROUNDDOWN(VLOOKUP(AU82,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP82*VLOOKUP(AU82,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":6},{"$f":"ROUNDUP(VLOOKUP(AU82,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP82*VLOOKUP(AU82,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":10},8,null,{"$f":"VLOOKUP(D82,'Prog Assums'!$N$132:$O$172,2,FALSE)","v":"B"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N82,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N82,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N82)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U82","v":1},null,null,null,null,null,null,null,null,null,{"$f":"IF($S82>0,VLOOKUP($D82,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"8m2 for up to 3"},{"$f":"IF($S82>0,VLOOKUP($D82,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"A"},null,null,{"$f":"VLOOKUP(D82,'Prog Assums'!$N$6:$Q$229,3,0)","v":2},{"$f":"VLOOKUP(D82,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},1,0,0,1,1,0,0,1,3,8,null,{"$f":"HLOOKUP(AG$12,$DF$15:$DI$165,67,FALSE)","v":0},{"$f":"3*(DE44+DE45)-IF((DE44+DE45)>2,2,0)-IF(DE84>0,DE84,0)","v":0},{"$f":"(3*(DF44+DF45))-IF((DF44+DF45)>0,DF83,0)","v":2},{"$f":"(4*(DG44+DG45))-IF((DG44+DG45)>0,DG83,0)","v":3},{"$f":"(3*(DH44+DH45))-IF((DH44+DH45)>0,DH83,0)","v":2},{"$f":"(3*(DI44+DI45))-IF((DI44+DI45)>0,DI83,0)","v":2},{"$f":"(3*(DJ44+DJ45))-IF((DJ44+DJ45)>0,DJ83,0)","v":2},{"$f":"(4*(DK44+DK45))-IF((DK44+DK45)>0,DK83,0)","v":3},{"$f":"(3*(DL44+DL45))-IF((DL44+DL45)>0,DL83,0)","v":0},{"$f":"(3*(DM44+DM45))-IF((DM44+DM45)>0,DM83,0)","v":0},{"$f":"VLOOKUP($C82,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":6},{"$f":"VLOOKUP($C82,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C82,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI82,VLOOKUP($C82,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":8},{"$f":"VLOOKUP($C82,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":9.1},{"$f":"VLOOKUP($C82,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":12},0,null,-1,-8,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY82:$YD82,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY82:$YD82)","v":0}]
[{"$f":"VLOOKUP($D83,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"RES12"},null,{"$f":"VLOOKUP($D83,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"RES13"},"Music practice rooms (extensive)",null,null,null,null,null,null,null,null,{"$f":"IF(D83=\"\",\"\",_xlfn.XLOOKUP(D83,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Music practice room (extensive)"},"Music practice room (extensive)16",null,null,{"$f":"IF(S83>0,ROUNDDOWN((S83-VLOOKUP(AU83,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU83,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":7},null,{"$f":"VLOOKUP(D83,'Prog Assums'!N$5:U$271,5,FALSE)","v":16},null,{"$f":"AK83","v":2},32,null,null,null,null,0,null,{"$f":"IF(S83>0,VLOOKUP(D83,'Prog Assums'!$N$138:$R$150,5,FALSE),0)","v":16},{"$f":"IF(S83>0,\"m2 minimum in new build\",\"\")","v":"m2 minimum in new build"},null,null,null,null,{"$f":"IF(AK83>0,16,0)","v":16},null,{"$f":"DD83","v":2},null,null,{"$f":"IF(U83>0,VLOOKUP(D83,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",{"$f":"VLOOKUP(D83,'Prog Assums'!N$139:T$210,7, FALSE)","v":7},{"$f":"ROUNDDOWN(VLOOKUP(AU83,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP83*VLOOKUP(AU83,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":15},{"$f":"ROUNDUP(VLOOKUP(AU83,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP83*VLOOKUP(AU83,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":19},32,null,{"$f":"VLOOKUP(D83,'Prog Assums'!$N$132:$O$172,2,FALSE)","v":"C"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N83,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N83,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N83)","v":2},"",null,"",0,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U83","v":2},null,null,null,null,null,null,null,null,null,{"$f":"IF($S83>0,VLOOKUP($D83,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"16m2 for up to 7"},{"$f":"IF($S83>0,VLOOKUP($D83,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"A"},null,null,{"$f":"VLOOKUP(D83,'Prog Assums'!$N$6:$Q$229,3,0)","v":2},{"$f":"VLOOKUP(D83,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},4,0,0,8,4,0,0,8,10,16,null,{"$f":"HLOOKUP(AG$12,$DF$15:$DI$165,68,FALSE)","v":2},null,1,1,1,1,1,1,1,1,{"$f":"VLOOKUP($C83,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":12},{"$f":"VLOOKUP($C83,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C83,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI83,VLOOKUP($C83,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":13.200000000000001},{"$f":"VLOOKUP($C83,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":16},{"$f":"VLOOKUP($C83,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":45},0,null,-2,-32,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY83:$YD83,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY83:$YD83)","v":0}]
[{"$f":"VLOOKUP($D84,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"RES14"},null,{"$f":"VLOOKUP($D84,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"RES14"},"Recording control spaces",null,null,null,null,null,null,null,null,{"$f":"IF(D84=\"\",\"\",_xlfn.XLOOKUP(D84,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Recording control space"},"Recording control space8",{"$f":"IF(VLOOKUP(D84,'Prog Assums'!N$128:V$174,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S84>0,ROUNDDOWN((S84-VLOOKUP(AU84,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU84,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":3},null,{"$f":"VLOOKUP(D84,'Prog Assums'!N$5:U$271,5,FALSE)","v":8},null,{"$f":"AK84","v":1},8,null,null,null,null,0,null,{"$f":"IF(S84>0,VLOOKUP(D84,'Prog Assums'!$N$138:$R$150,5,FALSE),0)","v":8},{"$f":"IF(S84>0,\"m2 minimum in new build\",\"\")","v":"m2 minimum in new build"},null,null,null,null,{"$f":"IF(AK84>0,8,0)","v":8},null,{"$f":"DD84","v":1},null,null,{"$f":"IF(U84>0,VLOOKUP(D84,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",{"$f":"VLOOKUP(D84,'Prog Assums'!N$139:T$210,7, FALSE)","v":3},{"$f":"ROUNDDOWN(VLOOKUP(AU84,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP84*VLOOKUP(AU84,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":6},{"$f":"ROUNDUP(VLOOKUP(AU84,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP84*VLOOKUP(AU84,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":10},8,null,{"$f":"VLOOKUP(D84,'Prog Assums'!$N$132:$O$172,2,FALSE)","v":"B"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N84,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N84,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N84)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U84","v":1},null,null,null,null,null,null,null,null,null,{"$f":"IF($S84>0,VLOOKUP($D84,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"8m2 for up to 3"},{"$f":"IF($S84>0,VLOOKUP($D84,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"A"},null,null,{"$f":"VLOOKUP(D84,'Prog Assums'!$N$6:$Q$229,3,0)","v":2},{"$f":"VLOOKUP(D84,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},1,0,0,1,1,0,0,1,6,12,null,{"$f":"HLOOKUP(AG$12,$DF$15:$DI$165,69,FALSE)","v":1},{"$f":"IF(K5=0,DE6,0)","v":0},0,{"$f":"DG7","v":0},0,0,0,{"$f":"DK7","v":0},0,0,{"$f":"VLOOKUP($C84,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":6},{"$f":"VLOOKUP($C84,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C84,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI84,VLOOKUP($C84,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":8},{"$f":"VLOOKUP($C84,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C84,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":45},0,null,-1,-8,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY84:$YD84,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY84:$YD84)","v":0}]
[{"$f":"VLOOKUP($D85,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"RES16"},null,{"$f":"VLOOKUP($D85,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"RES16"},"Lighting and audio control spaces",null,null,null,null,null,null,null,null,{"$f":"IF(D85=\"\",\"\",_xlfn.XLOOKUP(D85,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Lighting and audio control space"},"Lighting and audio control space6",{"$f":"IF(VLOOKUP(D85,'Prog Assums'!N$128:V$174,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S85>0,ROUNDDOWN((S85-VLOOKUP(AU85,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU85,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":2},null,{"$f":"VLOOKUP(D85,'Prog Assums'!N$5:U$271,5,FALSE)","v":6},null,{"$f":"AK85","v":1},6,null,null,null,null,0,null,{"$f":"IF(S85>0,VLOOKUP(D85,'Prog Assums'!$N$138:$R$150,5,FALSE),0)","v":6},{"$f":"IF(S85>0,\"m2 minimum in new build\",\"\")","v":"m2 minimum in new build"},null,null,null,null,{"$f":"IF(AK85>0,6,0)","v":6},null,1,null,null,{"$f":"IF(U85>0,VLOOKUP(D85,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",{"$f":"VLOOKUP(D85,'Prog Assums'!N$139:T$210,7, FALSE)","v":2},{"$f":"ROUNDDOWN(VLOOKUP(AU85,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP85*VLOOKUP(AU85,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":5},{"$f":"ROUNDUP(VLOOKUP(AU85,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP85*VLOOKUP(AU85,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":8},6,null,{"$f":"VLOOKUP(D85,'Prog Assums'!$N$132:$O$172,2,FALSE)","v":"B"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N85,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N85,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N85)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U85","v":1},null,null,null,null,null,null,null,null,null,{"$f":"IF($S85>0,VLOOKUP($D85,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"6m2 for up to 2"},{"$f":"IF($S85>0,VLOOKUP($D85,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"A"},null,null,{"$f":"VLOOKUP(D85,'Prog Assums'!$N$6:$Q$229,3,0)","v":2},{"$f":"VLOOKUP(D85,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},1,0,0,1,1,0,0,1,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C85,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":4},{"$f":"VLOOKUP($C85,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C85,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI85,VLOOKUP($C85,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":6},{"$f":"VLOOKUP($C85,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C85,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":45},0,null,-1,-6,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY85:$YD85,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY85:$YD85)","v":0}]
[{"$f":"VLOOKUP($D86,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D86,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},"-",null,null,null,null,null,null,null,null,{"$f":"IF(D86=\"\",\"\",_xlfn.XLOOKUP(D86,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},"-0",{"$f":"IF(VLOOKUP(D86,'Prog Assums'!N$128:V$174,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S86>0,ROUND((S86-VLOOKUP(AU86,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU86,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":"-"},null,{"$f":"VLOOKUP(D86,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},null,{"$f":"AK86","v":0},0,null,null,null,null,0,null,{"$f":"IF(S86>0,VLOOKUP(D86,'Prog Assums'!$N$138:$R$150,5,FALSE),0)","v":0},{"$f":"IF(S86>0,\"m2 minimum in new build\",\"\")","v":""},null,null,null,null,null,null,null,null,null,{"$f":"IF(U86>0,VLOOKUP(D86,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",{"$f":"VLOOKUP(D86,'Prog Assums'!N$139:T$210,7, FALSE)","v":"size"},{"$f":"ROUNDDOWN(VLOOKUP(AU86,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP86*VLOOKUP(AU86,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":{"$error":"#N/A"}},{"$f":"ROUNDUP(VLOOKUP(AU86,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP86*VLOOKUP(AU86,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":{"$error":"#N/A"}},0,null,{"$f":"VLOOKUP(D86,'Prog Assums'!$N$132:$O$172,2,FALSE)","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N86,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N86,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N86)","v":0},"",null,"",0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S86>0,VLOOKUP($D86,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S86>0,VLOOKUP($D86,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"VLOOKUP(D86,'Prog Assums'!$N$6:$Q$229,3,0)","v":0},{"$f":"VLOOKUP(D86,'Prog Assums'!$N$6:$Q$229,4,0)","v":0},{"$f":"IF(S86=0,0,MAXA(1,ROUNDUP((S86/CQ86)-CR86,0)))","v":0},0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C86,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C86,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C86,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI86,VLOOKUP($C86,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C86,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C86,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY86:$YD86,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY86:$YD86)","v":0}]
[null,null,null,"SEN and support spaces",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S87>0,VLOOKUP($D87,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S87>0,VLOOKUP($D87,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""}]
[{"$f":"VLOOKUP($D88,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"SEN02"},null,{"$f":"VLOOKUP($D88,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"SEN02"},"Medical treatment (MI) rooms",null,null,null,null,null,null,null,null,{"$f":"IF(D88=\"\",\"\",_xlfn.XLOOKUP(D88,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Medical treatment (MI) room"},{"$f":"CONCATENATE(M88,S88)","v":"Medical treatment (MI) room12"},null,null,{"$f":"ROUNDDOWN((AI88-VLOOKUP(AU88,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU88,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":4},null,{"$f":"VLOOKUP(D88,'Prog Assums'!N$5:U$271,5,FALSE)","v":12},null,{"$f":"AK88","v":1},{"$f":"MAXA((S88*U88)-Y88,0)","v":12},null,null,{"$f":"MAXA(0,(U88-1)*S88)","v":0},null,0,null,{"$f":"IF(U88>0,\"12\",\"NOTE\")","v":"12"},{"$f":"IF(V88>0,\"m2 min recommended\",\"MI room must be provided\")","v":"m2 min recommended"},null,null,null,null,12,null,{"$f":"1+IF(K12>0,1,0)","v":1},null,null,{"$f":"IF(U88>0,VLOOKUP(D88,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",{"$f":"VLOOKUP(D88,'Prog Assums'!N$139:T$210,7, FALSE)","v":4},{"$f":"ROUNDDOWN(VLOOKUP(AU88,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP88*VLOOKUP(AU88,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":10},{"$f":"ROUNDUP(VLOOKUP(AU88,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP88*VLOOKUP(AU88,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":13},{"$f":"MAXA((AI88*AK88)-AT88,0)","v":12},{"$f":"(AK88-1)*AI88","v":0},{"$f":"VLOOKUP(D88,'Prog Assums'!$N$132:$O$172,2,FALSE)","v":"C"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N88,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N88,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N88)","v":1},{"$f":"IF(ISERROR(BE88*BG88)=TRUE,\"\",BE88*BG88)","v":""},null,{"$f":"IF(ISERROR(BH88-Y88-V88)=TRUE,\"\",BH88-Y88-V88)","v":""},0,null,{"$f":"SUM(BO88:CK88)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(K12>0,1,0)","v":0},null,{"$f":"U88-CI88","v":1},null,{"$f":"IF($S88>0,VLOOKUP($D88,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"12m2 for up to 4"},{"$f":"IF($S88>0,VLOOKUP($D88,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"B"},null,null,{"$f":"VLOOKUP(D88,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D88,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},4,{"$f":"IF(CS88>14,IF(CS88<31,CS88,ROUNDDOWN(CS88/30,0)*30),0)","v":0},{"$f":"IF(S88>0,(V88/S88)*CT88,0)","v":0},{"$f":"IF(CS88>0,(V88/S88)*CS88,0)-CU88","v":4},{"$f":"IF(AK88=0,0,MAXA(1,ROUNDUP((AI88/CQ88)-CR88,0)))","v":4},{"$f":"IF(CW88>14,IF(CW88<31,CW88,ROUNDDOWN(CW88/30,0)*30),0)","v":0},{"$f":"IF(AK88>0,(AS88/AI88)*CX88,0)","v":0},{"$f":"IF(CW88>0,(AS88/AI88)*CW88,0)-CY88","v":4},{"$f":"ROUND(((DB88-4.5)/1.6),0)","v":5},12,null,1,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C88,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":6},{"$f":"VLOOKUP($C88,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C88,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI88,VLOOKUP($C88,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":12},{"$f":"VLOOKUP($C88,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C88,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":41},{"$f":"IF(ISERROR((SUM($EB88,$EH88,$EN88,$EU88)/SUM($EA88,$EG88,$EM88,$ET88)-$S88))=TRUE,0,IF($U88=0,0,(SUM($EB88,$EH88,$EN88,$EU88)/SUM($EA88,$EG88,$EM88,$ET88)-$S88)))","v":0},null,{"$f":"SUM(EA88,EG88,EM88,ET88)-U88","v":-1},{"$f":"SUM($EU88,$EN88,$EH88,$EB88)-$V88-$Y88","v":-12},null,null,0,null,0,{"$f":"EA88*DY88","v":0},null,null,0,null,0,{"$f":"EG88*EE88","v":0},null,null,{"$f":"IF(EN88>0,SUM(EN88/EM88),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY88:$YD88,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY88:$YD88)","v":0},null,null,null,{"$f":"IF(EU88>0,SUM(EU88/ET88),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY88:$YD88,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY88:$YD88)","v":0}]
[{"$f":"VLOOKUP($D89,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"SEN20"},null,{"$f":"VLOOKUP($D89,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"SEN20"},"SEN resource spaces",null,null,null,null,null,null,null,null,{"$f":"IF(D89=\"\",\"\",_xlfn.XLOOKUP(D89,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"SEN resource space"},{"$f":"CONCATENATE(M89,S89)","v":"SEN resource space16"},null,null,{"$f":"ROUNDDOWN((AI89-VLOOKUP(AU89,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU89,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":7},null,{"$f":"VLOOKUP(D89,'Prog Assums'!N$5:U$271,5,FALSE)","v":16},null,{"$f":"AK89","v":1},{"$f":"MAXA((S89*U89)-Y89,0)","v":16},null,null,{"$f":"MAXA(0,IF(K$14>0,(U89-1)*S89,0))","v":0},null,0,null,"Group room suitable for SEN/ multi-agency",null,null,null,null,null,16,null,{"$f":"1+IF(K12>0,ROUNDUP(K12/30,0),0)","v":1},null,null,{"$f":"IF(U89>0,VLOOKUP(D89,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},{"$f":"IF(O89=\"existing\",\"E\",\"\")","v":""},{"$f":"VLOOKUP(D89,'Prog Assums'!N$139:T$210,7, FALSE)","v":7},{"$f":"ROUNDDOWN(VLOOKUP(AU89,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP89*VLOOKUP(AU89,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":15},{"$f":"ROUNDUP(VLOOKUP(AU89,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP89*VLOOKUP(AU89,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":19},{"$f":"MAXA((AI89*AK89)-AT89,0)","v":16},{"$f":"(AK89-1)*AI89","v":0},{"$f":"VLOOKUP(D89,'Prog Assums'!$N$132:$O$172,2,FALSE)","v":"C"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N89,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N89,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N89)","v":1},{"$f":"IF(ISERROR(BE89*BG89)=TRUE,\"\",BE89*BG89)","v":""},null,{"$f":"IF(ISERROR(BH89-Y89-V89)=TRUE,\"\",BH89-Y89-V89)","v":""},{"$f":"BG89-U89","v":0},null,{"$f":"SUM(BO89:CK89)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(K12>0,ROUNDUP(K12/30,0),0)","v":0},null,{"$f":"U89-CI89","v":1},null,{"$f":"IF($S89>0,VLOOKUP($D89,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"16m2 for up to 7"},{"$f":"IF($S89>0,VLOOKUP($D89,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"B"},null,null,{"$f":"VLOOKUP(D89,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D89,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},7,{"$f":"IF(CS89>14,IF(CS89<31,CS89,ROUNDDOWN(CS89/30,0)*30),0)","v":0},0,7,7,0,0,7,8,16,null,1,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C89,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":12},{"$f":"VLOOKUP($C89,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C89,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI89,VLOOKUP($C89,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":16},{"$f":"VLOOKUP($C89,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C89,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":41},0,null,-1,-16,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY89:$YD89,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY89:$YD89)","v":0}]
[{"$f":"VLOOKUP($D90,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"RES00"},null,{"$f":"VLOOKUP($D90,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"RES00"},"Small group rooms",null,null,null,null,null,null,null,null,{"$f":"IF(D90=\"\",\"\",_xlfn.XLOOKUP(D90,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Small group room"},"Small group room9",null,null,{"$f":"ROUNDDOWN((AI90-VLOOKUP(AU90,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU90,'Prog Assums'!$E$38:$I$54,3,FALSE),0)","v":4},null,{"$f":"VLOOKUP(D90,'Prog Assums'!N$5:U$271,5,FALSE)","v":9},null,{"$f":"AK90","v":4},36,null,null,null,null,0,null,null,null,null,null,null,null,9,null,{"$f":"ROUND(K8/300,0)","v":4},null,null,{"$f":"IF(U90>0,VLOOKUP(D90,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",{"$f":"VLOOKUP(D90,'Prog Assums'!N$139:T$210,7, FALSE)","v":4},{"$f":"ROUNDDOWN(VLOOKUP(AU90,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP90*VLOOKUP(AU90,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":8},{"$f":"ROUNDUP(VLOOKUP(AU90,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP90*VLOOKUP(AU90,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":11},36,null,{"$f":"VLOOKUP(D90,'Prog Assums'!$N$132:$O$172,2,FALSE)","v":"B"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N90,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N90,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N90)","v":4},"",null,"",0,null,{"$f":"SUM(BO90:CK90)","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U90-CI90","v":4},null,{"$f":"IF($S90>0,VLOOKUP($D90,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"9m2 for up to 4"},{"$f":"IF($S90>0,VLOOKUP($D90,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"A"},null,null,{"$f":"VLOOKUP(D90,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D90,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},2,0,0,8,2,0,0,8,4,9,null,{"$f":"ROUND($K5/300,0)","v":3},{"$f":"ROUND(K$6/300,0)","v":1},null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C90,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":6},{"$f":"VLOOKUP($C90,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C90,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI90,VLOOKUP($C90,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":9},{"$f":"VLOOKUP($C90,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C90,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,-4,-36,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY90:$YD90,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY90:$YD90)","v":0}]
[{"$f":"VLOOKUP($D91,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"RES00"},null,{"$f":"VLOOKUP($D91,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"RES03"},"Small group rooms (medium)",null,null,null,null,null,null,null,null,{"$f":"IF(D91=\"\",\"\",_xlfn.XLOOKUP(D91,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Small group room (medium)"},"Small group room (medium)12",{"$f":"IF(VLOOKUP(D91,'Prog Assums'!N$128:V$174,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S91>0,ROUNDDOWN((S91-VLOOKUP(AU91,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU91,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":6},null,{"$f":"VLOOKUP(D91,'Prog Assums'!N$5:U$271,5,FALSE)","v":12},null,{"$f":"AK91","v":0},0,null,null,{"$f":"AT91","v":0},null,0,null,null,null,null,null,null,null,{"$f":"IF(K12>0,12,0)","v":0},null,{"$f":"IF(K12>0,ROUNDDOWN(K12/10,0),0)","v":0},null,null,{"$f":"IF(U91>0,VLOOKUP(D91,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",{"$f":"VLOOKUP(D91,'Prog Assums'!N$139:T$210,7, FALSE)","v":6},{"$f":"ROUNDDOWN(VLOOKUP(AU91,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP91*VLOOKUP(AU91,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":11},{"$f":"ROUNDUP(VLOOKUP(AU91,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP91*VLOOKUP(AU91,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":15},0,{"$f":"AK91*AI91","v":0},{"$f":"VLOOKUP(D91,'Prog Assums'!$N$132:$O$172,2,FALSE)","v":"B"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N91,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N91,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N91)","v":0},"",null,"",0,null,{"$f":"SUM(BO91:CJ91)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U91","v":0},null,{"$f":"U91-CI91","v":0},null,{"$f":"IF($S91>0,VLOOKUP($D91,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"12m2 for up to 6"},{"$f":"IF($S91>0,VLOOKUP($D91,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"A"},null,null,{"$f":"VLOOKUP(D91,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D91,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},4,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C91,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":12},{"$f":"VLOOKUP($C91,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C91,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI91,VLOOKUP($C91,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":12},{"$f":"VLOOKUP($C91,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C91,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY91:$YD91,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY91:$YD91)","v":0}]
[{"$f":"VLOOKUP($D92,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"RES00"},null,{"$f":"VLOOKUP($D92,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"RES04"},"Small group rooms (large SEN etc.)",null,null,null,null,null,null,null,null,{"$f":"IF(D92=\"\",\"\",_xlfn.XLOOKUP(D92,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Small group room (large SEN etc.)"},"Small group room (large SEN etc.)16",{"$f":"IF(VLOOKUP(D92,'Prog Assums'!N$128:V$174,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S92>0,ROUNDDOWN((S92-VLOOKUP(AU92,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU92,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":8},null,{"$f":"VLOOKUP(D92,'Prog Assums'!N$5:U$271,5,FALSE)","v":16},null,{"$f":"AK92","v":1},16,null,null,null,null,0,null,null,null,null,null,null,null,16,null,1,null,null,{"$f":"IF(U92>0,VLOOKUP(D92,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",{"$f":"VLOOKUP(D92,'Prog Assums'!N$139:T$210,7, FALSE)","v":9},{"$f":"ROUNDDOWN(VLOOKUP(AU92,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP92*VLOOKUP(AU92,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":16},{"$f":"ROUNDUP(VLOOKUP(AU92,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP92*VLOOKUP(AU92,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":20},16,null,{"$f":"VLOOKUP(D92,'Prog Assums'!$N$132:$O$172,2,FALSE)","v":"B"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N92,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N92,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N92)","v":1},"",null,"",0,null,{"$f":"SUM(BO92:CK92)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U92-CI92","v":1},null,{"$f":"IF($S92>0,VLOOKUP($D92,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"16m2 for up to 9"},{"$f":"IF($S92>0,VLOOKUP($D92,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":"A"},null,null,{"$f":"VLOOKUP(D92,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D92,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},7,0,0,7,7,0,0,7,8,16,null,{"$f":"IF($K5>1000,2,DD5)","v":1},null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C92,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":16},{"$f":"VLOOKUP($C92,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C92,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI92,VLOOKUP($C92,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":16},{"$f":"VLOOKUP($C92,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C92,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":41},0,null,-1,-16,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY92:$YD92,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY92:$YD92)","v":0}]
[{"$f":"VLOOKUP($D93,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D93,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},"-",null,null,null,null,null,null,null,null,{"$f":"IF(D93=\"\",\"\",_xlfn.XLOOKUP(D93,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},"-0",{"$f":"IF(VLOOKUP(D93,'Prog Assums'!N$128:V$174,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S93>0,ROUNDDOWN((S93-VLOOKUP(AU93,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU93,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":"-"},null,{"$f":"VLOOKUP(D93,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(U93>0,VLOOKUP(D93,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",{"$f":"VLOOKUP(D93,'Prog Assums'!N$139:T$210,7, FALSE)","v":"size"},{"$f":"ROUNDDOWN(VLOOKUP(AU93,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP93*VLOOKUP(AU93,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":{"$error":"#N/A"}},{"$f":"ROUNDUP(VLOOKUP(AU93,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP93*VLOOKUP(AU93,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":{"$error":"#N/A"}},0,null,{"$f":"VLOOKUP(D93,'Prog Assums'!$N$132:$O$172,2,FALSE)","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N93,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N93,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N93)","v":0},"",null,"",0,null,{"$f":"SUM(BO93:CK93)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U93","v":0},null,{"$f":"IF($S93>0,VLOOKUP($D93,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S93>0,VLOOKUP($D93,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"VLOOKUP(D93,'Prog Assums'!$N$6:$Q$229,3,0)","v":0},{"$f":"VLOOKUP(D93,'Prog Assums'!$N$6:$Q$229,4,0)","v":0},0,0,0,0,0,0,0,0,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C93,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C93,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C93,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI93,VLOOKUP($C93,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C93,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C93,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY93:$YD93,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY93:$YD93)","v":0}]
[{"$f":"VLOOKUP($D94,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D94,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},"-",null,null,null,null,null,null,null,null,{"$f":"IF(D94=\"\",\"\",_xlfn.XLOOKUP(D94,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},"-0",{"$f":"IF(VLOOKUP(D94,'Prog Assums'!N$128:V$174,9,FALSE)>0,\"retained\",\"\")","v":""},null,"-",null,{"$f":"VLOOKUP(D94,'Prog Assums'!N$5:U$271,5,FALSE)","v":0},null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(U94>0,VLOOKUP(D94,'Prog Assums'!$N$6:$S$169,6,FALSE),0)","v":0},"",{"$f":"VLOOKUP(D94,'Prog Assums'!N$139:T$210,7, FALSE)","v":"size"},{"$f":"ROUNDDOWN(VLOOKUP(AU94,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP94*VLOOKUP(AU94,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":{"$error":"#N/A"}},{"$f":"ROUNDUP(VLOOKUP(AU94,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP94*VLOOKUP(AU94,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":{"$error":"#N/A"}},0,{"$f":"IF(K$12>0,AI94*AK94,0)","v":0},{"$f":"VLOOKUP(D94,'Prog Assums'!$N$132:$O$172,2,FALSE)","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N94,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N94,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N94)","v":0},"",null,"",0,null,{"$f":"SUM(BO94:CK94)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U94","v":0},null,{"$f":"IF($S94>0,VLOOKUP($D94,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S94>0,VLOOKUP($D94,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"VLOOKUP(D94,'Prog Assums'!$N$6:$Q$229,3,0)","v":0},{"$f":"VLOOKUP(D94,'Prog Assums'!$N$6:$Q$229,4,0)","v":0},0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C94,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C94,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C94,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI94,VLOOKUP($C94,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C94,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C94,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY94:$YD94,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY94:$YD94)","v":0}]
[null,null,null,"TOTAL AREA",null,null,null,null,null,null,null,"BB103 range","BB103 range","BB103 range",{"$f":"ROUND(IF(K$4>0,50,75)+IF(K$6>0,50,0)+((K$4+K$5)*0.15)+(K$6*0.4),0)","v":350},"to",{"$f":"IF(AR$8>0,75,125)+(IF(K6>0,75,0)+(K4*0.25)+(K$5*0.25)+(K$6*0.5))","v":537.5},null,null,null,null,{"$f":"SUM(V76:V94)","v":353},null,null,{"$f":"SUM(Y76:Y94)","v":0},null,{"$f":"SUM(AA76:AA94)","v":0},null,{"$f":"IF(V95<O95,\"ERROR: total area for category is too low\",IF(V95>Q95,\"WARNING: total area for category is high\",\"OK: area within BB103 range\"))","v":"OK: area within BB103 range"},null,null,null,null,null,{"$f":"SUM(AS76:AS94)","v":353},null,{"$f":"SUM(AT76:AT94)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(BH76:BH94)","v":0},null,{"$f":"BH95-Y95-V95","v":-353},null,null,null,null,{"$f":"SUM(BO76:BO94)","v":0},null,{"$f":"SUM(BQ76:BQ94)","v":0},null,{"$f":"SUM(BS76:BS94)","v":0},null,{"$f":"SUM(BU76:BU94)","v":0},null,{"$f":"SUM(BW76:BW94)","v":0},null,{"$f":"SUM(BY76:BY94)","v":0},null,{"$f":"SUM(CA76:CA94)","v":1},null,{"$f":"SUM(CC76:CC94)","v":5},null,{"$f":"SUM(CE76:CE94)","v":0},null,{"$f":"SUM(CG76:CG94)","v":0},null,{"$f":"SUM(CI76:CI94)","v":0},null,{"$f":"SUM(CK76:CK94)","v":9},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(EU95,EN95,EH95,EB95)-SUM(Y95,V95)","v":-353},null,null,null,null,null,{"$f":"SUM(EB76:EB94)","v":0},null,null,null,null,null,{"$f":"SUM(EH76:EH94)","v":0},null,null,null,null,null,{"$f":"SUM(EN76:EN94)","v":0},null,null,null,null,null,null,{"$f":"SUM(EU76:EU94)","v":0}]
[]
[null,null,null,"SoA FOR MAINSTREAM SECONDARY (cont.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"average",null,null,null,null,null,null,null,"AREA",null,null,null,null,null,null,null,null,"recommended",null,null,null,null,null,null,"area range",null,null,null,null,null,null,null,null,null,null,null,null,null,"average area of space (m2)",null,"TOTAL no. of spaces","TOTAL AREA (incl supp)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"work",null,"re-","basic","work",null,"re-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIFFERENCES",null,null,null,null,null,{"$f":"DY13","v":0},null,null,null,null,null,{"$f":"EE13","v":0},null,null,null,null,null,{"$f":"EK13","v":0},null,null,null,null,null,null,{"$f":"ER13","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"area of",null,"TOTAL","TOTAL",null,null,"SUPP",null,"OF RE-",null,null,null,null,null,null,null,"area of",null,null,null,null,null,null,"max. group size","min for min group","max for max group",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BO15","v":"Mathematics"},null,{"$f":"BQ15","v":"English"},null,{"$f":"BS15","v":"MFL"},null,{"$f":"BU15","v":"Humanities"},null,{"$f":"BW15","v":"ICT and Business Studies"},null,{"$f":"BY15","v":"Science"},null,{"$f":"CA15","v":"DT/ Art"},null,{"$f":"CC15","v":"Perf arts, hall and dining"},null,{"$f":"CE15","v":"Sports/ PE"},null,{"$f":"CG15","v":"Admin"},null,{"$f":"CI15","v":"-"},null,{"$f":"CK15","v":"Balance"},null,null,null,null,null,null,null,null,"places","basic","source","wkpl'ce","places","basic","source","max."]
[null,null,null,{"$f":"S2","v":"[Insert Project Code and Scheme Name here in title sheet]"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"space",null,"no. of","AREA",null,null,"AREA",null,"TAINED",null,null,null,null,null,null,null,"space",null,"no. of",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"per ","work","work","allow-","per ","work","work","group",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"average",null,"TOTAL","TOTAL",null,null,"average",null,"TOTAL","TOTAL",null,null,"average",null,"TOTAL","TOTAL",null,null,"average",null,"TOTAL","TOTAL",null,null,null,"average",null,"TOTAL","TOTAL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(m2)",null,"spaces","(m2)",null,null,"(m2)",null,"SPACES",null,null,null,null,null,null,null,"(m2)",null,"spaces",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"room","places","places","ance","room","places","places","size",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"area of",null,"no.of","AREA",null,null,"area of",null,"no.of","AREA",null,null,"area of",null,"no.of","AREA",null,null,"area of",null,"no.of","AREA",null,null,null,"area of",null,"no.of","AREA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"space",null,"spaces",null,null,null,"space",null,"spaces",null,null,null,"space",null,"spaces",null,null,null,"space",null,"spaces",null,null,null,null,"space",null,"spaces"]
[]
[null,null,null,"Staff and Administration Areas",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"staff prep size based on rooms",null,null,null,null,null,null,null,null,null,null,null,{"$f":"ROUND(6+(BO61*2.1),0)","v":25},null,{"$f":"ROUND(6+(BQ61*2.1),0)","v":25},null,{"$f":"ROUND(6+(BS61*2.1),0)","v":21},null,{"$f":"ROUND(6+(BU61*2.1),0)","v":17},null,{"$f":"ROUND(6+(BW61*2.1),0)","v":14},null,{"$f":"ROUND(6+(BY61*2.1),0)","v":27},null,{"$f":"ROUND(6+(CA61*2.1),0)","v":21},null,{"$f":"ROUND(6+(CC61*2.1),0)","v":10},null,{"$f":"ROUND(6+(CE61*2.1),0)","v":6},null,{"$f":"ROUND(6+(CG61*2.1),0)","v":6},null,{"$f":"ROUND(6+(CI61*2.1),0)","v":6},null,{"$f":"ROUND(6+(CK61*2.1),0)","v":6}]
[{"$f":"VLOOKUP($D104,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"OFF30"},null,{"$f":"VLOOKUP($D104,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"OFF33"},"Staff workrooms (teaching staff)",null,null,null,null,null,null,null,null,{"$f":"IF(D104=\"\",\"\",_xlfn.XLOOKUP(D104,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Staff workrooms (teaching staff)"},{"$f":"CONCATENATE(M104,S104)","v":"Staff workrooms (teaching staff)19"},null,null,{"$f":"IF(S104>0,ROUND((S104-VLOOKUP(AU104,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU104,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":7},null,{"$f":"AI104","v":19},null,{"$f":"AK104","v":5},{"$f":"MAXA((S104*U104)-Y104,0)","v":95},null,null,null,null,{"$f":"IF(O104=\"retained\",V104+Y104,IF(O104=\"refurb'ed\",V104+Y104,0))","v":0},null,null,null,null,null,null,null,{"$f":"(ROUNDUP(K8/100,0)*2)-4-IF(K8/50>10,1,0)","v":19},null,5,null,null,null,{"$f":"IF(P104=\"existing\",\"E\",\"\")","v":""},null,12,35,{"$f":"MAXA((AI104*AK104)-AT104,0)","v":95},null,{"$f":"VLOOKUP(D104,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"D"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N104,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N104,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N104)","v":5},{"$f":"IF(ISERROR(BE104*BG104)=TRUE,\"\",BE104*BG104)","v":""},null,{"$f":"IF(ISERROR(BH104-Y104-V104)=TRUE,\"\",BH104-Y104-V104)","v":""},{"$f":"BG104-U104","v":0},null,{"$f":"SUM(BO104:CK104)","v":5},null,1,null,1,null,1,null,null,null,null,null,1,null,1,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S104>0,VLOOKUP($D104,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"varies"},{"$f":"IF($S104>0,VLOOKUP($D104,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D104,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D104,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},9,{"$f":"IF(CS104>14,IF(CS104<31,CS104,ROUNDDOWN(CS104/30,0)*30),0)","v":0},{"$f":"IF(S104>0,(V104/S104)*CT104,0)","v":0},{"$f":"IF(CS104>0,(V104/S104)*CS104,0)-CU104","v":45},{"$f":"IF(AK104=0,0,MAXA(1,ROUNDUP((AI104/CQ104)-CR104,0)))","v":9},{"$f":"IF(CW104>14,IF(CW104<31,CW104,ROUNDDOWN(CW104/30,0)*30),0)","v":0},{"$f":"IF(AK104>0,(AS104/AI104)*CX104,0)","v":0},{"$f":"IF(CW104>0,(AS104/AI104)*CW104,0)-CY104","v":45},"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C104,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":9},{"$f":"VLOOKUP($C104,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C104,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI104,VLOOKUP($C104,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":19},{"$f":"VLOOKUP($C104,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C104,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":50},{"$f":"IF(ISERROR((SUM($EB104,$EH104,$EN104,$EU104)/SUM($EA104,$EG104,$EM104,$ET104)-$S104))=TRUE,0,IF($U104=0,0,(SUM($EB104,$EH104,$EN104,$EU104)/SUM($EA104,$EG104,$EM104,$ET104)-$S104)))","v":0},null,{"$f":"SUM(EA104,EG104,EM104,ET104)-U104","v":-5},{"$f":"SUM($EU104,$EN104,$EH104,$EB104)-$V104-$Y104","v":-95},null,null,0,null,null,{"$f":"EA104*DY104","v":0},null,null,0,null,0,{"$f":"EG104*EE104","v":0},null,null,{"$f":"IF(EN104>0,SUM(EN104/EM104),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY104:$YD104,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY104:$YD104)","v":0},null,null,null,{"$f":"IF(EU104>0,SUM(EU104/ET104),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY104:$YD104,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY104:$YD104)","v":0}]
[{"$f":"VLOOKUP($D105,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"OFF30"},null,{"$f":"VLOOKUP($D105,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"OFF32"},"Staff workrooms (smaller teaching team)",null,null,null,null,null,null,null,null,{"$f":"IF(D105=\"\",\"\",_xlfn.XLOOKUP(D105,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Staff workrooms (smaller teaching team)"},"Staff workrooms (smaller teaching team)15",null,null,{"$f":"IF(S105>0,ROUND((S105-VLOOKUP(AU105,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU105,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":5},null,15,null,3,45,null,null,null,null,{"$f":"IF(O105=\"retained\",V105+Y105,IF(O105=\"refurb'ed\",V105+Y105,0))","v":0},null,null,null,null,null,null,null,{"$f":"MAXA(ROUND((AI104+3)*2/3,0),9)","v":15},null,{"$f":"IF(K6>0,3,1)","v":3},null,null,null,{"$f":"IF(P105=\"existing\",\"E\",\"\")","v":""},null,12,35,45,null,{"$f":"VLOOKUP(D105,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"D"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N105,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N105,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N105)","v":3},"",null,"",0,null,3,null,null,null,null,null,null,null,1,null,{"$f":"IF(K6>0,1,0)","v":1},null,null,null,null,null,{"$f":"IF(K6>0,1,0)","v":1},null,null,null,null,null,null,null,null,null,{"$f":"IF($S105>0,VLOOKUP($D105,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"varies"},{"$f":"IF($S105>0,VLOOKUP($D105,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D105,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D105,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},6,0,0,18,6,0,0,18,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C105,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":9},{"$f":"VLOOKUP($C105,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C105,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI105,VLOOKUP($C105,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":15},{"$f":"VLOOKUP($C105,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C105,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":50},0,null,-3,-45,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY105:$YD105,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY105:$YD105)","v":0}]
[{"$f":"VLOOKUP($D106,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"OFF50"},null,{"$f":"VLOOKUP($D106,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"OFF52"},{"$f":"IF(AD103=\"central staff room\",\"Staff rooms (prep and social)\",\"Staff rooms (social)\")","v":"Staff rooms (social)"},null,null,null,null,null,null,null,null,{"$f":"IF(D106=\"\",\"\",_xlfn.XLOOKUP(D106,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Staff room (social)"},"Staff room (social)41",null,null,{"$f":"IF(S106>0,ROUND((S106-VLOOKUP(AU106,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU106,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":24},null,41,null,1,41,null,null,null,null,0,null,"including kitchenette and pigeon holes",null,null,null,null,null,{"$f":"(ROUND(MAX(34,ROUND(K8/25,0),O130-SUM(AS104:AS105)-SUM(AS107:AS129),0)/7,0)*7)-1","v":41},null,1,null,null,null,"",null,30,140,41,null,{"$f":"VLOOKUP(D106,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"B"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N106,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N106,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N106)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U106","v":1},null,null,null,null,null,{"$f":"IF($S106>0,VLOOKUP($D106,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"varies"},{"$f":"IF($S106>0,VLOOKUP($D106,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D106,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D106,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},24,24,24,0,24,24,24,0,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C106,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":12},{"$f":"VLOOKUP($C106,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C106,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI106,VLOOKUP($C106,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":41},{"$f":"VLOOKUP($C106,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C106,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":150},0,null,-1,-41,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY106:$YD106,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY106:$YD106)","v":0}]
[{"$f":"VLOOKUP($D107,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"OFF40"},null,{"$f":"VLOOKUP($D107,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"OFF40"},"Meeting rooms (conference)",null,null,null,null,null,null,null,null,{"$f":"IF(D107=\"\",\"\",_xlfn.XLOOKUP(D107,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Meeting room (conference)"},"Meeting room (conference)19",null,null,{"$f":"IF(S107>0,ROUND((S107-VLOOKUP(AU107,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU107,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":9},null,19,null,1,19,null,null,null,null,0,null,null,null,null,null,null,null,{"$f":"MAXA(16,ROUND(K8/60,0))","v":19},null,{"$f":"IF($K8>750,1,0)","v":1},null,null,null,"",null,16,48,19,null,{"$f":"VLOOKUP(D107,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"C"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N107,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N107,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N107)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U107","v":1},null,null,null,null,null,{"$f":"IF($S107>0,VLOOKUP($D107,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"varies"},{"$f":"IF($S107>0,VLOOKUP($D107,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D107,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D107,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},9,0,0,9,9,0,0,9,{"$f":"ROUNDUP(((DB108-4)/1.6),0)","v":-3},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C107,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":12},{"$f":"VLOOKUP($C107,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C107,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI107,VLOOKUP($C107,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":19},{"$f":"VLOOKUP($C107,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C107,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":50},0,null,-1,-19,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY107:$YD107,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY107:$YD107)","v":0}]
[{"$f":"VLOOKUP($D108,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"ADM32"},null,{"$f":"VLOOKUP($D108,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"ADM32"},"Reception areas, community (50% circulation)",null,null,null,null,null,null,null,null,{"$f":"IF(D108=\"\",\"\",_xlfn.XLOOKUP(D108,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Reception area, community (50% circulation)"},"Reception area, community (50% circulation)8",null,null,"-",null,{"$f":"AI108+AJ108","v":8},null,1,{"$f":"MAXA((S108*U108)-Y108,0)-W108","v":4},{"$f":"(S108*U108)/2","v":4},null,null,null,0,null,"for community use outside core hours",null,null,null,null,null,4,4,1,null,null,null,"",null,null,null,4,null,{"$f":"VLOOKUP(D108,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"-"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N108,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N108,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N108)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U108","v":1},null,null,null,null,null,null,null,{"$f":"IF($S108>0,VLOOKUP($D108,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"[4m2]"},{"$f":"IF($S108>0,VLOOKUP($D108,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D108,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D108,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},2,0,0,1,1,0,0,1,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C108,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":4},{"$f":"VLOOKUP($C108,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C108,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI108,VLOOKUP($C108,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":4},{"$f":"VLOOKUP($C108,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C108,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,-1,-4,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY108:$YD108,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY108:$YD108)","v":0}]
[{"$f":"VLOOKUP($D109,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"ADM22"},null,{"$f":"VLOOKUP($D109,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"ADM22"},"Kitchenettes, bay",null,null,null,null,null,null,null,null,{"$f":"IF(D109=\"\",\"\",_xlfn.XLOOKUP(D109,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Kitchenette, bay"},"Kitchenette, bay3",{"$f":"IF(VLOOKUP(D109,'Prog Assums'!N$173:V$306,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S109>0,ROUND((S109-VLOOKUP(AU109,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU109,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":1},null,3,null,5,15,null,null,null,null,0,null,{"$f":"IF(D109=\"Kitchenettes, bay\",\"off each Staff workroom (teaching staff)\",\"\")","v":"off each Staff workroom (teaching staff)"},null,null,null,null,null,3,null,{"$f":"AK104","v":5},null,null,null,"",null,null,null,15,null,{"$f":"VLOOKUP(D109,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"B"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N109,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N109,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N109)","v":5},"",null,"",0,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U109","v":5},null,null,null,null,null,{"$f":"IF($S109>0,VLOOKUP($D109,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"4m2"},{"$f":"IF($S109>0,VLOOKUP($D109,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D109,'Prog Assums'!$N$6:$Q$229,3,0)","v":2.5},{"$f":"VLOOKUP(D109,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},1,0,0,5,1,0,0,5,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C109,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":4},{"$f":"VLOOKUP($C109,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C109,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI109,VLOOKUP($C109,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":4},{"$f":"VLOOKUP($C109,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C109,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":12},0,null,-5,-15,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY109:$YD109,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY109:$YD109)","v":0}]
[{"$f":"VLOOKUP($D110,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D110,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},{"$f":"IF(K12>0,\"Staff workrooms (specially resourced)\",\"-\")","v":"-"},null,null,null,null,null,null,null,null,{"$f":"IF(D110=\"\",\"\",_xlfn.XLOOKUP(D110,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},"-0",{"$f":"IF(VLOOKUP(D110,'Prog Assums'!N$173:V$306,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S110>0,ROUND((S110-VLOOKUP(AU110,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU110,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":"-"},null,0,null,0,0,null,null,{"$f":"AT110","v":0},null,0,null,null,null,null,null,null,null,{"$f":"IF(K12>0,4+ROUND(K12*0.4,0),0)","v":0},null,{"$f":"IF(K12>0,1,0)","v":0},null,null,null,"",null,null,null,0,{"$f":"IF(D$11>0,AI110*AK110,0)","v":0},{"$f":"VLOOKUP(D110,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"-"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N110,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N110,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N110)","v":0},"",null,"",0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(K12>0,1,0)","v":0},null,null,null,{"$f":"IF($S110>0,VLOOKUP($D110,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S110>0,VLOOKUP($D110,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"VLOOKUP(D110,'Prog Assums'!$N$6:$Q$229,3,0)","v":0},{"$f":"VLOOKUP(D110,'Prog Assums'!$N$6:$Q$229,4,0)","v":0},0,{"$f":"IF(CS110>14,IF(CS110<31,CS110,ROUNDDOWN(CS110/30,0)*30),0)","v":0},0,0,0,0,0,0,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C110,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C110,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C110,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI110,VLOOKUP($C110,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C110,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C110,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY110:$YD110,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY110:$YD110)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S111>0,VLOOKUP($D111,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S111>0,VLOOKUP($D111,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""}]
[null,null,null,"Admin suite",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"reception desk options",null,null,null,"office with 2 recep desks",null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S112>0,VLOOKUP($D112,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S112>0,VLOOKUP($D112,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""}]
[{"$f":"VLOOKUP($D113,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"ADM10"},null,{"$f":"VLOOKUP($D113,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"ADM11"},"Enclosed offices, admin (head)",null,null,null,null,null,null,null,null,{"$f":"IF(D113=\"\",\"\",_xlfn.XLOOKUP(D113,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Enclosed office, admin (head)"},{"$f":"CONCATENATE(M113,S113)","v":"Enclosed office, admin (head)16"},null,null,{"$f":"IF(S113>0,ROUND((S113-VLOOKUP(AU113,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU113,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":6},null,{"$f":"AI113","v":16},null,{"$f":"AK113","v":1},{"$f":"MAXA((S113*U113)-Y113,0)","v":16},null,null,null,null,0,null,null,null,null,null,null,null,16,null,1,null,null,null,"",{"$f":"VLOOKUP(D113,'Prog Assums'!N$139:T$210,7, FALSE)","v":5},10,25,16,null,{"$f":"VLOOKUP(D113,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"D"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N113,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N113,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N113)","v":1},{"$f":"IF(ISERROR(BE113*BG113)=TRUE,\"\",BE113*BG113)","v":""},null,{"$f":"IF(ISERROR(BH113-Y113-V113)=TRUE,\"\",BH113-Y113-V113)","v":""},0,null,{"$f":"SUM(BO113:CK113)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,{"$f":"IF($S113>0,VLOOKUP($D113,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"16m2"},{"$f":"IF($S113>0,VLOOKUP($D113,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D113,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D113,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},7,{"$f":"IF(CS113>14,IF(CS113<31,CS113,ROUNDDOWN(CS113/30,0)*30),0)","v":0},{"$f":"IF(S113>0,(V113/S113)*CT113,0)","v":0},{"$f":"IF(CS113>0,(V113/S113)*CS113,0)-CU113","v":7},{"$f":"IF(AK113=0,0,MAXA(1,ROUNDUP((AI113/CQ113)-CR113,0)))","v":7},{"$f":"IF(CW113>14,IF(CW113<31,CW113,ROUNDDOWN(CW113/30,0)*30),0)","v":0},{"$f":"IF(AK113>0,(AS113/AI113)*CX113,0)","v":0},{"$f":"IF(CW113>0,(AS113/AI113)*CW113,0)-CY113","v":7},"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C113,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":9},{"$f":"VLOOKUP($C113,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C113,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI113,VLOOKUP($C113,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":16},{"$f":"VLOOKUP($C113,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C113,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":41},{"$f":"IF(ISERROR((SUM($EB113,$EH113,$EN113,$EU113)/SUM($EA113,$EG113,$EM113,$ET113)-$S113))=TRUE,0,IF($U113=0,0,(SUM($EB113,$EH113,$EN113,$EU113)/SUM($EA113,$EG113,$EM113,$ET113)-$S113)))","v":0},null,{"$f":"SUM(EA113,EG113,EM113,ET113)-U113","v":-1},{"$f":"SUM($EU113,$EN113,$EH113,$EB113)-$V113-$Y113","v":-16},null,null,0,null,0,{"$f":"EA113*DY113","v":0},null,null,0,null,0,{"$f":"EG113*EE113","v":0},null,null,{"$f":"IF(EN113>0,SUM(EN113/EM113),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY113:$YD113,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY113:$YD113)","v":0},null,null,null,{"$f":"IF(EU113>0,SUM(EU113/ET113),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY113:$YD113,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY113:$YD113)","v":0}]
[{"$f":"VLOOKUP($D114,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"ADM10"},null,{"$f":"VLOOKUP($D114,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"ADM13"},"Enclosed offices, admin (PA)",null,null,null,null,null,null,null,null,{"$f":"IF(D114=\"\",\"\",_xlfn.XLOOKUP(D114,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Enclosed office, admin (PA)"},"Enclosed office, admin (PA)8",{"$f":"IF(VLOOKUP(D114,'Prog Assums'!N$173:V$306,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S114>0,MAXA(0,ROUND((S114-VLOOKUP(AU114,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU114,'Prog Assums'!$E$38:$I$54,3,FALSE),0)),\"-\")","v":1},null,{"$f":"AI114","v":8},null,1,8,null,null,null,null,0,null,null,null,null,null,null,null,8,null,1,null,null,null,"",{"$f":"VLOOKUP(D114,'Prog Assums'!N$139:T$210,7, FALSE)","v":1},6,10,8,null,{"$f":"VLOOKUP(D114,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"K"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N114,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N114,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N114)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U114","v":1},null,null,null,null,null,{"$f":"IF($S114>0,VLOOKUP($D114,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"8m2"},{"$f":"IF($S114>0,VLOOKUP($D114,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D114,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D114,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},2,0,0,2,2,0,0,2,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C114,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":7},{"$f":"VLOOKUP($C114,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C114,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI114,VLOOKUP($C114,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":8},{"$f":"VLOOKUP($C114,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C114,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":12},0,null,-1,-8,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY114:$YD114,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY114:$YD114)","v":0}]
[{"$f":"VLOOKUP($D115,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"ADM08"},null,{"$f":"VLOOKUP($D115,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"ADM08"},"Reprographics rooms",null,null,null,null,null,null,null,null,{"$f":"IF(D115=\"\",\"\",_xlfn.XLOOKUP(D115,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Reprographics room"},"Reprographics room20",{"$f":"IF(VLOOKUP(D115,'Prog Assums'!N$173:V$306,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S115>0,MAXA(0,ROUND((S115-VLOOKUP(AU115,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU115,'Prog Assums'!$E$38:$I$54,3,FALSE),0)),\"-\")","v":4},null,{"$f":"AI115","v":20},null,1,20,null,null,null,null,0,null,null,null,null,null,null,null,{"$f":"(ROUND((K8/60)/7,0)*7)-1","v":20},null,1,null,null,null,"",null,null,null,20,null,{"$f":"VLOOKUP(D115,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"K"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N115,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N115,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N115)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,{"$f":"IF($S115>0,VLOOKUP($D115,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"varies"},{"$f":"IF($S115>0,VLOOKUP($D115,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D115,'Prog Assums'!$N$6:$Q$229,3,0)","v":2},{"$f":"VLOOKUP(D115,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},6,0,0,6,6,0,0,6,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C115,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":6},{"$f":"VLOOKUP($C115,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C115,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI115,VLOOKUP($C115,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":20},{"$f":"VLOOKUP($C115,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C115,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":100},0,null,-1,-20,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY115:$YD115,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY115:$YD115)","v":0}]
[{"$f":"VLOOKUP($D116,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"ADM05"},null,{"$f":"VLOOKUP($D116,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"ADM07"},{"$f":"IF(AG112=\"office with 2 recep desks\",\"Enclosed offices, with recep desk (and window)\",\"Enclosed offices, with recep desk (only)\")","v":"Enclosed offices, with recep desk (and window)"},null,null,null,null,null,null,null,null,{"$f":"IF(D116=\"\",\"\",_xlfn.XLOOKUP(D116,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Enclosed office, with recep desk (and window)"},"Enclosed office, with recep desk (and window)41",{"$f":"IF(VLOOKUP(D116,'Prog Assums'!N$173:V$306,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S116>0,MAXA(0,ROUND((S116-VLOOKUP(AU116,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU116,'Prog Assums'!$E$38:$I$54,3,FALSE),0)),\"-\")","v":10},null,41,null,1,41,null,null,null,null,0,null,"to match option above",null,null,null,null,null,{"$f":"(ROUNDUP((K8/30)/7,0)*7)-1-IF(AI117>0,AI117+1,0)","v":41},null,1,null,null,null,"",null,null,null,41,null,{"$f":"VLOOKUP(D116,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"K"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N116,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N116,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N116)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,{"$f":"IF($S116>0,VLOOKUP($D116,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"varies"},{"$f":"IF($S116>0,VLOOKUP($D116,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D116,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D116,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},24,{"$f":"IF(CS116>14,IF(CS116<31,CS116,ROUNDDOWN(CS116/30,0)*30),0)","v":24},24,0,24,24,24,0,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C116,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":8},{"$f":"VLOOKUP($C116,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C116,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI116,VLOOKUP($C116,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":41},{"$f":"VLOOKUP($C116,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C116,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":100},0,null,-1,-41,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY116:$YD116,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY116:$YD116)","v":0}]
[{"$f":"VLOOKUP($D117,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D117,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},{"$f":"IF(AG112=\"office and finance/student support\",\"Enclosed offices, with recep window\",\"-\")","v":"-"},null,null,null,null,null,null,null,null,{"$f":"IF(D117=\"\",\"\",_xlfn.XLOOKUP(D117,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"-"},"-0",{"$f":"IF(VLOOKUP(D117,'Prog Assums'!N$173:V$306,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S117>0,MAXA(0,ROUND((S117-VLOOKUP(AU117,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU117,'Prog Assums'!$E$38:$I$54,3,FALSE),0)),\"-\")","v":"-"},null,0,null,0,0,null,null,null,null,0,null,null,null,null,null,null,null,{"$f":"IF(AG112=\"office and finance/student support\",(ROUNDUP((K8/60)/7,0)*7)-1,0)","v":0},null,{"$f":"IF(AG112=\"office and finance/student support\",1,0)","v":0},null,null,null,"",null,null,null,0,null,{"$f":"VLOOKUP(D117,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"-"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N117,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N117,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N117)","v":0},"",null,"",0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,{"$f":"IF($S117>0,VLOOKUP($D117,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S117>0,VLOOKUP($D117,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"VLOOKUP(D117,'Prog Assums'!$N$6:$Q$229,3,0)","v":0},{"$f":"VLOOKUP(D117,'Prog Assums'!$N$6:$Q$229,4,0)","v":0},0,0,0,0,0,0,0,0,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C117,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C117,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C117,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI117,VLOOKUP($C117,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C117,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C117,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY117:$YD117,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY117:$YD117)","v":0}]
[{"$f":"VLOOKUP($D118,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"ADM31"},null,{"$f":"VLOOKUP($D118,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"ADM31"},"Reception areas, entrance (50% circulation)",null,null,null,null,null,null,null,null,{"$f":"IF(D118=\"\",\"\",_xlfn.XLOOKUP(D118,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Reception area, entrance (50% circulation)"},"Reception area, entrance (50% circulation)16",null,null,"-",null,{"$f":"AI118+AJ118","v":16},null,1,{"$f":"MAXA((S118*U118)-Y118,0)-W118","v":8},{"$f":"(S118*U118)/2","v":8},null,null,null,0,null,"net area of this space only",null,null,null,null,null,8,8,1,null,null,null,"",null,3,15,8,null,{"$f":"VLOOKUP(D118,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"-"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N118,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N118,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N118)","v":0},"",null,"",-1,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,{"$f":"IF($S118>0,VLOOKUP($D118,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"[6m2]"},{"$f":"IF($S118>0,VLOOKUP($D118,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D118,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D118,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},7,0,0,3.5,2,0,0,2,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C118,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":4},{"$f":"VLOOKUP($C118,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C118,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI118,VLOOKUP($C118,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":8},{"$f":"VLOOKUP($C118,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C118,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,-1,-8,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY118:$YD118,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY118:$YD118)","v":0}]
[{"$f":"VLOOKUP($D119,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"ADM02"},null,{"$f":"VLOOKUP($D119,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"ADM02"},"Confidential meetings rooms (interview)",null,null,null,null,null,null,null,null,{"$f":"IF(D119=\"\",\"\",_xlfn.XLOOKUP(D119,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Confidential meeting room (interview)"},"Confidential meeting room (interview)6",null,null,{"$f":"IF(S119>0,ROUND((S119-VLOOKUP(AU119,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU119,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":4},null,6,null,1,6,null,null,null,null,0,null,"adjacent to entrance/reception",null,null,null,null,null,6,null,1,null,null,null,"",null,6,9,6,null,{"$f":"VLOOKUP(D119,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"A"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N119,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N119,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N119)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,{"$f":"IF($S119>0,VLOOKUP($D119,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"6m2 for 3"},{"$f":"IF($S119>0,VLOOKUP($D119,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D119,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D119,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},1,0,0,1,1,0,0,1,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C119,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":4},{"$f":"VLOOKUP($C119,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C119,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI119,VLOOKUP($C119,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":6},{"$f":"VLOOKUP($C119,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C119,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,-1,-6,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY119:$YD119,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY119:$YD119)","v":0}]
[{"$f":"VLOOKUP($D120,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"ADM03"},null,{"$f":"VLOOKUP($D120,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"ADM03"},"First aid posts (sick bay)",null,null,null,null,null,null,null,null,{"$f":"IF(D120=\"\",\"\",_xlfn.XLOOKUP(D120,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"First aid post (sick bay)"},"First aid post (sick bay)6",null,null,{"$f":"IF(S120>0,ROUND((S120-VLOOKUP(AU120,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU120,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":3},null,6,null,1,6,null,null,null,null,0,null,"adjacent to entrance/reception",null,null,null,null,null,{"$f":"IF(K8>1200,9,6)","v":6},null,1,null,null,null,"",null,6,9,6,null,{"$f":"VLOOKUP(D120,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"B"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N120,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N120,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N120)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,{"$f":"IF($S120>0,VLOOKUP($D120,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"6m2"},{"$f":"IF($S120>0,VLOOKUP($D120,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D120,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D120,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},1,{"$f":"IF(CS120>14,IF(CS120<31,CS120,ROUNDDOWN(CS120/30,0)*30),0)","v":0},0,1,1,0,0,1,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C120,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":4},{"$f":"VLOOKUP($C120,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C120,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI120,VLOOKUP($C120,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":6},{"$f":"VLOOKUP($C120,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C120,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,-1,-6,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY120:$YD120,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY120:$YD120)","v":0}]
[null,null,null,"Offices",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(no. of offices",{"$f":"U113+U114+SUM(U122:U129)","v":19},")",null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S121>0,VLOOKUP($D121,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S121>0,VLOOKUP($D121,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""}]
[{"$f":"VLOOKUP($D122,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"OFF00"},null,{"$f":"VLOOKUP($D122,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"OFF01"},"Offices (1-person)",null,null,null,null,null,null,null,null,{"$f":"IF(D122=\"\",\"\",_xlfn.XLOOKUP(D122,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Office (1-person)"},{"$f":"CONCATENATE(M122,S122)","v":"Office (1-person)7"},null,null,{"$f":"IF(S122>0,ROUND((S122-VLOOKUP(AU122,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU122,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":1},null,7,null,{"$f":"AK122","v":5},{"$f":"MAXA((S122*U122)-Y122,0)","v":35},null,null,null,null,0,null,"e.g. assistant head or pastoral head",null,null,null,null,null,7,null,{"$f":"ROUND(($K8/300),0)+IF(K6>0,1,0)","v":5},null,null,null,"",{"$f":"VLOOKUP(D122,'Prog Assums'!N$139:T$210,7, FALSE)","v":1},{"$f":"ROUNDDOWN(VLOOKUP(AU122,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP122*VLOOKUP(AU122,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":6},{"$f":"ROUNDUP(VLOOKUP(AU122,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP122*VLOOKUP(AU122,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":9},35,null,{"$f":"VLOOKUP(D122,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"D"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N122,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N122,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N122)","v":5},{"$f":"IF(ISERROR(BE122*BG122)=TRUE,\"\",BE122*BG122)","v":""},null,{"$f":"IF(ISERROR(BH122-Y122-V122)=TRUE,\"\",BH122-Y122-V122)","v":""},0,null,{"$f":"SUM(BO122:CK122)","v":5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U122","v":5},null,{"$f":"IF($S122>0,VLOOKUP($D122,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"7m2 for 1"},{"$f":"IF($S122>0,VLOOKUP($D122,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D122,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D122,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},1,{"$f":"IF(CS122>14,IF(CS122<31,CS122,ROUNDDOWN(CS122/30,0)*30),0)","v":0},{"$f":"IF(S122>0,(V122/S122)*CT122,0)","v":0},{"$f":"IF(CS122>0,(V122/S122)*CS122,0)-CU122","v":5},{"$f":"IF(AK122=0,0,MAXA(1,ROUNDUP((AI122/CQ122)-CR122,0)))","v":1},{"$f":"IF(CW122>14,IF(CW122<31,CW122,ROUNDDOWN(CW122/30,0)*30),0)","v":0},{"$f":"IF(AK122>0,(AS122/AI122)*CX122,0)","v":0},{"$f":"IF(CW122>0,(AS122/AI122)*CW122,0)-CY122","v":5},"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C122,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":6},{"$f":"VLOOKUP($C122,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C122,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI122,VLOOKUP($C122,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":7},{"$f":"VLOOKUP($C122,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C122,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":9},{"$f":"IF(ISERROR((SUM($EB122,$EH122,$EN122,$EU122)/SUM($EA122,$EG122,$EM122,$ET122)-$S122))=TRUE,0,IF($U122=0,0,(SUM($EB122,$EH122,$EN122,$EU122)/SUM($EA122,$EG122,$EM122,$ET122)-$S122)))","v":0},null,{"$f":"SUM(EA122,EG122,EM122,ET122)-U122","v":-5},{"$f":"SUM($EU122,$EN122,$EH122,$EB122)-$V122-$Y122","v":-35},null,null,0,null,0,{"$f":"EA122*DY122","v":0},null,null,0,null,0,{"$f":"EG122*EE122","v":0},null,null,{"$f":"IF(EN122>0,SUM(EN122/EM122),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY122:$YD122,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY122:$YD122)","v":0},null,null,null,{"$f":"IF(EU122>0,SUM(EU122/ET122),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY122:$YD122,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY122:$YD122)","v":0}]
[{"$f":"VLOOKUP($D123,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"OFF00"},null,{"$f":"VLOOKUP($D123,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"OFF11"},"Offices (with meeting area, 1-person)",null,null,null,null,null,null,null,null,{"$f":"IF(D123=\"\",\"\",_xlfn.XLOOKUP(D123,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Office (with meeting area, 1-person)"},"Office (with meeting area, 1-person)9",null,null,{"$f":"IF(S123>0,ROUND((S123-VLOOKUP(AU123,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU123,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":3},null,9,null,{"$f":"AK123","v":8},72,null,null,null,null,0,null,null,null,null,null,null,null,9,null,{"$f":"ROUND(($K5/600),0)+5+IF(K6>0,1,0)","v":8},null,null,null,"",{"$f":"VLOOKUP(D123,'Prog Assums'!N$139:T$210,7, FALSE)","v":3},{"$f":"ROUNDDOWN(VLOOKUP(AU123,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP123*VLOOKUP(AU123,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":9},{"$f":"ROUNDUP(VLOOKUP(AU123,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP123*VLOOKUP(AU123,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":11},72,null,{"$f":"VLOOKUP(D123,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"C"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N123,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N123,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N123)","v":8},"",null,"",0,null,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U123","v":8},null,{"$f":"IF($S123>0,VLOOKUP($D123,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"9m2 for 1+2"},{"$f":"IF($S123>0,VLOOKUP($D123,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D123,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D123,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},2,0,0,16,2,0,0,16,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C123,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":6},{"$f":"VLOOKUP($C123,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C123,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI123,VLOOKUP($C123,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":9},{"$f":"VLOOKUP($C123,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C123,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":13},0,null,-8,-72,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY123:$YD123,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY123:$YD123)","v":0}]
[{"$f":"VLOOKUP($D124,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"OFF00"},null,{"$f":"VLOOKUP($D124,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"OFF02"},"Offices (2-person)",null,null,null,null,null,null,null,null,{"$f":"IF(D124=\"\",\"\",_xlfn.XLOOKUP(D124,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Office (2-person)"},"Office (2-person)9",{"$f":"IF(VLOOKUP(D124,'Prog Assums'!N$173:V$306,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S124>0,ROUND((S124-VLOOKUP(AU124,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU124,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":2},null,{"$f":"VLOOKUP(D124,'Prog Assums'!N$173:T$212,5,FALSE)","v":9},null,0,0,null,null,null,null,0,null,null,null,null,null,null,null,9,null,null,null,null,null,"",{"$f":"VLOOKUP(D124,'Prog Assums'!N$139:T$210,7, FALSE)","v":2},{"$f":"ROUNDDOWN(VLOOKUP(AU124,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP124*VLOOKUP(AU124,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":8},{"$f":"ROUNDUP(VLOOKUP(AU124,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP124*VLOOKUP(AU124,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":11},0,null,{"$f":"VLOOKUP(D124,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"D"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N124,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N124,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N124)","v":0},"",null,"",0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U124","v":0},null,{"$f":"IF($S124>0,VLOOKUP($D124,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"9m2 for 2"},{"$f":"IF($S124>0,VLOOKUP($D124,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D124,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D124,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},2,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C124,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":6},{"$f":"VLOOKUP($C124,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C124,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI124,VLOOKUP($C124,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":9},{"$f":"VLOOKUP($C124,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C124,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":11},0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY124:$YD124,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY124:$YD124)","v":0}]
[{"$f":"VLOOKUP($D125,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"OFF00"},null,{"$f":"VLOOKUP($D125,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"OFF12"},"Offices (with meeting area, 2-person)",null,null,null,null,null,null,null,null,{"$f":"IF(D125=\"\",\"\",_xlfn.XLOOKUP(D125,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Office (with meeting area, 2-person)"},"Office (with meeting area, 2-person)11",{"$f":"IF(VLOOKUP(D125,'Prog Assums'!N$173:V$306,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S125>0,ROUND((S125-VLOOKUP(AU125,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU125,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":4},null,{"$f":"VLOOKUP(D125,'Prog Assums'!N$173:T$212,5,FALSE)","v":11},null,0,0,null,null,null,null,0,null,null,null,null,null,null,null,13,null,null,null,null,null,"",{"$f":"VLOOKUP(D125,'Prog Assums'!N$139:T$210,7, FALSE)","v":5},{"$f":"ROUNDDOWN(VLOOKUP(AU125,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP125*VLOOKUP(AU125,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":12},{"$f":"ROUNDUP(VLOOKUP(AU125,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP125*VLOOKUP(AU125,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":15},0,null,{"$f":"VLOOKUP(D125,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"C"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N125,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N125,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N125)","v":0},"",null,"",0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U125","v":0},null,{"$f":"IF($S125>0,VLOOKUP($D125,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"13m2 for 2+3"},{"$f":"IF($S125>0,VLOOKUP($D125,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D125,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D125,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},4,0,0,0,0,0,0,0,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C125,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":6},{"$f":"VLOOKUP($C125,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C125,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI125,VLOOKUP($C125,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":13},{"$f":"VLOOKUP($C125,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C125,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":16},0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY125:$YD125,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY125:$YD125)","v":0}]
[{"$f":"VLOOKUP($D126,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"OFF00"},null,{"$f":"VLOOKUP($D126,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"OFF06"},"Offices (exams)",null,null,null,null,null,null,null,null,{"$f":"IF(D126=\"\",\"\",_xlfn.XLOOKUP(D126,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Office (exams)"},{"$f":"CONCATENATE(M126,S126)","v":"Office (exams)9"},{"$f":"IF(VLOOKUP(D126,'Prog Assums'!N$173:V$306,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S126>0,ROUND((S126-VLOOKUP(AU126,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU126,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":2},null,{"$f":"VLOOKUP(D126,'Prog Assums'!N$173:T$212,5,FALSE)","v":9},null,{"$f":"AK126","v":1},{"$f":"MAXA((S126*U126)-Y126,0)","v":9},null,null,null,null,{"$f":"IF(O126=\"retained\",V126+Y126,IF(O126=\"refurb'ed\",V126+Y126,0))","v":0},null,null,null,null,null,null,null,9,null,1,null,null,null,{"$f":"IF(P126=\"existing\",\"E\",\"\")","v":""},{"$f":"VLOOKUP(D126,'Prog Assums'!N$139:T$210,7, FALSE)","v":2},{"$f":"ROUNDDOWN(VLOOKUP(AU126,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP126*VLOOKUP(AU126,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":8},{"$f":"ROUNDUP(VLOOKUP(AU126,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP126*VLOOKUP(AU126,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":11},{"$f":"MAXA((AI126*AK126)-AT126,0)","v":9},null,{"$f":"VLOOKUP(D126,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"D"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N126,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N126,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N126)","v":1},{"$f":"IF(ISERROR(BE126*BG126)=TRUE,\"\",BE126*BG126)","v":""},null,{"$f":"IF(ISERROR(BH126-Y126-V126)=TRUE,\"\",BH126-Y126-V126)","v":""},{"$f":"BG126-U126","v":0},null,{"$f":"SUM(BO126:CK126)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U126","v":1},null,null,null,{"$f":"IF($S126>0,VLOOKUP($D126,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"9m2 for 2"},{"$f":"IF($S126>0,VLOOKUP($D126,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D126,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D126,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},{"$f":"IF(S126=0,0,MAXA(1,ROUNDUP((S126/CQ126)-CR126,0)))","v":2},{"$f":"IF(CS126>14,IF(CS126<31,CS126,ROUNDDOWN(CS126/30,0)*30),0)","v":0},{"$f":"IF(S126>0,(V126/S126)*CT126,0)","v":0},{"$f":"IF(CS126>0,(V126/S126)*CS126,0)-CU126","v":2},{"$f":"IF(AK126=0,0,MAXA(1,ROUNDUP((AI126/CQ126)-CR126,0)))","v":2},{"$f":"IF(CW126>14,IF(CW126<31,CW126,ROUNDDOWN(CW126/30,0)*30),0)","v":0},{"$f":"IF(AK126>0,(AS126/AI126)*CX126,0)","v":0},{"$f":"IF(CW126>0,(AS126/AI126)*CW126,0)-CY126","v":2},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C126,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":6},{"$f":"VLOOKUP($C126,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C126,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI126,VLOOKUP($C126,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":9},{"$f":"VLOOKUP($C126,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C126,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,{"$f":"SUM(EA126,EG126,EM126,ET126)-U126","v":-1},-9,null,null,0,null,0,{"$f":"EA126*DY126","v":0},null,null,0,null,0,{"$f":"EG126*EE126","v":0},null,null,{"$f":"IF(EN126>0,SUM(EN126/EM126),0)","v":0},null,0,0,null,null,null,{"$f":"IF(EU126>0,SUM(EU126/ET126),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY126:$YD126,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY126:$YD126)","v":0}]
[{"$f":"VLOOKUP($D127,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"OFF00"},null,{"$f":"VLOOKUP($D127,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"OFF23"},"Offices (SENco, learning support)",null,null,null,null,null,null,null,null,{"$f":"IF(D127=\"\",\"\",_xlfn.XLOOKUP(D127,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Office (SENco, learning support)"},"Office (SENco, learning support)11",{"$f":"IF(VLOOKUP(D127,'Prog Assums'!N$173:V$306,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S127>0,ROUND((S127-VLOOKUP(AU127,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU127,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":4},null,{"$f":"VLOOKUP(D127,'Prog Assums'!N$173:T$212,5,FALSE)","v":11},null,1,11,null,null,null,null,0,null,"e.g. SENco and learning support",null,null,null,null,null,11,null,1,null,null,null,"",{"$f":"VLOOKUP(D127,'Prog Assums'!N$139:T$210,7, FALSE)","v":4},{"$f":"ROUNDDOWN(VLOOKUP(AU127,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP127*VLOOKUP(AU127,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":10},{"$f":"ROUNDUP(VLOOKUP(AU127,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP127*VLOOKUP(AU127,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":13},11,null,{"$f":"VLOOKUP(D127,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"C"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N127,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N127,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N127)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U127","v":1},null,null,null,{"$f":"IF($S127>0,VLOOKUP($D127,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"12m2 for 1+3"},{"$f":"IF($S127>0,VLOOKUP($D127,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D127,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D127,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},4,{"$f":"IF(CS127>14,IF(CS127<31,CS127,ROUNDDOWN(CS127/30,0)*30),0)","v":0},0,4,4,0,0,4,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C127,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":6},{"$f":"VLOOKUP($C127,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C127,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI127,VLOOKUP($C127,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":11},{"$f":"VLOOKUP($C127,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C127,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,-1,-11,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY127:$YD127,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY127:$YD127)","v":0}]
[{"$f":"VLOOKUP($D128,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"OFF30"},null,{"$f":"VLOOKUP($D128,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"OFF37"},"Staff workrooms (ICT technicians)",null,null,null,null,null,null,null,null,{"$f":"IF(D128=\"\",\"\",_xlfn.XLOOKUP(D128,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Staff workroom (ICT technicians)"},"Staff workroom (ICT technicians)11",{"$f":"IF(VLOOKUP(D128,'Prog Assums'!N$173:V$306,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S128>0,ROUND((S128-VLOOKUP(AU128,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU128,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":2},null,{"$f":"VLOOKUP(D128,'Prog Assums'!N$173:T$212,5,FALSE)","v":11},null,1,11,null,null,null,null,0,null,null,null,null,null,null,null,11,null,1,null,null,null,"",{"$f":"VLOOKUP(D128,'Prog Assums'!N$139:T$210,7, FALSE)","v":2},{"$f":"ROUNDDOWN(VLOOKUP(AU128,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP128*VLOOKUP(AU128,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":10},{"$f":"ROUNDUP(VLOOKUP(AU128,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP128*VLOOKUP(AU128,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":12},11,null,{"$f":"VLOOKUP(D128,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"E"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N128,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N128,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N128)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U128","v":1},null,{"$f":"IF($S128>0,VLOOKUP($D128,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"11m2 for 2"},{"$f":"IF($S128>0,VLOOKUP($D128,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D128,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D128,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},4,0,0,4,4,0,0,4,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C128,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":8},{"$f":"VLOOKUP($C128,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C128,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI128,VLOOKUP($C128,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":11},{"$f":"VLOOKUP($C128,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C128,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,-1,-11,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY128:$YD128,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY128:$YD128)","v":0}]
[{"$f":"VLOOKUP($D129,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"OFF30"},null,{"$f":"VLOOKUP($D129,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"OFF38"},"Staff workrooms (premises)",null,null,null,null,null,null,null,null,{"$f":"IF(D129=\"\",\"\",_xlfn.XLOOKUP(D129,'Prog Assums'!$N$7:$N$221,'Prog Assums'!$AQ$7:$AQ$221,\"\"))","v":"Staff workroom (premises)"},"Staff workroom (premises)11",{"$f":"IF(VLOOKUP(D129,'Prog Assums'!N$173:V$306,9,FALSE)>0,\"retained\",\"\")","v":""},null,{"$f":"IF(S129>0,ROUND((S129-VLOOKUP(AU129,'Prog Assums'!$E$38:$I$54,2,FALSE))/VLOOKUP(AU129,'Prog Assums'!$E$38:$I$54,3,FALSE),0),\"-\")","v":2},null,{"$f":"VLOOKUP(D129,'Prog Assums'!N$173:T$212,5,FALSE)","v":11},null,1,11,null,null,null,null,0,null,null,null,null,null,null,null,11,null,1,null,null,null,"",{"$f":"VLOOKUP(D129,'Prog Assums'!N$139:T$210,7, FALSE)","v":2},{"$f":"ROUNDDOWN(VLOOKUP(AU129,'Prog Assums'!$E$38:$I$54,2,FALSE)+(AP129*VLOOKUP(AU129,'Prog Assums'!$E$38:$I$54,3,FALSE)),0)","v":10},{"$f":"ROUNDUP(VLOOKUP(AU129,'Prog Assums'!$E$38:$I$54,4,FALSE)+(AP129*VLOOKUP(AU129,'Prog Assums'!$E$38:$I$54,5,FALSE)),0)","v":12},11,null,{"$f":"VLOOKUP(D129,'Prog Assums'!$N$173:$O$211,2,FALSE)","v":"E"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N129,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N129,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N129)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U129","v":1},null,{"$f":"IF($S129>0,VLOOKUP($D129,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"11m2 for 2"},{"$f":"IF($S129>0,VLOOKUP($D129,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D129,'Prog Assums'!$N$6:$Q$229,3,0)","v":1.5},{"$f":"VLOOKUP(D129,'Prog Assums'!$N$6:$Q$229,4,0)","v":4},4,0,0,4,4,0,0,4,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C129,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":8},{"$f":"VLOOKUP($C129,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C129,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI129,VLOOKUP($C129,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":11},{"$f":"VLOOKUP($C129,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C129,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,-1,-11,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY129:$YD129,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY129:$YD129)","v":0}]
[null,null,null,"TOTAL AREA",null,null,null,null,null,null,null,"BB103 range","BB103 range","BB103 range",{"$f":"ROUND(IF(K$4>0,75,100)+((K$4+K$5+K$6)*0.2),0)","v":325},"to",{"$f":"ROUND(IF(AR$8>0,125,175)+IF(K6>0,25,0)+(K$4*0.35)+(K$5*0.35)+(K$6*0.3),0)","v":583},null,null,null,null,{"$f":"SUM(V104:V129)","v":473},{"$f":"SUM(W104:W129)","v":12},null,{"$f":"SUM(Y104:Y129)","v":0},null,{"$f":"SUM(AA104:AA129)","v":0},null,{"$f":"IF(V130<O130,\"ERROR: total area for category is too low\",IF(V130>Q130,\"WARNING: total area for category is high\",\"OK: area within BB103 range\"))","v":"OK: area within BB103 range"},null,null,null,null,null,{"$f":"SUM(AS104:AS129)","v":473},null,{"$f":"SUM(AT104:AT129)","v":0},null,null,null,{"$f":"IF(Q130=\"existing\",\"E\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(BH104:BH129)","v":0},null,{"$f":"BH130-Y130-V130","v":-473},null,null,null,null,{"$f":"SUM(BO104:BO129)","v":1},null,{"$f":"SUM(BQ104:BQ129)","v":1},null,{"$f":"SUM(BS104:BS129)","v":1},null,{"$f":"SUM(BU104:BU129)","v":1},null,{"$f":"SUM(BW104:BW129)","v":1},null,{"$f":"SUM(BY104:BY129)","v":1},null,{"$f":"SUM(CA104:CA129)","v":1},null,{"$f":"SUM(CC104:CC129)","v":1},null,{"$f":"SUM(CE104:CE129)","v":1},null,{"$f":"SUM(CG104:CG129)","v":14},null,{"$f":"SUM(CI104:CI129)","v":2},null,{"$f":"SUM(CK104:CK129)","v":15},null,{"$f":"IF($S130>0,VLOOKUP($D130,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S130>0,VLOOKUP($D130,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(EU130,EN130,EH130,EB130)-SUM(Y130,V130)","v":-473},null,null,null,null,null,{"$f":"SUM(EB104:EB129)","v":0},null,null,null,null,null,{"$f":"SUM(EH104:EH129)","v":0},null,null,null,null,null,{"$f":"SUM(EN104:EN129)","v":0},null,null,null,null,null,null,{"$f":"SUM(EU104:EU129)","v":0}]
[null,null,null,"Storage: teaching storage",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S131>0,VLOOKUP($D131,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S131>0,VLOOKUP($D131,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""}]
[{"$f":"VLOOKUP($D132,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STT10"},null,{"$f":"VLOOKUP($D132,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STT13"},"Teaching resources stores (IT/ GT off corridor)",null,null,null,null,null,null,null,null,{"$f":"IF(D132=\"\",\"\",_xlfn.XLOOKUP(D132,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Teaching resources store (IT/ GT off corridor)"},{"$f":"CONCATENATE(M132,S132)","v":"Teaching resources store (IT/ GT off corridor)5"},null,null,null,null,{"$f":"AI132","v":5},null,{"$f":"ROUNDUP(((U20*AN20)+(U21*AN21)+(U22*AN22)+(U24*AN24)+(U27*AN27)+(U28*AN28)+(U29*AN29))/5.5,0)","v":6},{"$f":"MAXA((S132*U132)-Y132,0)","v":30},null,null,null,null,{"$f":"IF(O132=\"retained\",V132+Y132,IF(O132=\"refurb'ed\",V132+Y132,0))","v":0},null,{"$f":"(U20*AN20)+(U21*AN21)+(U22*AN22)+(U24*AN24)+(U27*AN27)+(U28*AN28)+(U29*AN29)","v":32},"m2 total recommended",null,null,null,null,5,null,{"$f":"ROUNDUP(((AK20*AN20)+(AK21*AN21)+(AK22*AN22)+(AK24*AN24)+(AK27*AN27)+(AK28*AN28)+(AK29*AN29))/5.5,0)","v":6},null,null,null,{"$f":"IF(O132=\"existing\",\"E\",\"\")","v":""},null,3,6,30,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N132,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N132,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N132)","v":6},{"$f":"IF(ISERROR(BE132*BG132)=TRUE,\"\",BE132*BG132)","v":""},null,{"$f":"IF(ISERROR(BH132-Y132-V132)=TRUE,\"\",BH132-Y132-V132)","v":""},{"$f":"BG132-U132","v":0},null,{"$f":"SUM(BO132:CK132)","v":6},null,{"$f":"ROUND($U132/5,0)","v":1},null,{"$f":"ROUND($U132/5,0)","v":1},null,{"$f":"ROUND($U132/5,0)","v":1},null,{"$f":"ROUNDUP($U132/5,0)","v":2},null,{"$f":"U132-BO132-BQ132-BS132-BU132","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S132>0,VLOOKUP($D132,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"5m2"},{"$f":"IF($S132>0,VLOOKUP($D132,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D132,'Prog Assums'!$N$6:$Q$253,3,0)","v":2},{"$f":"VLOOKUP(D132,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},1,{"$f":"IF(CS132>14,IF(CS132<31,CS132,ROUNDDOWN(CS132/30,0)*30),0)","v":0},{"$f":"IF(S132>0,(V132/S132)*CT132,0)","v":0},{"$f":"IF(CS132>0,(V132/S132)*CS132,0)-CU132","v":6},{"$f":"IF(AK132=0,0,MAXA(1,ROUNDUP((AI132/CQ132)-CR132,0)))","v":1},{"$f":"IF(CW132>14,IF(CW132<31,CW132,ROUNDDOWN(CW132/30,0)*30),0)","v":0},{"$f":"IF(AK132>0,(AS132/AI132)*CX132,0)","v":0},{"$f":"IF(CW132>0,(AS132/AI132)*CW132,0)-CY132","v":6},"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C132,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":2},{"$f":"VLOOKUP($C132,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C132,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI132,VLOOKUP($C132,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":5},{"$f":"VLOOKUP($C132,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C132,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},{"$f":"IF(ISERROR((SUM($EB132,$EH132,$EN132,$EU132)/SUM($EA132,$EG132,$EM132,$ET132)-$S132))=TRUE,0,IF($U132=0,0,(SUM($EB132,$EH132,$EN132,$EU132)/SUM($EA132,$EG132,$EM132,$ET132)-$S132)))","v":0},null,{"$f":"SUM(EA132,EG132,EM132,ET132)-U132","v":-6},{"$f":"SUM($EU132,$EN132,$EH132,$EB132)-$V132-$Y132","v":-30},null,null,0,null,0,{"$f":"EA132*DY132","v":0},null,null,0,null,0,{"$f":"EG132*EE132","v":0},null,null,{"$f":"IF(EN132>0,SUM(EN132/EM132),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY132:$YD132,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY132:$YD132)","v":0},null,null,null,{"$f":"IF(EU132>0,SUM(EU132/ET132),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY132:$YD132,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY132:$YD132)","v":0}]
[{"$f":"VLOOKUP($D133,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STT20"},null,{"$f":"VLOOKUP($D133,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STT21"},"Science prep rooms (central)",null,null,null,null,null,null,null,null,{"$f":"IF(D133=\"\",\"\",_xlfn.XLOOKUP(D133,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Science prep room (central)"},"Science prep room (central)111",null,null,null,null,{"$f":"AC133","v":111},null,1,111,null,null,null,null,{"$f":"IF(O133=\"retained\",V133+Y133,IF(O133=\"refurb'ed\",V133+Y133,0))","v":0},null,{"$f":"(ROUND((1+IF(K6>0,7,0)+(U32*AN32)+(U33*AN33)+(U34*AN34)+(U35*AN35)+(U36*AN36))/7,0)*7)-1","v":111},"m2 minimum recom'd",null,null,null,null,{"$f":"(ROUND((1+IF(K6>0,7,0)+(AK32*AN32)+(AK33*AN33)+(AK34*AN34)+(AK35*AN35)+(AK36*AN36))/7,0)*7)-1","v":111},null,1,null,null,null,"",null,{"$f":"7+(U32*AN32)+(U33*AN33)+(U34*AN34)+(U36*AN36)","v":113},{"$f":"(15*U31)","v":150},111,null,null,"total",{"$f":"ROUND(0.4*(DB32+DB33+DB34+DB36),0)+IF(K6>0,10)","v":10},"m2 recom'd",null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N133,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N133,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N133)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S133>0,VLOOKUP($D133,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"varies"},{"$f":"IF($S133>0,VLOOKUP($D133,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D133,'Prog Assums'!$N$6:$Q$253,3,0)","v":2.5},{"$f":"VLOOKUP(D133,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},41,30,30,11,41,30,30,11,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C133,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":12},{"$f":"VLOOKUP($C133,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C133,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI133,VLOOKUP($C133,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":111},{"$f":"VLOOKUP($C133,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C133,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":150},0,null,-1,-111,null,null,0,null,null,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY133:$YD133,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY133:$YD133)","v":0}]
[{"$f":"VLOOKUP($D134,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STT23"},null,{"$f":"VLOOKUP($D134,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STT23"},"Chemicals stores, science",null,null,null,null,null,null,null,null,{"$f":"IF(D134=\"\",\"\",_xlfn.XLOOKUP(D134,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Chemicals store, science"},"Chemicals store, science7",null,null,null,null,{"$f":"AC134","v":7},null,{"$f":"AK134","v":1},7,null,null,null,null,0,null,{"$f":"IF(K8>600,IF(K8>1350,10,7),4)","v":7},"m2 minimum recom'd",null,null,null,null,{"$f":"IF(K8>600,IF(K8>1350,10,7),4)","v":7},null,1,null,null,null,"",null,6,10,7,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N134,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N134,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N134)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S134>0,VLOOKUP($D134,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"7 or 10m2"},{"$f":"IF($S134>0,VLOOKUP($D134,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D134,'Prog Assums'!$N$6:$Q$253,3,0)","v":2},{"$f":"VLOOKUP(D134,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},1,0,0,1,1,0,0,1,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C134,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":6},{"$f":"VLOOKUP($C134,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C134,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI134,VLOOKUP($C134,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":7},{"$f":"VLOOKUP($C134,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C134,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,-1,-7,null,null,0,null,null,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY134:$YD134,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY134:$YD134)","v":0}]
[{"$f":"VLOOKUP($D135,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STT20"},null,{"$f":"VLOOKUP($D135,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STT22"},"Science prep rooms (satellite)",null,null,null,null,null,null,null,null,{"$f":"IF(D135=\"\",\"\",_xlfn.XLOOKUP(D135,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Science prep room (satellite)"},"Science prep room (satellite)0",{"$f":"IF(VLOOKUP(D135,'Prog Assums'!N$173:V$306,9,FALSE)>0,\"retained\",\"\")","v":""},null,null,null,{"$f":"AC135","v":0},null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N135,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N135,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N135)","v":0},"",null,"",0,null,0,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U135","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S135>0,VLOOKUP($D135,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S135>0,VLOOKUP($D135,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"VLOOKUP(D135,'Prog Assums'!$N$6:$Q$253,3,0)","v":2.5},{"$f":"VLOOKUP(D135,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C135,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":6},{"$f":"VLOOKUP($C135,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C135,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI135,VLOOKUP($C135,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":12},{"$f":"VLOOKUP($C135,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C135,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":50},0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY135:$YD135,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY135:$YD135)","v":0}]
[{"$f":"VLOOKUP($D136,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STT10"},null,{"$f":"VLOOKUP($D136,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STT16"},"Teaching resources stores (off art room)",null,null,null,null,null,null,null,null,{"$f":"IF(D136=\"\",\"\",_xlfn.XLOOKUP(D136,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Teaching resources store (off art room)"},"Teaching resources store (off art room)5",null,null,null,null,{"$f":"AI136","v":5},null,{"$f":"2*(U39+U40+U41)","v":6},30,null,null,null,null,0,null,"minimum 2 stores off each art space",null,null,null,null,null,5,null,{"$f":"2*(AK39+AK40+AK41)","v":6},null,null,null,"",null,4,10,30,null,null,"2 stores off each light practical space",null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N136,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N136,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N136)","v":6},"",null,"",0,null,6,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U136","v":6},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S136>0,VLOOKUP($D136,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"5m2"},{"$f":"IF($S136>0,VLOOKUP($D136,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D136,'Prog Assums'!$N$6:$Q$253,3,0)","v":2},{"$f":"VLOOKUP(D136,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},1,0,0,6,1,0,0,6,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C136,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":2},{"$f":"VLOOKUP($C136,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C136,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI136,VLOOKUP($C136,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":5},{"$f":"VLOOKUP($C136,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C136,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,-6,-30,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY136:$YD136,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY136:$YD136)","v":0}]
[{"$f":"VLOOKUP($D137,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STT32"},null,{"$f":"VLOOKUP($D137,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STT32"},"DT prep rooms",null,null,null,null,null,null,null,null,{"$f":"IF(D137=\"\",\"\",_xlfn.XLOOKUP(D137,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"DT prep room"},"DT prep room34",null,null,null,null,{"$f":"AC137","v":34},null,{"$f":"IF(U50>0,1,0)","v":1},34,null,null,null,null,0,null,{"$f":"IF(U50>1,41,34)","v":34},{"$f":"IF(U50>1,\"m2 min recom'd for 2+ workshops\",\"m2 min recom'd for 1 workshop\")","v":"m2 min recom'd for 1 workshop"},null,null,null,null,{"$f":"IF(AK50>1,41,34)","v":34},null,{"$f":"IF(AK50>0,1,0)","v":1},null,null,null,"",null,{"$f":"AC137","v":34},{"$f":"AQ137+10","v":44},34,null,null,{"$f":"IF(AW50>1,41,34)","v":34},"m2 min recom'd",null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N137,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N137,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N137)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U137","v":1},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S137>0,VLOOKUP($D137,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"34 or 41m2"},{"$f":"IF($S137>0,VLOOKUP($D137,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D137,'Prog Assums'!$N$6:$Q$253,3,0)","v":3.5},{"$f":"VLOOKUP(D137,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},6,0,0,6,6,0,0,6,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C137,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":34},{"$f":"VLOOKUP($C137,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C137,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI137,VLOOKUP($C137,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":34},{"$f":"VLOOKUP($C137,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C137,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":150},0,null,-1,-34,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY137:$YD137,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY137:$YD137)","v":0}]
[{"$f":"VLOOKUP($D138,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STT34"},null,{"$f":"VLOOKUP($D138,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STT34"},"Food prep rooms",null,null,null,null,null,null,null,null,{"$f":"IF(D138=\"\",\"\",_xlfn.XLOOKUP(D138,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Food prep room"},"Food prep room10",null,null,null,null,{"$f":"AC138","v":10},null,{"$f":"IF(U52>0,1,0)","v":1},10,null,null,null,null,0,null,10,"m2 minimum recom'd",null,null,null,null,10,null,{"$f":"IF(AK52>0,1,0)","v":1},null,null,null,"",null,4,15,10,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N138,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N138,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N138)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U138","v":1},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S138>0,VLOOKUP($D138,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"10m2"},{"$f":"IF($S138>0,VLOOKUP($D138,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D138,'Prog Assums'!$N$6:$Q$253,3,0)","v":3.5},{"$f":"VLOOKUP(D138,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},1,0,0,1,1,0,0,1,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C138,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":8},{"$f":"VLOOKUP($C138,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C138,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI138,VLOOKUP($C138,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":10},{"$f":"VLOOKUP($C138,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C138,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,-1,-10,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY138:$YD138,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY138:$YD138)","v":0}]
[{"$f":"VLOOKUP($D139,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STT10"},null,{"$f":"VLOOKUP($D139,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STT18"},"Teaching resources stores (off DT studio)",null,null,null,null,null,null,null,null,{"$f":"IF(D139=\"\",\"\",_xlfn.XLOOKUP(D139,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Teaching resources store (off DT studio)"},"Teaching resources store (off DT studio)5",null,null,null,null,{"$f":"AI139","v":5},null,{"$f":"2*(U54+U55+U56+U51+U53)","v":4},20,null,null,null,null,0,null,"2 stores off each light practical space",null,null,null,null,null,5,null,{"$f":"2*(AK54+AK55+AK56+AK51+AK53)","v":4},null,null,null,"",null,4,10,20,null,null,"2 stores off each light practical space",null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N139,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N139,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N139)","v":4},"",null,"",0,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U139","v":4},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S139>0,VLOOKUP($D139,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"5m2"},{"$f":"IF($S139>0,VLOOKUP($D139,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D139,'Prog Assums'!$N$6:$Q$253,3,0)","v":2},{"$f":"VLOOKUP(D139,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},1,0,0,4,1,0,0,4,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C139,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":2},{"$f":"VLOOKUP($C139,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C139,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI139,VLOOKUP($C139,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":5},{"$f":"VLOOKUP($C139,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C139,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,-4,-20,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY139:$YD139,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY139:$YD139)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S140>0,VLOOKUP($D140,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S140>0,VLOOKUP($D140,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""}]
[{"$f":"VLOOKUP($D141,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STT10"},null,{"$f":"VLOOKUP($D141,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STT17"},"Teaching resources stores (music)",null,null,null,null,null,null,null,null,{"$f":"IF(D141=\"\",\"\",_xlfn.XLOOKUP(D141,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Teaching resources store (music)"},{"$f":"CONCATENATE(M141,S141)","v":"Teaching resources store (music)5"},null,null,null,null,{"$f":"AI141","v":5},null,{"$f":"IF((U44+U45)>4,3,2)","v":2},{"$f":"MAXA((S141*U141)-Y141,0)","v":10},null,null,null,null,0,null,{"$f":"IF(U141>1,\"shared stores for music suite\",\"shared store for music suite\")","v":"shared stores for music suite"},null,null,null,null,null,5,null,{"$f":"IF((AK44+AK45)>4,3,2)","v":2},null,null,null,"",null,4,10,10,null,null,"1 store off each music or drama space",null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N141,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N141,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N141)","v":2},{"$f":"IF(ISERROR(BE141*BG141)=TRUE,\"\",BE141*BG141)","v":""},null,{"$f":"IF(ISERROR(BH141-Y141-V141)=TRUE,\"\",BH141-Y141-V141)","v":""},0,null,{"$f":"SUM(BO141:CK141)","v":2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U141","v":2},null,null,null,null,null,null,null,null,null,{"$f":"IF($S141>0,VLOOKUP($D141,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"5m2"},{"$f":"IF($S141>0,VLOOKUP($D141,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D141,'Prog Assums'!$N$6:$Q$253,3,0)","v":2},{"$f":"VLOOKUP(D141,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},1,{"$f":"IF(CS141>14,IF(CS141<31,CS141,ROUNDDOWN(CS141/30,0)*30),0)","v":0},{"$f":"IF(S141>0,(V141/S141)*CT141,0)","v":0},{"$f":"IF(CS141>0,(V141/S141)*CS141,0)-CU141","v":2},{"$f":"IF(AK141=0,0,MAXA(1,ROUNDUP((AI141/CQ141)-CR141,0)))","v":1},{"$f":"IF(CW141>14,IF(CW141<31,CW141,ROUNDDOWN(CW141/30,0)*30),0)","v":0},{"$f":"IF(AK141>0,(AS141/AI141)*CX141,0)","v":0},{"$f":"IF(CW141>0,(AS141/AI141)*CW141,0)-CY141","v":2},"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C141,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":2},{"$f":"VLOOKUP($C141,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C141,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI141,VLOOKUP($C141,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":5},{"$f":"VLOOKUP($C141,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C141,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},{"$f":"IF(ISERROR((SUM($EB141,$EH141,$EN141,$EU141)/SUM($EA141,$EG141,$EM141,$ET141)-$S141))=TRUE,0,IF($U141=0,0,(SUM($EB141,$EH141,$EN141,$EU141)/SUM($EA141,$EG141,$EM141,$ET141)-$S141)))","v":0},null,{"$f":"SUM(EA141,EG141,EM141,ET141)-U141","v":-2},{"$f":"SUM($EU141,$EN141,$EH141,$EB141)-$V141-$Y141","v":-10},null,null,0,null,0,{"$f":"EA141*DY141","v":0},null,null,0,null,0,{"$f":"EG141*EE141","v":0},null,null,{"$f":"IF(EN141>0,SUM(EN141/EM141),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY141:$YD141,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY141:$YD141)","v":0},null,null,null,{"$f":"IF(EU141>0,SUM(EU141/ET141),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY141:$YD141,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY141:$YD141)","v":0}]
[{"$f":"VLOOKUP($D142,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STT08"},null,{"$f":"VLOOKUP($D142,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STT08"},"Equipment stores, drama",null,null,null,null,null,null,null,null,{"$f":"IF(D142=\"\",\"\",_xlfn.XLOOKUP(D142,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Equipment store, drama"},"Equipment store, drama10",null,null,null,null,{"$f":"AI142","v":10},null,{"$f":"U46","v":1},10,null,null,null,null,0,null,"1 store off any drama space",null,null,null,null,null,10,null,{"$f":"AK46","v":1},null,null,null,"",null,8,15,10,null,null,"2 store off each music or drama space",null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N142,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N142,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N142)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U142","v":1},null,null,null,null,null,null,null,null,null,{"$f":"IF($S142>0,VLOOKUP($D142,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"10m2"},{"$f":"IF($S142>0,VLOOKUP($D142,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D142,'Prog Assums'!$N$6:$Q$253,3,0)","v":2},{"$f":"VLOOKUP(D142,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},1,0,0,1,1,0,0,1,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C142,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":6},{"$f":"VLOOKUP($C142,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C142,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI142,VLOOKUP($C142,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":10},{"$f":"VLOOKUP($C142,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C142,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,-1,-10,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY142:$YD142,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY142:$YD142)","v":0}]
[{"$f":"VLOOKUP($D143,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STT35"},null,{"$f":"VLOOKUP($D143,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STT35"},"Food stores, off food room",null,null,null,null,null,null,null,null,{"$f":"IF(D143=\"\",\"\",_xlfn.XLOOKUP(D143,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Food store, off food room"},"Food store, off food room5",{"$f":"IF(VLOOKUP(D143,'Prog Assums'!N$173:V$306,9,FALSE)>0,\"retained\",\"\")","v":""},null,null,null,{"$f":"VLOOKUP(D143,'Prog Assums'!N$213:T$251,5,FALSE)","v":5},null,{"$f":"U52-U138","v":0},0,null,null,null,null,0,null,null,null,null,null,null,null,5,null,{"$f":"AK52-AK138","v":0},null,null,null,"",null,null,null,0,null,null,"music instrument store recommended",null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N143,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N143,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N143)","v":0},"",null,"",0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U143","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S143>0,VLOOKUP($D143,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"5m2"},{"$f":"IF($S143>0,VLOOKUP($D143,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D143,'Prog Assums'!$N$6:$Q$253,3,0)","v":2},{"$f":"VLOOKUP(D143,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},1,0,0,0,0,0,0,0,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C143,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":2},{"$f":"VLOOKUP($C143,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C143,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI143,VLOOKUP($C143,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":5},{"$f":"VLOOKUP($C143,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C143,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":9},0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY143:$YD143,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY143:$YD143)","v":0}]
[{"$f":"VLOOKUP($D144,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STT10"},null,{"$f":"VLOOKUP($D144,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STT41"},"Teaching resources stores, room (off LRC)",null,null,null,null,null,null,null,null,{"$f":"IF(D144=\"\",\"\",_xlfn.XLOOKUP(D144,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Teaching resources store, room (off LRC)"},"Teaching resources store, room (off LRC)3",{"$f":"IF(VLOOKUP(D144,'Prog Assums'!N$173:V$306,9,FALSE)>0,\"retained\",\"\")","v":""},null,null,null,{"$f":"VLOOKUP(D144,'Prog Assums'!N$213:T$251,5,FALSE)","v":3},null,{"$f":"AK144","v":1},3,null,null,null,null,0,null,null,null,null,null,null,null,3,null,{"$f":"AK76","v":1},null,null,null,"",null,null,null,3,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N144,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N144,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N144)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U144","v":1},null,{"$f":"IF($S144>0,VLOOKUP($D144,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"3m2"},{"$f":"IF($S144>0,VLOOKUP($D144,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D144,'Prog Assums'!$N$6:$Q$253,3,0)","v":2},{"$f":"VLOOKUP(D144,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},1,0,0,1,1,0,0,1,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C144,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":1.5},{"$f":"VLOOKUP($C144,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C144,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI144,VLOOKUP($C144,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":3},{"$f":"VLOOKUP($C144,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C144,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,-1,-3,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY144:$YD144,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY144:$YD144)","v":0}]
[{"$f":"VLOOKUP($D145,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STT00"},null,{"$f":"VLOOKUP($D145,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STT42"},"Classroom stores, room (off SEN room)",null,null,null,null,null,null,null,null,{"$f":"IF(D145=\"\",\"\",_xlfn.XLOOKUP(D145,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Classroom store, room (off SEN room)"},"Classroom store, room (off SEN room)5",{"$f":"IF(VLOOKUP(D145,'Prog Assums'!N$173:V$306,9,FALSE)>0,\"retained\",\"\")","v":""},null,null,null,{"$f":"VLOOKUP(D145,'Prog Assums'!N$213:T$251,5,FALSE)","v":5},null,{"$f":"AK145","v":1},5,null,null,{"$f":"AT145","v":0},null,0,null,null,null,null,null,null,null,5,null,{"$f":"1+IF(K12>0,2,0)","v":1},null,null,null,"",null,null,null,5,{"$f":"IF(K$12>0,2*AI145,0)","v":0},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N145,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N145,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N145)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(K12>0,2,0)","v":0},null,{"$f":"U145-CI145","v":1},null,{"$f":"IF($S145>0,VLOOKUP($D145,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"5m2"},{"$f":"IF($S145>0,VLOOKUP($D145,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D145,'Prog Assums'!$N$6:$Q$253,3,0)","v":2},{"$f":"VLOOKUP(D145,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},1,{"$f":"IF(CS145>14,IF(CS145<31,CS145,ROUNDDOWN(CS145/30,0)*30),0)","v":0},0,1,1,0,0,1,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C145,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":2},{"$f":"VLOOKUP($C145,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C145,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI145,VLOOKUP($C145,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":5},{"$f":"VLOOKUP($C145,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C145,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,-1,-5,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY145:$YD145,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY145:$YD145)","v":0}]
[{"$f":"VLOOKUP($D146,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D146,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},"-",null,null,null,null,null,null,null,null,{"$f":"IF(D146=\"\",\"\",_xlfn.XLOOKUP(D146,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"-"},"-0",{"$f":"IF(VLOOKUP(D146,'Prog Assums'!N$173:V$306,9,FALSE)>0,\"retained\",\"\")","v":""},null,null,null,{"$f":"VLOOKUP(D146,'Prog Assums'!N$213:T$251,5,FALSE)","v":0},null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N146,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N146,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N146)","v":0},"",null,"",0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S146>0,VLOOKUP($D146,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S146>0,VLOOKUP($D146,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"VLOOKUP(D146,'Prog Assums'!$N$6:$Q$253,3,0)","v":0},{"$f":"VLOOKUP(D146,'Prog Assums'!$N$6:$Q$253,4,0)","v":0},0,{"$f":"IF(CS146>14,IF(CS146<31,CS146,ROUNDDOWN(CS146/30,0)*30),0)","v":0},0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C146,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C146,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C146,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI146,VLOOKUP($C146,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C146,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C146,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY146:$YD146,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY146:$YD146)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S147>0,VLOOKUP($D147,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S147>0,VLOOKUP($D147,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""}]
[{"$f":"VLOOKUP($D148,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STH00"},null,{"$f":"VLOOKUP($D148,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STH01"},"Sports equipment stores, internal (sports hall)",null,null,null,null,null,null,null,null,{"$f":"IF(D148=\"\",\"\",_xlfn.XLOOKUP(D148,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Sports equipment store, internal (sports hall)"},{"$f":"CONCATENATE(M148,S148)","v":"Sports equipment store, internal (sports hall)60"},null,null,null,null,{"$f":"AC148","v":60},null,{"$f":"U65","v":1},{"$f":"MAXA((S148*U148)-Y148,0)","v":60},null,null,{"$f":"IF((S148*U148)>60,(S148*U148)-60,0)","v":0},null,0,null,{"$f":"ROUNDUP(S65*0.1,0)","v":60},"m2 minimum recom'd",null,null,null,null,{"$f":"ROUNDUP(AI65*0.1,0)","v":60},null,{"$f":"AK65","v":1},null,null,null,"",null,{"$f":"S65*0.1","v":59.400000000000006},{"$f":"S65*0.125","v":74.25},60,null,null,{"$f":"ROUNDUP(Z65*0.1,0)","v":0},"m2 total recom'd",null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N148,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N148,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N148)","v":1},{"$f":"IF(ISERROR(BE148*BG148)=TRUE,\"\",BE148*BG148)","v":""},null,{"$f":"IF(ISERROR(BH148-Y148-V148)=TRUE,\"\",BH148-Y148-V148)","v":""},0,null,{"$f":"SUM(BO148:CK148)","v":1},null,null,null,null,null,null,null,{"$f":"BU65","v":0},null,{"$f":"BW65","v":0},null,{"$f":"BY65","v":0},null,{"$f":"CA65","v":0},null,{"$f":"CC65","v":0},null,{"$f":"U148","v":1},null,{"$f":"CG65","v":0},null,{"$f":"CI65","v":0},null,{"$f":"CK65","v":0},null,{"$f":"IF($S148>0,VLOOKUP($D148,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"10% of hall area"},{"$f":"IF($S148>0,VLOOKUP($D148,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D148,'Prog Assums'!$N$6:$Q$253,3,0)","v":2},{"$f":"VLOOKUP(D148,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},26,26,{"$f":"IF(S148>0,(V148/S148)*CT148,0)","v":26},{"$f":"IF(CS148>0,(V148/S148)*CS148,0)-CU148","v":0},{"$f":"IF(AK148=0,0,MAXA(1,ROUNDUP((AI148/CQ148)-CR148,0)))","v":26},{"$f":"IF(CW148>14,IF(CW148<31,CW148,ROUNDDOWN(CW148/30,0)*30),0)","v":26},{"$f":"IF(AK148>0,(AS148/AI148)*CX148,0)","v":26},{"$f":"IF(CW148>0,(AS148/AI148)*CW148,0)-CY148","v":0},"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C148,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":18},{"$f":"VLOOKUP($C148,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C148,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI148,VLOOKUP($C148,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":60},{"$f":"VLOOKUP($C148,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C148,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":150},{"$f":"IF(ISERROR((SUM($EB148,$EH148,$EN148,$EU148)/SUM($EA148,$EG148,$EM148,$ET148)-$S148))=TRUE,0,IF($U148=0,0,(SUM($EB148,$EH148,$EN148,$EU148)/SUM($EA148,$EG148,$EM148,$ET148)-$S148)))","v":0},null,{"$f":"SUM(EA148,EG148,EM148,ET148)-U148","v":-1},{"$f":"SUM($EU148,$EN148,$EH148,$EB148)-$V148-$Y148","v":-60},null,null,0,null,0,{"$f":"EA148*DY148","v":0},null,null,0,null,0,{"$f":"EG148*EE148","v":0},null,null,{"$f":"IF(EN148>0,SUM(EN148/EM148),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY148:$YD148,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY148:$YD148)","v":0},null,null,null,{"$f":"IF(EU148>0,SUM(EU148/ET148),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY148:$YD148,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY148:$YD148)","v":0}]
[{"$f":"VLOOKUP($D149,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STH00"},null,{"$f":"VLOOKUP($D149,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STH02"},"Sports equipment stores, internal (community)",null,null,null,null,null,null,null,null,{"$f":"IF(D149=\"\",\"\",_xlfn.XLOOKUP(D149,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Sports equipment store, internal (community)"},{"$f":"CONCATENATE(M149,S149)","v":"Sports equipment store, internal (community)4"},{"$f":"IF(VLOOKUP(D149,'Prog Assums'!N$173:V$306,9,FALSE)>0,\"retained\",\"\")","v":""},null,null,null,4,null,{"$f":"U148","v":1},{"$f":"MAXA((S149*U149)-Y149,0)","v":4},null,null,null,null,0,null,"may be locked cage in main PE store",null,null,null,null,null,4,null,{"$f":"AK148","v":1},null,null,null,"",null,null,null,4,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N149,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N149,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N149)","v":1},{"$f":"IF(ISERROR(BE149*BG149)=TRUE,\"\",BE149*BG149)","v":""},null,{"$f":"IF(ISERROR(BH149-Y149-V149)=TRUE,\"\",BH149-Y149-V149)","v":""},0,null,{"$f":"SUM(BO149:CK149)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U149","v":1},null,null,null,null,null,null,null,{"$f":"IF($S149>0,VLOOKUP($D149,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"10% of hall area"},{"$f":"IF($S149>0,VLOOKUP($D149,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D149,'Prog Assums'!$N$6:$Q$253,3,0)","v":2},{"$f":"VLOOKUP(D149,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},1,{"$f":"IF(CS149>14,IF(CS149<31,CS149,ROUNDDOWN(CS149/30,0)*30),0)","v":0},{"$f":"IF(S149>0,(V149/S149)*CT149,0)","v":0},{"$f":"IF(CS149>0,(V149/S149)*CS149,0)-CU149","v":1},1,0,0,1,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C149,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":2},{"$f":"VLOOKUP($C149,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C149,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI149,VLOOKUP($C149,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":4},{"$f":"VLOOKUP($C149,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C149,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":50},{"$f":"IF(ISERROR((SUM($EB149,$EH149,$EN149,$EU149)/SUM($EA149,$EG149,$EM149,$ET149)-$S149))=TRUE,0,IF($U149=0,0,(SUM($EB149,$EH149,$EN149,$EU149)/SUM($EA149,$EG149,$EM149,$ET149)-$S149)))","v":0},null,{"$f":"SUM(EA149,EG149,EM149,ET149)-U149","v":-1},{"$f":"SUM($EU149,$EN149,$EH149,$EB149)-$V149-$Y149","v":-4},null,null,0,null,0,{"$f":"EA149*DY149","v":0},null,null,0,null,0,{"$f":"EG149*EE149","v":0},null,null,{"$f":"IF(EN149>0,SUM(EN149/EM149),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY149:$YD149,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY149:$YD149)","v":0},null,null,null,{"$f":"IF(EU149>0,SUM(EU149/ET149),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY149:$YD149,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY149:$YD149)","v":0}]
[{"$f":"VLOOKUP($D150,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STH00"},null,{"$f":"VLOOKUP($D150,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STH03"},"Sports equipment stores, internal (activity studio)",null,null,null,null,null,null,null,null,{"$f":"IF(D150=\"\",\"\",_xlfn.XLOOKUP(D150,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Sports equipment store, internal (activity studio)"},{"$f":"CONCATENATE(M150,S150)","v":"Sports equipment store, internal (activity studio)15"},null,null,null,null,{"$f":"AC150","v":15},null,{"$f":"U66","v":1},{"$f":"MAXA((S150*U150)-Y150,0)","v":15},null,null,null,null,0,null,{"$f":"ROUNDUP(S66*0.1,0)","v":15},"m2 minimum recom'd",null,null,null,null,{"$f":"ROUNDDOWN(AI66*0.1,0)","v":15},null,{"$f":"AK66","v":1},null,null,null,"",null,{"$f":"S66*0.1","v":15},{"$f":"S66*0.125","v":18.75},15,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N150,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N150,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N150)","v":1},{"$f":"IF(ISERROR(BE150*BG150)=TRUE,\"\",BE150*BG150)","v":""},null,{"$f":"IF(ISERROR(BH150-Y150-V150)=TRUE,\"\",BH150-Y150-V150)","v":""},0,null,{"$f":"SUM(BO150:CK150)","v":1},null,null,null,null,null,{"$f":"BS66","v":0},null,{"$f":"BU66","v":0},null,{"$f":"BW66","v":0},null,{"$f":"BY66","v":0},null,{"$f":"CA66","v":0},null,null,null,{"$f":"U150","v":1},null,{"$f":"CG66","v":0},null,{"$f":"CI66","v":0},null,{"$f":"CK66","v":0},null,{"$f":"IF($S150>0,VLOOKUP($D150,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"10% of studio area"},{"$f":"IF($S150>0,VLOOKUP($D150,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D150,'Prog Assums'!$N$6:$Q$253,3,0)","v":2},{"$f":"VLOOKUP(D150,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},4,0,{"$f":"IF(S150>0,(V150/S150)*CT150,0)","v":0},{"$f":"IF(CS150>0,(V150/S150)*CS150,0)-CU150","v":4},4,0,0,4,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C150,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":12},{"$f":"VLOOKUP($C150,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C150,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI150,VLOOKUP($C150,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":15},{"$f":"VLOOKUP($C150,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C150,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":50},{"$f":"IF(ISERROR((SUM($EB150,$EH150,$EN150,$EU150)/SUM($EA150,$EG150,$EM150,$ET150)-$S150))=TRUE,0,IF($U150=0,0,(SUM($EB150,$EH150,$EN150,$EU150)/SUM($EA150,$EG150,$EM150,$ET150)-$S150)))","v":0},null,{"$f":"SUM(EA150,EG150,EM150,ET150)-U150","v":-1},{"$f":"SUM($EU150,$EN150,$EH150,$EB150)-$V150-$Y150","v":-15},null,null,0,null,0,{"$f":"EA150*DY150","v":0},null,null,0,null,0,{"$f":"EG150*EE150","v":0},null,null,{"$f":"IF(EN150>0,SUM(EN150/EM150),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY150:$YD150,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY150:$YD150)","v":0},null,null,null,{"$f":"IF(EU150>0,SUM(EU150/ET150),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY150:$YD150,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY150:$YD150)","v":0}]
[{"$f":"VLOOKUP($D151,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STH05"},null,{"$f":"VLOOKUP($D151,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STH05"},"Sports equipment stores, external",null,null,null,null,null,null,null,null,{"$f":"IF(D151=\"\",\"\",_xlfn.XLOOKUP(D151,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Sports equipment store, external"},{"$f":"CONCATENATE(M151,S151)","v":"Sports equipment store, external8"},null,null,null,null,{"$f":"AI151","v":8},null,1,{"$f":"MAXA((S151*U151)-Y151,0)","v":8},null,null,null,null,0,null,null,null,null,null,null,null,8,null,1,null,null,null,"",null,4,25,8,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N151,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N151,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N151)","v":1},{"$f":"IF(ISERROR(BE151*BG151)=TRUE,\"\",BE151*BG151)","v":""},null,{"$f":"IF(ISERROR(BH151-Y151-V151)=TRUE,\"\",BH151-Y151-V151)","v":""},0,null,{"$f":"SUM(BO151:CK151)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U151","v":1},null,null,null,null,null,null,null,{"$f":"IF($S151>0,VLOOKUP($D151,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"8m2"},{"$f":"IF($S151>0,VLOOKUP($D151,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D151,'Prog Assums'!$N$6:$Q$253,3,0)","v":2},{"$f":"VLOOKUP(D151,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},{"$f":"IF(S151=0,0,MAXA(1,ROUNDUP((S151/CQ151)-CR151,0)))","v":1},0,{"$f":"IF(S151>0,(V151/S151)*CT151,0)","v":0},{"$f":"IF(CS151>0,(V151/S151)*CS151,0)-CU151","v":1},1,0,0,1,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C151,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":2},{"$f":"VLOOKUP($C151,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C151,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI151,VLOOKUP($C151,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":8},{"$f":"VLOOKUP($C151,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C151,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},{"$f":"IF(ISERROR((SUM($EB151,$EH151,$EN151,$EU151)/SUM($EA151,$EG151,$EM151,$ET151)-$S151))=TRUE,0,IF($U151=0,0,(SUM($EB151,$EH151,$EN151,$EU151)/SUM($EA151,$EG151,$EM151,$ET151)-$S151)))","v":0},null,{"$f":"SUM(EA151,EG151,EM151,ET151)-U151","v":-1},{"$f":"SUM($EU151,$EN151,$EH151,$EB151)-$V151-$Y151","v":-8},null,null,0,null,0,{"$f":"EA151*DY151","v":0},null,null,0,null,0,{"$f":"EG151*EE151","v":0},null,null,{"$f":"IF(EN151>0,SUM(EN151/EM151),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY151:$YD151,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY151:$YD151)","v":0},null,null,null,{"$f":"IF(EU151>0,SUM(EU151/ET151),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY151:$YD151,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY151:$YD151)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S152>0,VLOOKUP($D152,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S152>0,VLOOKUP($D152,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""}]
[null,null,null,"Non-teaching storage",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AI153","v":0},null,{"$f":"AK153","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S153>0,VLOOKUP($D153,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S153>0,VLOOKUP($D153,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""}]
[{"$f":"VLOOKUP($D154,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STH10"},null,{"$f":"VLOOKUP($D154,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STH11"},{"$f":"IF(AC64>0, \"Furniture stores (chair/ table, off hall)\",\"Furniture stores (chair, off hall)\")","v":"Furniture stores (chair/ table, off hall)"},null,null,null,null,null,null,null,null,{"$f":"IF(D154=\"\",\"\",_xlfn.XLOOKUP(D154,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Furniture store (chair/ table, off hall)"},{"$f":"CONCATENATE(M154,S154)","v":"Furniture store (chair/ table, off hall)20"},null,null,null,null,{"$f":"AC154","v":20},null,{"$f":"AK154","v":1},{"$f":"MAXA((S154*U154)-Y154,0)","v":20},null,null,null,null,0,null,{"$f":"IF(AN10=\"dining\",ROUNDUP((S64-68)*0.1,0),ROUNDUP((S64)*0.1,0))","v":20},{"$f":"IF(AC64>0, \"m2 recom'd for chairs and tables\",\"m2 recom'd for chairs\")","v":"m2 recom'd for chairs and tables"},null,null,null,null,{"$f":"AC154","v":20},null,1,null,null,null,"",null,null,null,20,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N154,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N154,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N154)","v":1},{"$f":"IF(ISERROR(BE154*BG154)=TRUE,\"\",BE154*BG154)","v":""},null,{"$f":"IF(ISERROR(BH154-Y154-V154)=TRUE,\"\",BH154-Y154-V154)","v":""},0,null,{"$f":"SUM(BO154:CK154)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,{"$f":"IF($S154>0,VLOOKUP($D154,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":0},{"$f":"IF($S154>0,VLOOKUP($D154,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D154,'Prog Assums'!$N$6:$Q$253,3,0)","v":2},{"$f":"VLOOKUP(D154,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},6,{"$f":"IF(CS154>14,IF(CS154<31,CS154,ROUNDDOWN(CS154/30,0)*30),0)","v":0},{"$f":"IF(S154>0,(V154/S154)*CT154,0)","v":0},{"$f":"IF(CS154>0,(V154/S154)*CS154,0)-CU154","v":6},{"$f":"IF(AK154=0,0,MAXA(1,ROUNDUP((AI154/CQ154)-CR154,0)))","v":6},{"$f":"IF(CW154>14,IF(CW154<31,CW154,ROUNDDOWN(CW154/30,0)*30),0)","v":0},{"$f":"IF(AK154>0,(AS154/AI154)*CX154,0)","v":0},{"$f":"IF(CW154>0,(AS154/AI154)*CW154,0)-CY154","v":6},"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C154,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":6},{"$f":"VLOOKUP($C154,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C154,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI154,VLOOKUP($C154,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":20},{"$f":"VLOOKUP($C154,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C154,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":50},{"$f":"IF(ISERROR((SUM($EB154,$EH154,$EN154,$EU154)/SUM($EA154,$EG154,$EM154,$ET154)-$S154))=TRUE,0,IF($U154=0,0,(SUM($EB154,$EH154,$EN154,$EU154)/SUM($EA154,$EG154,$EM154,$ET154)-$S154)))","v":0},null,{"$f":"SUM(EA154,EG154,EM154,ET154)-U154","v":-1},{"$f":"SUM($EU154,$EN154,$EH154,$EB154)-$V154-$Y154","v":-20},null,null,0,null,0,{"$f":"EA154*DY154","v":0},null,null,0,null,0,{"$f":"EG154*EE154","v":0},null,null,{"$f":"IF(EN154>0,SUM(EN154/EM154),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY154:$YD154,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY154:$YD154)","v":0},null,null,null,{"$f":"IF(EU154>0,SUM(EU154/ET154),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY154:$YD154,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY154:$YD154)","v":0}]
[{"$f":"VLOOKUP($D155,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STN20"},null,{"$f":"VLOOKUP($D155,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STN22"},"General storerooms (central stock)",null,null,null,null,null,null,null,null,{"$f":"IF(D155=\"\",\"\",_xlfn.XLOOKUP(D155,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"General storeroom (central stock)"},"General storeroom (central stock)6",null,null,null,null,{"$f":"AI155","v":6},null,{"$f":"AK155","v":2},12,null,null,null,null,0,null,null,null,null,null,null,null,{"$f":"ROUND(((K8/150)+4)/AK155,0)","v":6},null,{"$f":"IF(K8>900,2,1)","v":2},null,null,null,"",null,5,10,12,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N155,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N155,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N155)","v":2},"",null,"",0,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U155","v":2},null,{"$f":"IF($S155>0,VLOOKUP($D155,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"8m2"},{"$f":"IF($S155>0,VLOOKUP($D155,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D155,'Prog Assums'!$N$6:$Q$253,3,0)","v":2},{"$f":"VLOOKUP(D155,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},1,0,0,2,1,0,0,2,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C155,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":1.5},{"$f":"VLOOKUP($C155,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C155,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI155,VLOOKUP($C155,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":8},{"$f":"VLOOKUP($C155,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C155,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,-2,-12,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY155:$YD155,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY155:$YD155)","v":0}]
[{"$f":"VLOOKUP($D156,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STN50"},null,{"$f":"VLOOKUP($D156,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STN50"},"Secure storerooms",null,null,null,null,null,null,null,null,{"$f":"IF(D156=\"\",\"\",_xlfn.XLOOKUP(D156,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Secure storeroom"},"Secure storeroom8",null,null,null,null,{"$f":"AI156","v":8},null,{"$f":"AK156","v":2},16,null,null,null,null,0,null,null,null,null,null,null,null,8,null,{"$f":"IF(K8>600,2,1)","v":2},null,null,null,"",null,5,10,16,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N156,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N156,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N156)","v":2},"",null,"",0,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U156","v":2},null,null,null,null,null,{"$f":"IF($S156>0,VLOOKUP($D156,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"8m2"},{"$f":"IF($S156>0,VLOOKUP($D156,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D156,'Prog Assums'!$N$6:$Q$253,3,0)","v":2},{"$f":"VLOOKUP(D156,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},1,0,0,2,1,0,0,2,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C156,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":1.5},{"$f":"VLOOKUP($C156,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C156,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI156,VLOOKUP($C156,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":8},{"$f":"VLOOKUP($C156,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C156,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,-2,-16,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY156:$YD156,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY156:$YD156)","v":0}]
[{"$f":"VLOOKUP($D157,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"CIR06"},null,{"$f":"VLOOKUP($D157,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"CIR06"},"Equipment stores, appliance bay",null,null,null,null,null,null,null,null,{"$f":"IF(D157=\"\",\"\",_xlfn.XLOOKUP(D157,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Equipment store, appliance bay"},"Equipment store, appliance bay1.5",null,null,null,null,{"$f":"AI157","v":1.5},null,{"$f":"AK157","v":4},6,null,null,{"$f":"AT157","v":0},null,0,null,"as 'bays' off circulation areas",null,null,null,null,null,1.5,null,{"$f":"IF(EVEN(K8/300)<K8/300,EVEN(K8/300)+2,EVEN(K8/300))+IF(K$12>0,1,0)","v":4},null,null,null,"",null,10,15,6,{"$f":"IF(K$12>0,AI157,0)","v":0},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N157,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N157,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N157)","v":4},"",null,"",0,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(K12>0,1,0)","v":0},null,{"$f":"U157-CI157","v":4},null,{"$f":"IF($S157>0,VLOOKUP($D157,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"1.5m2"},{"$f":"IF($S157>0,VLOOKUP($D157,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D157,'Prog Assums'!$N$6:$Q$253,3,0)","v":2},{"$f":"VLOOKUP(D157,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},1,0,0,4,1,0,0,4,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C157,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":1.5},{"$f":"VLOOKUP($C157,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C157,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI157,VLOOKUP($C157,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":1.5},{"$f":"VLOOKUP($C157,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C157,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":6},0,null,-4,-6,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY157:$YD157,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY157:$YD157)","v":0}]
[{"$f":"VLOOKUP($D158,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STH20"},null,{"$f":"VLOOKUP($D158,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STH20"},{"$f":"IF($AG$63=\"hall with bleacher seating\",\"Retractable seating storage (off hall)\",\"Furniture stores (chair, off hall)\")","v":"Retractable seating storage (off hall)"},null,null,null,null,null,null,null,null,{"$f":"IF(D158=\"\",\"\",_xlfn.XLOOKUP(D158,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Retractable seating storage (off hall)"},"Retractable seating storage (off hall)16",null,null,null,null,16,null,{"$f":"IF(U64>0,1,0)","v":1},16,null,null,null,null,0,null,null,null,null,null,null,null,16,null,{"$f":"IF(AK64>0,1,0)","v":1},null,null,null,"",null,16,20,16,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N158,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N158,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N158)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,{"$f":"IF($S158>0,VLOOKUP($D158,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"16m2"},{"$f":"IF($S158>0,VLOOKUP($D158,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D158,'Prog Assums'!$N$6:$Q$253,3,0)","v":2},{"$f":"VLOOKUP(D158,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},4,0,0,4,4,0,0,4,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C158,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":12},{"$f":"VLOOKUP($C158,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C158,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI158,VLOOKUP($C158,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":16},{"$f":"VLOOKUP($C158,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C158,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":50},0,null,-1,-16,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY158:$YD158,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY158:$YD158)","v":0}]
[{"$f":"VLOOKUP($D159,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D159,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"-"},"-",null,null,null,null,null,null,null,null,{"$f":"IF(D159=\"\",\"\",_xlfn.XLOOKUP(D159,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"-"},"-0",{"$f":"IF(VLOOKUP(D159,'Prog Assums'!N$173:V$306,9,FALSE)>0,\"retained\",\"\")","v":""},null,null,null,{"$f":"VLOOKUP(D159,'Prog Assums'!N$213:T$251,5,FALSE)","v":0},null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N159,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N159,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N159)","v":0},"",null,"",0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S159>0,VLOOKUP($D159,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S159>0,VLOOKUP($D159,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,{"$f":"VLOOKUP(D159,'Prog Assums'!$N$6:$Q$253,3,0)","v":0},{"$f":"VLOOKUP(D159,'Prog Assums'!$N$6:$Q$253,4,0)","v":0},0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C159,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C159,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C159,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI159,VLOOKUP($C159,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C159,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C159,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY159:$YD159,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY159:$YD159)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S160>0,VLOOKUP($D160,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S160>0,VLOOKUP($D160,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""}]
[{"$f":"VLOOKUP($D161,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STN00"},null,{"$f":"VLOOKUP($D161,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STN02"},"Coats and bags stores (lockers)",null,null,null,null,null,null,null,null,{"$f":"IF(D161=\"\",\"\",_xlfn.XLOOKUP(D161,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Coats and bag store (lockers)"},{"$f":"CONCATENATE(M161,S161)","v":"Coats and bag store (lockers)10"},null,null,null,null,{"$f":"AI161","v":10},null,{"$f":"AK161","v":6},{"$f":"MAXA((S161*U161)-Y161,0)","v":60},null,null,null,null,0,null,{"$f":"ROUND(V161/0.057,0)/(K8+K12)","v":0.93600000000000005},"of pupils can have locker if 4 tiers",null,null,null,null,{"$f":"ROUNDUP(MAXA(K8*0.05,O165-SUM(AS132:AS159)-SUM(AS162:AS164))/(5+IF(K6>0,1,0)),0)","v":10},null,{"$f":"5+IF(K6>0,1,0)","v":6},null,null,null,"",null,{"$f":"ROUNDDOWN((0.03*K8)/U161,0)","v":5},{"$f":"ROUND((0.06*K8)/U161,0)","v":11},60,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N161,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N161,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N161)","v":6},{"$f":"IF(ISERROR(BE161*BG161)=TRUE,\"\",BE161*BG161)","v":""},null,{"$f":"IF(ISERROR(BH161-Y161-V161)=TRUE,\"\",BH161-Y161-V161)","v":""},0,null,{"$f":"SUM(BO161:CK161)","v":6},null,1,null,1,null,1,null,1,null,{"$f":"IF(K6>K63,1,0)","v":1},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S161>0,VLOOKUP($D161,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"[1.5m2]"},{"$f":"IF($S161>0,VLOOKUP($D161,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D161,'Prog Assums'!$N$6:$Q$253,3,0)","v":2},{"$f":"VLOOKUP(D161,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},1,{"$f":"IF(CS161>14,IF(CS161<31,CS161,ROUNDDOWN(CS161/30,0)*30),0)","v":0},{"$f":"IF(S161>0,(V161/S161)*CT161,0)","v":0},{"$f":"IF(CS161>0,(V161/S161)*CS161,0)-CU161","v":6},{"$f":"IF(AK161=0,0,MAXA(1,ROUNDUP((AI161/CQ161)-CR161,0)))","v":1},{"$f":"IF(CW161>14,IF(CW161<31,CW161,ROUNDDOWN(CW161/30,0)*30),0)","v":0},{"$f":"IF(AK161>0,(AS161/AI161)*CX161,0)","v":0},{"$f":"IF(CW161>0,(AS161/AI161)*CW161,0)-CY161","v":6},"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C161,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":1.5},{"$f":"VLOOKUP($C161,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C161,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI161,VLOOKUP($C161,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":4},{"$f":"VLOOKUP($C161,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C161,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},{"$f":"IF(ISERROR((SUM($EB161,$EH161,$EN161,$EU161)/SUM($EA161,$EG161,$EM161,$ET161)-$S161))=TRUE,0,IF($U161=0,0,(SUM($EB161,$EH161,$EN161,$EU161)/SUM($EA161,$EG161,$EM161,$ET161)-$S161)))","v":0},null,{"$f":"SUM(EA161,EG161,EM161,ET161)-U161","v":-6},{"$f":"SUM($EU161,$EN161,$EH161,$EB161)-$V161-$Y161","v":-60},null,null,0,null,0,{"$f":"EA161*DY161","v":0},null,null,0,null,0,{"$f":"EG161*EE161","v":0},null,null,{"$f":"IF(EN161>0,SUM(EN161/EM161),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY161:$YD161,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY161:$YD161)","v":0},null,null,null,{"$f":"IF(EU161>0,SUM(EU161/ET161),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY161:$YD161,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY161:$YD161)","v":0}]
[{"$f":"VLOOKUP($D162,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STN00"},null,{"$f":"VLOOKUP($D162,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STN03"},"Coats and bags stores (community lockers)",null,null,null,null,null,null,null,null,{"$f":"IF(D162=\"\",\"\",_xlfn.XLOOKUP(D162,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Coats and bag store (community lockers)"},{"$f":"CONCATENATE(M162,S162)","v":"Coats and bag store (community lockers)3"},null,null,null,null,{"$f":"AI162","v":3},null,{"$f":"AK162","v":1},{"$f":"MAXA((S162*U162)-Y162,0)","v":3},null,null,{"$f":"IF(K$12>0,S162,0)","v":0},null,0,null,"for community use outside core hours",null,null,null,null,null,3,null,{"$f":"1+IF(K$12>0,1,0)","v":1},null,null,null,"",null,null,null,{"$f":"MAXA((AI162*AK162)-AT162,0)","v":3},{"$f":"IF(K$12>0,AI162,0)","v":0},null,"for community use outside core hours",null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N162,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N162,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N162)","v":1},{"$f":"IF(ISERROR(BE162*BG162)=TRUE,\"\",BE162*BG162)","v":""},null,{"$f":"IF(ISERROR(BH162-Y162-V162)=TRUE,\"\",BH162-Y162-V162)","v":""},0,null,{"$f":"SUM(BO162:CK162)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U162","v":1},null,null,null,{"$f":"IF(K12>0,1,0)","v":0},null,null,null,{"$f":"IF($S162>0,VLOOKUP($D162,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"4m2"},{"$f":"IF($S162>0,VLOOKUP($D162,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D162,'Prog Assums'!$N$6:$Q$253,3,0)","v":2},{"$f":"VLOOKUP(D162,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},1,{"$f":"IF(CS162>14,IF(CS162<31,CS162,ROUNDDOWN(CS162/30,0)*30),0)","v":0},{"$f":"IF(S162>0,(V162/S162)*CT162,0)","v":0},{"$f":"IF(CS162>0,(V162/S162)*CS162,0)-CU162","v":1},1,0,0,1,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C162,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":1.5},{"$f":"VLOOKUP($C162,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C162,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI162,VLOOKUP($C162,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":4},{"$f":"VLOOKUP($C162,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C162,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":12},{"$f":"IF(ISERROR((SUM($EB162,$EH162,$EN162,$EU162)/SUM($EA162,$EG162,$EM162,$ET162)-$S162))=TRUE,0,IF($U162=0,0,(SUM($EB162,$EH162,$EN162,$EU162)/SUM($EA162,$EG162,$EM162,$ET162)-$S162)))","v":0},null,{"$f":"SUM(EA162,EG162,EM162,ET162)-U162","v":-1},{"$f":"SUM($EU162,$EN162,$EH162,$EB162)-$V162-$Y162","v":-3},null,null,0,null,0,{"$f":"EA162*DY162","v":0},null,null,0,null,0,{"$f":"EG162*EE162","v":0},null,null,{"$f":"IF(EN162>0,SUM(EN162/EM162),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY162:$YD162,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY162:$YD162)","v":0},null,null,null,{"$f":"IF(EU162>0,SUM(EU162/ET162),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY162:$YD162,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY162:$YD162)","v":0}]
[{"$f":"VLOOKUP($D163,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STN31"},null,{"$f":"VLOOKUP($D163,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STN31"},"Cleaners' stores",null,null,null,null,null,null,null,null,{"$f":"IF(D163=\"\",\"\",_xlfn.XLOOKUP(D163,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Cleaners' store"},{"$f":"CONCATENATE(M163,S163)","v":"Cleaners' store1.5"},null,null,null,null,{"$f":"AI163","v":1.5},null,{"$f":"AK163","v":8},{"$f":"MAXA((S163*U163)-Y163,0)","v":12},null,null,null,null,0,null,null,null,null,null,null,null,1.5,null,{"$f":"IF(EVEN(K8/150)<K8/150,EVEN(K8/150)+2,EVEN(K8/150))","v":8},null,null,null,"",null,null,null,12,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N163,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N163,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N163)","v":8},{"$f":"IF(ISERROR(BE163*BG163)=TRUE,\"\",BE163*BG163)","v":""},null,{"$f":"IF(ISERROR(BH163-Y163-V163)=TRUE,\"\",BH163-Y163-V163)","v":""},0,null,{"$f":"SUM(BO163:CK163)","v":8},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U163","v":8},null,{"$f":"IF($S163>0,VLOOKUP($D163,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"1.5m2"},{"$f":"IF($S163>0,VLOOKUP($D163,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D163,'Prog Assums'!$N$6:$Q$253,3,0)","v":2},{"$f":"VLOOKUP(D163,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},1,{"$f":"IF(CS163>14,IF(CS163<31,CS163,ROUNDDOWN(CS163/30,0)*30),0)","v":0},{"$f":"IF(S163>0,(V163/S163)*CT163,0)","v":0},{"$f":"IF(CS163>0,(V163/S163)*CS163,0)-CU163","v":8},1,0,0,8,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C163,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":1.5},{"$f":"VLOOKUP($C163,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C163,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI163,VLOOKUP($C163,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":1.5},{"$f":"VLOOKUP($C163,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C163,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":12},{"$f":"IF(ISERROR((SUM($EB163,$EH163,$EN163,$EU163)/SUM($EA163,$EG163,$EM163,$ET163)-$S163))=TRUE,0,IF($U163=0,0,(SUM($EB163,$EH163,$EN163,$EU163)/SUM($EA163,$EG163,$EM163,$ET163)-$S163)))","v":0},null,{"$f":"SUM(EA163,EG163,EM163,ET163)-U163","v":-8},{"$f":"SUM($EU163,$EN163,$EH163,$EB163)-$V163-$Y163","v":-12},null,null,0,null,null,{"$f":"EA163*DY163","v":0},null,null,0,null,0,{"$f":"EG163*EE163","v":0},null,null,{"$f":"IF(EN163>0,SUM(EN163/EM163),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY163:$YD163,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY163:$YD163)","v":0},null,null,null,{"$f":"IF(EU163>0,SUM(EU163/ET163),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY163:$YD163,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY163:$YD163)","v":0}]
[{"$f":"VLOOKUP($D164,'Prog Assums'!$N$5:$AM$294,10, FALSE)","v":"STN32"},null,{"$f":"VLOOKUP($D164,'Prog Assums'!$N$5:$AM$294,8, FALSE)","v":"STN32"},"Equipment stores, maintenance",null,null,null,null,null,null,null,null,{"$f":"IF(D164=\"\",\"\",_xlfn.XLOOKUP(D164,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Equipment store, maintenance"},{"$f":"CONCATENATE(M164,S164)","v":"Equipment store, maintenance8"},null,null,null,null,{"$f":"AI164","v":8},null,{"$f":"AK164","v":1},{"$f":"MAXA((S164*U164)-Y164,0)","v":8},null,null,null,null,0,null,"1 of 8m2 minimum recommended",null,null,null,null,null,8,null,1,null,null,null,"",null,null,null,8,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N164,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N164,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N164)","v":1},{"$f":"IF(ISERROR(BE164*BG164)=TRUE,\"\",BE164*BG164)","v":""},null,{"$f":"IF(ISERROR(BH164-Y164-V164)=TRUE,\"\",BH164-Y164-V164)","v":""},{"$f":"BG164-U164","v":0},null,{"$f":"SUM(BO164:CK164)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U164","v":1},null,{"$f":"IF($S164>0,VLOOKUP($D164,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":"8m2"},{"$f":"IF($S164>0,VLOOKUP($D164,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,{"$f":"VLOOKUP(D164,'Prog Assums'!$N$6:$Q$253,3,0)","v":2},{"$f":"VLOOKUP(D164,'Prog Assums'!$N$6:$Q$253,4,0)","v":4},1,{"$f":"IF(CS164>14,IF(CS164<31,CS164,ROUNDDOWN(CS164/30,0)*30),0)","v":0},{"$f":"IF(S164>0,(V164/S164)*CT164,0)","v":0},{"$f":"IF(CS164>0,(V164/S164)*CS164,0)-CU164","v":1},1,0,0,1,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C164,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":4},{"$f":"VLOOKUP($C164,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C164,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI164,VLOOKUP($C164,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":8},{"$f":"VLOOKUP($C164,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C164,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},{"$f":"IF(ISERROR((SUM($EB164,$EH164,$EN164,$EU164)/SUM($EA164,$EG164,$EM164,$ET164)-$S164))=TRUE,0,IF($U164=0,0,(SUM($EB164,$EH164,$EN164,$EU164)/SUM($EA164,$EG164,$EM164,$ET164)-$S164)))","v":0},null,{"$f":"SUM(EA164,EG164,EM164,ET164)-U164","v":-1},{"$f":"SUM($EU164,$EN164,$EH164,$EB164)-$V164-$Y164","v":-8},null,null,0,null,0,{"$f":"EA164*DY164","v":0},null,null,0,null,0,{"$f":"EG164*EE164","v":0},null,null,{"$f":"IF(EN164>0,SUM(EN164/EM164),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY164:$YD164,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY164:$YD164)","v":0},null,null,null,{"$f":"IF(EU164>0,SUM(EU164/ET164),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY164:$YD164,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY164:$YD164)","v":0}]
[null,null,null,"TOTAL AREA",null,null,null,null,null,null,null,"BB103 range",null,null,{"$f":"ROUND(IF(K$4>0,75,125)+IF(K$6>0,25,0)+(K$4*0.15)+(K$5*0.25)+(K$6*0.3),0)","v":443},"to",{"$f":"ROUND(IF(AR$8>0,125,200)+IF(K$6>0,50,0)+(K$4*0.25)+((K$5+K$6)*0.4),0)","v":700},null,null,null,null,{"$f":"SUM(V132:V164)","v":510},null,null,{"$f":"SUM(Y132:Y164)","v":0},null,{"$f":"SUM(AA132:AA164)","v":0},null,{"$f":"IF(V165<O165,\"ERROR: total area for category is too low\",IF(V165>Q165,\"WARNING: total area for category is high\",\"OK: area within BB103 range\"))","v":"OK: area within BB103 range"},null,null,null,null,null,{"$f":"SUM(AS132:AS164)","v":510},null,{"$f":"SUM(AT132:AT164)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(BH132:BH164)","v":0},null,{"$f":"BH165-Y165-V165","v":-510},null,null,null,null,{"$f":"SUM(BO132:BO164)","v":2},null,{"$f":"SUM(BQ132:BQ164)","v":2},null,{"$f":"SUM(BS132:BS164)","v":2},null,{"$f":"SUM(BU132:BU164)","v":3},null,{"$f":"SUM(BW132:BW164)","v":2},null,{"$f":"SUM(BY132:BY164)","v":3},null,{"$f":"SUM(CA132:CA164)","v":12},null,{"$f":"SUM(CC132:CC164)","v":5},null,{"$f":"SUM(CE132:CE164)","v":5},null,{"$f":"SUM(CG132:CG164)","v":2},null,{"$f":"SUM(CI132:CI164)","v":0},null,{"$f":"SUM(CK132:CK164)","v":17},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(EU165,EN165,EH165,EB165)-SUM(Y165,V165)","v":-510},null,null,null,null,null,{"$f":"SUM(EB132:EB164)","v":0},null,null,null,null,null,{"$f":"SUM(EH132:EH164)","v":0},null,null,null,null,null,{"$f":"SUM(EN132:EN164)","v":0},null,null,null,null,null,null,{"$f":"SUM(EU132:EU164)","v":0}]
[null,null,null,"Float",null,null,null,null,null,null,null,null,null,null,0,"to",{"$f":"IF(AR$8>0,100,150)+(IF(K$6>0,100,0)+(K$4*0.15)+(K$5*0.4)+(K$6*0.3))","v":677.5},null,null,null,null,{"$f":"AF166","v":0},null,null,{"$f":"MAXA(S167-(Y61+Y73+Y95+Y130+Y165),0)","v":0},null,null,null,null,{"$f":"IF(AF166>0,\"NOTE: float available\",\"no float available\")","v":"no float available"},null,{"$f":"MAXA(O168-(V61+V73+V95+V130+V165),0)","v":0},{"$f":"IF(Y166>0,IF(AF166>0,\"plus supp float\",\"but supp float\"),\"\")","v":""},null,{"$f":"MAXA(O167-(AI61+AI73+AI95+AI130+AI165),0)","v":0},null,{"$f":"MAXA(S167-(AK61+AK73+AK95+AK130+AK165),0)","v":0},null,null,null,null,null,0,{"$f":"O167-#REF!","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BT166","v":0}]
[null,null,null,"Total Net Area",null,null,null,null,null,null,null,"BB103 range",null,null,{"$f":"ROUND(IF(AR8>0,500,750)+IF(K6>0,250)+(K4*2.9)+(K5*4.5)+(K$6*5),0)","v":6175},"to",{"$f":"ROUND(IF(AR8>0,575,875)+IF(K6>0,300)+(K4*3.1)+(K5*4.9)+(K$6*5.4),0)","v":6800},null,{"$f":"VLOOKUP(D12,'Prog Assums'!$B$82:$K$94,4,FALSE)+(K12*VLOOKUP(D12,'Prog Assums'!$B$82:$K$94,5,FALSE))","v":0},null,{"$f":"VLOOKUP(D12,'Prog Assums'!$B$82:$K$94,8,FALSE)+(K12*VLOOKUP(D12,'Prog Assums'!$B$82:$K$94,9,FALSE))","v":0},{"$f":"V61+V73+V95+V130+V165+V166","v":6175},{"$f":"W61+W73+W95+W130+W165+W166","v":12},null,{"$f":"Y61+Y73+Y95+Y130+Y165+Y166","v":0},null,{"$f":"AA61+AA73+AA95+AA130+AA165","v":0},null,{"$f":"IF((V167+Y167)>(O167+S167),IF((V167+Y167)>(Q167+U167),(V167+Y167)-Q167-U167,(V167+Y167)-O167-S167),\"OK\")","v":"OK"},{"$f":"IF((V167+Y167)>(O167+S167),IF(V167+Y167>(Q167+U167),\"m2 OVER MAXIMUM NET AREA\",\"m2 over minimum net area\"),\"\")","v":""},null,null,null,null,{"$f":"AI61+AI73+AI95+AI130+AI165+AI166","v":6175},null,{"$f":"AK61+AK73+AK95+AK130+AK165+AK166","v":0},null,null,null,null,null,null,null,{"$f":"AI167","v":6175},{"$f":"AK167","v":0},null,null,{"$f":"IF(AE167>AK167,\"over recommended net area\",\"\")","v":""},null,null,null,null,null,null,null,{"$f":"AY13*10.5","v":0},null,null,{"$f":"BH61+BH73+BH95+BH130+BH165+BH166","v":0},null,{"$f":"BH167-Y167-V167","v":-6175},null,null,null,null,{"$f":"BO61+BO73+BO95+BO130+BO165+BO166","v":12},null,{"$f":"BQ61+BQ73+BQ95+BQ130+BQ165+BQ166","v":12},null,{"$f":"BS61+BS73+BS95+BS130+BS165+BS166","v":10},null,{"$f":"BU61+BU73+BU95+BU130+BU165+BU166","v":9},null,{"$f":"BW61+BW73+BW95+BW130+BW165+BW166","v":7},null,{"$f":"BY61+BY73+BY95+BY130+BY165+BY166","v":14},null,{"$f":"CA61+CA73+CA95+CA130+CA165+CA166","v":21},null,{"$f":"CC61+CC73+CC95+CC130+CC165+CC166","v":15},null,{"$f":"CE61+CE73+CE95+CE130+CE165+CE166","v":8},null,{"$f":"CG61+CG73+CG95+CG130+CG165+CG166","v":16},null,{"$f":"CI61+CI73+CI95+CI130+CI165+CI166","v":2},null,{"$f":"CK61+CK73+CK95+CK130+CK165+CK166","v":42},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(EU167,EN167,EH167,EB167)-SUM(Y167,V167)","v":-6175},null,null,null,null,null,{"$f":"SUM(EB165+EB130+EB95+EB73+EB61)","v":0},null,null,null,null,null,{"$f":"SUM(EH165+EH130+EH95+EH73+EH61)","v":0},null,null,null,null,null,{"$f":"SUM(EN165+EN130+EN95+EN73+EN61)","v":0},null,null,null,null,null,null,{"$f":"SUM(EU165+EU130+EU95+EU73+EU61)","v":0}]
[null,null,null,"Recommended Net Area",null,null,null,null,null,null,null,null,null,null,{"$f":"ROUND(IF(AR8>0,500,750)+IF(K6>0,250)+(K4*2.9)+(K5*4.5)+(K$6*5),0)","v":6175},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF((V167+Y167)>O168,IF((V167+Y167)>Q167,(V167+Y167)-Q167,(V167+Y167)-O168),\"OK\")","v":"OK"},{"$f":"IF((V167+Y167)>O168,\"m2 over recommended net area\",IF((V167+Y167)<O168,\"m2 under recommended net area\",\"\"))","v":""},null,null,null,null,{"$f":"O168","v":6175}]
[]
[null,null,null,"Non-net Area",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"pupil toilets",null,"staff toilets"]
[{"$f":"VLOOKUP($D171,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"KIT00"},null,{"$f":"VLOOKUP($D171,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"KIT01"},"Food prep areas, kitchen (servery & wash-up)",null,null,null,null,null,null,null,null,{"$f":"IF(D171=\"\",\"\",_xlfn.XLOOKUP(D171,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Food prep area, kitchen (servery & wash-up)"},{"$f":"CONCATENATE(M171,S171)","v":"Food prep area, kitchen (servery & wash-up)97"},null,null,null,null,{"$f":"AI171","v":97},null,1,null,{"$f":"(S171*U171)-Y171","v":97},null,{"$f":"IF($K$12>0,ROUND(K12*0.065,0),0)","v":0},null,{"$f":"IF(O171=\"retained\",W171+Y171,IF(O171=\"refurb'ed\",W171+Y171,0))","v":0},null,{"$f":"ROUND(23+((K8+K12)*0.06),0)","v":91},"m2 min recom'd for full service",null,null,null,null,{"$f":"ROUNDDOWN(24+((K8+K12)*0.065),0)","v":97},null,1,null,null,null,{"$f":"IF(O171=\"existing\",\"E\",\"\")","v":""},null,{"$f":"ROUND(30+((K8+K12)*0.08),0)","v":120},{"$f":"ROUND(45+((K8+K12)*0.1),0)","v":158},{"$f":"MAXA((AI171*AK171)-AT171,0)","v":97},{"$f":"IF($K$12>0,ROUND(K12*0.065,0),0)","v":0},null,null,{"$f":"ROUND(AK8*0.1,0)","v":122},"m2 minimum recom'd",null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N171,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N171,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N171)","v":1},{"$f":"IF(ISERROR(BE171*BG171)=TRUE,\"\",BE171*BG171)","v":""},null,{"$f":"IF(ISERROR(BH171-Y171-W171)=TRUE,\"\",BH171-Y171-W171)","v":""},{"$f":"BG171-U171","v":0},null,{"$f":"SUM(BO171:CK171)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,{"$f":"IF($S171>0,VLOOKUP($D171,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":0},{"$f":"IF($S171>0,VLOOKUP($D171,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C171,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":25},{"$f":"VLOOKUP($C171,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C171,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI171,VLOOKUP($C171,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":97},{"$f":"VLOOKUP($C171,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C171,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":250},{"$f":"IF(ISERROR((SUM($EB171,$EH171,$EN171,$EU171)/SUM($EA171,$EG171,$EM171,$ET171)-$S171))=TRUE,0,IF($U171=0,0,(SUM($EB171,$EH171,$EN171,$EU171)/SUM($EA171,$EG171,$EM171,$ET171)-$S171)))","v":0},null,{"$f":"SUM(EA171,EG171,EM171,ET171)-U171","v":-1},{"$f":"SUM(EU171,EN171,EH171,EB171)-SUM(Y171,W171)","v":-97},null,null,0,null,0,{"$f":"EA171*DY171","v":0},null,null,0,null,0,{"$f":"EG171*EE171","v":0},null,null,{"$f":"IF(EN171>0,SUM(EN171/EM171),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY171:$YD171,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY171:$YD171)","v":0},null,null,null,{"$f":"IF(EU171>0,SUM(EU171/ET171),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY171:$YD171,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY171:$YD171)","v":0}]
[{"$f":"VLOOKUP($D172,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"KIT11"},null,{"$f":"VLOOKUP($D172,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"KIT11"},"Offices, kitchen",null,null,null,null,null,null,null,null,{"$f":"IF(D172=\"\",\"\",_xlfn.XLOOKUP(D172,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Office, kitchen"},{"$f":"CONCATENATE(M172,S172)","v":"Office, kitchen4"},null,null,null,null,4,null,1,null,4,null,null,null,{"$f":"IF(O172=\"retained\",W172+Y172,IF(O172=\"refurb'ed\",W172+Y172,0))","v":0},null,null,null,null,null,null,null,{"$f":"MROUND(0.5+((K$8+K$12)*0.003),0.5)","v":4},null,1,null,null,null,{"$f":"IF(O172=\"existing\",\"E\",\"\")","v":""},null,null,null,4,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N172,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N172,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N172)","v":1},{"$f":"IF(ISERROR(BE172*BG172)=TRUE,\"\",BE172*BG172)","v":""},null,{"$f":"IF(ISERROR(BH172-Y172-W172)=TRUE,\"\",BH172-Y172-W172)","v":""},{"$f":"BG172-U172","v":0},null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C172,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":1.5},{"$f":"VLOOKUP($C172,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C172,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI172,VLOOKUP($C172,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":3},{"$f":"VLOOKUP($C172,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C172,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,-1,-4,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY172:$YD172,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY172:$YD172)","v":0}]
[{"$f":"VLOOKUP($D173,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"KIT20"},null,{"$f":"VLOOKUP($D173,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"KIT21"},"Food stores, kitchen (dry)",null,null,null,null,null,null,null,null,{"$f":"IF(D173=\"\",\"\",_xlfn.XLOOKUP(D173,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Food store, kitchen (dry)"},{"$f":"CONCATENATE(M173,S173)","v":"Food store, kitchen (dry)5"},null,null,null,null,5,null,1,null,5,null,null,null,0,null,null,null,null,null,null,null,{"$f":"MROUND(1.5+((K$8+K$12)*0.003),0.5)","v":5},null,1,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N173,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N173,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N173)","v":1},null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C173,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":1.5},{"$f":"VLOOKUP($C173,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C173,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI173,VLOOKUP($C173,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":5},{"$f":"VLOOKUP($C173,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C173,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,-1,-5,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY173:$YD173,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY173:$YD173)","v":0}]
[{"$f":"VLOOKUP($D174,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"KIT25"},null,{"$f":"VLOOKUP($D174,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"KIT25"},"Cold stores, kitchen",null,null,null,null,null,null,null,null,{"$f":"IF(D174=\"\",\"\",_xlfn.XLOOKUP(D174,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Cold store, kitchen"},{"$f":"CONCATENATE(M174,S174)","v":"Cold store, kitchen4.5"},null,null,null,null,4.5,null,1,null,4.5,null,null,null,0,null,null,null,null,null,null,null,{"$f":"MROUND(0+((K$8+K$12)*0.004),0.5)","v":4.5},null,1,null,null,null,"default no.s",null,null,null,4.5,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N174,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N174,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N174)","v":1},null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C174,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":1.5},{"$f":"VLOOKUP($C174,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C174,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI174,VLOOKUP($C174,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":4},{"$f":"VLOOKUP($C174,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C174,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,-1,-4.5,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY174:$YD174,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY174:$YD174)","v":0}]
[{"$f":"VLOOKUP($D175,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"KIT25"},null,{"$f":"VLOOKUP($D175,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"KIT26"},"Cold stores, kitchen (freezer)",null,null,null,null,null,null,null,null,{"$f":"IF(D175=\"\",\"\",_xlfn.XLOOKUP(D175,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Cold store, kitchen (freezer)"},{"$f":"CONCATENATE(M175,S175)","v":"Cold store, kitchen (freezer)3.5"},null,null,null,null,3.5,null,1,null,3.5,null,null,null,0,null,null,null,null,null,null,null,{"$f":"MROUND(0+((K$8+K$12)*0.003),0.5)","v":3.5},null,1,null,null,null,null,null,null,null,3.5,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N175,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N175,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N175)","v":1},null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C175,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":1.5},{"$f":"VLOOKUP($C175,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C175,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI175,VLOOKUP($C175,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":3},{"$f":"VLOOKUP($C175,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C175,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,-1,-3.5,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY175:$YD175,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY175:$YD175)","v":0}]
[{"$f":"VLOOKUP($D176,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"KIT40"},null,{"$f":"VLOOKUP($D176,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"KIT40"},"Toilets, kitchen (with changing area)",null,null,null,null,null,null,null,null,{"$f":"IF(D176=\"\",\"\",_xlfn.XLOOKUP(D176,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Toilet, kitchen (with changing area)"},{"$f":"CONCATENATE(M176,S176)","v":"Toilet, kitchen (with changing area)6.5"},null,null,{"$f":"ROUNDDOWN(S176/1.5,0)","v":4},null,6.5,null,1,null,6.5,null,null,null,0,null,{"$f":"ROUNDDOWN(30+((K8+K12)*0.08),0)","v":120},"m2 min recom'd for total kitchen area",null,null,null,null,{"$f":"MROUND(4+((K$8+K$12)*0.002),0.5)","v":6.5},null,1,null,null,null,null,null,null,null,6.5,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N176,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N176,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N176)","v":1},null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C176,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":1.5},{"$f":"VLOOKUP($C176,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C176,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI176,VLOOKUP($C176,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":3},{"$f":"VLOOKUP($C176,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C176,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":12},0,null,-1,-6.5,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY176:$YD176,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY176:$YD176)","v":0}]
[null,null,null,"Toilets (and personal care)",null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,"(pupil toilets:",{"$f":"ROUNDUP((K8/20)+(K12/10),0)","v":57},"recom'd",null,{"$f":"U180+(Q182*U182)+IF(D183=\"Toilets, suite (pupils, other)\",Q183*U183,0)+IF(D184=\"Toilets, individual (pupil)\",Q184*U184,0)","v":58},"provided)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($S177>0,VLOOKUP($D177,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S177>0,VLOOKUP($D177,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""}]
[{"$f":"VLOOKUP($D178,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"TOC01"},null,{"$f":"VLOOKUP($D178,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"TOC01"},"Changing rooms, with showers (pupils)",null,null,null,null,null,null,null,null,{"$f":"IF(D178=\"\",\"\",_xlfn.XLOOKUP(D178,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Changing room, with showers (pupils)"},"Changing room, with showers (pupils)64",null,null,{"$f":"ROUND((S178-2)/1.1,0)","v":56},null,{"$f":"ROUNDUP(AC178/U178,0)","v":64},null,{"$f":"AK178","v":2},null,{"$f":"(S178*U178)-Y178","v":128},null,{"$f":"AT178","v":0},null,0,null,{"$f":"4+ROUND((K8+K12)*0.11,0)","v":128},"m2 for",null,{"$f":"ROUND((K8/10),0)","v":113},"incl shower cubicles",null,{"$f":"ROUND(AC178/2,0)","v":64},null,2,null,null,null,{"$f":"IF(O178=\"existing\",\"E\",\"\")","v":""},null,{"$f":"4+ROUND((K8+K12)*0.11,0)","v":128},{"$f":"44+ROUND((K8+K12)*0.13,0)","v":190},128,null,null,null,{"$f":"22+ROUND(AK8*0.1,0)","v":144},"m2 total minimum recom'd",null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N178,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N178,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N178)","v":2},{"$f":"IF(ISERROR(BE178*BG178)=TRUE,\"\",BE178*BG178)","v":""},null,{"$f":"IF(ISERROR(BH178-Y178-W178)=TRUE,\"\",BH178-Y178-W178)","v":""},{"$f":"BG178-U178","v":0},null,{"$f":"SUM(BO178:CK178)","v":2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,{"$f":"IF($S178>0,VLOOKUP($D178,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":0},{"$f":"IF($S178>0,VLOOKUP($D178,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C178,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":12},{"$f":"VLOOKUP($C178,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C178,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI178,VLOOKUP($C178,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":64},{"$f":"VLOOKUP($C178,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C178,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":150},{"$f":"IF(ISERROR((SUM($EB178,$EH178,$EN178,$EU178)/SUM($EA178,$EG178,$EM178,$ET178)-$S178))=TRUE,0,IF($U178=0,0,(SUM($EB178,$EH178,$EN178,$EU178)/SUM($EA178,$EG178,$EM178,$ET178)-$S178)))","v":0},null,{"$f":"SUM(EA178,EG178,EM178,ET178)-U178","v":-2},{"$f":"SUM(EU178,EN178,EH178,EB178)-SUM(Y178,W178)","v":-128},null,null,0,null,0,{"$f":"EA178*DY178","v":0},null,null,0,null,0,{"$f":"EG178*EE178","v":0},null,null,{"$f":"IF(EN178>0,SUM(EN178/EM178),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY178:$YD178,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY178:$YD178)","v":0},null,null,null,{"$f":"IF(EU178>0,SUM(EU178/ET178),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY178:$YD178,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY178:$YD178)","v":0}]
[{"$f":"VLOOKUP($D179,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"TOC02"},null,{"$f":"VLOOKUP($D179,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"TOC02"},"Accessible (and staff) changing rooms",null,null,null,null,null,null,null,null,{"$f":"IF(D179=\"\",\"\",_xlfn.XLOOKUP(D179,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Accessible (and staff) changing room"},"Accessible (and staff) changing room6",null,null,1,null,{"$f":"AC179","v":6},null,2,null,12,null,null,null,0,null,6,"m2 minimum including shower",null,null,null,null,6,null,2,null,null,null,"",null,null,null,12,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N179,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N179,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N179)","v":2},"",null,"",0,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,{"$f":"IF($S179>0,VLOOKUP($D179,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":0},{"$f":"IF($S179>0,VLOOKUP($D179,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C179,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":4},{"$f":"VLOOKUP($C179,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C179,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI179,VLOOKUP($C179,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":6},{"$f":"VLOOKUP($C179,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C179,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":12},0,null,-2,-12,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY179:$YD179,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY179:$YD179)","v":0}]
[{"$f":"VLOOKUP($D180,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"TOC04"},null,{"$f":"VLOOKUP($D180,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"TOC04"},"Hygiene rooms",null,null,null,null,null,null,null,null,{"$f":"IF(D180=\"\",\"\",_xlfn.XLOOKUP(D180,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Hygiene room"},"Hygiene room12",null,null,1,null,{"$f":"VLOOKUP(D180,'Prog Assums'!N$251:T$309,5,FALSE)","v":12},null,1,null,12,null,{"$f":"IF(D12=\"integrated SRP for PD\",S180,IF(D12=\"designated unit for PD\",S180,0))","v":0},null,0,null,12,"m2 minimum if ceiling-mounted hoist",null,null,null,null,12,null,{"$f":"1+IF(OR(D12=\"integrated SRP for PD\",D12=\"designated unit for PD\"),1,0)","v":1},null,null,1,"",null,24,{"$f":"ROUND(40+IF(K6>0,K5/20,0),0)","v":85},12,{"$f":"IF(D12=\"SRP for PD\",AI180,0)","v":0},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N180,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N180,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N180)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U180","v":1},null,{"$f":"IF($S180>0,VLOOKUP($D180,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":0},{"$f":"IF($S180>0,VLOOKUP($D180,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C180,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":9},{"$f":"VLOOKUP($C180,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C180,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI180,VLOOKUP($C180,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":12},{"$f":"VLOOKUP($C180,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C180,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":25},0,null,-1,-12,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY180:$YD180,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY180:$YD180)","v":0}]
[{"$f":"VLOOKUP($D181,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D181,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"-"},"-",null,null,null,null,null,null,null,null,{"$f":"IF(D181=\"\",\"\",_xlfn.XLOOKUP(D181,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"-"},{"$f":"CONCATENATE(M181,S181)","v":"-0"},null,null,1,null,{"$f":"VLOOKUP(D181,'Prog Assums'!N$251:T$309,5,FALSE)","v":0},null,{"$f":"AK181","v":0},null,{"$f":"(S181*U181)-Y181","v":0},null,{"$f":"IF(D13=\"integrated SRP for PD\",S181,IF(D13=\"designated unit for PD\",S181,0))","v":0},null,{"$f":"IF(O181=\"retained\",W181+Y181,IF(O181=\"refurb'ed\",W181+Y181,0))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(O181=\"existing\",\"E\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N181,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N181,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N181)","v":0},{"$f":"IF(ISERROR(BE181*BG181)=TRUE,\"\",BE181*BG181)","v":""},null,{"$f":"IF(ISERROR(BH181-Y181-W181)=TRUE,\"\",BH181-Y181-W181)","v":""},{"$f":"BG181-U181","v":0},null,{"$f":"SUM(BO181:CK181)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U181","v":0},null,{"$f":"IF($S181>0,VLOOKUP($D181,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S181>0,VLOOKUP($D181,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C181,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C181,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C181,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI181,VLOOKUP($C181,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C181,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C181,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},0,null,{"$f":"SUM(EA181,EG181,EM181,ET181)-U181","v":0},{"$f":"SUM(EU181,EN181,EH181,EB181)-SUM(Y181,W181)","v":0},null,null,0,null,0,{"$f":"EA181*DY181","v":0},null,null,0,null,0,{"$f":"EG181*EE181","v":0},null,null,{"$f":"IF(EN181>0,SUM(EN181/EM181),0)","v":0},null,0,0,null,null,null,{"$f":"IF(EU181>0,SUM(EU181/ET181),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY181:$YD181,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY181:$YD181)","v":0}]
[{"$f":"VLOOKUP($D182,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"TOC10"},null,{"$f":"VLOOKUP($D182,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"TOC13"},"Toilets, suite (pupils)",null,null,null,null,null,null,null,null,{"$f":"IF(D182=\"\",\"\",_xlfn.XLOOKUP(D182,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Toilets, suite (pupils)"},"Toilets, suite (pupils)26",null,null,{"$f":"ROUNDDOWN(S182/3.25,0)","v":8},null,{"$f":"AI182","v":26},null,6,null,156,null,null,null,0,null,null,null,null,null,null,null,{"$f":"ROUND((AC177-7)/(AK182*2),0)*6.5","v":26},null,{"$f":"5+IF(K6>0,1,0)-IF(K8<700,2)","v":6},null,null,{"$f":"ROUNDDOWN(AI182/3.25,0)","v":8},"",null,null,{"$f":"ROUND(ROUNDUP((K5+K6)/20,0)*3.7,0)","v":211},156,null,null,"-",null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N182,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N182,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N182)","v":6},"",null,"",0,null,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U182","v":6},null,{"$f":"IF($S182>0,VLOOKUP($D182,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":0},{"$f":"IF($S182>0,VLOOKUP($D182,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C182,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":5},{"$f":"VLOOKUP($C182,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C182,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI182,VLOOKUP($C182,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":19.5},{"$f":"VLOOKUP($C182,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C182,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":150},0,null,-6,-156,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY182:$YD182,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY182:$YD182)","v":0}]
[{"$f":"VLOOKUP($D183,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"TOC10"},null,{"$f":"VLOOKUP($D183,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"TOC14"},"Toilets, suite (pupils, other)",null,null,null,null,null,null,null,null,{"$f":"IF(D183=\"\",\"\",_xlfn.XLOOKUP(D183,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Toilets, suite (pupils, other)"},"Toilets, suite (pupils, other)6",null,null,{"$f":"IF(S183>0,MAX(ROUNDDOWN(S183/2.5,0),1),0)","v":2},null,{"$f":"AI183","v":6},null,3,null,18,null,{"$f":"IF($K$12>0,S183*ROUNDUP(K12/20,0),0)","v":0},null,0,null,{"$f":"IF(D183=\"other pupil toilet suite(s)\",\"2 in PE changing area\",\"\")","v":""},null,null,null,null,null,6,null,{"$f":"MAX(2,ROUNDUP((AC177-(AN182*AK182)-(AN184*AK184)-AN180)/2,0),0)+IF(K12>0,ROUNDUP(K12/20,0))","v":3},null,null,{"$f":"ROUNDDOWN(AI183/2.5,0)","v":2},"",null,null,null,18,{"$f":"IF($K$12>0,AI183*ROUNDUP(K12/20,0),0)","v":0},null,null,{"$f":"MAXA(CV182-AD182,S213-SUM(Y181S154:AE187)-SUM(AE187:AE209),4)","v":{"$error":"#NAME?"}},"m2 recommended",null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N183,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N183,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N183)","v":3},"",null,"",0,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,{"$f":"IF(K12>0,ROUNDUP(K12/20,0),0)","v":0},null,{"$f":"U183-CE183-CI183","v":1},null,{"$f":"IF($S183>0,VLOOKUP($D183,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":0},{"$f":"IF($S183>0,VLOOKUP($D183,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C183,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":5},{"$f":"VLOOKUP($C183,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C183,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI183,VLOOKUP($C183,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":12},{"$f":"VLOOKUP($C183,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C183,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":150},0,null,-3,-18,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY183:$YD183,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY183:$YD183)","v":0}]
[{"$f":"VLOOKUP($D184,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"TOC15"},null,{"$f":"VLOOKUP($D184,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"TOC15"},"Toilets, individual (pupil)",null,null,null,null,null,null,null,null,{"$f":"IF(D184=\"\",\"\",_xlfn.XLOOKUP(D184,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Toilet, individual (pupil)"},{"$f":"CONCATENATE(M184,S184)","v":"Toilet, individual (pupil)2"},null,null,{"$f":"IF(S184>0,MAX(ROUNDDOWN(S184/2.5,0),1),0)","v":1},null,{"$f":"AI184","v":2},null,3,null,{"$f":"(S184*U184)-Y184","v":6},null,null,null,{"$f":"IF(O184=\"retained\",W184+Y184,IF(O184=\"refurb'ed\",W184+Y184,0))","v":0},null,{"$f":"IF(D184=\"staff toilet suite(s)\",\"including lobby with coat hooks\",\"\")","v":""},null,null,null,null,null,2,null,{"$f":"AO6","v":3},null,null,{"$f":"ROUNDDOWN(AI184/2,0)","v":1},{"$f":"IF(O184=\"existing\",\"E\",\"\")","v":""},{"$f":"ROUNDDOWN(AI184/3,0)","v":0},3.5,null,{"$f":"MAXA((AI184*AK184)-AT184,0)","v":6},null,null,null,{"$f":"MAXA(ROUND(ROUNDUP(AK6/150,0)*CV184,0)-AE185,0)","v":0},"m2 recommended",null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N184,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N184,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N184)","v":3},{"$f":"IF(ISERROR(BE184*BG184)=TRUE,\"\",BE184*BG184)","v":""},null,{"$f":"IF(ISERROR(BH184-Y184-W184)=TRUE,\"\",BH184-Y184-W184)","v":""},{"$f":"BG184-U184","v":0},null,{"$f":"SUM(BO184:CK184)","v":3},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U184","v":3},null,{"$f":"IF($S184>0,VLOOKUP($D184,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":0},{"$f":"IF($S184>0,VLOOKUP($D184,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C184,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":2},{"$f":"VLOOKUP($C184,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C184,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI184,VLOOKUP($C184,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":2},{"$f":"VLOOKUP($C184,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C184,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":6},0,null,-3,-6,null,null,0,null,0,{"$f":"EA184*DY184","v":0},null,null,0,null,0,{"$f":"EG184*EE184","v":0},null,null,{"$f":"IF(EN184>0,SUM(EN184/EM184),0)","v":0},null,0,0,null,null,null,{"$f":"IF(EU184>0,SUM(EU184/ET184),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY184:$YD184,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY184:$YD184)","v":0}]
[{"$f":"VLOOKUP($D185,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"TOC10"},null,{"$f":"VLOOKUP($D185,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"TOC12"},"Toilets, suite (staff)",null,null,null,null,null,null,null,null,{"$f":"IF(D185=\"\",\"\",_xlfn.XLOOKUP(D185,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Toilets, suite (staff)"},"Toilets, suite (staff)6",null,null,{"$f":"IF(S185>0,MAX(ROUNDDOWN(S185/2.5,0),1),0)","v":2},null,6,null,2,null,12,null,null,null,0,null,{"$f":"IF(D185=\"individual toilet (pupil)\",\"in admin suite for sick room\",\"\")","v":""},null,null,null,null,null,6,null,2,null,null,null,"",null,null,null,12,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N185,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N185,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N185)","v":2},"",null,"",0,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U185","v":2},null,null,null,null,null,{"$f":"IF($S185>0,VLOOKUP($D185,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":0},{"$f":"IF($S185>0,VLOOKUP($D185,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C185,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":5},{"$f":"VLOOKUP($C185,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C185,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI185,VLOOKUP($C185,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":12},{"$f":"VLOOKUP($C185,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C185,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":150},0,null,-2,-12,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY185:$YD185,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY185:$YD185)","v":0}]
[{"$f":"VLOOKUP($D186,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D186,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"-"},"-",null,null,null,null,null,null,null,null,{"$f":"IF(D186=\"\",\"\",_xlfn.XLOOKUP(D186,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"-"},{"$f":"CONCATENATE(M186,S186)","v":"-0"},null,null,{"$f":"IF(S186>0,MAX(ROUNDDOWN(S186/2.5,0),1),0)","v":0},null,{"$f":"AI186","v":0},null,0,null,{"$f":"(S186*U186)-Y186","v":0},null,null,null,{"$f":"IF(O186=\"retained\",W186+Y186,IF(O186=\"refurb'ed\",W186+Y186,0))","v":0},null,{"$f":"IF(D186=\"individual toilet (pupil)\",\"in admin suite for sick room\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(O186=\"existing\",\"E\",\"\")","v":""},null,null,null,{"$f":"MAXA((AI186*AK186)-AT186,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N186,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N186,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N186)","v":0},{"$f":"IF(ISERROR(BE186*BG186)=TRUE,\"\",BE186*BG186)","v":""},null,{"$f":"IF(ISERROR(BH186-Y186-W186)=TRUE,\"\",BH186-Y186-W186)","v":""},{"$f":"BG186-U186","v":0},null,{"$f":"SUM(BO186:CK186)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U186","v":0},null,null,null,null,null,{"$f":"IF($S186>0,VLOOKUP($D186,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S186>0,VLOOKUP($D186,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C186,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":0},{"$f":"VLOOKUP($C186,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C186,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI186,VLOOKUP($C186,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":0},{"$f":"VLOOKUP($C186,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":0},{"$f":"VLOOKUP($C186,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":0},0,null,{"$f":"SUM(EA186,EG186,EM186,ET186)-U186","v":0},{"$f":"SUM(EU186,EN186,EH186,EB186)-SUM(Y186,W186)","v":0},null,null,0,null,0,{"$f":"EA186*DY186","v":0},null,null,0,null,0,{"$f":"EG186*EE186","v":0},null,null,{"$f":"IF(EN186>0,SUM(EN186/EM186),0)","v":0},null,0,0,null,null,null,{"$f":"IF(EU186>0,SUM(EU186/ET186),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY186:$YD186,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY186:$YD186)","v":0}]
[{"$f":"VLOOKUP($D187,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"TOC21"},null,{"$f":"VLOOKUP($D187,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"TOC21"},"Accessible (and staff) toilets",null,null,null,null,null,null,null,null,{"$f":"IF(D187=\"\",\"\",_xlfn.XLOOKUP(D187,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Accessible (and staff) toilet"},{"$f":"CONCATENATE(M187,S187)","v":"Accessible (and staff) toilet3.8"},null,null,null,null,{"$f":"AI187","v":3.8},null,5,null,{"$f":"(S187*U187)-Y187","v":19},null,{"$f":"IF($K$12>0,S187,0)","v":0},null,{"$f":"IF(O187=\"retained\",W187+Y187,IF(O187=\"refurb'ed\",W187+Y187,0))","v":0},null,"also for visitors and staff",null,null,null,null,null,3.8,null,{"$f":"MINA(AO6*2,ROUNDUP(K8/225,0)+IF(K12>0,1,0))","v":5},null,null,null,{"$f":"IF(O187=\"existing\",\"E\",\"\")","v":""},{"$f":"U187","v":5},null,null,{"$f":"MAXA((AI187*AK187)-AT187,0)","v":19},{"$f":"IF($K$12>0,AI187,0)","v":0},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N187,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N187,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N187)","v":5},{"$f":"IF(ISERROR(BE187*BG187)=TRUE,\"\",BE187*BG187)","v":""},null,{"$f":"IF(ISERROR(BH187-Y187-W187)=TRUE,\"\",BH187-Y187-W187)","v":""},{"$f":"BG187-U187","v":0},null,{"$f":"SUM(BO187:CK187)","v":5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(K12>0,1,0)","v":0},null,{"$f":"U187-CI187","v":5},null,{"$f":"IF($S187>0,VLOOKUP($D187,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":0},{"$f":"IF($S187>0,VLOOKUP($D187,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C187,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":3},{"$f":"VLOOKUP($C187,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C187,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI187,VLOOKUP($C187,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":3.75},{"$f":"VLOOKUP($C187,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C187,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":12},0,null,-5,-19,null,null,0,null,0,{"$f":"EA187*DY187","v":0},null,null,0,null,0,{"$f":"EG187*EE187","v":0},null,null,{"$f":"IF(EN187>0,SUM(EN187/EM187),0)","v":0},null,0,0,null,null,null,{"$f":"IF(EU187>0,SUM(EU187/ET187),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY187:$YD187,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY187:$YD187)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BH188>0,BH188/BH$167,\"\")","v":""}]
[null,null,null,"Plant ",null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(M189,W189)","v":""},null,null,"indicative % of net area: for new:",null,{"$f":"AK189","v":2.0016194331983806E-2},"incl ICT hubs and risers",null,null,null,null,null,null,null,null,{"$f":"IF(SUM(Y192:Y198)>0,SUM(Y192:Y198)/Y$167,0)","v":0},{"$f":"IF(AC189>0,\"for supp\",\"\")","v":""},null,{"$f":"IF(SUM(AA192:AA198)>0,SUM(AA192:AA198)/AA$167,0)","v":0},{"$f":"IF(AA189>0,\"for existing\",\"\")","v":""},null,null,null,{"$f":"SUM(AS189:AS198)/AI167","v":2.0016194331983806E-2},null,null,{"$f":"AQ189/SUM(AQ$189:AQ$209)","v":5.3504164331426039E-2},{"$f":"V$167*S189","v":123.60000000000001},null,{"$f":"1.5%+(10/V167)","v":1.6619433198380565E-2},3.5000000000000003E-2,{"$f":"AI189","v":0},null,null,null,2.5000000000000001E-2,"minimum rec'd for total area",null,null,null,null,null,null,{"$f":"IF(BH189>0,BH189/BH$167,\"\")","v":""}]
[{"$f":"VLOOKUP($D190,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"PLA10"},null,{"$f":"VLOOKUP($D190,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"PLA14"},{"$f":"IF(ROUND(K8/300,0)>5,\"Server rooms (5-cabinet)\",VLOOKUP(ROUND(K8/300,0),'Prog Assums'!M277:N282,2,FALSE))","v":"Server rooms (4-cabinet)"},null,null,null,null,null,null,null,null,{"$f":"IF(D190=\"\",\"\",_xlfn.XLOOKUP(D190,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Server room (4-cabinet)"},{"$f":"CONCATENATE(M190,W190)","v":"Server room (4-cabinet)15.6"},null,null,null,null,{"$f":"VLOOKUP(D190,'Prog Assums'!N277:R284,5,FALSE)","v":15.6},null,{"$f":"AK190","v":1},null,{"$f":"MAXA((S190*U190)-Y190,0)","v":15.6},null,null,null,{"$f":"IF(O190=\"retained\",W190+Y190,IF(O190=\"refurb'ed\",W190+Y190,0))","v":0},null,null,null,null,null,null,null,{"$f":"VLOOKUP(D190,'Prog Assums'!N277:R284,5,FALSE)","v":15.6},null,1,null,null,null,null,null,null,null,{"$f":"MAXA((AI190*AK190)-AT190,0)","v":15.6},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N190,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N190,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N190)","v":1},{"$f":"IF(ISERROR(BE190*BG190)=TRUE,\"\",BE190*BG190)","v":""},null,{"$f":"IF(ISERROR(BH190-Y190-W190)=TRUE,\"\",BH190-Y190-W190)","v":""},{"$f":"BG190-U190","v":0},null,{"$f":"SUM(BO190:CK190)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U190","v":1},null,{"$f":"IF($S190>0,VLOOKUP($D190,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":0},{"$f":"IF($S190>0,VLOOKUP($D190,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"S190*0.6","v":9.36},{"$f":"VLOOKUP($C190,'Prog Assums'!$U$5:$AI$306,11,FALSE)","v":11},{"$f":"VLOOKUP($C190,'Prog Assums'!$U$5:$AI$306,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C190,'Prog Assums'!$U$5:$AI$306,13,FALSE)=\"AS SOA\",$AI190,VLOOKUP($C190,'Prog Assums'!$U$5:$AI$306,13,FALSE))","v":15.6},{"$f":"VLOOKUP($C190,'Prog Assums'!$U$5:$AI$306,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C190,'Prog Assums'!$U$5:$AI$306,15,FALSE)","v":50},{"$f":"IF(ISERROR((SUM($EB190,$EH190,$EN190,$EU190)/SUM($EA190,$EG190,$EM190,$ET190)-$S190))=TRUE,0,IF($U190=0,0,(SUM($EB190,$EH190,$EN190,$EU190)/SUM($EA190,$EG190,$EM190,$ET190)-$S190)))","v":0},null,{"$f":"SUM(EA190,EG190,EM190,ET190)-U190","v":-1},{"$f":"SUM(EU190,EN190,EH190,EB190)-SUM(Y190,W190)","v":-15.6},null,null,0,null,0,{"$f":"EA190*DY190","v":0},null,null,0,null,0,{"$f":"EG190*EE190","v":0},null,null,{"$f":"IF(EN190>0,SUM(EN190/EM190),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY190:$YD190,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY190:$YD190)","v":0},null,null,null,{"$f":"IF(EU190>0,SUM(EU190/ET190),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY190:$YD190,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY190:$YD190)","v":0}]
[{"$f":"VLOOKUP($D191,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"PLA10"},null,{"$f":"VLOOKUP($D191,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"PLA18"},"Server rooms (ICT hub)",null,null,null,null,null,null,null,null,{"$f":"IF(D191=\"\",\"\",_xlfn.XLOOKUP(D191,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Server room (ICT hub)"},{"$f":"CONCATENATE(M191,W191)","v":"Server room (ICT hub)0"},null,null,null,null,{"$f":"VLOOKUP(D191,'Prog Assums'!N277:R284,5,FALSE)","v":7.5},null,{"$f":"AK191","v":0},null,{"$f":"MAXA((S191*U191)-Y191,0)","v":0},null,null,null,{"$f":"IF(O191=\"retained\",W191+Y191,IF(O191=\"refurb'ed\",W191+Y191,0))","v":0},null,null,null,null,null,null,null,{"$f":"VLOOKUP(D191,'Prog Assums'!N277:R284,5,FALSE)","v":7.5},null,{"$f":"MAXA(0,ROUND(K8/300,0)-5)","v":0},null,null,null,null,null,null,null,{"$f":"MAXA((AI191*AK191)-AT191,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N191,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N191,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N191)","v":0},"",null,{"$f":"IF(ISERROR(BH191-Y191-W191)=TRUE,\"\",BH191-Y191-W191)","v":""},{"$f":"BG191-U191","v":0},null,{"$f":"SUM(BO191:CK191)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U191","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C191,'Prog Assums'!$U$5:$AI$306,11,FALSE)","v":1},{"$f":"VLOOKUP($C191,'Prog Assums'!$U$5:$AI$306,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C191,'Prog Assums'!$U$5:$AI$306,13,FALSE)=\"AS SOA\",$AI191,VLOOKUP($C191,'Prog Assums'!$U$5:$AI$306,13,FALSE))","v":2},{"$f":"VLOOKUP($C191,'Prog Assums'!$U$5:$AI$306,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C191,'Prog Assums'!$U$5:$AI$306,15,FALSE)","v":10},{"$f":"IF(ISERROR((SUM($EB191,$EH191,$EN191,$EU191)/SUM($EA191,$EG191,$EM191,$ET191)-$S191))=TRUE,0,IF($U191=0,0,(SUM($EB191,$EH191,$EN191,$EU191)/SUM($EA191,$EG191,$EM191,$ET191)-$S191)))","v":0},null,{"$f":"SUM(EA191,EG191,EM191,ET191)-U191","v":0},{"$f":"SUM(EU191,EN191,EH191,EB191)-SUM(Y191,W191)","v":0},null,null,0,null,0,{"$f":"EA191*DY191","v":0},null,null,0,null,0,{"$f":"EG191*EE191","v":0},null,null,{"$f":"IF(EN191>0,SUM(EN191/EM191),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY191:$YD191,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY191:$YD191)","v":0},null,null,null,{"$f":"IF(EU191>0,SUM(EU191/ET191),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY191:$YD191,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY191:$YD191)","v":0}]
[{"$f":"VLOOKUP($D192,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"PLA20"},null,{"$f":"VLOOKUP($D192,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"PLA21"},"Plant rooms (heat source)",null,null,null,null,null,null,null,null,{"$f":"IF(D192=\"\",\"\",_xlfn.XLOOKUP(D192,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Plant room (heat source)"},{"$f":"CONCATENATE(M192,W192)","v":"Plant room (heat source)32"},null,null,null,null,{"$f":"AC192","v":32},null,1,null,{"$f":"MAXA((S192*U192)-Y192,0)","v":32},null,{"$f":"ROUND(Y$167*0.004,0)","v":0},null,0,null,{"$f":"ROUND(7+((V$167+Y$167)*0.004),0)","v":32},"m2 minimum recom'd in new build",null,null,null,null,{"$f":"ROUND(7+((AI$167+AK$167)*0.004),0)","v":32},null,{"$f":"1","v":1},null,null,null,null,null,null,null,32,{"$f":"ROUND(AT$167*0.015,0)","v":0},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N192,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N192,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N192)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U192","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C192,'Prog Assums'!$U$5:$AI$306,11,FALSE)","v":1},{"$f":"VLOOKUP($C192,'Prog Assums'!$U$5:$AI$306,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C192,'Prog Assums'!$U$5:$AI$306,13,FALSE)=\"AS SOA\",$AI192,VLOOKUP($C192,'Prog Assums'!$U$5:$AI$306,13,FALSE))","v":50},{"$f":"VLOOKUP($C192,'Prog Assums'!$U$5:$AI$306,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C192,'Prog Assums'!$U$5:$AI$306,15,FALSE)","v":150},{"$f":"IF(ISERROR((SUM($EB192,$EH192,$EN192,$EU192)/SUM($EA192,$EG192,$EM192,$ET192)-$S192))=TRUE,0,IF($U192=0,0,(SUM($EB192,$EH192,$EN192,$EU192)/SUM($EA192,$EG192,$EM192,$ET192)-$S192)))","v":0},null,{"$f":"SUM(EA192,EG192,EM192,ET192)-U192","v":-1},{"$f":"SUM(EU192,EN192,EH192,EB192)-SUM(Y192,W192)","v":-32},null,null,0,null,0,{"$f":"EA192*DY192","v":0},null,null,0,null,0,{"$f":"EG192*EE192","v":0},null,null,{"$f":"IF(EN192>0,SUM(EN192/EM192),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY192:$YD192,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY192:$YD192)","v":0},null,null,null,{"$f":"IF(EU192>0,SUM(EU192/ET192),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY192:$YD192,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY192:$YD192)","v":0}]
[{"$f":"VLOOKUP($D193,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"PLA20"},null,{"$f":"VLOOKUP($D193,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"PLA23"},"Plant rooms (cold water tanks)",null,null,null,null,null,null,null,null,{"$f":"IF(D193=\"\",\"\",_xlfn.XLOOKUP(D193,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Plant room (cold water tanks)"},{"$f":"CONCATENATE(M193,W193)","v":"Plant room (cold water tanks)28"},null,null,null,null,{"$f":"AC193","v":28},null,1,null,{"$f":"MAXA((S193*U193)-Y193,0)","v":28},null,{"$f":"ROUND(Y$167*0.004,0)","v":0},null,{"$f":"IF(O193=\"retained\",W193+Y193,IF(O193=\"refurb'ed\",W193+Y193,0))","v":0},null,{"$f":"ROUND(3+((V$167+Y$167)*0.004),0)","v":28},"m2 minimum recom'd in new build",null,null,null,null,{"$f":"ROUND(3+((AI$167+AK$167)*0.004),0)","v":28},null,1,null,null,null,null,null,null,null,{"$f":"MAXA((AI193*AK193)-AT193,0)","v":28},{"$f":"ROUND(AT$167*0.015,0)","v":0},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N193,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N193,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N193)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C193,'Prog Assums'!$U$5:$AI$306,11,FALSE)","v":1},{"$f":"VLOOKUP($C193,'Prog Assums'!$U$5:$AI$306,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C193,'Prog Assums'!$U$5:$AI$306,13,FALSE)=\"AS SOA\",$AI193,VLOOKUP($C193,'Prog Assums'!$U$5:$AI$306,13,FALSE))","v":50},{"$f":"VLOOKUP($C193,'Prog Assums'!$U$5:$AI$306,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C193,'Prog Assums'!$U$5:$AI$306,15,FALSE)","v":150},0,null,-1,-28,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY193:$YD193,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY193:$YD193)","v":0}]
[{"$f":"VLOOKUP($D194,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"PLA20"},null,{"$f":"VLOOKUP($D194,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"PLA25"},"Plant rooms (electrical intake)",null,null,null,null,null,null,null,null,{"$f":"IF(D194=\"\",\"\",_xlfn.XLOOKUP(D194,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Plant room (electrical intake)"},{"$f":"CONCATENATE(M194,W194)","v":"Plant room (electrical intake)28"},null,null,null,null,{"$f":"AC194","v":28},null,1,null,{"$f":"MAXA((S194*U194)-Y194,0)","v":28},null,0,null,{"$f":"IF(O194=\"retained\",W194+Y194,IF(O194=\"refurb'ed\",W194+Y194,0))","v":0},null,{"$f":"ROUND(3+((V$167+Y$167)*0.004),0)","v":28},"m2 minimum recom'd in new build",null,null,null,null,{"$f":"ROUND(3+((AI$167+AK$167)*0.004),0)","v":28},null,1,null,null,null,null,null,null,null,{"$f":"MAXA((AI194*AK194)-AT194,0)","v":28},{"$f":"ROUND(AT$167*0.015,0)","v":0},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N194,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N194,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N194)","v":1},"",null,"",0,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C194,'Prog Assums'!$U$5:$AI$306,11,FALSE)","v":1},{"$f":"VLOOKUP($C194,'Prog Assums'!$U$5:$AI$306,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C194,'Prog Assums'!$U$5:$AI$306,13,FALSE)=\"AS SOA\",$AI194,VLOOKUP($C194,'Prog Assums'!$U$5:$AI$306,13,FALSE))","v":50},{"$f":"VLOOKUP($C194,'Prog Assums'!$U$5:$AI$306,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C194,'Prog Assums'!$U$5:$AI$306,15,FALSE)","v":150},0,null,-1,-28,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY194:$YD194,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY194:$YD194)","v":0}]
[{"$f":"VLOOKUP($D195,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"PLA40"},null,{"$f":"VLOOKUP($D195,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"PLA43"},"Services shafts (enclosed electrical)",null,null,null,null,null,null,null,null,{"$f":"IF(D195=\"\",\"\",_xlfn.XLOOKUP(D195,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Services shaft (enclosed electrical)"},{"$f":"CONCATENATE(M195,S195)","v":"Services shaft (enclosed electrical)1"},null,null,null,null,1,null,{"$f":"ROUND(1+(V$167*0.001*AO6),0)","v":20},null,{"$f":"(S195*U195)-Y195","v":20},null,null,null,{"$f":"IF(O195=\"retained\",W195+Y195,IF(O195=\"refurb'ed\",W195+Y195,0))","v":0},null,"incl electrical risers and distribution boards",null,null,null,null,null,1,null,{"$f":"ROUND(1+(AI$167*0.001*AO6),0)","v":20},null,null,null,{"$f":"IF(O195=\"existing\",\"E\",\"\")","v":""},null,null,null,{"$f":"MAXA((AI195*AK195)-AT195,0)","v":20},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N195,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N195,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N195)","v":20},"",null,"",0,null,{"$f":"SUM(BO195:CK195)","v":20},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,null,{"$f":"IF($S195>0,VLOOKUP(#REF!,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":{"$error":"#REF!"}},{"$f":"IF($S195>0,VLOOKUP(#REF!,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C195,'Prog Assums'!$U$5:$AI$293,11,FALSE)","v":1},{"$f":"VLOOKUP($C195,'Prog Assums'!$U$5:$AI$293,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C195,'Prog Assums'!$U$5:$AI$293,13,FALSE)=\"AS SOA\",$AI195,VLOOKUP($C195,'Prog Assums'!$U$5:$AI$293,13,FALSE))","v":2},{"$f":"VLOOKUP($C195,'Prog Assums'!$U$5:$AI$293,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C195,'Prog Assums'!$U$5:$AI$293,15,FALSE)","v":10},{"$f":"IF(ISERROR((SUM($EB195,$EH195,$EN195,$EU195)/SUM($EA195,$EG195,$EM195,$ET195)-$S195))=TRUE,0,IF($U195=0,0,(SUM($EB195,$EH195,$EN195,$EU195)/SUM($EA195,$EG195,$EM195,$ET195)-$S195)))","v":0},null,{"$f":"SUM(EA195,EG195,EM195,ET195)-U195","v":-20},{"$f":"SUM(EU195,EN195,EH195,EB195)-SUM(Y195,W195)","v":-20},null,null,0,null,0,{"$f":"EA195*DY195","v":0},null,null,0,null,0,{"$f":"EG195*EE195","v":0},null,null,{"$f":"IF(EN195>0,SUM(EN195/EM195),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY195:$YD195,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY195:$YD195)","v":0},null,null,null,{"$f":"IF(EU195>0,SUM(EU195/ET195),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY195:$YD195,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY195:$YD195)","v":0}]
[{"$f":"VLOOKUP($D196,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"PLA40"},null,{"$f":"VLOOKUP($D196,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"PLA41"},"Services shafts (enclosed ventilation)",null,null,null,null,null,null,null,null,{"$f":"IF(D196=\"\",\"\",_xlfn.XLOOKUP(D196,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Services shaft (enclosed ventilation)"},"Services shaft (enclosed ventilation)0",null,null,{"$f":"IF(D196=\"-\",\"-\",VLOOKUP(D196,'Prog Assums'!$N$285:$O$300,2,FALSE))","v":"CTS"},null,null,null,null,null,0,null,null,null,0,null,{"$f":"IF(Q196=\"CTS\",\"Contractor to specify for approval\",\"\")","v":"Contractor to specify for approval"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N196,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N196,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N196)","v":0},"",null,"",0,null,{"$f":"SUM(BO196:CK196)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C196,'Prog Assums'!$U$5:$AI$306,11,FALSE)","v":1},{"$f":"VLOOKUP($C196,'Prog Assums'!$U$5:$AI$306,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C196,'Prog Assums'!$U$5:$AI$306,13,FALSE)=\"AS SOA\",$AI196,VLOOKUP($C196,'Prog Assums'!$U$5:$AI$306,13,FALSE))","v":2},{"$f":"VLOOKUP($C196,'Prog Assums'!$U$5:$AI$306,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C196,'Prog Assums'!$U$5:$AI$306,15,FALSE)","v":10},0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY196:$YD196,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY196:$YD196)","v":0}]
[{"$f":"VLOOKUP($D197,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"PLA40"},null,{"$f":"VLOOKUP($D197,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"PLA44"},"Services shafts (enclosed other)",null,null,null,null,null,null,null,null,{"$f":"IF(D197=\"\",\"\",_xlfn.XLOOKUP(D197,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Services shaft (enclosed other)"},"Services shaft (enclosed other)0",null,null,{"$f":"IF(D197=\"-\",\"-\",VLOOKUP(D197,'Prog Assums'!$N$285:$O$300,2,FALSE))","v":"CTS"},null,null,null,null,null,0,null,null,null,0,null,{"$f":"IF(Q197=\"CTS\",\"Contractor to specify for approval\",\"\")","v":"Contractor to specify for approval"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N197,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N197,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N197)","v":0},"",null,"",0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C197,'Prog Assums'!$U$5:$AI$306,11,FALSE)","v":1},{"$f":"VLOOKUP($C197,'Prog Assums'!$U$5:$AI$306,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C197,'Prog Assums'!$U$5:$AI$306,13,FALSE)=\"AS SOA\",$AI197,VLOOKUP($C197,'Prog Assums'!$U$5:$AI$306,13,FALSE))","v":2},{"$f":"VLOOKUP($C197,'Prog Assums'!$U$5:$AI$306,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C197,'Prog Assums'!$U$5:$AI$306,15,FALSE)","v":10},0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY197:$YD197,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY197:$YD197)","v":0}]
[{"$f":"VLOOKUP($D198,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D198,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"-"},"-",null,null,null,null,null,null,null,null,{"$f":"IF(D198=\"\",\"\",_xlfn.XLOOKUP(D198,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"-"},{"$f":"CONCATENATE(M198,W198)","v":"-0"},null,null,{"$f":"IF(D198=\"-\",\"-\",VLOOKUP(D198,'Prog Assums'!$N$285:$O$300,2,FALSE))","v":"-"},null,null,null,null,null,{"$f":"MAXA((S198*U198)-Y198,0)","v":0},null,null,null,{"$f":"IF(O198=\"retained\",W198+Y198,IF(O198=\"refurb'ed\",W198+Y198,0))","v":0},null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAXA((AI198*AK198)-AT198,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N198,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N198,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N198)","v":0},"",null,"",0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C198,'Prog Assums'!$U$5:$AI$306,11,FALSE)","v":0},{"$f":"VLOOKUP($C198,'Prog Assums'!$U$5:$AI$306,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C198,'Prog Assums'!$U$5:$AI$306,13,FALSE)=\"AS SOA\",$AI198,VLOOKUP($C198,'Prog Assums'!$U$5:$AI$306,13,FALSE))","v":0},{"$f":"VLOOKUP($C198,'Prog Assums'!$U$5:$AI$306,14,FALSE)","v":0},{"$f":"VLOOKUP($C198,'Prog Assums'!$U$5:$AI$306,15,FALSE)","v":0},{"$f":"IF(ISERROR((SUM($EB198,$EH198,$EN198,$EU198)/SUM($EA198,$EG198,$EM198,$ET198)-$S198))=TRUE,0,IF($U198=0,0,(SUM($EB198,$EH198,$EN198,$EU198)/SUM($EA198,$EG198,$EM198,$ET198)-$S198)))","v":0},null,{"$f":"SUM(EA198,EG198,EM198,ET198)-U198","v":0},{"$f":"SUM(EU198,EN198,EH198,EB198)-SUM(Y198,W198)","v":0},null,null,0,null,0,{"$f":"EA198*DY198","v":0},null,null,0,null,0,{"$f":"EG198*EE198","v":0},null,null,{"$f":"IF(EN198>0,SUM(EN198/EM198),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY198:$YD198,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY198:$YD198)","v":0},null,null,null,{"$f":"IF(EU198>0,SUM(EU198/ET198),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY198:$YD198,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY198:$YD198)","v":0}]
[{"$f":"VLOOKUP($D199,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"PLA20"},null,{"$f":"VLOOKUP($D199,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"PLA08"},"Stairways, plant (to roof)",null,null,null,null,null,null,null,null,{"$f":"IF(D199=\"\",\"\",_xlfn.XLOOKUP(D199,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Stairway, plant (to roof)"},{"$f":"CONCATENATE(M199,W199)","v":"Stairway, plant (to roof)0"},null,null,{"$f":"IF(D199=\"-\",\"-\",VLOOKUP(D199,'Prog Assums'!$N$285:$O$300,2,FALSE))","v":"CTS"},null,null,null,null,null,{"$f":"MAXA((S199*U199)-Y199,0)","v":0},null,null,null,{"$f":"IF(O199=\"retained\",W199+Y199,IF(O199=\"refurb'ed\",W199+Y199,0))","v":0},null,"Contractor to specify for approval",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAXA((AI199*AK199)-AT199,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N199,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N199,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N199)","v":0},"",null,"",0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,{"$f":"IF($S199>0,VLOOKUP($D199,'Prog Assums'!$N$5:$AM$294,12, FALSE),\"\")","v":""},{"$f":"IF($S199>0,VLOOKUP($D199,'Prog Assums'!$N$5:$AM$294,13, FALSE),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"S199*0.6","v":0},{"$f":"VLOOKUP($C199,'Prog Assums'!$U$5:$AI$306,11,FALSE)","v":1},{"$f":"VLOOKUP($C199,'Prog Assums'!$U$5:$AI$306,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C199,'Prog Assums'!$U$5:$AI$306,13,FALSE)=\"AS SOA\",$AI199,VLOOKUP($C199,'Prog Assums'!$U$5:$AI$306,13,FALSE))","v":20},{"$f":"VLOOKUP($C199,'Prog Assums'!$U$5:$AI$306,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C199,'Prog Assums'!$U$5:$AI$306,15,FALSE)","v":150},{"$f":"IF(ISERROR((SUM($EB199,$EH199,$EN199,$EU199)/SUM($EA199,$EG199,$EM199,$ET199)-$S199))=TRUE,0,IF($U199=0,0,(SUM($EB199,$EH199,$EN199,$EU199)/SUM($EA199,$EG199,$EM199,$ET199)-$S199)))","v":0},null,{"$f":"SUM(EA199,EG199,EM199,ET199)-U199","v":0},{"$f":"SUM(EU199,EN199,EH199,EB199)-SUM(Y199,W199)","v":0},null,null,0,null,0,{"$f":"EA199*DY199","v":0},null,null,0,null,0,{"$f":"EG199*EE199","v":0},null,null,{"$f":"IF(EN199>0,SUM(EN199/EM199),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY199:$YD199,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY199:$YD199)","v":0},null,null,null,{"$f":"IF(EU199>0,SUM(EU199/ET199),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY199:$YD199,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY199:$YD199)","v":0}]
[{"$f":"VLOOKUP($D200,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D200,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"-"},"-",null,null,null,null,null,null,null,null,{"$f":"IF(D200=\"\",\"\",_xlfn.XLOOKUP(D200,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"-"},{"$f":"CONCATENATE(M200,W200)","v":"-0"},null,null,{"$f":"IF(D200=\"-\",\"-\",VLOOKUP(D200,'Prog Assums'!$N$285:$O$300,2,FALSE))","v":"-"},null,null,null,null,null,{"$f":"MAXA((S200*U200)-Y200,0)","v":0},null,null,null,{"$f":"IF(O200=\"retained\",W200+Y200,IF(O200=\"refurb'ed\",W200+Y200,0))","v":0},null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAXA((AI200*AK200)-AT200,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N200,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N200,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N200)","v":0},"",null,"",0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C200,'Prog Assums'!$U$5:$AI$306,11,FALSE)","v":0},{"$f":"VLOOKUP($C200,'Prog Assums'!$U$5:$AI$306,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C200,'Prog Assums'!$U$5:$AI$306,13,FALSE)=\"AS SOA\",$AI200,VLOOKUP($C200,'Prog Assums'!$U$5:$AI$306,13,FALSE))","v":0},{"$f":"VLOOKUP($C200,'Prog Assums'!$U$5:$AI$306,14,FALSE)","v":0},{"$f":"VLOOKUP($C200,'Prog Assums'!$U$5:$AI$306,15,FALSE)","v":0},{"$f":"IF(ISERROR((SUM($EB200,$EH200,$EN200,$EU200)/SUM($EA200,$EG200,$EM200,$ET200)-$S200))=TRUE,0,IF($U200=0,0,(SUM($EB200,$EH200,$EN200,$EU200)/SUM($EA200,$EG200,$EM200,$ET200)-$S200)))","v":0},null,{"$f":"SUM(EA200,EG200,EM200,ET200)-U200","v":0},{"$f":"SUM(EU200,EN200,EH200,EB200)-SUM(Y200,W200)","v":0},null,null,0,null,0,{"$f":"EA200*DY200","v":0},null,null,0,null,0,{"$f":"EG200*EE200","v":0},null,null,{"$f":"IF(EN200>0,SUM(EN200/EM200),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY200:$YD200,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY200:$YD200)","v":0},null,null,null,{"$f":"IF(EU200>0,SUM(EU200/ET200),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY200:$YD200,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY200:$YD200)","v":0}]
[]
[null,null,null,"Circulation",null,null,null,null,null,null,null,null,null,null,null,null,"indicative % of net area: for new:",null,{"$f":"SUM(W202:Y207)/(V167+Y167)","v":0.2576356275303644},"incl circ noted above",null,null,{"$f":"W167","v":12},null,null,null,null,null,{"$f":"IF(SUM(Y203:Y207)>0,SUM(Y203:Y207)/Y$167,0)","v":0},{"$f":"IF(AC202>0,\"for supp\",\"\")","v":""},null,{"$f":"IF(SUM(AA203:AA207)>0,SUM(AA203:AA207)/AA$167,0)","v":0},{"$f":"IF(AF202>0,\"for existing\",\"\")","v":""},null,{"$f":"AS108+AS118","v":12},null,{"$f":"SUM(AS202:AS207)/AI167","v":0.2576356275303644},null,null,null,null,0.25,0.25,0.3,{"$f":"AI202","v":12},null,{"$f":"ROUND(IF(O214-SUM(AS167:AS200)-AS209>(AS167*AC203),O214-SUM(AS167:AS200)-AS209,AS167*AC203),1)","v":1590.9},null,0.25,"minimum rec'd for total area",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR((SUM($EB202,$EH202,$EN202,$EU202)/SUM($EA202,$EG202,$EM202,$ET202)-$S202))=TRUE,0,IF($U202=0,0,(SUM($EB202,$EH202,$EN202,$EU202)/SUM($EA202,$EG202,$EM202,$ET202)-$S202)))","v":0},null,{"$f":"SUM(EA202,EG202,EM202,ET202)-U202","v":0},{"$f":"SUM(EU202,EN202,EH202,EB202)-SUM(Y202,W202)","v":-12},null,null,0,null,0,{"$f":"EA202*DY202","v":0},null,null,0,null,0,{"$f":"EG202*EE202","v":0},null,null,{"$f":"IF(EN202>0,SUM(EN202/EM202),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,\"Refurb\",$EY202:$YD202,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,\"Refurb\",$EY202:$YD202)","v":0},null,null,null,{"$f":"IF(EU202>0,SUM(EU202/ET202),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY202:$YD202,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY202:$YD202)","v":0}]
[{"$f":"VLOOKUP($D203,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"CIR12"},null,{"$f":"VLOOKUP($D203,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"CIR12"},"Stairways   (area per floor)",null,null,null,null,null,null,null,null,{"$f":"IF(D203=\"\",\"\",_xlfn.XLOOKUP(D203,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Stairway"},{"$f":"CONCATENATE(M203,W203)","v":"Stairway324"},null,null,null,null,27,null,{"$f":"AK203","v":12},null,{"$f":"MAXA((S203*U203)-Y203,0)","v":324},null,null,null,0,null,{"$f":"IF(AO6<7,25%,19.5%+(2.5%*AO6/2))","v":0.25},{"$f":"VLOOKUP(AG6,'Prog Assums'!B18:D24,3,FALSE)","v":"of net min circulation for 3 storeys"},null,null,null,null,27,null,{"$f":"IF(AO$6=1,0,AO$6*(1+ROUNDUP(K8/400,0)))","v":12},null,null,null,null,null,null,null,{"$f":"MAXA((AI203*AK203)-AT203,0)","v":324},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N203,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N203,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N203)","v":12},{"$f":"IF(ISERROR(BE203*BG203)=TRUE,\"\",BE203*BG203)","v":""},null,{"$f":"IF(ISERROR(BH203-Y203-W203)=TRUE,\"\",BH203-Y203-W203)","v":""},{"$f":"BG203-U203","v":0},null,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U203","v":12},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C203,'Prog Assums'!$U$5:$AI$306,11,FALSE)","v":5},{"$f":"VLOOKUP($C203,'Prog Assums'!$U$5:$AI$306,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C203,'Prog Assums'!$U$5:$AI$306,13,FALSE)=\"AS SOA\",$AI203,VLOOKUP($C203,'Prog Assums'!$U$5:$AI$306,13,FALSE))","v":25},{"$f":"VLOOKUP($C203,'Prog Assums'!$U$5:$AI$306,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C203,'Prog Assums'!$U$5:$AI$306,15,FALSE)","v":50},0,null,-12,{"$f":"SUM(EU203,EN203,EH203,EB203)-SUM(Y203,W203)","v":-324},null,null,0,null,0,{"$f":"EA203*DY203","v":0},null,null,0,null,0,{"$f":"EG203*EE203","v":0},null,null,{"$f":"IF(EN203>0,SUM(EN203/EM203),0)","v":0},null,0,0,null,null,null,{"$f":"IF(EU203>0,SUM(EU203/ET203),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY203:$YD203,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY203:$YD203)","v":0}]
[{"$f":"VLOOKUP($D204,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"CIR13"},null,{"$f":"VLOOKUP($D204,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"CIR13"},"Lifts           (area per floor, incl space to wait)",null,null,null,null,null,null,null,null,{"$f":"IF(D204=\"\",\"\",_xlfn.XLOOKUP(D204,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Lift"},"Lift36",null,null,null,null,6,null,{"$f":"AK204","v":6},null,{"$f":"MAXA((S204*U204)-Y204,0)","v":36},null,null,null,0,null,{"$f":"MAXA(AC203,((O214-O168)-SUM(W171:W200)-W209)/V167)","v":0.2576356275303644},"of new build net area recommended",null,null,null,null,6,null,{"$f":"IF(AO$6=1,0,2*AO$6)","v":6},null,null,null,null,null,null,null,{"$f":"MAXA((AI204*AK204)-AT204,0)","v":36},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N204,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N204,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N204)","v":6},"",null,"",0,null,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C204,'Prog Assums'!$U$5:$AI$306,11,FALSE)","v":2},{"$f":"VLOOKUP($C204,'Prog Assums'!$U$5:$AI$306,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C204,'Prog Assums'!$U$5:$AI$306,13,FALSE)=\"AS SOA\",$AI204,VLOOKUP($C204,'Prog Assums'!$U$5:$AI$306,13,FALSE))","v":4},{"$f":"VLOOKUP($C204,'Prog Assums'!$U$5:$AI$306,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C204,'Prog Assums'!$U$5:$AI$306,15,FALSE)","v":10},0,null,-6,{"$f":"SUM(EU204,EN204,EH204,EB204)-SUM(Y204,W204)","v":-36},null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY204:$YD204,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY204:$YD204)","v":0}]
[{"$f":"VLOOKUP($D205,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"CIR03"},null,{"$f":"VLOOKUP($D205,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"CIR03"},"Lobbies",null,null,null,null,null,null,null,null,{"$f":"IF(D205=\"\",\"\",_xlfn.XLOOKUP(D205,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"Lobby"},"Lobby12",null,null,null,null,6,null,2,null,{"$f":"MAXA((S205*U205)-Y205,0)","v":12},null,null,null,0,null,null,null,null,null,null,null,6,null,2,null,null,null,null,null,null,null,{"$f":"MAXA((AI205*AK205)-AT205,0)","v":12},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N205,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N205,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N205)","v":2},"",null,"",0,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C205,'Prog Assums'!$U$5:$AI$306,11,FALSE)","v":3},{"$f":"VLOOKUP($C205,'Prog Assums'!$U$5:$AI$306,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C205,'Prog Assums'!$U$5:$AI$306,13,FALSE)=\"AS SOA\",$AI205,VLOOKUP($C205,'Prog Assums'!$U$5:$AI$306,13,FALSE))","v":6},{"$f":"VLOOKUP($C205,'Prog Assums'!$U$5:$AI$306,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C205,'Prog Assums'!$U$5:$AI$306,15,FALSE)","v":25},0,null,-2,{"$f":"SUM(EU205,EN205,EH205,EB205)-SUM(Y207,W205)","v":-12},null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY205:$YD205,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY205:$YD205)","v":0}]
[{"$f":"VLOOKUP($D206,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"-"},null,{"$f":"VLOOKUP($D206,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"-"},"-",null,null,null,null,null,null,null,null,{"$f":"IF(D206=\"\",\"\",_xlfn.XLOOKUP(D206,'Prog Assums'!$N$7:$N$305,'Prog Assums'!$AQ$7:$AQ$305,\"\"))","v":"-"},"-0",null,null,null,null,null,null,null,null,{"$f":"MAXA((S206*U206)-Y206,0)","v":0},null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAXA((AI206*AK206)-AT206,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N206,'Individual Spaces'!K:K))=TRUE,\"\",AVERAGEIF('Individual Spaces'!F:F,'Secondary SoA'!$N206,'Individual Spaces'!K:K))","v":""},null,{"$f":"COUNTIF('Individual Spaces'!F:F,'Secondary SoA'!$N206)","v":0},"",null,"",0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C206,'Prog Assums'!$U$5:$AI$306,11,FALSE)","v":0},{"$f":"VLOOKUP($C206,'Prog Assums'!$U$5:$AI$306,12,FALSE)","v":0},{"$f":"IF(VLOOKUP($C206,'Prog Assums'!$U$5:$AI$306,13,FALSE)=\"AS SOA\",$AI206,VLOOKUP($C206,'Prog Assums'!$U$5:$AI$306,13,FALSE))","v":0},{"$f":"VLOOKUP($C206,'Prog Assums'!$U$5:$AI$306,14,FALSE)","v":0},{"$f":"VLOOKUP($C206,'Prog Assums'!$U$5:$AI$306,15,FALSE)","v":0},0,null,0,{"$f":"SUM(EU206,EN206,EH206,EB206)-SUM(Y206,W206)","v":0},null,null,0,null,0,{"$f":"EA206*DY206","v":0},null,null,0,null,0,{"$f":"EG206*EE206","v":0},null,null,{"$f":"IF(EN206>0,SUM(EN206/EM206),0)","v":0},null,0,0,null,null,null,{"$f":"IF(EU206>0,SUM(EU206/ET206),0)","v":0},null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY206:$YD206,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY206:$YD206)","v":0}]
[{"$f":"VLOOKUP($D207,'Prog Assums'!$N$5:$AM$309,10, FALSE)","v":"CIR00"},null,{"$f":"VLOOKUP($D207,'Prog Assums'!$N$5:$AM$309,8, FALSE)","v":"CIR00"},"Circulation spaces (horizontal)",null,null,null,null,null,null,"remaining",null,{"$f":"D207","v":"Circulation spaces (horizontal)"},"Circulation spaces (horizontal)1206.9",null,null,null,null,{"$f":"ROUND(V$167*AC204,1)-SUM(W202:W206)+Y207","v":1206.9000000000001},null,null,null,{"$f":"MAXA(S207-Y207,0)","v":1206.9000000000001},null,{"$f":"ROUNDDOWN(MAXA(Y$167*0.225,S213-SUM(Y167:Y206)-Y209),0)","v":0},null,0,null,"incl.corridors and horizontal circulation",null,null,null,null,null,{"$f":"AS207","v":1206.9000000000001},null,null,null,null,null,null,null,null,null,{"$f":"ROUND(AU202-SUM(AS202:AS206),1)","v":1206.9000000000001},{"$f":"ROUNDDOWN(MAXA(AT$167*0.225,S213-SUM(AT167:AT198)-AT209),0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP($C207,'Prog Assums'!$U$5:$AI$306,11,FALSE)","v":1},{"$f":"VLOOKUP($C207,'Prog Assums'!$U$5:$AI$306,12,FALSE)","v":"-"},{"$f":"IF(VLOOKUP($C207,'Prog Assums'!$U$5:$AI$306,13,FALSE)=\"AS SOA\",$AI207,VLOOKUP($C207,'Prog Assums'!$U$5:$AI$306,13,FALSE))","v":50},{"$f":"VLOOKUP($C207,'Prog Assums'!$U$5:$AI$306,14,FALSE)","v":"-"},{"$f":"VLOOKUP($C207,'Prog Assums'!$U$5:$AI$306,15,FALSE)","v":500},0,null,0,{"$f":"SUM(EU207,EN207,EH207,EB207)-SUM(Y207,W207)","v":-1206.9000000000001},null,null,0,null,0,0,null,null,0,null,0,0,null,null,0,null,0,0,null,null,null,0,null,{"$f":"COUNTIFS($EY$2:$YD$2,'Prog Assums'!$B$130,$EY207:$YD207,\">0\")","v":0},{"$f":"SUMIF($EY$2:$YD$2,'Prog Assums'!$B$130,$EY207:$YD207)","v":0}]
[]
[null,null,null,"Partitions",null,null,null,null,null,null,null,null,{"$f":"D209","v":"Partitions"},{"$f":"CONCATENATE(M209,W209)","v":"Partitions272"},null,null," indicative % of net area",null,{"$f":"AP209","v":4.3999999999999997E-2},null,"for new build",null,{"$f":"ROUND((V$167-AA$167)*S209,0)+AA209","v":272},null,{"$f":"ROUND(Y$167*S209,0)","v":0},null,null,null,{"$f":"IF(Y209>0,Y209/Y$167,0)","v":0},{"$f":"IF(Y209>0,\"for supp\",\"\")","v":""},null,{"$f":"IF(AA209>0,AA209/AA$167,0)","v":0},{"$f":"IF(AA209>0,\"for existing\",\"\")","v":""},null,{"$f":"ROUND(AI$167*AP209,0)","v":272},null,{"$f":"AI209/AI167","v":4.4048582995951414E-2},null,null,{"$f":"AQ209/SUM(AQ$189:AQ$209)","v":0.14165243799121516},{"$f":"V$167*S209","v":271.7},4.3999999999999997E-2,4.3999999999999997E-2,0.06,{"$f":"AI209","v":272},{"$f":"ROUND(AT$167*AK209,0)","v":0},null,null,0.04,"minimum rec'd for total area",null,null,null,null,null,null,{"$f":"IF(BH209>0,BH209/BH$167,\"\")","v":""},null,null,null,null,{"$f":"BH209-Y209-W209","v":-272},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR((SUM($EB209,$EH209,$EN209,$EU209)/SUM($EA209,$EG209,$EM209,$ET209)-$S209))=TRUE,0,IF($U209=0,0,(SUM($EB209,$EH209,$EN209,$EU209)/SUM($EA209,$EG209,$EM209,$ET209)-$S209)))","v":0},null,{"$f":"SUM(EA209,EG209,EM209,ET209)-U209","v":{"$error":"#VALUE!"}},{"$f":"SUM(EU209,EN209,EH209,EB209)-SUM(Y209,W209)","v":-272},null,null,{"$f":"$S209","v":4.3999999999999997E-2},null,null,{"$f":"ROUNDUP(EB$167*DY209,1)","v":0},null,null,{"$f":"$S209","v":4.3999999999999997E-2},null,null,{"$f":"ROUNDUP(EH$167*EE209,1)","v":0},null,null,{"$f":"$S209","v":4.3999999999999997E-2},null,null,{"$f":"ROUNDUP(EN$167*EK209,1)","v":0},null,null,null,{"$f":"$S209","v":4.3999999999999997E-2},null,null,{"$f":"ROUNDUP(EU$167*ER209,1)","v":0}]
[]
[null,null,null,"TOTAL AREA",null,null,null,null,null,null,null,"BB103 range",null,null,{"$f":"V167*0.4","v":2470},"to",{"$f":"V167*0.45","v":2778.75},null,null,null,null,null,{"$f":"SUM(W171:W209)","v":2470},null,{"$f":"SUM(Y171:Y209)","v":0},null,{"$f":"SUM(AA171:AA209)","v":0},null,{"$f":"IF(W211<(O211-1),\"ERROR: total area for category is too low\",IF(W211>(Q211+1),\"WARNING: total area for category is high\",\"OK: area within BB103 range\"))","v":"OK: area within BB103 range"},null,null,null,null,null,{"$f":"SUM(AS171:AS209)","v":2470},null,{"$f":"SUM(AT171:AT209)","v":0},null,null,{"$f":"O213-V167-SUM(W171:W185)","v":2005.5},{"$f":"AD8-SUM(AA167:AA185)-AA190","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(BH171:BH209)","v":0},null,{"$f":"BH211-Y211-W211","v":-2470},null,null,null,null,{"$f":"SUM(BO171:BO209)","v":0},null,{"$f":"SUM(BQ171:BQ209)","v":0},null,{"$f":"SUM(BS171:BS209)","v":0},null,{"$f":"SUM(BU171:BU209)","v":0},null,{"$f":"SUM(BW171:BW209)","v":0},null,{"$f":"SUM(BY171:BY209)","v":0},null,{"$f":"SUM(CA171:CA209)","v":0},null,{"$f":"SUM(CC171:CC209)","v":6},null,{"$f":"SUM(CE171:CE209)","v":6},null,{"$f":"SUM(CG171:CG209)","v":2},null,{"$f":"SUM(CI171:CI209)","v":0},null,{"$f":"SUM(CK171:CK209)","v":60},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(EU211,EN211,EH211,EB211)-SUM(Y211,W211)","v":-2470},null,null,null,null,null,{"$f":"SUM(EB171:EB209)","v":0},null,null,null,null,null,{"$f":"SUM(EH171:EH209)","v":0},null,null,null,null,null,{"$f":"SUM(EN171:EN209)","v":0},null,null,null,null,null,null,{"$f":"SUM(EU171:EU209)","v":0}]
[]
[null,null,null,"Total Gross Area",null,null,null,null,null,null,null,"BB103 range",null,null,{"$f":"ROUND(IF(AR8>0,700,1050)+IF(K6>0,350)+(K4*4.1)+(K5*6.3)+(K6*7),0)","v":8645},"to",{"$f":"ROUND(IF(AR8>0,835,1270)+IF(K6>0,430)+(K4*4.5)+(K5*7.1)+(K6*7.85),0)","v":9856},null,{"$f":"VLOOKUP(D12,'Prog Assums'!$B$82:$K$94,6,FALSE)+(K12*VLOOKUP(D12,'Prog Assums'!$B$82:$K$94,7,FALSE))","v":0},null,{"$f":"IF(K12>0,75,0)+(K12*VLOOKUP(D12,'Prog Assums'!$B$82:$K$94,10,FALSE))","v":0},{"$f":"ROUNDUP(V167+W211,0)","v":8645},null,null,{"$f":"Y167+Y211","v":0},null,"-",null,{"$f":"IF((V213+Y213)>(O213+S213)*1.001,IF((V213+Y213)>(Q213+U213)*1.001,(V213+Y213)-Q213-U213,(V213+Y213)-O213-S213),\"OK\")","v":"OK"},{"$f":"IF((V213+Y213)>(O213+S213)*1.001,IF(V213+Y213>(Q213+U213)*1.001,\"m2 OVER MAXIMUM GROSS AREA\",\"m2 over minimum gross area\"),\"\")","v":""},null,null,null,null,{"$f":"AI167+AI211","v":8645},null,{"$f":"AK167+AK211","v":0},null,null,{"$f":"(V167-AA167)*(S189+S202+S209)","v":1986.2},{"$f":"AN211-AN213","v":19.299999999999955},null,null,null,{"$f":"AI213","v":8645},{"$f":"AK213","v":0},null,null,null,null,null,null,null,null,null,null,{"$f":"AY13*15","v":0},null,null,{"$f":"BH167+BH211","v":0},null,{"$f":"BH213-Y213-V213","v":-8645},null,null,null,null,{"$f":"BO167+BO211","v":12},null,{"$f":"BQ167+BQ211","v":12},null,{"$f":"BS167+BS211","v":10},null,{"$f":"BU167+BU211","v":9},null,{"$f":"BW167+BW211","v":7},null,{"$f":"BY167+BY211","v":14},null,{"$f":"CA167+CA211","v":21},null,{"$f":"CC167+CC211","v":21},null,{"$f":"CE167+CE211","v":14},null,{"$f":"CG167+CG211","v":18},null,{"$f":"CI167+CI211","v":2},null,{"$f":"CK167+CK211","v":102},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(EU213,EN213,EH213,EB213)-SUM(Y213,V213)","v":-8645},null,null,null,null,null,{"$f":"SUM(EB211+EB167)","v":0},null,null,null,null,null,{"$f":"SUM(EH211+EH167)","v":0},null,null,null,null,null,{"$f":"SUM(EN211+EN167)","v":0},null,null,null,null,null,null,{"$f":"SUM(EU211+EU167)","v":0}]
[null,null,null,"Recommended Gross Area",null,null,null,null,null,null,null,null,null,null,{"$f":"ROUND(IF(AR8>0,700,1050)+IF(K6>0,350)+(K4*4.1)+(K5*6.3)+(K6*7),0)","v":8645},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(V213>O214*1.001,IF(V213>Q213*1.001,V213-Q213,V213-O214),\"OK\")","v":"OK"},{"$f":"IF((V213+Y213)>O214*1.001,\"m2 over recommended gross area\",IF((V213+Y213)<O214*0.999,\"m2 under recommended gross area\",\"\"))","v":""}]
[]
[null,null,null,"Total Gross Area (including supplementary area)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"V213+Y213","v":8645},null,null,{"$f":"IF(AA213>0,\"of which\",\"\")","v":"of which"},null,{"$f":"AA167+AA211","v":0},null,{"$f":"IF(AA213>0,\"retained,    so:\",\"\")","v":"retained,    so:"},null,null,null,"gross area to be built*",null,{"$f":"V216-AA216","v":8645},"m2*",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Gross area above without partitions",{"$f":"EH213-EH209","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"Check Space is allocated within Individual Spaces","Unallocated existing spaces",null,null,{"$f":"IF(ISNUMBER(MATCH(EY$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!F:F,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(EZ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!G:G,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FA$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!H:H,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FB$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!I:I,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FC$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!J:J,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FD$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!K:K,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FE$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!L:L,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FF$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!M:M,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FG$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!N:N,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FH$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!O:O,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FI$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!P:P,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FJ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!Q:Q,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FK$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!R:R,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FL$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!S:S,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FM$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!T:T,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FN$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FO$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FP$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FQ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FR$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FS$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FT$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FU$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FV$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FW$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FX$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FY$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(FZ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GA$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GB$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GC$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GD$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GE$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GF$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GG$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GH$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GI$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GJ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GK$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GL$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GM$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GN$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GO$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GP$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GQ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GR$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GS$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GT$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GU$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GV$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GW$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GX$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GY$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(GZ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HA$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HB$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HC$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HD$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HE$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HF$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HG$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HH$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HI$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HJ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HK$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HL$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HM$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HN$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HO$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HP$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HQ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HR$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HS$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HT$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HU$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HV$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HW$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HX$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HY$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(HZ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IA$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IB$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IC$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(ID$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IE$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IF$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IG$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IH$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(II$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IJ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IK$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IL$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IM$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IN$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IO$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IP$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IQ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IR$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IS$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IT$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IU$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IV$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IW$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IX$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IY$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(IZ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JA$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JB$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JC$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JD$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JE$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JF$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JG$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JH$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JI$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JJ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JK$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JL$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JM$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JN$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JO$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JP$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JQ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JR$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JS$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JT$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JU$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JV$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JW$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JX$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JY$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(JZ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KA$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KB$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KC$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KD$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KE$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KF$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KG$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KH$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KI$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KJ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KK$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KL$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KM$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KN$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KO$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KP$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KQ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KR$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KS$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KT$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KU$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KV$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KW$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KX$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KY$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(KZ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LA$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LB$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LC$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LD$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LE$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LF$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LG$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LH$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LI$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LJ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LK$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LL$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LM$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LN$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LO$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LP$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LQ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LR$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LS$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LT$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LU$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LV$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LW$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LX$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LY$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(LZ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MA$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MB$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MC$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MD$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(ME$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MF$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MG$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MH$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MI$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MJ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MK$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(ML$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MM$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MN$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MO$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MP$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MQ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MR$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MS$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MT$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MU$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MV$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MW$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MX$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MY$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!U:U,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(MZ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!V:V,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NA$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!W:W,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NB$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!X:X,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NC$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!Y:Y,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(ND$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!Z:Z,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NE$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!AA:AA,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NF$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!AB:AB,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NG$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!AC:AC,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NH$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!AD:AD,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NI$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!AE:AE,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NJ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!AF:AF,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NK$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!AG:AG,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NL$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!AH:AH,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NM$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!AI:AI,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NN$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!AJ:AJ,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NO$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!AK:AK,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NP$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!AL:AL,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NQ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!AM:AM,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NR$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NS$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NT$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NU$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NV$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NW$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NX$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NY$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(NZ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OA$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OB$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OC$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OD$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OE$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OF$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OG$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OH$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OI$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OJ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OK$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OL$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OM$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(ON$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OO$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OP$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OQ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OR$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OS$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OT$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OU$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OV$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OW$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OX$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OY$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(OZ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PA$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PB$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PC$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PD$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PE$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PF$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PG$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PH$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PI$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PJ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PK$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PL$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PM$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PN$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PO$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PP$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PQ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PR$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PS$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PT$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PU$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PV$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PW$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PX$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PY$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(PZ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QA$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QB$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QC$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QD$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QE$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QF$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QG$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QH$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QI$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QJ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QK$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QL$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QM$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QN$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QO$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QP$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QQ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QR$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QS$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QT$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QU$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QV$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QW$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QX$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QY$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(QZ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RA$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RB$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RC$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RD$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RE$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RF$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RG$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RH$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RI$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RJ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RK$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RL$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RM$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RN$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RO$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RP$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RQ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RR$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RS$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RT$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RU$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RV$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RW$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RX$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RY$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(RZ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SA$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SB$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SC$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SD$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SE$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SF$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SG$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SH$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SI$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SJ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SK$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SL$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SM$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SN$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SO$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SP$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SQ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SR$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SS$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(ST$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SU$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SV$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SW$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SX$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SY$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(SZ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TA$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TB$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TC$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TD$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TE$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TF$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TG$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TH$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TI$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TJ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TK$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TL$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TM$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TN$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TO$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TP$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TQ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TR$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TS$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TT$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TU$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TV$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TW$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TX$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TY$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(TZ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UA$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UB$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UC$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UD$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UE$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UF$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UG$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UH$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UI$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UJ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UK$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UL$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UM$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UN$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UO$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UP$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UQ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UR$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(US$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UT$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UU$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UV$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UW$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UX$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UY$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(UZ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VA$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VB$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VC$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VD$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VE$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VF$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VG$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VH$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VI$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VJ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VK$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VL$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VM$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VN$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VO$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VP$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VQ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VR$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VS$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VT$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VU$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VV$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VW$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VX$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VY$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(VZ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WA$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WB$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WC$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WD$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WE$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WF$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WG$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WH$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WI$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WJ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WK$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WL$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WM$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WN$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WO$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WP$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WQ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WR$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WS$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WT$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WU$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WV$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WW$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WX$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WY$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(WZ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XA$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XB$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XC$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XD$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XE$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XF$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XG$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XH$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XI$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XJ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XK$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XL$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XM$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XN$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XO$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XP$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XQ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XR$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XS$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XT$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XU$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XV$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XW$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XX$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XY$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(XZ$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(YA$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(YB$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(YC$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"},{"$f":"IF(ISNUMBER(MATCH(YD$8,'Individual Spaces'!$R$4:OFFSET('Individual Spaces'!$R$4,MATCH(\"Non-Net Total : \",'Individual Spaces'!#REF!,0)-4,0)))=TRUE,\"YES\",\"NO\")","v":"NO"}]
[]
[null,null,null,"Gross area as proportion of net",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"V213/V167","v":1.4},null,null,{"$f":"IF(Y213>0,Y213/Y167,\"\")","v":""},null,{"$f":"IF(AA216>0,AA216/AA167,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BH213/BH167","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Total area of remodelled spaces without partitions",{"$f":"SUM(EY218:YD218)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"Remodelled existing spaces",null,null,{"$f":"IF(EY2=\"Remodel\",SUM(EY17:EY213),0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(HK2=\"Remodel\",SUM(HK17:HK213),0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(JW2=\"Remodel\",SUM(JW17:JW213),0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(MI2=\"Remodel\",SUM(MI17:MI213),0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(OU2=\"Remodel\",SUM(OU17:OU213),0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(RG2=\"Remodel\",SUM(RG17:RG213),0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(TS2=\"Remodel\",SUM(TS17:TS213),0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(WE2=\"Remodel\",SUM(WE17:WE213),0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"*Indicative area only if SoA adjusted to incorporate retained area for each space"]

{"sheet":"curriculum analysis (optional)","index":2,"n_rows":163,"n_cols":46,"rows_kept":163,"cut":false,"hidden":false,"merged":[]}
[]
[null,{"$f":"'Secondary SoA'!S2","v":"[Insert Project Code and Scheme Name here in title sheet]"},null,"Y7 curriculum",null,null,null,null,"Y8 curriculum",null,null,null,null,"Y9 curriculum",null,null,null,null,"Y10 curriculum",null,null,null,null,"Y11 curriculum",null,null,null,null,"Y12 curriculum",null,null,null,null,"Y13 curriculum",null,null,null,null,null,"Periods in cycle",50,null,"age range",{"$f":"'Secondary SoA'!K2","v":"11-18"}]
[]
[null,"CURRENT TIMETABLE",null,"number in cohort:",null,{"$f":"IF('Secondary SoA'!K5>0,'Secondary SoA'!K5/'Secondary SoA'!O5,0)","v":180},null,null,"number in cohort:",null,{"$f":"F4","v":180},null,null,"number in cohort:",null,{"$f":"F4","v":180},null,null,"number in cohort:",null,{"$f":"F4","v":180},null,null,"number in cohort:",null,{"$f":"F4","v":180},null,null,"number in cohort:",null,null,null,null,"number in cohort:",null,null,null,null,null,"total places",{"$f":"F4+K4+P4+U4+Z4+AE4+AJ4","v":900},null,"utilisation factor",{"$f":"AT4*0.9","v":0.63900000000000001},"to",{"$f":"VLOOKUP(AR2,'Prog Assums'!E6:L17,8,FALSE)","v":0.71}]
[]
[null,"Course title",null,"number of groups","number of periods","total","Typical group size",null,"number of groups","number of periods","total","Typical group size",null,"number of groups","number of periods","total","Typical group size",null,"number of groups","number of periods","total","Typical group size",null,"number of groups","number of periods","total","Typical group size",null,"number of groups","number of periods","total","Typical group size",null,"number of groups","number of periods","total","Typical group size",null,"totals","rooms req'd at 100% use","required no. of rooms","frequency of use","room capacity","basic work-places","actual no. of rooms","frequency of use"]
[null,"eg En/ Sci etc",null,null,null,null,"eg 30",null,null,null,null,"eg 30",null,null,null,null,"eg 30",null,null,null,null,"eg 30",null,null,null,null,"eg 30",null,null,null,null,"eg 30",null,null,null,null,"eg 30",null,null,null,null,null,null,null,"if known"]
["General teaching"]
[null,"English",null,null,null,{"$f":"IF(D9>0,IF(E9>0,D9*E9,\"check\"),IF(E9>0,\"check\",0))","v":0},{"$f":"IF(F9>0,IF((F$4/D9)<32,F$4/D9,\"tba\"),0)","v":0},{"$f":"G9*E9*D9","v":0},null,null,{"$f":"IF(I9>0,IF(J9>0,I9*J9,\"check\"),IF(J9>0,\"check\",0))","v":0},{"$f":"IF(K9>0,IF((K$4/I9)<32,K$4/I9,\"tba\"),0)","v":0},{"$f":"L9*J9*I9","v":0},null,null,{"$f":"IF(N9>0,IF(O9>0,N9*O9,\"check\"),IF(O9>0,\"check\",0))","v":0},{"$f":"IF(P9>0,IF((P$4/N9)<32,P$4/N9,\"tba\"),0)","v":0},{"$f":"Q9*O9*N9","v":0},null,null,{"$f":"IF(S9>0,IF(T9>0,S9*T9,\"check\"),IF(T9>0,\"check\",0))","v":0},{"$f":"IF(U9>0,IF((U$4/S9)<32,U$4/S9,\"tba\"),0)","v":0},{"$f":"V9*T9*S9","v":0},null,null,{"$f":"IF(X9>0,IF(Y9>0,X9*Y9,\"check\"),IF(Y9>0,\"check\",0))","v":0},{"$f":"IF(Z9>0,IF((Z$4/X9)<32,Z$4/X9,\"tba\"),0)","v":0},{"$f":"AA9*Y9*X9","v":0},null,null,{"$f":"IF(AC9>0,IF(AD9>0,AC9*AD9,\"check\"),IF(AD9>0,\"check\",0))","v":0},{"$f":"IF(AE9>0,IF((AE$4/AC9)<32,AE$4/AC9,\"tba\"),0)","v":0},{"$f":"AF9*AD9*AC9","v":0},null,null,{"$f":"IF(AH9>0,IF(AI9>0,AH9*AI9,\"check\"),IF(AI9>0,\"check\",0))","v":0},{"$f":"IF(AJ9>0,IF((AJ$4/AH9)<32,AJ$4/AH9,\"tba\"),0)","v":0},{"$f":"AK9*AI9*AH9","v":0},{"$f":"F9+K9+P9+U9+Z9+AE9+AJ9","v":0},{"$f":"AM9/AO$2","v":0},{"$f":"ROUNDUP((AN9+AN10)/0.95,0)","v":0},{"$f":"IF(AO9>0,SUM(AN9:AN10)/AO9,0)","v":0},null,null,null,{"$f":"IF(AS9>0,SUM(AN9:AN10)/AS9,0)","v":0}]
[null,null,null,null,null,{"$f":"IF(D10>0,IF(E10>0,D10*E10,\"check\"),IF(E10>0,\"check\",0))","v":0},{"$f":"IF(F10>0,IF((F$4/D10)<32,F$4/D10,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(I10>0,IF(J10>0,I10*J10,\"check\"),IF(J10>0,\"check\",0))","v":0},{"$f":"IF(K10>0,IF((K$4/I10)<32,K$4/I10,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(N10>0,IF(O10>0,N10*O10,\"check\"),IF(O10>0,\"check\",0))","v":0},{"$f":"IF(P10>0,IF((P$4/N10)<32,P$4/N10,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(S10>0,IF(T10>0,S10*T10,\"check\"),IF(T10>0,\"check\",0))","v":0},{"$f":"IF(U10>0,IF((U$4/S10)<32,U$4/S10,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(X10>0,IF(Y10>0,X10*Y10,\"check\"),IF(Y10>0,\"check\",0))","v":0},{"$f":"IF(Z10>0,IF((Z$4/X10)<32,Z$4/X10,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AC10>0,IF(AD10>0,AC10*AD10,\"check\"),IF(AD10>0,\"check\",0))","v":0},{"$f":"IF(AE10>0,IF((AE$4/AC10)<32,AE$4/AC10,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AH10>0,IF(AI10>0,AH10*AI10,\"check\"),IF(AI10>0,\"check\",0))","v":0},{"$f":"IF(AJ10>0,IF((AJ$4/AH10)<32,AJ$4/AH10,\"tba\"),0)","v":0},0,{"$f":"F10+K10+P10+U10+Z10+AE10+AJ10","v":0},{"$f":"AM10/AO$2","v":0}]
[null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
[null,"Maths",null,null,null,{"$f":"IF(D12>0,IF(E12>0,D12*E12,\"check\"),IF(E12>0,\"check\",0))","v":0},{"$f":"IF(F12>0,IF((F$4/D12)<32,F$4/D12,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(I12>0,IF(J12>0,I12*J12,\"check\"),IF(J12>0,\"check\",0))","v":0},{"$f":"IF(K12>0,IF((K$4/I12)<32,K$4/I12,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(N12>0,IF(O12>0,N12*O12,\"check\"),IF(O12>0,\"check\",0))","v":0},{"$f":"IF(P12>0,IF((P$4/N12)<32,P$4/N12,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(S12>0,IF(T12>0,S12*T12,\"check\"),IF(T12>0,\"check\",0))","v":0},{"$f":"IF(U12>0,IF((U$4/S12)<32,U$4/S12,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(X12>0,IF(Y12>0,X12*Y12,\"check\"),IF(Y12>0,\"check\",0))","v":0},{"$f":"IF(Z12>0,IF((Z$4/X12)<32,Z$4/X12,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AC12>0,IF(AD12>0,AC12*AD12,\"check\"),IF(AD12>0,\"check\",0))","v":0},{"$f":"IF(AE12>0,IF((AE$4/AC12)<32,AE$4/AC12,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AH12>0,IF(AI12>0,AH12*AI12,\"check\"),IF(AI12>0,\"check\",0))","v":0},{"$f":"IF(AJ12>0,IF((AJ$4/AH12)<32,AJ$4/AH12,\"tba\"),0)","v":0},0,{"$f":"F12+K12+P12+U12+Z12+AE12+AJ12","v":0},{"$f":"AM12/AO$2","v":0},{"$f":"ROUNDUP((AN12+AN13)/0.95,0)","v":0},{"$f":"IF(AO12>0,SUM(AN12:AN13)/AO12,0)","v":0},null,null,null,{"$f":"IF(AS12>0,SUM(AN12:AN13)/AS12,0)","v":0}]
[null,null,null,null,null,{"$f":"IF(D13>0,IF(E13>0,D13*E13,\"check\"),IF(E13>0,\"check\",0))","v":0},{"$f":"IF(F13>0,IF((F$4/D13)<32,F$4/D13,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(I13>0,IF(J13>0,I13*J13,\"check\"),IF(J13>0,\"check\",0))","v":0},{"$f":"IF(K13>0,IF((K$4/I13)<32,K$4/I13,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(N13>0,IF(O13>0,N13*O13,\"check\"),IF(O13>0,\"check\",0))","v":0},{"$f":"IF(P13>0,IF((P$4/N13)<32,P$4/N13,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(S13>0,IF(T13>0,S13*T13,\"check\"),IF(T13>0,\"check\",0))","v":0},{"$f":"IF(U13>0,IF((U$4/S13)<32,U$4/S13,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(X13>0,IF(Y13>0,X13*Y13,\"check\"),IF(Y13>0,\"check\",0))","v":0},{"$f":"IF(Z13>0,IF((Z$4/X13)<32,Z$4/X13,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AC13>0,IF(AD13>0,AC13*AD13,\"check\"),IF(AD13>0,\"check\",0))","v":0},{"$f":"IF(AE13>0,IF((AE$4/AC13)<32,AE$4/AC13,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AH13>0,IF(AI13>0,AH13*AI13,\"check\"),IF(AI13>0,\"check\",0))","v":0},{"$f":"IF(AJ13>0,IF((AJ$4/AH13)<32,AJ$4/AH13,\"tba\"),0)","v":0},0,{"$f":"F13+K13+P13+U13+Z13+AE13+AJ13","v":0},{"$f":"AM13/AO$2","v":0}]
[null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
[null,"MFL",null,null,null,{"$f":"IF(D15>0,IF(E15>0,D15*E15,\"check\"),IF(E15>0,\"check\",0))","v":0},{"$f":"IF(F15>0,IF((F$4/D15)<32,F$4/D15,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(I15>0,IF(J15>0,I15*J15,\"check\"),IF(J15>0,\"check\",0))","v":0},{"$f":"IF(K15>0,IF((K$4/I15)<32,K$4/I15,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(N15>0,IF(O15>0,N15*O15,\"check\"),IF(O15>0,\"check\",0))","v":0},{"$f":"IF(P15>0,IF((P$4/N15)<32,P$4/N15,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(S15>0,IF(T15>0,S15*T15,\"check\"),IF(T15>0,\"check\",0))","v":0},{"$f":"IF(U15>0,IF((U$4/S15)<32,U$4/S15,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(X15>0,IF(Y15>0,X15*Y15,\"check\"),IF(Y15>0,\"check\",0))","v":0},{"$f":"IF(Z15>0,IF((Z$4/X15)<32,Z$4/X15,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AC15>0,IF(AD15>0,AC15*AD15,\"check\"),IF(AD15>0,\"check\",0))","v":0},{"$f":"IF(AE15>0,IF((AE$4/AC15)<32,AE$4/AC15,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AH15>0,IF(AI15>0,AH15*AI15,\"check\"),IF(AI15>0,\"check\",0))","v":0},{"$f":"IF(AJ15>0,IF((AJ$4/AH15)<32,AJ$4/AH15,\"tba\"),0)","v":0},0,{"$f":"F15+K15+P15+U15+Z15+AE15+AJ15","v":0},{"$f":"AM15/AO$2","v":0},{"$f":"ROUNDUP((AN15+AN16)/0.95,0)","v":0},{"$f":"IF(AO15>0,SUM(AN15:AN16)/AO15,0)","v":0},null,null,null,{"$f":"IF(AS15>0,SUM(AN15:AN16)/AS15,0)","v":0}]
[null,null,null,null,null,{"$f":"IF(D16>0,IF(E16>0,D16*E16,\"check\"),IF(E16>0,\"check\",0))","v":0},{"$f":"IF(F16>0,IF((F$4/D16)<32,F$4/D16,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(I16>0,IF(J16>0,I16*J16,\"check\"),IF(J16>0,\"check\",0))","v":0},{"$f":"IF(K16>0,IF((K$4/I16)<32,K$4/I16,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(N16>0,IF(O16>0,N16*O16,\"check\"),IF(O16>0,\"check\",0))","v":0},{"$f":"IF(P16>0,IF((P$4/N16)<32,P$4/N16,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(S16>0,IF(T16>0,S16*T16,\"check\"),IF(T16>0,\"check\",0))","v":0},{"$f":"IF(U16>0,IF((U$4/S16)<32,U$4/S16,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(X16>0,IF(Y16>0,X16*Y16,\"check\"),IF(Y16>0,\"check\",0))","v":0},{"$f":"IF(Z16>0,IF((Z$4/X16)<32,Z$4/X16,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AC16>0,IF(AD16>0,AC16*AD16,\"check\"),IF(AD16>0,\"check\",0))","v":0},{"$f":"IF(AE16>0,IF((AE$4/AC16)<32,AE$4/AC16,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AH16>0,IF(AI16>0,AH16*AI16,\"check\"),IF(AI16>0,\"check\",0))","v":0},{"$f":"IF(AJ16>0,IF((AJ$4/AH16)<32,AJ$4/AH16,\"tba\"),0)","v":0},0,{"$f":"F16+K16+P16+U16+Z16+AE16+AJ16","v":0},{"$f":"AM16/AO$2","v":0}]
[null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
[null,"Geography",null,null,null,{"$f":"IF(D18>0,IF(E18>0,D18*E18,\"check\"),IF(E18>0,\"check\",0))","v":0},{"$f":"IF(F18>0,IF((F$4/D18)<32,F$4/D18,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(I18>0,IF(J18>0,I18*J18,\"check\"),IF(J18>0,\"check\",0))","v":0},{"$f":"IF(K18>0,IF((K$4/I18)<32,K$4/I18,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(N18>0,IF(O18>0,N18*O18,\"check\"),IF(O18>0,\"check\",0))","v":0},{"$f":"IF(P18>0,IF((P$4/N18)<32,P$4/N18,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(S18>0,IF(T18>0,S18*T18,\"check\"),IF(T18>0,\"check\",0))","v":0},{"$f":"IF(U18>0,IF((U$4/S18)<32,U$4/S18,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(X18>0,IF(Y18>0,X18*Y18,\"check\"),IF(Y18>0,\"check\",0))","v":0},{"$f":"IF(Z18>0,IF((Z$4/X18)<32,Z$4/X18,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AC18>0,IF(AD18>0,AC18*AD18,\"check\"),IF(AD18>0,\"check\",0))","v":0},{"$f":"IF(AE18>0,IF((AE$4/AC18)<32,AE$4/AC18,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AH18>0,IF(AI18>0,AH18*AI18,\"check\"),IF(AI18>0,\"check\",0))","v":0},{"$f":"IF(AJ18>0,IF((AJ$4/AH18)<32,AJ$4/AH18,\"tba\"),0)","v":0},0,{"$f":"F18+K18+P18+U18+Z18+AE18+AJ18","v":0},{"$f":"AM18/AO$2","v":0},{"$f":"ROUND(SUM(AN18:AN27)/0.95,0)","v":0},{"$f":"IF(AO18>0,SUM(AN18:AN27)/AO18,0)","v":0},null,null,null,{"$f":"IF(AS18>0,SUM(AN18:AN27)/AS18,0)","v":0}]
[null,"History",null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,"Religious Education",null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,{"$f":"SUM(AN9:AN27)","v":0},{"$f":"SUM(AO9:AO27)","v":0},{"$f":"IF(AO28>0,(AN28)/AO28,\"\")","v":""},{"$f":"IF(AP28<89%,\"could be higher\",\"\")","v":""},null,{"$f":"SUM(AS18,AS15,AS12,AS9,)","v":0},{"$f":"IF(AS28>0,AN28/AS28,0)","v":0}]
[null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,{"$f":"AO28-AO30","v":0},null,30,{"$f":"AO29*AQ29","v":0}]
["ICT/ business studies ",null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,{"$f":"IF(AE4+AJ4>0,ROUND(AO28*0.1,0),0)","v":0},null,24,{"$f":"AO30*AQ30","v":0}]
[null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
[null,"ICT",null,null,null,{"$f":"IF(D32>0,IF(E32>0,D32*E32,\"check\"),IF(E32>0,\"check\",0))","v":0},{"$f":"IF(F32>0,IF((F$4/D32)<32,F$4/D32,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(I32>0,IF(J32>0,I32*J32,\"check\"),IF(J32>0,\"check\",0))","v":0},{"$f":"IF(K32>0,IF((K$4/I32)<32,K$4/I32,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(N32>0,IF(O32>0,N32*O32,\"check\"),IF(O32>0,\"check\",0))","v":0},{"$f":"IF(P32>0,IF((P$4/N32)<32,P$4/N32,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(S32>0,IF(T32>0,S32*T32,\"check\"),IF(T32>0,\"check\",0))","v":0},{"$f":"IF(U32>0,IF((U$4/S32)<32,U$4/S32,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(X32>0,IF(Y32>0,X32*Y32,\"check\"),IF(Y32>0,\"check\",0))","v":0},{"$f":"IF(Z32>0,IF((Z$4/X32)<32,Z$4/X32,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AC32>0,IF(AD32>0,AC32*AD32,\"check\"),IF(AD32>0,\"check\",0))","v":0},{"$f":"IF(AE32>0,IF((AE$4/AC32)<32,AE$4/AC32,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AH32>0,IF(AI32>0,AH32*AI32,\"check\"),IF(AI32>0,\"check\",0))","v":0},{"$f":"IF(AJ32>0,IF((AJ$4/AH32)<32,AJ$4/AH32,\"tba\"),0)","v":0},0,{"$f":"F32+K32+P32+U32+Z32+AE32+AJ32","v":0},{"$f":"AM32/AO$2","v":0},{"$f":"ROUNDUP(SUM(AN32:AN37)/0.95,0)","v":0},{"$f":"IF(AO32>0,SUM(AN32:AN37)/AO32,0)","v":0},30,{"$f":"AO32*AQ32","v":0},null,{"$f":"IF(AS32>0,SUM(AN32:AN37)/AS32,0)","v":0}]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
["practical learning spaces",null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,{"$f":"P38+U38+Z38+AE38+AJ38","v":0},0]
["science ",null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
[null,"Science",null,null,null,{"$f":"IF(D40>0,IF(E40>0,D40*E40,\"check\"),IF(E40>0,\"check\",0))","v":0},{"$f":"IF(F40>0,IF((F$4/D40)<32,F$4/D40,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(I40>0,IF(J40>0,I40*J40,\"check\"),IF(J40>0,\"check\",0))","v":0},{"$f":"IF(K40>0,IF((K$4/I40)<32,K$4/I40,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(N40>0,IF(O40>0,N40*O40,\"check\"),IF(O40>0,\"check\",0))","v":0},{"$f":"IF(P40>0,IF((P$4/N40)<32,P$4/N40,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(S40>0,IF(T40>0,S40*T40,\"check\"),IF(T40>0,\"check\",0))","v":0},{"$f":"IF(U40>0,IF((U$4/S40)<32,U$4/S40,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(X40>0,IF(Y40>0,X40*Y40,\"check\"),IF(Y40>0,\"check\",0))","v":0},{"$f":"IF(Z40>0,IF((Z$4/X40)<32,Z$4/X40,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AC40>0,IF(AD40>0,AC40*AD40,\"check\"),IF(AD40>0,\"check\",0))","v":0},{"$f":"IF(AE40>0,IF((AE$4/AC40)<32,AE$4/AC40,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AH40>0,IF(AI40>0,AH40*AI40,\"check\"),IF(AI40>0,\"check\",0))","v":0},{"$f":"IF(AJ40>0,IF((AJ$4/AH40)<32,AJ$4/AH40,\"tba\"),0)","v":0},0,{"$f":"F40+K40+P40+U40+Z40+AE40+AJ40","v":0},{"$f":"AM40/AO$2","v":0},{"$f":"ROUNDUP(SUM(AN40:AN45)/0.95,0)","v":0},{"$f":"IF(AO40>0,SUM(AN40:AN45)/AO40,0)","v":0},30,{"$f":"AO40*AQ40","v":0},null,{"$f":"IF(AS40>0,SUM(AN40:AN45)/AS40,0)","v":0}]
[null,null,null,null,null,0,0,{"$f":"G41*E41*D41","v":0},null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
["art",null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
[null,null,null,null,null,{"$f":"IF(D47>0,IF(E47>0,D47*E47,\"check\"),IF(E47>0,\"check\",0))","v":0},{"$f":"IF(F47>0,IF((F$4/D47)<32,F$4/D47,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(I47>0,IF(J47>0,I47*J47,\"check\"),IF(J47>0,\"check\",0))","v":0},{"$f":"IF(K47>0,IF((K$4/I47)<32,K$4/I47,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(N47>0,IF(O47>0,N47*O47,\"check\"),IF(O47>0,\"check\",0))","v":0},{"$f":"IF(P47>0,IF((P$4/N47)<32,P$4/N47,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(S47>0,IF(T47>0,S47*T47,\"check\"),IF(T47>0,\"check\",0))","v":0},{"$f":"IF(U47>0,IF((U$4/S47)<32,U$4/S47,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(X47>0,IF(Y47>0,X47*Y47,\"check\"),IF(Y47>0,\"check\",0))","v":0},{"$f":"IF(Z47>0,IF((Z$4/X47)<32,Z$4/X47,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AC47>0,IF(AD47>0,AC47*AD47,\"check\"),IF(AD47>0,\"check\",0))","v":0},{"$f":"IF(AE47>0,IF((AE$4/AC47)<32,AE$4/AC47,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AH47>0,IF(AI47>0,AH47*AI47,\"check\"),IF(AI47>0,\"check\",0))","v":0},{"$f":"IF(AJ47>0,IF((AJ$4/AH47)<32,AJ$4/AH47,\"tba\"),0)","v":0},0,{"$f":"F47+K47+P47+U47+Z47+AE47+AJ47","v":0},{"$f":"AM47/AO$2","v":0},{"$f":"ROUNDUP(SUM(AN47:AN52)/0.95,0)","v":0},{"$f":"IF(AO47>0,SUM(AN47:AN52)/AO47,0)","v":0},30,{"$f":"AO47*AQ47","v":0},null,{"$f":"IF(AS47>0,SUM(AN47:AN52)/AS47,0)","v":0}]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
["music and drama",null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
[null,null,null,null,null,{"$f":"IF(D54>0,IF(E54>0,D54*E54,\"check\"),IF(E54>0,\"check\",0))","v":0},{"$f":"IF(F54>0,IF((F$4/D54)<32,F$4/D54,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(I54>0,IF(J54>0,I54*J54,\"check\"),IF(J54>0,\"check\",0))","v":0},{"$f":"IF(K54>0,IF((K$4/I54)<32,K$4/I54,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(N54>0,IF(O54>0,N54*O54,\"check\"),IF(O54>0,\"check\",0))","v":0},{"$f":"IF(P54>0,IF((P$4/N54)<32,P$4/N54,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(S54>0,IF(T54>0,S54*T54,\"check\"),IF(T54>0,\"check\",0))","v":0},{"$f":"IF(U54>0,IF((U$4/S54)<32,U$4/S54,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(X54>0,IF(Y54>0,X54*Y54,\"check\"),IF(Y54>0,\"check\",0))","v":0},{"$f":"IF(Z54>0,IF((Z$4/X54)<32,Z$4/X54,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AC54>0,IF(AD54>0,AC54*AD54,\"check\"),IF(AD54>0,\"check\",0))","v":0},{"$f":"IF(AE54>0,IF((AE$4/AC54)<32,AE$4/AC54,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AH54>0,IF(AI54>0,AH54*AI54,\"check\"),IF(AI54>0,\"check\",0))","v":0},{"$f":"IF(AJ54>0,IF((AJ$4/AH54)<32,AJ$4/AH54,\"tba\"),0)","v":0},0,{"$f":"F54+K54+P54+U54+Z54+AE54+AJ54","v":0},{"$f":"AM54/AO$2","v":0},{"$f":"ROUNDUP(SUM(AN54:AN57)/0.95,0)","v":0},{"$f":"IF(AO54>0,SUM(AN54:AN57)/AO54,0)","v":0},24,{"$f":"AO54*AQ54","v":0},null,{"$f":"IF(AS54>0,SUM(AN54:AN57)/AS54,0)","v":0}]
[null,null,null,null,null,{"$f":"IF(D55>0,IF(E55>0,D55*E55,\"check\"),IF(E55>0,\"check\",0))","v":0},{"$f":"IF(F55>0,IF((F$4/D55)<32,F$4/D55,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(I55>0,IF(J55>0,I55*J55,\"check\"),IF(J55>0,\"check\",0))","v":0},{"$f":"IF(K55>0,IF((K$4/I55)<32,K$4/I55,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(N55>0,IF(O55>0,N55*O55,\"check\"),IF(O55>0,\"check\",0))","v":0},{"$f":"IF(P55>0,IF((P$4/N55)<32,P$4/N55,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(S55>0,IF(T55>0,S55*T55,\"check\"),IF(T55>0,\"check\",0))","v":0},{"$f":"IF(U55>0,IF((U$4/S55)<32,U$4/S55,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(X55>0,IF(Y55>0,X55*Y55,\"check\"),IF(Y55>0,\"check\",0))","v":0},{"$f":"IF(Z55>0,IF((Z$4/X55)<32,Z$4/X55,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AC55>0,IF(AD55>0,AC55*AD55,\"check\"),IF(AD55>0,\"check\",0))","v":0},{"$f":"IF(AE55>0,IF((AE$4/AC55)<32,AE$4/AC55,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AH55>0,IF(AI55>0,AH55*AI55,\"check\"),IF(AI55>0,\"check\",0))","v":0},{"$f":"IF(AJ55>0,IF((AJ$4/AH55)<32,AJ$4/AH55,\"tba\"),0)","v":0},0,{"$f":"F55+K55+P55+U55+Z55+AE55+AJ55","v":0},{"$f":"AM55/AO$2","v":0}]
[null,null,null,null,null,{"$f":"IF(D56>0,IF(E56>0,D56*E56,\"check\"),IF(E56>0,\"check\",0))","v":0},{"$f":"IF(F56>0,IF((F$4/D56)<32,F$4/D56,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(I56>0,IF(J56>0,I56*J56,\"check\"),IF(J56>0,\"check\",0))","v":0},{"$f":"IF(K56>0,IF((K$4/I56)<32,K$4/I56,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(N56>0,IF(O56>0,N56*O56,\"check\"),IF(O56>0,\"check\",0))","v":0},{"$f":"IF(P56>0,IF((P$4/N56)<32,P$4/N56,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(S56>0,IF(T56>0,S56*T56,\"check\"),IF(T56>0,\"check\",0))","v":0},{"$f":"IF(U56>0,IF((U$4/S56)<32,U$4/S56,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(X56>0,IF(Y56>0,X56*Y56,\"check\"),IF(Y56>0,\"check\",0))","v":0},{"$f":"IF(Z56>0,IF((Z$4/X56)<32,Z$4/X56,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AC56>0,IF(AD56>0,AC56*AD56,\"check\"),IF(AD56>0,\"check\",0))","v":0},{"$f":"IF(AE56>0,IF((AE$4/AC56)<32,AE$4/AC56,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AH56>0,IF(AI56>0,AH56*AI56,\"check\"),IF(AI56>0,\"check\",0))","v":0},{"$f":"IF(AJ56>0,IF((AJ$4/AH56)<32,AJ$4/AH56,\"tba\"),0)","v":0},0,{"$f":"F56+K56+P56+U56+Z56+AE56+AJ56","v":0},{"$f":"AM56/AO$2","v":0}]
[null,null,null,null,null,{"$f":"IF(D57>0,IF(E57>0,D57*E57,\"check\"),IF(E57>0,\"check\",0))","v":0},{"$f":"IF(F57>0,IF((F$4/D57)<32,F$4/D57,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(I57>0,IF(J57>0,I57*J57,\"check\"),IF(J57>0,\"check\",0))","v":0},{"$f":"IF(K57>0,IF((K$4/I57)<32,K$4/I57,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(N57>0,IF(O57>0,N57*O57,\"check\"),IF(O57>0,\"check\",0))","v":0},{"$f":"IF(P57>0,IF((P$4/N57)<32,P$4/N57,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(S57>0,IF(T57>0,S57*T57,\"check\"),IF(T57>0,\"check\",0))","v":0},{"$f":"IF(U57>0,IF((U$4/S57)<32,U$4/S57,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(X57>0,IF(Y57>0,X57*Y57,\"check\"),IF(Y57>0,\"check\",0))","v":0},{"$f":"IF(Z57>0,IF((Z$4/X57)<32,Z$4/X57,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AC57>0,IF(AD57>0,AC57*AD57,\"check\"),IF(AD57>0,\"check\",0))","v":0},{"$f":"IF(AE57>0,IF((AE$4/AC57)<32,AE$4/AC57,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AH57>0,IF(AI57>0,AH57*AI57,\"check\"),IF(AI57>0,\"check\",0))","v":0},{"$f":"IF(AJ57>0,IF((AJ$4/AH57)<32,AJ$4/AH57,\"tba\"),0)","v":0},0,{"$f":"F57+K57+P57+U57+Z57+AE57+AJ57","v":0},{"$f":"AM57/AO$2","v":0}]
["design and technology",null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
[null,null,null,null,null,{"$f":"IF(D59>0,IF(E59>0,D59*E59,\"check\"),IF(E59>0,\"check\",0))","v":0},{"$f":"IF(F59>0,IF((F$4/D59)<32,F$4/D59,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(I59>0,IF(J59>0,I59*J59,\"check\"),IF(J59>0,\"check\",0))","v":0},{"$f":"IF(K59>0,IF((K$4/I59)<32,K$4/I59,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(N59>0,IF(O59>0,N59*O59,\"check\"),IF(O59>0,\"check\",0))","v":0},{"$f":"IF(P59>0,IF((P$4/N59)<32,P$4/N59,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(S59>0,IF(T59>0,S59*T59,\"check\"),IF(T59>0,\"check\",0))","v":0},{"$f":"IF(U59>0,IF((U$4/S59)<32,U$4/S59,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(X59>0,IF(Y59>0,X59*Y59,\"check\"),IF(Y59>0,\"check\",0))","v":0},{"$f":"IF(Z59>0,IF((Z$4/X59)<32,Z$4/X59,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AC59>0,IF(AD59>0,AC59*AD59,\"check\"),IF(AD59>0,\"check\",0))","v":0},{"$f":"IF(AE59>0,IF((AE$4/AC59)<32,AE$4/AC59,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AH59>0,IF(AI59>0,AH59*AI59,\"check\"),IF(AI59>0,\"check\",0))","v":0},{"$f":"IF(AJ59>0,IF((AJ$4/AH59)<32,AJ$4/AH59,\"tba\"),0)","v":0},0,{"$f":"F59+K59+P59+U59+Z59+AE59+AJ59","v":0},{"$f":"AM59/AO$2","v":0},{"$f":"ROUND(SUM(AN59:AN66)/0.9,0)","v":0},{"$f":"IF(AO59>0,SUM(AN59:AN66)/AO59,0)","v":0},24,{"$f":"AO59*AQ59","v":0},null,{"$f":"IF(AS59>0,SUM(AN59:AN66)/AS59,0)","v":0}]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,{"$f":"G64*E64*D64","v":0},null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
[null,null,null,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,null,null,0,0,0,0,0]
["PE (internal and external)",null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
[null,null,null,null,null,{"$f":"IF(D68>0,IF(E68>0,D68*E68,\"check\"),IF(E68>0,\"check\",0))","v":0},{"$f":"IF(F68>0,IF((F$4/D68)<32,F$4/D68,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(I68>0,IF(J68>0,I68*J68,\"check\"),IF(J68>0,\"check\",0))","v":0},{"$f":"IF(K68>0,IF((K$4/I68)<32,K$4/I68,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(N68>0,IF(O68>0,N68*O68,\"check\"),IF(O68>0,\"check\",0))","v":0},{"$f":"IF(P68>0,IF((P$4/N68)<32,P$4/N68,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(S68>0,IF(T68>0,S68*T68,\"check\"),IF(T68>0,\"check\",0))","v":0},{"$f":"IF(U68>0,IF((U$4/S68)<32,U$4/S68,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(X68>0,IF(Y68>0,X68*Y68,\"check\"),IF(Y68>0,\"check\",0))","v":0},{"$f":"IF(Z68>0,IF((Z$4/X68)<32,Z$4/X68,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AC68>0,IF(AD68>0,AC68*AD68,\"check\"),IF(AD68>0,\"check\",0))","v":0},{"$f":"IF(AE68>0,IF((AE$4/AC68)<32,AE$4/AC68,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AH68>0,IF(AI68>0,AH68*AI68,\"check\"),IF(AI68>0,\"check\",0))","v":0},{"$f":"IF(AJ68>0,IF((AJ$4/AH68)<32,AJ$4/AH68,\"tba\"),0)","v":0},0,{"$f":"F68+K68+P68+U68+Z68+AE68+AJ68","v":0},{"$f":"AM68/AO$2","v":0},{"$f":"ROUNDUP(SUM(AN68:AN71),0)","v":0},{"$f":"IF(AO68>0,SUM(AN68:AN71)/AO68,0)","v":0},30,{"$f":"AO68*AQ68","v":0},null,{"$f":"IF(AS68>0,SUM(AN68:AN71)/AS68,0)","v":0}]
[null,null,null,null,null,{"$f":"IF(D69>0,IF(E69>0,D69*E69,\"check\"),IF(E69>0,\"check\",0))","v":0},{"$f":"IF(F69>0,IF((F$4/D69)<32,F$4/D69,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(I69>0,IF(J69>0,I69*J69,\"check\"),IF(J69>0,\"check\",0))","v":0},{"$f":"IF(K69>0,IF((K$4/I69)<32,K$4/I69,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(N69>0,IF(O69>0,N69*O69,\"check\"),IF(O69>0,\"check\",0))","v":0},{"$f":"IF(P69>0,IF((P$4/N69)<32,P$4/N69,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(S69>0,IF(T69>0,S69*T69,\"check\"),IF(T69>0,\"check\",0))","v":0},{"$f":"IF(U69>0,IF((U$4/S69)<32,U$4/S69,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(X69>0,IF(Y69>0,X69*Y69,\"check\"),IF(Y69>0,\"check\",0))","v":0},{"$f":"IF(Z69>0,IF((Z$4/X69)<32,Z$4/X69,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AC69>0,IF(AD69>0,AC69*AD69,\"check\"),IF(AD69>0,\"check\",0))","v":0},{"$f":"IF(AE69>0,IF((AE$4/AC69)<32,AE$4/AC69,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AH69>0,IF(AI69>0,AH69*AI69,\"check\"),IF(AI69>0,\"check\",0))","v":0},{"$f":"IF(AJ69>0,IF((AJ$4/AH69)<32,AJ$4/AH69,\"tba\"),0)","v":0},0,{"$f":"F69+K69+P69+U69+Z69+AE69+AJ69","v":0},{"$f":"AM69/AO$2","v":0}]
[null,null,null,null,null,{"$f":"IF(D70>0,IF(E70>0,D70*E70,\"check\"),IF(E70>0,\"check\",0))","v":0},{"$f":"IF(F70>0,IF((F$4/D70)<32,F$4/D70,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(I70>0,IF(J70>0,I70*J70,\"check\"),IF(J70>0,\"check\",0))","v":0},{"$f":"IF(K70>0,IF((K$4/I70)<32,K$4/I70,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(N70>0,IF(O70>0,N70*O70,\"check\"),IF(O70>0,\"check\",0))","v":0},{"$f":"IF(P70>0,IF((P$4/N70)<32,P$4/N70,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(S70>0,IF(T70>0,S70*T70,\"check\"),IF(T70>0,\"check\",0))","v":0},{"$f":"IF(U70>0,IF((U$4/S70)<32,U$4/S70,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(X70>0,IF(Y70>0,X70*Y70,\"check\"),IF(Y70>0,\"check\",0))","v":0},{"$f":"IF(Z70>0,IF((Z$4/X70)<32,Z$4/X70,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AC70>0,IF(AD70>0,AC70*AD70,\"check\"),IF(AD70>0,\"check\",0))","v":0},{"$f":"IF(AE70>0,IF((AE$4/AC70)<32,AE$4/AC70,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AH70>0,IF(AI70>0,AH70*AI70,\"check\"),IF(AI70>0,\"check\",0))","v":0},{"$f":"IF(AJ70>0,IF((AJ$4/AH70)<32,AJ$4/AH70,\"tba\"),0)","v":0},0,{"$f":"F70+K70+P70+U70+Z70+AE70+AJ70","v":0},{"$f":"AM70/AO$2","v":0}]
[null,null,null,null,null,{"$f":"IF(D71>0,IF(E71>0,D71*E71,\"check\"),IF(E71>0,\"check\",0))","v":0},{"$f":"IF(F71>0,IF((F$4/D71)<32,F$4/D71,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(I71>0,IF(J71>0,I71*J71,\"check\"),IF(J71>0,\"check\",0))","v":0},{"$f":"IF(K71>0,IF((K$4/I71)<32,K$4/I71,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(N71>0,IF(O71>0,N71*O71,\"check\"),IF(O71>0,\"check\",0))","v":0},{"$f":"IF(P71>0,IF((P$4/N71)<32,P$4/N71,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(S71>0,IF(T71>0,S71*T71,\"check\"),IF(T71>0,\"check\",0))","v":0},{"$f":"IF(U71>0,IF((U$4/S71)<32,U$4/S71,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(X71>0,IF(Y71>0,X71*Y71,\"check\"),IF(Y71>0,\"check\",0))","v":0},{"$f":"IF(Z71>0,IF((Z$4/X71)<32,Z$4/X71,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AC71>0,IF(AD71>0,AC71*AD71,\"check\"),IF(AD71>0,\"check\",0))","v":0},{"$f":"IF(AE71>0,IF((AE$4/AC71)<32,AE$4/AC71,\"tba\"),0)","v":0},0,null,null,{"$f":"IF(AH71>0,IF(AI71>0,AH71*AI71,\"check\"),IF(AI71>0,\"check\",0))","v":0},{"$f":"IF(AJ71>0,IF((AJ$4/AH71)<32,AJ$4/AH71,\"tba\"),0)","v":0},0,{"$f":"F71+K71+P71+U71+Z71+AE71+AJ71","v":0},{"$f":"AM71/AO$2","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AM9:AM71)","v":0},{"$f":"SUM(AN28:AN71)","v":0}]
["totals/ check",null,null,null,{"$f":"SUM(E9:E72)","v":0},{"$f":"SUM(F9:F72)","v":0},null,null,null,{"$f":"SUM(J9:J72)","v":0},{"$f":"SUM(K9:K72)","v":0},null,null,null,{"$f":"SUM(O9:O72)","v":0},{"$f":"SUM(P9:P72)","v":0},null,null,null,{"$f":"SUM(T9:T72)","v":0},{"$f":"SUM(U9:U72)","v":0},null,null,null,{"$f":"SUM(Y9:Y72)","v":0},{"$f":"SUM(Z9:Z72)","v":0},null,null,null,{"$f":"SUM(AD9:AD72)","v":0},{"$f":"SUM(AE9:AE72)","v":0},null,null,null,{"$f":"SUM(AI9:AI72)","v":0},{"$f":"SUM(AJ9:AJ72)","v":0},null,null,{"$f":"F73+K73+P73+U73+Z73+AE73+AJ73","v":0},{"$f":"AM73/AO$2","v":0},{"$f":"AO28+AO32+AO40+AO47+AO54+AO59+AO61+AO68","v":0},null,null,{"$f":"SUM(AR28:AR68)","v":0},{"$f":"SUM(AS28:AS68)","v":0}]
[null,null,null,null,{"$f":"IF(E73=AO2, \"OK\",\"is number of periods in cycle correct?\")","v":"is number of periods in cycle correct?"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AR73/AO73","v":{"$error":"#DIV/0!"}},"workplaces per room"]
["Target",null,null,null,null,null,{"$f":"F4*AO2","v":9000},null,null,null,null,{"$f":"K4*AO2","v":9000},null,null,null,null,{"$f":"P4*AO2","v":9000},null,null,null,null,{"$f":"U4*AO2","v":9000},null,null,null,null,{"$f":"Z4*AO2","v":9000},null,null,null,null,{"$f":"AE4*AO2","v":0},null,null,null,null,{"$f":"AJ4*AO2","v":0},null,null,null,"overall frequency of use",{"$f":"AN73/AO73","v":{"$error":"#DIV/0!"}}]
["Actual",null,null,null,null,null,{"$f":"SUM(H9:H71)","v":0},null,null,null,null,{"$f":"SUM(M9:M71)","v":0},null,null,null,null,{"$f":"SUM(R9:R71)","v":0},null,null,null,null,{"$f":"SUM(W9:W71)","v":0},null,null,null,null,{"$f":"SUM(AB9:AB71)","v":0},null,null,null,null,{"$f":"SUM(AG9:AG71)","v":0},null,null,null,null,{"$f":"SUM(AL9:AL71)","v":0},null,null,null,null,null,null,null,"average group size",{"$f":"(AO4*AO2)/AM72","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"overall occupancy",{"$f":"AT76/AR74","v":{"$error":"#DIV/0!"}},null,null,"teachers @ 100% contact",{"$f":"AM73/AO2","v":0}]
["Difference",null,null,null,null,null,{"$f":"G76/G75","v":0},null,null,null,null,{"$f":"L76/L75","v":0},null,null,null,null,{"$f":"Q76/Q75","v":0},null,null,null,null,{"$f":"V76/V75","v":0},null,null,null,null,{"$f":"AA76/AA75","v":0},null,null,null,null,{"$f":"AF76/AF75","v":{"$error":"#DIV/0!"}},null,null,null,null,{"$f":"AK76/AK75","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,"teachers @ 75% contact",{"$f":"AT77/0.75","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"utilisation (incl outdoor PE)",{"$f":"AO4/AR73","v":{"$error":"#DIV/0!"}},null,null,"pupil: teacher ratio",{"$f":"AO4/AT78","v":{"$error":"#DIV/0!"}}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(G81:AK81)","v":0}]
[]
[]
[null,{"$f":"'Secondary SoA'!S2","v":"[Insert Project Code and Scheme Name here in title sheet]"},null,"Y7 curriculum",null,null,null,null,"Y8 curriculum",null,null,null,null,"Y9 curriculum",null,null,null,null,"Y10 curriculum",null,null,null,null,"Y11 curriculum",null,null,null,null,"Y12 curriculum",null,null,null,null,"Y13 curriculum",null,null,null,null,null,"Periods in cycle",{"$f":"'curriculum analysis (optional)'!AO2","v":50},null,"age range",{"$f":"'Secondary SoA'!K2","v":"11-18"}]
[]
[null,"FUTURE TIMETABLE",null,"number in cohort:",null,{"$f":"IF('Secondary SoA'!K5,'Secondary SoA'!K5/'Secondary SoA'!O5,0)","v":180},null,null,"number in cohort:",null,{"$f":"F86","v":180},null,null,"number in cohort:",null,{"$f":"F86","v":180},null,null,"number in cohort:",null,{"$f":"F86","v":180},null,null,"number in cohort:",null,{"$f":"F86","v":180},null,null,"number in cohort:",null,{"$f":"'Secondary SoA'!K6/2","v":112.5},null,null,"number in cohort:",null,{"$f":"'Secondary SoA'!K6-'curriculum analysis (optional)'!AE86","v":112.5},null,null,null,"total places",{"$f":"F86+K86+P86+U86+Z86+AE86+AJ86","v":1125},null,"utilisation factor",{"$f":"AT86*0.9","v":0.63900000000000001},"to",{"$f":"VLOOKUP(AR84,'Prog Assums'!E6:L17,8,FALSE)","v":0.71}]
[]
[null,"Course title",null,"number of groups","number of periods","total","Typical group size",null,"number of groups","number of periods","total","Typical group size",null,"number of groups","number of periods","total","Typical group size",null,"number of groups","number of periods","total","Typical group size",null,"number of groups","number of periods","total","Typical group size",null,"number of groups","number of periods","total","Typical group size",null,"number of groups","number of periods","total","Typical group size",null,"totals","rooms req'd at 100% use","required no. of rooms","frequency of use","room capacity","basic work-places","actual no. of rooms","frequency of use"]
[null,"eg En/ Sci etc",null,null,null,null,"eg 30",null,null,null,null,"eg 30",null,null,null,null,"eg 30",null,null,null,null,"eg 30",null,null,null,null,"eg 30",null,null,null,null,"eg 30",null,null,null,null,"eg 30",null,null,null,null,null,null,null,"if known"]
["General teaching"]
[null,{"$f":"'curriculum analysis (optional)'!B9","v":"English"},null,{"$f":"IF(F$86>0,ROUND(D9*F$86/F$4,0),0)","v":0},{"$f":"'curriculum analysis (optional)'!E9","v":0},{"$f":"IF(D91>0,IF(E91>0,D91*E91,\"check\"),IF(E91>0,\"check\",0))","v":0},{"$f":"IF(F91>0,IF((F$86/D91)<32,F$86/D91,\"tba\"),0)","v":0},{"$f":"G91*E91*D91","v":0},{"$f":"IF(K$86>0,ROUND(I9*K$86/K$4,0),0)","v":0},{"$f":"'curriculum analysis (optional)'!J9","v":0},{"$f":"IF(I91>0,IF(J91>0,I91*J91,\"check\"),IF(J91>0,\"check\",0))","v":0},{"$f":"IF(K91>0,IF((K$86/I91)<32,K$86/I91,\"tba\"),0)","v":0},{"$f":"L91*J91*I91","v":0},{"$f":"IF(P$86>0,ROUND(N9*P$86/P$4,0),0)","v":0},{"$f":"'curriculum analysis (optional)'!O9","v":0},{"$f":"IF(N91>0,IF(O91>0,N91*O91,\"check\"),IF(O91>0,\"check\",0))","v":0},{"$f":"IF(P91>0,IF((P$86/N91)<32,P$86/N91,\"tba\"),0)","v":0},{"$f":"Q91*O91*N91","v":0},{"$f":"IF(U$86>0,ROUND(S9*U$86/U$4,0),0)","v":0},{"$f":"'curriculum analysis (optional)'!T9","v":0},{"$f":"IF(S91>0,IF(T91>0,S91*T91,\"check\"),IF(T91>0,\"check\",0))","v":0},{"$f":"IF(U91>0,IF((U$86/S91)<32,U$86/S91,\"tba\"),0)","v":0},{"$f":"V91*T91*S91","v":0},{"$f":"IF(Z$86>0,ROUND(X9*Z$86/Z$4,0),0)","v":0},{"$f":"'curriculum analysis (optional)'!Y9","v":0},{"$f":"IF(X91>0,IF(Y91>0,X91*Y91,\"check\"),IF(Y91>0,\"check\",0))","v":0},{"$f":"IF(Z91>0,IF((Z$86/X91)<32,Z$86/X91,\"tba\"),0)","v":0},{"$f":"AA91*Y91*X91","v":0},{"$f":"'curriculum analysis (optional)'!AC9","v":0},{"$f":"'curriculum analysis (optional)'!AD9","v":0},{"$f":"IF(AC91>0,IF(AD91>0,AC91*AD91,\"check\"),IF(AD91>0,\"check\",0))","v":0},{"$f":"IF(AE91>0,IF((AE$86/AC91)<32,AE$86/AC91,\"tba\"),0)","v":0},{"$f":"AF91*AD91*AC91","v":0},{"$f":"'curriculum analysis (optional)'!AH9","v":0},{"$f":"'curriculum analysis (optional)'!AI9","v":0},{"$f":"IF(AH91>0,IF(AI91>0,AH91*AI91,\"check\"),IF(AI91>0,\"check\",0))","v":0},{"$f":"IF(AJ91>0,IF((AJ$86/AH91)<32,AJ$86/AH91,\"tba\"),0)","v":0},{"$f":"AK91*AI91*AH91","v":0},{"$f":"F91+K91+P91+U91+Z91+AE91+AJ91","v":0},{"$f":"AM91/AO$84","v":0},{"$f":"ROUNDUP((AN91+AN92)/0.95,0)","v":0},{"$f":"IF(AO91>0,SUM(AN91:AN92)/AO91,0)","v":0},null,null,null,{"$f":"IF(AS91>0,SUM(AN91:AN92)/AS91,0)","v":0}]
[null,{"$f":"'curriculum analysis (optional)'!B10","v":0},null,{"$f":"IF(F$86>0,ROUND(D10*F$86/F$4,0),0)","v":0},{"$f":"'curriculum analysis (optional)'!E10","v":0},{"$f":"IF(D92>0,IF(E92>0,D92*E92,\"check\"),IF(E92>0,\"check\",0))","v":0},{"$f":"IF(F92>0,IF((F$86/D92)<32,F$86/D92,\"tba\"),0)","v":0},{"$f":"G92*E92*D92","v":0},{"$f":"IF(K$86>0,ROUND(I10*K$86/K$4,0),0)","v":0},{"$f":"'curriculum analysis (optional)'!J10","v":0},{"$f":"IF(I92>0,IF(J92>0,I92*J92,\"check\"),IF(J92>0,\"check\",0))","v":0},{"$f":"IF(K92>0,IF((K$86/I92)<32,K$86/I92,\"tba\"),0)","v":0},{"$f":"L92*J92*I92","v":0},{"$f":"IF(P$86>0,ROUND(N10*P$86/P$4,0),0)","v":0},{"$f":"'curriculum analysis (optional)'!O10","v":0},{"$f":"IF(N92>0,IF(O92>0,N92*O92,\"check\"),IF(O92>0,\"check\",0))","v":0},{"$f":"IF(P92>0,IF((P$86/N92)<32,P$86/N92,\"tba\"),0)","v":0},{"$f":"Q92*O92*N92","v":0},{"$f":"IF(U$86>0,ROUND(S10*U$86/U$4,0),0)","v":0},{"$f":"'curriculum analysis (optional)'!T10","v":0},{"$f":"IF(S92>0,IF(T92>0,S92*T92,\"check\"),IF(T92>0,\"check\",0))","v":0},{"$f":"IF(U92>0,IF((U$86/S92)<32,U$86/S92,\"tba\"),0)","v":0},{"$f":"V92*T92*S92","v":0},{"$f":"IF(Z$86>0,ROUND(X10*Z$86/Z$4,0),0)","v":0},{"$f":"'curriculum analysis (optional)'!Y10","v":0},{"$f":"IF(X92>0,IF(Y92>0,X92*Y92,\"check\"),IF(Y92>0,\"check\",0))","v":0},{"$f":"IF(Z92>0,IF((Z$86/X92)<32,Z$86/X92,\"tba\"),0)","v":0},{"$f":"AA92*Y92*X92","v":0},{"$f":"'curriculum analysis (optional)'!AC10","v":0},{"$f":"'curriculum analysis (optional)'!AD10","v":0},{"$f":"IF(AC92>0,IF(AD92>0,AC92*AD92,\"check\"),IF(AD92>0,\"check\",0))","v":0},{"$f":"IF(AE92>0,IF((AE$86/AC92)<32,AE$86/AC92,\"tba\"),0)","v":0},{"$f":"AF92*AD92*AC92","v":0},{"$f":"'curriculum analysis (optional)'!AH10","v":0},{"$f":"'curriculum analysis (optional)'!AI10","v":0},{"$f":"IF(AH92>0,IF(AI92>0,AH92*AI92,\"check\"),IF(AI92>0,\"check\",0))","v":0},{"$f":"IF(AJ92>0,IF((AJ$86/AH92)<32,AJ$86/AH92,\"tba\"),0)","v":0},{"$f":"AK92*AI92*AH92","v":0},{"$f":"F92+K92+P92+U92+Z92+AE92+AJ92","v":0},{"$f":"AM92/AO$84","v":0}]
[null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
[null,{"$f":"'curriculum analysis (optional)'!B12","v":"Maths"},null,0,{"$f":"'curriculum analysis (optional)'!E12","v":0},{"$f":"IF(D94>0,IF(E94>0,D94*E94,\"check\"),IF(E94>0,\"check\",0))","v":0},{"$f":"IF(F94>0,IF((F$86/D94)<32,F$86/D94,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!J12","v":0},{"$f":"IF(I94>0,IF(J94>0,I94*J94,\"check\"),IF(J94>0,\"check\",0))","v":0},{"$f":"IF(K94>0,IF((K$86/I94)<32,K$86/I94,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!O12","v":0},{"$f":"IF(N94>0,IF(O94>0,N94*O94,\"check\"),IF(O94>0,\"check\",0))","v":0},{"$f":"IF(P94>0,IF((P$86/N94)<32,P$86/N94,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!T12","v":0},{"$f":"IF(S94>0,IF(T94>0,S94*T94,\"check\"),IF(T94>0,\"check\",0))","v":0},{"$f":"IF(U94>0,IF((U$86/S94)<32,U$86/S94,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!Y12","v":0},{"$f":"IF(X94>0,IF(Y94>0,X94*Y94,\"check\"),IF(Y94>0,\"check\",0))","v":0},{"$f":"IF(Z94>0,IF((Z$86/X94)<32,Z$86/X94,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AC12","v":0},{"$f":"'curriculum analysis (optional)'!AD12","v":0},{"$f":"IF(AC94>0,IF(AD94>0,AC94*AD94,\"check\"),IF(AD94>0,\"check\",0))","v":0},{"$f":"IF(AE94>0,IF((AE$86/AC94)<32,AE$86/AC94,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AH12","v":0},{"$f":"'curriculum analysis (optional)'!AI12","v":0},{"$f":"IF(AH94>0,IF(AI94>0,AH94*AI94,\"check\"),IF(AI94>0,\"check\",0))","v":0},{"$f":"IF(AJ94>0,IF((AJ$86/AH94)<32,AJ$86/AH94,\"tba\"),0)","v":0},0,{"$f":"F94+K94+P94+U94+Z94+AE94+AJ94","v":0},0,{"$f":"ROUNDUP((AN94+AN95)/0.95,0)","v":0},{"$f":"IF(AO94>0,SUM(AN94:AN95)/AO94,0)","v":0},null,null,null,{"$f":"IF(AS94>0,SUM(AN94:AN95)/AS94,0)","v":0}]
[null,{"$f":"'curriculum analysis (optional)'!B13","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E13","v":0},{"$f":"IF(D95>0,IF(E95>0,D95*E95,\"check\"),IF(E95>0,\"check\",0))","v":0},{"$f":"IF(F95>0,IF((F$86/D95)<32,F$86/D95,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!J13","v":0},{"$f":"IF(I95>0,IF(J95>0,I95*J95,\"check\"),IF(J95>0,\"check\",0))","v":0},{"$f":"IF(K95>0,IF((K$86/I95)<32,K$86/I95,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!O13","v":0},{"$f":"IF(N95>0,IF(O95>0,N95*O95,\"check\"),IF(O95>0,\"check\",0))","v":0},{"$f":"IF(P95>0,IF((P$86/N95)<32,P$86/N95,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!T13","v":0},{"$f":"IF(S95>0,IF(T95>0,S95*T95,\"check\"),IF(T95>0,\"check\",0))","v":0},{"$f":"IF(U95>0,IF((U$86/S95)<32,U$86/S95,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!Y13","v":0},{"$f":"IF(X95>0,IF(Y95>0,X95*Y95,\"check\"),IF(Y95>0,\"check\",0))","v":0},{"$f":"IF(Z95>0,IF((Z$86/X95)<32,Z$86/X95,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AC13","v":0},{"$f":"'curriculum analysis (optional)'!AD13","v":0},{"$f":"IF(AC95>0,IF(AD95>0,AC95*AD95,\"check\"),IF(AD95>0,\"check\",0))","v":0},{"$f":"IF(AE95>0,IF((AE$86/AC95)<32,AE$86/AC95,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AH13","v":0},{"$f":"'curriculum analysis (optional)'!AI13","v":0},{"$f":"IF(AH95>0,IF(AI95>0,AH95*AI95,\"check\"),IF(AI95>0,\"check\",0))","v":0},{"$f":"IF(AJ95>0,IF((AJ$86/AH95)<32,AJ$86/AH95,\"tba\"),0)","v":0},0,{"$f":"F95+K95+P95+U95+Z95+AE95+AJ95","v":0},0]
[null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
[null,{"$f":"'curriculum analysis (optional)'!B15","v":"MFL"},null,0,{"$f":"'curriculum analysis (optional)'!E15","v":0},{"$f":"IF(D97>0,IF(E97>0,D97*E97,\"check\"),IF(E97>0,\"check\",0))","v":0},{"$f":"IF(F97>0,IF((F$86/D97)<32,F$86/D97,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!J15","v":0},{"$f":"IF(I97>0,IF(J97>0,I97*J97,\"check\"),IF(J97>0,\"check\",0))","v":0},{"$f":"IF(K97>0,IF((K$86/I97)<32,K$86/I97,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!O15","v":0},{"$f":"IF(N97>0,IF(O97>0,N97*O97,\"check\"),IF(O97>0,\"check\",0))","v":0},{"$f":"IF(P97>0,IF((P$86/N97)<32,P$86/N97,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!T15","v":0},{"$f":"IF(S97>0,IF(T97>0,S97*T97,\"check\"),IF(T97>0,\"check\",0))","v":0},{"$f":"IF(U97>0,IF((U$86/S97)<32,U$86/S97,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!Y15","v":0},{"$f":"IF(X97>0,IF(Y97>0,X97*Y97,\"check\"),IF(Y97>0,\"check\",0))","v":0},{"$f":"IF(Z97>0,IF((Z$86/X97)<32,Z$86/X97,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AC15","v":0},{"$f":"'curriculum analysis (optional)'!AD15","v":0},{"$f":"IF(AC97>0,IF(AD97>0,AC97*AD97,\"check\"),IF(AD97>0,\"check\",0))","v":0},{"$f":"IF(AE97>0,IF((AE$86/AC97)<32,AE$86/AC97,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AH15","v":0},{"$f":"'curriculum analysis (optional)'!AI15","v":0},{"$f":"IF(AH97>0,IF(AI97>0,AH97*AI97,\"check\"),IF(AI97>0,\"check\",0))","v":0},{"$f":"IF(AJ97>0,IF((AJ$86/AH97)<32,AJ$86/AH97,\"tba\"),0)","v":0},0,{"$f":"F97+K97+P97+U97+Z97+AE97+AJ97","v":0},0,{"$f":"ROUNDUP((AN97+AN98)/0.95,0)","v":0},{"$f":"IF(AO97>0,SUM(AN97:AN98)/AO97,0)","v":0},null,null,null,{"$f":"IF(AS97>0,SUM(AN97:AN98)/AS97,0)","v":0}]
[null,{"$f":"'curriculum analysis (optional)'!B16","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E16","v":0},{"$f":"IF(D98>0,IF(E98>0,D98*E98,\"check\"),IF(E98>0,\"check\",0))","v":0},{"$f":"IF(F98>0,IF((F$86/D98)<32,F$86/D98,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!J16","v":0},{"$f":"IF(I98>0,IF(J98>0,I98*J98,\"check\"),IF(J98>0,\"check\",0))","v":0},{"$f":"IF(K98>0,IF((K$86/I98)<32,K$86/I98,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!O16","v":0},{"$f":"IF(N98>0,IF(O98>0,N98*O98,\"check\"),IF(O98>0,\"check\",0))","v":0},{"$f":"IF(P98>0,IF((P$86/N98)<32,P$86/N98,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!T16","v":0},{"$f":"IF(S98>0,IF(T98>0,S98*T98,\"check\"),IF(T98>0,\"check\",0))","v":0},{"$f":"IF(U98>0,IF((U$86/S98)<32,U$86/S98,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!Y16","v":0},{"$f":"IF(X98>0,IF(Y98>0,X98*Y98,\"check\"),IF(Y98>0,\"check\",0))","v":0},{"$f":"IF(Z98>0,IF((Z$86/X98)<32,Z$86/X98,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AC16","v":0},{"$f":"'curriculum analysis (optional)'!AD16","v":0},{"$f":"IF(AC98>0,IF(AD98>0,AC98*AD98,\"check\"),IF(AD98>0,\"check\",0))","v":0},{"$f":"IF(AE98>0,IF((AE$86/AC98)<32,AE$86/AC98,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AH16","v":0},{"$f":"'curriculum analysis (optional)'!AI16","v":0},{"$f":"IF(AH98>0,IF(AI98>0,AH98*AI98,\"check\"),IF(AI98>0,\"check\",0))","v":0},{"$f":"IF(AJ98>0,IF((AJ$86/AH98)<32,AJ$86/AH98,\"tba\"),0)","v":0},0,{"$f":"F98+K98+P98+U98+Z98+AE98+AJ98","v":0},0]
[null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
[null,{"$f":"'curriculum analysis (optional)'!B18","v":"Geography"},null,0,{"$f":"'curriculum analysis (optional)'!E18","v":0},{"$f":"IF(D100>0,IF(E100>0,D100*E100,\"check\"),IF(E100>0,\"check\",0))","v":0},{"$f":"IF(F100>0,IF((F$86/D100)<32,F$86/D100,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!J18","v":0},{"$f":"IF(I100>0,IF(J100>0,I100*J100,\"check\"),IF(J100>0,\"check\",0))","v":0},{"$f":"IF(K100>0,IF((K$86/I100)<32,K$86/I100,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!O18","v":0},{"$f":"IF(N100>0,IF(O100>0,N100*O100,\"check\"),IF(O100>0,\"check\",0))","v":0},{"$f":"IF(P100>0,IF((P$86/N100)<32,P$86/N100,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!T18","v":0},{"$f":"IF(S100>0,IF(T100>0,S100*T100,\"check\"),IF(T100>0,\"check\",0))","v":0},{"$f":"IF(U100>0,IF((U$86/S100)<32,U$86/S100,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!Y18","v":0},{"$f":"IF(X100>0,IF(Y100>0,X100*Y100,\"check\"),IF(Y100>0,\"check\",0))","v":0},{"$f":"IF(Z100>0,IF((Z$86/X100)<32,Z$86/X100,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AC18","v":0},{"$f":"'curriculum analysis (optional)'!AD18","v":0},{"$f":"IF(AC100>0,IF(AD100>0,AC100*AD100,\"check\"),IF(AD100>0,\"check\",0))","v":0},{"$f":"IF(AE100>0,IF((AE$86/AC100)<32,AE$86/AC100,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AH18","v":0},{"$f":"'curriculum analysis (optional)'!AI18","v":0},{"$f":"IF(AH100>0,IF(AI100>0,AH100*AI100,\"check\"),IF(AI100>0,\"check\",0))","v":0},{"$f":"IF(AJ100>0,IF((AJ$86/AH100)<32,AJ$86/AH100,\"tba\"),0)","v":0},0,{"$f":"F100+K100+P100+U100+Z100+AE100+AJ100","v":0},0,{"$f":"ROUND(SUM(AN100:AN109)/0.95,0)","v":0},{"$f":"IF(AO100>0,SUM(AN100:AN109)/AO100,0)","v":0},null,null,null,{"$f":"IF(AS100>0,SUM(AN100:AN109)/AS100,0)","v":0}]
[null,{"$f":"'curriculum analysis (optional)'!B19","v":"History"},null,0,{"$f":"'curriculum analysis (optional)'!E19","v":0},{"$f":"IF(D101>0,IF(E101>0,D101*E101,\"check\"),IF(E101>0,\"check\",0))","v":0},{"$f":"IF(F101>0,IF((F$86/D101)<32,F$86/D101,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!J19","v":0},{"$f":"IF(I101>0,IF(J101>0,I101*J101,\"check\"),IF(J101>0,\"check\",0))","v":0},{"$f":"IF(K101>0,IF((K$86/I101)<32,K$86/I101,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!O19","v":0},{"$f":"IF(N101>0,IF(O101>0,N101*O101,\"check\"),IF(O101>0,\"check\",0))","v":0},{"$f":"IF(P101>0,IF((P$86/N101)<32,P$86/N101,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!T19","v":0},{"$f":"IF(S101>0,IF(T101>0,S101*T101,\"check\"),IF(T101>0,\"check\",0))","v":0},{"$f":"IF(U101>0,IF((U$86/S101)<32,U$86/S101,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!Y19","v":0},{"$f":"IF(X101>0,IF(Y101>0,X101*Y101,\"check\"),IF(Y101>0,\"check\",0))","v":0},{"$f":"IF(Z101>0,IF((Z$86/X101)<32,Z$86/X101,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AC19","v":0},{"$f":"'curriculum analysis (optional)'!AD19","v":0},{"$f":"IF(AC101>0,IF(AD101>0,AC101*AD101,\"check\"),IF(AD101>0,\"check\",0))","v":0},{"$f":"IF(AE101>0,IF((AE$86/AC101)<32,AE$86/AC101,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AH19","v":0},{"$f":"'curriculum analysis (optional)'!AI19","v":0},{"$f":"IF(AH101>0,IF(AI101>0,AH101*AI101,\"check\"),IF(AI101>0,\"check\",0))","v":0},{"$f":"IF(AJ101>0,IF((AJ$86/AH101)<32,AJ$86/AH101,\"tba\"),0)","v":0},0,{"$f":"F101+K101+P101+U101+Z101+AE101+AJ101","v":0},0]
[null,{"$f":"'curriculum analysis (optional)'!B20","v":"Religious Education"},null,0,{"$f":"'curriculum analysis (optional)'!E20","v":0},0,{"$f":"IF(F102>0,IF((F$86/D102)<32,F$86/D102,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!J20","v":0},0,{"$f":"IF(K102>0,IF((K$86/I102)<32,K$86/I102,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!O20","v":0},0,{"$f":"IF(P102>0,IF((P$86/N102)<32,P$86/N102,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!T20","v":0},0,{"$f":"IF(U102>0,IF((U$86/S102)<32,U$86/S102,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!Y20","v":0},0,{"$f":"IF(Z102>0,IF((Z$86/X102)<32,Z$86/X102,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AC20","v":0},{"$f":"'curriculum analysis (optional)'!AD20","v":0},0,{"$f":"IF(AE102>0,IF((AE$86/AC102)<32,AE$86/AC102,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AH20","v":0},{"$f":"'curriculum analysis (optional)'!AI20","v":0},0,{"$f":"IF(AJ102>0,IF((AJ$86/AH102)<32,AJ$86/AH102,\"tba\"),0)","v":0},0,{"$f":"F102+K102+P102+U102+Z102+AE102+AJ102","v":0},0]
[null,{"$f":"'curriculum analysis (optional)'!B21","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E21","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J21","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O21","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T21","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y21","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC21","v":0},{"$f":"'curriculum analysis (optional)'!AD21","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH21","v":0},{"$f":"'curriculum analysis (optional)'!AI21","v":0},0,0,0,0,0]
[null,{"$f":"'curriculum analysis (optional)'!B22","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E22","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J22","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O22","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T22","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y22","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC22","v":0},{"$f":"'curriculum analysis (optional)'!AD22","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH22","v":0},{"$f":"'curriculum analysis (optional)'!AI22","v":0},0,0,0,0,0]
[null,{"$f":"'curriculum analysis (optional)'!B23","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E23","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J23","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O23","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T23","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y23","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC23","v":0},{"$f":"'curriculum analysis (optional)'!AD23","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH23","v":0},{"$f":"'curriculum analysis (optional)'!AI23","v":0},0,0,0,0,0]
[null,{"$f":"'curriculum analysis (optional)'!B24","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E24","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J24","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O24","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T24","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y24","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC24","v":0},{"$f":"'curriculum analysis (optional)'!AD24","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH24","v":0},{"$f":"'curriculum analysis (optional)'!AI24","v":0},0,0,0,0,0]
[null,{"$f":"'curriculum analysis (optional)'!B25","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E25","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J25","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O25","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T25","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y25","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC25","v":0},{"$f":"'curriculum analysis (optional)'!AD25","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH25","v":0},{"$f":"'curriculum analysis (optional)'!AI25","v":0},0,0,0,0,0]
[null,{"$f":"'curriculum analysis (optional)'!B26","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E26","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J26","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O26","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T26","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y26","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC26","v":0},{"$f":"'curriculum analysis (optional)'!AD26","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH26","v":0},{"$f":"'curriculum analysis (optional)'!AI26","v":0},0,0,0,0,0]
[null,{"$f":"'curriculum analysis (optional)'!B27","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E27","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J27","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O27","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T27","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y27","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC27","v":0},{"$f":"'curriculum analysis (optional)'!AD27","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH27","v":0},{"$f":"'curriculum analysis (optional)'!AI27","v":0},0,0,0,0,0]
[null,null,null,null,null,null,null,{"$f":"G110*E110*D110","v":0},null,null,null,null,{"$f":"L110*J110*I110","v":0},null,null,null,null,{"$f":"Q110*O110*N110","v":0},null,null,null,null,{"$f":"V110*T110*S110","v":0},null,null,null,null,{"$f":"AA110*Y110*X110","v":0},null,null,null,null,{"$f":"AF110*AD110*AC110","v":0},null,null,null,null,{"$f":"AK110*AI110*AH110","v":0},null,{"$f":"SUM(AN91:AN109)","v":0},{"$f":"SUM(AO91:AO109)","v":0},{"$f":"IF(AO110>0,(AN110)/AO110,\"\")","v":""},{"$f":"IF(AP110<89%,\"could be higher\",\"\")","v":""},null,{"$f":"SUM(AS100,AS97,AS94,AS91,)","v":0},{"$f":"IF(AS110>0,AN110/AS110,0)","v":0}]
[null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,{"$f":"AO110-AO112","v":0},null,30,{"$f":"AO111*AQ111","v":0}]
["ICT/ business studies ",null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,{"$f":"IF(AE86+AJ86>0,ROUND(AO110*0.1,0),0)","v":0},null,24,{"$f":"AO112*AQ112","v":0}]
[null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
[null,{"$f":"'curriculum analysis (optional)'!B32","v":"ICT"},null,0,{"$f":"'curriculum analysis (optional)'!E32","v":0},{"$f":"IF(D114>0,IF(E114>0,D114*E114,\"check\"),IF(E114>0,\"check\",0))","v":0},{"$f":"IF(F114>0,IF((F$86/D114)<32,F$86/D114,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!J32","v":0},{"$f":"IF(I114>0,IF(J114>0,I114*J114,\"check\"),IF(J114>0,\"check\",0))","v":0},{"$f":"IF(K114>0,IF((K$86/I114)<32,K$86/I114,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!O32","v":0},{"$f":"IF(N114>0,IF(O114>0,N114*O114,\"check\"),IF(O114>0,\"check\",0))","v":0},{"$f":"IF(P114>0,IF((P$86/N114)<32,P$86/N114,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!T32","v":0},{"$f":"IF(S114>0,IF(T114>0,S114*T114,\"check\"),IF(T114>0,\"check\",0))","v":0},{"$f":"IF(U114>0,IF((U$86/S114)<32,U$86/S114,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!Y32","v":0},{"$f":"IF(X114>0,IF(Y114>0,X114*Y114,\"check\"),IF(Y114>0,\"check\",0))","v":0},{"$f":"IF(Z114>0,IF((Z$86/X114)<32,Z$86/X114,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AC32","v":0},{"$f":"'curriculum analysis (optional)'!AD32","v":0},{"$f":"IF(AC114>0,IF(AD114>0,AC114*AD114,\"check\"),IF(AD114>0,\"check\",0))","v":0},{"$f":"IF(AE114>0,IF((AE$86/AC114)<32,AE$86/AC114,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AH32","v":0},{"$f":"'curriculum analysis (optional)'!AI32","v":0},{"$f":"IF(AH114>0,IF(AI114>0,AH114*AI114,\"check\"),IF(AI114>0,\"check\",0))","v":0},{"$f":"IF(AJ114>0,IF((AJ$86/AH114)<32,AJ$86/AH114,\"tba\"),0)","v":0},0,0,{"$f":"AM114/AO$84","v":0},{"$f":"ROUNDUP(SUM(AN114:AN119)/0.95,0)","v":0},{"$f":"IF(AO114>0,SUM(AN114:AN119)/AO114,0)","v":0},30,{"$f":"AO114*AQ114","v":0},null,{"$f":"IF(AS114>0,SUM(AN114:AN119)/AS114,0)","v":0}]
[null,{"$f":"'curriculum analysis (optional)'!B33","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E33","v":0},0,0,{"$f":"G115*E115*D115","v":0},0,{"$f":"'curriculum analysis (optional)'!J33","v":0},0,0,{"$f":"L115*J115*I115","v":0},0,{"$f":"'curriculum analysis (optional)'!O33","v":0},0,0,{"$f":"Q115*O115*N115","v":0},0,{"$f":"'curriculum analysis (optional)'!T33","v":0},0,0,{"$f":"V115*T115*S115","v":0},0,{"$f":"'curriculum analysis (optional)'!Y33","v":0},0,0,{"$f":"AA115*Y115*X115","v":0},{"$f":"'curriculum analysis (optional)'!AC33","v":0},{"$f":"'curriculum analysis (optional)'!AD33","v":0},0,0,{"$f":"AF115*AD115*AC115","v":0},{"$f":"'curriculum analysis (optional)'!AH33","v":0},{"$f":"'curriculum analysis (optional)'!AI33","v":0},0,0,{"$f":"AK115*AI115*AH115","v":0},{"$f":"F115+K115+P115+U115+Z115+AE115+AJ115","v":0},0]
[null,{"$f":"'curriculum analysis (optional)'!B34","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E34","v":0},0,0,{"$f":"G116*E116*D116","v":0},0,{"$f":"'curriculum analysis (optional)'!J34","v":0},0,0,{"$f":"L116*J116*I116","v":0},0,{"$f":"'curriculum analysis (optional)'!O34","v":0},0,0,{"$f":"Q116*O116*N116","v":0},0,{"$f":"'curriculum analysis (optional)'!T34","v":0},0,0,{"$f":"V116*T116*S116","v":0},0,{"$f":"'curriculum analysis (optional)'!Y34","v":0},0,0,{"$f":"AA116*Y116*X116","v":0},{"$f":"'curriculum analysis (optional)'!AC34","v":0},{"$f":"'curriculum analysis (optional)'!AD34","v":0},0,0,{"$f":"AF116*AD116*AC116","v":0},{"$f":"'curriculum analysis (optional)'!AH34","v":0},{"$f":"'curriculum analysis (optional)'!AI34","v":0},0,0,{"$f":"AK116*AI116*AH116","v":0},{"$f":"F116+K116+P116+U116+Z116+AE116+AJ116","v":0},0]
[null,{"$f":"'curriculum analysis (optional)'!B35","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E35","v":0},0,0,{"$f":"G117*E117*D117","v":0},0,{"$f":"'curriculum analysis (optional)'!J35","v":0},0,0,{"$f":"L117*J117*I117","v":0},0,{"$f":"'curriculum analysis (optional)'!O35","v":0},0,0,{"$f":"Q117*O117*N117","v":0},0,{"$f":"'curriculum analysis (optional)'!T35","v":0},0,0,{"$f":"V117*T117*S117","v":0},0,{"$f":"'curriculum analysis (optional)'!Y35","v":0},0,0,{"$f":"AA117*Y117*X117","v":0},{"$f":"'curriculum analysis (optional)'!AC35","v":0},{"$f":"'curriculum analysis (optional)'!AD35","v":0},0,0,{"$f":"AF117*AD117*AC117","v":0},{"$f":"'curriculum analysis (optional)'!AH35","v":0},{"$f":"'curriculum analysis (optional)'!AI35","v":0},0,0,{"$f":"AK117*AI117*AH117","v":0},{"$f":"F117+K117+P117+U117+Z117+AE117+AJ117","v":0},0]
[null,{"$f":"'curriculum analysis (optional)'!B36","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E36","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J36","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O36","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T36","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y36","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC36","v":0},{"$f":"'curriculum analysis (optional)'!AD36","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH36","v":0},{"$f":"'curriculum analysis (optional)'!AI36","v":0},0,0,0,0,0]
[null,{"$f":"'curriculum analysis (optional)'!B37","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E37","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J37","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O37","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T37","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y37","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC37","v":0},{"$f":"'curriculum analysis (optional)'!AD37","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH37","v":0},{"$f":"'curriculum analysis (optional)'!AI37","v":0},0,0,0,0,0]
["practical learning spaces",null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,{"$f":"P120+U120+Z120+AE120+AJ120","v":0},0]
["science ",null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
[null,{"$f":"'curriculum analysis (optional)'!B40","v":"Science"},null,0,{"$f":"'curriculum analysis (optional)'!E40","v":0},{"$f":"IF(D122>0,IF(E122>0,D122*E122,\"check\"),IF(E122>0,\"check\",0))","v":0},{"$f":"IF(F122>0,IF((F$86/D122)<32,F$86/D122,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!J40","v":0},{"$f":"IF(I122>0,IF(J122>0,I122*J122,\"check\"),IF(J122>0,\"check\",0))","v":0},{"$f":"IF(K122>0,IF((K$86/I122)<32,K$86/I122,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!O40","v":0},{"$f":"IF(N122>0,IF(O122>0,N122*O122,\"check\"),IF(O122>0,\"check\",0))","v":0},{"$f":"IF(P122>0,IF((P$86/N122)<32,P$86/N122,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!T40","v":0},{"$f":"IF(S122>0,IF(T122>0,S122*T122,\"check\"),IF(T122>0,\"check\",0))","v":0},{"$f":"IF(U122>0,IF((U$86/S122)<32,U$86/S122,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!Y40","v":0},{"$f":"IF(X122>0,IF(Y122>0,X122*Y122,\"check\"),IF(Y122>0,\"check\",0))","v":0},{"$f":"IF(Z122>0,IF((Z$86/X122)<32,Z$86/X122,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AC40","v":0},{"$f":"'curriculum analysis (optional)'!AD40","v":0},{"$f":"IF(AC122>0,IF(AD122>0,AC122*AD122,\"check\"),IF(AD122>0,\"check\",0))","v":0},{"$f":"IF(AE122>0,IF((AE$86/AC122)<32,AE$86/AC122,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AH40","v":0},{"$f":"'curriculum analysis (optional)'!AI40","v":0},{"$f":"IF(AH122>0,IF(AI122>0,AH122*AI122,\"check\"),IF(AI122>0,\"check\",0))","v":0},{"$f":"IF(AJ122>0,IF((AJ$86/AH122)<32,AJ$86/AH122,\"tba\"),0)","v":0},0,{"$f":"F122+K122+P122+U122+Z122+AE122+AJ122","v":0},{"$f":"AM122/AO$84","v":0},{"$f":"ROUNDUP(SUM(AN122:AN127)/0.95,0)","v":0},{"$f":"IF(AO122>0,SUM(AN122:AN127)/AO122,0)","v":0},30,{"$f":"AO122*AQ122","v":0},null,{"$f":"IF(AS122>0,SUM(AN122:AN127)/AS122,0)","v":0}]
[null,{"$f":"'curriculum analysis (optional)'!B41","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E41","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J41","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O41","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T41","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y41","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC41","v":0},{"$f":"'curriculum analysis (optional)'!AD41","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH41","v":0},{"$f":"'curriculum analysis (optional)'!AI41","v":0},0,0,0,0,0]
[null,{"$f":"'curriculum analysis (optional)'!B42","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E42","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J42","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O42","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T42","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y42","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC42","v":0},{"$f":"'curriculum analysis (optional)'!AD42","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH42","v":0},{"$f":"'curriculum analysis (optional)'!AI42","v":0},0,0,0,0,0]
[null,{"$f":"'curriculum analysis (optional)'!B43","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E43","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J43","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O43","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T43","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y43","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC43","v":0},{"$f":"'curriculum analysis (optional)'!AD43","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH43","v":0},{"$f":"'curriculum analysis (optional)'!AI43","v":0},0,0,0,0,0]
[null,{"$f":"'curriculum analysis (optional)'!B44","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E44","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J44","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O44","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T44","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y44","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC44","v":0},{"$f":"'curriculum analysis (optional)'!AD44","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH44","v":0},{"$f":"'curriculum analysis (optional)'!AI44","v":0},0,0,0,0,0]
[null,{"$f":"'curriculum analysis (optional)'!B45","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E45","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J45","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O45","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T45","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y45","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC45","v":0},{"$f":"'curriculum analysis (optional)'!AD45","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH45","v":0},{"$f":"'curriculum analysis (optional)'!AI45","v":0},0,0,0,0,0]
["art",null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
[null,{"$f":"'curriculum analysis (optional)'!B47","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E47","v":0},{"$f":"IF(D129>0,IF(E129>0,D129*E129,\"check\"),IF(E129>0,\"check\",0))","v":0},{"$f":"IF(F129>0,IF((F$86/D129)<32,F$86/D129,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!J47","v":0},{"$f":"IF(I129>0,IF(J129>0,I129*J129,\"check\"),IF(J129>0,\"check\",0))","v":0},{"$f":"IF(K129>0,IF((K$86/I129)<32,K$86/I129,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!O47","v":0},{"$f":"IF(N129>0,IF(O129>0,N129*O129,\"check\"),IF(O129>0,\"check\",0))","v":0},{"$f":"IF(P129>0,IF((P$86/N129)<32,P$86/N129,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!T47","v":0},{"$f":"IF(S129>0,IF(T129>0,S129*T129,\"check\"),IF(T129>0,\"check\",0))","v":0},{"$f":"IF(U129>0,IF((U$86/S129)<32,U$86/S129,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!Y47","v":0},{"$f":"IF(X129>0,IF(Y129>0,X129*Y129,\"check\"),IF(Y129>0,\"check\",0))","v":0},{"$f":"IF(Z129>0,IF((Z$86/X129)<32,Z$86/X129,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AC47","v":0},{"$f":"'curriculum analysis (optional)'!AD47","v":0},{"$f":"IF(AC129>0,IF(AD129>0,AC129*AD129,\"check\"),IF(AD129>0,\"check\",0))","v":0},{"$f":"IF(AE129>0,IF((AE$86/AC129)<32,AE$86/AC129,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AH47","v":0},{"$f":"'curriculum analysis (optional)'!AI47","v":0},{"$f":"IF(AH129>0,IF(AI129>0,AH129*AI129,\"check\"),IF(AI129>0,\"check\",0))","v":0},{"$f":"IF(AJ129>0,IF((AJ$86/AH129)<32,AJ$86/AH129,\"tba\"),0)","v":0},0,0,{"$f":"AM129/AO$84","v":0},{"$f":"ROUNDUP(SUM(AN129:AN134)/0.95,0)","v":0},{"$f":"IF(AO129>0,SUM(AN129:AN134)/AO129,0)","v":0},30,{"$f":"AO129*AQ129","v":0},null,{"$f":"IF(AS129>0,SUM(AN129:AN134)/AS129,0)","v":0}]
[null,{"$f":"'curriculum analysis (optional)'!B48","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E48","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J48","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O48","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T48","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y48","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC48","v":0},{"$f":"'curriculum analysis (optional)'!AD48","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH48","v":0},{"$f":"'curriculum analysis (optional)'!AI48","v":0},0,0,0,0,0]
[null,{"$f":"'curriculum analysis (optional)'!B49","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E49","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J49","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O49","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T49","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y49","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC49","v":0},{"$f":"'curriculum analysis (optional)'!AD49","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH49","v":0},{"$f":"'curriculum analysis (optional)'!AI49","v":0},0,0,0,0,0]
[null,{"$f":"'curriculum analysis (optional)'!B50","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E50","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J50","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O50","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T50","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y50","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC50","v":0},{"$f":"'curriculum analysis (optional)'!AD50","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH50","v":0},{"$f":"'curriculum analysis (optional)'!AI50","v":0},0,0,0,0,0]
[null,{"$f":"'curriculum analysis (optional)'!B51","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E51","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J51","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O51","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T51","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y51","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC51","v":0},{"$f":"'curriculum analysis (optional)'!AD51","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH51","v":0},{"$f":"'curriculum analysis (optional)'!AI51","v":0},0,0,0,0,0]
[null,{"$f":"'curriculum analysis (optional)'!B52","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E52","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J52","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O52","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T52","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y52","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC52","v":0},{"$f":"'curriculum analysis (optional)'!AD52","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH52","v":0},{"$f":"'curriculum analysis (optional)'!AI52","v":0},0,0,0,0,0]
["music and drama",null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
[null,{"$f":"'curriculum analysis (optional)'!B54","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E54","v":0},{"$f":"IF(D136>0,IF(E136>0,D136*E136,\"check\"),IF(E136>0,\"check\",0))","v":0},{"$f":"IF(F136>0,IF((F$86/D136)<32,F$86/D136,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!J54","v":0},{"$f":"IF(I136>0,IF(J136>0,I136*J136,\"check\"),IF(J136>0,\"check\",0))","v":0},{"$f":"IF(K136>0,IF((K$86/I136)<32,K$86/I136,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!O54","v":0},{"$f":"IF(N136>0,IF(O136>0,N136*O136,\"check\"),IF(O136>0,\"check\",0))","v":0},{"$f":"IF(P136>0,IF((P$86/N136)<32,P$86/N136,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!T54","v":0},{"$f":"IF(S136>0,IF(T136>0,S136*T136,\"check\"),IF(T136>0,\"check\",0))","v":0},{"$f":"IF(U136>0,IF((U$86/S136)<32,U$86/S136,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!Y54","v":0},{"$f":"IF(X136>0,IF(Y136>0,X136*Y136,\"check\"),IF(Y136>0,\"check\",0))","v":0},{"$f":"IF(Z136>0,IF((Z$86/X136)<32,Z$86/X136,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AC54","v":0},{"$f":"'curriculum analysis (optional)'!AD54","v":0},{"$f":"IF(AC136>0,IF(AD136>0,AC136*AD136,\"check\"),IF(AD136>0,\"check\",0))","v":0},{"$f":"IF(AE136>0,IF((AE$86/AC136)<32,AE$86/AC136,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AH54","v":0},{"$f":"'curriculum analysis (optional)'!AI54","v":0},{"$f":"IF(AH136>0,IF(AI136>0,AH136*AI136,\"check\"),IF(AI136>0,\"check\",0))","v":0},{"$f":"IF(AJ136>0,IF((AJ$86/AH136)<32,AJ$86/AH136,\"tba\"),0)","v":0},0,{"$f":"F136+K136+P136+U136+Z136+AE136+AJ136","v":0},{"$f":"AM136/AO$84","v":0},{"$f":"ROUNDUP(SUM(AN136:AN139)/0.95,0)","v":0},{"$f":"IF(AO136>0,SUM(AN136:AN139)/AO136,0)","v":0},24,{"$f":"AO136*AQ136","v":0},null,{"$f":"IF(AS136>0,SUM(AN136:AN139)/AS136,0)","v":0}]
[null,{"$f":"'curriculum analysis (optional)'!B55","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E55","v":0},{"$f":"IF(D137>0,IF(E137>0,D137*E137,\"check\"),IF(E137>0,\"check\",0))","v":0},{"$f":"IF(F137>0,IF((F$86/D137)<32,F$86/D137,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!J55","v":0},{"$f":"IF(I137>0,IF(J137>0,I137*J137,\"check\"),IF(J137>0,\"check\",0))","v":0},{"$f":"IF(K137>0,IF((K$86/I137)<32,K$86/I137,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!O55","v":0},{"$f":"IF(N137>0,IF(O137>0,N137*O137,\"check\"),IF(O137>0,\"check\",0))","v":0},{"$f":"IF(P137>0,IF((P$86/N137)<32,P$86/N137,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!T55","v":0},{"$f":"IF(S137>0,IF(T137>0,S137*T137,\"check\"),IF(T137>0,\"check\",0))","v":0},{"$f":"IF(U137>0,IF((U$86/S137)<32,U$86/S137,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!Y55","v":0},{"$f":"IF(X137>0,IF(Y137>0,X137*Y137,\"check\"),IF(Y137>0,\"check\",0))","v":0},{"$f":"IF(Z137>0,IF((Z$86/X137)<32,Z$86/X137,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AC55","v":0},{"$f":"'curriculum analysis (optional)'!AD55","v":0},{"$f":"IF(AC137>0,IF(AD137>0,AC137*AD137,\"check\"),IF(AD137>0,\"check\",0))","v":0},{"$f":"IF(AE137>0,IF((AE$86/AC137)<32,AE$86/AC137,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AH55","v":0},{"$f":"'curriculum analysis (optional)'!AI55","v":0},{"$f":"IF(AH137>0,IF(AI137>0,AH137*AI137,\"check\"),IF(AI137>0,\"check\",0))","v":0},{"$f":"IF(AJ137>0,IF((AJ$86/AH137)<32,AJ$86/AH137,\"tba\"),0)","v":0},0,{"$f":"F137+K137+P137+U137+Z137+AE137+AJ137","v":0},{"$f":"AM137/AO$84","v":0}]
[null,{"$f":"'curriculum analysis (optional)'!B56","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E56","v":0},{"$f":"IF(D138>0,IF(E138>0,D138*E138,\"check\"),IF(E138>0,\"check\",0))","v":0},{"$f":"IF(F138>0,IF((F$86/D138)<32,F$86/D138,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!J56","v":0},{"$f":"IF(I138>0,IF(J138>0,I138*J138,\"check\"),IF(J138>0,\"check\",0))","v":0},{"$f":"IF(K138>0,IF((K$86/I138)<32,K$86/I138,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!O56","v":0},{"$f":"IF(N138>0,IF(O138>0,N138*O138,\"check\"),IF(O138>0,\"check\",0))","v":0},{"$f":"IF(P138>0,IF((P$86/N138)<32,P$86/N138,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!T56","v":0},{"$f":"IF(S138>0,IF(T138>0,S138*T138,\"check\"),IF(T138>0,\"check\",0))","v":0},{"$f":"IF(U138>0,IF((U$86/S138)<32,U$86/S138,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!Y56","v":0},{"$f":"IF(X138>0,IF(Y138>0,X138*Y138,\"check\"),IF(Y138>0,\"check\",0))","v":0},{"$f":"IF(Z138>0,IF((Z$86/X138)<32,Z$86/X138,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AC56","v":0},{"$f":"'curriculum analysis (optional)'!AD56","v":0},{"$f":"IF(AC138>0,IF(AD138>0,AC138*AD138,\"check\"),IF(AD138>0,\"check\",0))","v":0},{"$f":"IF(AE138>0,IF((AE$86/AC138)<32,AE$86/AC138,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AH56","v":0},{"$f":"'curriculum analysis (optional)'!AI56","v":0},{"$f":"IF(AH138>0,IF(AI138>0,AH138*AI138,\"check\"),IF(AI138>0,\"check\",0))","v":0},{"$f":"IF(AJ138>0,IF((AJ$86/AH138)<32,AJ$86/AH138,\"tba\"),0)","v":0},0,{"$f":"F138+K138+P138+U138+Z138+AE138+AJ138","v":0},{"$f":"AM138/AO$84","v":0}]
[null,{"$f":"'curriculum analysis (optional)'!B57","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E57","v":0},{"$f":"IF(D139>0,IF(E139>0,D139*E139,\"check\"),IF(E139>0,\"check\",0))","v":0},{"$f":"IF(F139>0,IF((F$86/D139)<32,F$86/D139,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!J57","v":0},{"$f":"IF(I139>0,IF(J139>0,I139*J139,\"check\"),IF(J139>0,\"check\",0))","v":0},{"$f":"IF(K139>0,IF((K$86/I139)<32,K$86/I139,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!O57","v":0},{"$f":"IF(N139>0,IF(O139>0,N139*O139,\"check\"),IF(O139>0,\"check\",0))","v":0},{"$f":"IF(P139>0,IF((P$86/N139)<32,P$86/N139,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!T57","v":0},{"$f":"IF(S139>0,IF(T139>0,S139*T139,\"check\"),IF(T139>0,\"check\",0))","v":0},{"$f":"IF(U139>0,IF((U$86/S139)<32,U$86/S139,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!Y57","v":0},{"$f":"IF(X139>0,IF(Y139>0,X139*Y139,\"check\"),IF(Y139>0,\"check\",0))","v":0},{"$f":"IF(Z139>0,IF((Z$86/X139)<32,Z$86/X139,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AC57","v":0},{"$f":"'curriculum analysis (optional)'!AD57","v":0},{"$f":"IF(AC139>0,IF(AD139>0,AC139*AD139,\"check\"),IF(AD139>0,\"check\",0))","v":0},{"$f":"IF(AE139>0,IF((AE$86/AC139)<32,AE$86/AC139,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AH57","v":0},{"$f":"'curriculum analysis (optional)'!AI57","v":0},{"$f":"IF(AH139>0,IF(AI139>0,AH139*AI139,\"check\"),IF(AI139>0,\"check\",0))","v":0},{"$f":"IF(AJ139>0,IF((AJ$86/AH139)<32,AJ$86/AH139,\"tba\"),0)","v":0},0,{"$f":"F139+K139+P139+U139+Z139+AE139+AJ139","v":0},{"$f":"AM139/AO$84","v":0}]
["design and technology",null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
[null,{"$f":"'curriculum analysis (optional)'!B59","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E59","v":0},{"$f":"IF(D141>0,IF(E141>0,D141*E141,\"check\"),IF(E141>0,\"check\",0))","v":0},{"$f":"IF(F141>0,IF((F$86/D141)<32,F$86/D141,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!J59","v":0},{"$f":"IF(I141>0,IF(J141>0,I141*J141,\"check\"),IF(J141>0,\"check\",0))","v":0},{"$f":"IF(K141>0,IF((K$86/I141)<32,K$86/I141,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!O59","v":0},{"$f":"IF(N141>0,IF(O141>0,N141*O141,\"check\"),IF(O141>0,\"check\",0))","v":0},{"$f":"IF(P141>0,IF((P$86/N141)<32,P$86/N141,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!T59","v":0},{"$f":"IF(S141>0,IF(T141>0,S141*T141,\"check\"),IF(T141>0,\"check\",0))","v":0},{"$f":"IF(U141>0,IF((U$86/S141)<32,U$86/S141,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!Y59","v":0},{"$f":"IF(X141>0,IF(Y141>0,X141*Y141,\"check\"),IF(Y141>0,\"check\",0))","v":0},{"$f":"IF(Z141>0,IF((Z$86/X141)<32,Z$86/X141,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AC59","v":0},{"$f":"'curriculum analysis (optional)'!AD59","v":0},{"$f":"IF(AC141>0,IF(AD141>0,AC141*AD141,\"check\"),IF(AD141>0,\"check\",0))","v":0},{"$f":"IF(AE141>0,IF((AE$86/AC141)<32,AE$86/AC141,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AH59","v":0},{"$f":"'curriculum analysis (optional)'!AI59","v":0},{"$f":"IF(AH141>0,IF(AI141>0,AH141*AI141,\"check\"),IF(AI141>0,\"check\",0))","v":0},{"$f":"IF(AJ141>0,IF((AJ$86/AH141)<32,AJ$86/AH141,\"tba\"),0)","v":0},0,{"$f":"F141+K141+P141+U141+Z141+AE141+AJ141","v":0},{"$f":"AM141/AO$84","v":0},{"$f":"ROUND(SUM(AN141:AN148)/0.9,0)","v":0},{"$f":"IF(AO141>0,SUM(AN141:AN148)/AO141,0)","v":0},24,{"$f":"AO141*AQ141","v":0},null,{"$f":"IF(AS141>0,SUM(AN141:AN148)/AS141,0)","v":0}]
[null,{"$f":"'curriculum analysis (optional)'!B60","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E60","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J60","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O60","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T60","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y60","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC60","v":0},{"$f":"'curriculum analysis (optional)'!AD60","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH60","v":0},{"$f":"'curriculum analysis (optional)'!AI60","v":0},0,0,0,0,{"$f":"AM142/AO$84","v":0}]
[null,{"$f":"'curriculum analysis (optional)'!B61","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E61","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J61","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O61","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T61","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y61","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC61","v":0},{"$f":"'curriculum analysis (optional)'!AD61","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH61","v":0},{"$f":"'curriculum analysis (optional)'!AI61","v":0},0,0,0,{"$f":"F143+K143+P143+U143+Z143+AE143+AJ143","v":0},0]
[null,{"$f":"'curriculum analysis (optional)'!B62","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E62","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J62","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O62","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T62","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y62","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC62","v":0},{"$f":"'curriculum analysis (optional)'!AD62","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH62","v":0},{"$f":"'curriculum analysis (optional)'!AI62","v":0},0,0,0,{"$f":"F144+K144+P144+U144+Z144+AE144+AJ144","v":0},0]
[null,{"$f":"'curriculum analysis (optional)'!B63","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E63","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J63","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O63","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T63","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y63","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC63","v":0},{"$f":"'curriculum analysis (optional)'!AD63","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH63","v":0},{"$f":"'curriculum analysis (optional)'!AI63","v":0},0,0,0,{"$f":"F145+K145+P145+U145+Z145+AE145+AJ145","v":0},0]
[null,{"$f":"'curriculum analysis (optional)'!B64","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E64","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J64","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O64","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T64","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y64","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC64","v":0},{"$f":"'curriculum analysis (optional)'!AD64","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH64","v":0},{"$f":"'curriculum analysis (optional)'!AI64","v":0},0,0,0,{"$f":"F146+K146+P146+U146+Z146+AE146+AJ146","v":0},0]
[null,{"$f":"'curriculum analysis (optional)'!B65","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E65","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J65","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O65","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T65","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y65","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC65","v":0},{"$f":"'curriculum analysis (optional)'!AD65","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH65","v":0},{"$f":"'curriculum analysis (optional)'!AI65","v":0},0,0,0,0,0]
[null,{"$f":"'curriculum analysis (optional)'!B66","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E66","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!J66","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!O66","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!T66","v":0},0,0,0,0,{"$f":"'curriculum analysis (optional)'!Y66","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AC66","v":0},{"$f":"'curriculum analysis (optional)'!AD66","v":0},0,0,0,{"$f":"'curriculum analysis (optional)'!AH66","v":0},{"$f":"'curriculum analysis (optional)'!AI66","v":0},0,0,0,0,0]
["PE (internal and external)",null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
[null,{"$f":"'curriculum analysis (optional)'!B68","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E68","v":0},{"$f":"IF(D150>0,IF(E150>0,D150*E150,\"check\"),IF(E150>0,\"check\",0))","v":0},{"$f":"IF(F150>0,IF((F$86/D150)<32,F$86/D150,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!J68","v":0},{"$f":"IF(I150>0,IF(J150>0,I150*J150,\"check\"),IF(J150>0,\"check\",0))","v":0},{"$f":"IF(K150>0,IF((K$86/I150)<32,K$86/I150,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!O68","v":0},{"$f":"IF(N150>0,IF(O150>0,N150*O150,\"check\"),IF(O150>0,\"check\",0))","v":0},{"$f":"IF(P150>0,IF((P$86/N150)<32,P$86/N150,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!T68","v":0},{"$f":"IF(S150>0,IF(T150>0,S150*T150,\"check\"),IF(T150>0,\"check\",0))","v":0},{"$f":"IF(U150>0,IF((U$86/S150)<32,U$86/S150,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!Y68","v":0},{"$f":"IF(X150>0,IF(Y150>0,X150*Y150,\"check\"),IF(Y150>0,\"check\",0))","v":0},{"$f":"IF(Z150>0,IF((Z$86/X150)<32,Z$86/X150,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AC68","v":0},{"$f":"'curriculum analysis (optional)'!AD68","v":0},{"$f":"IF(AC150>0,IF(AD150>0,AC150*AD150,\"check\"),IF(AD150>0,\"check\",0))","v":0},{"$f":"IF(AE150>0,IF((AE$86/AC150)<32,AE$86/AC150,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AH68","v":0},{"$f":"'curriculum analysis (optional)'!AI68","v":0},{"$f":"IF(AH150>0,IF(AI150>0,AH150*AI150,\"check\"),IF(AI150>0,\"check\",0))","v":0},{"$f":"IF(AJ150>0,IF((AJ$86/AH150)<32,AJ$86/AH150,\"tba\"),0)","v":0},0,{"$f":"F150+K150+P150+U150+Z150+AE150+AJ150","v":0},{"$f":"AM150/AO$84","v":0},{"$f":"ROUNDUP(SUM(AN150:AN153),0)","v":0},{"$f":"IF(AO150>0,SUM(AN150:AN153)/AO150,0)","v":0},30,{"$f":"AO150*AQ150","v":0},null,{"$f":"IF(AS150>0,SUM(AN150:AN153)/AS150,0)","v":0}]
[null,{"$f":"'curriculum analysis (optional)'!B69","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E69","v":0},{"$f":"IF(D151>0,IF(E151>0,D151*E151,\"check\"),IF(E151>0,\"check\",0))","v":0},{"$f":"IF(F151>0,IF((F$86/D151)<32,F$86/D151,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!J69","v":0},{"$f":"IF(I151>0,IF(J151>0,I151*J151,\"check\"),IF(J151>0,\"check\",0))","v":0},{"$f":"IF(K151>0,IF((K$86/I151)<32,K$86/I151,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!O69","v":0},{"$f":"IF(N151>0,IF(O151>0,N151*O151,\"check\"),IF(O151>0,\"check\",0))","v":0},{"$f":"IF(P151>0,IF((P$86/N151)<32,P$86/N151,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!T69","v":0},{"$f":"IF(S151>0,IF(T151>0,S151*T151,\"check\"),IF(T151>0,\"check\",0))","v":0},{"$f":"IF(U151>0,IF((U$86/S151)<32,U$86/S151,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!Y69","v":0},{"$f":"IF(X151>0,IF(Y151>0,X151*Y151,\"check\"),IF(Y151>0,\"check\",0))","v":0},{"$f":"IF(Z151>0,IF((Z$86/X151)<32,Z$86/X151,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AC69","v":0},{"$f":"'curriculum analysis (optional)'!AD69","v":0},{"$f":"IF(AC151>0,IF(AD151>0,AC151*AD151,\"check\"),IF(AD151>0,\"check\",0))","v":0},{"$f":"IF(AE151>0,IF((AE$86/AC151)<32,AE$86/AC151,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AH69","v":0},{"$f":"'curriculum analysis (optional)'!AI69","v":0},{"$f":"IF(AH151>0,IF(AI151>0,AH151*AI151,\"check\"),IF(AI151>0,\"check\",0))","v":0},{"$f":"IF(AJ151>0,IF((AJ$86/AH151)<32,AJ$86/AH151,\"tba\"),0)","v":0},0,{"$f":"F151+K151+P151+U151+Z151+AE151+AJ151","v":0},{"$f":"AM151/AO$84","v":0}]
[null,{"$f":"'curriculum analysis (optional)'!B70","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E70","v":0},{"$f":"IF(D152>0,IF(E152>0,D152*E152,\"check\"),IF(E152>0,\"check\",0))","v":0},{"$f":"IF(F152>0,IF((F$86/D152)<32,F$86/D152,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!J70","v":0},{"$f":"IF(I152>0,IF(J152>0,I152*J152,\"check\"),IF(J152>0,\"check\",0))","v":0},{"$f":"IF(K152>0,IF((K$86/I152)<32,K$86/I152,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!O70","v":0},{"$f":"IF(N152>0,IF(O152>0,N152*O152,\"check\"),IF(O152>0,\"check\",0))","v":0},{"$f":"IF(P152>0,IF((P$86/N152)<32,P$86/N152,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!T70","v":0},{"$f":"IF(S152>0,IF(T152>0,S152*T152,\"check\"),IF(T152>0,\"check\",0))","v":0},{"$f":"IF(U152>0,IF((U$86/S152)<32,U$86/S152,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!Y70","v":0},{"$f":"IF(X152>0,IF(Y152>0,X152*Y152,\"check\"),IF(Y152>0,\"check\",0))","v":0},{"$f":"IF(Z152>0,IF((Z$86/X152)<32,Z$86/X152,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AC70","v":0},{"$f":"'curriculum analysis (optional)'!AD70","v":0},{"$f":"IF(AC152>0,IF(AD152>0,AC152*AD152,\"check\"),IF(AD152>0,\"check\",0))","v":0},{"$f":"IF(AE152>0,IF((AE$86/AC152)<32,AE$86/AC152,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AH70","v":0},{"$f":"'curriculum analysis (optional)'!AI70","v":0},{"$f":"IF(AH152>0,IF(AI152>0,AH152*AI152,\"check\"),IF(AI152>0,\"check\",0))","v":0},{"$f":"IF(AJ152>0,IF((AJ$86/AH152)<32,AJ$86/AH152,\"tba\"),0)","v":0},0,{"$f":"F152+K152+P152+U152+Z152+AE152+AJ152","v":0},{"$f":"AM152/AO$84","v":0}]
[null,{"$f":"'curriculum analysis (optional)'!B71","v":0},null,0,{"$f":"'curriculum analysis (optional)'!E71","v":0},{"$f":"IF(D153>0,IF(E153>0,D153*E153,\"check\"),IF(E153>0,\"check\",0))","v":0},{"$f":"IF(F153>0,IF((F$86/D153)<32,F$86/D153,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!J71","v":0},{"$f":"IF(I153>0,IF(J153>0,I153*J153,\"check\"),IF(J153>0,\"check\",0))","v":0},{"$f":"IF(K153>0,IF((K$86/I153)<32,K$86/I153,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!O71","v":0},{"$f":"IF(N153>0,IF(O153>0,N153*O153,\"check\"),IF(O153>0,\"check\",0))","v":0},{"$f":"IF(P153>0,IF((P$86/N153)<32,P$86/N153,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!T71","v":0},{"$f":"IF(S153>0,IF(T153>0,S153*T153,\"check\"),IF(T153>0,\"check\",0))","v":0},{"$f":"IF(U153>0,IF((U$86/S153)<32,U$86/S153,\"tba\"),0)","v":0},0,0,{"$f":"'curriculum analysis (optional)'!Y71","v":0},{"$f":"IF(X153>0,IF(Y153>0,X153*Y153,\"check\"),IF(Y153>0,\"check\",0))","v":0},{"$f":"IF(Z153>0,IF((Z$86/X153)<32,Z$86/X153,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AC71","v":0},{"$f":"'curriculum analysis (optional)'!AD71","v":0},{"$f":"IF(AC153>0,IF(AD153>0,AC153*AD153,\"check\"),IF(AD153>0,\"check\",0))","v":0},{"$f":"IF(AE153>0,IF((AE$86/AC153)<32,AE$86/AC153,\"tba\"),0)","v":0},0,{"$f":"'curriculum analysis (optional)'!AH71","v":0},{"$f":"'curriculum analysis (optional)'!AI71","v":0},{"$f":"IF(AH153>0,IF(AI153>0,AH153*AI153,\"check\"),IF(AI153>0,\"check\",0))","v":0},{"$f":"IF(AJ153>0,IF((AJ$86/AH153)<32,AJ$86/AH153,\"tba\"),0)","v":0},0,{"$f":"F153+K153+P153+U153+Z153+AE153+AJ153","v":0},{"$f":"AM153/AO$84","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AM91:AM153)","v":0},{"$f":"SUM(AN110:AN153)","v":0}]
["totals/ check",null,null,null,{"$f":"SUM(E91:E154)","v":0},{"$f":"SUM(F91:F154)","v":0},null,null,null,{"$f":"SUM(J91:J154)","v":0},{"$f":"SUM(K91:K154)","v":0},null,null,null,{"$f":"SUM(O91:O154)","v":0},{"$f":"SUM(P91:P154)","v":0},null,null,null,{"$f":"SUM(T91:T154)","v":0},{"$f":"SUM(U91:U154)","v":0},null,null,null,{"$f":"SUM(Y91:Y154)","v":0},{"$f":"SUM(Z91:Z154)","v":0},null,null,null,{"$f":"SUM(AD91:AD154)","v":0},{"$f":"SUM(AE91:AE154)","v":0},null,null,null,{"$f":"SUM(AI91:AI154)","v":0},{"$f":"SUM(AJ91:AJ154)","v":0},null,null,{"$f":"F155+K155+P155+U155+Z155+AE155+AJ155","v":0},{"$f":"AM155/AO$84","v":0},{"$f":"AO110+AO114+AO122+AO129+AO136+AO141+AO143+AO150","v":0},null,null,{"$f":"SUM(AR110:AR150)","v":0},{"$f":"SUM(AS110:AS150)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AR155/AO155","v":{"$error":"#DIV/0!"}},"workplaces per room"]
["Target",null,null,null,null,null,{"$f":"F86*AO84","v":9000},null,null,null,null,{"$f":"K86*AO84","v":9000},null,null,null,null,{"$f":"P86*AO84","v":9000},null,null,null,null,{"$f":"U86*AO84","v":9000},null,null,null,null,{"$f":"Z86*AO84","v":9000},null,null,null,null,{"$f":"AE86*AO84","v":5625},null,null,null,null,{"$f":"AJ86*AO84","v":5625},null,null,null,"overall frequency of use",{"$f":"AN155/AO155","v":{"$error":"#DIV/0!"}}]
["Actual",null,null,null,null,null,{"$f":"SUM(H91:H153)","v":0},null,null,null,null,{"$f":"SUM(M91:M153)","v":0},null,null,null,null,{"$f":"SUM(R91:R153)","v":0},null,null,null,null,{"$f":"SUM(W91:W153)","v":0},null,null,null,null,{"$f":"SUM(AB91:AB153)","v":0},null,null,null,null,{"$f":"SUM(AG91:AG153)","v":0},null,null,null,null,{"$f":"SUM(AL91:AL153)","v":0},null,null,null,null,{"$f":"IF(AP157>88%,\"frequency of use high\",IF(AP157<80%,\"frequency of use low\",\"OK\"))","v":{"$error":"#DIV/0!"}},null,null,"average group size",{"$f":"(AO86*AO84)/AM154","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"overall occupancy",{"$f":"AT158/AR156","v":{"$error":"#DIV/0!"}},null,null,"teachers @ 100% contact",{"$f":"AM155/AO84","v":0}]
["Difference",null,null,null,null,null,{"$f":"G158/G157","v":0},null,null,null,null,{"$f":"L158/L157","v":0},null,null,null,null,{"$f":"Q158/Q157","v":0},null,null,null,null,{"$f":"V158/V157","v":0},null,null,null,null,{"$f":"AA158/AA157","v":0},null,null,null,null,{"$f":"AF158/AF157","v":0},null,null,null,null,{"$f":"AK158/AK157","v":0},null,null,null,null,{"$f":"IF(AP159>90%,\"occupancy high\",IF(AP159<75%,\"occupancy low\",\"\"))","v":{"$error":"#DIV/0!"}},null,null,"teachers @ 75% contact",{"$f":"AT159/0.75","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"utilisation (incl outdoor PE)",{"$f":"AO86/AR155","v":{"$error":"#DIV/0!"}},null,null,"pupil: teacher ratio",{"$f":"AO86/AT160","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AP161>AT86,\"utilisation too high\",IF(AP161<AR86,\"utilisation too low\",\"\"))","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(G163:AK163)","v":0}]

{"sheet":"Existing Spaces","index":3,"n_rows":517,"n_cols":30,"rows_kept":517,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Key to Blocks",null,null,null,null,null,null,null,{"$f":"'Secondary SoA'!$S$2","v":"[Insert Project Code and Scheme Name here in title sheet]"}]
[]
[null,"Block \n","Block ref",null,null,null,"Spaces in \nAs New SOA","Existing Spaces",null,"No of Existing Spaces",null,"Net Area",null,"Non Net Area",null,"SoA Area\n(min)",null,"SoA Area\n(max)",null,"SOA Area"]
[null,"E.g. AA","S",null,null,null,{"$f":"SUM('Secondary SoA'!$U$19,'Secondary SoA'!$U$26,'Secondary SoA'!$U$31,'Secondary SoA'!$U$38,'Secondary SoA'!$U$43,'Secondary SoA'!$U$49,'Secondary SoA'!$U$58)","v":56},{"$f":"COUNTA($P$15:$P$517)","v":1},null,"Basic Teaching",null,{"$f":"SUMIF($P$15:$P$517,\"1\",$L$15:$L$517)","v":56},null,{"$f":"SUMIF($P$15:$P$517,\"1\",$N$15:$N$517)","v":0},null,{"$f":"'Secondary SoA'!$O$61","v":3330},null,{"$f":"'Secondary SoA'!$Q$61","v":3918},null,{"$f":"'Secondary SoA'!$V$61","v":3573}]
[null,null,null,null,null,null,{"$f":"SUM('Secondary SoA'!$U$64:$U$72)","v":5},{"$f":"COUNTA($Q$15:$Q$517)","v":0},null,"Large Spaces",null,{"$f":"SUMIF($Q$15:$Q$517,\"1\",$L$15:$L$517)","v":0},null,{"$f":"SUMIF($Q$15:$Q$517,\"1\",$N$15:$N$517)","v":0},null,{"$f":"'Secondary SoA'!$O$73","v":1050},null,{"$f":"'Secondary SoA'!$Q$73","v":1460},null,{"$f":"'Secondary SoA'!$V$73","v":1266}]
[null,null,null,null,null,null,{"$f":"SUM('Secondary SoA'!$U$76:$U$94)","v":15},{"$f":"COUNTA($R$15:$R$517)","v":0},null,"Learning Resource Area",null,{"$f":"SUMIF($R$15:$R$517,\"1\",$L$15:$L$517)","v":0},null,{"$f":"SUMIF($R$15:$R$517,\"1\",$N$15:$N$517)","v":0},null,{"$f":"'Secondary SoA'!$O$95","v":350},null,{"$f":"'Secondary SoA'!$Q$95","v":537.5},null,{"$f":"'Secondary SoA'!$V$95","v":353}]
[null,null,null,null,null,null,{"$f":"SUM('Secondary SoA'!$U$104:$U$129)","v":40},{"$f":"COUNTA($S$15:$S$517)","v":0},null,"Staff and Administration",null,{"$f":"SUMIF($S$15:$S$517,\"1\",$L$15:$L$517)","v":0},null,{"$f":"SUMIF($S$15:$S$517,\"1\",$N$15:$N$517)","v":0},null,{"$f":"'Secondary SoA'!$O$130","v":325},null,{"$f":"'Secondary SoA'!$Q$130","v":583},null,{"$f":"'Secondary SoA'!$V$130","v":473}]
[null,null,null,null,null,null,{"$f":"SUM('Secondary SoA'!$U$132:$U$164)","v":55},{"$f":"COUNTA($T$15:$T$517)","v":0},null,"Storage",null,{"$f":"SUMIF($T$15:$T$517,\"1\",$L$15:$L$517)","v":0},null,{"$f":"SUMIF($T$15:$T$517,\"1\",$N$15:$N$517)","v":0},null,{"$f":"'Secondary SoA'!$O$165","v":443},null,{"$f":"'Secondary SoA'!$Q$165","v":700},null,{"$f":"'Secondary SoA'!$V$165","v":510}]
[null,null,null,null,null,null,null,null,null,"Non Net",null,{"$f":"SUMIF($U$15:$U$517,\"1\",$L$15:$L$517)","v":0},null,{"$f":"SUMIF($U$15:$U$517,\"1\",$N$15:$N$517)","v":0},null,{"$f":"'Secondary SoA'!$O$211","v":2470},null,{"$f":"'Secondary SoA'!$Q$211","v":2778.75},null,{"$f":"'Secondary SoA'!$W$211","v":2470}]
[null,null,null,null,null,null,null,null,null,"Unassigned",null,{"$f":"SUMIF($AF:$AF,\"0\",$L:$L)+SUMIF($AF:$AF,\"0\",$N:$N)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"Totals - ",{"$f":"SUM(L5:L11)","v":56},null,{"$f":"SUM(N5:N11)","v":0},null,{"$f":"SUM(P5:Q11)","v":7968},null,{"$f":"SUM(R5:S11)","v":9977.25},null,{"$f":"SUM(T5:U11)","v":8645}]
[]
[null,null,null,null,"No. ",null,"Block","Room Number",null,"Room Name\n\n(based on the activities the room is designed or equipped to accommodate)\n",null,"Net Area (m2)\n",null,"Non Net Area (m2)\n",null,"Basic Teaching","Large Spaces","Learning Resource Area","Staff and Administration","Storage","Non Net",null,null,null,null,null,null,"Block ref:\nSelected (S)\nUntouched (U) To be demolished (X)"]
[null,null,null,null,{"$f":"IF(F15=\"\",\"\",MAX($E$1:$E14)+1)","v":1},{"$f":"IF(OR($AB15<>\"\",$U15<>\"\",$T15<>\"\",$S15<>\"\",$R15<>\"\",$Q15<>\"\",$P15<>\"\",$N15<>\"\",$L15<>\"\",$J15<>\"\",$H15<>\"\",$G15<>\"\"),\"Information Entered\",\"\")","v":"Information Entered"},"E.g. AA",101,null,"classroom",null,56,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,"S",null,{"$f":"IF($P15<>\"\",\"GT\",IF($Q15<>\"\",\"LARGE\",IF($R15<>\"\",\"SEN\",IF($S15<>\"\",\"ADMIN\",IF($T15<>\"\",\"ST\",IF($U15<>\"\",\"NET\",\"\"))))))","v":"GT"}]
[null,null,null,null,{"$f":"IF(F16=\"\",\"\",MAX($E$1:$E15)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($P16<>\"\",\"GT\",IF($Q16<>\"\",\"LARGE\",IF($R16<>\"\",\"SEN\",IF($S16<>\"\",\"ADMIN\",IF($T16<>\"\",\"ST\",IF($U16<>\"\",\"NET\",\"\"))))))","v":""}]
[null,null,null,null,{"$f":"IF(F17=\"\",\"\",MAX($E$1:$E16)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F18=\"\",\"\",MAX($E$1:$E17)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F19=\"\",\"\",MAX($E$1:$E18)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F20=\"\",\"\",MAX($E$1:$E19)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F21=\"\",\"\",MAX($E$1:$E20)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F22=\"\",\"\",MAX($E$1:$E21)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F23=\"\",\"\",MAX($E$1:$E22)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F24=\"\",\"\",MAX($E$1:$E23)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F25=\"\",\"\",MAX($E$1:$E24)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F26=\"\",\"\",MAX($E$1:$E25)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F27=\"\",\"\",MAX($E$1:$E26)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F28=\"\",\"\",MAX($E$1:$E27)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F29=\"\",\"\",MAX($E$1:$E28)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F30=\"\",\"\",MAX($E$1:$E29)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F31=\"\",\"\",MAX($E$1:$E30)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F32=\"\",\"\",MAX($E$1:$E31)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F33=\"\",\"\",MAX($E$1:$E32)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F34=\"\",\"\",MAX($E$1:$E33)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F35=\"\",\"\",MAX($E$1:$E34)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F36=\"\",\"\",MAX($E$1:$E35)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F37=\"\",\"\",MAX($E$1:$E36)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F38=\"\",\"\",MAX($E$1:$E37)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F39=\"\",\"\",MAX($E$1:$E38)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F40=\"\",\"\",MAX($E$1:$E39)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F41=\"\",\"\",MAX($E$1:$E40)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F42=\"\",\"\",MAX($E$1:$E41)+1)","v":""},{"$f":"IF(OR($AB42<>\"\",$U42<>\"\",$T42<>\"\",$S42<>\"\",$R42<>\"\",$Q42<>\"\",$P42<>\"\",$N42<>\"\",$L42<>\"\",$J43<>\"\",$H42<>\"\",$G42<>\"\"),\"Information Entered\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F43=\"\",\"\",MAX($E$1:$E42)+1)","v":""},{"$f":"IF(OR($AB43<>\"\",$U43<>\"\",$T43<>\"\",$S43<>\"\",$R43<>\"\",$Q43<>\"\",$P43<>\"\",$N43<>\"\",$L43<>\"\",$J43<>\"\",$H43<>\"\",$G43<>\"\"),\"Information Entered\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F44=\"\",\"\",MAX($E$1:$E43)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F45=\"\",\"\",MAX($E$1:$E44)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F46=\"\",\"\",MAX($E$1:$E45)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F47=\"\",\"\",MAX($E$1:$E46)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F48=\"\",\"\",MAX($E$1:$E47)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F49=\"\",\"\",MAX($E$1:$E48)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F50=\"\",\"\",MAX($E$1:$E49)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F51=\"\",\"\",MAX($E$1:$E50)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F52=\"\",\"\",MAX($E$1:$E51)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F53=\"\",\"\",MAX($E$1:$E52)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F54=\"\",\"\",MAX($E$1:$E53)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F55=\"\",\"\",MAX($E$1:$E54)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F56=\"\",\"\",MAX($E$1:$E55)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F57=\"\",\"\",MAX($E$1:$E56)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F58=\"\",\"\",MAX($E$1:$E57)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F59=\"\",\"\",MAX($E$1:$E58)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F60=\"\",\"\",MAX($E$1:$E59)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F61=\"\",\"\",MAX($E$1:$E60)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F62=\"\",\"\",MAX($E$1:$E61)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F63=\"\",\"\",MAX($E$1:$E62)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F64=\"\",\"\",MAX($E$1:$E63)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F65=\"\",\"\",MAX($E$1:$E64)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F66=\"\",\"\",MAX($E$1:$E65)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F67=\"\",\"\",MAX($E$1:$E66)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F68=\"\",\"\",MAX($E$1:$E67)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F69=\"\",\"\",MAX($E$1:$E68)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F70=\"\",\"\",MAX($E$1:$E69)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F71=\"\",\"\",MAX($E$1:$E70)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F72=\"\",\"\",MAX($E$1:$E71)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F73=\"\",\"\",MAX($E$1:$E72)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F74=\"\",\"\",MAX($E$1:$E73)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F75=\"\",\"\",MAX($E$1:$E74)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F76=\"\",\"\",MAX($E$1:$E75)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F77=\"\",\"\",MAX($E$1:$E76)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F78=\"\",\"\",MAX($E$1:$E77)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F79=\"\",\"\",MAX($E$1:$E78)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F80=\"\",\"\",MAX($E$1:$E79)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($P80<>\"\",\"GT\",IF($Q80<>\"\",\"LARGE\",IF($R80<>\"\",\"SEN\",IF($S80<>\"\",\"ADMIN\",IF($T80<>\"\",\"ST\",IF($U80<>\"\",\"NET\",\"\"))))))","v":""}]
[null,null,null,null,{"$f":"IF(F81=\"\",\"\",MAX($E$1:$E80)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F82=\"\",\"\",MAX($E$1:$E81)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F83=\"\",\"\",MAX($E$1:$E82)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F84=\"\",\"\",MAX($E$1:$E83)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F85=\"\",\"\",MAX($E$1:$E84)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F86=\"\",\"\",MAX($E$1:$E85)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F87=\"\",\"\",MAX($E$1:$E86)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F88=\"\",\"\",MAX($E$1:$E87)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F89=\"\",\"\",MAX($E$1:$E88)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F90=\"\",\"\",MAX($E$1:$E89)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F91=\"\",\"\",MAX($E$1:$E90)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F92=\"\",\"\",MAX($E$1:$E91)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F93=\"\",\"\",MAX($E$1:$E92)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F94=\"\",\"\",MAX($E$1:$E93)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F95=\"\",\"\",MAX($E$1:$E94)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F96=\"\",\"\",MAX($E$1:$E95)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F97=\"\",\"\",MAX($E$1:$E96)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F98=\"\",\"\",MAX($E$1:$E97)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F99=\"\",\"\",MAX($E$1:$E98)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F100=\"\",\"\",MAX($E$1:$E99)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F101=\"\",\"\",MAX($E$1:$E100)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F102=\"\",\"\",MAX($E$1:$E101)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F103=\"\",\"\",MAX($E$1:$E102)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F104=\"\",\"\",MAX($E$1:$E103)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F105=\"\",\"\",MAX($E$1:$E104)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F106=\"\",\"\",MAX($E$1:$E105)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F107=\"\",\"\",MAX($E$1:$E106)+1)","v":""},{"$f":"IF(OR($AB107<>\"\",$U107<>\"\",$T107<>\"\",$S107<>\"\",$R107<>\"\",$Q107<>\"\",$P107<>\"\",$N107<>\"\",$L107<>\"\",$J107<>\"\",$H107<>\"\",$G107<>\"\"),\"Information Entered\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F108=\"\",\"\",MAX($E$1:$E107)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F109=\"\",\"\",MAX($E$1:$E108)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F110=\"\",\"\",MAX($E$1:$E109)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F111=\"\",\"\",MAX($E$1:$E110)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F112=\"\",\"\",MAX($E$1:$E111)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F113=\"\",\"\",MAX($E$1:$E112)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F114=\"\",\"\",MAX($E$1:$E113)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F115=\"\",\"\",MAX($E$1:$E114)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F116=\"\",\"\",MAX($E$1:$E115)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F117=\"\",\"\",MAX($E$1:$E116)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F118=\"\",\"\",MAX($E$1:$E117)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F119=\"\",\"\",MAX($E$1:$E118)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F120=\"\",\"\",MAX($E$1:$E119)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F121=\"\",\"\",MAX($E$1:$E120)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F122=\"\",\"\",MAX($E$1:$E121)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F123=\"\",\"\",MAX($E$1:$E122)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F124=\"\",\"\",MAX($E$1:$E123)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F125=\"\",\"\",MAX($E$1:$E124)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F126=\"\",\"\",MAX($E$1:$E125)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F127=\"\",\"\",MAX($E$1:$E126)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F128=\"\",\"\",MAX($E$1:$E127)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F129=\"\",\"\",MAX($E$1:$E128)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F130=\"\",\"\",MAX($E$1:$E129)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F131=\"\",\"\",MAX($E$1:$E130)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F132=\"\",\"\",MAX($E$1:$E131)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F133=\"\",\"\",MAX($E$1:$E132)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F134=\"\",\"\",MAX($E$1:$E133)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F135=\"\",\"\",MAX($E$1:$E134)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F136=\"\",\"\",MAX($E$1:$E135)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F137=\"\",\"\",MAX($E$1:$E136)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F138=\"\",\"\",MAX($E$1:$E137)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F139=\"\",\"\",MAX($E$1:$E138)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F140=\"\",\"\",MAX($E$1:$E139)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F141=\"\",\"\",MAX($E$1:$E140)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F142=\"\",\"\",MAX($E$1:$E141)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F143=\"\",\"\",MAX($E$1:$E142)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F144=\"\",\"\",MAX($E$1:$E143)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($P144<>\"\",\"GT\",IF($Q144<>\"\",\"LARGE\",IF($R144<>\"\",\"SEN\",IF($S144<>\"\",\"ADMIN\",IF($T144<>\"\",\"ST\",IF($U144<>\"\",\"NET\",\"\"))))))","v":""}]
[null,null,null,null,{"$f":"IF(F145=\"\",\"\",MAX($E$1:$E144)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F146=\"\",\"\",MAX($E$1:$E145)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F147=\"\",\"\",MAX($E$1:$E146)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F148=\"\",\"\",MAX($E$1:$E147)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F149=\"\",\"\",MAX($E$1:$E148)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F150=\"\",\"\",MAX($E$1:$E149)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F151=\"\",\"\",MAX($E$1:$E150)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F152=\"\",\"\",MAX($E$1:$E151)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F153=\"\",\"\",MAX($E$1:$E152)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F154=\"\",\"\",MAX($E$1:$E153)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F155=\"\",\"\",MAX($E$1:$E154)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F156=\"\",\"\",MAX($E$1:$E155)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F157=\"\",\"\",MAX($E$1:$E156)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F158=\"\",\"\",MAX($E$1:$E157)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F159=\"\",\"\",MAX($E$1:$E158)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F160=\"\",\"\",MAX($E$1:$E159)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F161=\"\",\"\",MAX($E$1:$E160)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F162=\"\",\"\",MAX($E$1:$E161)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F163=\"\",\"\",MAX($E$1:$E162)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F164=\"\",\"\",MAX($E$1:$E163)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F165=\"\",\"\",MAX($E$1:$E164)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F166=\"\",\"\",MAX($E$1:$E165)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F167=\"\",\"\",MAX($E$1:$E166)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F168=\"\",\"\",MAX($E$1:$E167)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F169=\"\",\"\",MAX($E$1:$E168)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F170=\"\",\"\",MAX($E$1:$E169)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F171=\"\",\"\",MAX($E$1:$E170)+1)","v":""},{"$f":"IF(OR($AB171<>\"\",$U171<>\"\",$T171<>\"\",$S171<>\"\",$R171<>\"\",$Q171<>\"\",$P171<>\"\",$N171<>\"\",$L171<>\"\",$J171<>\"\",$H171<>\"\",$G171<>\"\"),\"Information Entered\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F172=\"\",\"\",MAX($E$1:$E171)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F173=\"\",\"\",MAX($E$1:$E172)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F174=\"\",\"\",MAX($E$1:$E173)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F175=\"\",\"\",MAX($E$1:$E174)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F176=\"\",\"\",MAX($E$1:$E175)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F177=\"\",\"\",MAX($E$1:$E176)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F178=\"\",\"\",MAX($E$1:$E177)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F179=\"\",\"\",MAX($E$1:$E178)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F180=\"\",\"\",MAX($E$1:$E179)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F181=\"\",\"\",MAX($E$1:$E180)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F182=\"\",\"\",MAX($E$1:$E181)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F183=\"\",\"\",MAX($E$1:$E182)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F184=\"\",\"\",MAX($E$1:$E183)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F185=\"\",\"\",MAX($E$1:$E184)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F186=\"\",\"\",MAX($E$1:$E185)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F187=\"\",\"\",MAX($E$1:$E186)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F188=\"\",\"\",MAX($E$1:$E187)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F189=\"\",\"\",MAX($E$1:$E188)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F190=\"\",\"\",MAX($E$1:$E189)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F191=\"\",\"\",MAX($E$1:$E190)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F192=\"\",\"\",MAX($E$1:$E191)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F193=\"\",\"\",MAX($E$1:$E192)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F194=\"\",\"\",MAX($E$1:$E193)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F195=\"\",\"\",MAX($E$1:$E194)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F196=\"\",\"\",MAX($E$1:$E195)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F197=\"\",\"\",MAX($E$1:$E196)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F198=\"\",\"\",MAX($E$1:$E197)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F199=\"\",\"\",MAX($E$1:$E198)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F200=\"\",\"\",MAX($E$1:$E199)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F201=\"\",\"\",MAX($E$1:$E200)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F202=\"\",\"\",MAX($E$1:$E201)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F203=\"\",\"\",MAX($E$1:$E202)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F204=\"\",\"\",MAX($E$1:$E203)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F205=\"\",\"\",MAX($E$1:$E204)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F206=\"\",\"\",MAX($E$1:$E205)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F207=\"\",\"\",MAX($E$1:$E206)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F208=\"\",\"\",MAX($E$1:$E207)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($P208<>\"\",\"GT\",IF($Q208<>\"\",\"LARGE\",IF($R208<>\"\",\"SEN\",IF($S208<>\"\",\"ADMIN\",IF($T208<>\"\",\"ST\",IF($U208<>\"\",\"NET\",\"\"))))))","v":""}]
[null,null,null,null,{"$f":"IF(F209=\"\",\"\",MAX($E$1:$E208)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F210=\"\",\"\",MAX($E$1:$E209)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F211=\"\",\"\",MAX($E$1:$E210)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F212=\"\",\"\",MAX($E$1:$E211)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F213=\"\",\"\",MAX($E$1:$E212)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F214=\"\",\"\",MAX($E$1:$E213)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F215=\"\",\"\",MAX($E$1:$E214)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F216=\"\",\"\",MAX($E$1:$E215)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F217=\"\",\"\",MAX($E$1:$E216)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F218=\"\",\"\",MAX($E$1:$E217)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F219=\"\",\"\",MAX($E$1:$E218)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F220=\"\",\"\",MAX($E$1:$E219)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F221=\"\",\"\",MAX($E$1:$E220)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F222=\"\",\"\",MAX($E$1:$E221)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F223=\"\",\"\",MAX($E$1:$E222)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F224=\"\",\"\",MAX($E$1:$E223)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F225=\"\",\"\",MAX($E$1:$E224)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F226=\"\",\"\",MAX($E$1:$E225)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F227=\"\",\"\",MAX($E$1:$E226)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F228=\"\",\"\",MAX($E$1:$E227)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F229=\"\",\"\",MAX($E$1:$E228)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F230=\"\",\"\",MAX($E$1:$E229)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F231=\"\",\"\",MAX($E$1:$E230)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F232=\"\",\"\",MAX($E$1:$E231)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F233=\"\",\"\",MAX($E$1:$E232)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F234=\"\",\"\",MAX($E$1:$E233)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F235=\"\",\"\",MAX($E$1:$E234)+1)","v":""},{"$f":"IF(OR($AB235<>\"\",$U235<>\"\",$T235<>\"\",$S235<>\"\",$R235<>\"\",$Q235<>\"\",$P235<>\"\",$N235<>\"\",$L235<>\"\",$J235<>\"\",$H235<>\"\",$G235<>\"\"),\"Information Entered\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F236=\"\",\"\",MAX($E$1:$E235)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F237=\"\",\"\",MAX($E$1:$E236)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F238=\"\",\"\",MAX($E$1:$E237)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F239=\"\",\"\",MAX($E$1:$E238)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F240=\"\",\"\",MAX($E$1:$E239)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F241=\"\",\"\",MAX($E$1:$E240)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F242=\"\",\"\",MAX($E$1:$E241)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F243=\"\",\"\",MAX($E$1:$E242)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F244=\"\",\"\",MAX($E$1:$E243)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F245=\"\",\"\",MAX($E$1:$E244)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F246=\"\",\"\",MAX($E$1:$E245)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F247=\"\",\"\",MAX($E$1:$E246)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F248=\"\",\"\",MAX($E$1:$E247)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F249=\"\",\"\",MAX($E$1:$E248)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F250=\"\",\"\",MAX($E$1:$E249)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F251=\"\",\"\",MAX($E$1:$E250)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F252=\"\",\"\",MAX($E$1:$E251)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F253=\"\",\"\",MAX($E$1:$E252)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F254=\"\",\"\",MAX($E$1:$E253)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F255=\"\",\"\",MAX($E$1:$E254)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F256=\"\",\"\",MAX($E$1:$E255)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F257=\"\",\"\",MAX($E$1:$E256)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F258=\"\",\"\",MAX($E$1:$E257)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F259=\"\",\"\",MAX($E$1:$E258)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F260=\"\",\"\",MAX($E$1:$E259)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F261=\"\",\"\",MAX($E$1:$E260)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F262=\"\",\"\",MAX($E$1:$E261)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F263=\"\",\"\",MAX($E$1:$E262)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F264=\"\",\"\",MAX($E$1:$E263)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F265=\"\",\"\",MAX($E$1:$E264)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F266=\"\",\"\",MAX($E$1:$E265)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F267=\"\",\"\",MAX($E$1:$E266)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F268=\"\",\"\",MAX($E$1:$E267)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F269=\"\",\"\",MAX($E$1:$E268)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F270=\"\",\"\",MAX($E$1:$E269)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F271=\"\",\"\",MAX($E$1:$E270)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F272=\"\",\"\",MAX($E$1:$E271)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($P272<>\"\",\"GT\",IF($Q272<>\"\",\"LARGE\",IF($R272<>\"\",\"SEN\",IF($S272<>\"\",\"ADMIN\",IF($T272<>\"\",\"ST\",IF($U272<>\"\",\"NET\",\"\"))))))","v":""}]
[null,null,null,null,{"$f":"IF(F273=\"\",\"\",MAX($E$1:$E272)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F274=\"\",\"\",MAX($E$1:$E273)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F275=\"\",\"\",MAX($E$1:$E274)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F276=\"\",\"\",MAX($E$1:$E275)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F277=\"\",\"\",MAX($E$1:$E276)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F278=\"\",\"\",MAX($E$1:$E277)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F279=\"\",\"\",MAX($E$1:$E278)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F280=\"\",\"\",MAX($E$1:$E279)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F281=\"\",\"\",MAX($E$1:$E280)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F282=\"\",\"\",MAX($E$1:$E281)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F283=\"\",\"\",MAX($E$1:$E282)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F284=\"\",\"\",MAX($E$1:$E283)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($N284<>\"\",1,\"\")","v":""},null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F285=\"\",\"\",MAX($E$1:$E284)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F286=\"\",\"\",MAX($E$1:$E285)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F287=\"\",\"\",MAX($E$1:$E286)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F288=\"\",\"\",MAX($E$1:$E287)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F289=\"\",\"\",MAX($E$1:$E288)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F290=\"\",\"\",MAX($E$1:$E289)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F291=\"\",\"\",MAX($E$1:$E290)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F292=\"\",\"\",MAX($E$1:$E291)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F293=\"\",\"\",MAX($E$1:$E292)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F294=\"\",\"\",MAX($E$1:$E293)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F295=\"\",\"\",MAX($E$1:$E294)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F296=\"\",\"\",MAX($E$1:$E295)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F297=\"\",\"\",MAX($E$1:$E296)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F298=\"\",\"\",MAX($E$1:$E297)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F299=\"\",\"\",MAX($E$1:$E298)+1)","v":""},{"$f":"IF(OR($AB299<>\"\",$U299<>\"\",$T299<>\"\",$S299<>\"\",$R299<>\"\",$Q299<>\"\",$P299<>\"\",$N299<>\"\",$L299<>\"\",$J299<>\"\",$H299<>\"\",$G299<>\"\"),\"Information Entered\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F300=\"\",\"\",MAX($E$1:$E299)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F301=\"\",\"\",MAX($E$1:$E300)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F302=\"\",\"\",MAX($E$1:$E301)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F303=\"\",\"\",MAX($E$1:$E302)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F304=\"\",\"\",MAX($E$1:$E303)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F305=\"\",\"\",MAX($E$1:$E304)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F306=\"\",\"\",MAX($E$1:$E305)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F307=\"\",\"\",MAX($E$1:$E306)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F308=\"\",\"\",MAX($E$1:$E307)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F309=\"\",\"\",MAX($E$1:$E308)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F310=\"\",\"\",MAX($E$1:$E309)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F311=\"\",\"\",MAX($E$1:$E310)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F312=\"\",\"\",MAX($E$1:$E311)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F313=\"\",\"\",MAX($E$1:$E312)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F314=\"\",\"\",MAX($E$1:$E313)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F315=\"\",\"\",MAX($E$1:$E314)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F316=\"\",\"\",MAX($E$1:$E315)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F317=\"\",\"\",MAX($E$1:$E316)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F318=\"\",\"\",MAX($E$1:$E317)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F319=\"\",\"\",MAX($E$1:$E318)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F320=\"\",\"\",MAX($E$1:$E319)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F321=\"\",\"\",MAX($E$1:$E320)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F322=\"\",\"\",MAX($E$1:$E321)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F323=\"\",\"\",MAX($E$1:$E322)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F324=\"\",\"\",MAX($E$1:$E323)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F325=\"\",\"\",MAX($E$1:$E324)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F326=\"\",\"\",MAX($E$1:$E325)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F327=\"\",\"\",MAX($E$1:$E326)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F328=\"\",\"\",MAX($E$1:$E327)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F329=\"\",\"\",MAX($E$1:$E328)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F330=\"\",\"\",MAX($E$1:$E329)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F331=\"\",\"\",MAX($E$1:$E330)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F332=\"\",\"\",MAX($E$1:$E331)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F333=\"\",\"\",MAX($E$1:$E332)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F334=\"\",\"\",MAX($E$1:$E333)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F335=\"\",\"\",MAX($E$1:$E334)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F336=\"\",\"\",MAX($E$1:$E335)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,{"$f":"IF($P336<>\"\",\"GT\",IF($Q336<>\"\",\"LARGE\",IF($R336<>\"\",\"SEN\",IF($S336<>\"\",\"ADMIN\",IF($T336<>\"\",\"ST\",IF($U336<>\"\",\"NET\",\"\"))))))","v":""}]
[null,null,null,null,{"$f":"IF(F337=\"\",\"\",MAX($E$1:$E336)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F338=\"\",\"\",MAX($E$1:$E337)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F339=\"\",\"\",MAX($E$1:$E338)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F340=\"\",\"\",MAX($E$1:$E339)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F341=\"\",\"\",MAX($E$1:$E340)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F342=\"\",\"\",MAX($E$1:$E341)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F343=\"\",\"\",MAX($E$1:$E342)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F344=\"\",\"\",MAX($E$1:$E343)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F345=\"\",\"\",MAX($E$1:$E344)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F346=\"\",\"\",MAX($E$1:$E345)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F347=\"\",\"\",MAX($E$1:$E346)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F348=\"\",\"\",MAX($E$1:$E347)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($N348<>\"\",1,\"\")","v":""},null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F349=\"\",\"\",MAX($E$1:$E348)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F350=\"\",\"\",MAX($E$1:$E349)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F351=\"\",\"\",MAX($E$1:$E350)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F352=\"\",\"\",MAX($E$1:$E351)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F353=\"\",\"\",MAX($E$1:$E352)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F354=\"\",\"\",MAX($E$1:$E353)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F355=\"\",\"\",MAX($E$1:$E354)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F356=\"\",\"\",MAX($E$1:$E355)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F357=\"\",\"\",MAX($E$1:$E356)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F358=\"\",\"\",MAX($E$1:$E357)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F359=\"\",\"\",MAX($E$1:$E358)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F360=\"\",\"\",MAX($E$1:$E359)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F361=\"\",\"\",MAX($E$1:$E360)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F362=\"\",\"\",MAX($E$1:$E361)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F363=\"\",\"\",MAX($E$1:$E362)+1)","v":""},{"$f":"IF(OR($AB363<>\"\",$U363<>\"\",$T363<>\"\",$S363<>\"\",$R363<>\"\",$Q363<>\"\",$P363<>\"\",$N363<>\"\",$L363<>\"\",$J363<>\"\",$H363<>\"\",$G363<>\"\"),\"Information Entered\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F364=\"\",\"\",MAX($E$1:$E363)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F365=\"\",\"\",MAX($E$1:$E364)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F366=\"\",\"\",MAX($E$1:$E365)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F367=\"\",\"\",MAX($E$1:$E366)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F368=\"\",\"\",MAX($E$1:$E367)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F369=\"\",\"\",MAX($E$1:$E368)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F370=\"\",\"\",MAX($E$1:$E369)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F371=\"\",\"\",MAX($E$1:$E370)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F372=\"\",\"\",MAX($E$1:$E371)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F373=\"\",\"\",MAX($E$1:$E372)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F374=\"\",\"\",MAX($E$1:$E373)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F375=\"\",\"\",MAX($E$1:$E374)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F376=\"\",\"\",MAX($E$1:$E375)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F377=\"\",\"\",MAX($E$1:$E376)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F378=\"\",\"\",MAX($E$1:$E377)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F379=\"\",\"\",MAX($E$1:$E378)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F380=\"\",\"\",MAX($E$1:$E379)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F381=\"\",\"\",MAX($E$1:$E380)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F382=\"\",\"\",MAX($E$1:$E381)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F383=\"\",\"\",MAX($E$1:$E382)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F384=\"\",\"\",MAX($E$1:$E383)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F385=\"\",\"\",MAX($E$1:$E384)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F386=\"\",\"\",MAX($E$1:$E385)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F387=\"\",\"\",MAX($E$1:$E386)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F388=\"\",\"\",MAX($E$1:$E387)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F389=\"\",\"\",MAX($E$1:$E388)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F390=\"\",\"\",MAX($E$1:$E389)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F391=\"\",\"\",MAX($E$1:$E390)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F392=\"\",\"\",MAX($E$1:$E391)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F393=\"\",\"\",MAX($E$1:$E392)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F394=\"\",\"\",MAX($E$1:$E393)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F395=\"\",\"\",MAX($E$1:$E394)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F396=\"\",\"\",MAX($E$1:$E395)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F397=\"\",\"\",MAX($E$1:$E396)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F398=\"\",\"\",MAX($E$1:$E397)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F399=\"\",\"\",MAX($E$1:$E398)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F400=\"\",\"\",MAX($E$1:$E399)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,{"$f":"IF($P400<>\"\",\"GT\",IF($Q400<>\"\",\"LARGE\",IF($R400<>\"\",\"SEN\",IF($S400<>\"\",\"ADMIN\",IF($T400<>\"\",\"ST\",IF($U400<>\"\",\"NET\",\"\"))))))","v":""}]
[null,null,null,null,{"$f":"IF(F401=\"\",\"\",MAX($E$1:$E400)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F402=\"\",\"\",MAX($E$1:$E401)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F403=\"\",\"\",MAX($E$1:$E402)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F404=\"\",\"\",MAX($E$1:$E403)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F405=\"\",\"\",MAX($E$1:$E404)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F406=\"\",\"\",MAX($E$1:$E405)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F407=\"\",\"\",MAX($E$1:$E406)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F408=\"\",\"\",MAX($E$1:$E407)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F409=\"\",\"\",MAX($E$1:$E408)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F410=\"\",\"\",MAX($E$1:$E409)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F411=\"\",\"\",MAX($E$1:$E410)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F412=\"\",\"\",MAX($E$1:$E411)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($N412<>\"\",1,\"\")","v":""},null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F413=\"\",\"\",MAX($E$1:$E412)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F414=\"\",\"\",MAX($E$1:$E413)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F415=\"\",\"\",MAX($E$1:$E414)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F416=\"\",\"\",MAX($E$1:$E415)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F417=\"\",\"\",MAX($E$1:$E416)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F418=\"\",\"\",MAX($E$1:$E417)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F419=\"\",\"\",MAX($E$1:$E418)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F420=\"\",\"\",MAX($E$1:$E419)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F421=\"\",\"\",MAX($E$1:$E420)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F422=\"\",\"\",MAX($E$1:$E421)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F423=\"\",\"\",MAX($E$1:$E422)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F424=\"\",\"\",MAX($E$1:$E423)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F425=\"\",\"\",MAX($E$1:$E424)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F426=\"\",\"\",MAX($E$1:$E425)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F427=\"\",\"\",MAX($E$1:$E426)+1)","v":""},{"$f":"IF(OR($AB427<>\"\",$U427<>\"\",$T427<>\"\",$S427<>\"\",$R427<>\"\",$Q427<>\"\",$P427<>\"\",$N427<>\"\",$L427<>\"\",$J427<>\"\",$H427<>\"\",$G427<>\"\"),\"Information Entered\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F428=\"\",\"\",MAX($E$1:$E427)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F429=\"\",\"\",MAX($E$1:$E428)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F430=\"\",\"\",MAX($E$1:$E429)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F431=\"\",\"\",MAX($E$1:$E430)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F432=\"\",\"\",MAX($E$1:$E431)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F433=\"\",\"\",MAX($E$1:$E432)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F434=\"\",\"\",MAX($E$1:$E433)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F435=\"\",\"\",MAX($E$1:$E434)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F436=\"\",\"\",MAX($E$1:$E435)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F437=\"\",\"\",MAX($E$1:$E436)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F438=\"\",\"\",MAX($E$1:$E437)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F439=\"\",\"\",MAX($E$1:$E438)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F440=\"\",\"\",MAX($E$1:$E439)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F441=\"\",\"\",MAX($E$1:$E440)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F442=\"\",\"\",MAX($E$1:$E441)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F443=\"\",\"\",MAX($E$1:$E442)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F444=\"\",\"\",MAX($E$1:$E443)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F445=\"\",\"\",MAX($E$1:$E444)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F446=\"\",\"\",MAX($E$1:$E445)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F447=\"\",\"\",MAX($E$1:$E446)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F448=\"\",\"\",MAX($E$1:$E447)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F449=\"\",\"\",MAX($E$1:$E448)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F450=\"\",\"\",MAX($E$1:$E449)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F451=\"\",\"\",MAX($E$1:$E450)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F452=\"\",\"\",MAX($E$1:$E451)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F453=\"\",\"\",MAX($E$1:$E452)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F454=\"\",\"\",MAX($E$1:$E453)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F455=\"\",\"\",MAX($E$1:$E454)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F456=\"\",\"\",MAX($E$1:$E455)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F457=\"\",\"\",MAX($E$1:$E456)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F458=\"\",\"\",MAX($E$1:$E457)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F459=\"\",\"\",MAX($E$1:$E458)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F460=\"\",\"\",MAX($E$1:$E459)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F461=\"\",\"\",MAX($E$1:$E460)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F462=\"\",\"\",MAX($E$1:$E461)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F463=\"\",\"\",MAX($E$1:$E462)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F464=\"\",\"\",MAX($E$1:$E463)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,{"$f":"IF($P464<>\"\",\"GT\",IF($Q464<>\"\",\"LARGE\",IF($R464<>\"\",\"SEN\",IF($S464<>\"\",\"ADMIN\",IF($T464<>\"\",\"ST\",IF($U464<>\"\",\"NET\",\"\"))))))","v":""}]
[null,null,null,null,{"$f":"IF(F465=\"\",\"\",MAX($E$1:$E464)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F466=\"\",\"\",MAX($E$1:$E465)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F467=\"\",\"\",MAX($E$1:$E466)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F468=\"\",\"\",MAX($E$1:$E467)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F469=\"\",\"\",MAX($E$1:$E468)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F470=\"\",\"\",MAX($E$1:$E469)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F471=\"\",\"\",MAX($E$1:$E470)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F472=\"\",\"\",MAX($E$1:$E471)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F473=\"\",\"\",MAX($E$1:$E472)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F474=\"\",\"\",MAX($E$1:$E473)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F475=\"\",\"\",MAX($E$1:$E474)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F476=\"\",\"\",MAX($E$1:$E475)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($N476<>\"\",1,\"\")","v":""},null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F477=\"\",\"\",MAX($E$1:$E476)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F478=\"\",\"\",MAX($E$1:$E477)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F479=\"\",\"\",MAX($E$1:$E478)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F480=\"\",\"\",MAX($E$1:$E479)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F481=\"\",\"\",MAX($E$1:$E480)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F482=\"\",\"\",MAX($E$1:$E481)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F483=\"\",\"\",MAX($E$1:$E482)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F484=\"\",\"\",MAX($E$1:$E483)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F485=\"\",\"\",MAX($E$1:$E484)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F486=\"\",\"\",MAX($E$1:$E485)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F487=\"\",\"\",MAX($E$1:$E486)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F488=\"\",\"\",MAX($E$1:$E487)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F489=\"\",\"\",MAX($E$1:$E488)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F490=\"\",\"\",MAX($E$1:$E489)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F491=\"\",\"\",MAX($E$1:$E490)+1)","v":""},{"$f":"IF(OR($AB491<>\"\",$U491<>\"\",$T491<>\"\",$S491<>\"\",$R491<>\"\",$Q491<>\"\",$P491<>\"\",$N491<>\"\",$L491<>\"\",$J491<>\"\",$H491<>\"\",$G491<>\"\"),\"Information Entered\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F492=\"\",\"\",MAX($E$1:$E491)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F493=\"\",\"\",MAX($E$1:$E492)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F494=\"\",\"\",MAX($E$1:$E493)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F495=\"\",\"\",MAX($E$1:$E494)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F496=\"\",\"\",MAX($E$1:$E495)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F497=\"\",\"\",MAX($E$1:$E496)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F498=\"\",\"\",MAX($E$1:$E497)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F499=\"\",\"\",MAX($E$1:$E498)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F500=\"\",\"\",MAX($E$1:$E499)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F501=\"\",\"\",MAX($E$1:$E500)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F502=\"\",\"\",MAX($E$1:$E501)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F503=\"\",\"\",MAX($E$1:$E502)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F504=\"\",\"\",MAX($E$1:$E503)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F505=\"\",\"\",MAX($E$1:$E504)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F506=\"\",\"\",MAX($E$1:$E505)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F507=\"\",\"\",MAX($E$1:$E506)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F508=\"\",\"\",MAX($E$1:$E507)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F509=\"\",\"\",MAX($E$1:$E508)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F510=\"\",\"\",MAX($E$1:$E509)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F511=\"\",\"\",MAX($E$1:$E510)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F512=\"\",\"\",MAX($E$1:$E511)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F513=\"\",\"\",MAX($E$1:$E512)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F514=\"\",\"\",MAX($E$1:$E513)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F515=\"\",\"\",MAX($E$1:$E514)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F516=\"\",\"\",MAX($E$1:$E515)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]
[null,null,null,null,{"$f":"IF(F517=\"\",\"\",MAX($E$1:$E516)+1)","v":""},"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,""]

{"sheet":"(Manual) ADS Template","index":4,"n_rows":267,"n_cols":23,"rows_kept":267,"cut":false,"hidden":true,"merged":[[3,0,3,4],[5,10,5,12],[5,16,5,18],[5,20,5,22],[6,10,6,12],[6,16,6,18],[6,20,6,22],[8,10,8,12],[8,16,8,22],[9,16,10,22],[1,6,1,7],[2,16,3,18],[2,20,3,22],[14,6,15,7],[20,10,20,12],[20,16,20,18],[20,20,20,22],[22,10,22,12],[23,10,23,12],[23,16,23,18],[23,20,23,22],[11,3,11,4],[11,6,11,7],[11,10,11,12],[11,16,11,18],[11,20,11,22],[12,6,13,7],[32,10,32,12],[32,16,32,18],[32,20,32,22],[34,2,34,3],[34,10,34,12],[34,16,34,18],[34,20,34,22],[28,6,28,7],[28,10,28,12],[28,16,28,18],[28,20,28,22],[30,10,30,12],[30,16,30,18],[30,20,30,22],[43,10,43,12],[43,16,43,18],[43,20,43,22],[48,2,49,2],[48,3,49,4],[48,6,49,6],[48,10,49,12],[48,16,49,18],[48,20,49,22],[77,10,77,12],[78,2,78,4],[98,10,98,12],[98,16,98,18],[98,20,98,22],[100,16,101,18],[100,20,101,22],[52,16,53,18],[52,20,53,22],[54,10,54,12],[55,2,55,4],[75,16,76,18],[75,20,76,22],[133,20,133,22],[138,10,138,12],[139,16,139,18],[139,20,139,22],[102,10,102,12],[117,16,118,18],[117,20,118,22],[119,10,119,12],[123,16,124,18],[123,20,124,22],[141,4,142,4],[144,2,144,4],[155,2,155,4],[155,6,155,7],[158,6,159,7],[158,10,158,12],[125,10,125,12],[133,10,133,12],[133,16,133,18],[164,16,164,18],[164,20,164,22],[165,2,165,4],[165,6,165,7],[166,6,166,7],[166,16,166,18],[166,20,166,22],[158,16,158,18],[158,20,158,22],[160,10,160,12],[160,16,160,18],[160,20,160,22],[162,3,162,4],[162,6,162,7],[162,10,162,12],[162,16,162,18],[162,20,162,22],[188,10,188,12],[189,10,189,12],[174,2,174,4],[174,6,174,7],[175,2,175,4],[176,2,176,4],[178,16,178,18],[178,20,178,22],[167,6,168,7],[170,2,170,4],[170,6,172,6],[171,2,171,4],[172,2,172,4],[173,2,173,4],[190,6,190,7],[191,2,191,4],[194,2,194,4],[194,6,196,6],[196,2,196,4],[202,3,202,4],[202,6,202,7],[179,2,180,3],[181,2,182,3],[183,2,183,4],[188,2,189,3],[205,20,205,22],[206,3,206,4],[206,10,206,12],[206,16,206,18],[206,20,206,22],[202,10,202,12],[202,16,202,18],[202,20,202,22],[203,10,203,12],[204,3,204,4],[204,10,204,12],[204,16,204,18],[204,20,204,22],[207,10,207,12],[208,10,208,12],[209,10,209,12],[210,10,210,12],[211,10,211,12],[212,10,212,12],[205,3,205,4],[205,10,205,12],[205,16,205,18],[220,10,220,12],[222,6,222,7],[222,10,222,12],[222,16,222,18],[222,20,222,22],[224,10,224,12],[224,16,224,18],[224,20,224,22],[214,10,214,12],[215,10,215,12],[216,10,216,12],[217,10,217,12],[218,10,218,12],[219,10,219,12],[229,6,229,7],[229,10,229,12],[229,16,229,18],[229,20,229,22],[231,10,231,12],[233,3,233,4],[233,10,233,12],[233,16,233,18],[233,20,233,22],[238,6,239,7],[265,3,265,4],[265,6,265,7],[265,10,265,12],[265,16,265,18],[265,20,265,22],[235,10,235,12],[235,16,235,18],[235,20,235,22],[237,10,237,12],[237,16,237,18],[237,20,237,22]]}
[]
["AREA DATA SHEETS",null,null,null,null,null,"notes & information for client",null,null,null,null,"Area data for:",null,null,null,null,null,null,null,"compliance checks"]
["for spaces in: ",null,null,null,null,null,{"$f":"MAX(MAX($G$1:$H2),MAX($F3:F$3))+1","v":1},null,null,null,null,{"$f":"MAX(MAX($J$1:$N2),MAX($J3:K$3))+1","v":1},null,null,null,null,"Contractor's Proposal",null,null,null,"Practical Completion"]
["[name of school]",null,null,null,null,null,{"$f":"MAX(MAX($G$1:$H3),MAX($F4:F$4))+1","v":2},null,null,null,null,{"$f":"MAX(MAX($J$1:$N3),MAX($J4:K$4))+1","v":2}]
["Key Data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"identify below if new/ remodel or refurb/ redec'n"]
[null,null,"reference code",null,"name of individual space",null,"Contractor to amend to individual space name in SoA",null,null,null,"Generic"]
[null,null,null,null,"ref code for individual space",null,"Contractor to amend to individual space code if in SoA ",null,null,null,"Generic",null,null,null,null,null,"code on drawing",null,null,null,"code on drawing"]
[null,"1. Function"]
[null,null,"Summary description",null,null,null,"brief description of space",null,null,null,{"$f":"MAX(MAX($J$1:$N8),MAX($J9:J$9))+1","v":3},null,null,null,null,null,"NOTE: if value is left blank, the proposal is deemed to be as the requirement, unless Contractor to Specify (CTS). 'Note ref.' must be provided where differences are proposed, referencing supporting information."]
[null,null,"Required Area",null,null,null,{"$f":"MAX(MAX($G$1:$H9),MAX($F10:F$10))+1","v":3},null,null,null,{"$f":"MAX(MAX($J$1:$N9),MAX($J10:J$10))+1","v":4},{"$f":"MAX(MAX($J$1:$N9),MAX($J10:K$10))+1","v":5},null,null,null,null,"List any changes to activities described below (or leave blank if there are no changes)"]
[]
[null,null,"Activities description","Range of activities or uses to be accommodated",null,null,"This text box describes the activities that should be able to take place in the space, which in turn will influence the choice of F&E and many of the requirements below, including the area.",null,null,null,{"$f":"MAX(MAX($J$1:$N11),MAX($J12:J$12))+1","v":6}]
[null,null,null,null,null,null,"maximum (not average) teaching group, or max group incl meeting area in staff & admin spaces, as SoA"]
[null,null,null,null,"Maximum group size/ Net capacity workplaces",null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N13),MAX($J14:J$14))+1","v":7},"/",{"$f":"MAX(MAX($J$1:$N13),MAX($J14:L$14))+1","v":8}]
[null,null,null,null,"number of staff",null,"staff or adults over and above pupils in teaching spaces, staff workstations in staff and admin spaces",null,null,null,{"$f":"MAX(MAX($J$1:$N14),MAX($J15:J$15))+1","v":9}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Actual area provided (m2)"]
[null,null,null,null,"Area Guidelines Category",null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N16),MAX($J17:J$17))+1","v":10},null,null,null,null,null,"actual area",null,"note ref.",null,"actual area",null,"note ref."]
[null,null,null,null,"Area Guidelines Zone",null,{"$f":"MAX(MAX($G$1:$H17),MAX($F18:F$18))+1","v":4},null,null,null,{"$f":"MAX(MAX($J$1:$N17),MAX($J18:J$18))+1","v":11}]
[null,null,null,null,"Net capacity category",null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N18),MAX($J19:J$19))+1","v":12}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"identify if available for community use during or after school day"]
[null,null,"Community use",null,"Third Party Use",null,"community use during or outside core school day",null,null,null,{"$f":"MAX(MAX($J$1:$N20),MAX($J21:J$21))+1","v":13}]
[null,null,"FM issues"]
[null,null,"Availability Priority Category",null,null,null,"As SoA",null,null,null,{"$f":"MAX(MAX($J$1:$N22),MAX($J23:J$23))+1","v":14}]
[null,null,"Consequential Unavailability",null,null,null,"As SoA",null,null,null,{"$f":"MAX(MAX($J$1:$N23),MAX($J24:J$24))+1","v":15}]
[]
[]
["Location and Space"]
[null,"2. Location and access",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"actual location",null,null,null,"actual location"]
[null,null,"Location",null,null,null,"school to identify where this space should be located",null,null,null,{"$f":"MAX(MAX($J$1:$N28),MAX($J29:J$29))+1","v":16}]
[]
[null,null,"Access requirements",null,null,null,"disabled access options",null,null,null,{"$f":"MAX(MAX($J$1:$N30),MAX($J31:J$31))+1","v":17}]
[null,"3. Organisation",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"actual enclosure/ adjacency",null,null,null,"actual enclosure/ adjacency"]
[null,null,"Enclosure requirements",null,null,null,"enclosed/ semi-enclosed/ open plan",null,null,null,{"$f":"MAX(MAX($J$1:$N32),MAX($J33:J$33))+1","v":18}]
[]
[null,null,"Adjacency requirements",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N34),MAX($J35:J$35))+1","v":19}]
[null,"4. Space",null,null,null,null,null,null,null,null,"If new / remodel",null,"If refurb / redec'n"]
[null,null,"Minimum area (m2)",null,null,null,{"$f":"MAX(MAX($G$1:$H36),MAX($F37:F$37))+1","v":5},null,null,null,{"$f":"MAX(MAX($J$1:$N36),MAX($J37:J$37))+1","v":20},null,{"$f":"MAX(MAX($J$1:$N36),MAX($J37:L$37))+1","v":21},null,null,null,"actual dims",null,"note ref.",null,"actual dims",null,"note ref."]
[]
[null,null,"Minimum ceiling height",null,null,null,{"$f":"MAX(MAX($G$1:$H38),MAX($F39:F$39))+1","v":6},null,null,null,{"$f":"MAX(MAX($J$1:$N38),MAX($J39:J$39))+1","v":22},null,{"$f":"MAX(MAX($J$1:$N38),MAX($J39:L$39))+1","v":23}]
[null,null,"Space depth (mm)",null,"where required",null,{"$f":"MAX(MAX($G$1:$H39),MAX($F40:F$40))+1","v":7},null,null,null,{"$f":"MAX(MAX($J$1:$N39),MAX($J40:J$40))+1","v":24},null,{"$f":"MAX(MAX($J$1:$N39),MAX($J40:L$40))+1","v":25}]
[]
[]
["Fabric and environment"]
[null,"5. External door(s)",null,null,"if required or preferred",null,"i.e. direct access via external door",null,null,null,{"$f":"MAX(MAX($J$1:$N43),MAX($J44:J$44))+1","v":26}]
[]
[null,"6. Windows and internal doorsets",null,null,null,null,null,null,null,null,"If new / remodel",null,"If refurb / redec'n",null,null,null,"actual dimension",null,null,null,"actual dimension"]
[null,null,"Window sill height (mm)",null,null,null,{"$f":"MAX(MAX($G$1:$H46),MAX($F47:F$47))+1","v":8},null,null,null,"CTS",{"$f":"MAX(MAX($J$1:$N46),MAX($J47:K$47))+1","v":27},{"$f":"MAX(MAX($J$1:$N46),MAX($J47:L$47))+1","v":28}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"description of window solution"]
[null,null,"Specific external door or window requirements","ironmongery, access, locks, integral or external blinds (for blinds see FF&E below)",null,null,"(requirement for external door identified in Access to outdoors above)",null,null,null,{"$f":"MAX(MAX($J$1:$N48),MAX($J49:J$49))+1","v":29}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"If new / remodel",null,"If refurb / redec'n",null,null,null,"description of entrance doorset solution"]
[null,null,"Doorset from circulation",null," including atria",null,"see tech annexe doorsets",null,null,null,{"$f":"MAX(MAX($J$1:$N52),MAX($J53:J$53))+1","v":30},null,{"$f":"MAX(MAX($J$1:$N52),MAX($J53:L$53))+1","v":31},null,null,null,{"$f":"INT(MAX(MAX($P$1:$Y52),MAX($P53:P53)))+1.01","v":1.01}]
[]
[null,null,"Description",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N54),MAX($J55:J$55))+1","v":32},null,null,null,null,null,"value",null,"note ref.",null,"value",null,"note ref."]
[null,null,"Acoustic airborne sound insulation rating for door into space from: corridor or non-teaching area",null,null,null,{"$f":"MAX(MAX($G$1:$H55),MAX($F56:F$56))+1","v":9},null,null,null,{"$f":"MAX(MAX($J$1:$N55),MAX($J56:J$56))+1","v":33},null,{"$f":"MAX(MAX($J$1:$N55),MAX($J56:L$56))+1","v":34},null,null,null,{"$f":"Q53+0.01","v":1.02}]
[null,null,"Door leaf width",null,null,null,"mm",null,null,null,{"$f":"MAX(MAX($J$1:$N56),MAX($J57:J$57))+1","v":35},null,{"$f":"MAX(MAX($J$1:$N56),MAX($J57:L$57))+1","v":36},null,null,null,{"$f":"Q56+0.02","v":1.04}]
[null,null,"Minimum clear opening width",null,null,null,"effective clear width in mm",null,null,null,{"$f":"MAX(MAX($J$1:$N57),MAX($J58:J$58))+1","v":37},null,{"$f":"MAX(MAX($J$1:$N57),MAX($J58:L$58))+1","v":38},null,null,null,{"$f":"Q57+0.01","v":1.05}]
[null,null,"Minimum clear opening height",null,null,null,"effective clear height in mm",null,null,null,{"$f":"MAX(MAX($J$1:$N58),MAX($J59:J$59))+1","v":39},null,{"$f":"MAX(MAX($J$1:$N58),MAX($J59:L$59))+1","v":40},null,null,null,1.06]
[null,null,"Minimum mechanical durability",null,null,null,{"$f":"MAX(MAX($G$1:$H59),MAX($F60:F$60))+1","v":10},null,null,null,{"$f":"MAX(MAX($J$1:$N59),MAX($J60:J$60))+1","v":41},null,{"$f":"MAX(MAX($J$1:$N59),MAX($J60:L$60))+1","v":42},null,null,null,1.07]
[null,null,"Minimum mechanical strength",null,null,null,"BS EN1192:2000",null,null,null,{"$f":"MAX(MAX($J$1:$N60),MAX($J61:J$61))+1","v":43},null,{"$f":"MAX(MAX($J$1:$N60),MAX($J61:L$61))+1","v":44},null,null,null,1.08]
[null,null,"Minimum fire and smoke resistance (value of \"##\") ",null,null,null,{"$f":"MAX(MAX($G$1:$H61),MAX($F62:F$62))+1","v":11},null,null,null,{"$f":"MAX(MAX($J$1:$N61),MAX($J62:J$62))+1","v":45},null,{"$f":"MAX(MAX($J$1:$N61),MAX($J62:L$62))+1","v":46},null,null,null,1.0900000000000001]
[null,null,"Minimum security rating",null,null,null,{"$f":"MAX(MAX($G$1:$H62),MAX($F63:F$63))+1","v":12},null,null,null,{"$f":"MAX(MAX($J$1:$N62),MAX($J63:J$63))+1","v":47},null,{"$f":"MAX(MAX($J$1:$N62),MAX($J63:L$63))+1","v":48},null,null,null,1.1000000000000001]
[null,null,"Minimum hygrothermal performance",null,null,null,"class defined in BS EN1192:2000 and BS EN1294:2000",null,null,null,{"$f":"MAX(MAX($J$1:$N63),MAX($J64:J$64))+1","v":49},null,{"$f":"MAX(MAX($J$1:$N63),MAX($J64:L$64))+1","v":50},null,null,null,1.1100000000000001]
[null,null,"Vision panels",null,null,null,"min height and width as FOS",null,null,null,{"$f":"MAX(MAX($J$1:$N64),MAX($J65:J$65))+1","v":51},null,{"$f":"MAX(MAX($J$1:$N64),MAX($J65:L$65))+1","v":52},null,null,null,1.1200000000000001]
[]
[null,null,"Ironmongery hardware:","Closer",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N66),MAX($J67:J$67))+1","v":53},null,{"$f":"MAX(MAX($J$1:$N66),MAX($J67:L$67))+1","v":54},null,null,null,{"$f":"Q65+0.01","v":1.1300000000000001}]
[null,null,null,"Electromagnetic hold open device",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N67),MAX($J68:J$68))+1","v":55},null,{"$f":"MAX(MAX($J$1:$N67),MAX($J68:L$68))+1","v":56},null,null,null,{"$f":"Q67+0.01","v":1.1400000000000001}]
[null,null,null,"Hinges",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N68),MAX($J69:J$69))+1","v":57},null,{"$f":"MAX(MAX($J$1:$N68),MAX($J69:L$69))+1","v":58},null,null,null,{"$f":"Q68+0.01","v":1.1500000000000001}]
[null,null,null,"Cylinder/ lock",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N69),MAX($J70:J$70))+1","v":59},null,{"$f":"MAX(MAX($J$1:$N69),MAX($J70:L$70))+1","v":60},null,null,null,1.1600000000000001]
[null,null,null,"Lever handle",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N70),MAX($J71:J$71))+1","v":61},null,{"$f":"MAX(MAX($J$1:$N70),MAX($J71:L$71))+1","v":62},null,null,null,1.1700000000000002]
[null,null,null,"Vertical pull handle",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N71),MAX($J72:J$72))+1","v":63},null,{"$f":"MAX(MAX($J$1:$N71),MAX($J72:L$72))+1","v":64},null,null,null,1.1800000000000002]
[null,null,null,"Staff-only access control system",null,null,{"$f":"MAX(MAX($G$1:$H72),MAX($F73:F$73))+1","v":13},null,null,null,{"$f":"MAX(MAX($J$1:$N72),MAX($J73:J$73))+1","v":65},null,{"$f":"MAX(MAX($J$1:$N72),MAX($J73:L$73))+1","v":66},null,null,null,1.1900000000000002]
[null,null,null,"Door protection",null,null,"kick plate height (mm)",null,null,null,{"$f":"MAX(MAX($J$1:$N73),MAX($J74:J$74))+1","v":67},null,{"$f":"MAX(MAX($J$1:$N73),MAX($J74:L$74))+1","v":68},null,null,null,1.2000000000000002]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"description of interlinking doorset solution"]
[null,null,"Doorset to adjacent space of similar type",null,null,null,"see tech annexe doorsets",null,null,null,{"$f":"MAX(MAX($J$1:$N75),MAX($J76:J$76))+1","v":69},null,{"$f":"MAX(MAX($J$1:$N75),MAX($J76:L$76))+1","v":70},null,null,null,{"$f":"INT(MAX(MAX($P$1:$Y75),MAX($P76:P76)))+1.01","v":2.0099999999999998}]
[]
[null,null,"Description",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N77),MAX($J78:J$78))+1","v":71},null,null,null,null,null,"value",null,"note ref.",null,"value",null,"note ref."]
[null,null,"Acoustic airborne sound insulation rating for door into space from: teaching space (eg. of same type)",null,null,null,{"$f":"MAX(MAX($G$1:$H78),MAX($F79:F$79))+1","v":14},null,null,null,{"$f":"MAX(MAX($J$1:$N78),MAX($J79:J$79))+1","v":72},null,{"$f":"MAX(MAX($J$1:$N78),MAX($J79:L$79))+1","v":73},null,null,null,{"$f":"Q76+0.02","v":2.0299999999999998}]
[null,null,"Door leaf width",null,null,null,"mm",null,null,null,{"$f":"MAX(MAX($J$1:$N79),MAX($J80:J$80))+1","v":74},null,{"$f":"MAX(MAX($J$1:$N79),MAX($J80:L$80))+1","v":75},null,null,null,{"$f":"Q79+0.01","v":2.0399999999999996}]
[null,null,"Minimum clear opening width",null,null,null,"effective clear width in mm",null,null,null,{"$f":"MAX(MAX($J$1:$N80),MAX($J81:J$81))+1","v":76},null,{"$f":"MAX(MAX($J$1:$N80),MAX($J81:L$81))+1","v":77},null,null,null,{"$f":"Q80+0.01","v":2.0499999999999994}]
[null,null,"Minimum clear opening height",null,null,null,"effective clear height in mm",null,null,null,{"$f":"MAX(MAX($J$1:$N81),MAX($J82:J$82))+1","v":78},null,{"$f":"MAX(MAX($J$1:$N81),MAX($J82:L$82))+1","v":79},null,null,null,2.0599999999999992]
[null,null,"Minimum mechanical durability",null,null,null,{"$f":"MAX(MAX($G$1:$H82),MAX($F83:F$83))+1","v":15},null,null,null,{"$f":"MAX(MAX($J$1:$N82),MAX($J83:J$83))+1","v":80},null,{"$f":"MAX(MAX($J$1:$N82),MAX($J83:L$83))+1","v":81},null,null,null,2.069999999999999]
[null,null,"Minimum mechanical strength",null,null,null,"BS EN1192:2000",null,null,null,{"$f":"MAX(MAX($J$1:$N83),MAX($J84:J$84))+1","v":82},null,{"$f":"MAX(MAX($J$1:$N83),MAX($J84:L$84))+1","v":83},null,null,null,2.0799999999999987]
[null,null,"Minimum fire and smoke resistance (value of \"##\") ",null,null,null,{"$f":"MAX(MAX($G$1:$H84),MAX($F85:F$85))+1","v":16},null,null,null,{"$f":"MAX(MAX($J$1:$N84),MAX($J85:J$85))+1","v":84},null,{"$f":"MAX(MAX($J$1:$N84),MAX($J85:L$85))+1","v":85},null,null,null,2.0899999999999985]
[null,null,"Minimum security rating",null,null,null,{"$f":"MAX(MAX($G$1:$H85),MAX($F86:F$86))+1","v":17},null,null,null,{"$f":"MAX(MAX($J$1:$N85),MAX($J86:J$86))+1","v":86},null,{"$f":"MAX(MAX($J$1:$N85),MAX($J86:L$86))+1","v":87},null,null,null,2.0999999999999983]
[null,null,"Minimum hygrothermal performance",null,null,null,"class defined in BS EN1192:2000 and BS EN1294:2000",null,null,null,{"$f":"MAX(MAX($J$1:$N86),MAX($J87:J$87))+1","v":88},null,{"$f":"MAX(MAX($J$1:$N86),MAX($J87:L$87))+1","v":89},null,null,null,2.1099999999999981]
[null,null,"Vision panels",null,null,null,"min height and width as FOS",null,null,null,{"$f":"MAX(MAX($J$1:$N87),MAX($J88:J$88))+1","v":90},null,{"$f":"MAX(MAX($J$1:$N87),MAX($J88:L$88))+1","v":91},null,null,null,2.1199999999999979]
[]
[null,null,"Ironmongery hardware:","Closer",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N89),MAX($J90:J$90))+1","v":92},null,{"$f":"MAX(MAX($J$1:$N89),MAX($J90:L$90))+1","v":93},null,null,null,{"$f":"Q88+0.01","v":2.1299999999999977}]
[null,null,null,"Electromagnetic hold open device",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N90),MAX($J91:J$91))+1","v":94},null,{"$f":"MAX(MAX($J$1:$N90),MAX($J91:L$91))+1","v":95},null,null,null,{"$f":"Q90+0.01","v":2.1399999999999975}]
[null,null,null,"Hinges",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N91),MAX($J92:J$92))+1","v":96},null,{"$f":"MAX(MAX($J$1:$N91),MAX($J92:L$92))+1","v":97},null,null,null,{"$f":"Q91+0.01","v":2.1499999999999972}]
[null,null,null,"Cylinder/ lock",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N92),MAX($J93:J$93))+1","v":98},null,{"$f":"MAX(MAX($J$1:$N92),MAX($J93:L$93))+1","v":99},null,null,null,2.159999999999997]
[null,null,null,"Lever handle",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N93),MAX($J94:J$94))+1","v":100},null,{"$f":"MAX(MAX($J$1:$N93),MAX($J94:L$94))+1","v":101},null,null,null,2.1699999999999968]
[null,null,null,"Vertical pull handle",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N94),MAX($J95:J$95))+1","v":102},null,{"$f":"MAX(MAX($J$1:$N94),MAX($J95:L$95))+1","v":103},null,null,null,2.1799999999999966]
[null,null,null,"Staff-only access control system",null,null,{"$f":"MAX(MAX($G$1:$H95),MAX($F96:F$96))+1","v":18},null,null,null,{"$f":"MAX(MAX($J$1:$N95),MAX($J96:J$96))+1","v":104},null,{"$f":"MAX(MAX($J$1:$N95),MAX($J96:L$96))+1","v":105},null,null,null,2.1899999999999964]
[null,null,null,"Door protection",null,null,"kick plate height (mm)",null,null,null,{"$f":"MAX(MAX($J$1:$N96),MAX($J97:J$97))+1","v":106},null,{"$f":"MAX(MAX($J$1:$N96),MAX($J97:L$97))+1","v":107},null,null,null,2.1999999999999962]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"specific doorset requirements met and additions"]
[null,null,"Specific doorset requirements",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N98),MAX($J99:J$99))+1","v":108}]
[null,"7. Finishes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"description of floor finish solution"]
[null,null,"Floor finish",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N100),MAX($J101:J$101))+1","v":109},null,{"$f":"MAX(MAX($J$1:$N100),MAX($J101:L$101))+1","v":110},null,null,null,{"$f":"INT(MAX(MAX($P$1:$Y100),MAX($P101:P101)))+1.01","v":3.01}]
[]
[null,null,"Description",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N102),MAX($J103:J$103))+1","v":111},null,null,null,null,null,"value",null,"note ref.",null,"value",null,"note ref."]
[null,null,"BS EN 14041:2004 Essential characteristics",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N103),MAX($J104:J$104))+1","v":112},null,{"$f":"MAX(MAX($J$1:$N103),MAX($J104:L$104))+1","v":113},null,null,null,{"$f":"Q101+0.01","v":3.0199999999999996}]
[null,null,"BS EN ISO 10874:2012 durability classification",null,null,null,"European Flooring Use classification ",null,null,null,{"$f":"MAX(MAX($J$1:$N104),MAX($J105:J$105))+1","v":114},null,{"$f":"MAX(MAX($J$1:$N104),MAX($J105:L$105))+1","v":115},null,null,null,{"$f":"Q104+0.01","v":3.0299999999999994}]
[null,null,"BS EN 14904: 2006 Sports floor elasticity",null,null,null,"Area elastic (A3) or point elastic (P3)",null,null,null,{"$f":"MAX(MAX($J$1:$N105),MAX($J106:J$106))+1","v":116},null,{"$f":"MAX(MAX($J$1:$N105),MAX($J106:L$106))+1","v":117},null,null,null,{"$f":"Q105+0.01","v":3.0399999999999991}]
[null,null,"Minimum reflectance ",null,null,null,"0.3 for all habitable rooms",null,null,null,{"$f":"MAX(MAX($J$1:$N106),MAX($J107:J$107))+1","v":118},null,{"$f":"MAX(MAX($J$1:$N106),MAX($J107:L$107))+1","v":119},null,null,null,3.0499999999999989]
[null,null,"Minimum Required Life  (years)",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N107),MAX($J108:J$108))+1","v":120},null,{"$f":"MAX(MAX($J$1:$N107),MAX($J108:L$108))+1","v":121},null,null,null,3.0599999999999987]
[null,null,"Slip Resistance",null,null,null,"(Ramp test rating, or R value)",null,null,null,{"$f":"MAX(MAX($J$1:$N108),MAX($J109:J$109))+1","v":122},null,{"$f":"MAX(MAX($J$1:$N108),MAX($J109:L$109))+1","v":123},null,null,null,3.0699999999999985]
[null,null,"Slip Resistance Value (SRV)",null,null,null,"and surface roughness",null,null,null,{"$f":"MAX(MAX($J$1:$N109),MAX($J110:J$110))+1","v":124},null,{"$f":"MAX(MAX($J$1:$N109),MAX($J110:L$110))+1","v":125},null,null,null,3.0799999999999983]
[null,null,"Water Resistance",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N110),MAX($J111:J$111))+1","v":126},null,{"$f":"MAX(MAX($J$1:$N110),MAX($J111:L$111))+1","v":127},null,null,null,3.0899999999999981]
[null,null,"Fire Performance",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N111),MAX($J112:J$112))+1","v":128},null,{"$f":"MAX(MAX($J$1:$N111),MAX($J112:L$112))+1","v":129},null,null,null,3.0999999999999979]
[null,null,"Hygiene Performance",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N112),MAX($J113:J$113))+1","v":130},null,{"$f":"MAX(MAX($J$1:$N112),MAX($J113:L$113))+1","v":131},null,null,null,3.1099999999999977]
[null,null,"BS EN 14041:2004 Electrostatic rating",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N113),MAX($J114:J$114))+1","v":132},null,{"$f":"MAX(MAX($J$1:$N113),MAX($J114:L$114))+1","v":133},null,null,null,3.1199999999999974]
[null,null,"Chemical Resistance",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N114),MAX($J115:J$115))+1","v":134},null,{"$f":"MAX(MAX($J$1:$N114),MAX($J115:L$115))+1","v":135},null,null,null,3.1299999999999972]
[null,null,"Heat Resistance",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N115),MAX($J116:J$116))+1","v":136},null,{"$f":"MAX(MAX($J$1:$N115),MAX($J116:L$116))+1","v":137},null,null,null,3.139999999999997]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"description of ceiling/ soffit finish solution"]
[null,null,"Ceiling finish",null,"or soffit finish",null,"see technical annexe - ceiling finish",null,null,null,{"$f":"MAX(MAX($J$1:$N117),MAX($J118:J$118))+1","v":138},null,{"$f":"MAX(MAX($J$1:$N117),MAX($J118:L$118))+1","v":139},null,null,null,{"$f":"INT(MAX(MAX($P$1:$Y117),MAX($P118:P118)))+1.01","v":4.01}]
[]
[null,null,"Description",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N119),MAX($J120:J$120))+1","v":140},null,null,null,null,null,"value",null,"note ref.",null,"value",null,"note ref."]
[null,null,"Minimum reflectance ",null,null,null,"0.7 for all habitable rooms",null,null,null,{"$f":"MAX(MAX($J$1:$N120),MAX($J121:J$121))+1","v":141},null,"",null,null,null,{"$f":"Q118+0.01","v":4.0199999999999996}]
[null,null,"Hygrothermal performance",null,null,null,"generally as wall finish below",null,null,null,{"$f":"MAX(MAX($J$1:$N121),MAX($J122:J$122))+1","v":142},null," ",null,null,null,{"$f":"Q121+0.01","v":4.0299999999999994}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"description of wall finish solution"]
[null,null,"Wall finish",null,null,null,"see technical annexe - wall finish",null,null,null,{"$f":"MAX(MAX($J$1:$N123),MAX($J124:J$124))+1","v":143},null,{"$f":"MAX(MAX($J$1:$N123),MAX($J124:L$124))+1","v":144},null,null,null,{"$f":"INT(MAX(MAX($P$1:$Y123),MAX($P124:P124)))+1.01","v":5.01}]
[]
[null,null,"Description",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N125),MAX($J126:J$126))+1","v":145},null,null,null,null,null,"value",null,"note ref.",null,"value",null,"note ref."]
[null,null,"Minimum reflectance ",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N126),MAX($J127:J$127))+1","v":146},null,{"$f":"MAX(MAX($J$1:$N126),MAX($J127:L$127))+1","v":147},null,null,null,{"$f":"Q124+0.01","v":5.0199999999999996}]
[null,null,"Impervious ",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N127),MAX($J128:J$128))+1","v":148},null,{"$f":"MAX(MAX($J$1:$N127),MAX($J128:L$128))+1","v":149},null,null,null,{"$f":"Q127+0.01","v":5.0299999999999994}]
[null,null,"Jointless",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N128),MAX($J129:J$129))+1","v":150},null,{"$f":"MAX(MAX($J$1:$N128),MAX($J129:L$129))+1","v":151},null,null,null,{"$f":"Q128+0.01","v":5.0399999999999991}]
[null,null,"Smooth",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N129),MAX($J130:J$130))+1","v":152},null,{"$f":"MAX(MAX($J$1:$N129),MAX($J130:L$130))+1","v":153},null,null,null,{"$f":"Q129+0.01","v":5.0499999999999989}]
[null,null,"Hygrothermal performance",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N130),MAX($J131:J$131))+1","v":154},null,{"$f":"MAX(MAX($J$1:$N130),MAX($J131:L$131))+1","v":155},null,null,null,{"$f":"Q130+0.01","v":5.0599999999999987}]
[null,null,"Acoustic wall finish and absorbent panels",null,null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N131),MAX($J132:K$132))+1","v":156},null,null,null,null,{"$f":"Q131+0.01","v":5.0699999999999985}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"specific finishes requirements met and additions"]
[null,null,"Specific finishes requirements",null,"incl part-covering, colour or pattern",null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N133),MAX($J134:J$134))+1","v":157}]
[]
[]
[null,"8. Environmental requirements",null,null,null,null,null,null,null,null,"If new / remodel",null,"If refurb / redec'n",null,null,null,"identify if daylight provided",null,null,null,"identify if daylight provided"]
[null,null,"Daylight and lighting requirements",null,null,null,"see technical annexe lighting ",null,null,null,{"$f":"MAX(MAX($J$1:$N137),MAX($J138:J$138))+1","v":158},null,{"$f":"MAX(MAX($J$1:$N137),MAX($J138:L$138))+1","v":159},null,null,null,null,null,"Yes/ No",null,null,null,"Yes/ No"]
[null,null,"Daylighting",null,null,null,null,null,null,null,null,null,null,null,null,null,"lighting system solution"]
[null,null,"Direct daylighting requirement",null,null,null,"required, preferred or not required",null,null,null,{"$f":"MAX(MAX($J$1:$N139),MAX($J140:J$140))+1","v":160},null,{"$f":"MAX(MAX($J$1:$N139),MAX($J140:L$140))+1","v":161},null,null,null,{"$f":"INT(MAX(MAX($P$1:$Y139),MAX($P140:P140)))+1.01","v":6.01}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"value",null,"note ref."]
[null,null,"For new build:                                   Daylight Autonomy",null,"Required in 80% of spaces where daylight required (above)",null,"Percentage of regularly used area that has an illuminance of 300 lux for half of core hours",null,null,null,{"$f":"MAX(MAX($J$1:$N141),MAX($J142:J$142))+1","v":162},null,{"$f":"MAX(MAX($J$1:$N141),MAX($J142:L$142))+1","v":163},null,null,null,{"$f":"Q140+0.01","v":6.02}]
[null,null,"Usable daylight Index, UDI-a ",null,null,null,{"$f":"MAX(MAX($G$1:$H142),MAX($F143:F$143))+1","v":19},null,null,null,{"$f":"MAX(MAX($J$1:$N142),MAX($J143:J$143))+1","v":164},null,{"$f":"MAX(MAX($J$1:$N142),MAX($J143:L$143))+1","v":165},null,null,null,{"$f":"Q142+0.01","v":6.0299999999999994}]
[null,null,"For refurbishment:","Minimum uniformity of daylight ",null,null,"(under diffuse sky) where daylight provided",null,null,null,{"$f":"MAX(MAX($J$1:$N143),MAX($J144:J$144))+1","v":166},null,{"$f":"MAX(MAX($J$1:$N143),MAX($J144:L$144))+1","v":167},null,null,null,{"$f":"Q143+0.01","v":6.0399999999999991}]
[]
[null,null,"Lighting system",null,null,null,null,null,null,null,null,null,null,null,null,null,"value",null,"note ref.",null,"value",null,"note ref."]
[null,null,"Minimum horizontal/ task illuminance (lux)",null,null,null,"maintained average",null,null,null,{"$f":"MAX(MAX($J$1:$N146),MAX($J147:J$147))+1","v":168},null,{"$f":"MAX(MAX($J$1:$N146),MAX($J147:L$147))+1","v":169},null,null,null,{"$f":"Q144+0.01","v":6.0499999999999989}]
[null,null,"Maximum horizontal illuminance (lux)",null,null,null,"maintained average",null,null,null,{"$f":"MAX(MAX($J$1:$N147),MAX($J148:J$148))+1","v":170},null,{"$f":"MAX(MAX($J$1:$N147),MAX($J148:L$148))+1","v":171},null,null,null,{"$f":"Q147+0.01","v":6.0599999999999987}]
[null,null,"Minimum ceiling luminance",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N148),MAX($J149:J$149))+1","v":172},null,{"$f":"MAX(MAX($J$1:$N148),MAX($J149:L$149))+1","v":173},null,null,null,{"$f":"Q148+0.01","v":6.0699999999999985}]
[null,null,"Minimum cylindrical illuminance (lux)",null,null,null,"at head height in teaching and learning spaces",null,null,null,{"$f":"MAX(MAX($J$1:$N149),MAX($J150:J$150))+1","v":174},null,{"$f":"MAX(MAX($J$1:$N149),MAX($J150:L$150))+1","v":175},null,null,null,6.0799999999999983]
[null,null,"Max. CIBSE limiting glare index",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N150),MAX($J151:J$151))+1","v":176},null,{"$f":"MAX(MAX($J$1:$N150),MAX($J151:L$151))+1","v":177},null,null,null,6.0899999999999981]
[null,null,"Modelling Index",null,null,null,{"$f":"MAX(MAX($G$1:$H151),MAX($F152:F$152))+1","v":20},null,null,null,{"$f":"MAX(MAX($J$1:$N151),MAX($J152:J$152))+1","v":178},null,{"$f":"MAX(MAX($J$1:$N151),MAX($J152:L$152))+1","v":179},null,null,null,6.0999999999999979]
[null,null,"Minimum uniformity of artificial lighting",null,null,null,"at task position",null,null,null,{"$f":"MAX(MAX($J$1:$N152),MAX($J153:J$153))+1","v":180},null,{"$f":"MAX(MAX($J$1:$N152),MAX($J153:L$153))+1","v":181},null,null,null,6.1099999999999977]
[null,null,"Min. colour rendering (Ra)",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N153),MAX($J154:J$154))+1","v":182},null,{"$f":"MAX(MAX($J$1:$N153),MAX($J154:L$154))+1","v":183},null,null,null,6.1199999999999974]
[null,null,"Maximum lighting energy units (W/m2.100 lux)",null,null,null,"Contractor to Specify using suggested figures in technical annexe",null,null,null,null,{"$f":"MAX(MAX($J$1:$N154),MAX($J155:K$155))+1","v":184}]
[null,null,"Minimum initial efficacy - Luminaire lumens / circuit watt with allowance for control factors as in Approved Documents in support of Part L ",null,null,null,"(excluding track-mounted and emergency lighting) or higher if Part L changes in 2013.  Contractor to Specify using suggested figures in technical annexe",null,null,null,{"$f":"MAX(MAX($J$1:$N155),MAX($J156:J$156))+1","v":185},{"$f":"MAX(MAX($J$1:$N155),MAX($J156:K$156))+1","v":186},{"$f":"MAX(MAX($J$1:$N155),MAX($J156:L$156))+1","v":187}]
[null,null,"Lighting Energy Numerical Index (LENI) ",null,null,null,"Contractor to specify (CTS) in new build (kWh/m2)",null,null,null,{"$f":"MAX(MAX($J$1:$N156),MAX($J157:J$157))+1","v":188},null,{"$f":"MAX(MAX($J$1:$N156),MAX($J157:L$157))+1","v":189}]
[]
[null,null,"Lighting controls",null,null,null,"d-daylight linking, sw - central manual switching, occ - occupancy, dim - dimming to 10 lux",null,null,null,{"$f":"MAX(MAX($J$1:$N158),MAX($J159:J$159))+1","v":190},null,null,null,null,null,{"$f":"Q154+0.01","v":6.1299999999999972}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"identify any emergency lighting",null,null,null,"identify any emergency lighting"]
[null,null,"Emergency lighting",null,null,null,"If community use or high risk areas",null,null,null,{"$f":"MAX(MAX($J$1:$N160),MAX($J161:J$161))+1","v":191},null,null,null,null,null,{"$f":"Q159+0.01","v":6.139999999999997}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"specific lighting requirements met and additions"]
[null,null,"Specific lighting requirements","over and above those already required",null,null,"notes, including specialist and task lighting  (all occupied spaces shall allow for data screens to be used in a variety of positions without glare)",null,null,null,{"$f":"MAX(MAX($J$1:$N162),MAX($J163:J$163))+1","v":192}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"thermal comfort solution"]
[null,null,"Temperature and thermal comfort",null,null,null,"see technical annexe - temperature T",null,null,null,{"$f":"MAX(MAX($J$1:$N164),MAX($J165:J$165))+1","v":193},null,{"$f":"MAX(MAX($J$1:$N164),MAX($J165:L$165))+1","v":194},null,null,null,{"$f":"INT(MAX(MAX($P$1:$Y164),MAX($P165:P165)))+1","v":7}]
[null,null,"Normal maintained air temperature (1m above floor level at centre of room) (oC)",null,null,null,"to be achieved by heating system in less than 20 minutes after closing any external doors",null,null,null,{"$f":"MAX(MAX($J$1:$N165),MAX($J166:J$166))+1","v":195},null,{"$f":"MAX(MAX($J$1:$N165),MAX($J166:L$166))+1","v":196},null,null,null,{"$f":"Q165+0.01","v":7.01}]
[null,null,"Type of ventilation",null,null,null,"Contractor to specify (CTS): nat vent, mech vent or hybrid",null,null,null,null,{"$f":"MAX(MAX($J$1:$N166),MAX($J$166:K167))+1","v":197}]
[null,null,"Minimum maintained air temperature (oC)",null,null,null,"provided by heating system in heating season, during maximum occupancy (1m above floor level)",null,null,null,{"$f":"MAX(MAX($J$1:$N167),MAX($J168:J$168))+1","v":198},null,{"$f":"MAX(MAX($J$1:$N167),MAX($J168:L$168))+1","v":199},null,null,null,{"$f":"Q166+0.01","v":7.02}]
[null,null,"Maximum maintained air temperature (oC)",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N168),MAX($J169:J$169))+1","v":200},null,{"$f":"MAX(MAX($J$1:$N168),MAX($J169:L$169))+1","v":201},null,null,null,{"$f":"Q168+0.01","v":7.0299999999999994}]
[null,null,"CIBSE summertime overheating criteria:",null,null,null,null,null,null,null,null,null,null,null,null,null,"value",null,"note ref.",null,"value",null,"note ref."]
[null,null,"1. Maximum hours of exceedence",null,null,null,"For new build only. 2 out of 3 of the CIBSE summertime overheating criteria must be met ",null,null,null,{"$f":"MAX(MAX($J$1:$N170),MAX($J171:J$171))+1","v":202},null,{"$f":"MAX(MAX($J$1:$N170),MAX($J171:L$171))+1","v":203},null,null,null,{"$f":"Q169+0.01","v":7.0399999999999991}]
[null,null,"2. maximum daily weighted exceedence",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N171),MAX($J172:J$172))+1","v":204},null,{"$f":"MAX(MAX($J$1:$N171),MAX($J172:L$172))+1","v":205},null,null,null,{"$f":"Q171+0.01","v":7.0499999999999989}]
[null,null,"3. Upper limit temperature: maximum ΔT",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N172),MAX($J173:J$173))+1","v":206},null,{"$f":"MAX(MAX($J$1:$N172),MAX($J173:L$173))+1","v":207},null,null,null,7.0599999999999987]
[null,null,"Maximum hours when air temperature in the space is above 28oC",null,null,null,"In refurbishment and naturally ventilated spaces only",null,null,null,{"$f":"MAX(MAX($J$1:$N173),MAX($J174:J$174))+1","v":208},null,{"$f":"MAX(MAX($J$1:$N173),MAX($J174:L$174))+1","v":209},null,null,null,7.0699999999999985]
[null,null,"Maximum difference between internal air temperature and external air temperature  - oC",null,null,null,"In refurbishment, when external temperature > 20°C, when the spaces are occupied for more than 30 mins",null,null,null,{"$f":"MAX(MAX($J$1:$N174),MAX($J175:J$175))+1","v":210},null,{"$f":"MAX(MAX($J$1:$N174),MAX($J175:L$175))+1","v":211},null,null,null,7.0799999999999983]
[null,null,"Maximum hours outside heating season when air temperature in the space is above 25oC  (oC)",null,null,null,{"$f":"MAX(MAX($G$1:$H175),MAX($F176:F$176))+1","v":21},null,null,null,{"$f":"MAX(MAX($J$1:$N175),MAX($J176:J$176))+1","v":212},null,{"$f":"MAX(MAX($J$1:$N175),MAX($J176:L$176))+1","v":213},null,null,null,7.0899999999999981]
[null,null,"Minimum air temperature of air delivered at 1.4m above floor level in occupied zone  (oC)",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N176),MAX($J177:J$177))+1","v":214},null,{"$f":"MAX(MAX($J$1:$N176),MAX($J177:L$177))+1","v":215},null,null,null,7.0999999999999979]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ventilation system solution"]
[null,null,"Ventilation",null,null,null,"see technical annexe - ventilation  V",null,null,null,{"$f":"MAX(MAX($J$1:$N178),MAX($J179:J$179))+1","v":216},null,{"$f":"MAX(MAX($J$1:$N178),MAX($J179:L$179))+1","v":217},null,null,null,{"$f":"INT(MAX(MAX($P$1:$Y178),MAX($P179:P179)))+1","v":8}]
[null,null,"Operational target for maximum average daily concentration of carbon dioxide (ppm) ",null,"for mechanical ventilation",null,"parts per million (ppm)",null,null,null,{"$f":"MAX(MAX($J$1:$N179),MAX($J180:J$180))+1","v":218},null,{"$f":"MAX(MAX($J$1:$N179),MAX($J180:L$180))+1","v":219},null,null,null,{"$f":"Q179+0.01","v":8.01}]
[null,null,null,null,"for natural ventilation",null,"parts per million (ppm)",null,null,null,{"$f":"MAX(MAX($J$1:$N180),MAX($J181:J$181))+1","v":220},null,{"$f":"MAX(MAX($J$1:$N180),MAX($J181:L$181))+1","v":221},null,null,null,{"$f":"Q180+0.01","v":8.02}]
[null,null,"Maximum carbon dioxide concentration not to be exceeded for more than 20 minutes each day (ppm) ",null,"for mechanical ventilation",null,"parts per million (ppm)",null,null,null,{"$f":"MAX(MAX($J$1:$N181),MAX($J182:J$182))+1","v":222},null,{"$f":"MAX(MAX($J$1:$N181),MAX($J182:L$182))+1","v":223},null,null,null,8.0299999999999994]
[null,null,null,null,"for natural ventilation",null,"parts per million (ppm)",null,null,null,{"$f":"MAX(MAX($J$1:$N182),MAX($J183:J$183))+1","v":224},null,{"$f":"MAX(MAX($J$1:$N182),MAX($J183:L$183))+1","v":225},null,null,null,8.0399999999999991]
[null,null,"Minimum rate of ventilation when occupied",null,null,null,"litres per second per person (l/s/p)",null,null,null,{"$f":"MAX(MAX($J$1:$N183),MAX($J184:J$184))+1","v":226},null,{"$f":"MAX(MAX($J$1:$N183),MAX($J184:L$184))+1","v":227},null,null,null,8.0499999999999989]
[null,null,"Maximum winter time cold air inlet velocity (m/s)",null,null,null,"meters per second during occupation",null,null,null,{"$f":"MAX(MAX($J$1:$N184),MAX($J185:J$185))+1","v":228},null,{"$f":"MAX(MAX($J$1:$N184),MAX($J185:L$185))+1","v":229},null,null,null,8.0599999999999987]
[null,null,"Minimum capability rate of ventilation",null,null,null,"in air changes per hour (ach)",null,null,null,{"$f":"MAX(MAX($J$1:$N185),MAX($J186:J$186))+1","v":230},null,{"$f":"MAX(MAX($J$1:$N185),MAX($J186:L$186))+1","v":231},null,null,null,8.0699999999999985]
[]
[null,null,"Acoustics",null,null,null,"see technical annexe - acoustics  A",null,null,null,{"$f":"MAX(MAX($J$1:$N187),MAX($J188:J$188))+1","v":232},null,{"$f":"MAX(MAX($J$1:$N187),MAX($J188:L$188))+1","v":233},null,null,null,null,"see acoustics report",null,null,"value",null,"note ref."]
[null,null,"Room classification (for airborne sound insulation)",null,"Activity noise level",null,"(Source room) Low/Average/High/Very High",null,null,null,{"$f":"MAX(MAX($J$1:$N188),MAX($J189:J$189))+1","v":234}]
[null,null,null,null,"Noise tolerance",null,"(Receiving room) Low/Medium/High",null,null,null,{"$f":"MAX(MAX($J$1:$N189),MAX($J190:J$190))+1","v":235}]
[null,null,"Minimum Dw (dB) ",null,null,null,"Contractor to specify (CTS) with reference to Acoustic Performance Standards for PSBP",null,null,null,{"$f":"MAX(MAX($J$1:$N190),MAX($J191:J$191))+1","v":236},{"$f":"MAX(MAX($J$1:$N190),MAX($J191:K$191))+1","v":237},{"$f":"MAX(MAX($J$1:$N190),MAX($J191:L$191))+1","v":238}]
[null,null,"Maximum indoor ambient noise level for ventilation to achieve 1500ppm Carbon Dioxide concentration ",null,null,null,{"$f":"MAX(MAX($G$1:$H191),MAX($F192:F$192))+1","v":22},null,null,null,{"$f":"MAX(MAX($J$1:$N191),MAX($J192:J$192))+1","v":239},null,{"$f":"MAX(MAX($J$1:$N191),MAX($J192:L$192))+1","v":240}]
[null,null,"Maximum impact sound pressure from above  ",null,null,null,"sound pressure level L’w ",null,null,null,{"$f":"MAX(MAX($J$1:$N192),MAX($J193:J$193))+1","v":241},null,{"$f":"MAX(MAX($J$1:$N192),MAX($J193:L$193))+1","v":242}]
[null,null,"Either:"]
[null,null,"Minimum composite Rw (dB) of corridor** wall, glazing and ventilators in walls with ventilators ",null,null,null,"Contractor to identify which measure is being used and mark other as N/A",null,null,null,{"$f":"MAX(MAX($J$1:$N194),MAX($J195:J$195))+1","v":243},null,{"$f":"MAX(MAX($J$1:$N194),MAX($J195:L$195))+1","v":244}]
[null,null,"Or:"]
[null,null,"Minimum composite Rw (dB) of corridor** wall and glazing without ventilators ",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N196),MAX($J197:J$197))+1","v":245},null,{"$f":"MAX(MAX($J$1:$N196),MAX($J197:L$197))+1","v":246}]
[null,null,"Minimum Dn,e,w – 10logN dB for ventilators in walls",null,null,null,"Dn,e,w – 10logN3 (dB) where applicable",null,null,null,{"$f":"MAX(MAX($J$1:$N197),MAX($J198:J$198))+1","v":247},null,{"$f":"MAX(MAX($J$1:$N197),MAX($J198:L$198))+1","v":248}]
[]
[null,null,"Reverberation",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N199),MAX($J200:J$200))+1","v":249},null,{"$f":"MAX(MAX($J$1:$N199),MAX($J200:L$200))+1","v":250},null,null,null,"actual reverberation time"]
[null,null,"Maximum reverberation time",null,null,null,"seconds",null,null,null,{"$f":"MAX(MAX($J$1:$N200),MAX($J201:J$201))+1","v":251},null,{"$f":"MAX(MAX($J$1:$N200),MAX($J201:L$201))+1","v":252},null,null,null,{"$f":"INT(MAX(MAX($P$1:$Y200),MAX($P201:P201)))+2.01","v":10.01}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"specific environmental requirements met and additions"]
[null,null,"Specific environmental requirements","(extraction units and fume cupboards covered under fittings, dim out covered under lighting)",null,null,"requirements not covered in environmental headings above, including special exhaust ventilation, surface temp of heat emitters, minimum STI in open plan areas and intermittent ventilation (as Part L Table 6.1a) ",null,null,null,{"$f":"MAX(MAX($J$1:$N202),MAX($J203:J$203))+1","v":253}]
[null,"9. Building services",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"description of building services solutions"]
[null,null,"Gas supply","As described",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N204),MAX($J205:J$205))+1","v":254}]
[null,null,"Specific electrical services requirements","Including specialist power",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N205),MAX($J206:J$206))+1","v":255}]
[null,null,"Specific wet services requirements","(water supply, drainage, sanitary ware and fixtures)",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N206),MAX($J207:J$207))+1","v":256}]
[null,null,"Power sockets",null,null,null,null,null,null,null,null,null,null,null,null,null,"value",null,"note ref.",null,"value",null,"note ref."]
[null,null,null,"Trunking at dado level",null,null,{"$f":"MAX(MAX($G$1:$H208),MAX($F209:F$209))+1","v":23},null,null,null,{"$f":"MAX(MAX($J$1:$N208),MAX($J209:J$210))+1","v":257}]
[null,null,null,"Double Power Socket Total",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N209),MAX($J210:J$210))+1","v":258}]
[null,null,null,"Single Power Socket Total",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N210),MAX($J211:J$211))+1","v":259}]
[null,null,null,"Additional Power (Double Socket)",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N211),MAX($J212:J$212))+1","v":260}]
[null,null,null,"Cleaner's Power (single socket)",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N212),MAX($J$212:J213))+1","v":261}]
[null,null,"Communication and ICT infrastructure"]
[null,null,null,"Voice over Internet Protocol (VoIP)",null,null,"Telephone system using data sockets",null,null,null,{"$f":"MAX(MAX($J$1:$N214),MAX($J215:J$215))+1","v":262}]
[null,null,null,"Wifi AP Data Point",null,null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N215),MAX($J216:J$216))+1","v":263}]
[null,null,null,"Data Points Total",null,null,"As specified in FOS",null,null,null,{"$f":"MAX(MAX($J$1:$N216),MAX($J217:J$217))+1","v":264}]
[null,null,null,"Additional Data",null,null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N217),MAX($J218:J$218))+1","v":265}]
[null,null,null,"TV Signal point - IPTV",null,null,"Central controller or receiver box",null,null,null,{"$f":"MAX(MAX($J$1:$N218),MAX($J219:J$219))+1","v":266}]
[null,null,null,"Projector AV faceplate",null,null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N219),MAX($J220:J$220))+1","v":267}]
[null,null,null,"PA and alarms",null,null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N220),MAX($J$220:J221))+1","v":268}]
[null,"10. Safety and security",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"specific safety and security requirements met and additions"]
[null,null,"Specific requirements",null,null,null,"school to add additional requirements if necessary, including space between F&E",null,null,null,{"$f":"MAX(MAX($J$1:$N222),MAX($J223:J$223))+1","v":269}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"identify if sprinklers provided"]
[null,null,"Sprinklers, where supplied",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N224),MAX($J225:J$225))+1","v":270}]
[]
[]
[null,"11. Fittings, furniture and equipment"]
[null,"Signage",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"specific signage requirements met and additions"]
[null,null,"Specific signage requirements",null,null,null,"Not including doorset signage (covered below)",null,null,null,{"$f":"MAX(MAX($J$1:$N229),MAX($J230:J$230))+1","v":271}]
[]
[null,null,"Nameplate",null,"at entry to space",null,"Description on or adjacent to entrance or door ",null,null,null,{"$f":"MAX(MAX($J$1:$N231),MAX($J232:J$232))+1","v":272},null,null,null,null,null,null,null,"Yes/ No",null,null,null,"Yes/ No"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"identify any fire fighting equipment provided"]
[null,null,"Fire fighting equipment","including fire extinguisher and holder",null,null,"Contractor to specify particular appliances where provided",null,null,null,{"$f":"MAX(MAX($J$1:$N233),MAX($J234:J$234))+1","v":273}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"identify any first aid equipment provided"]
[null,null,"First aid equipment",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N235),MAX($J236:J$236))+1","v":274}]
[null,"Curtains and blinds",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"specific curtain and blind requirements met and additions"]
[null,null,"Specific curtain and blinds requirements",null,null,null,"To internal and external windows and doors only",null,null,null,{"$f":"MAX(MAX($J$1:$N237),MAX($J238:J$238))+1","v":275}]
["ICT equipment",null,null,null,null,null,"Contractor to Specify (CTS) ICT below, based on ICT Solution Summary and discussion with school"]
[null,"Fixed ICT equipment",null,null,null,null,null,null,null,null,"group",null,"quantity",null,null,null,null,null,null,null,"group",null,"quantity"]
[null,null,"Projector",null,"Separate",null,"",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N240),MAX($J241:L$241))+1","v":276}]
[null,null,"",null,"Wall Mounted",null,"",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N241),MAX($J242:L$242))+1","v":277}]
[null,null,"",null,"Ceiling Mounted",null,"",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N242),MAX($J243:L$243))+1","v":278}]
[null,null,"",null,"Theatre",null,"",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N243),MAX($J244:L$244))+1","v":279}]
[null,null,"Interactive Whiteboard",null,"",null,"",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N244),MAX($J245:L$245))+1","v":280}]
[null,null,"Integrated IWB and projector",null,"",null,"",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N245),MAX($J246:L$246))+1","v":281}]
[null,null,"Speakers",null,"",null,"",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N246),MAX($J247:L$247))+1","v":282}]
[null,null,"Digital Display",null,"",null,"(Plasma or LCD)",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N247),MAX($J248:L$248))+1","v":283}]
[null,null,"Electric Screen",null,"",null,"",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N248),MAX($J249:L$249))+1","v":284}]
[null,null,"Sound Field",null,"",null,"",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N249),MAX($J250:L$250))+1","v":285}]
[null,"Loose ICT equipment"]
[null,null,"Projector - Mobile",null,"",null,"",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N251),MAX($J252:L$252))+1","v":286}]
[null,null,"Teacher Laptop/Desktop",null,"",null,"",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N252),MAX($J253:L$253))+1","v":287}]
[null,null,"Computer",null,"Desktop",null,"",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N253),MAX($J254:L$254))+1","v":288}]
[null,null,"",null,"Laptop",null,"",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N254),MAX($J255:L$255))+1","v":289}]
[null,null,"",null,"Netbook",null,"",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N255),MAX($J256:L$256))+1","v":290}]
[null,null,"",null,"Tablet",null,"",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N256),MAX($J257:L$257))+1","v":291}]
[null,null,"Printer",null,"Multi-function Device",null,"",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N257),MAX($J258:L$258))+1","v":292}]
[null,null,"",null,"Workgroup",null,"",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N258),MAX($J259:L$259))+1","v":293}]
[null,null,"",null,"Large Form Factor",null,"",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N259),MAX($J260:L$260))+1","v":294}]
[null,null,"Laptop Trolley",null,"",null,"",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N260),MAX($J261:L$261))+1","v":295}]
[null,null,"Networked Peripheral",null,"Scanner",null,"",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N261),MAX($J262:L$262))+1","v":296}]
[null,null,"",null,"VC Unit",null,"",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N262),MAX($J263:L$263))+1","v":297}]
[null,null,"",null,"Visualiser",null,"",null,null,null,"Gp3",null,{"$f":"MAX(MAX($J$1:$N263),MAX($J264:L$264))+1","v":298}]
["FF&E",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"specific FF&E requirements met and additions"]
[null,null,"Specific FF&E requirements","incl. extraction units and fume cupboards.\n\nFF&E should comply to requirements in FF&E matrix for reference number listed below.",null,null,{"$f":"MAX(MAX($G$1:$H265),MAX($F266:F$266))+1","v":24},null,null,null,{"$f":"MAX(MAX($J$1:$N265),MAX($J266:J$266))+1","v":299}]
[null,"Fittings",null,null,null,null,null,null,null,null,"group",null,"quantity",null,null,null,"group",null,"quantity",null,"group",null,"quantity"]

{"sheet":"(Manual) FFELib","index":5,"n_rows":1837,"n_cols":145,"rows_kept":1837,"cut":false,"hidden":true,"merged":[]}
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACT01","ACT05","ACT22","ADM01","ADM02","ADM03","ADM04","ADM05","ADM06","ADM08","ADM11","ADM13","ADM20","ADM21","CIR00","CIR01","CLA02","CLA12","CLA13","CLA18","CLA31","CLA32","CLA35","CLA41","DAT02","DAT03","DAT04","DAT05","DAT12","DAT15","DAT22","DAT25","DAT28","DAT32","DAT35","DAT43","DAT46","DAT48","DAT49","DIN01","DIN04","DIN05","HAL01","HAL11","HAL12","HAL13","KIT00","KIT01","KIT02","KIT03","KIT04","KIT05","KIT06","KIT07","KIT08","KIT09","LIB01","LIB05","LIB06","OFF00","OFF10","OFF15","OFF20","OFF31","OFF32","OFF33","OFF35","OFF41","OFF42","PER01","PER02","PER04","PER05","PLA01","PLA02","PRA01","PRA11","PRA12","PRI03","PRI04","PRI13","PRI22","PRI23","PRI26","PRI32","PRI33","PRI36","RES00","RES12","RES13","RES14","RES16","RES21","RES22","RES41","SCI02","SCI05","SCI11","SEN01","SEN06","SEN11","SPH00","SPH20","STH00","STH05","STH10","STH20","STN01","STN02","STN04","STN21","STN31","STT03","STT05","STT08","STT10","STT21","STT23","STT32","STT34","STT35","SUP01","TOC01","TOC02","TOC03","TOC04","TOC11","TOC13","TOC15","TOC21","TOC22"]
["ADM01 (Entrance and reception)","ADM01","Fittings","Noticeboard ","(number)","BOA001","Area in SoA x 0.35",null,"Gp2","/=ROUND(K$10*0.35,0)",null,null,null,"APP001",{"$f":"COUNTIFS($B$5:$B$1819,O$4,$F$5:$F$1819,$N5)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Y$4,$F$5:$F$1819,$N5)","v":0},0,1,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AI$4,$F$5:$F$1819,$N5)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AS$4,$F$5:$F$1819,$N5)","v":0},0,0,0,2,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BC$4,$F$5:$F$1819,$N5)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BM$4,$F$5:$F$1819,$N5)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BW$4,$F$5:$F$1819,$N5)","v":0},0,0,1,1,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CG$4,$F$5:$F$1819,$N5)","v":0},0,0,0,0,0,2,2,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CQ$4,$F$5:$F$1819,$N5)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DA$4,$F$5:$F$1819,$N5)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DK$4,$F$5:$F$1819,$N5)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DU$4,$F$5:$F$1819,$N5)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EE$4,$F$5:$F$1819,$N5)","v":0},0,0,0,0,0,0,0,0,0,0]
["ADM01 (Entrance and reception)","ADM01","Fitted Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"APP001X",0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM01 (Entrance and reception)","ADM01","Fitted equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"APP002",0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,1,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM01 (Entrance and reception)","ADM01","Fixed Furniture","Display unit (tall)",null,"DIS01X",null,null,"Gp3",1,null,null,null,"APP002X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM01 (Entrance and reception)","ADM01","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1,null,null,null,"APP003",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM01 (Entrance and reception)","ADM01","Loose Furniture","Upholstered easy chair",null,"CHA200","Area in SoA x 0.75",null,"Gp3","/=ROUND(K$10*0.75,0)",null,null,null,"APP003X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM01 (Entrance and reception)","ADM01","Loose Furniture","Table, Coffee",null,"TAB600",null,null,"Gp3",1,null,null,null,"APP004",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM01 (Entrance and reception)","ADM01","Loose Equipment","Small Bin ",null,"BIN001",null,null,"Gp3",1,null,null,null,"APP004X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0]
["ADM02 (Interview room)","ADM02","Fittings","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"APP005X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0]
["ADM02 (Interview room)","ADM02","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1,null,null,null,"BAR001",1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM02 (Interview room)","ADM02","Fitted equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"BED001",{"$f":"COUNTIFS($B$5:$B$1819,O$4,$F$5:$F$1819,$N15)","v":0},0,0,0,0,0,1,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Y$4,$F$5:$F$1819,$N15)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AI$4,$F$5:$F$1819,$N15)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AS$4,$F$5:$F$1819,$N15)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BC$4,$F$5:$F$1819,$N15)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BM$4,$F$5:$F$1819,$N15)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BW$4,$F$5:$F$1819,$N15)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CG$4,$F$5:$F$1819,$N15)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CQ$4,$F$5:$F$1819,$N15)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DA$4,$F$5:$F$1819,$N15)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DK$4,$F$5:$F$1819,$N15)","v":1},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DU$4,$F$5:$F$1819,$N15)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EE$4,$F$5:$F$1819,$N15)","v":0},0,0,0,0,0,0,0,0,0,0]
["ADM02 (Interview room)","ADM02","Fixed Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"BED002",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM02 (Interview room)","ADM02","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1,null,null,null,"BEN02X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0]
["ADM02 (Interview room)","ADM02","Loose Furniture","Visitors Chair (with arms)/Admin",null,"CHA302",null,null,"Gp3",4,null,null,null,"BIM001",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM02 (Interview room)","ADM02","Loose Furniture","Meeting table, Admin",null,"TAB505",null,null,"Gp3",1,null,null,null,"BIN001",0,0,0,1,1,1,1,1,1,1,1,1,0,1,0,0,1,1,1,1,1,1,1,1,1,1,1,1,1,0,1,1,1,1,1,1,1,1,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,1,1,1,1,1,0,0,1,1,1,0,1,1,1,1,0,0,0,0,0,1,0,1,1,1,0,1,1,0,1,0,0,0,0,0,0,1,1,1,1,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM02 (Interview room)","ADM02","Loose Equipment","Small Bin ",null,"BIN001",null,null,"Gp3",1,null,null,null,"BIN002",0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,1,1,1,1,1,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,1,1,1,1,0,1,1,1,0,1,1,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,1,1,0,0,0,0,0,0,0,0,0,0,0]
["ADM03 (Sick bay)","ADM03","Fittings","No FF&E Listed of This Type",null,null,"Handwash basin included in sanitary package",null,null,null,null,null,null,"BIN003",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM03 (Sick bay)","ADM03","Fitted Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"BOA001",1,1,0,1,0,0,0,1,1,1,0,1,0,1,0,0,1,1,1,1,1,2,1,1,1,1,1,1,1,1,1,1,1,0,0,1,1,1,0,0,0,0,1,0,1,1,0,0,0,1,0,0,0,0,0,0,1,1,1,1,1,0,1,0,0,0,0,0,0,1,1,1,1,0,0,1,0,1,0,0,1,0,0,0,0,0,0,0,1,1,1,1,0,1,0,1,1,1,1,1,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM03 (Sick bay)","ADM03","Fitted equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"BOA002",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,1,1,1,1,0,0,0,0,0,0,0,0,0,0,0,1,0,0,1,1,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM03 (Sick bay)","ADM03","Fixed Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"BOA003",0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM03 (Sick bay)","ADM03","Fixed Equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"BOAW01",{"$f":"COUNTIFS($B$5:$B$1819,O$4,$F$5:$F$1819,$N25)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Y$4,$F$5:$F$1819,$N25)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AI$4,$F$5:$F$1819,$N25)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AS$4,$F$5:$F$1819,$N25)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BC$4,$F$5:$F$1819,$N25)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BM$4,$F$5:$F$1819,$N25)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BW$4,$F$5:$F$1819,$N25)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CG$4,$F$5:$F$1819,$N25)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CQ$4,$F$5:$F$1819,$N25)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DA$4,$F$5:$F$1819,$N25)","v":0},0,0,0,0,0,0,0,1,1,{"$f":"COUNTIFS($B$5:$B$1819,DK$4,$F$5:$F$1819,$N25)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DU$4,$F$5:$F$1819,$N25)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EE$4,$F$5:$F$1819,$N25)","v":0},0,0,0,0,0,0,0,0,0,0]
["ADM03 (Sick bay)","ADM03","Loose Furniture","Upholstered easy chair",null,"CHA200",null,null,"Gp3",2,null,null,null,"BOD01",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM03 (Sick bay)","ADM03","Loose Equipment","Small Bin ",null,"BIN001",null,null,"Gp3",1,null,null,null,"BOD02",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM04 (Sick room)","ADM04","Fittings","No FF&E Listed of This Type",null,null,"Handwash basin included in sanitary package",null,null,null,null,null,null,"BOLW02",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM04 (Sick room)","ADM04","Fitted Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"BOO001",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM04 (Sick room)","ADM04","Fitted equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"BOO002",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM04 (Sick room)","ADM04","Fixed Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"BOTD02",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM04 (Sick room)","ADM04","Fixed Equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"BOW01",0,0,0,0,1,0,0,1,1,1,1,0,0,0,0,0,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,0,1,0,0,0,1,1,1,0,0,0,1,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,1,0,1,1,1,1,0,0,1,0,1,1,0,1,1,1,0,1,1,0,1,0,0,1,0,0,0,0,1,1,1,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,1,1,0,0,0,0,0,0,0,0,0,0,0]
["ADM04 (Sick room)","ADM04","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1,null,null,null,"CAB104",0,0,0,0,0,0,0,1,1,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,1,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM04 (Sick room)","ADM04","Loose Furniture","Medical Bed",null,"BED001",null,null,"Gp3",1,null,null,null,"CAB105",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM04 (Sick room)","ADM04","Loose Furniture","Upholstered easy chair",null,"CHA200",null,null,"Gp3",2,null,null,null,"CHA001",{"$f":"COUNTIFS($B$5:$B$1819,O$4,$F$5:$F$1819,$N35)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Y$4,$F$5:$F$1819,$N35)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AI$4,$F$5:$F$1819,$N35)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AS$4,$F$5:$F$1819,$N35)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BC$4,$F$5:$F$1819,$N35)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BM$4,$F$5:$F$1819,$N35)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BW$4,$F$5:$F$1819,$N35)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CG$4,$F$5:$F$1819,$N35)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CQ$4,$F$5:$F$1819,$N35)","v":1},0,0,0,0,0,0,1,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DA$4,$F$5:$F$1819,$N35)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DK$4,$F$5:$F$1819,$N35)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DU$4,$F$5:$F$1819,$N35)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EE$4,$F$5:$F$1819,$N35)","v":0},0,0,0,0,0,0,0,0,0,0]
["ADM04 (Sick room)","ADM04","Loose Equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"CHA002",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,1,1,1,1,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM05 (General office)","ADM05","Fittings","Noticeboard ",null,"BOA001","As SoA max group size / 2.75",null,"Gp2","/=ROUND(K$14/2.75,0)",null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM05 (General office)","ADM05","Fittings","Reception desk (visitors)",null,"FFE980","1 bespoke, with shelf for wheelchair user",null,"Gp2",1,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM05 (General office)","ADM05","Fittings","Reception desk (pupils/finance)",null,"FFE981","1 bespoke, if 'general office (2 recep desks)'",null,"Gp2","CTS",null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM05 (General office)","ADM05","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM05 (General office)","ADM05","Fitted equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM05 (General office)","ADM05","Fixed Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM05 (General office)","ADM05","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM05 (General office)","ADM05","Loose Furniture","Side filing unit (2 dr)/Admin",null,"CAB104","As SoA max group size / 3",null,"Gp3","/=ROUND(K$14/3,0)",null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM05 (General office)","ADM05","Loose Furniture","Operators chair (with arms)/Admin",null,"CHA303","As SoA max group size",null,"Gp3","/=K$14",null,null,null,null,{"$f":"COUNTIFS($B$5:$B$1819,O$4,$F$5:$F$1819,$N45)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Y$4,$F$5:$F$1819,$N45)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AI$4,$F$5:$F$1819,$N45)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AS$4,$F$5:$F$1819,$N45)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BC$4,$F$5:$F$1819,$N45)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BM$4,$F$5:$F$1819,$N45)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BW$4,$F$5:$F$1819,$N45)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CG$4,$F$5:$F$1819,$N45)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CQ$4,$F$5:$F$1819,$N45)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DA$4,$F$5:$F$1819,$N45)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DK$4,$F$5:$F$1819,$N45)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DU$4,$F$5:$F$1819,$N45)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EE$4,$F$5:$F$1819,$N45)","v":0},0,0,0,0,0,0,0,0,0,0]
["ADM05 (General office)","ADM05","Loose Furniture","Screen (Desk mounted)",null,"SCR003","As SoA max group size / 2",null,"Gp3","/=ROUND(K$14/2,0)",null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM05 (General office)","ADM05","Loose Furniture","Pedestal unit/Admin",null,"STO101","As SoA max group size",null,"Gp3","/=K$14",null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM05 (General office)","ADM05","Loose Furniture","Low tambour unit/Admin",null,"STO101","As SoA max group size / 4",null,"Gp3","/=ROUND(K$14/4,0)",null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM05 (General office)","ADM05","Loose Furniture","Tall tambour unit/Admin",null,"STO102","As SoA max group size / 1.5",null,"Gp3","/=ROUND(K$14/1.5,0)",null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM05 (General office)","ADM05","Loose Furniture","Table, ICT/Admin ",null,"TAB503","As SoA max group size",null,"Gp3","/=K$14",null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM05 (General office)","ADM05","Loose Equipment","Small Bin ",null,"BIN001",null,null,"Gp3",3,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM05 (General office)","ADM05","Loose Equipment","Photocopier",null,"EQ227",null,null,"Gp3",1,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM05 (General office)","ADM05","Loose Equipment","Paper Shredder",null,"EQ228",null,null,"Gp3",1,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM06 (student services office)","ADM06","Fittings","Noticeboard ",null,"BOA001","As SoA max group size / 2.75",null,"Gp2","/=ROUND(K$14/2.75,0)",null,null,null,"CUB001",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,1,1,0,0,0,0,0,0,0,0,0,0,0]
["ADM06 (student services office)","ADM06","Fittings","Reception desk (pupils/finance)",null,"FFE981","Bespoke, with access for wheelchair user",null,"Gp2",1,null,null,null,"CUB002",{"$f":"COUNTIFS($B$5:$B$1819,O$4,$F$5:$F$1819,$N55)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Y$4,$F$5:$F$1819,$N55)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AI$4,$F$5:$F$1819,$N55)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AS$4,$F$5:$F$1819,$N55)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BC$4,$F$5:$F$1819,$N55)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BM$4,$F$5:$F$1819,$N55)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BW$4,$F$5:$F$1819,$N55)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CG$4,$F$5:$F$1819,$N55)","v":0},0,0,0,0,0,0,0,1,0,{"$f":"COUNTIFS($B$5:$B$1819,CQ$4,$F$5:$F$1819,$N55)","v":1},1,1,0,1,1,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DA$4,$F$5:$F$1819,$N55)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DK$4,$F$5:$F$1819,$N55)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DU$4,$F$5:$F$1819,$N55)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EE$4,$F$5:$F$1819,$N55)","v":0},0,0,0,0,0,0,0,0,0,0]
["ADM06 (student services office)","ADM06","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1,null,null,null,"CUB003",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM06 (student services office)","ADM06","Fitted equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"CUB004",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM06 (student services office)","ADM06","Fixed Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"CUB005",0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM06 (student services office)","ADM06","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1,null,null,null,"CUB008",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM06 (student services office)","ADM06","Loose Furniture","Side filing unit (2 dr)/Admin",null,"CAB104","As SoA max group size / 4",null,"Gp3","/=ROUND(K$14/4,0)",null,null,null,"CUB009",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM06 (student services office)","ADM06","Loose Furniture","Operators chair (with arms)/Admin",null,"CHA303","As SoA max group size",null,"Gp3","/=K$14",null,null,null,"CUB011",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM06 (student services office)","ADM06","Loose Furniture","Screen (Desk mounted)",null,"SCR003","As SoA max group size / 2",null,"Gp3","/=ROUND(K$14/2,0)",null,null,null,"CUB012",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,1,1,1,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM06 (student services office)","ADM06","Loose Furniture","Pedestal unit/Admin",null,"STO101","As SoA max group size",null,"Gp3","/=K$14",null,null,null,"CUP001X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM06 (student services office)","ADM06","Loose Furniture","Tall tambour unit/Admin",null,"STO102","As SoA max group size / 1.5",null,"Gp3","/=ROUND(K$14/1.5,0)",null,null,null,"CUP003",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM06 (student services office)","ADM06","Loose Furniture","Table, ICT/Admin ",null,"TAB503","As SoA max group size",null,"Gp3","/=K$14",null,null,null,"CUP004",{"$f":"COUNTIFS($B$5:$B$1819,O$4,$F$5:$F$1819,$N65)","v":0},0,0,0,0,0,0,0,0,1,{"$f":"COUNTIFS($B$5:$B$1819,Y$4,$F$5:$F$1819,$N65)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AI$4,$F$5:$F$1819,$N65)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AS$4,$F$5:$F$1819,$N65)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BC$4,$F$5:$F$1819,$N65)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BM$4,$F$5:$F$1819,$N65)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BW$4,$F$5:$F$1819,$N65)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CG$4,$F$5:$F$1819,$N65)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CQ$4,$F$5:$F$1819,$N65)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DA$4,$F$5:$F$1819,$N65)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DK$4,$F$5:$F$1819,$N65)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DU$4,$F$5:$F$1819,$N65)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EE$4,$F$5:$F$1819,$N65)","v":0},0,0,0,0,0,0,0,0,0,0]
["ADM06 (student services office)","ADM06","Loose Equipment","Small Bin ",null,"BIN001",null,null,"Gp3",3,null,null,null,"CUP006",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM06 (student services office)","ADM06","Loose Equipment","Photocopier",null,"EQ227",null,null,"Gp3",1,null,null,null,"CUP010",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM06 (student services office)","ADM06","Loose Equipment","Paper Shredder",null,"EQ228",null,null,"Gp3",1,null,null,null,"CUP012",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM08 (Reprographics room)","ADM08","Fittings","Noticeboard ",null,"BOA001","Area in SoA x 0.15",null,"Gp2","/=ROUND(K$10*0.15,0)",null,null,null,"CUP013",0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,1,0,0,0,0,0,0,0,0,0,0,0,1,0,1,1,1,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM08 (Reprographics room)","ADM08","Fittings","Worktop 600 deep Solid","(m length)","WKTK600S","Area in SoA x 0.2 + 1",null,"Gp2","/=ROUND(K$10*0.2,1)+1",null,null,null,"CUP014",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM08 (Reprographics room)","ADM08","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1,null,null,null,"CUR001",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM08 (Reprographics room)","ADM08","Fitted Furniture","Cupboard unit (2 doors)",null,"CUP004",null,null,"Gp3",2,null,null,null,"CUR002",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM08 (Reprographics room)","ADM08","Fitted Furniture","Underbench 24 tray unit (w/o doors)",null,"TRU001","Area in SoA x 0.1",null,"Gp3","/=ROUND(K$10*0.1,0)",null,null,null,"DIN001",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM08 (Reprographics room)","ADM08","Fitted Furniture","Shelving (set of 3)","(number)","SHE100","Area in SoA x 0.09",null,"Gp2","/=ROUND(K$10*0.07,0)",null,null,null,"DIN003",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM08 (Reprographics room)","ADM08","Fitted equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"DIN004",{"$f":"COUNTIFS($B$5:$B$1819,O$4,$F$5:$F$1819,$N75)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Y$4,$F$5:$F$1819,$N75)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AI$4,$F$5:$F$1819,$N75)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AS$4,$F$5:$F$1819,$N75)","v":0},0,0,0,0,0,0,0,0,1,{"$f":"COUNTIFS($B$5:$B$1819,BC$4,$F$5:$F$1819,$N75)","v":0},0,0,0,0,1,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BM$4,$F$5:$F$1819,$N75)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BW$4,$F$5:$F$1819,$N75)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CG$4,$F$5:$F$1819,$N75)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CQ$4,$F$5:$F$1819,$N75)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DA$4,$F$5:$F$1819,$N75)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DK$4,$F$5:$F$1819,$N75)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DU$4,$F$5:$F$1819,$N75)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EE$4,$F$5:$F$1819,$N75)","v":0},0,0,0,0,0,0,0,0,0,0]
["ADM08 (Reprographics room)","ADM08","Fixed Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"DIN005",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM08 (Reprographics room)","ADM08","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1,null,null,null,"DIS01X",0,0,0,1,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM08 (Reprographics room)","ADM08","Loose Furniture","ICT staff chair",null,"CHA301","Area in SoA x 0.09",null,"Gp3","/=ROUND(K$10*0.07,0)",null,null,null,"EQ001X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,1,0,0,1,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM08 (Reprographics room)","ADM08","Loose Furniture","Low tambour unit/Admin",null,"STO103","Area in SoA x 0.15",null,"Gp3","/=ROUND(K$10*0.15,0)",null,null,null,"EQ003X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM08 (Reprographics room)","ADM08","Loose Furniture","Table, ICT/Admin ",null,"TAB501","Area in SoA x 0.09",null,"Gp3","/=ROUND(K$10*0.07,0)",null,null,null,"EQ004X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM08 (Reprographics room)","ADM08","Loose Equipment","Small Bin ",null,"BIN001",null,null,"Gp3",1,null,null,null,"EQ005X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM08 (Reprographics room)","ADM08","Loose Equipment","Large Bin ",null,"BIN002",null,null,"Gp3",2,null,null,null,"EQ006X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM08 (Reprographics room)","ADM08","Loose Equipment","Photocopier",null,"EQ227","To be agreed with school. ",null,"Gp3","CTS",null,null,null,"EQ201",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM08 (Reprographics room)","ADM08","Loose Equipment","SS Trolley",null,"TRO001",null,null,"Gp3",1,null,null,null,"EQ202",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM11 (Heads office)","ADM11","Fittings","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"EQ204",{"$f":"COUNTIFS($B$5:$B$1819,O$4,$F$5:$F$1819,$N85)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Y$4,$F$5:$F$1819,$N85)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AI$4,$F$5:$F$1819,$N85)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AS$4,$F$5:$F$1819,$N85)","v":0},0,0,0,0,0,0,1,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BC$4,$F$5:$F$1819,$N85)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BM$4,$F$5:$F$1819,$N85)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BW$4,$F$5:$F$1819,$N85)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CG$4,$F$5:$F$1819,$N85)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CQ$4,$F$5:$F$1819,$N85)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DA$4,$F$5:$F$1819,$N85)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DK$4,$F$5:$F$1819,$N85)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DU$4,$F$5:$F$1819,$N85)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EE$4,$F$5:$F$1819,$N85)","v":0},0,0,0,0,0,0,0,0,0,0]
["ADM11 (Heads office)","ADM11","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1,null,null,null,"EQ205",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM11 (Heads office)","ADM11","Fitted Furniture","Coat hooks (6)",null,"STO001",null,null,"Gp2",1,null,null,null,"EQ213",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM11 (Heads office)","ADM11","Fitted equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"EQ214",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,1,1,1,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM11 (Heads office)","ADM11","Fixed Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"EQ222",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM11 (Heads office)","ADM11","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1,null,null,null,"EQ224",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,1,1,1,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM11 (Heads office)","ADM11","Loose Furniture","Visitors Chair (with arms)/Admin",null,"CHA302","As SoA max group size - 1",null,"Gp3","/=K$14-1",null,null,null,"EQ225",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM11 (Heads office)","ADM11","Loose Furniture","Meeting table/Admin",null,"TAB505","As SoA max group size - 5 / 2",null,"Gp3","/=ROUND((K$14-5)/2,0)",null,null,null,"EQ227",0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM11 (Heads office)","ADM11","Loose Furniture","Meeting table, Semi-circular/Admin",null,"TAB500",null,null,"Gp3",2,null,null,null,"EQ230",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM11 (Heads office)","ADM11","Loose Furniture","Executive chair (with arms)/Admin",null,"CHA304",null,null,"Gp3",1,null,null,null,"EQ233",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM11 (Heads office)","ADM11","Loose Furniture","Tall tambour unit/Admin",null,"STO102",null,null,"Gp3",1,null,null,null,"EQ234",{"$f":"COUNTIFS($B$5:$B$1819,O$4,$F$5:$F$1819,$N95)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Y$4,$F$5:$F$1819,$N95)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AI$4,$F$5:$F$1819,$N95)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AS$4,$F$5:$F$1819,$N95)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BC$4,$F$5:$F$1819,$N95)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BM$4,$F$5:$F$1819,$N95)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BW$4,$F$5:$F$1819,$N95)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CG$4,$F$5:$F$1819,$N95)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CQ$4,$F$5:$F$1819,$N95)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DA$4,$F$5:$F$1819,$N95)","v":0},0,0,1,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DK$4,$F$5:$F$1819,$N95)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DU$4,$F$5:$F$1819,$N95)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EE$4,$F$5:$F$1819,$N95)","v":0},0,0,0,0,0,0,0,0,0,0]
["ADM11 (Heads office)","ADM11","Loose Furniture","Low tambour unit/Admin",null,"STO102",null,null,"Gp3",1,null,null,null,"EQ235",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM11 (Heads office)","ADM11","Loose Furniture","Pedestal unit/Admin",null,"STO103",null,null,"Gp3",1,null,null,null,"EXT001",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM11 (Heads office)","ADM11","Loose Furniture","Table, ICT/Admin ",null,"TAB504",null,null,"Gp3",1,null,null,null,"FFE912",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM11 (Heads office)","ADM11","Loose Equipment","Small Bin ",null,"BIN001",null,null,"Gp3",1,null,null,null,"FFE932",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM13 (Office (PA to head))","ADM13","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1,null,null,null,"FFE934",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM13 (Office (PA to head))","ADM13","Fitted Furniture","Shelving (set of 3)","(number)","SHE100","As SoA max group size",null,"Gp2","/=K$14",null,null,null,"FFE954",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM13 (Office (PA to head))","ADM13","Fitted equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"FFE980",0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM13 (Office (PA to head))","ADM13","Fixed Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"FFE981",0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM13 (Office (PA to head))","ADM13","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1,null,null,null,"FFE987",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0]
["ADM13 (Office (PA to head))","ADM13","Loose Furniture","Side filing unit (2 dr)/Admin",null,"CAB104",null,null,"Gp3",1,null,null,null,"FUM001Ft",{"$f":"COUNTIFS($B$5:$B$1819,O$4,$F$5:$F$1819,$N105)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Y$4,$F$5:$F$1819,$N105)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AI$4,$F$5:$F$1819,$N105)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AS$4,$F$5:$F$1819,$N105)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BC$4,$F$5:$F$1819,$N105)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BM$4,$F$5:$F$1819,$N105)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BW$4,$F$5:$F$1819,$N105)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CG$4,$F$5:$F$1819,$N105)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CQ$4,$F$5:$F$1819,$N105)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DA$4,$F$5:$F$1819,$N105)","v":0},0,0,0,0,1,1,1,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DK$4,$F$5:$F$1819,$N105)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DU$4,$F$5:$F$1819,$N105)","v":0},0,0,0,0,0,1,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EE$4,$F$5:$F$1819,$N105)","v":0},0,0,0,0,0,0,0,0,0,0]
["ADM13 (Office (PA to head))","ADM13","Loose Furniture","ICT staff chair",null,"CHA301","As SoA max group size",null,"Gp3","/=K$14",null,null,null,"FUM002Ft",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM13 (Office (PA to head))","ADM13","Loose Furniture","Pedestal unit/Admin",null,"STO101","As SoA max group size",null,"Gp3","/=K$14",null,null,null,"HOI001",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0]
["ADM13 (Office (PA to head))","ADM13","Loose Furniture","Low tambour unit/Admin",null,"STO103",null,null,"Gp3",2,null,null,null,"KLN001X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM13 (Office (PA to head))","ADM13","Loose Furniture","Table, ICT/Admin ",null,"TAB502","As SoA max group size",null,"Gp3","/=K$14",null,null,null,"LIB03X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM13 (Office (PA to head))","ADM13","Loose Equipment","Small Bin ",null,"BIN001","As SoA max group size",null,"Gp3","/=K$14",null,null,null,"LIB04X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM20 (Kitchenette)","ADM20","Fittings","Worktop (standing)","(m length)","WKTL600","to 1 wall",null,"Gp2",2.4,null,null,null,"LIB05X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM20 (Kitchenette)","ADM20","Fittings","SS sink double drainer",null,"SIN004",null,null,"Gp2",1,null,null,null,"LIG001",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM20 (Kitchenette)","ADM20","Fitted Furniture","Underbench 2 door cupboard",null,"CUB005",null,null,"Gp2",1,null,null,null,"LIG001X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM20 (Kitchenette)","ADM20","Fitted Furniture","Wall cupboard unit (2 doors)",null,"CUP013",null,null,"Gp2",1,null,null,null,"LIG002",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM20 (Kitchenette)","ADM20","Fitted equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"LIG003",{"$f":"COUNTIFS($B$5:$B$1819,O$4,$F$5:$F$1819,$N115)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Y$4,$F$5:$F$1819,$N115)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AI$4,$F$5:$F$1819,$N115)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AS$4,$F$5:$F$1819,$N115)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BC$4,$F$5:$F$1819,$N115)","v":0},0,1,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BM$4,$F$5:$F$1819,$N115)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BW$4,$F$5:$F$1819,$N115)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CG$4,$F$5:$F$1819,$N115)","v":0},1,1,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CQ$4,$F$5:$F$1819,$N115)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DA$4,$F$5:$F$1819,$N115)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DK$4,$F$5:$F$1819,$N115)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DU$4,$F$5:$F$1819,$N115)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EE$4,$F$5:$F$1819,$N115)","v":0},0,0,0,0,0,0,0,0,0,0]
["ADM20 (Kitchenette)","ADM20","Fixed Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"LOC014X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM20 (Kitchenette)","ADM20","Fixed Equipment","Dishwasher",null,"APP001X",null,null,"Gp3",1,null,null,null,"LOC015",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM20 (Kitchenette)","ADM20","Loose Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"MAC001X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM20 (Kitchenette)","ADM20","Loose Equipment","Refrigerator ",null,"APP002",null,null,"Gp3",1,null,null,null,"MAC002X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM20 (Kitchenette)","ADM20","Loose Equipment","Microwave",null,"APP001",null,null,"Gp3",1,null,null,null,"MAC003X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM21 (Community entrance)","ADM21","Fittings","Noticeboard ","(number)","BOA001","Area in SoA x 0.35",null,"Gp2","/=ROUND(K$10*0.35,0)",null,null,null,"MAC004X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM21 (Community entrance)","ADM21","Fitted Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"MAC009X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM21 (Community entrance)","ADM21","Fitted equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"MAC010X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM21 (Community entrance)","ADM21","Fixed Furniture","Display unit (tall)",null,"DIS01X",null,null,null,null,null,null,null,"MAC011X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM21 (Community entrance)","ADM21","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,null,null,null,null,null,"MAC012X",{"$f":"COUNTIFS($B$5:$B$1819,O$4,$F$5:$F$1819,$N125)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Y$4,$F$5:$F$1819,$N125)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AI$4,$F$5:$F$1819,$N125)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AS$4,$F$5:$F$1819,$N125)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BC$4,$F$5:$F$1819,$N125)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BM$4,$F$5:$F$1819,$N125)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BW$4,$F$5:$F$1819,$N125)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CG$4,$F$5:$F$1819,$N125)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CQ$4,$F$5:$F$1819,$N125)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DA$4,$F$5:$F$1819,$N125)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DK$4,$F$5:$F$1819,$N125)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DU$4,$F$5:$F$1819,$N125)","v":0},0,0,0,0,0,0,0,1,0,{"$f":"COUNTIFS($B$5:$B$1819,EE$4,$F$5:$F$1819,$N125)","v":0},0,0,0,0,0,0,0,0,0,0]
["ADM21 (Community entrance)","ADM21","Loose Furniture","Upholstered easy chair",null,"CHA200","Area in SoA x 0.75",null,"Gp3","/=ROUND(K$10*0.75,0)",null,null,null,"MAC014X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM21 (Community entrance)","ADM21","Loose Furniture","Table, Coffee",null,"TAB600",null,null,null,null,null,null,null,"MAC016X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,1,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["ADM21 (Community entrance)","ADM21","Loose Equipment","Small Bin ",null,"BIN001",null,null,null,null,null,null,null,"MAC018X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CIR00 (Circulation)","CIR00","Fittings","Noticeboard ",null,"BOA003","1 per 10m length of corridor",null,"Gp2","CTS",null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CIR00 (Circulation)","CIR00","Fitted Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CIR00 (Circulation)","CIR00","Fitted equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CIR00 (Circulation)","CIR00","Fixed Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CIR00 (Circulation)","CIR00","Fixed Equipment","Clock (Wall mounted)",null,"CLO001X",null,null,"Gp3","CTS",null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CIR00 (Circulation)","CIR00","Loose Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CIR00 (Circulation)","CIR00","Loose Equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CIR01 (Corridor)","CIR01","Fittings","Noticeboard ",null,"BOA003","1 per 10m length of corridor",null,"Gp2","CTS",null,null,null,null,null,{"$f":"COUNTIFS($B$5:$B$1819,P$4,$F$5:$F$1819,$N136)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Z$4,$F$5:$F$1819,$N136)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AJ$4,$F$5:$F$1819,$N136)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AT$4,$F$5:$F$1819,$N136)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BD$4,$F$5:$F$1819,$N136)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BN$4,$F$5:$F$1819,$N136)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BX$4,$F$5:$F$1819,$N136)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CH$4,$F$5:$F$1819,$N136)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CR$4,$F$5:$F$1819,$N136)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DB$4,$F$5:$F$1819,$N136)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DL$4,$F$5:$F$1819,$N136)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DV$4,$F$5:$F$1819,$N136)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EF$4,$F$5:$F$1819,$N136)","v":0},0,0,0,0,0,0,0,0,0]
["CIR01 (Corridor)","CIR01","Fitted Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CIR01 (Corridor)","CIR01","Fitted equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CIR01 (Corridor)","CIR01","Fixed Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CIR01 (Corridor)","CIR01","Fixed Equipment","Clock (Wall mounted)",null,"CLO001X",null,null,"Gp3",1,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CIR01 (Corridor)","CIR01","Loose Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CIR01 (Corridor)","CIR01","Loose Equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["DIN01 (Dining area(s))","DIN01","Fittings","Noticeboard ",null,"BOA002",null,null,"Gp2",1,null,null,null,"RAC005",{"$f":"COUNTIFS($B$5:$B$1819,O$4,$F$5:$F$1819,$N143)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["DIN01 (Dining area(s))","DIN01","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",2,null,null,null,"RAC007",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["DIN01 (Dining area(s))","DIN01","Fitted equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"RP001",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["DIN01 (Dining area(s))","DIN01","Fixed Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"RP002",0,{"$f":"COUNTIFS($B$5:$B$1819,P$4,$F$5:$F$1819,$N146)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Z$4,$F$5:$F$1819,$N146)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AJ$4,$F$5:$F$1819,$N146)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AT$4,$F$5:$F$1819,$N146)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BD$4,$F$5:$F$1819,$N146)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BN$4,$F$5:$F$1819,$N146)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BX$4,$F$5:$F$1819,$N146)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CH$4,$F$5:$F$1819,$N146)","v":0},0,0,0,0,0,0,1,0,1,{"$f":"COUNTIFS($B$5:$B$1819,CR$4,$F$5:$F$1819,$N146)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DB$4,$F$5:$F$1819,$N146)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DL$4,$F$5:$F$1819,$N146)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DV$4,$F$5:$F$1819,$N146)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EF$4,$F$5:$F$1819,$N146)","v":0},0,0,0,0,0,0,0,0,0]
["DIN01 (Dining area(s))","DIN01","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1,null,null,null,"RP003",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["DIN01 (Dining area(s))","DIN01","Loose Furniture","Folding table and 8 stool set*",null,"DIN001","Option 1: as SoA max group size / 8 ",null,"Gp3","CTS",null,null,null,"RP004",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["DIN01 (Dining area(s))","DIN01","Loose Furniture","Classroom chair",null,"CHA004","Option 2: as SoA max group size",null,"Gp3","/=K14",null,null,null,"RP005",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["DIN01 (Dining area(s))","DIN01","Loose Furniture","Circular folding tilting top table*",null,"DIN004","Option 2: as SoA max group size / 4 , and",null,"Gp3","/=ROUND(K$14/4,0)",null,null,null,"RP007",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["DIN01 (Dining area(s))","DIN01","Loose Equipment","Large Bin ",null,"BIN002","As SoA max group size / 40",null,"Gp3","/=ROUND(K$14/40,0)",null,null,null,"SAF002X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT00 (School kitchen prep & s)","KIT00","Fittings","Contractor to list FF&E of this type",null,"CTS001",null,null,"Gp2","CTS",null,null,null,"SAF003X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT00 (School kitchen prep & s)","KIT00","Fitted Furniture","Contractor to list FF&E of this type",null,"CTS002",null,null,"Gp2","CTS",null,null,null,"SCR001",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT00 (School kitchen prep & s)","KIT00","Fitted equipment","Contractor to list FF&E of this type",null,"CTS003",null,null,"Gp2","CTS",null,null,null,"SCR002",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,1,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT00 (School kitchen prep & s)","KIT00","Fixed Furniture","Contractor to list FF&E of this type",null,"CTS004",null,null,"Gp2","CTS",null,null,null,"SCR003",0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT00 (School kitchen prep & s)","KIT00","Fixed Equipment","Contractor to list FF&E of this type",null,"CTS005",null,null,"Gp2","CTS",null,null,null,"SHE010",0,{"$f":"COUNTIFS($B$5:$B$1819,P$4,$F$5:$F$1819,$N156)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Z$4,$F$5:$F$1819,$N156)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AJ$4,$F$5:$F$1819,$N156)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AT$4,$F$5:$F$1819,$N156)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BD$4,$F$5:$F$1819,$N156)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BN$4,$F$5:$F$1819,$N156)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BX$4,$F$5:$F$1819,$N156)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CH$4,$F$5:$F$1819,$N156)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CR$4,$F$5:$F$1819,$N156)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DB$4,$F$5:$F$1819,$N156)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DL$4,$F$5:$F$1819,$N156)","v":0},0,0,0,0,0,0,0,0,1,{"$f":"COUNTIFS($B$5:$B$1819,DV$4,$F$5:$F$1819,$N156)","v":0},0,1,1,1,0,0,0,0,1,{"$f":"COUNTIFS($B$5:$B$1819,EF$4,$F$5:$F$1819,$N156)","v":0},0,0,0,0,0,0,0,0,0]
["KIT00 (School kitchen prep & s)","KIT00","Loose Furniture","Contractor to list FF&E of this type",null,"CTS006",null,null,"Gp2","CTS",null,null,null,"SHE020",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,0,0,0]
["KIT00 (School kitchen prep & s)","KIT00","Loose Equipment","Contractor to list FF&E of this type",null,"CTS007",null,null,"Gp2","CTS",null,null,null,"SHE030",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT01 (School kitchen prepa...","KIT01","Fittings","Contractor to list FF&E of this type",null,"CTS001","based on discussion with school",null,"Gp2","CTS",null,null,null,"SHE040",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT01 (School kitchen prepa...","KIT01","Fitted Furniture","Contractor to list FF&E of this type",null,"CTS002","based on discussion with school",null,"Gp2","CTS",null,null,null,"SHE100",0,0,0,0,0,0,0,0,0,1,0,1,0,0,0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,1,1,1,1,0,1,1,1,1,0,0,0,1,0,1,1,0,1,1,1,0,1,1,0,0,0,0,0,0,0,1,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,1,1,0,0,0,0,0,0,0,0,0,0,0]
["KIT01 (School kitchen prepa...","KIT01","Fitted equipment","Contractor to list FF&E of this type",null,"CTS003","based on discussion with school",null,"Gp2","CTS",null,null,null,"SIN001",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT01 (School kitchen prepa...","KIT01","Fixed Furniture","Contractor to list FF&E of this type",null,"CTS004","based on legacy FF&E and discussion with school",null,"Gp2","CTS",null,null,null,"SIN002",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT01 (School kitchen prepa...","KIT01","Fixed Equipment","Contractor to list FF&E of this type",null,"CTS005","based on legacy FF&E and discussion with school",null,"Gp2","CTS",null,null,null,"SIN003",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0]
["KIT01 (School kitchen prepa...","KIT01","Loose Furniture","Contractor to list FF&E of this type",null,"CTS006","based on legacy FF&E and discussion with school",null,"Gp2","CTS",null,null,null,"SIN004",0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,1,0,0,0,0,0,0,0,0,0,1,1,1,0,1,0,1,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT01 (School kitchen prepa...","KIT01","Loose Equipment","Contractor to list FF&E of this type",null,"CTS007","based on legacy FF&E and discussion with school",null,"Gp2","CTS",null,null,null,"SIN005",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT02 (School kitchen serve...","KIT02","Fittings","Contractor to list FF&E of this type",null,"CTS001","based on discussion with school",null,"Gp2","CTS",null,null,null,"SIN006",0,{"$f":"COUNTIFS($B$5:$B$1819,P$4,$F$5:$F$1819,$N166)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Z$4,$F$5:$F$1819,$N166)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AJ$4,$F$5:$F$1819,$N166)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AT$4,$F$5:$F$1819,$N166)","v":0},0,0,1,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BD$4,$F$5:$F$1819,$N166)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BN$4,$F$5:$F$1819,$N166)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BX$4,$F$5:$F$1819,$N166)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CH$4,$F$5:$F$1819,$N166)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CR$4,$F$5:$F$1819,$N166)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DB$4,$F$5:$F$1819,$N166)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DL$4,$F$5:$F$1819,$N166)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DV$4,$F$5:$F$1819,$N166)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EF$4,$F$5:$F$1819,$N166)","v":0},0,0,0,0,0,0,0,0,0]
["KIT02 (School kitchen serve...","KIT02","Fitted Furniture","Contractor to list FF&E of this type",null,"CTS002","based on discussion with school",null,"Gp2","CTS",null,null,null,"SIN007",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT02 (School kitchen serve...","KIT02","Fitted equipment","Contractor to list FF&E of this type",null,"CTS003","based on discussion with school",null,"Gp2","CTS",null,null,null,"SIN008",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT02 (School kitchen serve...","KIT02","Fixed Furniture","Contractor to list FF&E of this type",null,"CTS004","based on legacy FF&E and discussion with school",null,"Gp2","CTS",null,null,null,"SIN009",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT02 (School kitchen serve...","KIT02","Fixed Equipment","Contractor to list FF&E of this type",null,"CTS005","based on legacy FF&E and discussion with school",null,"Gp2","CTS",null,null,null,"SPO001",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT02 (School kitchen serve...","KIT02","Loose Furniture","Contractor to list FF&E of this type",null,"CTS006","based on legacy FF&E and discussion with school",null,"Gp2","CTS",null,null,null,"SPO002",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT02 (School kitchen serve...","KIT02","Loose Equipment","Contractor to list FF&E of this type",null,"CTS007","based on legacy FF&E and discussion with school",null,"Gp2","CTS",null,null,null,"SPO003",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT03 (School kitchen office)","KIT03","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1,null,null,null,"SPO004",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT03 (School kitchen office)","KIT03","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1,null,null,null,"SPO005",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT03 (School kitchen office)","KIT03","Fitted equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"SPO006",{"$f":"COUNTIFS($B$5:$B$1819,O$4,$F$5:$F$1819,$N175)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT03 (School kitchen office)","KIT03","Fixed Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"SPO010",0,{"$f":"COUNTIFS($B$5:$B$1819,P$4,$F$5:$F$1819,$N176)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Z$4,$F$5:$F$1819,$N176)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AJ$4,$F$5:$F$1819,$N176)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AT$4,$F$5:$F$1819,$N176)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BD$4,$F$5:$F$1819,$N176)","v":0},0,0,0,1,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BN$4,$F$5:$F$1819,$N176)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BX$4,$F$5:$F$1819,$N176)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CH$4,$F$5:$F$1819,$N176)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CR$4,$F$5:$F$1819,$N176)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DB$4,$F$5:$F$1819,$N176)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DL$4,$F$5:$F$1819,$N176)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DV$4,$F$5:$F$1819,$N176)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EF$4,$F$5:$F$1819,$N176)","v":0},0,0,0,0,0,0,0,0,0]
["KIT03 (School kitchen office)","KIT03","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp2",1,null,null,null,"SPO011",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT03 (School kitchen office)","KIT03","Loose Furniture","Operators chair (with arms)/Admin",null,"CHA303",null,null,"Gp2",1,null,null,null,"SPO012",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT03 (School kitchen office)","KIT03","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp 2",1,null,null,null,"SPO013",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT03 (School kitchen office)","KIT03","Loose Furniture","Table, ICT/Admin ",null,"TAB501",null,null,"Gp 2",1,null,null,null,"SPO014",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT03 (School kitchen office)","KIT03","Loose Equipment","Small Bin ",null,"BIN001",null,null,"Gp2",1,null,null,null,"SPO015",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT04 (School kitchen staff","KIT04","Fittings","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT04 (School kitchen staff","KIT04","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT04 (School kitchen staff","KIT04","Fitted Furniture","Locker two person workwear ",null,"LOC015X","As SoA max group size / 2 ,",null,"Gp 2","/=ROUND(K$14/2,0)",null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT04 (School kitchen staff","KIT04","Fitted equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT04 (School kitchen staff","KIT04","Fixed Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,null,0,{"$f":"COUNTIFS($B$5:$B$1819,P$4,$F$5:$F$1819,$N186)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Z$4,$F$5:$F$1819,$N186)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AJ$4,$F$5:$F$1819,$N186)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AT$4,$F$5:$F$1819,$N186)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BD$4,$F$5:$F$1819,$N186)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BN$4,$F$5:$F$1819,$N186)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BX$4,$F$5:$F$1819,$N186)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CH$4,$F$5:$F$1819,$N186)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CR$4,$F$5:$F$1819,$N186)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DB$4,$F$5:$F$1819,$N186)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DL$4,$F$5:$F$1819,$N186)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DV$4,$F$5:$F$1819,$N186)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EF$4,$F$5:$F$1819,$N186)","v":0},0,0,0,0,0,0,0,0,0]
["KIT04 (School kitchen staff","KIT04","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp2",1,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT04 (School kitchen staff","KIT04","Loose Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT04 (School kitchen staff","KIT04","Loose Equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT05 (School kitchen store)","KIT05","Fittings","Contractor to list FF&E of this type",null,"CTS001",null,null,"Gp2","CTS",null,null,null,"SPO025",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT05 (School kitchen store)","KIT05","Fitted Furniture","Contractor to list FF&E of this type",null,"CTS002",null,null,"Gp2","CTS",null,null,null,"SPO027",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT05 (School kitchen store)","KIT05","Fitted equipment","Contractor to list FF&E of this type",null,"CTS003",null,null,"Gp2","CTS",null,null,null,"SPO028",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT05 (School kitchen store)","KIT05","Fixed Furniture","Contractor to list FF&E of this type",null,"CTS004",null,null,"Gp2","CTS",null,null,null,"SPO029",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT05 (School kitchen store)","KIT05","Fixed Equipment","Contractor to list FF&E of this type",null,"CTS005",null,null,"Gp2","CTS",null,null,null,"SPO030",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT05 (School kitchen store)","KIT05","Loose Furniture","Contractor to list FF&E of this type",null,"CTS006",null,null,"Gp2","CTS",null,null,null,"SPO032",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT05 (School kitchen store)","KIT05","Loose Equipment","Contractor to list FF&E of this type",null,"CTS007",null,null,"Gp3","CTS",null,null,null,"SPO033",0,{"$f":"COUNTIFS($B$5:$B$1819,P$4,$F$5:$F$1819,$N196)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Z$4,$F$5:$F$1819,$N196)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AJ$4,$F$5:$F$1819,$N196)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AT$4,$F$5:$F$1819,$N196)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BD$4,$F$5:$F$1819,$N196)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BN$4,$F$5:$F$1819,$N196)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BX$4,$F$5:$F$1819,$N196)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CH$4,$F$5:$F$1819,$N196)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CR$4,$F$5:$F$1819,$N196)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DB$4,$F$5:$F$1819,$N196)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DL$4,$F$5:$F$1819,$N196)","v":1},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DV$4,$F$5:$F$1819,$N196)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EF$4,$F$5:$F$1819,$N196)","v":0},0,0,0,0,0,0,0,0,0]
["KIT06 (School kitchen dry s...","KIT06","Fittings","Contractor to list FF&E of this type",null,"CTS001","based on discussion with school",null,"Gp2","CTS",null,null,null,"SPO034",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT06 (School kitchen dry s...","KIT06","Fitted Furniture","Contractor to list FF&E of this type",null,"CTS002","based on discussion with school",null,"Gp2","CTS",null,null,null,"SPO035",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT06 (School kitchen dry s...","KIT06","Fitted equipment","Contractor to list FF&E of this type",null,"CTS003","based on discussion with school",null,"Gp2","CTS",null,null,null,"SPO036",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT06 (School kitchen dry s...","KIT06","Fixed Furniture","Contractor to list FF&E of this type",null,"CTS004","based on legacy FF&E and discussion with school",null,"Gp2","CTS",null,null,null,"SPO037",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT06 (School kitchen dry s...","KIT06","Fixed Equipment","Contractor to list FF&E of this type",null,"CTS005","based on legacy FF&E and discussion with school",null,"Gp2","CTS",null,null,null,"SPO038",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT06 (School kitchen dry s...","KIT06","Loose Furniture","Contractor to list FF&E of this type",null,"CTS006","based on legacy FF&E and discussion with school",null,"Gp2","CTS",null,null,null,"SPO039",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT06 (School kitchen dry s...","KIT06","Loose Equipment","Contractor to list FF&E of this type",null,"CTS007","based on legacy FF&E and discussion with school",null,"Gp2","CTS",null,null,null,"SPO040",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT07 (School kitchen cold ...","KIT07","Fittings","Contractor to list FF&E of this type",null,"CTS001","based on discussion with school",null,"Gp2","CTS",null,null,null,"STO001",0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT07 (School kitchen cold ...","KIT07","Fitted Furniture","Contractor to list FF&E of this type",null,"CTS002","based on discussion with school",null,"Gp2","CTS",null,null,null,"STO002",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT07 (School kitchen cold ...","KIT07","Fitted equipment","Contractor to list FF&E of this type",null,"CTS003","based on discussion with school",null,"Gp2","CTS",null,null,null,"STO011",0,{"$f":"COUNTIFS($B$5:$B$1819,P$4,$F$5:$F$1819,$N206)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Z$4,$F$5:$F$1819,$N206)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AJ$4,$F$5:$F$1819,$N206)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AT$4,$F$5:$F$1819,$N206)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BD$4,$F$5:$F$1819,$N206)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BN$4,$F$5:$F$1819,$N206)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BX$4,$F$5:$F$1819,$N206)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CH$4,$F$5:$F$1819,$N206)","v":0},0,0,0,0,0,0,1,0,1,{"$f":"COUNTIFS($B$5:$B$1819,CR$4,$F$5:$F$1819,$N206)","v":0},1,0,1,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DB$4,$F$5:$F$1819,$N206)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DL$4,$F$5:$F$1819,$N206)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DV$4,$F$5:$F$1819,$N206)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EF$4,$F$5:$F$1819,$N206)","v":0},0,0,0,0,0,0,0,0,0]
["KIT07 (School kitchen cold ...","KIT07","Fixed Furniture","Contractor to list FF&E of this type",null,"CTS004","based on legacy FF&E and discussion with school",null,"Gp2","CTS",null,null,null,"STO01X",{"$f":"COUNTIFS($B$5:$B$1819,O$4,$F$5:$F$1819,$N207)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT07 (School kitchen cold ...","KIT07","Fixed Equipment","Contractor to list FF&E of this type",null,"CTS005","based on legacy FF&E and discussion with school",null,"Gp2","CTS",null,null,null,"STO02X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT07 (School kitchen cold ...","KIT07","Loose Furniture","Contractor to list FF&E of this type",null,"CTS006","based on legacy FF&E and discussion with school",null,"Gp2","CTS",null,null,null,"STO03X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT07 (School kitchen cold ...","KIT07","Loose Equipment","Contractor to list FF&E of this type",null,"CTS007","based on legacy FF&E and discussion with school",null,"Gp2","CTS",null,null,null,"STO05X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,1,0,0,0,0,0,0,1,0,1,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT08 (School kitchen freez...","KIT08","Fittings","Contractor to list FF&E of this type",null,"CTS001","based on discussion with school",null,"Gp2","CTS",null,null,null,"STO06X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT08 (School kitchen freez...","KIT08","Fitted Furniture","Contractor to list FF&E of this type",null,"CTS002","based on discussion with school",null,"Gp2","CTS",null,null,null,"STO07X",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT08 (School kitchen freez...","KIT08","Fitted equipment","Contractor to list FF&E of this type",null,"CTS003","based on discussion with school",null,"Gp2","CTS",null,null,null,"STO101",0,0,0,0,0,0,0,2,1,0,0,1,0,0,0,0,1,1,1,1,1,1,1,1,1,1,1,1,0,1,1,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,1,1,1,1,0,0,1,1,0,0,1,1,1,0,0,0,0,0,0,0,0,1,1,1,0,1,1,0,0,0,0,0,0,0,0,0,1,1,1,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,1,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT08 (School kitchen freez...","KIT08","Fixed Furniture","Contractor to list FF&E of this type",null,"CTS004","based on legacy FF&E and discussion with school",null,"Gp2","CTS",null,null,null,"STO102",0,0,0,0,0,0,0,1,1,0,2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT08 (School kitchen freez...","KIT08","Fixed Equipment","Contractor to list FF&E of this type",null,"CTS005","based on legacy FF&E and discussion with school",null,"Gp2","CTS",null,null,null,"STO103",0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT08 (School kitchen freez...","KIT08","Loose Furniture","Contractor to list FF&E of this type",null,"CTS006","based on legacy FF&E and discussion with school",null,"Gp2","CTS",null,null,null,"TAB001",0,{"$f":"COUNTIFS($B$5:$B$1819,P$4,$F$5:$F$1819,$N216)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Z$4,$F$5:$F$1819,$N216)","v":0},0,0,0,0,1,1,1,1,0,{"$f":"COUNTIFS($B$5:$B$1819,AJ$4,$F$5:$F$1819,$N216)","v":0},0,1,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AT$4,$F$5:$F$1819,$N216)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BD$4,$F$5:$F$1819,$N216)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BN$4,$F$5:$F$1819,$N216)","v":0},0,0,0,0,0,1,1,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BX$4,$F$5:$F$1819,$N216)","v":0},0,1,0,0,0,0,0,1,1,{"$f":"COUNTIFS($B$5:$B$1819,CH$4,$F$5:$F$1819,$N216)","v":1},0,0,0,1,1,1,0,0,1,{"$f":"COUNTIFS($B$5:$B$1819,CR$4,$F$5:$F$1819,$N216)","v":1},1,0,1,1,0,1,1,1,0,{"$f":"COUNTIFS($B$5:$B$1819,DB$4,$F$5:$F$1819,$N216)","v":0},0,1,0,0,0,0,1,1,0,{"$f":"COUNTIFS($B$5:$B$1819,DL$4,$F$5:$F$1819,$N216)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DV$4,$F$5:$F$1819,$N216)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EF$4,$F$5:$F$1819,$N216)","v":0},0,0,0,0,0,0,0,0,0]
["KIT08 (School kitchen freez...","KIT08","Loose Equipment","Contractor to list FF&E of this type",null,"CTS007","based on legacy FF&E and discussion with school",null,"Gp2","CTS",null,null,null,"TAB002",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,1,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT09 (School kitchen toile...","KIT09","Fittings","Contractor to list FF&E of this type",null,"CTS001","based on discussion with school",null,"Gp 2","CTS",null,null,null,"TAB003",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,0,1,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT09 (School kitchen toile...","KIT09","Fitted Furniture","Contractor to list FF&E of this type",null,"CTS002","based on discussion with school",null,"Gp 2","CTS",null,null,null,"TAB004",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT09 (School kitchen toile...","KIT09","Fitted equipment","Contractor to list FF&E of this type",null,"CTS003","based on discussion with school",null,"Gp 2","CTS",null,null,null,"TAB010",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT09 (School kitchen toile...","KIT09","Fixed Furniture","Contractor to list FF&E of this type",null,"CTS004","based on legacy FF&E and discussion with school",null,"Gp 2","CTS",null,null,null,"TAB01E",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT09 (School kitchen toile...","KIT09","Fixed Equipment","Contractor to list FF&E of this type",null,"CTS005","based on legacy FF&E and discussion with school",null,"Gp 2","CTS",null,null,null,"TAB01R",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT09 (School kitchen toile...","KIT09","Loose Furniture","Contractor to list FF&E of this type",null,"CTS006","based on legacy FF&E and discussion with school",null,"Gp 2","CTS",null,null,null,"TAB01SC",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KIT09 (School kitchen toile...","KIT09","Loose Equipment","Contractor to list FF&E of this type",null,"CTS007","based on legacy FF&E and discussion with school",null,"Gp 2","CTS",null,null,null,"TAB01TZ",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF00 (Office only)","OFF00","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1,null,null,null,"TAB02R",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,1,1,1,1,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF00 (Office only)","OFF00","Fitted Furniture","Shelving (set of 3)","(number)","SHE100","As SoA max group size",null,"Gp2","/=K$14",null,null,null,"TAB02SC",0,{"$f":"COUNTIFS($B$5:$B$1819,P$4,$F$5:$F$1819,$N226)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Z$4,$F$5:$F$1819,$N226)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AJ$4,$F$5:$F$1819,$N226)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AT$4,$F$5:$F$1819,$N226)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BD$4,$F$5:$F$1819,$N226)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BN$4,$F$5:$F$1819,$N226)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BX$4,$F$5:$F$1819,$N226)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CH$4,$F$5:$F$1819,$N226)","v":0},0,0,0,0,0,1,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CR$4,$F$5:$F$1819,$N226)","v":0},0,0,0,0,1,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DB$4,$F$5:$F$1819,$N226)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DL$4,$F$5:$F$1819,$N226)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DV$4,$F$5:$F$1819,$N226)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EF$4,$F$5:$F$1819,$N226)","v":0},0,0,0,0,0,0,0,0,0]
["OFF00 (Office only)","OFF00","Fitted equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"TAB02TZ",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,1,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF00 (Office only)","OFF00","Fixed Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"TAB03R",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,1,0,0,0,1,0,3,0,0,0,0,0,0,0,0,0,0,2,2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF00 (Office only)","OFF00","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1,null,null,null,"TAB03SC",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF00 (Office only)","OFF00","Loose Furniture","Side filing unit (2 dr)/Admin",null,"CAB104",null,null,"Gp3",1,null,null,null,"TAB03TZ",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF00 (Office only)","OFF00","Loose Furniture","ICT staff chair",null,"CHA301","As SoA max group size",null,"Gp3","/=K$14",null,null,null,"TAB04R",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF00 (Office only)","OFF00","Loose Furniture","Pedestal unit/Admin",null,"STO101","As SoA max group size",null,"Gp3","/=K$14",null,null,null,"TAB05TZ",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF00 (Office only)","OFF00","Loose Furniture","Low tambour unit/Admin",null,"STO103",null,null,"Gp3",2,null,null,null,"TAB06R",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,1,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,1,0,0,0,0,0,1,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF00 (Office only)","OFF00","Loose Furniture","Table, ICT/Admin ",null,"TAB502","As SoA max group size",null,"Gp3","/=K$14",null,null,null,"TAB06R/TAB01SC",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF00 (Office only)","OFF00","Loose Equipment","Small Bin ",null,"BIN001","As SoA max group size",null,"Gp3","/=K$14",null,null,null,"TAB100",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF10 (Office and meeting)","OFF10","Fittings","Noticeboard ",null,"BOA001","As SoA max group size / 3",null,"Gp2","/=ROUND(K$14/3,0)",null,null,null,"TAB101",0,{"$f":"COUNTIFS($B$5:$B$1819,P$4,$F$5:$F$1819,$N236)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Z$4,$F$5:$F$1819,$N236)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AJ$4,$F$5:$F$1819,$N236)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AT$4,$F$5:$F$1819,$N236)","v":0},0,0,1,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BD$4,$F$5:$F$1819,$N236)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BN$4,$F$5:$F$1819,$N236)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BX$4,$F$5:$F$1819,$N236)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CH$4,$F$5:$F$1819,$N236)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CR$4,$F$5:$F$1819,$N236)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DB$4,$F$5:$F$1819,$N236)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DL$4,$F$5:$F$1819,$N236)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DV$4,$F$5:$F$1819,$N236)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EF$4,$F$5:$F$1819,$N236)","v":0},0,0,0,0,0,0,0,0,0]
["OFF10 (Office and meeting)","OFF10","Fitted Furniture","Shelving (set of 3)",null,"SHE100","As SoA max group size / 2",null,"Gp2","/=ROUND(K$14/2,0)",null,null,null,"TAB102",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF10 (Office and meeting)","OFF10","Fitted equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"TAB200S",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF10 (Office and meeting)","OFF10","Fixed Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"TAB201",{"$f":"COUNTIFS($B$5:$B$1819,O$4,$F$5:$F$1819,$N239)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF10 (Office and meeting)","OFF10","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1,null,null,null,"TAB201S",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF10 (Office and meeting)","OFF10","Loose Furniture","Visitors Chair (with arms)/Admin",null,"CHA302","As SoA max group size / 2 rounded up",null,"Gp3","/=ROUNDUP(K$14/2,0)",null,null,null,"TAB203",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF10 (Office and meeting)","OFF10","Loose Furniture","Operators chair (with arms)/Admin",null,"CHA303","As SoA max group size / 2 rounded down",null,"Gp3","/=ROUNDDOWN(K$14/2,0)",null,null,null,"TAB204",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF10 (Office and meeting)","OFF10","Loose Furniture","Side filing unit (2 dr)/Admin",null,"CAB104",null,null,"Gp3",1,null,null,null,"TAB205",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF10 (Office and meeting)","OFF10","Loose Furniture","Pedestal unit/Admin",null,"STO101","As SoA max group size / 2 rounded down",null,"Gp3","/=ROUNDDOWN(K$14/2,0)",null,null,null,"TAB206",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF10 (Office and meeting)","OFF10","Loose Furniture","Low tambour unit/Admin",null,"STO103","1 in 1 person office only",null,"Gp3","/=IF(K14>3,0,1)",null,null,null,"TAB208",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF10 (Office and meeting)","OFF10","Loose Furniture","Table, ICT/Admin ",null,"TAB502","As SoA max group size / 2 rounded down",null,"Gp3","/=ROUNDDOWN(K$14/2,0)",null,null,null,"TAB210",0,{"$f":"COUNTIFS($B$5:$B$1819,P$4,$F$5:$F$1819,$N246)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Z$4,$F$5:$F$1819,$N246)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AJ$4,$F$5:$F$1819,$N246)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AT$4,$F$5:$F$1819,$N246)","v":0},0,0,0,1,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BD$4,$F$5:$F$1819,$N246)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BN$4,$F$5:$F$1819,$N246)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BX$4,$F$5:$F$1819,$N246)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CH$4,$F$5:$F$1819,$N246)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CR$4,$F$5:$F$1819,$N246)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DB$4,$F$5:$F$1819,$N246)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DL$4,$F$5:$F$1819,$N246)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DV$4,$F$5:$F$1819,$N246)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EF$4,$F$5:$F$1819,$N246)","v":0},0,0,0,0,0,0,0,0,0]
["OFF10 (Office and meeting)","OFF10","Loose Furniture","Meeting table/Admin",null,"TAB506","As SoA max group size / 6 rounded up",null,"Gp3","/=ROUNDUP(K$14/6,0)",null,null,null,"TAB310",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF10 (Office and meeting)","OFF10","Loose Equipment","Small Bin ",null,"BIN001","As SoA max group size / 2",null,"Gp3","/=ROUNDUP(K$14/6,0)",null,null,null,"TAB311",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF15 (Office and workroom)","OFF15","Fittings","Noticeboard ",null,"BOA002",null,null,"Gp2",2,null,null,null,"TAB312",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF15 (Office and workroom)","OFF15","Fittings","Worktop 600 deep Solid","(m length)","WKTK600S","To 1 wall.",null,"Gp2","/=ROUND(K$10/3.5,1)",null,null,null,"TAB313",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF15 (Office and workroom)","OFF15","Fitted Furniture","Shelving (set of 3)",null,"SHE100","As SoA max group size",null,"Gp2","/=K$14",null,null,null,"TAB400",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF15 (Office and workroom)","OFF15","Fitted Furniture","Underbench 24 tray unit",null,"TRU001","As SoA max group size",null,"Gp2","/=K$14",null,null,null,"TAB401",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF15 (Office and workroom)","OFF15","Fitted equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"TAB500",0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF15 (Office and workroom)","OFF15","Fixed Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"TAB501",0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,1,1,1,1,0,0,0,0,0,1,0,0,0,0,1,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,1,1,1,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF15 (Office and workroom)","OFF15","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1,null,null,null,"TAB502",0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,1,1,1,1,0,1,1,1,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF15 (Office and workroom)","OFF15","Fixed Equipment","Key safe",null,"SAF002X","1 in premises managers office only",null,"Gp3","CTS",null,null,null,"TAB503",0,{"$f":"COUNTIFS($B$5:$B$1819,P$4,$F$5:$F$1819,$N256)","v":0},0,0,0,0,0,1,1,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Z$4,$F$5:$F$1819,$N256)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AJ$4,$F$5:$F$1819,$N256)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AT$4,$F$5:$F$1819,$N256)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BD$4,$F$5:$F$1819,$N256)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BN$4,$F$5:$F$1819,$N256)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BX$4,$F$5:$F$1819,$N256)","v":1},0,0,0,1,1,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CH$4,$F$5:$F$1819,$N256)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CR$4,$F$5:$F$1819,$N256)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DB$4,$F$5:$F$1819,$N256)","v":0},0,0,0,0,0,0,0,0,1,{"$f":"COUNTIFS($B$5:$B$1819,DL$4,$F$5:$F$1819,$N256)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DV$4,$F$5:$F$1819,$N256)","v":0},0,0,0,0,1,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EF$4,$F$5:$F$1819,$N256)","v":0},0,0,0,0,0,0,0,0,0]
["OFF15 (Office and workroom)","OFF15","Fixed Equipment","General safe",null,"SAF003X","1 in premises managers office only",null,"Gp3","CTS",null,null,null,"TAB504",0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF15 (Office and workroom)","OFF15","Loose Furniture","ICT staff chair",null,"CHA301","As SoA max group size",null,"Gp3","/=K$14",null,null,null,"TAB505",0,0,0,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF15 (Office and workroom)","OFF15","Loose Furniture","Pedestal unit/Admin",null,"STO101","As SoA max group size",null,"Gp3","/=K$14",null,null,null,"TAB506",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF15 (Office and workroom)","OFF15","Loose Furniture","Tall tambour unit/Admin",null,"STO102","In ICT managers office only: As SoA max group size",null,"Gp3","CTS",null,null,null,"TAB600",0,0,0,1,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF15 (Office and workroom)","OFF15","Loose Furniture","Low tambour unit/Admin",null,"STO103",null,null,"Gp3",1,null,null,null,"TAB601",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF15 (Office and workroom)","OFF15","Loose Furniture","Table, ICT/Admin ",null,"TAB503","As SoA max group size",null,"Gp3","/=K$14",null,null,null,"TAB700",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF15 (Office and workroom)","OFF15","Loose Equipment","Small Bin ",null,"BIN001",null,null,"Gp3",1,null,null,null,"TR0001",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF20 (Office and pastoral)","OFF20","Fittings","Noticeboard ",null,"BOA001","As SoA max group size / 3",null,"Gp2","/=ROUND(K$14/3,0)",null,null,null,"TR0002",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,1,1,1,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF20 (Office and pastoral)","OFF20","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",1,null,null,null,"TRA002",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,1,0,1,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF20 (Office and pastoral)","OFF20","Fitted equipment","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"TRA003",0,{"$f":"COUNTIFS($B$5:$B$1819,P$4,$F$5:$F$1819,$N266)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Z$4,$F$5:$F$1819,$N266)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AJ$4,$F$5:$F$1819,$N266)","v":0},0,0,0,0,0,0,0,0,1,{"$f":"COUNTIFS($B$5:$B$1819,AT$4,$F$5:$F$1819,$N266)","v":1},1,1,0,0,1,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BD$4,$F$5:$F$1819,$N266)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BN$4,$F$5:$F$1819,$N266)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BX$4,$F$5:$F$1819,$N266)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CH$4,$F$5:$F$1819,$N266)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CR$4,$F$5:$F$1819,$N266)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DB$4,$F$5:$F$1819,$N266)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DL$4,$F$5:$F$1819,$N266)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DV$4,$F$5:$F$1819,$N266)","v":0},0,0,0,0,0,0,1,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EF$4,$F$5:$F$1819,$N266)","v":0},0,0,0,0,0,0,0,0,0]
["OFF20 (Office and pastoral)","OFF20","Fixed Furniture","No FF&E Listed of This Type",null,null,null,null,null,null,null,null,null,"TRA004",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF20 (Office and pastoral)","OFF20","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1,null,null,null,"TRO001",0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0]
["OFF20 (Office and pastoral)","OFF20","Loose Furniture","Operators chair (with arms)/Admin",null,"CHA303","As SoA max group size / 2 rounded down",null,"Gp3","/=ROUNDDOWN(K$14/2,0)",null,null,null,"TRU001",0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,0,1,1,1,1,0,0,1,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF20 (Office and pastoral)","OFF20","Loose Furniture","Side filing unit (2 dr)/Admin",null,"CAB104",null,null,"Gp3",1,null,null,null,"TRU002",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF20 (Office and pastoral)","OFF20","Loose Furniture","Pedestal unit/Admin",null,"STO101","As SoA max group size / 2 rounded down",null,"Gp3","/=ROUNDDOWN(K$14/2,0)",null,null,null,"TRU003",{"$f":"COUNTIFS($B$5:$B$1819,O$4,$F$5:$F$1819,$N271)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF20 (Office and pastoral)","OFF20","Loose Furniture","Table, ICT/Admin ",null,"TAB502","As SoA max group size / 2 rounded down",null,"Gp3","/=ROUNDDOWN(K$14/2,0)",null,null,null,"TRU004",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF20 (Office and pastoral)","OFF20","Loose Furniture","Upholstered chairs",null,"TAB506","As SoA max group size / 2 rounded up",null,"Gp3","/=ROUNDUP(K$14/2,0)",null,null,null,"TRU005",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF20 (Office and pastoral)","OFF20","Loose Furniture","Table, Coffee (round)",null,"TAB601",null,null,"Gp3",1,null,null,null,"Various",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF20 (Office and pastoral)","OFF20","Loose Equipment","Small Bin ",null,"BIN001","As SoA max group size / 2",null,"Gp3","/=ROUNDUP(K$14/6,0)",null,null,null,"WKTH600",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF31 (Staff room (prep social)","OFF31","Fittings","Noticeboard ",null,"BOA002","As max group size / 20",null,"Gp2","/=ROUND(K$14/20,0)",null,null,null,"WKTH600S",0,{"$f":"COUNTIFS($B$5:$B$1819,P$4,$F$5:$F$1819,$N276)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,Z$4,$F$5:$F$1819,$N276)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AJ$4,$F$5:$F$1819,$N276)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,AT$4,$F$5:$F$1819,$N276)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BD$4,$F$5:$F$1819,$N276)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BN$4,$F$5:$F$1819,$N276)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,BX$4,$F$5:$F$1819,$N276)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CH$4,$F$5:$F$1819,$N276)","v":0},0,0,0,0,0,0,1,0,0,{"$f":"COUNTIFS($B$5:$B$1819,CR$4,$F$5:$F$1819,$N276)","v":0},0,0,1,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DB$4,$F$5:$F$1819,$N276)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DL$4,$F$5:$F$1819,$N276)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,DV$4,$F$5:$F$1819,$N276)","v":0},0,0,0,0,0,0,0,0,0,{"$f":"COUNTIFS($B$5:$B$1819,EF$4,$F$5:$F$1819,$N276)","v":0},0,0,0,0,0,0,0,0,0]
["OFF31 (Staff room (prep social)","OFF31","Fittings","SS single bowl sink (right hand drainer)",null,"SIN004",null,null,"Gp2",1,null,null,null,"WKTI12",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,1,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF31 (Staff room (prep social)","OFF31","Fittings","Worktop 600 deep","(m length)","WKTL600","To 1 wall",null,"Gp2",7.8,null,null,null,"WKTI600S",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF31 (Staff room (prep social)","OFF31","Fitted Furniture","Underbench 2 door cupboard",null,"CUB005",null,null,"Gp2",2,null,null,null,"WKTI75",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF31 (Staff room (prep social)","OFF31","Fitted Furniture","Wall cupboard unit (2 doors)",null,"CUP013",null,null,"Gp2",1,null,null,null,"WKTJ600",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF31 (Staff room (prep social)","OFF31","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",1,null,null,null,"WKTJ600S",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF31 (Staff room (prep social)","OFF31","Fitted Furniture","Coat hooks (12)",null,"STO002","As max group size /12",null,"Gp2","/=ROUNDUP(K$14/12,0)",null,null,null,"WKTK450S",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF31 (Staff room (prep social)","OFF31","Fitted equipment","Wall mounted water boiler",null,"APP004",null,null,"Gp2",1,null,null,null,"WKTK600S",0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,1,1,0,1,1,1,1,0,1,1,1,1,0,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,1,1,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,2,0,1,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0]
["OFF31 (Staff room (prep social)","OFF31","Fixed Furniture","Pigeon Holes unit (with tray unit under)",null,"STO03X","size to suit number of staff",null,"Gp2",1,null,null,null,"WKTL12S",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF31 (Staff room (prep social)","OFF31","Fixed Equipment","Dishwasher",null,"APP001X",null,null,"Gp3",1,null,null,null,"WKTL600",0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF31 (Staff room (prep social)","OFF31","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1,null,null,null,"WKTL600S",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF31 (Staff room (prep social)","OFF31","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",1,null,null,null,"WKTM600S",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["OFF31 (Staff room (prep social)","OFF31","Loose Furniture","Practical stool",null,"CHA024","As max group size x 0.15",null,"Gp3","/=ROUNDUP(K$14*0.15,0)"]
["OFF31 (Staff room (prep social)","OFF31","Loose Furniture","Upholstered easy chair",null,"CHA200","As max group size x 0.45",null,"Gp3","/=ROUND(K$14*0.45,0)"]
["OFF31 (Staff room (prep social)","OFF31","Loose Furniture","Screen",null,"SCR001","As max group size x 0.15",null,"Gp3","/=ROUND(K$14*0.15,0)"]
["OFF31 (Staff room (prep social)","OFF31","Loose Furniture","Table, Coffee (round)",null,"TAB601","As max group size x 0.05",null,"Gp3","/=ROUND(K$14*0.05,0)"]
["OFF31 (Staff room (prep social)","OFF31","Loose Furniture","Classroom chair",null,"CHA006","As max group size x 0.4",null,"Gp3","/=ROUNDDOWN(K$14*0.4,0)"]
["OFF31 (Staff room (prep social)","OFF31","Loose Furniture","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["OFF31 (Staff room (prep social)","OFF31","Loose Furniture","Semicircular table",null,"TAB01SC","As max group size x 0.07",null,"Gp3","/=ROUNDUP(K$14*0.07,0)"]
["OFF31 (Staff room (prep social)","OFF31","Loose Furniture","Rectangular table",null,"TAB06R","As max group size x 0.15 - 1",null,"Gp3","/=ROUNDUP(K$14*0.15,0)-1"]
["OFF31 (Staff room (prep social)","OFF31","Loose Equipment","Microwave",null,"APP001",null,null,"Gp3",1]
["OFF31 (Staff room (prep social)","OFF31","Loose Equipment","Refrigerator ",null,"APP002",null,null,"Gp3",1]
["OFF32 (Staff room social)","OFF32","Fittings","Noticeboard ",null,"BOA002","As max group size / 20",null,"Gp2","/=ROUND(K$14/20,0)"]
["OFF32 (Staff room social)","OFF32","Fittings","SS single bowl sink (right hand drainer)",null,"SIN004",null,null,"Gp2",1]
["OFF32 (Staff room social)","OFF32","Fittings","Worktop 600 deep","(m length)","WKTL600","To 1 wall",null,"Gp2",7.8]
["OFF32 (Staff room social)","OFF32","Fitted Furniture","Underbench 2 door cupboard",null,"CUB005",null,null,"Gp2",2]
["OFF32 (Staff room social)","OFF32","Fitted Furniture","Wall cupboard unit (2 doors)",null,"CUP013",null,null,"Gp2",1]
["OFF32 (Staff room social)","OFF32","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",1]
["OFF32 (Staff room social)","OFF32","Fitted Furniture","Coat hooks (12)",null,"STO002","As max group size /12",null,"Gp2","/=ROUNDUP(K$14/12,0)"]
["OFF32 (Staff room social)","OFF32","Fitted equipment","Wall mounted water boiler",null,"APP004",null,null,"Gp2",1]
["OFF32 (Staff room social)","OFF32","Fixed Furniture","Pigeon Holes unit (with tray unit under)",null,"STO03X","size to suit number of staff",null,"Gp2",1]
["OFF32 (Staff room social)","OFF32","Fixed Equipment","Dishwasher",null,"APP001X",null,null,"Gp3",1]
["OFF32 (Staff room social)","OFF32","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["OFF32 (Staff room social)","OFF32","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",1]
["OFF32 (Staff room social)","OFF32","Loose Furniture","Practical stool",null,"CHA024","As max group size x 0.15",null,"Gp3","/=ROUND(K$14*0.15,0)"]
["OFF32 (Staff room social)","OFF32","Loose Furniture","Upholstered easy chair",null,"CHA200","As max group size x 0.85",null,"Gp3","/=ROUND(K$14*0.85,0)"]
["OFF32 (Staff room social)","OFF32","Loose Furniture","Screen",null,"SCR001","As max group size x 0.15",null,"Gp3","/=ROUND(K$14*0.15,0)"]
["OFF32 (Staff room social)","OFF32","Loose Furniture","Adjustable table",null,"TAB004",null,null,"Gp3",1]
["OFF32 (Staff room social)","OFF32","Loose Furniture","Table, Coffee",null,"TAB600","As max group size x 0.15",null,"Gp3","/=ROUND(K$14*0.15,0)"]
["OFF32 (Staff room social)","OFF32","Loose Furniture","Table, Coffee (round)",null,"TAB601","As max group size x 0.1",null,"Gp3","/=ROUND(K$14*0.1,0)"]
["OFF32 (Staff room social)","OFF32","Loose Equipment","Microwave",null,"APP001",null,null,"Gp3",1]
["OFF32 (Staff room social)","OFF32","Loose Equipment","Refrigerator ",null,"APP002",null,null,"Gp3",1]
["OFF33 (Staff work room)","OFF33","Fittings","Noticeboard ",null,"BOA002",null,null,"Gp2",2]
["OFF33 (Staff work room)","OFF33","Fittings","Worktop 600 deep Solid","(m length)","WKTK600S","To full-length of 2 walls, not including door ",null,"Gp2","CTS"]
["OFF33 (Staff work room)","OFF33","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",3]
["OFF33 (Staff work room)","OFF33","Fitted Furniture","Coat hooks (6)",null,"STO001",null,null,"Gp2",1]
["OFF33 (Staff work room)","OFF33","Fitted equipment","No FF&E Listed of This Type"]
["OFF33 (Staff work room)","OFF33","Fixed Furniture","No FF&E Listed of This Type"]
["OFF33 (Staff work room)","OFF33","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["OFF33 (Staff work room)","OFF33","Loose Furniture","Side filing unit (2 dr)/Admin",null,"CAB104",null,null,"Gp3",1]
["OFF33 (Staff work room)","OFF33","Loose Furniture","ICT staff chair",null,"CHA301","As SoA max group size ",null,"Gp3","/=K$14"]
["OFF33 (Staff work room)","OFF33","Loose Furniture","Pedestal unit/Admin",null,"STO101","As SoA max group size ",null,"Gp3","/=K$14"]
["OFF33 (Staff work room)","OFF33","Loose Furniture","Table, ICT/Admin ",null,"TAB503","As SoA max group size / 2",null,"Gp3","/=ROUND(K$14/2,0)"]
["OFF33 (Staff work room)","OFF33","Loose Equipment","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["OFF35 (Staff wk rm (with sink)","OFF35","Fittings","Noticeboard ",null,"BOA002",null,null,"Gp2",2]
["OFF35 (Staff wk rm (with sink)","OFF35","Fittings","SS single bowl sink (right hand drainer)",null,"SIN004",null,null,"Gp2",1]
["OFF35 (Staff wk rm (with sink)","OFF35","Fittings","Worktop 600 deep Solid","(m length)","WKTK600S","To full-length of 2 walls, not including door ",null,"Gp2","CTS"]
["OFF35 (Staff wk rm (with sink)","OFF35","Fittings","Worktop 600 deep","(m length)","WKTL600",null,null,"Gp2",2.4]
["OFF35 (Staff wk rm (with sink)","OFF35","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",3]
["OFF35 (Staff wk rm (with sink)","OFF35","Fitted Furniture","Underbench 1 door cupboard",null,"CUB009","under sink",null,"Gp2","CTS"]
["OFF35 (Staff wk rm (with sink)","OFF35","Fitted Furniture","Wall cupboard unit (2 doors)",null,"CUP013","above sink",null,"Gp2","CTS"]
["OFF35 (Staff wk rm (with sink)","OFF35","Fitted Furniture","Coat hooks (6)",null,"STO001",null,null,"Gp2",1]
["OFF35 (Staff wk rm (with sink)","OFF35","Fitted equipment","No FF&E Listed of This Type"]
["OFF35 (Staff wk rm (with sink)","OFF35","Fixed Furniture","No FF&E Listed of This Type"]
["OFF35 (Staff wk rm (with sink)","OFF35","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["OFF35 (Staff wk rm (with sink)","OFF35","Fixed Equipment","Dishwasher",null,"APP001X",null,null,"Gp3",1]
["OFF35 (Staff wk rm (with sink)","OFF35","Loose Furniture","Side filing unit (2 dr)/Admin",null,"CAB104",null,null,"Gp3",1]
["OFF35 (Staff wk rm (with sink)","OFF35","Loose Furniture","ICT staff chair",null,"CHA301","As SoA max group size ",null,"Gp3","/=K$14"]
["OFF35 (Staff wk rm (with sink)","OFF35","Loose Furniture","Pedestal unit/Admin",null,"STO101","As SoA max group size ",null,"Gp3","/=K$14"]
["OFF35 (Staff wk rm (with sink)","OFF35","Loose Furniture","Table, ICT/Admin ",null,"TAB503","As SoA max group size / 2",null,"Gp3","/=ROUND(K$14/2,0)"]
["OFF35 (Staff wk rm (with sink)","OFF35","Loose Equipment","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["OFF35 (Staff wk rm (with sink)","OFF35","Loose Equipment","Refrigerator ",null,"APP002","under sink drainer",null,"Gp3",1]
["OFF41 (Conference and meeti...","OFF41","Fittings","No FF&E Listed of This Type"]
["OFF41 (Conference and meeti...","OFF41","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["OFF41 (Conference and meeti...","OFF41","Fitted equipment","No FF&E Listed of This Type"]
["OFF41 (Conference and meeti...","OFF41","Fixed Furniture","No FF&E Listed of This Type"]
["OFF41 (Conference and meeti...","OFF41","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["OFF41 (Conference and meeti...","OFF41","Loose Furniture","Visitors Chair (with arms)/Admin",null,"CHA302","As SoA max group size ",null,"Gp3","/=K14"]
["OFF41 (Conference and meeti...","OFF41","Loose Furniture","Meeting table, Semi-circular/Admin",null,"TAB500",null,null,"Gp3",2]
["OFF41 (Conference and meeti...","OFF41","Loose Furniture","Meeting table/Admin",null,"TAB505","As SoA max group size - 6 / 2",null,"Gp3","/=MAX(0,ROUND((K$14-6)/2,0))"]
["OFF41 (Conference and meeti...","OFF41","Loose Furniture","Low tambour unit/Admin",null,"STO103","As SoA max group size / 5",null,"Gp3","/=ROUND(K$14/5,0)"]
["OFF41 (Conference and meeti...","OFF41","Loose Equipment","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["OFF42 (Laundry)","OFF42","Fittings","SS single sink (right hand drainer)",null,"SIN003",null,null,"Gp2","CTS"]
["OFF42 (Laundry)","OFF42","Fittings","Worktop 600 deep Solid",null,"WKTK600S",null,null,"Gp2","CTS"]
["OFF42 (Laundry)","OFF42","Fitted Furniture","Underbench 2 door cupboard",null,"CUB001",null,null,"Gp2","CTS"]
["OFF42 (Laundry)","OFF42","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2","CTS"]
["OFF42 (Laundry)","OFF42","Fitted equipment","No FF&E Listed of This Type"]
["OFF42 (Laundry)","OFF42","Fixed Furniture","No FF&E Listed of This Type"]
["OFF42 (Laundry)","OFF42","Fixed Equipment","Tumble drier",null,"APP004X",null,null,"Gp3",1]
["OFF42 (Laundry)","OFF42","Fixed Equipment","Washing machine",null,"APP005X",null,null,"Gp3",1]
["OFF42 (Laundry)","OFF42","Loose Furniture","No FF&E Listed of This Type"]
["OFF42 (Laundry)","OFF42","Loose Equipment","No FF&E Listed of This Type"]
["PLA01 (Plant room)","PLA01","Fittings","Contractor to list FF&E of this type",null,"CTS001",null,null,"Gp2","CTS"]
["PLA01 (Plant room)","PLA01","Fitted Furniture","Contractor to list FF&E of this type",null,"CTS002",null,null,"Gp2","CTS"]
["PLA01 (Plant room)","PLA01","Fitted equipment","Contractor to list FF&E of this type",null,"CTS003",null,null,"Gp2","CTS"]
["PLA01 (Plant room)","PLA01","Fixed Furniture","Contractor to list FF&E of this type",null,"CTS004",null,null,"Gp2","CTS"]
["PLA01 (Plant room)","PLA01","Fixed Equipment","Contractor to list FF&E of this type",null,"CTS005",null,null,"Gp2","CTS"]
["PLA01 (Plant room)","PLA01","Loose Furniture","Contractor to list FF&E of this type",null,"CTS006",null,null,"Gp2","CTS"]
["PLA01 (Plant room)","PLA01","Loose Equipment","Contractor to list FF&E of this type",null,"CTS007",null,null,"Gp2","CTS"]
["PLA02 (Server room)","PLA02","Fittings","Contractor to list FF&E of this type",null,"CTS001","based on discussion with school",null,"Gp2","CTS"]
["PLA02 (Server room)","PLA02","Fitted Furniture","Contractor to list FF&E of this type",null,"CTS002","based on discussion with school",null,"Gp2","CTS"]
["PLA02 (Server room)","PLA02","Fitted equipment","Contractor to list FF&E of this type",null,"CTS003","based on discussion with school",null,"Gp2","CTS"]
["PLA02 (Server room)","PLA02","Fixed Furniture","Contractor to list FF&E of this type",null,"CTS004",null,null,"Gp2","CTS"]
["PLA02 (Server room)","PLA02","Fixed Equipment","Contractor to list FF&E of this type",null,"CTS005",null,null,"Gp2","CTS"]
["PLA02 (Server room)","PLA02","Loose Furniture","Contractor to list FF&E of this type",null,"CTS006",null,null,"Gp2","CTS"]
["PLA02 (Server room)","PLA02","Loose Equipment","Contractor to list FF&E of this type",null,"CTS007",null,null,"Gp2","CTS"]
["RES00 (Group room)","RES00","Fittings","No FF&E Listed of This Type"]
["RES00 (Group room)","RES00","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["RES00 (Group room)","RES00","Fitted equipment","No FF&E Listed of This Type"]
["RES00 (Group room)","RES00","Fixed Furniture","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["RES00 (Group room)","RES00","Fixed Equipment","No FF&E Listed of This Type"]
["RES00 (Group room)","RES00","Loose Furniture","Classroom chair",null,"CHA001","if nursery only: max group size in SoA - 1",null,"Gp3","CTS"]
["RES00 (Group room)","RES00","Loose Furniture","Classroom chair",null,"CHA002","or if YR and/or KS1 only: max group size in SoA - 1",null,"Gp3","CTS"]
["RES00 (Group room)","RES00","Loose Furniture","Classroom chair",null,"CHA003","or if any KS2: max group size in SoA - 1",null,"Gp3","CTS"]
["RES00 (Group room)","RES00","Loose Furniture","Classroom chair",null,"CHA005","or if 11-18: max group size in SoA - 1",null,"Gp3","/=K$14-1"]
["RES00 (Group room)","RES00","Loose Furniture","Classroom chair",null,"CHA006","or if 14-18 only: max group size in SoA - 1",null,"Gp3","CTS"]
["RES00 (Group room)","RES00","Loose Furniture","ICT Teachers chair",null,"CHA301","max group size in SoA / 4",null,"Gp3","/=ROUND(K$14/4,0)"]
["RES00 (Group room)","RES00","Loose Furniture","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["RES00 (Group room)","RES00","Loose Furniture","Rectangular table",null,"TAB01R","if nursery only: max group size in SoA -1 / 2",null,"Gp3","CTS"]
["RES00 (Group room)","RES00","Loose Furniture","Rectangular table",null,"TAB02R","or if YR and/or KS1 only: max group size in SoA -1 / 2",null,"Gp3","CTS"]
["RES00 (Group room)","RES00","Loose Furniture","Rectangular table",null,"TAB03R","or if any KS2: max group size in SoA -1 / 2",null,"Gp3","CTS"]
["RES00 (Group room)","RES00","Loose Furniture","Rectangular table",null,"TAB03R","or if 11-18: max group size in SoA -1 / 2",null,"Gp3","/=ROUNDUP((K$14-1)/2,0)"]
["RES00 (Group room)","RES00","Loose Furniture","Rectangular table",null,"TAB03R","or if 14-18 only: max group size in SoA -1 / 2",null,"Gp3","CTS"]
["RES00 (Group room)","RES00","Loose Equipment","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["SEN01 (SEN resource base)","SEN01","Fittings","Noticeboard",null,"BOA001",null,null,"Gp2",1]
["SEN01 (SEN resource base)","SEN01","Fitted Furniture","Whiteboard",null,"BOAW01",null,null,"Gp2",1]
["SEN01 (SEN resource base)","SEN01","Fitted equipment","No FF&E Listed of This Type"]
["SEN01 (SEN resource base)","SEN01","Fixed Furniture","No FF&E Listed of This Type"]
["SEN01 (SEN resource base)","SEN01","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["SEN01 (SEN resource base)","SEN01","Loose Furniture","Classroom chair",null,"CHA003","if primary: max group size in SoA - 1",null,"Gp3","CTS"]
["SEN01 (SEN resource base)","SEN01","Loose Furniture","Classroom chair",null,"CHA005","or if secondary: max group size in SoA - 1",null,"Gp3","/=K$14-1"]
["SEN01 (SEN resource base)","SEN01","Loose Furniture","ICT Teachers chair",null,"CHA301","max group size in SoA / 4",null,"Gp3","/=ROUND(K$14/4,0)"]
["SEN01 (SEN resource base)","SEN01","Loose Furniture","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["SEN01 (SEN resource base)","SEN01","Loose Furniture","Rectangular table",null,"TAB03R","if primary: max group size in SoA -1 / 2",null,"Gp3","CTS"]
["SEN01 (SEN resource base)","SEN01","Loose Furniture","Rectangular table",null,"TAB03R","or if secondary: max group size in SoA -1 / 2",null,"Gp3","/=ROUNDUP((K$14-1)/2,0)"]
["SEN01 (SEN resource base)","SEN01","Loose Furniture","60 Tray unit (2 doors)",null,"TRA004",null,null,"Gp3",1]
["SEN01 (SEN resource base)","SEN01","Loose Equipment","No FF&E Listed of This Type"]
["SEN06 (Inclusion immersion...)","SEN06","Fittings","Noticeboard",null,"BOA001",null,null,"Gp2",1]
["SEN06 (Inclusion immersion...)","SEN06","Fitted Furniture","Whiteboard",null,"BOAW01",null,null,"Gp2",1]
["SEN06 (Inclusion immersion...)","SEN06","Fitted equipment","No FF&E Listed of This Type"]
["SEN06 (Inclusion immersion...)","SEN06","Fixed Furniture","No FF&E Listed of This Type"]
["SEN06 (Inclusion immersion...)","SEN06","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["SEN06 (Inclusion immersion...)","SEN06","Loose Furniture","Small Bin",null,"BIM001",null,null,"Gp3",1]
["SEN06 (Inclusion immersion...)","SEN06","Loose Furniture","Classroom chair",null,"CHA003","if primary: max group size in SoA",null,"Gp3","CTS"]
["SEN06 (Inclusion immersion...)","SEN06","Loose Furniture","Classroom chair",null,"CHA005","or if secondary: max group size in SoA ",null,"Gp3","CTS"]
["SEN06 (Inclusion immersion...)","SEN06","Loose Furniture","ICT Teachers chair",null,"CHA301",null,null,"Gp3",1]
["SEN06 (Inclusion immersion...)","SEN06","Loose Furniture","Pedestal unit/ Admin",null,"STO101",null,null,"Gp3",1]
["SEN06 (Inclusion immersion...)","SEN06","Loose Furniture","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["SEN06 (Inclusion immersion...)","SEN06","Loose Furniture","Rectangular table",null,"TAB03R","if primary: max group size in SoA / 2",null,"Gp3","CTS"]
["SEN06 (Inclusion immersion...)","SEN06","Loose Furniture","Rectangular table",null,"TAB03R","or if secondary: max group size in SoA / 2",null,"Gp3","CTS"]
["SEN06 (Inclusion immersion...)","SEN06","Loose Furniture","Table. ICT/ Admin",null,"TAB501",null,null,"Gp3",1]
["SEN06 (Inclusion immersion...)","SEN06","Loose Equipment","No FF&E Listed of This Type"]
["SEN11 (SEN therapy and MI r...","SEN11","Fittings","Noticeboard ",null,"BOA002",null,null,"Gp2",1]
["SEN11 (SEN therapy and MI r...","SEN11","Fittings","Curtian tracking","(m length)","CUR001","Around bed",null,"Gp2",3]
["SEN11 (SEN therapy and MI r...","SEN11","Fittings","Curtains",null,"CUR002","Around bed",null,"Gp2",3]
["SEN11 (SEN therapy and MI r...","SEN11","Fittings","SS single bowl sink (left hand drainer)",null,"SIN004",null,null,"Gp2",1]
["SEN11 (SEN therapy and MI r...","SEN11","Fittings","Worktop 600 deep","(m length)","WKTL600","to 1 wall",null,"Gp2",1.8]
["SEN11 (SEN therapy and MI r...","SEN11","Fitted Furniture","Underbench 2 door cupboard",null,"CUB005",null,null,"Gp2",1]
["SEN11 (SEN therapy and MI r...","SEN11","Fitted Furniture","Wall cupboard unit (2 doors)",null,"CUP013",null,null,"Gp2",1]
["SEN11 (SEN therapy and MI r...","SEN11","Fitted equipment","No FF&E Listed of This Type"]
["SEN11 (SEN therapy and MI r...","SEN11","Fixed Furniture","No FF&E Listed of This Type"]
["SEN11 (SEN therapy and MI r...","SEN11","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["SEN11 (SEN therapy and MI r...","SEN11","Loose Furniture","Medical Bed",null,"BED001",null,null,"Gp3",1]
["SEN11 (SEN therapy and MI r...","SEN11","Loose Furniture","Side filing unit (2 dr)/Admin",null,"CAB104",null,null,"Gp3",1]
["SEN11 (SEN therapy and MI r...","SEN11","Loose Furniture","Upholstered easy chair",null,"CHA200",null,null,"Gp3",1]
["SEN11 (SEN therapy and MI r...","SEN11","Loose Furniture","ICT staff chair",null,"CHA301",null,null,"Gp3",1]
["SEN11 (SEN therapy and MI r...","SEN11","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["SEN11 (SEN therapy and MI r...","SEN11","Loose Furniture","Table, ICT/Admin ",null,"TAB503",null,null,"Gp3",1]
["SEN11 (SEN therapy and MI r...","SEN11","Loose Equipment","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["STH00 (PE store(s))","STH00","Fittings","Contractor to list FF&E of This Type",null,null,null,null,"Gp2","CTS"]
["STH00 (PE store(s))","STH00","Fitted Furniture","Contractor to list FF&E of This Type",null,null,null,null,"Gp2","CTS"]
["STH00 (PE store(s))","STH00","Fitted equipment","Contractor to list FF&E of This Type",null,null,null,null,"Gp2","CTS"]
["STH00 (PE store(s))","STH00","Fixed Furniture","Contractor to list FF&E of This Type",null,null,null,null,"Gp2","CTS"]
["STH00 (PE store(s))","STH00","Fixed Equipment","Contractor to list FF&E of This Type",null,null,null,null,"Gp2","CTS"]
["STH00 (PE store(s))","STH00","Loose Furniture","Contractor to list FF&E of This Type",null,null,null,null,"Gp3","CTS"]
["STH00 (PE store(s))","STH00","Loose Equipment","Contractor to list FF&E of This Type",null,null,null,null,"Gp3","CTS"]
["STH05 (External PE store)","STH05","Fittings","Contractor to list FF&E of This Type",null,null,null,null,"Gp2","CTS"]
["STH05 (External PE store)","STH05","Fitted Furniture","Contractor to list FF&E of This Type",null,null,null,null,"Gp2","CTS"]
["STH05 (External PE store)","STH05","Fitted equipment","Contractor to list FF&E of This Type",null,null,null,null,"Gp2","CTS"]
["STH05 (External PE store)","STH05","Fixed Furniture","Contractor to list FF&E of This Type",null,null,null,null,"Gp2","CTS"]
["STH05 (External PE store)","STH05","Fixed Equipment","Contractor to list FF&E of This Type",null,null,null,null,"Gp2","CTS"]
["STH05 (External PE store)","STH05","Loose Furniture","Contractor to list FF&E of This Type",null,null,null,null,"Gp3","CTS"]
["STH05 (External PE store)","STH05","Loose Equipment","Contractor to list FF&E of This Type",null,null,null,null,"Gp3","CTS"]
["STH10 (Furniture store)","STH10","Fittings","No FF&E Listed of This Type"]
["STH10 (Furniture store)","STH10","Fitted Furniture","No FF&E Listed of This Type"]
["STH10 (Furniture store)","STH10","Fitted equipment","No FF&E Listed of This Type"]
["STH10 (Furniture store)","STH10","Fixed Furniture","No FF&E Listed of This Type"]
["STH10 (Furniture store)","STH10","Fixed Equipment","No FF&E Listed of This Type"]
["STH10 (Furniture store)","STH10","Loose Furniture","No FF&E Listed of This Type"]
["STH10 (Furniture store)","STH10","Loose Equipment","No FF&E Listed of This Type"]
["STN01 (Personal storage (cl...","STN01","Fittings","No FF&E Listed of This Type"]
["STN01 (Personal storage (cl...","STN01","Fitted Furniture","Coat hooks (6)","(m length)","STO001","To 1 wall. Minimum space between hooks 133mm",null,"Gp2","/=ROUND((K10/0.55)*0.2,1)"]
["STN01 (Personal storage (cl...","STN01","Fitted Furniture","Coat hooks (12)","(m length)","STO002","To 1 wall. Minimum space between hooks 133mm",null,"Gp2","/=ROUND((K10/0.72)*0.8,1)"]
["STN01 (Personal storage (cl...","STN01","Fitted equipment","No FF&E Listed of This Type"]
["STN01 (Personal storage (cl...","STN01","Fixed Furniture","No FF&E Listed of This Type"]
["STN01 (Personal storage (cl...","STN01","Fixed Equipment","No FF&E Listed of This Type"]
["STN01 (Personal storage (cl...","STN01","Loose Furniture","No FF&E Listed of This Type"]
["STN01 (Personal storage (cl...","STN01","Loose Equipment","No FF&E Listed of This Type"]
["STN02 (Personal storage (lo","STN02","Fittings","No FF&E Listed of This Type"]
["STN02 (Personal storage (lo","STN02","Fitted Furniture","Locker (single, 4 high)","(no of lockers)","LOC014X","To 1 wall. 13 lockers per m length.",null,"Gp2","/=ROUND((K10/0.75)*13.33,1)"]
["STN02 (Personal storage (lo","STN02","Fitted equipment","No FF&E Listed of This Type"]
["STN02 (Personal storage (lo","STN02","Fixed Furniture","No FF&E Listed of This Type"]
["STN02 (Personal storage (lo","STN02","Fixed Equipment","No FF&E Listed of This Type"]
["STN02 (Personal storage (lo","STN02","Loose Furniture","No FF&E Listed of This Type"]
["STN02 (Personal storage (lo","STN02","Loose Equipment","No FF&E Listed of This Type"]
["STN04 (Wheelchair and appli...","STN04","Fittings","No FF&E Listed of This Type"]
["STN04 (Wheelchair and appli...","STN04","Fitted Furniture","No FF&E Listed of This Type"]
["STN04 (Wheelchair and appli...","STN04","Fitted equipment","No FF&E Listed of This Type"]
["STN04 (Wheelchair and appli...","STN04","Fixed Furniture","No FF&E Listed of This Type"]
["STN04 (Wheelchair and appli...","STN04","Fixed Equipment","No FF&E Listed of This Type"]
["STN04 (Wheelchair and appli...","STN04","Loose Furniture","No FF&E Listed of This Type"]
["STN04 (Wheelchair and appli...","STN04","Loose Equipment","No FF&E Listed of This Type"]
["STN21 (Secure and exam and ...","STN21","Fittings","No FF&E Listed of This Type"]
["STN21 (Secure and exam and ...","STN21","Fitted Furniture","Stockroom shelving (set of 5) ","(m2)","SHE010","to 2 walls",null,"Gp2","/=ROUND(K10*1.33,1)"]
["STN21 (Secure and exam and ...","STN21","Fitted equipment","No FF&E Listed of This Type"]
["STN21 (Secure and exam and ...","STN21","Fixed Furniture","No FF&E Listed of This Type"]
["STN21 (Secure and exam and ...","STN21","Fixed Equipment","No FF&E Listed of This Type"]
["STN21 (Secure and exam and ...","STN21","Loose Furniture","Security cabinet (2 door)/Admin",null,"CAB105",null,null,"Gp3",1]
["STN21 (Secure and exam and ...","STN21","Loose Equipment","No FF&E Listed of This Type"]
["STN31 (Cleaners store)","STN31","Fittings","Belfast sink (large)",null,"SIN001","Low mounted",null,"Gp2",1]
["STN31 (Cleaners store)","STN31","Fitted Furniture","Stockroom shelving (set of 5) ","(m2)","SHE030","To 1 wall.  Total sq m",null,"Gp2",1.8]
["STN31 (Cleaners store)","STN31","Fitted equipment","No FF&E Listed of This Type"]
["STN31 (Cleaners store)","STN31","Fixed Furniture","No FF&E Listed of This Type"]
["STN31 (Cleaners store)","STN31","Fixed Equipment","No FF&E Listed of This Type"]
["STN31 (Cleaners store)","STN31","Loose Furniture","No FF&E Listed of This Type"]
["STN31 (Cleaners store)","STN31","Loose Equipment","No FF&E Listed of This Type"]
["STT05 (Specialist store)","STT05","Fittings","No FF&E Listed of This Type"]
["STT05 (Specialist store)","STT05","Fitted Furniture","Stockroom shelving (set of 5) ","(m2)","SHE010","To 1 wall unless for art. Total sq m",null,"Gp2",4.5]
["STT05 (Specialist store)","STT05","Fitted Furniture","Stockroom shelving (set of 5) ","(m2)","SHE040","To 1 wall if for art. Total sq m",null,"Gp2",5.0999999999999996]
["STT05 (Specialist store)","STT05","Fitted Furniture","Stockroom shelving (set of 5) ","(m2)","SHE020","To 2 walls. Total sq m",null,"Gp2",6.5]
["STT05 (Specialist store)","STT05","Fitted equipment","No FF&E Listed of This Type"]
["STT05 (Specialist store)","STT05","Fixed Furniture","No FF&E Listed of This Type"]
["STT05 (Specialist store)","STT05","Fixed Equipment","No FF&E Listed of This Type"]
["STT05 (Specialist store)","STT05","Loose Furniture","No FF&E Listed of This Type"]
["STT05 (Specialist store)","STT05","Loose Equipment","No FF&E Listed of This Type"]
["STT10 (General store)","STT10","Fittings","No FF&E Listed of This Type"]
["STT10 (General store)","STT10","Fitted Furniture","Stockroom shelving (set of 5) ","(m2)","SHE010","To 1 wall if under 4m2, to 3 walls if over. Area in SoA + 5 if over 4m2",null,"Gp2","/=ROUND(IF(K10>4,K10+5,K10),1)"]
["STT10 (General store)","STT10","Fitted equipment","No FF&E Listed of This Type"]
["STT10 (General store)","STT10","Fixed Furniture","No FF&E Listed of This Type"]
["STT10 (General store)","STT10","Fixed Equipment","No FF&E Listed of This Type"]
["STT10 (General store)","STT10","Loose Furniture","No FF&E Listed of This Type"]
["STT10 (General store)","STT10","Loose Equipment","No FF&E Listed of This Type"]
["SUP01 (Chapel)","SUP01","Fittings","Contractor to list FF&E of this type",null,"CTS001","based on discussion with school",null,"Gp2","CTS"]
["SUP01 (Chapel)","SUP01","Fitted Furniture","Contractor to list FF&E of this type",null,"CTS002","based on discussion with school",null,"Gp2","CTS"]
["SUP01 (Chapel)","SUP01","Fitted equipment","Contractor to list FF&E of this type",null,"CTS003","based on discussion with school",null,"Gp2","CTS"]
["SUP01 (Chapel)","SUP01","Fixed Furniture","Contractor to list FF&E of this type",null,"CTS004","based on any legacy FF&E and discussion with school",null,"Gp3","CTS"]
["SUP01 (Chapel)","SUP01","Fixed Equipment","Contractor to list FF&E of this type",null,"CTS005","based on any legacy FF&E and discussion with school",null,"Gp3","CTS"]
["SUP01 (Chapel)","SUP01","Loose Furniture","Contractor to list FF&E of this type",null,"CTS006","based on any legacy FF&E and discussion with school",null,"Gp3","CTS"]
["SUP01 (Chapel)","SUP01","Loose Equipment","Contractor to list FF&E of this type",null,"CTS007","based on any legacy FF&E and discussion with school",null,"Gp3","CTS"]
["TOC03 (Hygiene rm (without","TOC03","Fittings","Showerbed",null,"APP007X","Specification of shower bed to be agreed with school",null,"Gp2",1]
["TOC03 (Hygiene rm (without","TOC03","Fittings","Ceiling mounted hoist with track",null,"HOI001",null,null,"Gp2",1]
["TOC03 (Hygiene rm (without","TOC03","Fittings","Mirror 1500 high 600 above ffl",null,"MIR001","600 above floor level",null,"Gp2",1]
["TOC03 (Hygiene rm (without","TOC03","Fitted Furniture","No FF&E Listed of This Type"]
["TOC03 (Hygiene rm (without","TOC03","Fitted equipment","No FF&E Listed of This Type"]
["TOC03 (Hygiene rm (without","TOC03","Fixed Furniture","No FF&E Listed of This Type"]
["TOC03 (Hygiene rm (without","TOC03","Fixed Equipment","No FF&E Listed of This Type"]
["TOC03 (Hygiene rm (without","TOC03","Loose Furniture","No FF&E Listed of This Type"]
["TOC03 (Hygiene rm (without","TOC03","Loose Equipment","No FF&E Listed of This Type"]
["TOC04 (Hygiene room (with w","TOC04","Fittings","Showerbed",null,"APP007X","specification of shower bed to be agreed with school",null,"Gp2",1]
["TOC04 (Hygiene room (with w","TOC04","Fittings","Ceiling mounted hoist with track",null,"HOI001",null,null,"Gp2",1]
["TOC04 (Hygiene room (with w","TOC04","Fittings","Mirror 1500 high 600 above ffl",null,"MIR001","600 above floor level",null,"Gp2",1]
["TOC04 (Hygiene room (with w","TOC04","Fitted Furniture","No FF&E Listed of This Type"]
["TOC04 (Hygiene room (with w","TOC04","Fitted equipment","No FF&E Listed of This Type"]
["TOC04 (Hygiene room (with w","TOC04","Fixed Furniture","No FF&E Listed of This Type"]
["TOC04 (Hygiene room (with w","TOC04","Fixed Equipment","No FF&E Listed of This Type"]
["TOC04 (Hygiene room (with w","TOC04","Loose Furniture","No FF&E Listed of This Type"]
["TOC04 (Hygiene room (with w","TOC04","Loose Equipment","No FF&E Listed of This Type"]
["TOC13 (Pupil toilet suite)","TOC13","Fittings","No FF&E Listed of This Type"]
["TOC13 (Pupil toilet suite)","TOC13","Fitted Furniture","No FF&E Listed of This Type"]
["TOC13 (Pupil toilet suite)","TOC13","Fitted equipment","No FF&E Listed of This Type"]
["TOC13 (Pupil toilet suite)","TOC13","Fixed Furniture","No FF&E Listed of This Type"]
["TOC13 (Pupil toilet suite)","TOC13","Fixed Equipment","No FF&E Listed of This Type"]
["TOC13 (Pupil toilet suite)","TOC13","Loose Furniture","No FF&E Listed of This Type"]
["TOC13 (Pupil toilet suite)","TOC13","Loose Equipment","No FF&E Listed of This Type"]
["TOC15 (Individual toilet)","TOC15","Fittings","No FF&E Listed of This Type"]
["TOC15 (Individual toilet)","TOC15","Fitted Furniture","No FF&E Listed of This Type"]
["TOC15 (Individual toilet)","TOC15","Fitted equipment","No FF&E Listed of This Type"]
["TOC15 (Individual toilet)","TOC15","Fixed Furniture","No FF&E Listed of This Type"]
["TOC15 (Individual toilet)","TOC15","Fixed Equipment","No FF&E Listed of This Type"]
["TOC15 (Individual toilet)","TOC15","Loose Furniture","No FF&E Listed of This Type"]
["TOC15 (Individual toilet)","TOC15","Loose Equipment","No FF&E Listed of This Type"]
["TOC21 (Staff and accessible...","TOC21","Fittings","No FF&E Listed of This Type"]
["TOC21 (Staff and accessible...","TOC21","Fitted Furniture","No FF&E Listed of This Type"]
["TOC21 (Staff and accessible...","TOC21","Fitted equipment","No FF&E Listed of This Type"]
["TOC21 (Staff and accessible...","TOC21","Fixed Furniture","No FF&E Listed of This Type"]
["TOC21 (Staff and accessible...","TOC21","Fixed Equipment","No FF&E Listed of This Type"]
["TOC21 (Staff and accessible...","TOC21","Loose Furniture","No FF&E Listed of This Type"]
["TOC21 (Staff and accessible...","TOC21","Loose Equipment","No FF&E Listed of This Type"]
["TOC22 (Staff toilet suite)","TOC22","Fittings","No FF&E Listed of This Type"]
["TOC22 (Staff toilet suite)","TOC22","Fitted Furniture","No FF&E Listed of This Type"]
["TOC22 (Staff toilet suite)","TOC22","Fitted equipment","No FF&E Listed of This Type"]
["TOC22 (Staff toilet suite)","TOC22","Fixed Furniture","No FF&E Listed of This Type"]
["TOC22 (Staff toilet suite)","TOC22","Fixed Equipment","No FF&E Listed of This Type"]
["TOC22 (Staff toilet suite)","TOC22","Loose Furniture","No FF&E Listed of This Type"]
["TOC22 (Staff toilet suite)","TOC22","Loose Equipment","No FF&E Listed of This Type"]
["HAL11 (Studio)","HAL11","Fittings","Worktop 600 deep","(m length)","WKTJ600","to full-length of 1 wall","CTS","Gp2","CTS"]
["HAL11 (Studio)","HAL11","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["HAL11 (Studio)","HAL11","Fitted Furniture","Underbench 2 door cupboard",null,"CUB003","to match workbench",null,"Gp2","CTS"]
["HAL11 (Studio)","HAL11","Fitted Furniture","Shelving (set of 3)",null,"SHE100","to match workbench",null,"Gp2","CTS"]
["HAL11 (Studio)","HAL11","Fitted Furniture","Underbench 18 tray unit",null,"TRU002","to match workbench",null,"Gp2","CTS"]
["HAL11 (Studio)","HAL11","Fitted equipment","No FF&E Listed of This Type"]
["HAL11 (Studio)","HAL11","Fixed Furniture","No FF&E Listed of This Type"]
["HAL11 (Studio)","HAL11","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["HAL11 (Studio)","HAL11","Loose Furniture","Classroom chair",null,"CHA004",null,null,"Gp3",30]
["HAL11 (Studio)","HAL11","Loose Furniture","Trapezoidal table",null,"TAB02TZ",null,null,"Gp3",8]
["HAL11 (Studio)","HAL11","Loose Equipment","No FF&E Listed of This Type"]
["HAL12 (Small hall)","HAL12","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["HAL12 (Small hall)","HAL12","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["HAL12 (Small hall)","HAL12","Fitted equipment","No FF&E Listed of This Type"]
["HAL12 (Small hall)","HAL12","Fixed Furniture","Contractor to list FF&E of This Type",null,"CTS004","based on any legacy FF&E and discussion with school",null,"Gp3","CTS"]
["HAL12 (Small hall)","HAL12","Fixed Equipment","Contractor to list FF&E of This Type",null,"CTS005","based on any legacy FF&E and discussion with school",null,"Gp3","CTS"]
["HAL12 (Small hall)","HAL12","Loose Furniture","Contractor to list FF&E of This Type",null,"CTS006","based on any legacy FF&E and discussion with school",null,"Gp3","CTS"]
["HAL12 (Small hall)","HAL12","Loose Equipment","Contractor to list FF&E of This Type",null,"CTS007","based on any legacy FF&E and discussion with school",null,"Gp3","CTS"]
["HAL13 (Main hall)","HAL13","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["HAL13 (Main hall)","HAL13","Fittings","Lighting rig",null,"LIG001","sufficient for 12 circuits above and in front of performance area",null,"Gp2",1]
["HAL13 (Main hall)","HAL13","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["HAL13 (Main hall)","HAL13","Fitted equipment","Climbing frame (3 section)",null,"SPO001",null,null,"Gp2",1]
["HAL13 (Main hall)","HAL13","Fitted equipment","Wall hinged rope frame",null,"SPO002",null,null,"Gp2",1]
["HAL13 (Main hall)","HAL13","Fixed Furniture","No FF&E Listed of This Type"]
["HAL13 (Main hall)","HAL13","Fixed Equipment","Clock (wall mounted)",null,"EQ001X",null,null,"Gp3",1]
["HAL13 (Main hall)","HAL13","Fixed Equipment","Stage lanterns",null,"LIG001X",null,null,"Gp3",24]
["HAL13 (Main hall)","HAL13","Loose Furniture","Classroom chair",null,"CHA004","option 2: as SoA max group size","CTS","Gp3","CTS"]
["HAL13 (Main hall)","HAL13","Loose Furniture","Folding table and 12 stool set",null,"DIN003","option 1: as SoA max group size / 12, or","CTS","Gp3","CTS"]
["HAL13 (Main hall)","HAL13","Loose Furniture","Circular folding tilting top table*",null,"DIN004","option 2: as SoA max group size / 6 , and","CTS","Gp3","CTS"]
["HAL13 (Main hall)","HAL13","Loose Equipment","Vaulting box (small)",null,"SPO010",null,null,"Gp3",1]
["HAL13 (Main hall)","HAL13","Loose Equipment","Vaulting box (med)",null,"SPO011",null,null,"Gp3",1]
["HAL13 (Main hall)","HAL13","Loose Equipment","Vaulting box (large)",null,"SPO012",null,null,"Gp3",1]
["HAL13 (Main hall)","HAL13","Loose Equipment","Balance benches (short)",null,"SPO013",null,null,"Gp3",1]
["HAL13 (Main hall)","HAL13","Loose Equipment","Balance benches (med)",null,"SPO014",null,null,"Gp3",1]
["HAL13 (Main hall)","HAL13","Loose Equipment","Trestle ",null,"SPO015",null,null,"Gp3",1]
["HAL13 (Main hall)","HAL13","Loose Equipment","Balance beam with hooks",null,"SPO016",null,null,"Gp3",1]
["HAL13 (Main hall)","HAL13","Loose Equipment","Ladder with hooks",null,"SPO017",null,null,"Gp3",1]
["HAL13 (Main hall)","HAL13","Loose Equipment","Safety matting",null,"SPO025",null,null,"Gp3",10]
["HAL13 (Main hall)","HAL13","Loose Equipment","Pair of five-a-side football goals",null,"SPO036",null,null,"Gp3",1]
["LIB01 (Library )","LIB01","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",2]
["LIB01 (Library )","LIB01","Fittings","Worktop 600 deep",null,"WKTH600","to 1 wall",null,"Gp2","/=ROUND(K10/4.2,1)"]
["LIB01 (Library )","LIB01","Fitted Furniture","No FF&E Listed of This Type"]
["LIB01 (Library )","LIB01","Fitted equipment","No FF&E Listed of This Type"]
["LIB01 (Library )","LIB01","Fixed Furniture","Single sided starter unit (tall)",null,"LIB03X","Max group size in SoA / 9",null,"Gp3","/=ROUND(K$14/9,0)"]
["LIB01 (Library )","LIB01","Fixed Furniture","Single sided starter unit (med)",null,"LIB04X","Max group size in SoA / 3",null,"Gp3","/=ROUND(K$14/3,0)"]
["LIB01 (Library )","LIB01","Fixed Furniture","Single sided starter unit (low)",null,"LIB05X","Max group size in SoA / 8",null,"Gp3","/=ROUND(K$14/8,0)"]
["LIB01 (Library )","LIB01","Fixed Equipment","No FF&E Listed of This Type"]
["LIB01 (Library )","LIB01","Loose Furniture","Classroom chair",null,"CHA002","either if YR and/or KS1 only: max group size in SoA / 2",null,"Gp3","CTS"]
["LIB01 (Library )","LIB01","Loose Furniture","Classroom chair ",null,"CHA003","or if any KS2: max group size in SoA / 2",null,"Gp3","/=ROUND(K$14/2,0)"]
["LIB01 (Library )","LIB01","Loose Furniture","Upholstered primay pupils easy chair",null,"CHA201","Max group size in SoA / 4",null,"Gp3","/=ROUND(K$14/4,0)"]
["LIB01 (Library )","LIB01","Loose Furniture","ICT pupil chair ",null,"CHA300","Max group size in SoA / 4",null,"Gp3","/=ROUND(K$14/4,0)"]
["LIB01 (Library )","LIB01","Loose Furniture","Semi-circular table",null,"TAB02R","either if YR and/or KS1 only: max group size in SoA / 6",null,"Gp3","CTS"]
["LIB01 (Library )","LIB01","Loose Furniture","Semi-circular table ",null,"TAB03R","or if any KS2: max group size in SoA / 6",null,"Gp3","/=ROUND(K$14/6,0)"]
["LIB01 (Library )","LIB01","Loose Furniture","Table, ICT/Admin ",null,"TAB501",null,null,"Gp3",1]
["LIB01 (Library )","LIB01","Loose Furniture","Mobile book trolley ",null,"TR0001",null,null,"Gp3",1]
["LIB01 (Library )","LIB01","Loose Equipment","No FF&E Listed of This Type"]
["PRA01 (ICT rich practical r...","PRA01","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["PRA01 (ICT rich practical r...","PRA01","Fittings","Belfast sink (large)",null,"SIN001",null,null,"Gp2",1]
["PRA01 (ICT rich practical r...","PRA01","Fittings","Worktop 600 deep Solid","(m length)","WKTJ600S","to 2 walls, or 1 wall if area less than 45m2","CTS","Gp2","/=IF(K$10>45,14.4,7.2)"]
["PRA01 (ICT rich practical r...","PRA01","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["PRA01 (ICT rich practical r...","PRA01","Fitted Furniture","Shelving (set of 3)",null,"SHE100","SoA max group size / 5",null,"Gp2","/=ROUND(K$14/5,0)"]
["PRA01 (ICT rich practical r...","PRA01","Fitted equipment","No FF&E Listed of This Type"]
["PRA01 (ICT rich practical r...","PRA01","Fixed Furniture","No FF&E Listed of This Type"]
["PRA01 (ICT rich practical r...","PRA01","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["PRA01 (ICT rich practical r...","PRA01","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp2",1]
["PRA01 (ICT rich practical r...","PRA01","Loose Furniture","ICT pupil chair ",null,"CHA300","SoA max group size",null,"Gp2","/=K$14"]
["PRA01 (ICT rich practical r...","PRA01","Loose Furniture","Semi-circular table",null,"TAB001",null,null,"Gp2",1]
["PRA01 (ICT rich practical r...","PRA01","Loose Furniture","Rectangular table",null,"TAB04R","SoA max group size / 2 - 1",null,"Gp2","/=ROUND(K$14/2,0)-1"]
["PRA01 (ICT rich practical r...","PRA01","Loose Equipment","No FF&E Listed of This Type"]
["PRA11 (Food bay and practic...","PRA11","Fittings","SS single bowl sink (right hand drainer)",null,"SIN004",null,null,"Gp2",1]
["PRA11 (Food bay and practic...","PRA11","Fittings","Worktop 600 deep Solid",null,"WKTJ600S","to parts of 2 walls or peninsulas",null,"Gp2","CTS"]
["PRA11 (Food bay and practic...","PRA11","Fitted Furniture","Underbench 2 door cupboard",null,"CUB003",null,null,"Gp2",3]
["PRA11 (Food bay and practic...","PRA11","Fitted Furniture","Underbench 1 door cupboard",null,"CUB008",null,null,"Gp2",2]
["PRA11 (Food bay and practic...","PRA11","Fitted Furniture","Oven housing unit",null,"CUP014",null,null,"Gp2",1]
["PRA11 (Food bay and practic...","PRA11","Fitted equipment","Cooker Hob Electric (inset)",null,"APP001",null,null,"Gp2",1]
["PRA11 (Food bay and practic...","PRA11","Fitted equipment","Mini oven (inset) Primary",null,"APP002",null,null,"Gp2",1]
["PRA11 (Food bay and practic...","PRA11","Fixed Furniture","No FF&E Listed of This Type",null,null,null,null,"Gp3"]
["PRA11 (Food bay and practic...","PRA11","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["PRA11 (Food bay and practic...","PRA11","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",1]
["PRA11 (Food bay and practic...","PRA11","Loose Furniture","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["PRA11 (Food bay and practic...","PRA11","Loose Furniture","SS Trolley",null,"TRO001",null,null,"Gp3",1]
["PRA11 (Food bay and practic...","PRA11","Loose Equipment","Microwave",null,"APP001",null,null,"Gp3",2]
["PRA11 (Food bay and practic...","PRA11","Loose Equipment","Compact fridge (Primary)",null,"APP004",null,null,"Gp3",1]
["PRA12 (Food science DT art)","PRA12","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["PRA12 (Food science DT art)","PRA12","Fittings","Belfast sink (large)",null,"SIN001","1 if art or DT",null,"Gp2",1]
["PRA12 (Food science DT art)","PRA12","Fittings","SS single bowl sink (right hand drainer)",null,"SIN004","SoA max group size / 15",null,"Gp2","/=ROUND(K$14/15,0)"]
["PRA12 (Food science DT art)","PRA12","Fittings","Worktop 600 deep Solid",null,"WKTJ600S","to 2.5 walls, or 1.5 walls if area less than 45m2",null,"Gp2","/=3.9+IF(K$10>45,14.4,7.2)"]
["PRA12 (Food science DT art)","PRA12","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["PRA12 (Food science DT art)","PRA12","Fitted Furniture","Underbench 2 door cupboard",null,"CUB003","SoA max group size / 4",null,"Gp2","/=ROUNDDOWN(K$14/4,0)"]
["PRA12 (Food science DT art)","PRA12","Fitted Furniture","Underbench 1 door cupboard",null,"CUB008","to match side benching length",null,"Gp2","/=ROUNDUP(M271/4,0)"]
["PRA12 (Food science DT art)","PRA12","Fitted Furniture","Underbench paper unit",null,"CUB011","1 if art or DT",null,"Gp2",1]
["PRA12 (Food science DT art)","PRA12","Fitted Furniture","Oven housing unit",null,"CUP014","SoA max group size / 15 if food",null,"Gp2","/=ROUND(K$14/15,0)"]
["PRA12 (Food science DT art)","PRA12","Fitted Furniture","Shelving (set of 3)",null,"SHE100","SoA max group size / 4",null,"Gp2","/=ROUNDDOWN(K$14/4,0)"]
["PRA12 (Food science DT art)","PRA12","Fitted Furniture","Coat hooks (12)",null,"STO002",null,null,"Gp2",1]
["PRA12 (Food science DT art)","PRA12","Fitted equipment","Cooker Hob Electric (inset)",null,"APP001","SoA max group size / 15 if food",null,"Gp2","/=ROUND(K$14/15,0)"]
["PRA12 (Food science DT art)","PRA12","Fitted equipment","Mini oven (inset) Primary",null,"APP002","SoA max group size / 15 if food",null,"Gp2","/=ROUND(K$14/15,0)"]
["PRA12 (Food science DT art)","PRA12","Fixed Furniture","No FF&E Listed of This Type"]
["PRA12 (Food science DT art)","PRA12","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["PRA12 (Food science DT art)","PRA12","Loose Furniture","Classroom chair",null,"CHA002","if YR and/or KS1 only: SoA max group size - 4","CTS","Gp3","CTS"]
["PRA12 (Food science DT art)","PRA12","Loose Furniture","Classroom chair",null,"CHA003","if any KS2: SoA max group size - 4","CTS","Gp3","/=K$14-4"]
["PRA12 (Food science DT art)","PRA12","Loose Furniture","ICT pupil chair ",null,"CHA300",null,null,"Gp3",4]
["PRA12 (Food science DT art)","PRA12","Loose Furniture","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["PRA12 (Food science DT art)","PRA12","Loose Furniture","Rectangular table",null,"TAB02R","if YR and/or KS1 only: SoA max group size / 3.33","CTS","Gp3","CTS"]
["PRA12 (Food science DT art)","PRA12","Loose Furniture","Rectangular table",null,"TAB03R","if any KS2: SoA max group size / 3.33","CTS","Gp3","/=ROUND((K$14)/3.33,0)"]
["PRA12 (Food science DT art)","PRA12","Loose Furniture","Semi-circular table",null,"TAB02SC","if YR and/or KS1 only: SoA max group size / 5","CTS","Gp3","CTS"]
["PRA12 (Food science DT art)","PRA12","Loose Furniture","Semi-circular table",null,"TAB03SC","if any KS2: SoA max group size / 5","CTS","Gp3","/=ROUND((K$14)/5,0)"]
["PRA12 (Food science DT art)","PRA12","Loose Furniture","SS Trolley",null,"TRO001",null,null,"Gp3",1]
["PRA12 (Food science DT art)","PRA12","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",2]
["PRA12 (Food science DT art)","PRA12","Loose Equipment","Microwave",null,"APP001",null,null,"Gp3",2]
["PRA12 (Food science DT art)","PRA12","Loose Equipment","Compact fridge (Primary)",null,"APP004",null,null,"Gp3",1]
["PRA12 (Food science DT art)","PRA12","Loose Equipment","Spring loaded drier (A2)",null,"EQ213","1 if art","CTS","Gp3",1]
["PRA12 (Food science DT art)","PRA12","Loose Equipment","Spring loaded drier (A3)",null,"EQ214","1 if art","CTS","Gp3",1]
["PRA12 (Food science DT art)","PRA12","Loose Equipment","Art Easel  (Primary)",null,"EQ224","2 if art","CTS","Gp3",2]
["PRI03 (Nursery playroom)","PRI03","Fittings","Noticeboard ",null,"BOA002",null,null,"Gp2",3]
["PRI03 (Nursery playroom)","PRI03","Fittings","SS single bowl sink (right hand drainer)",null,"SIN004",null,null,"Gp2",1]
["PRI03 (Nursery playroom)","PRI03","Fittings","Worktop 600 deep Solid","(m length)","WKTH600S","to part of wall, or 1 wall if over 55m2",null,"Gp2","/=IF(K10>55,7.2,3.9)"]
["PRI03 (Nursery playroom)","PRI03","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["PRI03 (Nursery playroom)","PRI03","Fitted Furniture","Underbench 2 door cupboard",null,"CUB002","to match side benching length",null,"Gp2","/=ROUNDUP(M270/2,0)"]
["PRI03 (Nursery playroom)","PRI03","Fitted Furniture","Underbench paper unit",null,"CUB012","if over 55m2",null,"Gp2","/=IF(K14>55,1,0)"]
["PRI03 (Nursery playroom)","PRI03","Fitted Furniture","Wall cupboard unit (2 doors)",null,"CUP013","SoA max group size / 9",null,"Gp2","/=ROUND(K$14/9,0)"]
["PRI03 (Nursery playroom)","PRI03","Fitted Furniture","Shelving (set of 3)",null,"SHE100","SoA max group size / 13 + 3 if over 55m2",null,"Gp2","/=ROUND(K$14/11,0) + IF(K10>55,3,0)"]
["PRI03 (Nursery playroom)","PRI03","Fitted Furniture","Underbench 12 tray unit",null,"TRU004","to match side benching length",null,"Gp2","/=ROUNDDOWN(M270/2,0)"]
["PRI03 (Nursery playroom)","PRI03","Fitted equipment","No FF&E Listed of This Type"]
["PRI03 (Nursery playroom)","PRI03","Fixed Furniture","No FF&E Listed of This Type"]
["PRI03 (Nursery playroom)","PRI03","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["PRI03 (Nursery playroom)","PRI03","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["PRI03 (Nursery playroom)","PRI03","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",1]
["PRI03 (Nursery playroom)","PRI03","Loose Furniture","Classroom chair",null,"CHA002","SoA max group size - 2",null,"Gp3","/=K14-2"]
["PRI03 (Nursery playroom)","PRI03","Loose Furniture","Upholstered easy chair",null,"CHA200",null,null,"Gp3",1]
["PRI03 (Nursery playroom)","PRI03","Loose Furniture","Upholstered primay pupils easy chair",null,"CHA201","Max group size in SoA / 11",null,"Gp3","/=ROUND(K14/11,0)"]
["PRI03 (Nursery playroom)","PRI03","Loose Furniture","Screen (Low)",null,"SCR002",null,null,"Gp3",1]
["PRI03 (Nursery playroom)","PRI03","Loose Furniture","Kinderbox",null,"STO011",null,null,"Gp3",1]
["PRI03 (Nursery playroom)","PRI03","Loose Furniture","Trapezoidal table",null,"TAB02TZ","Max group size in SoA / 3",null,"Gp3","/=ROUNDDOWN(K14/3,0)"]
["PRI03 (Nursery playroom)","PRI03","Loose Furniture","Mobile book trolley (hinged)",null,"TR0002",null,null,"Gp3",1]
["PRI03 (Nursery playroom)","PRI03","Loose Furniture","18 Tray unit",null,"TRA002","Max group size in SoA / 11",null,"Gp3","/=ROUND(K14/11,0)"]
["PRI03 (Nursery playroom)","PRI03","Loose Equipment","Spring loaded drier (A3)",null,"EQ214",null,null,"Gp3",1]
["PRI03 (Nursery playroom)","PRI03","Loose Equipment","Art Easel  (Primary)",null,"EQ224",null,null,"Gp3",1]
["PRI03 (Nursery playroom)","PRI03","Loose Equipment","Oven (Role Play Kitchen)",null,"RP001",null,null,"Gp3",1]
["PRI03 (Nursery playroom)","PRI03","Loose Equipment","Sink (Role Play Kitchen)",null,"RP002",null,null,"Gp3",1]
["PRI03 (Nursery playroom)","PRI03","Loose Equipment","Fridge (Role Play Kitchen)",null,"RP003",null,null,"Gp3",1]
["PRI03 (Nursery playroom)","PRI03","Loose Equipment","Washing machine (Role Play Kitchen)",null,"RP004",null,null,"Gp3",1]
["PRI03 (Nursery playroom)","PRI03","Loose Equipment","Bed (Role play)",null,"RP005",null,null,"Gp3",1]
["PRI03 (Nursery playroom)","PRI03","Loose Equipment","Dressing up trolley",null,"RP007",null,null,"Gp3",1]
["PRI03 (Nursery playroom)","PRI03","Loose Equipment","Water Tray",null,"RP009",null,null,"Gp3",1]
["PRI04 (Nursery 2 to 3 year old)","PRI04","Fittings","Contractor to list FF&E of this type",null,"CTS001","based on discussion with school",null,"Gp2","CTS"]
["PRI04 (Nursery 2 to 3 year old)","PRI04","Fitted Furniture","Contractor to list FF&E of this type",null,"CTS002","based on discussion with school",null,"Gp2","CTS"]
["PRI04 (Nursery 2 to 3 year old)","PRI04","Fitted equipment","Contractor to list FF&E of this type",null,"CTS003","based on discussion with school",null,"Gp2","CTS"]
["PRI04 (Nursery 2 to 3 year old)","PRI04","Fixed Furniture","Contractor to list FF&E of this type",null,"CTS004","based on any legacy FF&E and discussion with school",null,"Gp2","CTS"]
["PRI04 (Nursery 2 to 3 year old)","PRI04","Fixed Equipment","Contractor to list FF&E of this type",null,"CTS005","based on any legacy FF&E and discussion with school",null,"Gp2","CTS"]
["PRI04 (Nursery 2 to 3 year old)","PRI04","Loose Furniture","Contractor to list FF&E of this type",null,"CTS006","based on any legacy FF&E and discussion with school",null,"Gp3","CTS"]
["PRI04 (Nursery 2 to 3 year old)","PRI04","Loose Equipment","Contractor to list FF&E of this type",null,"CTS007","based on any legacy FF&E and discussion with school",null,"Gp3","CTS"]
["PRI13 (Reception classroom)","PRI13","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",3]
["PRI13 (Reception classroom)","PRI13","Fittings","SS single bowl sink (right hand drainer)",null,"SIN004",null,null,"Gp2",1]
["PRI13 (Reception classroom)","PRI13","Fittings","Worktop 600 deep Solid","(m length)","WKTI600S","to part of 1 or 2 walls",null,"Gp2","/=IF(K$10>62,7.2,ROUND(K$10/11.3,1))"]
["PRI13 (Reception classroom)","PRI13","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["PRI13 (Reception classroom)","PRI13","Fitted Furniture","Underbench 2 door cupboard",null,"CUB002","SoA max group size / 7.5",null,"Gp2","/=ROUND(K$14/7.5,0)"]
["PRI13 (Reception classroom)","PRI13","Fitted Furniture","Underbench paper unit",null,"CUB012","SoA max group size / 30",null,"Gp2","/=ROUNDDOWN(K$14/30,0)"]
["PRI13 (Reception classroom)","PRI13","Fitted Furniture","Wall cupboard unit (2 doors)",null,"CUP013","SoA max group size / 15",null,"Gp2","/=ROUND(K$14/15,0)"]
["PRI13 (Reception classroom)","PRI13","Fitted Furniture","Underbench 18 tray unit",null,"TRU003","1 if area is more than 62m2",null,"Gp2","/=IF(K$10>62,1,0)"]
["PRI13 (Reception classroom)","PRI13","Fitted Furniture","Shelving (set of 3)",null,"SHE100","SoA max group size / 15 + 1",null,"Gp2","/=ROUND(K$14/15,0) + 1"]
["PRI13 (Reception classroom)","PRI13","Fitted equipment","No FF&E Listed of This Type"]
["PRI13 (Reception classroom)","PRI13","Fixed Furniture","No FF&E Listed of This Type"]
["PRI13 (Reception classroom)","PRI13","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["PRI13 (Reception classroom)","PRI13","Loose Furniture","Classroom chair",null,"CHA001","SoA max group size",null,"Gp3","/=ROUND(K$14,0)"]
["PRI13 (Reception classroom)","PRI13","Loose Furniture","Upholstered easy chair",null,"CHA200",null,null,"Gp3",1]
["PRI13 (Reception classroom)","PRI13","Loose Furniture","Upholstered primay pupils easy chair",null,"CHA201",null,null,"Gp3",2]
["PRI13 (Reception classroom)","PRI13","Loose Furniture","ICT Teachers chair",null,"CHA301",null,null,"Gp3",1]
["PRI13 (Reception classroom)","PRI13","Loose Furniture","Screen (Low)",null,"SCR002",null,null,"Gp3",1]
["PRI13 (Reception classroom)","PRI13","Loose Furniture","Kinderbox",null,"STO011",null,null,"Gp3",1]
["PRI13 (Reception classroom)","PRI13","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["PRI13 (Reception classroom)","PRI13","Loose Furniture","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["PRI13 (Reception classroom)","PRI13","Loose Furniture","Rectangular table",null,"TAB01R","SoA max group size - 2 x 0.3",null,"Gp3","/=ROUND((K$14-2)*0.3,0)"]
["PRI13 (Reception classroom)","PRI13","Loose Furniture","Trapezoidal table",null,"TAB01TZ","SoA max group size - 2 x 0.2",null,"Gp3","/=ROUND((K$14-2)*0.2,0)"]
["PRI13 (Reception classroom)","PRI13","Loose Furniture","Table, ICT/Admin ",null,"TAB501",null,null,"Gp3",1]
["PRI13 (Reception classroom)","PRI13","Loose Furniture","Mobile book trolley (hinged)",null,"TR0002",null,null,"Gp3",1]
["PRI13 (Reception classroom)","PRI13","Loose Furniture","18 Tray unit",null,"TRA002","SoA max group size / 15",null,"Gp3","/=ROUND(K$14/15,0)"]
["PRI13 (Reception classroom)","PRI13","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["PRI13 (Reception classroom)","PRI13","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",1]
["PRI13 (Reception classroom)","PRI13","Loose Equipment","Spring loaded drier (A3)",null,"EQ214",null,null,"Gp3",1]
["PRI13 (Reception classroom)","PRI13","Loose Equipment","Art Easel  (Primary)",null,"EQ224",null,null,"Gp3",1]
["PRI13 (Reception classroom)","PRI13","Loose Equipment","Oven (Role Play Kitchen)",null,"RP001",null,null,"Gp3",1]
["PRI13 (Reception classroom)","PRI13","Loose Equipment","Sink (Role Play Kitchen)",null,"RP002",null,null,"Gp3",1]
["PRI13 (Reception classroom)","PRI13","Loose Equipment","Fridge (Role Play Kitchen)",null,"RP003",null,null,"Gp3",1]
["PRI13 (Reception classroom)","PRI13","Loose Equipment","Washing machine (Role Play Kitchen)",null,"RP004",null,null,"Gp3",1]
["PRI13 (Reception classroom)","PRI13","Loose Equipment","Bed (Role play)",null,"RP005",null,null,"Gp3",1]
["PRI13 (Reception classroom)","PRI13","Loose Equipment","Dressing up trolley",null,"RP007",null,null,"Gp3",1]
["PRI13 (Reception classroom)","PRI13","Loose Equipment","Water Tray",null,"RP009",null,null,"Gp3",1]
["PRI22 (Classbase with sink)","PRI22","Fittings","Noticeboard ",null,"BOA002",null,null,"Gp2",2]
["PRI22 (Classbase with sink)","PRI22","Fittings","SS single bowl sink (left hand drainer)",null,"SIN005",null,null,"Gp2",1]
["PRI22 (Classbase with sink)","PRI22","Fittings","Worktop 600 deep Solid","(m length)","WKTI600S","To 1 wall","CTS","Gp2",5.5]
["PRI22 (Classbase with sink)","PRI22","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["PRI22 (Classbase with sink)","PRI22","Fitted Furniture","Underbench 2 door cupboard",null,"CUB002",null,null,"Gp2",5]
["PRI22 (Classbase with sink)","PRI22","Fitted Furniture","Underbench paper unit",null,"CUB012",null,null,"Gp2",1]
["PRI22 (Classbase with sink)","PRI22","Fitted Furniture","Wall cupboard unit (2 doors)",null,"CUP013",null,null,"Gp2",3]
["PRI22 (Classbase with sink)","PRI22","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",1]
["PRI22 (Classbase with sink)","PRI22","Fitted Furniture","Underbench 18 tray unit",null,"TRU003",null,null,"Gp2",1]
["PRI22 (Classbase with sink)","PRI22","Fitted equipment","No FF&E Listed of This Type"]
["PRI22 (Classbase with sink)","PRI22","Fixed Furniture","No FF&E Listed of This Type"]
["PRI22 (Classbase with sink)","PRI22","Fixed equipment","No FF&E Listed of This Type"]
["PRI22 (Classbase with sink)","PRI22","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["PRI22 (Classbase with sink)","PRI22","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",1]
["PRI22 (Classbase with sink)","PRI22","Loose Furniture","Classroom chair",null,"CHA002","either if YR and/or KS1 only","CTS","Gp3",30]
["PRI22 (Classbase with sink)","PRI22","Loose Furniture","Classroom chair ",null,"CHA003","or if any KS2","CTS","Gp3","CTS"]
["PRI22 (Classbase with sink)","PRI22","Loose Furniture","Upholstered easy chair",null,"CHA200",null,null,"Gp3",1]
["PRI22 (Classbase with sink)","PRI22","Loose Furniture","ICT Teachers chair",null,"CHA301",null,null,"Gp3",1]
["PRI22 (Classbase with sink)","PRI22","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["PRI22 (Classbase with sink)","PRI22","Loose Furniture","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["PRI22 (Classbase with sink)","PRI22","Loose Furniture","Rectangular table",null,"TAB02R","either if YR and/or KS1 only","CTS","Gp3",11]
["PRI22 (Classbase with sink)","PRI22","Loose Furniture","Rectangular table",null,"TAB03R","or if any KS2","CTS","Gp3","CTS"]
["PRI22 (Classbase with sink)","PRI22","Loose Furniture","Trapezoidal table",null,"TAB02TZ","either if YR and/or KS1 only","CTS","Gp3",2]
["PRI22 (Classbase with sink)","PRI22","Loose Furniture","Trapezoidal table",null,"TAB03TZ","or if any KS2","CTS","Gp3","CTS"]
["PRI22 (Classbase with sink)","PRI22","Loose Furniture","Table, ICT/Admin ",null,"TAB501",null,null,"Gp3",1]
["PRI22 (Classbase with sink)","PRI22","Loose Furniture","Mobile book trolley (hinged)",null,"TR0002",null,null,"Gp3",1]
["PRI22 (Classbase with sink)","PRI22","Loose Equipment","Spring loaded drier (A3)",null,"EQ214",null,null,"Gp3",1]
["PRI22 (Classbase with sink)","PRI22","Loose Equipment","Art Easel  (Primary)",null,"EQ224",null,null,"Gp3",1]
["PRI23 (Infant classroom)","PRI23","Fittings","Noticeboard ",null,"BOA002",null,null,"Gp2",2]
["PRI23 (Infant classroom)","PRI23","Fittings","SS single bowl sink (right hand drainer)",null,"SIN004",null,null,"Gp2",1]
["PRI23 (Infant classroom)","PRI23","Fittings","Worktop 600 deep Solid","(m length)","WKTI600S","To parts of 2 walls, or 1 wall if more than 55m2","CTS","Gp2","/=IF(K10>55,7.2,5.5)"]
["PRI23 (Infant classroom)","PRI23","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["PRI23 (Infant classroom)","PRI23","Fitted Furniture","Underbench 2 door cupboard",null,"CUB002","3, or 4 if more than 55m2","CTS","Gp2","/=IF(K$10>55,4,3)"]
["PRI23 (Infant classroom)","PRI23","Fitted Furniture","Underbench paper unit",null,"CUB012",null,null,"Gp2",1]
["PRI23 (Infant classroom)","PRI23","Fitted Furniture","Wall cupboard unit (2 doors)",null,"CUP013","2, or 3 if more than 55m2","CTS","Gp2","/=IF(K$10>55,3,2)"]
["PRI23 (Infant classroom)","PRI23","Fitted Furniture","Shelving (set of 3)",null,"SHE100","1, or 2 if more than 55m2","CTS","Gp2","/=IF(K$10>55,2,1)"]
["PRI23 (Infant classroom)","PRI23","Fitted Furniture","Underbench 18 tray unit",null,"TRU003",null,null,"Gp2",1]
["PRI23 (Infant classroom)","PRI23","Fitted equipment","No FF&E Listed of This Type"]
["PRI23 (Infant classroom)","PRI23","Fixed Furniture","No FF&E Listed of This Type"]
["PRI23 (Infant classroom)","PRI23","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["PRI23 (Infant classroom)","PRI23","Loose Furniture","Classroom chair",null,"CHA002","SoA max group size","CTS","Gp3","/=ROUND(K$14,0)"]
["PRI23 (Infant classroom)","PRI23","Loose Furniture","Upholstered easy chair",null,"CHA200",null,null,"Gp3",1]
["PRI23 (Infant classroom)","PRI23","Loose Furniture","Upholstered primay pupils easy chair",null,"CHA201",null,null,"Gp3",2]
["PRI23 (Infant classroom)","PRI23","Loose Furniture","ICT pupil chair ",null,"CHA300",null,null,"Gp3",2]
["PRI23 (Infant classroom)","PRI23","Loose Furniture","ICT Teachers chair",null,"CHA301",null,null,"Gp3",1]
["PRI23 (Infant classroom)","PRI23","Loose Furniture","Screen (Low)",null,"SCR002",null,null,"Gp3",1]
["PRI23 (Infant classroom)","PRI23","Loose Furniture","Kinderbox",null,"STO011",null,null,"Gp3",1]
["PRI23 (Infant classroom)","PRI23","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["PRI23 (Infant classroom)","PRI23","Loose Furniture","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["PRI23 (Infant classroom)","PRI23","Loose Furniture","Rectangular table",null,"TAB02R","SoA max group size / 2 - 1","CTS","Gp3","/=ROUND(K$14*0.5,0)-1"]
["PRI23 (Infant classroom)","PRI23","Loose Furniture","Trapezoidal table",null,"TAB02TZ",null,null,"Gp3",1]
["PRI23 (Infant classroom)","PRI23","Loose Furniture","Table, ICT/Admin ",null,"TAB501",null,null,"Gp3",1]
["PRI23 (Infant classroom)","PRI23","Loose Furniture","Table, Coffee",null,"TAB600",null,null,"Gp3",1]
["PRI23 (Infant classroom)","PRI23","Loose Furniture","Table, Coffee (round)",null,"TAB601",null,null,"Gp3",1]
["PRI23 (Infant classroom)","PRI23","Loose Furniture","Mobile book trolley (hinged)",null,"TR0002",null,null,"Gp3",1]
["PRI23 (Infant classroom)","PRI23","Loose Furniture","18 Tray unit",null,"TRA002",null,null,"Gp3",2]
["PRI23 (Infant classroom)","PRI23","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["PRI23 (Infant classroom)","PRI23","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",1]
["PRI23 (Infant classroom)","PRI23","Loose Equipment","Spring loaded drier (A3)",null,"EQ214",null,null,"Gp3",1]
["PRI23 (Infant classroom)","PRI23","Loose Equipment","Art Easel  (Primary)",null,"EQ224",null,null,"Gp3",1]
["PRI26 (Shared without sink)","PRI26","Fittings","No FF&E Listed of This Type"]
["PRI26 (Shared without sink)","PRI26","Fitted Furniture","No FF&E Listed of This Type"]
["PRI26 (Shared without sink)","PRI26","Fitted equipment","No FF&E Listed of This Type"]
["PRI26 (Shared without sink)","PRI26","Fixed Furniture","No FF&E Listed of This Type"]
["PRI26 (Shared without sink)","PRI26","Fixed Equipment","No FF&E Listed of This Type"]
["PRI26 (Shared without sink)","PRI26","Loose Furniture","Bookcase",null,"BOO001","SoA max group size / 5","CTS","Gp3","/=ROUND(K$14/5,0)"]
["PRI26 (Shared without sink)","PRI26","Loose Furniture","Classroom chair ",null,"CHA002","SoA max group size","CTS","Gp3","/=K$14"]
["PRI26 (Shared without sink)","PRI26","Loose Furniture","Rectangular table ",null,"TAB02R","SoA max group size / 5","CTS","Gp3","/=ROUND(K$14/5,0)"]
["PRI26 (Shared without sink)","PRI26","Loose Furniture","Trapezoidal table",null,"TAB02TZ","SoA max group size / 7","CTS","Gp4","/=ROUND(K$14/7,0)"]
["PRI26 (Shared without sink)","PRI26","Loose Furniture","18 Tray Unit",null,"TRA002","SoA max group size / 5","CTS","Gp3","/=ROUND(K$14/5,0)"]
["PRI26 (Shared without sink)","PRI26","Loose Furniture","Upholstered easy chair",null,"CHA200","SoA max group size / 5","CTS","Gp3","/=ROUND(K$14/5,0)"]
["PRI26 (Shared without sink)","PRI26","Loose Furniture","Screen (Low)",null,"SCR002",null,null,"Gp3",1]
["PRI26 (Shared without sink)","PRI26","Loose Equipment","No FF&E Listed of This Type"]
["PRI32 (Classbase without sink)","PRI32","Fittings","Noticeboard ",null,"BOA002",null,null,"Gp2",2]
["PRI32 (Classbase without sink)","PRI32","Fittings","Worktop 600 deep Solid","(m length)","WKTH600S","To part of 1 wall","CTS","Gp2",5.5]
["PRI32 (Classbase without sink)","PRI32","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["PRI32 (Classbase without sink)","PRI32","Fitted Furniture","Underbench 2 door cupboard",null,"CUB002",null,null,"Gp2",2]
["PRI32 (Classbase without sink)","PRI32","Fitted Furniture","Underbench paper unit",null,"CUB012",null,null,"Gp2",1]
["PRI32 (Classbase without sink)","PRI32","Fitted Furniture","Wall cupboard unit (2 doors)",null,"CUP013",null,null,"Gp2",2]
["PRI32 (Classbase without sink)","PRI32","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",1]
["PRI32 (Classbase without sink)","PRI32","Fitted equipment","No FF&E Listed of This Type"]
["PRI32 (Classbase without sink)","PRI32","Fixed Furniture","No FF&E Listed of This Type"]
["PRI32 (Classbase without sink)","PRI32","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["PRI32 (Classbase without sink)","PRI32","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["PRI32 (Classbase without sink)","PRI32","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",1]
["PRI32 (Classbase without sink)","PRI32","Loose Furniture","Classroom chair",null,"CHA002",null,null,"Gp3",30]
["PRI32 (Classbase without sink)","PRI32","Loose Furniture","Upholstered easy chair",null,"CHA200",null,null,"Gp3",1]
["PRI32 (Classbase without sink)","PRI32","Loose Furniture","ICT Teachers chair",null,"CHA301",null,null,"Gp3",1]
["PRI32 (Classbase without sink)","PRI32","Loose Furniture","Kinderbox",null,"STO011",null,null,"Gp3",1]
["PRI32 (Classbase without sink)","PRI32","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["PRI32 (Classbase without sink)","PRI32","Loose Furniture","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["PRI32 (Classbase without sink)","PRI32","Loose Furniture","Rectangular table",null,"TAB02R",null,null,"Gp3",11]
["PRI32 (Classbase without sink)","PRI32","Loose Furniture","Trapezoidal table",null,"TAB02TZ",null,null,"Gp3",2]
["PRI32 (Classbase without sink)","PRI32","Loose Furniture","Table, ICT/Admin ",null,"TAB501",null,null,"Gp3",1]
["PRI32 (Classbase without sink)","PRI32","Loose Furniture","Mobile book trolley (hinged)",null,"TR0002",null,null,"Gp3",1]
["PRI32 (Classbase without sink)","PRI32","Loose Furniture","18 Tray unit",null,"TRA002",null,null,"Gp3",2]
["PRI32 (Classbase without sink)","PRI32","Loose Equipment","No FF&E Listed of This Type"]
["PRI33 (Junior classroom)","PRI33","Fittings","Noticeboard ",null,"BOA002",null,null,"Gp2",2]
["PRI33 (Junior classroom)","PRI33","Fittings","SS single bowl sink (right hand drainer)",null,"SIN004",null,null,"Gp2",1]
["PRI33 (Junior classroom)","PRI33","Fittings","Worktop 600 deep",null,"WKTJ600","To parts of 2 walls, or 1 wall if more than 55m2","CTS","Gp2","/=IF(K$10>55,7.2,5.5)"]
["PRI33 (Junior classroom)","PRI33","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["PRI33 (Junior classroom)","PRI33","Fitted Furniture","Underbench 2 door cupboard",null,"CUB002","3, or 4 if more than 55m2",null,"Gp2","/=IF(K$10>55,4,3)"]
["PRI33 (Junior classroom)","PRI33","Fitted Furniture","Underbench paper unit",null,"CUB012",null,null,"Gp2",1]
["PRI33 (Junior classroom)","PRI33","Fitted Furniture","Wall cupboard unit (2 doors)",null,"CUP013","2, or 3 if more than 55m2",null,"Gp2","/=IF(K$10>55,3,2)"]
["PRI33 (Junior classroom)","PRI33","Fitted Furniture","Shelving (set of 3)",null,"SHE100","1, or 2 if more than 55m2",null,"Gp2","/=IF(K$10>55,2,1)"]
["PRI33 (Junior classroom)","PRI33","Fitted equipment","No FF&E Listed of This Type"]
["PRI33 (Junior classroom)","PRI33","Fixed Furniture","No FF&E Listed of This Type"]
["PRI33 (Junior classroom)","PRI33","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["PRI33 (Junior classroom)","PRI33","Loose Furniture","Classroom chair (Y3, 4, 5)",null,"CHA003","if Y3, 4 or 5: SoA max group size","CTS","Gp3","/=ROUND(K$14,0)"]
["PRI33 (Junior classroom)","PRI33","Loose Furniture","Classroom chair (Y6)",null,"CHA004","if Y6: SoA max group size ","CTS","Gp3","CTS"]
["PRI33 (Junior classroom)","PRI33","Loose Furniture","ICT pupil chair ",null,"CHA300","2 if extensive only (zone D)","CTS","Gp3","/=IF(K18=\"Zone D\", 2,0)"]
["PRI33 (Junior classroom)","PRI33","Loose Furniture","ICT Teachers chair",null,"CHA301",null,null,"Gp3",1]
["PRI33 (Junior classroom)","PRI33","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["PRI33 (Junior classroom)","PRI33","Loose Furniture","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["PRI33 (Junior classroom)","PRI33","Loose Furniture","Rectangular table (Y3, 4, 5)",null,"TAB03R","if Y3, 4 or 5: SoA max group size / 2 - 1","CTS","Gp3","/=ROUND(K$14*0.5,0)-1"]
["PRI33 (Junior classroom)","PRI33","Loose Furniture","Rectangular table (Y6)",null,"TAB04R","if Y6: SoA max group size / 2","CTS","Gp3","CTS"]
["PRI33 (Junior classroom)","PRI33","Loose Furniture","Table, ICT/Admin ",null,"TAB501",null,null,"Gp3",1]
["PRI33 (Junior classroom)","PRI33","Loose Furniture","18 Tray unit",null,"TRA002",null,null,"Gp3",2]
["PRI33 (Junior classroom)","PRI33","Loose Furniture","Bookcase",null,"BOO002","3 if Y6 class","CTS","Gp3","CTS"]
["PRI33 (Junior classroom)","PRI33","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["PRI33 (Junior classroom)","PRI33","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",1]
["PRI33 (Junior classroom)","PRI33","Loose Equipment","Spring loaded drier (A3)",null,"EQ214",null,null,"Gp3",1]
["PRI33 (Junior classroom)","PRI33","Loose Equipment","Art Easel  (Primary)",null,"EQ224",null,null,"Gp3",1]
["PRI36 (Shared teach with sink)","PRI36","Fittings","SS single bowl sink (right hand drainer)",null,"SIN004",null,null,"Gp2",1]
["PRI36 (Shared teach with sink)","PRI36","Fittings","Worktop 600 deep Solid","(m length)","WKTH600","To part of 1 wall","CTS","Gp2",2.4]
["PRI36 (Shared teach with sink)","PRI36","Fitted Furniture","No FF&E Listed of This Type"]
["PRI36 (Shared teach with sink)","PRI36","Fitted equipment","No FF&E Listed of This Type"]
["PRI36 (Shared teach with sink)","PRI36","Fixed Furniture","No FF&E Listed of This Type"]
["PRI36 (Shared teach with sink)","PRI36","Fixed Equipment","No FF&E Listed of This Type"]
["PRI36 (Shared teach with sink)","PRI36","Loose Furniture","Bookcase",null,"BOO001","SoA max group size / 5","CTS","Gp3","/=ROUND(K$14/5,0)"]
["PRI36 (Shared teach with sink)","PRI36","Loose Furniture","Classroom chair ",null,"CHA002","SoA max group size","CTS","Gp3","/=K$14"]
["PRI36 (Shared teach with sink)","PRI36","Loose Furniture","Semi circular table",null,"TAB02SC","SoA max group size / 3","CTS","Gp3","/=ROUND(K$14/3,0)"]
["PRI36 (Shared teach with sink)","PRI36","Loose Equipment","No FF&E Listed of This Type"]
["RES41 (Pupil changing (dry))","RES41","Fittings","Half Height mirror",null,"MIR002",null,null,"Gp2",1]
["RES41 (Pupil changing (dry))","RES41","Fitted Furniture","Single bench with integral hook rails","(m length)","BEN02X","400mm length per pupil in SoA max group size",null,"Gp2","/=K14*0.4"]
["RES41 (Pupil changing (dry))","RES41","Fitted equipment","No FF&E Listed of This Type"]
["RES41 (Pupil changing (dry))","RES41","Fixed Furniture","Clock (wall mounted)"]
["RES41 (Pupil changing (dry))","RES41","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["RES41 (Pupil changing (dry))","RES41","Loose Furniture","No FF&E Listed of This Type"]
["RES41 (Pupil changing (dry))","RES41","Loose Equipment","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["STT03 (Teaching storage bay)","STT03","Fittings","No FF&E Listed of This Type"]
["STT03 (Teaching storage bay)","STT03","Fitted Furniture","Stockroom shelving (set of 5) ","(m length)","SHE020","to fit 3 walls of storeroom","CTS","Gp2",5.0999999999999996]
["STT03 (Teaching storage bay)","STT03","Fitted equipment","No FF&E Listed of This Type"]
["STT03 (Teaching storage bay)","STT03","Fixed Furniture","No FF&E Listed of This Type"]
["STT03 (Teaching storage bay)","STT03","Fixed Equipment","No FF&E Listed of This Type"]
["STT03 (Teaching storage bay)","STT03","Loose Furniture","No FF&E Listed of This Type"]
["STT03 (Teaching storage bay)","STT03","Loose Equipment","No FF&E Listed of This Type"]
["TOC11 (Foundation toilets)","TOC11","Fittings","No FF&E Listed of This Type"]
["TOC11 (Foundation toilets)","TOC11","Fitted Furniture","No FF&E Listed of This Type"]
["TOC11 (Foundation toilets)","TOC11","Fitted equipment","No FF&E Listed of This Type"]
["TOC11 (Foundation toilets)","TOC11","Fixed Furniture","No FF&E Listed of This Type"]
["TOC11 (Foundation toilets)","TOC11","Fixed Equipment","No FF&E Listed of This Type"]
["TOC11 (Foundation toilets)","TOC11","Loose Furniture","No FF&E Listed of This Type"]
["TOC11 (Foundation toilets)","TOC11","Loose Equipment","No FF&E Listed of This Type"]
["ACT01 (Dance studio)","ACT01","Fittings","Barres","(m length)","BAR001","42-48mm diam. timber on two walls",null,"Gp2","/=ROUND((10*2)+(K10/5)-2,1)"]
["ACT01 (Dance studio)","ACT01","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["ACT01 (Dance studio)","ACT01","Fittings","Full height mirror","(m length)","MIR001","between 0.15 and 2.3m above FFL on one wall",null,"Gp2",7.8]
["ACT01 (Dance studio)","ACT01","Fitted Furniture","No FF&E Listed of This Type"]
["ACT01 (Dance studio)","ACT01","Fitted equipment","No FF&E Listed of This Type"]
["ACT01 (Dance studio)","ACT01","Fixed Furniture","No FF&E Listed of This Type"]
["ACT01 (Dance studio)","ACT01","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["ACT01 (Dance studio)","ACT01","Loose Furniture","No FF&E Listed of This Type"]
["ACT01 (Dance studio)","ACT01","Loose Equipment","No FF&E Listed of This Type"]
["ACT05 (Activity studio)","ACT05","Fittings","Barres",null,"BAR001","42-48mm diam. timber on one wall",null,"Gp2","/=ROUND((K10/5)-2,1)"]
["ACT05 (Activity studio)","ACT05","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["ACT05 (Activity studio)","ACT05","Fitted Furniture","No FF&E Listed of This Type"]
["ACT05 (Activity studio)","ACT05","Fitted equipment","No FF&E Listed of This Type"]
["ACT05 (Activity studio)","ACT05","Fixed Furniture","No FF&E Listed of This Type"]
["ACT05 (Activity studio)","ACT05","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["ACT05 (Activity studio)","ACT05","Loose Furniture","No FF&E Listed of This Type"]
["ACT05 (Activity studio)","ACT05","Loose Equipment","No FF&E Listed of This Type"]
["ACT22 (Fitness exercise)","ACT22","Fittings","No FF&E Listed of This Type"]
["ACT22 (Fitness exercise)","ACT22","Fitted Furniture","No FF&E Listed of This Type"]
["ACT22 (Fitness exercise)","ACT22","Fitted equipment","No FF&E Listed of This Type"]
["ACT22 (Fitness exercise)","ACT22","Fixed Furniture","Contractor to list FF&E of this type",null,"CTS005","based on any legacy FF&E and discussion with school",null,"Gp3","CTS"]
["ACT22 (Fitness exercise)","ACT22","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["ACT22 (Fitness exercise)","ACT22","Fixed Equipment","Contractor to list FF&E of this type",null,"CTS004","based on any legacy FF&E and discussion with school",null,"Gp3","CTS"]
["ACT22 (Fitness exercise)","ACT22","Loose Furniture","Contractor to list FF&E of this type",null,"CTS006","based on any legacy FF&E and discussion with school",null,"Gp3","CTS"]
["ACT22 (Fitness exercise)","ACT22","Loose Equipment","Contractor to list FF&E of this type",null,"CTS007","based on any legacy FF&E and discussion with school",null,"Gp3","CTS"]
["CLA02 (Seminar room)","CLA02","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["CLA02 (Seminar room)","CLA02","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["CLA02 (Seminar room)","CLA02","Fitted equipment","No FF&E Listed of This Type"]
["CLA02 (Seminar room)","CLA02","Fixed Furniture","No FF&E Listed of This Type"]
["CLA02 (Seminar room)","CLA02","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["CLA02 (Seminar room)","CLA02","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["CLA02 (Seminar room)","CLA02","Loose Furniture","Classroom chair",null,"CHA005","As SoA max group size",null,"Gp3","/=K14"]
["CLA02 (Seminar room)","CLA02","Loose Furniture","ICT staff chair",null,"CHA301",null,null,"Gp3",1]
["CLA02 (Seminar room)","CLA02","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["CLA02 (Seminar room)","CLA02","Loose Furniture","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["CLA02 (Seminar room)","CLA02","Loose Furniture","Rectangular table",null,"TAB06R","As SoA max group size / 2",null,"Gp3","/=ROUNDUP(K14/2,0)"]
["CLA02 (Seminar room)","CLA02","Loose Furniture","Table, ICT/Admin ",null,"TAB501",null,null,"Gp3",1]
["CLA02 (Seminar room)","CLA02","Loose Equipment","No FF&E Listed of This Type"]
["CLA12 (General classroom)","CLA12","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["CLA12 (General classroom)","CLA12","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["CLA12 (General classroom)","CLA12","Fitted equipment","No FF&E Listed of This Type"]
["CLA12 (General classroom)","CLA12","Fixed Furniture","No FF&E Listed of This Type"]
["CLA12 (General classroom)","CLA12","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["CLA12 (General classroom)","CLA12","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["CLA12 (General classroom)","CLA12","Loose Furniture","Classroom chair",null,"CHA005","As SoA max group size",null,"Gp3","/=K14"]
["CLA12 (General classroom)","CLA12","Loose Furniture","ICT staff chair",null,"CHA301",null,null,"Gp3",1]
["CLA12 (General classroom)","CLA12","Loose Furniture","Cupd unit 3 compartment",null,"CUP006","1 + 1 if over 60m2",null,"Gp3","/=IF(K10>60,2,1)"]
["CLA12 (General classroom)","CLA12","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["CLA12 (General classroom)","CLA12","Loose Furniture","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["CLA12 (General classroom)","CLA12","Loose Furniture","Rectangular table",null,"TAB06R","As SoA max group size / 2",null,"Gp3","/=ROUNDUP(K14/2,0)"]
["CLA12 (General classroom)","CLA12","Loose Furniture","Table, ICT/Admin ",null,"TAB501",null,null,"Gp3",1]
["CLA12 (General classroom)","CLA12","Loose Equipment","No FF&E Listed of This Type"]
["CLA13 (Extensive classroom)","CLA13","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["CLA13 (Extensive classroom)","CLA13","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["CLA13 (Extensive classroom)","CLA13","Fitted equipment","No FF&E Listed of This Type"]
["CLA13 (Extensive classroom)","CLA13","Fixed Furniture","No FF&E Listed of This Type"]
["CLA13 (Extensive classroom)","CLA13","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["CLA13 (Extensive classroom)","CLA13","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["CLA13 (Extensive classroom)","CLA13","Loose Furniture","Classroom chair",null,"CHA005","As SoA max group size",null,"Gp3","/=K14"]
["CLA13 (Extensive classroom)","CLA13","Loose Furniture","ICT staff chair",null,"CHA301",null,null,"Gp3",1]
["CLA13 (Extensive classroom)","CLA13","Loose Furniture","Cupd unit 3 compartment",null,"CUP006",null,null,"Gp3",1]
["CLA13 (Extensive classroom)","CLA13","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["CLA13 (Extensive classroom)","CLA13","Loose Furniture","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["CLA13 (Extensive classroom)","CLA13","Loose Furniture","Rectangular table",null,"TAB06R","As SoA max group size / 2",null,"Gp3","/=ROUNDUP(K14/2,0)"]
["CLA13 (Extensive classroom)","CLA13","Loose Furniture","Table, ICT/Admin ",null,"TAB501",null,null,"Gp3",1]
["CLA13 (Extensive classroom)","CLA13","Loose Equipment","No FF&E Listed of This Type"]
["CLA18 (Open learning area)","CLA18","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["CLA18 (Open learning area)","CLA18","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["CLA18 (Open learning area)","CLA18","Fitted equipment","No FF&E Listed of This Type"]
["CLA18 (Open learning area)","CLA18","Fixed Furniture","No FF&E Listed of This Type"]
["CLA18 (Open learning area)","CLA18","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["CLA18 (Open learning area)","CLA18","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["CLA18 (Open learning area)","CLA18","Loose Furniture","Classroom chair",null,"CHA005","As SoA max group size",null,"Gp3","/=K14"]
["CLA18 (Open learning area)","CLA18","Loose Furniture","ICT staff chair",null,"CHA301",null,null,"Gp3",1]
["CLA18 (Open learning area)","CLA18","Loose Furniture","Cupd unit 3 compartment",null,"CUP006",null,null,"Gp3",1]
["CLA18 (Open learning area)","CLA18","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["CLA18 (Open learning area)","CLA18","Loose Furniture","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["CLA18 (Open learning area)","CLA18","Loose Furniture","Rectangular table",null,"TAB06R","As SoA max group size / 2",null,"Gp3","/=ROUNDUP(K14/2,0)"]
["CLA18 (Open learning area)","CLA18","Loose Furniture","Table, ICT/Admin ",null,"TAB501",null,null,"Gp3",1]
["CLA18 (Open learning area)","CLA18","Loose Equipment","No FF&E Listed of This Type"]
["CLA31 (Temporarily ICT-rich...)","CLA31","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["CLA31 (Temporarily ICT-rich...)","CLA31","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["CLA31 (Temporarily ICT-rich...)","CLA31","Fitted Furniture","Shelving (set of 3)",null,"SHE100"]
["CLA31 (Temporarily ICT-rich...)","CLA31","Fitted equipment","No FF&E Listed of This Type"]
["CLA31 (Temporarily ICT-rich...)","CLA31","Fixed Furniture","No FF&E Listed of This Type"]
["CLA31 (Temporarily ICT-rich...)","CLA31","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["CLA31 (Temporarily ICT-rich...)","CLA31","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["CLA31 (Temporarily ICT-rich...)","CLA31","Loose Furniture","ICT pupil chair ",null,"CHA300","As max group size",null,"Gp3","/=K14"]
["CLA31 (Temporarily ICT-rich...)","CLA31","Loose Furniture","ICT staff chair",null,"CHA301",null,null,"Gp3",1]
["CLA31 (Temporarily ICT-rich...)","CLA31","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["CLA31 (Temporarily ICT-rich...)","CLA31","Loose Furniture","Adjustable table",null,"TAB002",null,null,"Gp3",1]
["CLA31 (Temporarily ICT-rich...)","CLA31","Loose Furniture","Rectangular table",null,"TAB06R","As SoA max group size / 2",null,"Gp3","/=ROUNDUP(K14/2,0)"]
["CLA31 (Temporarily ICT-rich...)","CLA31","Loose Furniture","Table, ICT/Admin ",null,"TAB502",null,null,"Gp3",1]
["CLA31 (Temporarily ICT-rich...)","CLA31","Loose Equipment","No FF&E Listed of This Type"]
["CLA32 (ICT-rich classroom)","CLA32","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",2]
["CLA32 (ICT-rich classroom)","CLA32","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",2]
["CLA32 (ICT-rich classroom)","CLA32","Fittings","Worktop 1200 deep ","(m length)","WKTI12","to 2 peninsulas from 1 wall.",null,"Gp2","/=ROUND(K$14*0.22,0)"]
["CLA32 (ICT-rich classroom)","CLA32","Fittings","Worktop 600 deep Solid","(m length)","WKTK600S","To 2 walls. ",null,"Gp2","/=ROUND(K$14*0.48,0)"]
["CLA32 (ICT-rich classroom)","CLA32","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["CLA32 (ICT-rich classroom)","CLA32","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",4]
["CLA32 (ICT-rich classroom)","CLA32","Fitted equipment","No FF&E Listed of This Type"]
["CLA32 (ICT-rich classroom)","CLA32","Fixed Furniture","No FF&E Listed of This Type"]
["CLA32 (ICT-rich classroom)","CLA32","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["CLA32 (ICT-rich classroom)","CLA32","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp2",1]
["CLA32 (ICT-rich classroom)","CLA32","Loose Furniture","ICT pupil chair ",null,"CHA300","As max group size",null,"Gp2","/=K14"]
["CLA32 (ICT-rich classroom)","CLA32","Loose Furniture","ICT staff chair",null,"CHA301",null,null,"Gp2",1]
["CLA32 (ICT-rich classroom)","CLA32","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp2",1]
["CLA32 (ICT-rich classroom)","CLA32","Loose Furniture","Adjustable table",null,"TAB002",null,null,"Gp2",1]
["CLA32 (ICT-rich classroom)","CLA32","Loose Furniture","Table, ICT/Admin ",null,"TAB502",null,null,"Gp2",1]
["CLA32 (ICT-rich classroom)","CLA32","Loose Equipment","No FF&E Listed of This Type"]
["CLA35 (ICT-rich learning area)","CLA35","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",2]
["CLA35 (ICT-rich learning area)","CLA35","Fittings","Worktop 1200 deep ",null,"WKTI12","to 2 peninsulas from column, power-pole or similar",null,"Gp2","/=ROUND(K$14*0.22,0)"]
["CLA35 (ICT-rich learning area)","CLA35","Fittings","Worktop 600 deep Solid",null,"WKTK600S","To 2 walls. ",null,"Gp2","/=ROUND(K$14*0.48,0)"]
["CLA35 (ICT-rich learning area)","CLA35","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["CLA35 (ICT-rich learning area)","CLA35","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",4]
["CLA35 (ICT-rich learning area)","CLA35","Fitted equipment","No FF&E Listed of This Type"]
["CLA35 (ICT-rich learning area)","CLA35","Fixed Furniture","No FF&E Listed of This Type"]
["CLA35 (ICT-rich learning area)","CLA35","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["CLA35 (ICT-rich learning area)","CLA35","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp2",1]
["CLA35 (ICT-rich learning area)","CLA35","Loose Furniture","ICT pupil chair ",null,"CHA300","As max group size",null,"Gp2","/=K14"]
["CLA35 (ICT-rich learning area)","CLA35","Loose Furniture","ICT staff chair",null,"CHA301",null,null,"Gp2",1]
["CLA35 (ICT-rich learning area)","CLA35","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp2",1]
["CLA35 (ICT-rich learning area)","CLA35","Loose Furniture","Adjustable table",null,"TAB002",null,null,"Gp2",1]
["CLA35 (ICT-rich learning area)","CLA35","Loose Furniture","Table, ICT/Admin ",null,"TAB502",null,null,"Gp2",1]
["CLA35 (ICT-rich learning area)","CLA35","Loose Equipment","No FF&E Listed of This Type"]
["CLA41 (ICT and business stu...","CLA41","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",2]
["CLA41 (ICT and business stu...","CLA41","Fittings","Worktop 750 deep ","(m length)","WKTI75","to 2 walls",null,"Gp2","/=ROUND(7.8+(K10/7.8),1)"]
["CLA41 (ICT and business stu...","CLA41","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["CLA41 (ICT and business stu...","CLA41","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",4]
["CLA41 (ICT and business stu...","CLA41","Fitted equipment","No FF&E Listed of This Type"]
["CLA41 (ICT and business stu...","CLA41","Fixed Furniture","No FF&E Listed of This Type"]
["CLA41 (ICT and business stu...","CLA41","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["CLA41 (ICT and business stu...","CLA41","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["CLA41 (ICT and business stu...","CLA41","Loose Furniture","ICT pupil chair ",null,"CHA300","As SoA max group size",null,"Gp3","/=K14"]
["CLA41 (ICT and business stu...","CLA41","Loose Furniture","ICT staff chair",null,"CHA301",null,null,"Gp3",1]
["CLA41 (ICT and business stu...","CLA41","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["CLA41 (ICT and business stu...","CLA41","Loose Furniture","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["CLA41 (ICT and business stu...","CLA41","Loose Furniture","Rectangular table",null,"TAB06R","As SoA max group size / 4",null,"Gp3","/=ROUNDDOWN(K14/4,0)"]
["CLA41 (ICT and business stu...","CLA41","Loose Furniture","Table, ICT/Admin ",null,"TAB502",null,null,"Gp3",1]
["CLA41 (ICT and business stu...","CLA41","Loose Equipment","No FF&E Listed of This Type"]
["DAT02 (General art room)","DAT02","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",3]
["DAT02 (General art room)","DAT02","Fittings","Belfast sink (large)",null,"SIN001",null,null,"Gp2",2]
["DAT02 (General art room)","DAT02","Fittings","Worktop 600 deep Solid","(m length)","WKTK600S","to 2 walls, except door",null,"Gp2","/=ROUND(7.8+(K10/7.8)-2,1)"]
["DAT02 (General art room)","DAT02","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["DAT02 (General art room)","DAT02","Fitted Furniture","Underbench 2 door cupboard",null,"CUB004",null,null,"Gp2",4]
["DAT02 (General art room)","DAT02","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",6]
["DAT02 (General art room)","DAT02","Fitted Furniture","Underbench 24 tray unit",null,"TRU001",null,null,"Gp2",2]
["DAT02 (General art room)","DAT02","Fitted Furniture","Underbench portfolio unit",null,"TRU005",null,null,"Gp2",2]
["DAT02 (General art room)","DAT02","Fitted equipment","No FF&E Listed of This Type"]
["DAT02 (General art room)","DAT02","Fixed Furniture","Coats and bags storage unit",null,"STO05X",null,null,"Gp3",2]
["DAT02 (General art room)","DAT02","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["DAT02 (General art room)","DAT02","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["DAT02 (General art room)","DAT02","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",3]
["DAT02 (General art room)","DAT02","Loose Furniture","Practical stool",null,"CHA024","As SoA max group size - ICT pupil chairs",null,"Gp3","/=K14-M287"]
["DAT02 (General art room)","DAT02","Loose Furniture","ICT pupil chair ",null,"CHA300","only if above 83m2",null,"Gp3","/=IF(K10/1>83,2,0)"]
["DAT02 (General art room)","DAT02","Loose Furniture","ICT staff chair",null,"CHA301",null,null,"Gp3",1]
["DAT02 (General art room)","DAT02","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["DAT02 (General art room)","DAT02","Loose Furniture","Adjustable table",null,"TAB003",null,null,"Gp3",1]
["DAT02 (General art room)","DAT02","Loose Furniture","ICT table (Pupils) ",null,"TAB010","only if above 83m2",null,"Gp3","/=IF(K14/1>83,1,0)"]
["DAT02 (General art room)","DAT02","Loose Furniture","Practical rectangular table",null,"TAB204","As SoA max group size / 2",null,"Gp3","/=ROUNDUP(K14/2,0)"]
["DAT02 (General art room)","DAT02","Loose Furniture","Table, ICT/Admin ",null,"TAB502",null,null,"Gp3",1]
["DAT02 (General art room)","DAT02","Loose Equipment","Spring loaded drier (A2)",null,"EQ213",null,null,"Gp3",2]
["DAT02 (General art room)","DAT02","Loose Equipment","Desk mounted Easel trolley",null,"EQ222",null,null,"Gp3",1]
["DAT02 (General art room)","DAT02","Loose Equipment","Lightbox ",null,"EQ225",null,null,"Gp3",1]
["DAT03 (3D Art room)","DAT03","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",4]
["DAT03 (3D Art room)","DAT03","Fittings","Belfast sink (large)",null,"SIN001",null,null,"Gp2",2]
["DAT03 (3D Art room)","DAT03","Fittings","Worktop 600 deep Solid","(m length)","WKTK600S","to 2 walls, except door",null,"Gp2","/=ROUND(7.8+(K10/7.8)-2,1)"]
["DAT03 (3D Art room)","DAT03","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["DAT03 (3D Art room)","DAT03","Fitted Furniture","Underbench 2 door cupboard",null,"CUB004",null,null,"Gp2",5]
["DAT03 (3D Art room)","DAT03","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",5]
["DAT03 (3D Art room)","DAT03","Fitted Furniture","Underbench 24 tray unit",null,"TRU001",null,null,"Gp2",2]
["DAT03 (3D Art room)","DAT03","Fitted Furniture","Underbench portfolio unit",null,"TRU005",null,null,"Gp2",2]
["DAT03 (3D Art room)","DAT03","Fitted equipment","No FF&E Listed of This Type"]
["DAT03 (3D Art room)","DAT03","Fixed Furniture","Coats and bags storage unit",null,"STO05X",null,null,"Gp2",2]
["DAT03 (3D Art room)","DAT03","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["DAT03 (3D Art room)","DAT03","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["DAT03 (3D Art room)","DAT03","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",3]
["DAT03 (3D Art room)","DAT03","Loose Furniture","Practical stool",null,"CHA024","As SoA max group size",null,"Gp3","/=K14"]
["DAT03 (3D Art room)","DAT03","Loose Furniture","ICT staff chair",null,"CHA301",null,null,"Gp3",1]
["DAT03 (3D Art room)","DAT03","Loose Furniture","Cupboard unit (2 doors)",null,"CUP003",null,null,"Gp3",1]
["DAT03 (3D Art room)","DAT03","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["DAT03 (3D Art room)","DAT03","Loose Furniture","Adjustable table",null,"TAB003",null,null,"Gp3",1]
["DAT03 (3D Art room)","DAT03","Loose Furniture","Practical rectangular table",null,"TAB204","As SoA max group size / 2 + 1",null,"Gp3","/=ROUND(K14/2,0)+1"]
["DAT03 (3D Art room)","DAT03","Loose Furniture","Table, ICT/Admin ",null,"TAB501",null,null,"Gp3",1]
["DAT03 (3D Art room)","DAT03","Loose Equipment","Spring loaded drier (A2)",null,"EQ213",null,null,"Gp3",1]
["DAT03 (3D Art room)","DAT03","Loose Equipment","Desk mounted Easel trolley",null,"EQ222",null,null,"Gp3",1]
["DAT03 (3D Art room)","DAT03","Loose Equipment","Lightbox ",null,"EQ225",null,null,"Gp3",1]
["DAT03 (3D Art room)","DAT03","Loose Equipment","Sculpture stand",null,"EQ226",null,null,"Gp3",2]
["DAT04 (3D art room (ceramics))","DAT04","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",4]
["DAT04 (3D art room (ceramics))","DAT04","Fittings","Belfast sink (large)",null,"SIN001",null,null,"Gp2",2]
["DAT04 (3D art room (ceramics))","DAT04","Fittings","Worktop 600 deep Solid","(m length)","WKTK600S","to 2 walls, except door",null,"Gp2","/=ROUND(7.8+(K10/7.8)-2,1)"]
["DAT04 (3D art room (ceramics))","DAT04","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["DAT04 (3D art room (ceramics))","DAT04","Fitted Furniture","Underbench 2 door cupboard",null,"CUB004",null,null,"Gp2",6]
["DAT04 (3D art room (ceramics))","DAT04","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",4]
["DAT04 (3D art room (ceramics))","DAT04","Fitted Furniture","Underbench 24 tray unit",null,"TRU001",null,null,"Gp2",4]
["DAT04 (3D art room (ceramics))","DAT04","Fitted Furniture","Underbench portfolio unit",null,"TRU005",null,null,"Gp2",1]
["DAT04 (3D art room (ceramics))","DAT04","Fitted equipment","No FF&E Listed of This Type"]
["DAT04 (3D art room (ceramics))","DAT04","Fixed Furniture","Coats and bags storage unit",null,"STO05X",null,null,"Gp2",2]
["DAT04 (3D art room (ceramics))","DAT04","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["DAT04 (3D art room (ceramics))","DAT04","Fixed Equipment","Pugg mill",null,"EQ001X",null,null,"Gp2",1]
["DAT04 (3D art room (ceramics))","DAT04","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["DAT04 (3D art room (ceramics))","DAT04","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",3]
["DAT04 (3D art room (ceramics))","DAT04","Loose Furniture","Practical stool",null,"CHA024","As SoA max group size",null,"Gp3","/=K14"]
["DAT04 (3D art room (ceramics))","DAT04","Loose Furniture","ICT staff chair",null,"CHA301",null,null,"Gp3",1]
["DAT04 (3D art room (ceramics))","DAT04","Loose Furniture","Cupboard unit (2 doors)",null,"CUP003",null,null,"Gp3",1]
["DAT04 (3D art room (ceramics))","DAT04","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["DAT04 (3D art room (ceramics))","DAT04","Loose Furniture","Adjustable table",null,"TAB003",null,null,"Gp3",1]
["DAT04 (3D art room (ceramics))","DAT04","Loose Furniture","Practical rectangular table",null,"TAB204","As SoA max group size / 2",null,"Gp3","/=K14/2"]
["DAT04 (3D art room (ceramics))","DAT04","Loose Furniture","Wedging bench",null,"TAB400",null,null,"Gp3",1]
["DAT04 (3D art room (ceramics))","DAT04","Loose Furniture","Table, ICT/Admin ",null,"TAB502",null,null,"Gp3",1]
["DAT04 (3D art room (ceramics))","DAT04","Loose Equipment","Spring loaded drier (A2)",null,"EQ213",null,null,"Gp3",1]
["DAT04 (3D art room (ceramics))","DAT04","Loose Equipment","Desk mounted Easel trolley",null,"EQ222",null,null,"Gp3",1]
["DAT05 (3D art room (textiles)","DAT05","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",4]
["DAT05 (3D art room (textiles)","DAT05","Fittings","Belfast sink (large)",null,"SIN001",null,null,"Gp2",2]
["DAT05 (3D art room (textiles)","DAT05","Fittings","Screen wash sink",null,"SIN009",null,null,"Gp2",1]
["DAT05 (3D art room (textiles)","DAT05","Fittings","Worktop 600 deep Solid","(m length)","WKTK600S","to 2 walls, except screenwash sink",null,"Gp2","/=ROUND(6.5+(K10/7.8),1)"]
["DAT05 (3D art room (textiles)","DAT05","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["DAT05 (3D art room (textiles)","DAT05","Fitted Furniture","Underbench 2 door cupboard",null,"CUB004",null,null,"Gp2",5]
["DAT05 (3D art room (textiles)","DAT05","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",4]
["DAT05 (3D art room (textiles)","DAT05","Fitted Furniture","Underbench 24 tray unit",null,"TRU001",null,null,"Gp2",2]
["DAT05 (3D art room (textiles)","DAT05","Fitted Furniture","Underbench portfolio unit",null,"TRU005",null,null,"Gp2",2]
["DAT05 (3D art room (textiles)","DAT05","Fitted equipment","No FF&E Listed of This Type"]
["DAT05 (3D art room (textiles)","DAT05","Fixed Furniture","Coats and bags storage unit",null,"STO05X",null,null,"Gp2",2]
["DAT05 (3D art room (textiles)","DAT05","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp2",1]
["DAT05 (3D art room (textiles)","DAT05","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["DAT05 (3D art room (textiles)","DAT05","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",3]
["DAT05 (3D art room (textiles)","DAT05","Loose Furniture","Practical stool",null,"CHA024","As SoA max group size",null,"Gp3","/=K14"]
["DAT05 (3D art room (textiles)","DAT05","Loose Furniture","ICT staff chair",null,"CHA301",null,null,"Gp3",1]
["DAT05 (3D art room (textiles)","DAT05","Loose Furniture","Cupboard unit (2 doors)",null,"CUP003",null,null,"Gp3",1]
["DAT05 (3D art room (textiles)","DAT05","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["DAT05 (3D art room (textiles)","DAT05","Loose Furniture","Adjustable table",null,"TAB003",null,null,"Gp3",1]
["DAT05 (3D art room (textiles)","DAT05","Loose Furniture","Practical rectangular table",null,"TAB204","As SoA max group size / 2",null,"Gp3","/=K14/2"]
["DAT05 (3D art room (textiles)","DAT05","Loose Furniture","Screen Printing table",null,"TAB401",null,null,"Gp3",1]
["DAT05 (3D art room (textiles)","DAT05","Loose Furniture","Table, ICT/Admin ",null,"TAB502",null,null,"Gp3",1]
["DAT05 (3D art room (textiles)","DAT05","Loose Equipment","Spring loaded drier (A2)",null,"EQ213",null,null,"Gp3",1]
["DAT05 (3D art room (textiles)","DAT05","Loose Equipment","Desk mounted Easel trolley",null,"EQ222",null,null,"Gp3",1]
["DAT12 (Hair and beauty salo","DAT12","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["DAT12 (Hair and beauty salo","DAT12","Fittings","Curtian tracking","(m length)","CUR001","SoA max group size / 3",null,"Gp2","/=2.9*M285"]
["DAT12 (Hair and beauty salo","DAT12","Fittings","Curtains","(m length)","CUR002","SoA max group size / 3",null,"Gp2","/=ROUND(M269*1.33,1)"]
["DAT12 (Hair and beauty salo","DAT12","Fittings","Half Height mirror",null,"MIR002","SoA max group size / 3",null,"Gp2","/=ROUND(K14/3,0)"]
["DAT12 (Hair and beauty salo","DAT12","Fittings","Specialist backwash sinks",null,"SIN008","SoA max group size / 9",null,"Gp2","/=ROUND(K14/9,0)"]
["DAT12 (Hair and beauty salo","DAT12","Fittings","Worktop 450 deep Solid","(m length)","WKTI450S","to 2 walls, except door",null,"Gp2","/=ROUND(7.8+(K10/7.8)-2,1)"]
["DAT12 (Hair and beauty salo","DAT12","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["DAT12 (Hair and beauty salo","DAT12","Fitted Furniture","Underbench 2 door cupboard",null,"CUB004",null,null,"Gp2",2]
["DAT12 (Hair and beauty salo","DAT12","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",2]
["DAT12 (Hair and beauty salo","DAT12","Fitted equipment","No FF&E Listed of This Type"]
["DAT12 (Hair and beauty salo","DAT12","Fixed Furniture","Coats and bags storage unit",null,"STO05X",null,null,"Gp2",2]
["DAT12 (Hair and beauty salo","DAT12","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["DAT12 (Hair and beauty salo","DAT12","Loose Furniture","Specialist massage bed",null,"BED002","SoA max group size / 3",null,"Gp3","/=ROUND(K$14/3,0)"]
["DAT12 (Hair and beauty salo","DAT12","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["DAT12 (Hair and beauty salo","DAT12","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",2]
["DAT12 (Hair and beauty salo","DAT12","Loose Furniture","Upholstered easy chair",null,"CHA200","SoA max group size / 8",null,"Gp2","/=ROUND(K$14/8,0)"]
["DAT12 (Hair and beauty salo","DAT12","Loose Furniture","ICT staff chair",null,"CHA301",null,null,"Gp3",2]
["DAT12 (Hair and beauty salo","DAT12","Loose Furniture","Salon chair with arms",null,"CHA305","SoA max group size / 1.5",null,"Gp3","/=ROUND(K$14/1.5,0)"]
["DAT12 (Hair and beauty salo","DAT12","Loose Furniture","Circular mobile tilt top table",null,"DIN005",null,null,"Gp3",1]
["DAT12 (Hair and beauty salo","DAT12","Loose Furniture","Specialist mobile salon trolley unit",null,"RAC007","SoA max group size / 1.5",null,"Gp3","/=ROUND(K$14/1.5,0)"]
["DAT12 (Hair and beauty salo","DAT12","Loose Furniture","Screen",null,"SCR001","SoA max group size / 8",null,"Gp2","/=ROUND(K$14/8,0)"]
["DAT12 (Hair and beauty salo","DAT12","Loose Furniture","Table, ICT/Admin ",null,"TAB502",null,null,"Gp3",1]
["DAT12 (Hair and beauty salo","DAT12","Loose Furniture","Sepcialist manicure table with drawers",null,"TAB700",null,null,"Gp3",1]
["DAT12 (Hair and beauty salo","DAT12","Loose Equipment","No FF&E Listed of This Type"]
["DAT15 (Photography studio)","DAT15","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["DAT15 (Photography studio)","DAT15","Fittings","SS single bowl sink (right hand drainer)",null,"SIN004",null,null,"Gp2",1]
["DAT15 (Photography studio)","DAT15","Fittings","Worktop 600 deep Solid","(m length)","WKTK600S","to full-length of external wall","CTS","Gp2","CTS"]
["DAT15 (Photography studio)","DAT15","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["DAT15 (Photography studio)","DAT15","Fitted Furniture","Underbench 2 door cupboard",null,"CUB004",null,null,"Gp2",4]
["DAT15 (Photography studio)","DAT15","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",2]
["DAT15 (Photography studio)","DAT15","Fitted Furniture","Underbench 24 tray unit",null,"TRU001",null,null,"Gp2",2]
["DAT15 (Photography studio)","DAT15","Fitted Furniture","Underbench portfolio unit",null,"TRU005",null,null,"Gp2",1]
["DAT15 (Photography studio)","DAT15","Fitted equipment","No FF&E Listed of This Type"]
["DAT15 (Photography studio)","DAT15","Fixed Furniture","No FF&E Listed of This Type"]
["DAT15 (Photography studio)","DAT15","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["DAT15 (Photography studio)","DAT15","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",2]
["DAT15 (Photography studio)","DAT15","Loose Furniture","Practical stool",null,"CHA024","as SoA max group size",null,"Gp3","/=ROUND(K$14,0)"]
["DAT15 (Photography studio)","DAT15","Loose Furniture","ICT staff chair",null,"CHA301",null,null,"Gp3",1]
["DAT15 (Photography studio)","DAT15","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["DAT15 (Photography studio)","DAT15","Loose Furniture","Adjustable table",null,"TAB003",null,null,"Gp3",1]
["DAT15 (Photography studio)","DAT15","Loose Furniture","Practical rectangular table",null,"TAB204","as SoA max group size / 2",null,"Gp3","/=ROUND(K$14,0)"]
["DAT15 (Photography studio)","DAT15","Loose Furniture","Table, ICT/Admin ",null,"TAB502",null,null,"Gp3",1]
["DAT15 (Photography studio)","DAT15","Loose Equipment","Photo light tent",null,"EQ233",null,null,"Gp3",1]
["DAT15 (Photography studio)","DAT15","Loose Equipment","Lightbox ",null,"EQ225",null,null,"Gp3",1]
["DAT15 (Photography studio)","DAT15","Loose Equipment","Screen",null,"SCR001",null,null,"Gp3",2]
["DAT15 (Photography studio)","DAT15","Loose Equipment","Stage lanterns with stand",null,"LIG001",null,null,"Gp3",1]
["DAT22 (Graphic products)","DAT22","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["DAT22 (Graphic products)","DAT22","Fittings","SS single bowl sink (right hand drainer)",null,"SIN004",null,null,"Gp2",1]
["DAT22 (Graphic products)","DAT22","Fittings","Worktop 1200 deep ","(m length)","WKTI12",null,null,"Gp2",6]
["DAT22 (Graphic products)","DAT22","Fittings","Worktop 750 deep ","(m length)","WKTI75","2 peninsulas from 1 wall",null,"Gp2",7]
["DAT22 (Graphic products)","DAT22","Fittings","Worktop 600 deep Solid","(m length)","WKTK600S","to 1 wall",null,"Gp2",5]
["DAT22 (Graphic products)","DAT22","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["DAT22 (Graphic products)","DAT22","Fitted Furniture","Underbench 2 door cupboard",null,"CUB004",null,null,"Gp2",3]
["DAT22 (Graphic products)","DAT22","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",4]
["DAT22 (Graphic products)","DAT22","Fitted Furniture","Underbench 24 tray unit",null,"TRU001",null,null,"Gp2",1]
["DAT22 (Graphic products)","DAT22","Fitted equipment","No FF&E Listed of This Type"]
["DAT22 (Graphic products)","DAT22","Fixed Furniture","No FF&E Listed of This Type"]
["DAT22 (Graphic products)","DAT22","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["DAT22 (Graphic products)","DAT22","Fixed Equipment","Scrollsaw",null,"MAC016X",null,null,"Gp3",1]
["DAT22 (Graphic products)","DAT22","Fixed Equipment","CNC Engraver",null,"MAC101X",null,null,"Gp3",1]
["DAT22 (Graphic products)","DAT22","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["DAT22 (Graphic products)","DAT22","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",2]
["DAT22 (Graphic products)","DAT22","Loose Furniture","Practical stool",null,"CHA024",null,null,"Gp3",8]
["DAT22 (Graphic products)","DAT22","Loose Furniture","ICT pupil chair ",null,"CHA300",null,null,"Gp3",18]
["DAT22 (Graphic products)","DAT22","Loose Furniture","ICT staff chair",null,"CHA301",null,null,"Gp3",1]
["DAT22 (Graphic products)","DAT22","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["DAT22 (Graphic products)","DAT22","Loose Furniture","Adjustable table",null,"TAB002",null,null,"Gp3",1]
["DAT22 (Graphic products)","DAT22","Loose Furniture","Practical rectangular table",null,"TAB205",null,null,"Gp3",2]
["DAT22 (Graphic products)","DAT22","Loose Furniture","Table, ICT/Admin ",null,"TAB501",null,null,"Gp3",1]
["DAT22 (Graphic products)","DAT22","Loose Furniture","Table, ICT/Admin ",null,"TAB502",null,null,"Gp3",1]
["DAT22 (Graphic products)","DAT22","Loose Furniture","24 Tray unit",null,"TRA003",null,null,"Gp3",1]
["DAT22 (Graphic products)","DAT22","Loose Equipment","Plastics strip bender",null,"EQ201",null,null,"Gp3",1]
["DAT22 (Graphic products)","DAT22","Loose Equipment","Lightbox ",null,"EQ225",null,null,"Gp3",1]
["DAT22 (Graphic products)","DAT22","Loose Equipment","Drawing boards trolley",null,"EQ230",null,null,"Gp3",1]
["DAT22 (Graphic products)","DAT22","Loose Equipment","Vacuum former (large)",null,"MAC106",null,null,"Gp3",1]
["DAT22 (Graphic products)","DAT22","Loose Equipment","CNC Cutter/plotter",null,"MAC107X",null,null,"Gp3",1]
["DAT25 (Constructional texti...","DAT25","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",3]
["DAT25 (Constructional texti...","DAT25","Fittings","SS single bowl sink (right hand drainer)",null,"SIN004",null,null,"Gp2",1]
["DAT25 (Constructional texti...","DAT25","Fittings","Worktop 600 deep Solid","(m length)","WKTK600S","to 1 wall",null,"Gp2",7.8]
["DAT25 (Constructional texti...","DAT25","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["DAT25 (Constructional texti...","DAT25","Fitted Furniture","Underbench 2 door cupboard",null,"CUB004",null,null,"Gp2",3]
["DAT25 (Constructional texti...","DAT25","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",6]
["DAT25 (Constructional texti...","DAT25","Fitted Furniture","Underbench 24 tray unit",null,"TRU001",null,null,"Gp2",3]
["DAT25 (Constructional texti...","DAT25","Fitted equipment","No FF&E Listed of This Type"]
["DAT25 (Constructional texti...","DAT25","Fixed Furniture","No FF&E Listed of This Type"]
["DAT25 (Constructional texti...","DAT25","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["DAT25 (Constructional texti...","DAT25","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["DAT25 (Constructional texti...","DAT25","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",2]
["DAT25 (Constructional texti...","DAT25","Loose Furniture","ICT pupil chair ",null,"CHA300",null,null,"Gp3",24]
["DAT25 (Constructional texti...","DAT25","Loose Furniture","ICT staff chair",null,"CHA301",null,null,"Gp3",1]
["DAT25 (Constructional texti...","DAT25","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["DAT25 (Constructional texti...","DAT25","Loose Furniture","Adjustable table",null,"TAB004",null,null,"Gp3",1]
["DAT25 (Constructional texti...","DAT25","Loose Furniture","Practical rectangular table",null,"TAB201",null,null,"Gp3",15]
["DAT25 (Constructional texti...","DAT25","Loose Furniture","Practical rectangular table",null,"TAB206",null,null,"Gp3",1]
["DAT25 (Constructional texti...","DAT25","Loose Furniture","Table, ICT/Admin ",null,"TAB502",null,null,"Gp3",1]
["DAT25 (Constructional texti...","DAT25","Loose Furniture","24 Tray unit",null,"TRA003",null,null,"Gp3",1]
["DAT25 (Constructional texti...","DAT25","Loose Equipment","Spring loaded drier (A3)",null,"EQ214",null,null,"Gp3",1]
["DAT25 (Constructional texti...","DAT25","Loose Equipment","Lightbox ",null,"EQ225",null,null,"Gp3",1]
["DAT28 (Electronics and cont...","DAT28","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["DAT28 (Electronics and cont...","DAT28","Fittings","SS single bowl sink (right hand drainer)",null,"SIN004",null,null,"Gp2",1]
["DAT28 (Electronics and cont...","DAT28","Fittings","Worktop 1200 deep ","(m length)","WKTI12","2 peninsula from external wall",null,"Gp2",6]
["DAT28 (Electronics and cont...","DAT28","Fittings","Worktop 600 deep Solid","(m length)","WKTK600S","to 1 wall",null,"Gp2",13.5]
["DAT28 (Electronics and cont...","DAT28","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["DAT28 (Electronics and cont...","DAT28","Fitted Furniture","Underbench 2 door cupboard",null,"CUB004",null,null,"Gp2",6]
["DAT28 (Electronics and cont...","DAT28","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",4]
["DAT28 (Electronics and cont...","DAT28","Fitted Furniture","Underbench 24 tray unit",null,"TRU001",null,null,"Gp2",1]
["DAT28 (Electronics and cont...","DAT28","Fitted equipment","No FF&E Listed of This Type"]
["DAT28 (Electronics and cont...","DAT28","Fixed Furniture","No FF&E Listed of This Type"]
["DAT28 (Electronics and cont...","DAT28","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["DAT28 (Electronics and cont...","DAT28","Fixed Equipment","Bench vice",null,"EQ001X",null,null,"Gp3",1]
["DAT28 (Electronics and cont...","DAT28","Fixed Equipment","Scrollsaw",null,"MAC016X",null,null,"Gp3",1]
["DAT28 (Electronics and cont...","DAT28","Fixed Equipment","Bench Sander",null,"MAC018X",null,null,"Gp3",1]
["DAT28 (Electronics and cont...","DAT28","Fixed Equipment","CAD Engraver",null,"MAC101X",null,null,"Gp3",1]
["DAT28 (Electronics and cont...","DAT28","Fixed Equipment","CAD Cutter/plotter",null,"MAC107X",null,null,"Gp3",1]
["DAT28 (Electronics and cont...","DAT28","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["DAT28 (Electronics and cont...","DAT28","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",2]
["DAT28 (Electronics and cont...","DAT28","Loose Furniture","Practical stool",null,"CHA024",null,null,"Gp3",8]
["DAT28 (Electronics and cont...","DAT28","Loose Furniture","ICT pupil chair ",null,"CHA300",null,null,"Gp3",16]
["DAT28 (Electronics and cont...","DAT28","Loose Furniture","ICT staff chair",null,"CHA301",null,null,"Gp3",1]
["DAT28 (Electronics and cont...","DAT28","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["DAT28 (Electronics and cont...","DAT28","Loose Furniture","Adjustable table",null,"TAB002",null,null,"Gp3",1]
["DAT28 (Electronics and cont...","DAT28","Loose Furniture","Practical rectangular table",null,"TAB201",null,null,"Gp3",1]
["DAT28 (Electronics and cont...","DAT28","Loose Furniture","Practical rectangular table",null,"TAB205",null,null,"Gp3",2]
["DAT28 (Electronics and cont...","DAT28","Loose Furniture","Table, ICT/Admin ",null,"TAB501",null,null,"Gp3",1]
["DAT28 (Electronics and cont...","DAT28","Loose Furniture","24 Tray unit",null,"TRA003",null,null,"Gp3",1]
["DAT28 (Electronics and cont...","DAT28","Loose Equipment","Drawing boards trolley",null,"EQ230",null,null,"Gp3",1]
["DAT28 (Electronics and cont...","DAT28","Loose Equipment","PCB Spray Processor",null,"MAC105",null,null,"Gp3",2]
["DAT28 (Electronics and cont...","DAT28","Loose Equipment","Cutter/plotter",null,"MAC109",null,null,"Gp3",1]
["DAT32 (Food studio)","DAT32","Fittings","SS single bowl sink (right hand drainer)",null,"SIN004",null,null,"Gp2",1]
["DAT32 (Food studio)","DAT32","Fittings","Hand wash basin",null,"SIN007",null,null,"Gp2",1]
["DAT32 (Food studio)","DAT32","Fittings","Worktop 600 deep ","(m length)","WKTL600S","To 1 wall and teachers demo bench",null,"Gp2",13.5]
["DAT32 (Food studio)","DAT32","Fittings","Infill panel to demo bench",null,"FFE934",null,null,"Gp2",1]
["DAT32 (Food studio)","DAT32","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["DAT32 (Food studio)","DAT32","Fitted Furniture","Underbench 2 door cupboard",null,"CUB005",null,null,"Gp2",8]
["DAT32 (Food studio)","DAT32","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",4]
["DAT32 (Food studio)","DAT32","Fitted equipment","No FF&E Listed of This Type"]
["DAT32 (Food studio)","DAT32","Fixed Furniture","No FF&E Listed of This Type"]
["DAT32 (Food studio)","DAT32","Fixed Equipment","Cooker (electric)",null,"APP002X","or bulit-in oven and hob",null,"Gp2",1]
["DAT32 (Food studio)","DAT32","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["DAT32 (Food studio)","DAT32","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["DAT32 (Food studio)","DAT32","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",2]
["DAT32 (Food studio)","DAT32","Loose Furniture","Practical stool",null,"CHA024","As SoA max group size ",null,"Gp3","/=K14"]
["DAT32 (Food studio)","DAT32","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["DAT32 (Food studio)","DAT32","Loose Furniture","Adjustable table",null,"TAB003",null,null,"Gp3",1]
["DAT32 (Food studio)","DAT32","Loose Furniture","Practical rectangular table",null,"TAB208",null,null,"Gp3","/=K14/2"]
["DAT32 (Food studio)","DAT32","Loose Furniture","24 Tray unit",null,"TRA003",null,null,"Gp3",1]
["DAT32 (Food studio)","DAT32","Loose Equipment","No FF&E Listed of This Type"]
["DAT35 (Food room)","DAT35","Fittings","SS single bowl sink (right hand drainer)",null,"SIN004",null,null,"Gp2",1]
["DAT35 (Food room)","DAT35","Fittings","SS single bowl sink (left hand drainer)",null,"SIN005","SoA max group size / 12",null,"Gp2","/=ROUND(K$14/12,0)"]
["DAT35 (Food room)","DAT35","Fittings","SS double bowl sink (double drainer) ",null,"SIN006","SoA max group size / 5",null,"Gp2","/=ROUND(K$14/5,0)"]
["DAT35 (Food room)","DAT35","Fittings","Hand wash basin",null,"SIN007",null,null,"Gp2",1]
["DAT35 (Food room)","DAT35","Fittings","Worktop 1200 deep ","(m length)","WKTL12S","3 x 2.4m peninsulas from 1 wall",null,"Gp2",7.2]
["DAT35 (Food room)","DAT35","Fittings","Worktop 600 deep ","(m length)","WKTL600S","to 3 walls, except door","CTS","Gp2","/=ROUND((2*K10/7.8)+7.8+1.8,1)"]
["DAT35 (Food room)","DAT35","Fittings","Worktop 600 deep ","(m length)","WKTL600S","1 for demonstration, except if 97m2 '1 of 2' food rooms",null,"Gp2","CTS"]
["DAT35 (Food room)","DAT35","Fittings","Infill panel to demo bench",null,"FFE934",null,null,"Gp2",1]
["DAT35 (Food room)","DAT35","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["DAT35 (Food room)","DAT35","Fitted Furniture","Underbench 2 door cupboard",null,"CUB005",null,null,"Gp2","/=ROUND(K$14/1.5,0)"]
["DAT35 (Food room)","DAT35","Fitted Furniture","Underbench 1 door cupboard",null,"CUB009",null,null,"Gp2","/=ROUND(K$14/1.33,0)"]
["DAT35 (Food room)","DAT35","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",3]
["DAT35 (Food room)","DAT35","Fitted Furniture","Practical adjustable table (hob)",null,"TAB100","1, except if 97m2 '2 of 2' food rooms",null,"Gp2","CTS"]
["DAT35 (Food room)","DAT35","Fitted Furniture","Practical adjustable table (sink)",null,"TAB101","1, except if 97m2 '2 of 2' food rooms",null,"Gp2","CTS"]
["DAT35 (Food room)","DAT35","Fitted equipment","No FF&E Listed of This Type"]
["DAT35 (Food room)","DAT35","Fixed Furniture","No FF&E Listed of This Type"]
["DAT35 (Food room)","DAT35","Fixed Equipment","Cooker (electric)",null,"APP002X","SoA max group size / 4",null,"Gp2","/=ROUND(K$14/4,0)"]
["DAT35 (Food room)","DAT35","Fixed Equipment","Cooker (gas)",null,"APP003X","SoA max group size / 4 - 1",null,"Gp2","/=ROUND(K$14/4,0)-1"]
["DAT35 (Food room)","DAT35","Fixed Equipment","Cooker hob (electric inset)",null,"APP001","1 for demonstration, except if 97m2 '1 of 2' food rooms",null,"Gp2","CTS"]
["DAT35 (Food room)","DAT35","Fixed Equipment","Oven (inset)",null,"APP003","1 for demonstration, except if 97m2 '1 of 2' food rooms",null,"Gp2","CTS"]
["DAT35 (Food room)","DAT35","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["DAT35 (Food room)","DAT35","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["DAT35 (Food room)","DAT35","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",2]
["DAT35 (Food room)","DAT35","Loose Furniture","Practical stool",null,"CHA024","SoA max group size",null,"Gp3","/=K$14"]
["DAT35 (Food room)","DAT35","Loose Furniture","Adjustable table",null,"TAB003",null,null,"Gp3",1]
["DAT35 (Food room)","DAT35","Loose Furniture","Practical rectangular table",null,"TAB208","SoA max group size / 2 - 1",null,"Gp3","/=ROUND(K$14/2,0)-1"]
["DAT35 (Food room)","DAT35","Loose Equipment","Microwave",null,"APP001",null,null,"Gp3",3]
["DAT43 (Resistant materials ...","DAT43","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["DAT43 (Resistant materials ...","DAT43","Fittings","SS single bowl sink (right hand drainer)",null,"SIN004",null,null,"Gp2",1]
["DAT43 (Resistant materials ...","DAT43","Fittings","Worktop 600 deep Solid","(m length)","WKTK600S","to part of 1 wall",null,"Gp2",7.8]
["DAT43 (Resistant materials ...","DAT43","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["DAT43 (Resistant materials ...","DAT43","Fitted Furniture","Underbench 2 door cupboard",null,"CUB005",null,null,"Gp2",5]
["DAT43 (Resistant materials ...","DAT43","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",2]
["DAT43 (Resistant materials ...","DAT43","Fitted Furniture","Underbench 24 tray unit",null,"TRU001",null,null,"Gp2",1]
["DAT43 (Resistant materials ...","DAT43","Fitted equipment","No FF&E Listed of This Type"]
["DAT43 (Resistant materials ...","DAT43","Fixed Furniture","Coats and bags storage unit",null,"STO05X","2 if 104m2 single workshop",null,"Gp2","CTS"]
["DAT43 (Resistant materials ...","DAT43","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["DAT43 (Resistant materials ...","DAT43","Fixed Equipment","Floorstanding Drill",null,"MAC001X",null,null,"Gp2",2]
["DAT43 (Resistant materials ...","DAT43","Fixed Equipment","Bandfacer",null,"MAC002X",null,null,"Gp2",2]
["DAT43 (Resistant materials ...","DAT43","Fixed Equipment","Polisher",null,"MAC003X",null,null,"Gp2",1]
["DAT43 (Resistant materials ...","DAT43","Fixed Equipment","Metal lathe",null,"MAC004X","1, except if 97m2 '1 of 2' workshops",null,"Gp2","CTS"]
["DAT43 (Resistant materials ...","DAT43","Fixed Equipment","Scrollsaw",null,"MAC016X",null,null,"Gp2",1]
["DAT43 (Resistant materials ...","DAT43","Fixed Equipment","CAD Engraver",null,"MAC101X",null,null,"Gp2",1]
["DAT43 (Resistant materials ...","DAT43","Fixed Equipment","CAD Router",null,"MAC106X",null,null,"Gp2",1]
["DAT43 (Resistant materials ...","DAT43","Fixed Equipment","CNC Lathe",null,"MAC104X",null,null,"Gp2",1]
["DAT43 (Resistant materials ...","DAT43","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["DAT43 (Resistant materials ...","DAT43","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",2]
["DAT43 (Resistant materials ...","DAT43","Loose Furniture","Practical stool",null,"CHA024",null,null,"Gp3",24]
["DAT43 (Resistant materials ...","DAT43","Loose Furniture","Tool cupboard (2 doors)",null,"CUP010",null,null,"Gp3",2]
["DAT43 (Resistant materials ...","DAT43","Loose Furniture","Practical rectangular table",null,"TAB210","2 if 104m2 single workshop",null,"Gp3","CTS"]
["DAT43 (Resistant materials ...","DAT43","Loose Furniture","Practical rectangular table",null,"TAB203",null,null,"Gp3",3]
["DAT43 (Resistant materials ...","DAT43","Loose Furniture","RM adjustable table",null,"TAB310",null,null,"Gp3",1]
["DAT43 (Resistant materials ...","DAT43","Loose Furniture","Workshop multi bench (4 positions)",null,"TAB311",null,null,"Gp3",5]
["DAT43 (Resistant materials ...","DAT43","Loose Furniture","Workshop multi bench (2 positions)",null,"TAB312",null,null,"Gp3",1]
["DAT43 (Resistant materials ...","DAT43","Loose Furniture","60 Tray unit (2 doors)",null,"TRA004",null,null,"Gp3",2]
["DAT43 (Resistant materials ...","DAT43","Loose Equipment","Plastics Line bender",null,"EQ201",null,null,"Gp3",1]
["DAT43 (Resistant materials ...","DAT43","Loose Equipment","Fretsaw",null,"EQ202",null,null,"Gp3",1]
["DAT43 (Resistant materials ...","DAT43","Loose Equipment","Vacuum former (large)",null,"MAC106","1, except if 97m2 '2 of 2' workshops",null,"Gp3","CTS"]
["DAT46 (RM with heat bay)","DAT46","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["DAT46 (RM with heat bay)","DAT46","Fittings","SS single bowl sink (right hand drainer)",null,"SIN004",null,null,"Gp2",1]
["DAT46 (RM with heat bay)","DAT46","Fittings","Worktop 600 deep Solid","(m length)","WKTK600S","to part of 1 wall","CTS","Gp2",4.5]
["DAT46 (RM with heat bay)","DAT46","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["DAT46 (RM with heat bay)","DAT46","Fitted Furniture","Underbench 2 door cupboard",null,"CUB005",null,null,"Gp2",3]
["DAT46 (RM with heat bay)","DAT46","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",1]
["DAT46 (RM with heat bay)","DAT46","Fitted equipment","No FF&E Listed of This Type"]
["DAT46 (RM with heat bay)","DAT46","Fixed Furniture","No FF&E Listed of This Type"]
["DAT46 (RM with heat bay)","DAT46","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["DAT46 (RM with heat bay)","DAT46","Fixed Equipment","Chip forge",null,"MAC009X",null,null,"Gp2",1]
["DAT46 (RM with heat bay)","DAT46","Fixed Equipment","Floorstanding Drill",null,"MAC001X",null,null,"Gp2",1]
["DAT46 (RM with heat bay)","DAT46","Fixed Equipment","Bandfacer",null,"MAC002X",null,null,"Gp2",1]
["DAT46 (RM with heat bay)","DAT46","Fixed Equipment","Polisher",null,"MAC003X",null,null,"Gp2",1]
["DAT46 (RM with heat bay)","DAT46","Fixed Equipment","Metal lathe",null,"MAC004X",null,null,"Gp2",1]
["DAT46 (RM with heat bay)","DAT46","Fixed Equipment","Crucible furnace",null,"MAC011X",null,null,"Gp2",1]
["DAT46 (RM with heat bay)","DAT46","Fixed Equipment","Scrollsaw",null,"MAC016X",null,null,"Gp2",1]
["DAT46 (RM with heat bay)","DAT46","Fixed Equipment","CAD Engraver",null,"MAC101X",null,null,"Gp2",1]
["DAT46 (RM with heat bay)","DAT46","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["DAT46 (RM with heat bay)","DAT46","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",2]
["DAT46 (RM with heat bay)","DAT46","Loose Furniture","Practical stool",null,"CHA024","SoA max group size ",null,"Gp3","/=K14"]
["DAT46 (RM with heat bay)","DAT46","Loose Furniture","Tool cupboard (2 doors)",null,"CUP010",null,null,"Gp3",1]
["DAT46 (RM with heat bay)","DAT46","Loose Furniture","RM adjustable table",null,"TAB310",null,null,"Gp3",1]
["DAT46 (RM with heat bay)","DAT46","Loose Furniture","Workshop multi bench (4 positions)",null,"TAB311","SoA max group size / 4 - 1",null,"Gp3","/=ROUND(K$14/4,0)-1"]
["DAT46 (RM with heat bay)","DAT46","Loose Furniture","Workshop multi bench (2 positions)",null,"TAB312",null,null,"Gp3",1]
["DAT46 (RM with heat bay)","DAT46","Loose Furniture","Heat treatment table with vice",null,"TAB313",null,null,"Gp3",1]
["DAT46 (RM with heat bay)","DAT46","Loose Furniture","24 Tray unit",null,"TRA003",null,null,"Gp3",1]
["DAT46 (RM with heat bay)","DAT46","Loose Equipment","Plastics Line bender",null,"EQ201",null,null,"Gp3",1]
["DAT46 (RM with heat bay)","DAT46","Loose Equipment","Fretsaw",null,"EQ202",null,null,"Gp3",1]
["DAT46 (RM with heat bay)","DAT46","Loose Equipment","Moulding bench",null,"EQ205",null,null,"Gp3",1]
["DAT46 (RM with heat bay)","DAT46","Loose Equipment","CNC Lathe",null,"MAC104X",null,null,"Gp3",1]
["DAT46 (RM with heat bay)","DAT46","Loose Equipment","CNC Printer",null,"MAC105X",null,null,"Gp3",1]
["DAT46 (RM with heat bay)","DAT46","Loose Equipment","Vacuum former (small)",null,"MAC106",null,null,"Gp3",1]
["DAT48 (Engineering workshop)","DAT48","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["DAT48 (Engineering workshop)","DAT48","Fittings","SS single bowl sink (right hand drainer)",null,"SIN004",null,null,"Gp2",1]
["DAT48 (Engineering workshop)","DAT48","Fittings","Worktop 600 deep Solid","(m length)","WKTK600S","to half of 1 wall",null,"Gp2","/=ROUND(K10/15.6,1)"]
["DAT48 (Engineering workshop)","DAT48","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["DAT48 (Engineering workshop)","DAT48","Fitted Furniture","Underbench 2 door cupboard",null,"CUB005",null,null,"Gp2",3]
["DAT48 (Engineering workshop)","DAT48","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",1]
["DAT48 (Engineering workshop)","DAT48","Fitted Furniture","Underbench 24 tray unit",null,"TRU001",null,null,"Gp2",1]
["DAT48 (Engineering workshop)","DAT48","Fitted equipment","No FF&E Listed of This Type"]
["DAT48 (Engineering workshop)","DAT48","Fixed Furniture","Coats and bags storage unit",null,"STO05X",null,null,"Gp2",1]
["DAT48 (Engineering workshop)","DAT48","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["DAT48 (Engineering workshop)","DAT48","Fixed Equipment","Floorstanding Drill",null,"MAC001X",null,null,"Gp2",1]
["DAT48 (Engineering workshop)","DAT48","Fixed Equipment","Polisher",null,"MAC003X",null,null,"Gp2",1]
["DAT48 (Engineering workshop)","DAT48","Fixed Equipment","Metal lathe",null,"MAC004X",null,null,"Gp2",1]
["DAT48 (Engineering workshop)","DAT48","Fixed Equipment","Milling machine",null,"MAC014X","Only if 104m2 workshop or larger",null,"Gp2",1]
["DAT48 (Engineering workshop)","DAT48","Fixed Equipment","Crucible furnace",null,"MAC011X",null,null,"Gp2",1]
["DAT48 (Engineering workshop)","DAT48","Fixed Equipment","Scrollsaw",null,"MAC016X",null,null,"Gp2",1]
["DAT48 (Engineering workshop)","DAT48","Fixed Equipment","Bench grinder",null,"MAC019X",null,null,"Gp2",1]
["DAT48 (Engineering workshop)","DAT48","Fixed Equipment","Welding bench",null,"MAC024X",null,null,"Gp2",1]
["DAT48 (Engineering workshop)","DAT48","Fixed Equipment","CNC Engraver",null,"MAC101X",null,null,"Gp2",1]
["DAT48 (Engineering workshop)","DAT48","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["DAT48 (Engineering workshop)","DAT48","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",2]
["DAT48 (Engineering workshop)","DAT48","Loose Furniture","Practical stool",null,"CHA024","SoA max group size ",null,"Gp3","/=K14"]
["DAT48 (Engineering workshop)","DAT48","Loose Furniture","Tool cupboard (2 doors)",null,"CUP010",null,null,"Gp3",2]
["DAT48 (Engineering workshop)","DAT48","Loose Furniture","RM adjustable table",null,"TAB310",null,null,"Gp3",1]
["DAT48 (Engineering workshop)","DAT48","Loose Furniture","Workshop multi bench (4 positions)",null,"TAB311","SoA max group size / 4 - 1",null,"Gp3","/=ROUND(K$14/4,0)-1"]
["DAT48 (Engineering workshop)","DAT48","Loose Furniture","Heat treatment table with vice",null,"TAB313",null,null,"Gp3",2]
["DAT48 (Engineering workshop)","DAT48","Loose Equipment","Tube bender",null,"EQ202",null,null,"Gp3",1]
["DAT48 (Engineering workshop)","DAT48","Loose Equipment","Sheet metal bender",null,"EQ204",null,null,"Gp3",1]
["DAT48 (Engineering workshop)","DAT48","Loose Equipment","Moulding bench",null,"EQ205",null,null,"Gp3",1]
["DAT48 (Engineering workshop)","DAT48","Loose Equipment","CNC Lathe",null,"MAC104X",null,null,"Gp3",1]
["DAT48 (Engineering workshop)","DAT48","Loose Equipment","CNC Laser cutter",null,"MAC108",null,null,"Gp3",1]
["DAT49 (Construction workshop)","DAT49","Fittings","Contractor to list FF&E of this type",null,"CTS001","based on discussion with school",null,"Gp2","CTS"]
["DAT49 (Construction workshop)","DAT49","Fitted Furniture","Contractor to list FF&E of this type",null,"CTS002","based on discussion with school",null,"Gp2","CTS"]
["DAT49 (Construction workshop)","DAT49","Fitted equipment","Contractor to list FF&E of this type",null,"CTS003","based on discussion with school",null,"Gp2","CTS"]
["DAT49 (Construction workshop)","DAT49","Fixed Furniture","Contractor to list FF&E of this type",null,"CTS004","based on any legacy FF&E and discussion with school",null,"Gp2","CTS"]
["DAT49 (Construction workshop)","DAT49","Fixed Equipment","Contractor to list FF&E of this type",null,"CTS005","based on any legacy FF&E and discussion with school",null,"Gp2","CTS"]
["DAT49 (Construction workshop)","DAT49","Loose Furniture","Contractor to list FF&E of this type",null,"CTS006","based on any legacy FF&E and discussion with school",null,"Gp3","CTS"]
["DAT49 (Construction workshop)","DAT49","Loose Equipment","Contractor to list FF&E of this type",null,"CTS007","based on any legacy FF&E and discussion with school",null,"Gp3","CTS"]
["DIN04 (Social space)","DIN04","Fittings","Noticeboard ",null,"BOA002",null,null,"Gp2",3]
["DIN04 (Social space)","DIN04","Fittings","Worktop 600 deep Solid","(m length)","WKTM600S","To 1 wall.  As max group size / 9",null,"Gp2","/=ROUND(K$14/9,1)"]
["DIN04 (Social space)","DIN04","Fitted Furniture","No FF&E Listed of This Type"]
["DIN04 (Social space)","DIN04","Fitted equipment","No FF&E Listed of This Type"]
["DIN04 (Social space)","DIN04","Fixed Furniture","Coats and bags storage unit",null,"STO05X",null,null,"Gp3",1]
["DIN04 (Social space)","DIN04","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["DIN04 (Social space)","DIN04","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",2]
["DIN04 (Social space)","DIN04","Loose Furniture","Upholstered easy chair",null,"CHA200","As SoA max group size / 1.1",null,"Gp3","/=ROUND(K$14/1.1,0)"]
["DIN04 (Social space)","DIN04","Loose Furniture","ICT pupil chair ",null,"CHA300","As SoA max group size / 9 ",null,"Gp3","/=ROUND(K$14/9,0)"]
["DIN04 (Social space)","DIN04","Loose Furniture","Screen",null,"SCR001","As SoA max group size / 11",null,"Gp3","/=ROUND(K$14/11,0)"]
["DIN04 (Social space)","DIN04","Loose Furniture","Table, Coffee (round)",null,"TAB601","As SoA max group size / 9 ",null,"Gp3","/=ROUND(K$14/9,0)"]
["DIN04 (Social space)","DIN04","Loose Equipment","No FF&E Listed of This Type"]
["DIN05 (Sixth form social sp...","DIN05","Fittings","Noticeboard ",null,"BOA002",null,null,"Gp2",3]
["DIN05 (Sixth form social sp...","DIN05","Fittings","Worktop 600 deep Solid","(m length)","WKTM600S","To 1 wall.  As max group size / 9",null,"Gp2","/=ROUND(K$14/9,1)"]
["DIN05 (Sixth form social sp...","DIN05","Fitted Furniture","No FF&E Listed of This Type"]
["DIN05 (Sixth form social sp...","DIN05","Fitted equipment","No FF&E Listed of This Type"]
["DIN05 (Sixth form social sp...","DIN05","Fixed Furniture","Coats and bags storage unit",null,"STO05X",null,null,"Gp3",1]
["DIN05 (Sixth form social sp...","DIN05","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["DIN05 (Sixth form social sp...","DIN05","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",2]
["DIN05 (Sixth form social sp...","DIN05","Loose Furniture","Upholstered easy chair",null,"CHA200","As SoA max group size / 1.25",null,"Gp3","/=ROUND(K$14/1.25,0)"]
["DIN05 (Sixth form social sp...","DIN05","Loose Furniture","ICT pupil chair ",null,"CHA300","As SoA max group size / 9 ",null,"Gp3","/=ROUND(K$14/9,0)"]
["DIN05 (Sixth form social sp...","DIN05","Loose Furniture","Rectangular table",null,"TAB06R","As SoA max group size / 14 (for ICT use)",null,"Gp3","/=ROUNDUP(K14/14,0)"]
["DIN05 (Sixth form social sp...","DIN05","Loose Furniture","Screen",null,"SCR001","As SoA max group size / 11",null,"Gp3","/=ROUND(K$14/11,0)"]
["DIN05 (Sixth form social sp...","DIN05","Loose Furniture","Table, Coffee (round)",null,"TAB601","As SoA max group size / 9 ",null,"Gp3","/=ROUND(K$14/9,0)"]
["DIN05 (Sixth form social sp...","DIN05","Loose Equipment","No FF&E Listed of This Type"]
["HAL01 (Main hall)","HAL01","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["HAL01 (Main hall)","HAL01","Fittings","Lighting rig",null,"LIG001","sufficient for 24 circuits above and in front of performance area",null,"Gp2","CTS"]
["HAL01 (Main hall)","HAL01","Fitted Furniture","Curtain tracking","(m length)","LIG002","between longest two walls","CTS","Gp2",12]
["HAL01 (Main hall)","HAL01","Fitted Furniture","Curtains","(m length)","LIG003","as tracking ","CTS","Gp2",16]
["HAL01 (Main hall)","HAL01","Fitted equipment","No FF&E Listed of This Type"]
["HAL01 (Main hall)","HAL01","Fixed Furniture","No FF&E Listed of This Type"]
["HAL01 (Main hall)","HAL01","Fixed Equipment","Clock (wall mounted)",null,"EQ001X",null,null,"Gp3",1]
["HAL01 (Main hall)","HAL01","Fixed Equipment","Stage lanterns",null,"LIG001X",null,null,"Gp3",24]
["HAL01 (Main hall)","HAL01","Loose Furniture","Classroom chair",null,"CHA005","As SoA max group size / 3.5",null,"Gp3","/=ROUND(K$14/3.5,0)"]
["HAL01 (Main hall)","HAL01","Loose Furniture","Exam table",null,"TAB01E","As SoA max group size / 3.5 if exams",null,"Gp3","/=ROUND(K$14/3.5,0)"]
["HAL01 (Main hall)","HAL01","Loose Equipment","Sound system",null,"MUS009","speakers, amplification and controls to lighting control room",null,"Gp3",1]
["LIB05 (Library resource cen","LIB05","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",2]
["LIB05 (Library resource cen","LIB05","Fittings","Worktop (sitting)","(m length)","WKTI75","to 1 wall",null,"Gp2","/=ROUND(K$14*0.2,0)"]
["LIB05 (Library resource cen","LIB05","Fittings","Library desk",null,"FFE912","including shelf for wheelchair user",null,"Gp2",1]
["LIB05 (Library resource cen","LIB05","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["LIB05 (Library resource cen","LIB05","Fitted equipment","No FF&E Listed of This Type"]
["LIB05 (Library resource cen","LIB05","Fixed Furniture","Shelving units ","(no of shelves)","LIB020X,LIB030X,LIB040X,LIB01X,LIB02X,LIB03X,  LIB04X,LIB05X,LIB06X, LIB07X","no. of shelves as SoA max group size x 0.3",45,"Gp3","/=ROUND(K$14*0.3,0)"]
["LIB05 (Library resource cen","LIB05","Fixed Equipment","Clock (wall mounted)",null,"EQ001X",null,null,"Gp3",1]
["LIB05 (Library resource cen","LIB05","Loose Furniture","Classroom chair",null,"CHA005","As SoA max group size x 0.6",46,"Gp3","/=ROUND(K$14*0.6,0)"]
["LIB05 (Library resource cen","LIB05","Loose Furniture","Upholstered easy chair",null,"CHA200","As SoA max group size x 0.1",12,"Gp3","/=ROUND(K$14*0.1,0)"]
["LIB05 (Library resource cen","LIB05","Loose Furniture","ICT pupil chair ",null,"CHA300","As SoA max group size x 0.34",12,"Gp3","/=ROUND(K$14*0.34,0)"]
["LIB05 (Library resource cen","LIB05","Loose Furniture","Adjustable table",null,"TAB001",null,1,"Gp3",1]
["LIB05 (Library resource cen","LIB05","Loose Furniture","ICT table",null,"TAB010","As SoA max group size x 0.17",12,"Gp3","/=ROUND(K$14*0.17,0)"]
["LIB05 (Library resource cen","LIB05","Loose Furniture","Table (various)",null,"TAB06R/TAB01SC","As SoA max group size x 0.3",21,"Gp3","/=ROUND(K$14*0.3,0)"]
["LIB05 (Library resource cen","LIB05","Loose Furniture","Coffee table",null,"TAB600",null,2,"Gp3",2]
["LIB05 (Library resource cen","LIB05","Loose Equipment","Small Bin ",null,"BIN001",null,null,"Gp3",3]
["LIB06 (Sixth form study are...","LIB06","Fittings","Noticeboard",null,"BOA001",null,null,"Gp2",2]
["LIB06 (Sixth form study are...","LIB06","Fitted Furniture","No FF&E Listed of This Type"]
["LIB06 (Sixth form study are...","LIB06","Fitted equipment","No FF&E Listed of This Type"]
["LIB06 (Sixth form study are...","LIB06","Fixed Furniture","No FF&E Listed of This Type"]
["LIB06 (Sixth form study are...","LIB06","Fixed Equipment","Classroom chair",null,"CHA006","As SoA max group size / 2",null,"Gp3","/=ROUND(K$14/2,0)"]
["LIB06 (Sixth form study are...","LIB06","Fixed Equipment","Upholstered easy chair",null,"CHA200","As SoA max group size / 2",null,"Gp3","/=ROUND(K$14/2,0)"]
["LIB06 (Sixth form study are...","LIB06","Fixed Equipment","ICT pupil chair ",null,"CHA300","As SoA max group size / 0.07",null,"Gp3","/=ROUND(K$14/0.07,0)"]
["LIB06 (Sixth form study are...","LIB06","Fixed Equipment","Clock (wall mounted)",null,"EQ001X",null,null,"Gp3",1]
["LIB06 (Sixth form study are...","LIB06","Fixed Equipment","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["LIB06 (Sixth form study are...","LIB06","Fixed Equipment","Rectangular table",null,"TAB06R","As SoA max group size / 0.07 (for ICT use)",null,"Gp3","/=ROUND(K$14/0.07,0)"]
["LIB06 (Sixth form study are...","LIB06","Fixed Equipment","Table (various)",null,"TAB06R/TAB01SC","As SoA max group size / 0.07",null,"Gp3","/=ROUND(K$14/0.07,0)"]
["LIB06 (Sixth form study are...","LIB06","Fixed Equipment","Coffee table",null,"TAB600","As SoA max group size / 0.03",null,"Gp3","/=ROUND(K$14/0.03,0)"]
["LIB06 (Sixth form study are...","LIB06","Loose Furniture","No FF&E Listed of This Type"]
["LIB06 (Sixth form study are...","LIB06","Loose Equipment","Small Bin ",null,"BIN001",null,null,"Gp3",3]
["PER01 (Music classroom)","PER01","Fittings","Noticeboard",null,"BOA001",null,null,"Gp2",2]
["PER01 (Music classroom)","PER01","Fittings","Worktop (sitting)","(m length)","WKTI75","to full-length of 2 walls except door",null,"Gp2","/=ROUND(7.8+(K10/7.8)-2,1)"]
["PER01 (Music classroom)","PER01","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["PER01 (Music classroom)","PER01","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",3]
["PER01 (Music classroom)","PER01","Fitted equipment","No FF&E Listed of This Type"]
["PER01 (Music classroom)","PER01","Fixed Furniture","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["PER01 (Music classroom)","PER01","Fixed Equipment","No FF&E Listed of This Type"]
["PER01 (Music classroom)","PER01","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["PER01 (Music classroom)","PER01","Loose Furniture","Classroom chair",null,"CHA005",null,null,"Gp3",30]
["PER01 (Music classroom)","PER01","Loose Furniture","Piano stool",null,"CHA030",null,null,"Gp3",1]
["PER01 (Music classroom)","PER01","Loose Furniture","ICT staff chair",null,"CHA301",null,null,"Gp3",1]
["PER01 (Music classroom)","PER01","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["PER01 (Music classroom)","PER01","Loose Furniture","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["PER01 (Music classroom)","PER01","Loose Furniture","Trapezoidal table",null,"TAB05TZ",null,null,"Gp3",4]
["PER01 (Music classroom)","PER01","Loose Furniture","Rectangular table",null,"TAB06R",null,null,"Gp3",2]
["PER01 (Music classroom)","PER01","Loose Furniture","Table, ICT/Admin ",null,"TAB501",null,null,"Gp3",1]
["PER01 (Music classroom)","PER01","Loose Equipment","Upright piano",null,"MUS001",null,null,"Gp3",1]
["PER02 (Extensive music clas...","PER02","Fittings","Noticeboard",null,"BOA001",null,null,"Gp2",3]
["PER02 (Extensive music clas...","PER02","Fittings","Worktop (sitting)","(m length)","WKTI75","to full length of 2 walls ",null,"Gp2","/=ROUND(7.8+(K10/7.8),1)"]
["PER02 (Extensive music clas...","PER02","Fittings","Worktop 1200 deep ","(m length)","WKTI12","2 x average 5.4m peninsulas from 1 wall",null,"Gp2",10.8]
["PER02 (Extensive music clas...","PER02","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["PER02 (Extensive music clas...","PER02","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",3]
["PER02 (Extensive music clas...","PER02","Fitted equipment","No FF&E Listed of This Type"]
["PER02 (Extensive music clas...","PER02","Fixed Furniture","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["PER02 (Extensive music clas...","PER02","Fixed Equipment","No FF&E Listed of This Type"]
["PER02 (Extensive music clas...","PER02","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["PER02 (Extensive music clas...","PER02","Loose Furniture","Classroom chair",null,"CHA005",null,null,"Gp3",30]
["PER02 (Extensive music clas...","PER02","Loose Furniture","Piano stool",null,"CHA030",null,null,"Gp3",1]
["PER02 (Extensive music clas...","PER02","Loose Furniture","ICT staff chair",null,"CHA301",null,null,"Gp3",1]
["PER02 (Extensive music clas...","PER02","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["PER02 (Extensive music clas...","PER02","Loose Furniture","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["PER02 (Extensive music clas...","PER02","Loose Furniture","Trapezoidal table",null,"TAB05TZ",null,null,"Gp3",5]
["PER02 (Extensive music clas...","PER02","Loose Furniture","Rectangular table",null,"TAB06R",null,null,"Gp3",2]
["PER02 (Extensive music clas...","PER02","Loose Furniture","Table, ICT/Admin ",null,"TAB501",null,null,"Gp3",1]
["PER02 (Extensive music clas...","PER02","Loose Equipment","Upright piano",null,"MUS001",null,null,"Gp3",1]
["PER04 (Music recital and dr...","PER04","Fittings","Noticeboard",null,"BOA001",null,null,"Gp2",3]
["PER04 (Music recital and dr...","PER04","Fittings","Curtain tracking","(m length)","LIG002","Perimeter of room","CTS","Gp2","/=ROUND(((K10/7.8)+7.8)*2,1)"]
["PER04 (Music recital and dr...","PER04","Fittings","Curtains","(m length)","LIG003",null,"CTS","Gp2","/=ROUND(M269*1.2,1)"]
["PER04 (Music recital and dr...","PER04","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["PER04 (Music recital and dr...","PER04","Fitted Furniture","Shelving (set of 3)","(m2)","SHE100",null,null,"Gp2",3]
["PER04 (Music recital and dr...","PER04","Fitted equipment","No FF&E Listed of This Type"]
["PER04 (Music recital and dr...","PER04","Fixed Furniture","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["PER04 (Music recital and dr...","PER04","Fixed Equipment","No FF&E Listed of This Type"]
["PER04 (Music recital and dr...","PER04","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp3",1]
["PER04 (Music recital and dr...","PER04","Loose Furniture","Classroom chair",null,"CHA005",null,null,"Gp3",30]
["PER04 (Music recital and dr...","PER04","Loose Furniture","Piano stool",null,"CHA030",null,null,"Gp3",1]
["PER04 (Music recital and dr...","PER04","Loose Furniture","ICT staff chair",null,"CHA301",null,null,"Gp3",1]
["PER04 (Music recital and dr...","PER04","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["PER04 (Music recital and dr...","PER04","Loose Furniture","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["PER04 (Music recital and dr...","PER04","Loose Furniture","Rectangular table",null,"TAB06R",null,null,"Gp3",5]
["PER04 (Music recital and dr...","PER04","Loose Furniture","Table, ICT/Admin ",null,"TAB501",null,null,"Gp3",1]
["PER04 (Music recital and dr...","PER04","Loose Equipment","Stage lanterns with stands",null,"LIG001","to be agreed with school",null,"Gp3","CTS"]
["PER04 (Music recital and dr...","PER04","Loose Equipment","Upright piano",null,"MUS001",null,null,"Gp3",1]
["PER05 (Drama studio)","PER05","Fittings","Noticeboard",null,"BOA001",null,null,"Gp2",1]
["PER05 (Drama studio)","PER05","Fittings","Lighting rig",null,"LIG001","Perimeter of room, with 12 circuits",null,"Gp2","CTS"]
["PER05 (Drama studio)","PER05","Fittings","Curtain tracking","(m length)","LIG002","Perimeter of room","CTS","Gp2","/=ROUND(((K10/7.8)+7.8)*2,1)"]
["PER05 (Drama studio)","PER05","Fittings","Curtains","(m length)","LIG003","to match tracking","CTS","Gp2","/=ROUND(M270*1.2,1)"]
["PER05 (Drama studio)","PER05","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["PER05 (Drama studio)","PER05","Fitted equipment","No FF&E Listed of This Type"]
["PER05 (Drama studio)","PER05","Fixed Furniture","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["PER05 (Drama studio)","PER05","Fixed Equipment","Stage lanterns",null,"LIG001X","to be agreed with school","CTS","Gp3",12]
["PER05 (Drama studio)","PER05","Loose Furniture","Small bin",null,"BIN001",null,null,"Gp3",1]
["PER05 (Drama studio)","PER05","Loose Furniture","Large props bin",null,"BIN003",null,null,"Gp3",2]
["PER05 (Drama studio)","PER05","Loose Furniture","Classroom chair",null,"CHA005",null,null,"Gp3",30]
["PER05 (Drama studio)","PER05","Loose Furniture","Rectangular table",null,"TAB06R",null,null,"Gp3",7]
["PER05 (Drama studio)","PER05","Loose Equipment","Sound system",null,"MUS009","to be agreed with school","CTS","Gp3",1]
["RES12 (Music practice and g...","RES12","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["RES12 (Music practice and g...","RES12","Fittings","Mirror",null,"MIR001",null,null,"Gp2",1]
["RES12 (Music practice and g...","RES12","Fitted Furniture","No FF&E Listed of This Type"]
["RES12 (Music practice and g...","RES12","Fitted equipment","No FF&E Listed of This Type"]
["RES12 (Music practice and g...","RES12","Fixed Furniture","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["RES12 (Music practice and g...","RES12","Fixed Equipment","Classroom chair",null,"CHA005",null,null,"Gp3",3]
["RES12 (Music practice and g...","RES12","Fixed Equipment","Piano stool",null,"CHA030",null,null,"Gp3",1]
["RES12 (Music practice and g...","RES12","Fixed Equipment","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["RES12 (Music practice and g...","RES12","Loose Furniture","No FF&E Listed of This Type"]
["RES12 (Music practice and g...","RES12","Loose Equipment","Upright piano",null,"MUS001",null,null,"Gp3",1]
["RES13 (Extensive music prac)","RES13","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["RES13 (Extensive music prac)","RES13","Fittings","Mirror",null,"MIR001",null,null,"Gp2",1]
["RES13 (Extensive music prac)","RES13","Fitted Furniture","No FF&E Listed of This Type"]
["RES13 (Extensive music prac)","RES13","Fitted equipment","No FF&E Listed of This Type"]
["RES13 (Extensive music prac)","RES13","Fixed Furniture","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["RES13 (Extensive music prac)","RES13","Fixed Equipment","Classroom chair",null,"CHA005",null,null,"Gp3",3]
["RES13 (Extensive music prac)","RES13","Fixed Equipment","Piano stool",null,"CHA030",null,null,"Gp3",1]
["RES13 (Extensive music prac)","RES13","Fixed Equipment","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["RES13 (Extensive music prac)","RES13","Loose Furniture","No FF&E Listed of This Type"]
["RES13 (Extensive music prac)","RES13","Loose Equipment","Upright piano",null,"MUS001",null,null,"Gp3",1]
["RES14 (Control room for rec...","RES14","Fittings","Noticeboard per metre",null,"BOA001",null,null,"Gp2",2]
["RES14 (Control room for rec...","RES14","Fittings","Worktop (sitting)",null,"WKTI75","to 2 walls","CTS","Gp2",4]
["RES14 (Control room for rec...","RES14","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["RES14 (Control room for rec...","RES14","Fitted equipment","No FF&E Listed of This Type"]
["RES14 (Control room for rec...","RES14","Fixed Furniture","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["RES14 (Control room for rec...","RES14","Fixed Equipment","No FF&E Listed of This Type"]
["RES14 (Control room for rec...","RES14","Loose Furniture","ICT pupil chair",null,"CHA300",null,null,"Gp3",3]
["RES14 (Control room for rec...","RES14","Loose Equipment","Control desk console",null,"MUS009","amplification and controls to adjacent music space",null,"Gp3",1]
["RES16 (Lighting and audio c...","RES16","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["RES16 (Lighting and audio c...","RES16","Fittings","Worktop (sitting)","(m length)","WKTK600S","to 1 wall","CTS","Gp2",3]
["RES16 (Lighting and audio c...","RES16","Fitted Furniture","No FF&E Listed of This Type"]
["RES16 (Lighting and audio c...","RES16","Fitted equipment","No FF&E Listed of This Type"]
["RES16 (Lighting and audio c...","RES16","Fixed Furniture","Clock (wall mounted)",null,"EQ001X",null,null,"Gp3",1]
["RES16 (Lighting and audio c...","RES16","Fixed Equipment","No FF&E Listed of This Type"]
["RES16 (Lighting and audio c...","RES16","Loose Furniture","Operators chair (with arms)/Admin",null,"CHA303",null,null,"Gp3",2]
["RES16 (Lighting and audio c...","RES16","Loose Equipment","Control desk console",null,"MUS009","speakers, amplification and controls to main hall",null,"Gp3",1]
["RES21 (Kiln room)","RES21","Fittings","No FF&E Listed of This Type"]
["RES21 (Kiln room)","RES21","Fitted Furniture","Stockroom shelving (set of 5) ","(m2)","SHE030","to  1 wall","CTS","Gp2",4]
["RES21 (Kiln room)","RES21","Fitted equipment","No FF&E Listed of This Type"]
["RES21 (Kiln room)","RES21","Fixed Furniture","No FF&E Listed of This Type"]
["RES21 (Kiln room)","RES21","Fixed Equipment","Front loading kiln ",null,"KLN001X",null,null,"Gp3",1]
["RES21 (Kiln room)","RES21","Loose Furniture","No FF&E Listed of This Type"]
["RES21 (Kiln room)","RES21","Loose Equipment","No FF&E Listed of This Type"]
["RES22 (Dark room)","RES22","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp1",1]
["RES22 (Dark room)","RES22","Fittings","Belfast sink (large)",null,"SIN001",null,null,"Gp1",2]
["RES22 (Dark room)","RES22","Fittings","Worktop 600 deep Solid","(m length)","WKTK600S","to full-length of 2 opposite walls less adjustable table",null,"Gp1","CTS"]
["RES22 (Dark room)","RES22","Fittings","Screen 600 high Solid","(m length)","WKTK600S","above worktop, to match number of enlargers",null,"Gp1","CTS"]
["RES22 (Dark room)","RES22","Fitted Furniture","Underbench 2 door cupboard",null,"CUB004","to match bench length",null,"Gp1",5]
["RES22 (Dark room)","RES22","Fitted Furniture","Underbench 24 tray unit",null,"TRU001","to match bench length",null,"Gp1",2]
["RES22 (Dark room)","RES22","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp1",1]
["RES22 (Dark room)","RES22","Fitted equipment","No FF&E Listed of This Type"]
["RES22 (Dark room)","RES22","Fixed Furniture","No FF&E Listed of This Type"]
["RES22 (Dark room)","RES22","Fixed Equipment","No FF&E Listed of This Type"]
["RES22 (Dark room)","RES22","Loose Furniture","Large Bin",null,"BIN002",null,null,"Gp3",1]
["RES22 (Dark room)","RES22","Loose Furniture","Adjustable table",null,"TAB001",null,null,"Gp3",1]
["RES22 (Dark room)","RES22","Loose equipment","Paper strimmer",null,"EQ233",null,null,"Gp3",1]
["RES22 (Dark room)","RES22","Loose equipment","Enlarger",null,"EQ234","to match number of pupils (as SoA)",null,"Gp3","CTS"]
["RES22 (Dark room)","RES22","Loose equipment","Chemical trays",null,"EQ235","to match number of pupils (as SoA)",null,"Gp3","CTS"]
["RES22 (Dark room)","RES22","Loose equipment","Drying cabinet",null,"EQ236",null,null,"Gp3",1]
["SCI02 (Science studio)","SCI02","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["SCI02 (Science studio)","SCI02","Fittings","Belfast sink (medium)",null,"SIN002",null,null,"Gp2",1]
["SCI02 (Science studio)","SCI02","Fittings","Belfast sink (small)",null,"SIN003",null,null,"Gp2",1]
["SCI02 (Science studio)","SCI02","Fittings","Worktop 600 deep Solid","(m length)","WKTK600S","to 1 wall","CTS","Gp2","/=ROUND(K10/7.8,1)"]
["SCI02 (Science studio)","SCI02","Fitted Furniture","Teacher serviced bollard (wet)",null,"BOLW02",null,null,"Gp2",1]
["SCI02 (Science studio)","SCI02","Fitted Furniture","Teacher serviced bollard (dry)",null,"BOTD02",null,null,"Gp2",1]
["SCI02 (Science studio)","SCI02","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["SCI02 (Science studio)","SCI02","Fitted Furniture","Underbench 2 door cupboard",null,"CUB001",null,null,"Gp2","/=ROUND(K10/12,0)"]
["SCI02 (Science studio)","SCI02","Fitted Furniture","Infill panel",null,"FFE934",null,null,"Gp2",1]
["SCI02 (Science studio)","SCI02","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2","/=ROUND(K10/12,0)"]
["SCI02 (Science studio)","SCI02","Fitted equipment","Fume cupboard (semi ducted)",null,"FUM001Ft","1 for every 3 science studios ",null,"Gp2","CTS"]
["SCI02 (Science studio)","SCI02","Fixed Furniture","No FF&E Listed of This Type"]
["SCI02 (Science studio)","SCI02","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["SCI02 (Science studio)","SCI02","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp2",1]
["SCI02 (Science studio)","SCI02","Loose Furniture","Practical stool",null,"CHA024","As max group size + 1",null,"Gp2","/=K$14+1"]
["SCI02 (Science studio)","SCI02","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp2",1]
["SCI02 (Science studio)","SCI02","Loose Furniture","Adjustable table",null,"TAB003",null,null,"Gp2",1]
["SCI02 (Science studio)","SCI02","Loose Furniture","Science table",null,"TAB200S","As max group size / 5",null,"Gp2","/=ROUND(K$14/5,0)"]
["SCI02 (Science studio)","SCI02","Loose Furniture","Science table",null,"TAB201S","As max group size / 3.3",null,"Gp2","/=ROUND(K$14/3.3,0)"]
["SCI02 (Science studio)","SCI02","Loose Equipment","No FF&E Listed of This Type"]
["SCI05 (General science labo","SCI05","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["SCI05 (General science labo","SCI05","Fittings","Belfast sink (meduim)",null,"SIN002",null,null,"Gp2",1]
["SCI05 (General science labo","SCI05","Fittings","Belfast sink (small)",null,"SIN003",null,null,"Gp2",2]
["SCI05 (General science labo","SCI05","Fittings","Worktop 600 deep Solid","(m length)","WKTK600S","to 1 wall",null,"Gp2","/=ROUND(K10/7.8,1)"]
["SCI05 (General science labo","SCI05","Fittings","Infill panel to demo bench",null,"FFE934",null,null,"Gp2",1]
["SCI05 (General science labo","SCI05","Fitted Furniture","Serviced bollard (dry)",null,"BOD01",null,null,"Gp2",5]
["SCI05 (General science labo","SCI05","Fitted Furniture","Teacher serviced bollard (wet)",null,"BOLW02",null,null,"Gp2",1]
["SCI05 (General science labo","SCI05","Fitted Furniture","Teacher serviced bollard (dry)",null,"BOTD02",null,null,"Gp2",1]
["SCI05 (General science labo","SCI05","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["SCI05 (General science labo","SCI05","Fitted Furniture","Underbench 2 door cupboard",null,"CUB001",null,null,"Gp2","/=ROUND(K10/9,0)"]
["SCI05 (General science labo","SCI05","Fitted Furniture","Adjustable table ",null,"TAB102",null,null,"Gp2",1]
["SCI05 (General science labo","SCI05","Fitted equipment","Fume cupboard (semi ducted)",null,"FUM001Ft","1 for every 3 general laboratories (rounded up)",null,"Gp2","CTS"]
["SCI05 (General science labo","SCI05","Fixed Furniture","No FF&E Listed of This Type"]
["SCI05 (General science labo","SCI05","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["SCI05 (General science labo","SCI05","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp2",1]
["SCI05 (General science labo","SCI05","Loose Furniture","Practical stool",null,"CHA024","As max group size + 1",null,"Gp2","/=K$14+1"]
["SCI05 (General science labo","SCI05","Loose Furniture","Tray racking  (57)",null,"RAC001",null,null,"Gp2",2]
["SCI05 (General science labo","SCI05","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp2",1]
["SCI05 (General science labo","SCI05","Loose Furniture","Science table",null,"TAB200S","As max group size / 2 plus teacher",null,"Gp2","/=ROUND(K$14/2,0)"]
["SCI05 (General science labo","SCI05","Loose Equipment","No FF&E Listed of This Type"]
["SCI11 (Specialist sci lab)","SCI11","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",2]
["SCI11 (Specialist sci lab)","SCI11","Fittings","Belfast sink (medium)",null,"SIN002",null,null,"Gp2",1]
["SCI11 (Specialist sci lab)","SCI11","Fittings","Belfast sink (small)",null,"SIN003",null,null,"Gp2",2]
["SCI11 (Specialist sci lab)","SCI11","Fittings","Worktop 600 deep Solid","(m length)","WKTK600S","to 1 wall",null,"Gp2","/=ROUND(K10/7.8,1)"]
["SCI11 (Specialist sci lab)","SCI11","Fittings","Infill panel to demo bench",null,"FFE934",null,null,"Gp2",1]
["SCI11 (Specialist sci lab)","SCI11","Fitted Furniture","Serviced bollard (wet and dry)",null,"BOWD01",null,null,"Gp2",5]
["SCI11 (Specialist sci lab)","SCI11","Fitted Furniture","Teacher serviced bollard (wet)",null,"BOLW02",null,null,"Gp2",1]
["SCI11 (Specialist sci lab)","SCI11","Fitted Furniture","Teacher serviced bollard (dry)",null,"BOTD02",null,null,"Gp2",1]
["SCI11 (Specialist sci lab)","SCI11","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["SCI11 (Specialist sci lab)","SCI11","Fitted Furniture","Underbench 2 door cupboard",null,"CUB001",null,null,"Gp2","/=ROUND(K10/9,0)"]
["SCI11 (Specialist sci lab)","SCI11","Fitted Furniture","Adjustable table ",null,"TAB102",null,null,"Gp2",1]
["SCI11 (Specialist sci lab)","SCI11","Fitted equipment","Fume cupboard (ducted)",null,"FUM001Ft","1 for every 3 specialist laboratories (rounded up)","or","Gp2",1]
["SCI11 (Specialist sci lab)","SCI11","Fitted equipment","Fume cupboard (semi-ducted)",null,"FUM002Ft","1 for every 3 specialist laboratories (rounded up)",null,"Gp2","CTS"]
["SCI11 (Specialist sci lab)","SCI11","Fixed Furniture","Coats and bags storage unit",null,"STO05X",null,null,"Gp2",2]
["SCI11 (Specialist sci lab)","SCI11","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["SCI11 (Specialist sci lab)","SCI11","Loose Furniture","Small Bin ",null,"BIN001",null,null,"Gp2",1]
["SCI11 (Specialist sci lab)","SCI11","Loose Furniture","Practical stool",null,"CHA024","As max group size + 1",null,"Gp2","/=K$14+1"]
["SCI11 (Specialist sci lab)","SCI11","Loose Furniture","Tray racking  (57)",null,"RAC001",null,null,"Gp2",2]
["SCI11 (Specialist sci lab)","SCI11","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp2",1]
["SCI11 (Specialist sci lab)","SCI11","Loose Furniture","Science table",null,"TAB200S","As max group size / 2  plus teacher",null,"Gp2","/=ROUND(K$14/2,0)"]
["SCI11 (Specialist sci lab)","SCI11","Loose Equipment","No FF&E Listed of This Type"]
["SPH00 (school sports hall)","SPH00","Fittings","No FF&E Listed of This Type"]
["SPH00 (school sports hall)","SPH00","Fitted Furniture","No FF&E Listed of This Type"]
["SPH00 (school sports hall)","SPH00","Fitted equipment","Rebound screens ",null,"FFE932",null,null,"Gp2",1]
["SPH00 (school sports hall)","SPH00","Fitted equipment","Pair hinged basketball goals",null,"SPO003",null,null,"Gp2",1]
["SPH00 (school sports hall)","SPH00","Fitted equipment","Pair of fixed basketball goals",null,"SPO004",null,null,"Gp2",1]
["SPH00 (school sports hall)","SPH00","Fitted equipment","Spring loaded metal cricket stumps ",null,"SPO005",null,null,"Gp2",1]
["SPH00 (school sports hall)","SPH00","Fitted equipment","Full width division net ",null,"SPO006",null,null,"Gp2",1]
["SPH00 (school sports hall)","SPH00","Fixed Furniture","No FF&E Listed of This Type"]
["SPH00 (school sports hall)","SPH00","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["SPH00 (school sports hall)","SPH00","Loose Furniture","No FF&E Listed of This Type"]
["SPH00 (school sports hall)","SPH00","Loose Equipment","School model trampoline ",null,"SPO019",null,null,"Gp3",1]
["SPH00 (school sports hall)","SPH00","Loose Equipment","Hydraulically assisted lift / lower  roller stands ",null,"SPO020",null,null,"Gp3",1]
["SPH00 (school sports hall)","SPH00","Loose Equipment","PVC dust cover ",null,"SPO021",null,null,"Gp3",1]
["SPH00 (school sports hall)","SPH00","Loose Equipment","PVC covered  agility mat ",null,"SPO022",null,null,"Gp3",10]
["SPH00 (school sports hall)","SPH00","Loose Equipment","Timber vaulting box with optional transporter",null,"SPO023",null,null,"Gp3",1]
["SPH00 (school sports hall)","SPH00","Loose Equipment","School springboard",null,"SPO024",null,null,"Gp3",1]
["SPH00 (school sports hall)","SPH00","Loose Equipment","Safety matting ",null,"SPO025",null,null,"Gp3",2]
["SPH00 (school sports hall)","SPH00","Loose Equipment","Horizontal trolley for mats",null,"SPO027",null,null,"Gp3",1]
["SPH00 (school sports hall)","SPH00","Loose Equipment","Traditional timber benches with hooks one end",null,"SPO028",null,null,"Gp3",4]
["SPH00 (school sports hall)","SPH00","Loose Equipment","Traditional timber benches with hooks one end",null,"SPO029",null,null,"Gp3",4]
["SPH00 (school sports hall)","SPH00","Loose Equipment","Multipurpose judo / gym / wrestling matting",null,"SPO030","to create 8m2 of matting",null,"Gp3",1]
["SPH00 (school sports hall)","SPH00","Loose Equipment","School model table tennis tables ",null,"SPO032",null,null,"Gp3",4]
["SPH00 (school sports hall)","SPH00","Loose Equipment","Freestanding netball posts and nets",null,"SPO033",null,null,"Gp3",2]
["SPH00 (school sports hall)","SPH00","Loose Equipment","Pair of badminton posts with nets",null,"SPO034",null,null,"Gp3",4]
["SPH00 (school sports hall)","SPH00","Loose Equipment","Pair of volleyball posts and net",null,"SPO035",null,null,"Gp3",1]
["SPH00 (school sports hall)","SPH00","Loose Equipment","Pair of five-a-side football goals",null,"SPO036",null,null,"Gp3",1]
["SPH00 (school sports hall)","SPH00","Loose Equipment","Pair of tennis posts and net",null,"SPO037",null,null,"Gp3",1]
["SPH00 (school sports hall)","SPH00","Loose Equipment","Pair hockey goals ",null,"SPO038",null,null,"Gp3",1]
["SPH00 (school sports hall)","SPH00","Loose Equipment","Pair of aluminium handball goals.",null,"SPO039",null,null,"Gp3",1]
["SPH00 (school sports hall)","SPH00","Loose Equipment","Cricket practice net ",null,"SPO040",null,null,"Gp3",2]
["SPH00 (school sports hall)","SPH00","Loose Equipment","Exercise mats ",null,"SPO041",null,null,"Gp3",30]
["SPH20 (Community sports hall)","SPH20","Fittings","Noticeboard ",null,"BOA001",null,null,"Gp2",1]
["SPH20 (Community sports hall)","SPH20","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["SPH20 (Community sports hall)","SPH20","Fitted equipment","No FF&E Listed of This Type"]
["SPH20 (Community sports hall)","SPH20","Fixed Furniture","Contractor to list FF&E of This Type",null,"CTS004","based on any legacy FF&E and discussion with school",null,"Gp3","CTS"]
["SPH20 (Community sports hall)","SPH20","Fixed Equipment","Contractor to list FF&E of This Type",null,"CTS005","based on any legacy FF&E and discussion with school",null,"Gp3","CTS"]
["SPH20 (Community sports hall)","SPH20","Loose Furniture","Contractor to list FF&E of This Type",null,"CTS006","based on any legacy FF&E and discussion with school",null,"Gp3","CTS"]
["SPH20 (Community sports hall)","SPH20","Loose Equipment","Contractor to list FF&E of This Type",null,"CTS007","based on any legacy FF&E and discussion with school",null,"Gp3","CTS"]
["STH20 (Bleacher seating)","STH20","Fittings","Bleacher seating units (seats)",null,"CHA401","number of seats provided","CTS","Gp2","CTS"]
["STH20 (Bleacher seating)","STH20","Fitted Furniture","No FF&E Listed of This Type"]
["STH20 (Bleacher seating)","STH20","Fitted equipment","No FF&E Listed of This Type"]
["STH20 (Bleacher seating)","STH20","Fixed Furniture","No FF&E Listed of This Type"]
["STH20 (Bleacher seating)","STH20","Fixed Equipment","No FF&E Listed of This Type"]
["STH20 (Bleacher seating)","STH20","Loose Furniture","No FF&E Listed of This Type"]
["STH20 (Bleacher seating)","STH20","Loose Equipment","No FF&E Listed of This Type"]
["STT08 (Drama store (off room))","STT08","Fittings","No FF&E Listed of This Type"]
["STT08 (Drama store (off room))","STT08","Fitted Furniture","Stockroom shelving (set of 5) ","(m2)","SHE010","to 1 wall","CTS","Gp2",15]
["STT08 (Drama store (off room))","STT08","Fitted equipment","No FF&E Listed of This Type"]
["STT08 (Drama store (off room))","STT08","Fixed Furniture","No FF&E Listed of This Type"]
["STT08 (Drama store (off room))","STT08","Fixed Equipment","No FF&E Listed of This Type"]
["STT08 (Drama store (off room))","STT08","Loose Furniture","No FF&E Listed of This Type"]
["STT08 (Drama store (off room))","STT08","Loose Equipment","No FF&E Listed of This Type"]
["STT21 (Science prep room)","STT21","Fittings","Noticeboard ",null,"BOA001","As SoA Typical Area x 0.04",null,"Gp2","/=ROUND(K$10*0.04,0)"]
["STT21 (Science prep room)","STT21","Fittings","Belfast sink (medium)",null,"SIN002",null,null,"Gp2",2]
["STT21 (Science prep room)","STT21","Fittings","Worktop 1200 deep Solid","(m length)","WKTL12S","In peninsulas. As SoA Typical Area x 0.03",null,"Gp2","/=ROUND(K$10*0.03,1)"]
["STT21 (Science prep room)","STT21","Fittings","Worktop 600 deep Solid","(m length)","WKTL600S","Along wall. As SoA Typical Area x 0.14",null,"Gp2","/=ROUND(K$10*0.14,1)"]
["STT21 (Science prep room)","STT21","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["STT21 (Science prep room)","STT21","Fitted Furniture","Underbench 2 door cupboard",null,"CUB001","As SoA Typical Area x 0.05",null,"Gp2","/=ROUND(K$10*0.05,0)"]
["STT21 (Science prep room)","STT21","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",1]
["STT21 (Science prep room)","STT21","Fitted equipment","Fume cupboard (ducted)",null,"FUM001Ft",null,null,"Gp2",1]
["STT21 (Science prep room)","STT21","Fixed Furniture","No FF&E Listed of This Type"]
["STT21 (Science prep room)","STT21","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["STT21 (Science prep room)","STT21","Fixed Equipment","Distillation unit",null,"EQ003X",null,null,"Gp3",1]
["STT21 (Science prep room)","STT21","Fixed Equipment","Drying oven",null,"EQ004X",null,null,"Gp3",1]
["STT21 (Science prep room)","STT21","Fixed Equipment","Glasswasher",null,"EQ005X",null,null,"Gp3",1]
["STT21 (Science prep room)","STT21","Fixed Equipment","Ice maker",null,"EQ006X",null,null,"Gp3",1]
["STT21 (Science prep room)","STT21","Fixed Equipment","Radioactive cupboard",null,"CUP001X",null,null,"Gp3",1]
["STT21 (Science prep room)","STT21","Loose Furniture","Side filing unit (2 dr)/Admin",null,"CAB104",null,null,"Gp3",1]
["STT21 (Science prep room)","STT21","Loose Furniture","Practical stool",null,"CHA024","As SoA Typical Area x 0.07",null,"Gp3","/=ROUND(K$10*0.07,0)"]
["STT21 (Science prep room)","STT21","Loose Furniture","Operators chair (with arms)/Admin",null,"CHA303",null,null,"Gp3",2]
["STT21 (Science prep room)","STT21","Loose Furniture","Tray racking  (57)",null,"RAC001","As SoA Typical Area x 0.35",null,"Gp3","/=ROUND(K$10*0.35,0)"]
["STT21 (Science prep room)","STT21","Loose Furniture","Tray trolley (12)",null,"RAC005","As SoA Typical Area x 0.07",null,"Gp3","/=ROUND(K$10*0.07,0)"]
["STT21 (Science prep room)","STT21","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",2]
["STT21 (Science prep room)","STT21","Loose Furniture","Table, ICT/Admin ",null,"TAB503",null,null,"Gp3",2]
["STT21 (Science prep room)","STT21","Loose Equipment","Refrigerator ",null,"APP002",null,null,"Gp3",1]
["STT21 (Science prep room)","STT21","Loose Equipment","Large Bin ",null,"BIN002",null,null,"Gp3",1]
["STT23 (Chemical store)","STT23","Fittings","No FF&E Listed of This Type"]
["STT23 (Chemical store)","STT23","Fitted Furniture","Stockroom shelving (set of 5) ","(m2)","SHE020","to 1 wall",null,"Gp2","/=3"]
["STT23 (Chemical store)","STT23","Fitted equipment","No FF&E Listed of This Type"]
["STT23 (Chemical store)","STT23","Fixed Furniture","No FF&E Listed of This Type"]
["STT23 (Chemical store)","STT23","Fixed Equipment","No FF&E Listed of This Type"]
["STT23 (Chemical store)","STT23","Loose Furniture","Chemical Cupboard (2 doors)",null,"CUP012","As SoA area x 0.4 rounded",null,"Gp3","/=ROUND(K$10*0.4,0)"]
["STT23 (Chemical store)","STT23","Loose Equipment","No FF&E Listed of This Type"]
["STT32 (Multi-materials stor...","STT32","Fittings","SS single sink (right hand drainer)",null,"SIN003",null,null,"Gp2",1]
["STT32 (Multi-materials stor...","STT32","Fittings","Worktop 600 deep Solid","(m length)","WKTK600S","to part of 1 wall","CTS","Gp2",3.8]
["STT32 (Multi-materials stor...","STT32","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["STT32 (Multi-materials stor...","STT32","Fitted Furniture","Underbench 2 door cupboard",null,"CUB001",null,null,"Gp2",3]
["STT32 (Multi-materials stor...","STT32","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",1]
["STT32 (Multi-materials stor...","STT32","Fitted Furniture","Coat hooks (6)",null,"STO001",null,null,"Gp2",3]
["STT32 (Multi-materials stor...","STT32","Fitted equipment","Dust extraction unit",null,"EXT001",null,null,"Gp2",1]
["STT32 (Multi-materials stor...","STT32","Fixed Furniture","No FF&E Listed of This Type"]
["STT32 (Multi-materials stor...","STT32","Fixed Equipment","Clock (wall mounted)",null,"EQ001X",null,null,"Gp3",1]
["STT32 (Multi-materials stor...","STT32","Fixed Equipment","Circular saw",null,"MAC010X",null,null,"Gp2",1]
["STT32 (Multi-materials stor...","STT32","Fixed Equipment","Planer",null,"MAC012X","1 if prep area is over 35m2",null,"Gp2","CTS"]
["STT32 (Multi-materials stor...","STT32","Fixed Equipment","Bench grinder",null,"MAC019X",null,null,"Gp2",1]
["STT32 (Multi-materials stor...","STT32","Fixed Equipment","Hacksaw",null,"MAC022X",null,null,"Gp2",1]
["STT32 (Multi-materials stor...","STT32","Fixed Equipment","Board racking ",null,"STO01X",null,null,"Gp2",1]
["STT32 (Multi-materials stor...","STT32","Fixed Equipment","Timber planks racking (horizontal)",null,"STO06X","1 if prep area is over 35m2",null,"Gp3","CTS"]
["STT32 (Multi-materials stor...","STT32","Fixed Equipment","Timber planks racking (vertical)",null,"STO07X","1 if prep area is under 35m2",null,"Gp3","CTS"]
["STT32 (Multi-materials stor...","STT32","Fixed Equipment","Metal rod and tube racking ",null,"STO02X",null,null,"Gp3",1]
["STT32 (Multi-materials stor...","STT32","Fixed Equipment","Bench vice",null,"MAC023X",null,null,"Gp3",1]
["STT32 (Multi-materials stor...","STT32","Loose Furniture","Large Bin ",null,"BIN002",null,null,"Gp3",1]
["STT32 (Multi-materials stor...","STT32","Loose Furniture","ICT staff chair",null,"CHA301",null,null,"Gp3",1]
["STT32 (Multi-materials stor...","STT32","Loose Furniture","Tool cupboard (2 doors)",null,"CUP010",null,null,"Gp3",1]
["STT32 (Multi-materials stor...","STT32","Loose Furniture","Pedestal unit/Admin",null,"STO101",null,null,"Gp3",1]
["STT32 (Multi-materials stor...","STT32","Loose Furniture","Table, ICT/Admin ",null,"TAB502",null,null,"Gp3",1]
["STT32 (Multi-materials stor...","STT32","Loose Furniture","Tray unit (24)",null,"TRA003",null,null,"Gp3",1]
["STT32 (Multi-materials stor...","STT32","Loose Furniture","SS Trolley",null,"TRO001",null,null,"Gp3",1]
["STT32 (Multi-materials stor...","STT32","Loose Equipment","No FF&E Listed of This Type"]
["STT34 (Food store and prep ...","STT34","Fittings","SS single sink (right hand drainer)",null,"SIN003",null,null,"Gp2",1]
["STT34 (Food store and prep ...","STT34","Fittings","Worktop 600 deep Solid","(m length)","WKTK600S","to short wall","CTS","Gp2",3]
["STT34 (Food store and prep ...","STT34","Fitted Furniture","Whiteboard",null,"BOW01",null,null,"Gp2",1]
["STT34 (Food store and prep ...","STT34","Fitted Furniture","Underbench 2 door cupboard",null,"CUB001",null,null,"Gp2",1]
["STT34 (Food store and prep ...","STT34","Fitted Furniture","Shelving (set of 3)",null,"SHE100",null,null,"Gp2",2]
["STT34 (Food store and prep ...","STT34","Fitted equipment","Washer",null,"APP004X",null,null,"Gp2",1]
["STT34 (Food store and prep ...","STT34","Fitted equipment","Tumble Drier",null,"APP005X",null,null,"Gp2",1]
["STT34 (Food store and prep ...","STT34","Fixed Furniture","No FF&E Listed of This Type"]
["STT34 (Food store and prep ...","STT34","Fixed Equipment","Clock (wall mounted)",null,"CLO001X",null,null,"Gp3",1]
["STT34 (Food store and prep ...","STT34","Loose Furniture","Large Bin ",null,"BIN002",null,null,"Gp3",1]
["STT34 (Food store and prep ...","STT34","Loose Furniture","Tray racking ",null,"RAC001",null,null,"Gp3",2]
["STT34 (Food store and prep ...","STT34","Loose Furniture","SS Trolley",null,"TRO001",null,null,"Gp3",1]
["STT34 (Food store and prep ...","STT34","Loose Equipment","Tall larder fridge",null,"APP006",null,null,"Gp3",2]
["STT35 (Food store (off food...","STT35","Fittings","No FF&E Listed of This Type"]
["STT35 (Food store (off food...","STT35","Fitted Furniture","Stockroom shelving (set of 5) ","(m2)","SHE010","To 1 wall. Total sq m","CTS","Gp2",4.5]
["STT35 (Food store (off food...","STT35","Fitted Furniture","Stockroom shelving (set of 5) ","(m2)","SHE020","To 2 walls. Total sq m","CTS","Gp2",6.5]
["STT35 (Food store (off food...","STT35","Fitted equipment","No FF&E Listed of This Type"]
["STT35 (Food store (off food...","STT35","Fixed Furniture","No FF&E Listed of This Type"]
["STT35 (Food store (off food...","STT35","Fixed Equipment","No FF&E Listed of This Type"]
["STT35 (Food store (off food...","STT35","Loose Furniture","No FF&E Listed of This Type"]
["STT35 (Food store (off food...","STT35","Loose Equipment","No FF&E Listed of This Type"]
["TOC01 (Pupil changing and s","TOC01","Fittings","Curtains to shower cubicles","(m length)","FFE987","1m for each cubicle (as SoA group size / 8)","CTS","Gp2","/=ROUND(K$14/8,0)"]
["TOC01 (Pupil changing and s","TOC01","Fittings","Mirror","(number)","MIR001","As max group size /15","CTS","Gp2","/=ROUND(K$14/15,0)"]
["TOC01 (Pupil changing and s","TOC01","Fitted Furniture","Single bench with integral hook rails","(m length)","BEN02X","400mm length per pupil in SoA max group size",null,"Gp2","/=K14*0.4"]
["TOC01 (Pupil changing and s","TOC01","Fitted equipment","No FF&E Listed of This Type"]
["TOC01 (Pupil changing and s","TOC01","Fixed Furniture","No FF&E Listed of This Type"]
["TOC01 (Pupil changing and s","TOC01","Fixed Equipment","No FF&E Listed of This Type"]
["TOC01 (Pupil changing and s","TOC01","Loose Furniture","No FF&E Listed of This Type"]
["TOC01 (Pupil changing and s","TOC01","Loose Equipment","No FF&E Listed of This Type"]
["TOC02 (Accessible changing ...","TOC02","Fittings","Curtains to shower cubicles","(m length)","FFE987","1m for each cubicle ","CTS","Gp2",1]
["TOC02 (Accessible changing ...","TOC02","Fittings","Mirror","(number)","MIR001",null,null,"Gp2",1]
["TOC02 (Accessible changing ...","TOC02","Fitted Furniture","Single bench with coat rail","(m length)","BEN02X",null,"CTS","Gp2","CTS"]
["TOC02 (Accessible changing ...","TOC02","Fitted equipment","No FF&E Listed of This Type"]
["TOC02 (Accessible changing ...","TOC02","Fixed Furniture","No FF&E Listed of This Type"]
["TOC02 (Accessible changing ...","TOC02","Fixed Equipment","No FF&E Listed of This Type"]
["TOC02 (Accessible changing ...","TOC02","Loose Furniture","No FF&E Listed of This Type"]
["TOC02 (Accessible changing ...","TOC02","Loose Equipment","No FF&E Listed of This Type"]
["TOC54 (Special hygiene faci -nf","TOC54","Fittings","Showerbed",null,"APP007X","specfication of shower bed to be checked with school",null,"Gp1","CTS"]
["TOC54 (Special hygiene faci -nf","TOC54","Fittings","Ceiling mounted hoist with track",null,"HOI001",null,null,"Gp1",1]
["TOC54 (Special hygiene faci -nf","TOC54","Fittings","Mirror 1500 high 600 above ffl",null,"MIR001","600 above floor level",null,"Gp1",1]
["TOC54 (Special hygiene faci -nf","TOC54","Fitted Furniture","No FF&E Listed of This Type"]
["TOC54 (Special hygiene faci -nf","TOC54","Fitted equipment","No FF&E Listed of This Type"]
["TOC54 (Special hygiene faci -nf","TOC54","Fixed Furniture","No FF&E Listed of This Type"]
["TOC54 (Special hygiene faci -nf","TOC54","Fixed Equipment","No FF&E Listed of This Type"]
["TOC54 (Special hygiene faci -nf","TOC54","Loose Furniture","No FF&E Listed of This Type"]
["TOC54 (Special hygiene faci -nf","TOC54","Loose Equipment","No FF&E Listed of This Type"]
["TOC53 (Special hygiene faci -nf","TOC53","Fittings","Showerbed",null,"APP007X","specfication of shower bed to be checked with school",null,"Gp1","CTS"]
["TOC53 (Special hygiene faci -nf","TOC53","Fittings","Ceiling mounted hoist with track",null,"HOI001",null,null,"Gp1",1]
["TOC53 (Special hygiene faci -nf","TOC53","Fittings","Mirror 1500 high 600 above ffl",null,"MIR001","600 above floor level",null,"Gp1",1]
["TOC53 (Special hygiene faci -nf","TOC53","Fitted Furniture","No FF&E Listed of This Type"]
["TOC53 (Special hygiene faci -nf","TOC53","Fitted equipment","No FF&E Listed of This Type"]
["TOC53 (Special hygiene faci -nf","TOC53","Fixed Furniture","No FF&E Listed of This Type"]
["TOC53 (Special hygiene faci -nf","TOC53","Fixed Equipment","No FF&E Listed of This Type"]
["TOC53 (Special hygiene faci -nf","TOC53","Loose Furniture","No FF&E Listed of This Type"]
["TOC53 (Special hygiene faci -nf","TOC53","Loose Equipment","No FF&E Listed of This Type"]

{"sheet":"(Manual) GenLib","index":6,"n_rows":135,"n_cols":303,"rows_kept":135,"cut":false,"hidden":true,"merged":[]}
[]
[null,null,null,null,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,42,43,44,45,46,47,48,49,50,51,52,53,54,55,56,57,58,59,60,61,62,63,64,65,66,67,68,69,70,71,72,73,74,75,76,77,78,79,80,81,82,83,84,85,86,87,88,89,90,91,92,93,94,95,96,97,98,99,100,101,102,103,104,105,106,107,108,109,110,111,112,113,114,115,116,117,118,119,120,121,122,123,124,125,126,127,128,129,130,131,132,133,134,135,136,137,138,139,140,141,142,143,144,145,146,147,148,149,150,151,152,153,154,155,156,157,158,159,160,161,162,163,164,165,166,167,168,169,170,171,172,173,174,175,176,177,178,179,180,181,182,183,184,185,186,187,188,189,190,191,192,193,194,195,196,197,198,199,200,201,202,203,204,205,206,207,208,209,210,211,212,213,214,215,216,217,218,219,220,221,222,223,224,225,226,227,228,229,230,231,232,233,234,235,236,237,238,239,240,241,242,243,244,245,246,247,248,249,250,251,252,253,254,255,256,257,258,259,260,261,262,263,264,265,266,267,268,269,270,271,272,273,274,275,276,277,278,279,280,281,282,283,284,285,286,287,288,289,290,291,292,293,294,295,296,297,298,299]
["ADM01 (Entrance and reception)",null,null,null,"Entrance/ reception","ADM01"," \"Public side\" of reception area, over and above circulation space","As SoA","m2","First point of contact for visitors to the school. Welcoming visitors.","As SoA","N/A","N/A","Staff and admin","N/A","General","Yes ",4,"interview room","As SoA","Full disabled access required","Enclosed  (but could be in open plan area)","As SSDB","As SoA","As SoA",2400,2400,"CTS",null,"Entrance Door ",null,"As existing","Contractor to specify if provided","Type DD5v","Note 1","Circulation, with vision panel",0,"  ",926,null,"825 (1650)",null,2000,null,2,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"Yes",null,"Yes",null,"Standard",null,"Yes",null,"No",null,"Pull face",null,"Optional",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1d","Note 1","Durable carpet, lino, rubber or vinyl","Yes",null,"Commercial 33",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L5","Type L5","Required","Preferred","N/A","N/A",0.8,"N/A",0.3,0.3,200,200,300,300,70,70,"N/A","N/A",22,22,"0.3 to 0.5","0.3 to 0.5",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","If fire exit","300 available and limiting glare index of 19 to reception desk","Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V2b","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"A3.45/65","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,"N/A","N/A","N/A","N/A","N/A","N/A","R15","R15","<=1.5","<=2.0","A means of increasing the air velocity during the summer shall be provided.  Openable windows required where possible if window(s) provided.If space is refurbished, see Note 2 in tech annexe.      ","None","Power sockets as FOS, on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Secure supervised entrance; no unauthorised access to rest of school.","Contractor to Specify if provided",null,"N/A","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'Required area' defined in the SoAs. Reception desk in adjacent office"]
["ADM02 (Interview room)",null,null,null,"Interview room","ADM02","Room off reception area for meetings with visitors without the need to access the main school",6,"m2","Interviews, some of which will be in private, with parents and visitors. Small group meetings for both staff and parents.",4,"N/A",0,"Staff and admin","N/A","General","Optional ",4,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB",6,6,2400,2400,"CTS",null,"Not Required unless for fire. CTS if provided.",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.1","Note 1","General, no vision panel","N/A",null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"No",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,"2 doors required, to allow second exit for staff, unless agreed otherwise by Authority","Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V6","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A2.40/60","/=K188","Low","Low",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08","R08","<=0.8","<=0.8","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.       ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["ADM03 (Sick bay)",null,null,null,"Sick bay","ADM03","Semi-open bay for pupils who are feeling unwell",4,"m2","Passively supervised area for pupils who are ill, may need initial treatment and/or are waiting for parents/carers to pick them up.",2,"N/A","N/A","Staff and admin","N/A","General","None",2,"none","As SoA","Disabled access into the area preferred","Semi-enclosed","As SSDB, off entrance/ reception",4,4,2400,2100,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","N/A","N/A","No internal door required",null,"  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V6","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A1.45/65","/=K188","Low","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Cold, with hot and cold handwash [if possible, or if bay is not close to toilets]","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Ability to supervise essential","Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["ADM04 (Sick room)",null,null,null,"Sick room","ADM04","Room for pupils who are feeling unwell",6,"m2","Supervised area for pupils who are ill, may need initial treatment and/or are waiting for parents/carers to pick them up.",3,"N/A","N/A","Staff and admin","N/A","General","None",2,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB, toilet nearby",6,6,2400,2400,"CTS",null,"Not Required ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V6","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A1.45/65","/=K188","Low","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,33,30,40,35,32,32,"R10","R10","<=1.0","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.       ","None","Power sockets where appropriate, plus cleaners' SSSO at low level","Cold, with hot and cold handwash to handwash basin","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Means to keep sensitive documents securely","Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["ADM05 (General office)",null,null,null,"General office","ADM05","Main office for administrative staff, with reception desk for visitors, off entrance/ reception area",26,"m2","Administrative support to staff and welfare support to pupils. Managing and controlling access to and from the school. Welcoming visitors and pupils at reception desk.",8,"N/A","as SoA","Staff and admin","Zone K","General","None",4,"reception","As SoA","Disabled access into the space required","Enclosed. Open at reception desk","As SSDB, entrance/ reception adjacent","As SoA","As SoA",2700,2400,"CTS",null,"Not Required unless for fire. CTS if provided Contractor to specify if provided",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Type F1","General carpet, lino, rubber or vinyl","Yes","Yes","Commercial 32","Commercial 32","N/A","N/A","0.2, 0.15 if carpet","0.2, 0.15 if carpet",10,10,"No","No","No","No","No","No","Yes","Yes","Moderate","Moderate","Yes","Yes","No","No","No","No","Type C1","Note 1","General",0.7,"Normal","Type W1n","Type W1n","General",0.5,0.5,"N/A","N/A","N/A","N/A","Yes","Yes","Normal","Normal","N/A"," ","Type L1.1a","Type L1.1a","Required","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,"N/A","N/A",19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V7","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"10 (see note)",null,0.3,null,"N/A",null,"A1.45/65","Note 1","Low","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,33,30,40,35,32,32,"R10","R10","<=1.0","<=1.0","A means of increasing the air velocity during the summer shall be provided.  20 l/s per reprographics machine that is operated more than 30 minutes per hour or 10l/s/p whichever is greater   ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None [unless tea making facilities not nearby]   ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Means to keep sensitive documents securely","Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the ' max group size' defined in the SoAs. 1 bespoke reception desk in wall opening to entrance/ reception, with shelf for wheelchair users, plus 1 for pupils if general office (2 recep desks)."]
["ADM06 (student services office)",null,null,null,"Student services office","ADM06","Main office for finance staff, with reception desk for pupils","As SoA","m2","Administrative support and welfare support to pupils. Managing and controlling pupil access to and from the school. Welcoming pupils at reception desk.","As SoA","N/A","/=K14","Staff and admin","Zone K","General","None",4,"reception","As SoA","Disabled access into the space required","Enclosed. Open at reception desk","As SSDB, entrance/ reception adjacent","As SoA","As SoA",2700,2400,"CTS",null,"Not Required unless for fire. CTS if provided Contractor to specify if provided",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1a","Type L1.1a","Required","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,"N/A","N/A",19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V7","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"10 (see note)",null,0.3,null,"N/A",null,"A1.45/65","/=K188","Low","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,33,30,40,35,32,32,"R10","R10","<=1.0","<=1.0","A means of increasing the air velocity during the summer shall be provided.  20 l/s per reprographics machine that is operated more than 30 minutes per hour or 10l/s/p whichever is greater. If space is refurbished, see Note 2 in tech annexe.      ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None [unless tea making facilities not nearby]   ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Means to keep sensitive documents securely","Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the ' max group size' defined in the SoAs. 1 bespoke reception desk in wall opening ."]
["ADM08 (Reprographics room)",null,null,null,"Reprographics room","ADM08","Room for reprographics and photocopying machines","As SoA","m2","Administrative work. Collating, finishing, photocopying, printing, scanning. Storage of paper and printing resources.","N/A","N/A","/=ROUND(K10/13,0)","Staff and admin","N/A","General","None",4,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB","As SoA","As SoA",2400,2400,"N/A",null,"Not Required unless for fire. CTS if provided Contractor to specify if provided",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F2c","Type F2c","Chemical resistant lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"N/A","N/A","N/A","N/A","Yes","Yes","Yes","Yes","Moderate","Moderate","Yes","Yes","Yes","Yes","No","No","Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Suitable for heavy movable FF&E on castors ","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V7","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"10 (see note)",null,0.3,null,"N/A",null,"A1.45/65","/=K188","Low","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,33,30,40,35,32,32,"R10","R10","<=1.0","<=1.0","A means of increasing the air velocity during the summer shall be provided.  20 l/s per reprographics machine that is operated more than 30 minutes per hour or 10l/s/p whichever is greater. If space is refurbished, see Note 2 in tech annexe.      ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the required area defined in the SoA. "]
["ADM11 (Heads office)",null,null,null,"Heads office (meeting room)","ADM11","Office for head teacher and meetings of staff, visitors or other adults",16,"m2","Administrative tasks (including use of ICT) small group meetings and interviews. Privacy important.",5,"N/A",1,"Staff and admin","Zone D","General","None",3,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB",16,15,2400,2400,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1","Note 1","General, no vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"No",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.1","Note 1","General, no vision panel","N/A",null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"No",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1a","Type L1.1a","Required","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,"N/A","N/A",19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V6","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A1.45/65","/=K188","Low","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,33,30,40,35,32,32,"R10","R10","<=1.0","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.      ","None","Power sockets as FOS, on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Means to keep sensitive documents securely","Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the ' max group size' defined in the SoAs. "]
["ADM13 (Office (PA to head))",null,null,null,"Office (PA to head)","ADM13","Office for one or more members of staff with admin storage ","As SoA","m2","Administrative tasks (including use of ICT) and filing.","As SoA","N/A","/=K14","Staff and admin","Zone K","General","None",2,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB","As SoA","As SoA",2400,2400,"CTS",null,"Not Required ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","As SSDB",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1b","Type L1.1b","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V6","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A1.45/65","/=K188","Low","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,33,30,40,35,32,32,"R10","R10","<=1.0","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.      ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'max group size' defined in the SoA.  This equals the workstations for staff using the office on a permanent/semi permanent basis "]
["ADM20 (Kitchenette)",null,null,null,"Kitchenette","ADM20","A small room or bay for staff to make drinks and snacks",4,"m2","Making drinks and/or snacks for staff, pupils or visitors."," N/A ","N/A","N/A","Staff and admin","N/A","N/A","None",2,"none","As SoA","Not required","Enclosed or semi-enclosed","As SSDB",4,4,2400,2400,1700,"minimum","Not Required ",null,"As existing","Contractor to specify if provided","Type D1.2vh","Note 1","Strong, with vision panel, humid areas",30,"  ",926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"Yes",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F2sh","Type F2sh","Light practical hygienic lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","N/A","N/A","Yes","Yes","Yes","Yes","High","High","Yes","Yes","No","No","No","No","Type C2","Note 1","Humid",0.7,"Humid","Type W3h","Type W3h","Humid",0.5,0.5,"Yes","Yes","Yes","Yes","Yes","Yes","Humid","Humid","N/A","Suitable for heavy movable FF&E on castors ","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V6","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A1.45/65","/=K188","Low","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,33,30,40,35,32,32,"R10","R10","<=1.0","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.      ","None","Power sockets as FOS, on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot and cold drinking water to sink.","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Need to be able to clean surfaces thoroughly to maintain hygiene; safe distances around cooker(s).","Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["ADM21 (Community entrance)",null,null,null,"Community entrance/ reception","ADM21"," Public side of reception area, over and above circulation space",4,"m2","Managing and controlling access to and from facilities used by the community such as sports halls.","N/A","N/A","N/A","Staff and admin","N/A","General","Yes ",4,"interview room","As SoA","Full disabled access required","Enclosed  (but could be in open plan area)","As SSDB",4,3,2400,2400,"N/A",null,"Entrance Door ",null,"As existing","Contractor to specify if provided","Type DD5v","Note 1","Circulation, with vision panel",0,"  ",926,null,"825 (1650)",null,2000,null,2,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"Yes",null,"Yes",null,"Standard",null,"Yes",null,"No",null,"Pull face",null,"Optional",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1d","Note 1","Durable carpet, lino, rubber or vinyl","Yes",null,"Commercial 33",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L5","Type L5","Required","Preferred","N/A","N/A",0.8,"N/A",0.3,0.3,200,200,300,300,70,70,"N/A","N/A",22,22,"0.3 to 0.5","0.3 to 0.5",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","If fire exit","300 available and limiting glare index of 19 to reception desk if provided","Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,"N/A",200,15,15,"Type V2b","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"A3.45/65","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,"N/A","N/A","N/A","N/A","N/A","N/A","R15","R15","<=1.5","<=2.0","A means of increasing the air velocity during the summer shall be provided.  Openable windows required where possible if window(s) provided. If space is refurbished, see Note 2 in tech annexe.","None","Power sockets as FOS, on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Secure supervised entrance; no unauthorised access to rest of school.","Contractor to Specify if provided",null,"N/A","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","optional seating or vending area for community use"]
["CIR00 (Circulation)",null,null,null,"Circulation","CIR00","Circulation areas including corridor space between rooms, stairwells and lobbies","varies",null,"Circulation of pupils and others between spaces."," N/A ","N/A","N/A","Non-net","N/A","Non-net","CTS",3,"none","CTS","Full disabled and trolley access required","Enclosed","CTS","N/A","N/A",2400,2400,1800,"minimum","CTS if provided ",null,"As existing","Contractor to specify if provided","N/A","Note 1","No internal door required",null,"  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Type DD5v","Note 1","Circulation, with vision panel",0,null,926,null,"825 (1650)",null,2000,null,2,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"Yes",null,"  Yes ",null,"Standard",null,"Yes",null,"No",null,"Pull face",null,"  Optional ",null,200,null,null,"Type F1d","Type F1d","Durable carpet, lino, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A","0.2, 0.15 if carpet","0.2, 0.15 if carpet",10,10,"No","No","No","No","No","No","Yes","Yes","Moderate","Moderate","Yes","Yes","No","No","No","No","Type C1","Note 1","General",0.7,"Normal","Type W4","Type W4","Rough",0.5,0.5,"N/A","N/A","N/A","N/A","N/A","N/A","Normal","Normal","N/A"," ","Type L6","Type L6","Preferred","Preferred","N/A","N/A","N/A","N/A",0.3,0.3,100,100,150,150,70,70,"N/A","N/A",25,25,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d,occ, sw","If fire exit",null,"Type T7","Type T7",18,18,"Contractor to specify (CTS)",15,15,21,21,40,"N/A",6,"N/A",4,"N/A","N/A","N/A","N/A","N/A",200,200,12,12,"Type V2b","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"A6.45/65","Note 1","High","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,33,30,40,35,32,32,"R00","R00","N/A","N/A","A means of increasing the air velocity in circulation areas during the summer shall be provided.  Openable windows required where possible if window(s) provided   ","None","Cleaners' SSSO at low level as required","Drinking water available on each floor","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS if Fire Containment.","Contractor to Specify",null,"Add here text to be included on sign","CTS","CTS","Contractor to specify if provided","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["CIR01 (Corridor)",null,null,null,"Corridor","CIR01","Corridor space between rooms","varies",null," Circulation between spaces."," N/A ","N/A","N/A","Non-net","N/A","Non-net","CTS",3,"none","CTS","Full disabled and trolley access required","Enclosed","As SSDB","N/A","N/A",2400,2400,1800,"minimum","Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","N/A","Note 1","No internal door required",null,"  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Type DD5v","Note 1","Circulation, with vision panel",0,null,926,null,"825 (1650)",null,2000,null,2,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"Yes",null,"  Yes ",null,"Standard",null,"Yes",null,"No",null,"Pull face",null,"  Optional ",null,200,null,null,"Type F1d","Type F1d","Durable carpet, lino, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A","0.2, 0.15 if carpet","0.2, 0.15 if carpet",10,10,"No","No","No","No","No","No","Yes","Yes","Moderate","Moderate","Yes","Yes","No","No","No","No","Type C1","Note 1","General",0.7,"Normal","Type W4","Type W4","Rough",0.5,0.5,"N/A","N/A","N/A","N/A","N/A","N/A","Normal","Normal","N/A"," ","Type L6","Type L6","Preferred","Preferred","N/A","N/A","N/A","N/A","N/A",0.3,100,100,150,150,70,70,"N/A","N/A",25,25,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d,occ, sw","If fire exit",null,"Type T7","Type T7",18,18,"Contractor to specify (CTS)",15,15,21,21,40,"N/A",6,"N/A",4,"N/A","N/A","N/A","N/A","N/A","N/A",200,12,12,"Type V2b","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"A3.45/65","Note 1","Average","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,"N/A","N/A","N/A","N/A","N/A","N/A","R00","R00","N/A","N/A","A means of increasing the air velocity in circulation areas during the summer shall be provided.  Openable windows required where possible if window(s) provided   ","None","Cleaners' SSSO at low level as required","Drinking water available on each floor","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Fire Containment.","Contractor to Specify",null,"Add here text to be included on sign","CTS","CTS","Contractor to specify if provided","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["DIN01 (Dining area(s))",null,null,null,"Dining area(s)","DIN01","Area generally set out for dining ","As SoA","m2","Can also be used for school events such as parents meetings/presentations, teacher consultations or whole school teacher meetings. Dining for hot and cold meals from servery area(s) within space or adjacent.","As SoA","N/A","N/A","Halls and dining","N/A","Large and performance","Yes",4,"none","As SoA","Disabled access required to all areas except some  seating","Enclosed, semi-enclosed or open plan","As SSDB","As SoA","As SoA",3000,2700,"CTS",null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type DD1.1v","Note 1","Double general, with vision panels",30,"  ",926,null,"825 (1500)",null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type DD1.1v","Note 1","Double general, with vision panels",35,null,926,null,"825 (1500)",null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,"Plain meeting stiles. Doors specified will only be applicable to enclosed dining areas","Type F2cdw","Type F2cdw","Durable waterproof lino, resin, rubber or vinyl","Yes","Yes","Commercial 34","Commercial 34","N/A","N/A",0.2,0.2,10,10,"No","No","No","No","Yes","Yes","Yes","Yes","High","High","Yes","Yes","No","No","No","No","Type C1","Note 1","General",0.7,"Normal","Type W2ns","Note 1","Dining",0.5,null,"Yes",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L5","Type L5","Required","Preferred","N/A","N/A",0.8,"N/A",0.3,0.3,200,200,300,300,70,70,"N/A","N/A",22,22,"0.3 to 0.5","0.3 to 0.5",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","If fire exit","300 available and limiting glare index of 19 to reception desk if provided within the space","Type T4","Type T4",21,21,"Contractor to specify (CTS)",19,19,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,16,16,"Type V2","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A6.45/65","/=K188","High","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,33,30,40,35,32,32,"R10.2","R10.2","<=1.0","<=1.5","A means of increasing the air velocity during the summer shall be provided.  Ventilation rate to suit occupancy. If space is refurbished, see Note 2 in tech annexe.   ","None","Power sockets as FOS, where appropriate, plus cleaners' SSSO at low level","Drinking water fountain","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Tables laid out to allow queuing to servery between tables and return of trays before exit. FF&E to provide number of covers as max group size in SoA. Some FF&E proportional to area of space."]
["KIT00 (School kitchen prep & s)",null,null,null,"School kitchen prep & servery","KIT00","Preparation, servery and admin areas of commercial kitchen for preparing and serving school meals and administrative tasks.","CTS","m2","Preparing, cooking and serving hot and cold meals for pupils and staff, as well as dishwashing and cleaning, by commercial catering staff. Also to include area or separate room for administrative tasks (including use of ICT) and filing by commercial catering staff."," N/A ","N/A","N/A","Non-net","N/A","Non-net","None",4,"dining area and any servery areas","As SoA","Disabled access into the area required","Enclosed","As SSDB","N/A","N/A",2700,2400,"CTS",null,"Deliveries ",null,"As existing","Contractor to specify if provided","Type D1.2vh","Note 1","Strong, with vision panel, humid areas",30,"  ",926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"Yes",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F8","Note 1","Heat resistant wet area ceramic, resin, rubber or vinyl","Yes for vinyl",null,"Commercial 34",null,"N/A",null,0.2,null,10,null,"R11",null,"Minimum SRV 36",null,"Yes",null,"Yes",null,"High",null,"No",null,"Yes",null,"Yes",null,"Type C2","Note 1","Humid",0.7,"Humid","Type W3h","Type W3h","Humid",0.5,0.5,"Yes","Yes","Yes","Yes","Yes","Yes","Humid","Humid","N/A"," ","Type L7.1","Type L7.1","Preferred","Preferred","N/A","N/A","N/A","N/A",0.3,0.3,500,500,750,750,"N/A","N/A","N/A","N/A",22,22,"N/A","N/A",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","sw","Yes","see FOS","Type T5a","Type T5a",20,20,"Contractor to specify (CTS)",15,15,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A",12,12,"Type V2c","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"A5.50/65","/=K188","High","High",null,"Contractor to specify (CTS)",null,50,50,65,65,"N/A","N/A","N/A","N/A","N/A","N/A","R15","R15","<=1.5","<=2.0","Workplace regulations apply.  Openable windows required where possible where window(s) provided, HSE guidance applies. If space is refurbished, see Note 2 in tech annexe.   ","Yes, to gas appliances where provided","Power sockets to suit FF&E provided and work areas, plus cleaners' SSSO at low level","Hot and cold, with hot and cold handwash, to suit FF&E specified  ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Fire Containment.","Contractor to Specify if provided",null,"Add here text to be included on sign","CTS","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","All FF&E shall be provided as Group 2 by the contractor in a suitable and safe layout which allows for the preferences of the school and catering provider"]
["KIT01 (School kitchen prepa...",null,null,null,"School kitchen preparation area","KIT01","Preparation area of commercial kitchen for preparing school meals","CTS","m2","Preparing and cooking meals for pupils and staff as well as dishwashing and cleaning by commercial catering staff."," N/A ","N/A","N/A","Non-net","N/A","Non-net","None",4,"dining area and any servery areas","As SoA","Disabled access into the area required","Enclosed","As SSDB","N/A","N/A",2700,2400,"N/A",null,"Deliveries ",null,"As existing","Contractor to specify if provided","Type D1.2vh","Note 1","Strong, with vision panel, humid areas",30,"  ",926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"Yes",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F8","Note 1","Heat resistant wet area ceramic, resin, rubber or vinyl","Yes for vinyl",null,"Commercial 34",null,"N/A",null,0.2,null,10,null,"R11",null,"Minimum SRV 36",null,"Yes",null,"Yes",null,"High",null,"No",null,"Yes",null,"Yes",null,"Type C2","Note 1","Humid",0.7,"Humid","Type W3h","Type W3h","Humid",0.5,0.5,"Yes","Yes","Yes","Yes","Yes","Yes","Humid","Humid","N/A"," ","Type L7.1","Type L7.1","Preferred","Preferred","N/A","N/A","N/A","N/A","N/A",0.3,500,500,750,750,"N/A","N/A","N/A","N/A",22,22,"N/A","N/A",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","sw","Yes","see FOS","Type T5a","Type T5a",20,20,"Contractor to specify (CTS)",15,15,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A",12,12,"Type V2c","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"A5.50/65","/=K188","High","High",null,"Contractor to specify (CTS)",null,50,50,65,65,"N/A","N/A","N/A","N/A","N/A","N/A","R15","R15","<=1.5","<=2.0","Workplace regulations apply.  Openable windows required where possible where window(s) provided, HSE guidance applies. If space is refurbished, see Note 2 in tech annexe.   ","Yes, to gas appliances where provided","Power sockets to suit FF&E provided and work areas, plus cleaners' SSSO at low level","Hot and cold, with hot and cold handwash, to suit FF&E specified  ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Fire Containment.","Contractor to Specify if provided",null,"Add here text to be included on sign","CTS","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","All FF&E shall be provided as Group 2 by the contractor in a suitable and safe layout which allows for the preferences of the school and catering provider"]
["KIT02 (School kitchen serve...",null,null,null,"School kitchen servery area","KIT02","Servery area of commercial kitchen for serving school meals","CTS","m2","Serving and storing hot meals for pupils and staff by commercial catering staff."," N/A ","N/A","N/A","Non-net","N/A","Non-net","None",4,"dining area and any servery areas","As SoA","Disabled access into the area required","Semi-enclosed","Off kitchen preparation area, unless as SSDB","N/A","N/A",2700,2400,"N/A",null,"Not Required",null,"As existing","Contractor to specify if provided","N/A","Note 1","No internal door required",null,"  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Type D1.2vh","Note 1","Strong, with vision panel, humid areas",30,null,926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"Yes",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F8","Note 1","Heat resistant wet area ceramic, resin, rubber or vinyl","Yes for vinyl",null,"Commercial 34",null,"N/A",null,0.2,null,10,null,"R11",null,"Minimum SRV 36",null,"Yes",null,"Yes",null,"High",null,"No",null,"Yes",null,"Yes",null,"Type C2","Note 1","Humid",0.7,"Humid","Type W3h","Type W3h","Humid",0.5,0.5,"Yes","Yes","Yes","Yes","Yes","Yes","Humid","Humid","N/A"," ","Type L7.1","Type L7.1","Preferred","Preferred","N/A","N/A","N/A","N/A","N/A",0.3,500,500,750,750,"N/A","N/A","N/A","N/A",22,22,"N/A","N/A",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","sw","Yes","see FOS","Type T5a","Type T5a",20,20,"Contractor to specify (CTS)",15,15,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A",12,12,"Type V2c","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"A5.50/65","/=K188","High","High",null,"Contractor to specify (CTS)",null,50,50,65,65,"N/A","N/A","N/A","N/A","N/A","N/A","R15","R15","<=1.5","<=2.0","Workplace regulations apply. Openable windows required where possible if window(s) provided. HSE guidance applies. If space is refurbished, see Note 2 in tech annexe.","Yes, to gas appliances where provided","Power sockets to suit FF&E provided and work areas, plus cleaners' SSSO at low level","Hot and cold, to suit FF&E specified ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Fire Containment.","Contractor to Specify if provided",null,"Add here text to be included on sign","CTS","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","All FF&E shall be provided as Group 2 by the contractor in a suitable and safe layout which allows for the preferences of the school and catering provider"]
["KIT03 (School kitchen office)",null,null,null,"School kitchen office","KIT03","Commercial kitchen office for use by school catering staff","CTS","m2","Administrative tasks (including use of ICT) and filing by commercial catering staff."," N/A ","N/A","N/A","Non-net","N/A","Non-net","None",4,"dining area and any servery areas","As SoA","Disabled access into the area required","Enclosed","As SSDB","N/A","N/A",2400,2400,"N/A",null,"Not Required",null,"As existing","Contractor to specify if provided","Type D1.2vh","Note 1","Strong, with vision panel, humid areas",30,"  ",926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"Yes",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Type F8","Note 1","Heat resistant wet area ceramic, resin, rubber or vinyl","Yes for vinyl",null,"Commercial 34",null,"N/A",null,0.2,null,10,null,"R11",null,"Minimum SRV 36",null,"Yes",null,"Yes",null,"High",null,"No",null,"Yes",null,"Yes",null,"Type C2","Note 1","Humid areas and toilets",0.7,"Humid","Type W3h","Type W3h","Humid",0.5,0.5,"Yes","Yes","Yes","Yes","Yes","Yes","Humid","Humid","N/A"," ","Type L7.1","Type L7.1","Preferred","Preferred","N/A","N/A","N/A","N/A","N/A",0.3,500,500,750,750,"N/A","N/A","N/A","N/A",22,22,"N/A","N/A",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","sw","Yes","see FOS","Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,"N/A",200,15,15,"Type V6","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A1.45/65","/=K188","Low","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,33,30,40,35,32,32,"R10","R10","<=1.0","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.  ","None","Power sockets to suit FF&E provided and work areas, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Fire Containment.","Contractor to Specify if provided",null,"Add here text to be included on sign","CTS","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","All FF&E shall be provided as Group 2 by the contractor in a suitable and safe layout which allows for the preferences of the school and catering provider"]
["KIT04 (School kitchen staff",null,null,null,"School kitchen staff/ changing area","KIT04","Commercial kitchen staff and changing area for use by school catering staff, as part of school kitchen suite",6,"m2","Changing. Storage of personal belongings and clothing.",4,"N/A",4,"Non-net","N/A","Non-net","None",4,"dining area and any servery areas","As SoA","Full disabled access not required","Enclosed","Off kitchen prep area, or as SSDB","N/A","N/A",2400,2400,"N/A",null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.2vh","Note 1","Strong, with vision panel, humid areas",30,"  ",926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"Yes",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Type F8","Type F8","Heat resistant wet area ceramic, resin, rubber or vinyl","Yes for vinyl","Yes for vinyl","Commercial 34","Commercial 34","N/A","N/A",0.2,0.2,10,10,"R11","R11","Minimum SRV 36","Minimum SRV 36","Yes","Yes","Yes","Yes","High","High","No","No","Yes","Yes","Yes","Yes","Type C2","Note 1","Humid",0.7,"Humid","Type W3h","Type W3h","Humid",0.5,0.5,"Yes","Yes","Yes","Yes","Yes","Yes","Humid","Humid","N/A"," ","Type L7.1","Type L7.1","Preferred","Preferred","N/A","N/A","N/A","N/A","N/A",0.3,500,500,750,750,"N/A","N/A","N/A","N/A",22,22,"N/A","N/A",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","sw","Yes","see FOS","Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,"N/A",200,15,15,"Type V6","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A1.45/65","Note 1","Low","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,33,30,40,35,32,32,"R10","R10","<=1.0","<=1.0","A means of increasing the air velocity during the summer shall be provided.     ","None","Power sockets to suit FF&E provided and work areas, plus cleaners' SSSO at low level","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Fire Containment.","Contractor to Specify",null,"Add here text to be included on sign","CTS","CTS","Contractor to specify if provided","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","All FF&E shall be provided as Group 2 by the contractor in a suitable and safe layout which allows for the preferences of the school and catering provider"]
["KIT05 (School kitchen store)",null,null,null,"School kitchen store","KIT05","Commercial kitchen dry store for use by school catering staff, as part of school kitchen suite","CTS","m2","Storing cold or dry foodstuffs for use by commercial catering staff, as part of school kitchen suite."," N/A "," N/A "," N/A ","Non-net","N/A","Non-net","None",4,"dining area, all other school kitchen areas, any servery areas","As SoA","Disabled and trolley access into the area required","Enclosed","As SSDB",2,2,2400,2400,"N/A",null,"Not Required ",null,"As existing","Contractor to specify if provided","Type D6h","Note 1","Store room in humid areas",0,"  ",926,null,825,null,2000,null,3,null,3,null,30,null,"Yes",null,"Yes",null,"No",null,"No",null,"No",null,"Standard",null,"Yes",null,"No",null,"Pull face",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F2sch","Type F2sch","Light practical non-slip hygienic  lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","SRV36 + 20 microns","SRV36 + 20 microns","Yes","Yes","Yes","Yes","High","High","Yes","Yes","Yes","Yes","No","No","Type C2","Note 1","Humid",0.7,"Humid","Type W2h","Type W2h","Humid areas and toilets",0.5,0.5,"Yes","Yes","N/A","N/A","Yes","Yes","Humid","Humid","N/A"," ","Type L7.3","Type L7.3","Not required","Not required","N/A","N/A","N/A","N/A",0.3,"N/A",200,200,300,300,"N/A","N/A","N/A","N/A",25,25,"N/A","N/A",0.4,0.4,60,60,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","sw","No",null,"Type T9","Type T9",5,5,"Contractor to specify (CTS)","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","Type V2b","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"N/A","/=K188",null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A",null,null,"     ","None","None","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Fire Containment.","Contractor to Specify if provided",null,"Add here text to be included on sign","CTS","CTS","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","All FF&E shall be provided as Group 2 by the contractor in a suitable and safe layout which allows for the preferences of the school and catering provider"]
["KIT06 (School kitchen dry s...",null,null,null,"School kitchen dry store","KIT06","Commercial kitchen dry store for use by school catering staff, as part of school kitchen suite","CTS","m2","Storing dry foodstuffs for use by commercial catering staff, as part of school kitchen suite."," N/A "," N/A "," N/A ","Non-net","N/A","Non-net","None",4,"dining area, all other school kitchen areas, any servery areas","As SoA","Disabled and trolley access into the area required","Enclosed","As SSDB",2,2,2400,2400,"N/A",null,"Not Required ",null,"As existing","Contractor to specify if provided","Type D6h","Note 1","Store room in humid areas",0,"  ",926,null,825,null,2000,null,3,null,3,null,30,null,"Yes",null,"Yes",null,"No",null,"No",null,"No",null,"Standard",null,"Yes",null,"No",null,"Pull face",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F2sch","Type F2sch","Light practical non-slip hygienic  lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","SRV36 + 20 microns","SRV36 + 20 microns","Yes","Yes","Yes","Yes","High","High","Yes","Yes","Yes","Yes","No","No","Type C2","Note 1","Humid",0.7,"Humid","Type W2h","Type W2h","Humid areas and toilets",0.5,0.5,"Yes","Yes","N/A","N/A","Yes","Yes","Humid","Humid","N/A"," ","Type L7.3","Type L7.3","Not required","Not required","N/A","N/A","N/A","N/A","N/A","N/A",200,200,300,300,"N/A","N/A","N/A","N/A",25,25,"N/A","N/A",0.4,0.4,60,60,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","sw","No",null,"Type T9","Type T9",5,5,"Contractor to specify (CTS)","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","Type V2b","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"N/A","/=K188",null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A",null,null,"Contractor to specify to suit best practice standards and guidance. If space is refurbished, see Note 2 in tech annexe.    ","None","None","None","CTS","N/A","N/A","N/A","CTS","N/A","N/A","N/A","CTS","N/A","N/A","CTS","Fire Containment.","Contractor to Specify if provided",null,"Add here text to be included on sign","CTS","CTS","None","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","All FF&E shall be provided as Group 2 by the contractor in a suitable and safe layout which allows for the preferences of the school and catering provider"]
["KIT07 (School kitchen cold ...",null,null,null,"School kitchen cold store","KIT07","Commercial kitchen cold store for use by school catering staff, as part of school kitchen suite","CTS","m2","Storing refrigerated cold foodstuffs for use by commercial catering staff, as part of school kitchen suite."," N/A "," N/A "," N/A ","Non-net","N/A","Non-net","None",4,"dining area, all other school kitchen areas, any servery areas","As SoA","Disabled and trolley access into the area required","Enclosed","As SSDB",2,2,2400,2400,"N/A",null,"Not Required ",null,"As existing","Contractor to specify if provided","CTS","CTS","CTS",null,"  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Door to be designed to suit refrigerated facility as specified by the Contractor","CTS","CTS","CTS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CTS","CTS",null,null,null,"CTS","CTS",null,null,null,null,null,null,null,null,null,null,null,null,"Contractor to specify to suit best practice standards and guidance ","Type L7.3","Type L7.3","Not required","Not required","N/A","N/A","N/A","N/A","N/A","N/A",200,200,300,300,"N/A","N/A","N/A","N/A",25,25,"N/A","N/A",0.4,0.4,60,60,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","sw","No","Contractor to specify to suit best practice standards and guidance","CTS","CTS",null,null,"Contractor to specify (CTS)",null,null,null,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","Note 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","/=K188",null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A",null,null,"Contractor to specify to suit best practice standards and guidance. If space is refurbished, see Note 2 in tech annexe.    ","None","CTS","None","CTS","N/A","N/A","N/A","CTS","N/A","N/A","N/A","CTS","N/A","N/A","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","CTS","CTS","None","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","All FF&E shall be provided as Group 2 by the contractor in a suitable and safe layout which allows for the preferences of the school and catering provider"]
["KIT08 (School kitchen freez...",null,null,null,"School kitchen freezer store","KIT08","Commercial kitchen freezer store for use by school catering staff, as part of school kitchen suite","CTS","m2","Storing frozen foodstuffs for use by commercial catering staff, as part of school kitchen suite."," N/A "," N/A "," N/A ","Non-net","N/A","Non-net","None",4,"dining area, all other school kitchen areas, any servery areas","As SoA","Disabled and trolley access into the area required","Enclosed","As SSDB",2,2,2400,2400,"N/A",null,"Not Required ",null,"As existing","Contractor to specify if provided","CTS","CTS","CTS",null,"  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Door to be designed to suit refrigerated facility as specified by the Contractor","CTS","CTS","CTS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CTS","CTS",null,null,null,"CTS","CTS",null,null,null,null,null,null,null,null,null,null,null,null,"Contractor to specify to suit best practice standards and guidance ","Type L7.3","Type L7.3","Not required","Not required","N/A","N/A","N/A","N/A","N/A","N/A",200,200,300,300,"N/A","N/A","N/A","N/A",25,25,"N/A","N/A",0.4,0.4,60,60,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","sw","CTS","Contractor to specify to suit best practice standards and guidance. If space is refurbished, see Note 2 in tech annexe.    ","CTS","CTS",null,null,"Contractor to specify (CTS)",null,null,null,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","Note 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","/=K188",null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A",null,null,"Contractor to specify to suit best practice standards and guidance","None","CTS","None","CTS","N/A","N/A","N/A","CTS","N/A","N/A","N/A","CTS","N/A","N/A","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","CTS","CTS","None","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","All FF&E shall be provided as Group 2 by the contractor in a suitable and safe layout which allows for the preferences of the school and catering provider"]
["KIT09 (School kitchen toile...",null,null,null,"School kitchen toilet area","KIT09","Commercial kitchen toilet area for use by school catering staff, as part of school kitchen suite",2,"m2",null,"N/A","N/A","N/A","Non-net","N/A","Non-net","None ",3,"none if others available","As SoA","Disabled access not required","Enclosed","As SSDB",2,2,2400,2200,"N/A",null,"Not Required ",null,"As existing","Contractor to specify if provided","Type D4.1n","Note 1","Suitable for toilets",30,"  ",926,null,825,null,2000,null,8,null,3,null,30,null,"Yes",null,"Yes",null,"No",null,"No",null,"No",null,"See note",null,"Deadlock only",null,"No",null,"Pull face",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Door leaf shall open inwards but be openable outwards in an emergency","Type F2sch","Type F2sch","Light practical non-slip hygienic  lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","SRV36 + 20 microns","SRV36 + 20 microns","Yes","Yes","Yes","Yes","High","High","Yes","Yes","Yes","Yes","No","No","Type C2","Note 1","Humid",0.7,"Humid","Type W2h","Type W2h","Humid areas and toilets",0.5,0.5,"Yes","Yes","N/A","N/A","Yes","Yes","Humid","Humid","N/A",null,"Type L7.2","Type L7.2","Preferred","Preferred","N/A","N/A","N/A","N/A","N/A",0.3,200,200,300,300,70,70,"N/A","N/A",22,22,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No",null,"Type T7a","Type T7a",18,18,"Contractor to specify (CTS)",15,15,21,21,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A",12,12,"Type V2d","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"A3.50/65","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,50,50,65,65,"N/A","N/A","N/A","N/A","N/A","N/A","R15","R15","<=1.5","<=2.0","Intermittent extract of 6l/s per WC/urinal and 15l/s per shower/bath. If space is refurbished, see Note 2 in tech annexe.       ","None","To hand dryers if provided","Cold, with hot and cold handwash. Single mixer spray tap to whb. Sanitary ware, including hand washing and drying, to suit the number of wcs provided. Cartridge-type lockable soap dispenser. High velocity electric hand dryer or paper towel dispenser, to be agreed with school. Lockable sheet dispensing toilet paper holders. Sanitary bin.","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","N/A","CTS","Fire Containment.","Contractor to Specify if provided",null,"Add here text to be included on sign","CTS","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","All FF&E shall be provided as Group 2 by the contractor in a suitable and safe layout which allows for the preferences of the school and catering provider"]
["OFF00 (Office only)",null,null,null,"Office (only)","OFF00","Office for one or more members of staff with admin storage ",9,"m2","Administrative tasks (including use of ICT) and filing.",2,"N/A","/=K14","Staff and admin","Zone D","General","None",2,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB","As SoA","As SoA",2400,2400,"CTS",null,"Not Required ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V6","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A1.45/65","/=K188","Low","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,33,30,40,35,32,32,"R10","R10","<=1.0","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.         ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'max group size' defined in the SoA.  This equals the workstations for staff using the office on a permanent/semi permanent basis "]
["OFF10 (Office and meeting)",null,null,null,"Office/ meeting room","OFF10","Office for one or more members of staff, with space for meetings",13,"m2","Administrative tasks (including use of ICT). Small group meetings and interviews. ",5,"N/A","/=ROUNDDOWN(K14/2,0)","Staff and admin","Zone C","General","None",3,"none","As SoA","Disabled access into the area preferred","Enclosed","As SSDB","As SoA","As SoA",2400,2400,"CTS",null,"Not Required ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V6","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A1.45/65","/=K188","Low","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,33,30,40,35,32,32,"R10","R10","<=1.0","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.    ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'max group size' defined in the SoA.  This includes workstations for staff using the office on a permanent/semi permanent basis plus seats for having meetings."]
["OFF15 (Office and workroom)",null,null,null,"Office/workroom (technical staff)","OFF15","Office and workroom for one or more premises managers, caretakers or ICT technicians, with space for repair of equipment","As SoA","m2","Administrative tasks (including use of ICT). Basic maintenance and repair of ICT and other equipment. Storing small tools and items of IT equipment. Storing manuals and small maintenance equipment.","As SoA","N/A","/=K14","Staff and admin","Zone E","General","None",2,"none","As SoA","Disabled access into the area required","Enclosed","As SSDB","As SoA","As SoA",2400,2400,"CTS",null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V6","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A1.45/65","/=K188","Low","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,33,30,40,35,32,32,"R10","R10","<=1.0","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.    ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'max group size' defined in the SoA.  This equals the workstations for staff using the office on a permanent/semi permanent basis "]
["OFF20 (Office and pastoral)",null,null,null,"Office/ pastoral room","OFF20","Office for one or more members of staff, with space for informal meetings","As SoA","m2","Administrative tasks (including use of ICT) small informal meetings and interviews. Counselling.","As SoA","N/A","/=ROUNDDOWN(K14/2,0)","Staff and admin","Zone C","General","None",3,"none","As SoA","Disabled access into the area preferred","Enclosed","As SSDB","As SoA","As SoA",2400,2400,"N/A",null,"Not Required ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V6","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A1.45/65","/=K188","Low","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,33,30,40,35,32,32,"R10","R10","<=1.0","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.        ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'max group size' defined in the SoA.  This includes workstations for staff using the office on a permanent/semi permanent basis plus soft seating for informal meetings."]
["OFF31 (Staff room (prep social)",null,null,null,"Staff room (prep and social)","OFF31","Main space for any staff in school to work, meet and socialise, including preparation of teaching resources","As SoA","m2","Informal meeting and discussion during breaks. Lesson preparation and research mainly using tables. Limited ICT access. Marking and recording pupils work. Receiving post. Relaxing and taking refreshments.","As SoA","N/A","/=ROUNDUP(K14*0.15,0)","Staff and admin","Zone C","General","None",3,"none","As SoA","Disabled access into the area required","Enclosed","As SSDB","As SoA","As SoA",2700,2400,"CTS",null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1","Type L1.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V6","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A1.45/65","/=K188","Low","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,33,30,40,35,32,32,"R10","R10","<=1.0","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot and cold handwash and drinking water, including sink, teapoint, and dishwasher  ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'max group size' defined in the SoA.  This includes some workstations, some table-based seating and seating for socialising and informal meetings. "]
["OFF32 (Staff room social)",null,null,null,"Staff room (social)","OFF32","Main space for any staff in school to meet and socialise","As SoA","m2","Informal meeting and discussion during breaks. Limited ICT access. Receiving post/notices. Relaxing and taking refreshments.","As SoA","N/A",0,"Staff and admin","Zone B","General","None",3,"none","As SoA","Disabled access into the area required","Enclosed","As SSDB","As SoA","As SoA",2700,2400,"CTS",null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1","Type L1.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V6","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A1.45/65","/=K188","Low","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,33,30,40,35,32,32,"R10","R10","<=1.0","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.    ","None","Power sockets as FOS, on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot and cold handwash and drinking water, including sink, teapoint, and dishwasher  ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'max group size' defined in the SoA.  This equals seating for socialising and informal meetings. "]
["OFF33 (Staff work room)",null,null,null,"Staff work room","OFF33","Space for staff in [school or suite] to work and meet","As SoA","m2","Lesson preparation and research mainly using ICT with a hot desk arrangement. Marking and recording pupils work. Storage of some of staff's personal and teaching resources. Team meeting and discussions.","As SoA","N/A","/=K14","Staff and admin","Zone D","General","None",3,"none","As SoA","Disabled access into the area required","Enclosed","As SSDB","As SoA","As SoA",2700,2400,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V6","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A1.45/65","/=K188","Low","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,33,30,40,35,32,32,"R10","R10","<=1.0","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.    ","None","Power sockets as FOS, on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'max group size' defined in the SoA.  This equals the workstations for staff using the office on a semi permanent basis "]
["OFF35 (Staff wk rm (with sink)",null,null,null,"Staff work room (with sink)","OFF35","Space for staff in [school or suite] to work and meet","As SoA","m2","Lesson preparation and research mainly using ICT with a hot desk arrangement. Making drinks and/or snacks for staff, pupils or visitors. Marking and recording pupils work. Storage of some of staff's personal and teaching resources. Team meeting and discussions.","As SoA","N/A","/=K14","Staff and admin","Zone D","General","None",3,"none","As SoA","Disabled access into the area required","Enclosed","As SSDB","As SoA","As SoA",2700,2400,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","water resistant floor finish around sink area","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V6","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A1.45/65","/=K188","Low","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,33,30,40,35,32,32,"R10","R10","<=1.0","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.    ","None","Power sockets as FOS, on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot and cold handwash and drinking water, including sink and teapoint  ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'max group size' defined in the SoA.  This equals the workstations for staff using the office on a semi permanent basis "]
["OFF41 (Conference and meeti...",null,null,null,"Conference/ meeting room","OFF41","Conference room for meetings of staff, governors and other adults","As SoA","m2","Meeting room for staff with internal and external visitors etc. Privacy important. Small scale presentations using ICT.","As SoA","N/A",0,"Staff and admin","Zone C","General","Optional ",2,"none","As SoA","Disabled access into the area required","Enclosed","As SSDB","As SoA","As SoA",2400,2400,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V6","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A2.40/60","/=K188","Low","Low",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08","R08","<=0.8","<=0.8","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.    ","None","Power sockets as FOS, on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'max group size' defined in the SoA.  "]
["OFF42 (Laundry)",null,null,null,"Laundry","OFF42","Room for washing, drying and sorting pupils clothes","As SoA","m2"," Washing, drying and sorting pupils clothes.",2,"N/A","N/A","Non-net","N/A","Non-net","None",null,null,"As SoA","Disabled access into the space required","Enclosed","As SSDB",4,4,2400,2400,"N/A",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.2vhs","Note 1","Special, strong, with vision panel, humid areas",30,"  ",1026,null,925,null,2000,null,5,null,4,null,30,null,"Yes",null,"Yes",null,"Yes",null,"No",null,"No",null,"Protected",null,"Yes",null,"Yes",null,"No",null,"Yes",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Ergonomic handle and access control system to be agreed with school","Type F7","Note 1","Wet area ceramic, resin, rubber or vinyl","Yes for vinyl",null,"Commercial 34",null,"N/A",null,0.2,null,10,null,"Yes, see note",null,"Minimum SRV 36",null,"Yes",null,"Yes",null,"High",null,"No",null,"Yes",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W2h","Type W2h","Humid areas and toilets",0.5,0.5,"Yes","Yes","N/A","N/A","Yes","Yes","Humid","Humid","N/A","Barefoot areas shall be barefoot slip resistance category B Tiling above sink as a minimum","Type L2.1","Type L2.1","Required","Required",0.5,"N/A",0.8,"N/A","N/A",0.3,500,500,750,750,165,165,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,"N/A",200,15,15,"Type V6","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.40/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R15","R15","<=1.5","<=2.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.    ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["PLA01 (Plant room)",null,null,null,"Plant room","PLA01","Internal room or cupboard for mechanical or electrical plant","CTS","m2","Mechanical or electrical plant facilities"," N/A ","N/A","N/A","Non-net","N/A","Non-net","None",7,"none","As SoA","Full disabled access not required","Enclosed","As SSDB","N/A","N/A","N/A"," N/A ","CTS",null,"Required in main plant room",null,"As existing","Contractor to specify if provided","Type D8","Note 1","Fire-resistant cupboard or plant",0,"  ",926,null,825,null,2000,null,3,null,4,null,60,null,"Yes",null,"No",null,"No",null,"Yes",null,"No",null,"Standard",null,"Yes",null,"No",null,"Pull face",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Door should open outwards and be able to be unlocked from inside the room.","Type F3","Note 1","Heavy practical concrete, resin, rubber or vinyl","Yes for rubber or vinyl",null,"Commercial 34",null,"N/A",null,0.2,null,10,null,"R11",null,"Minimum SRV 36",null,"Yes",null,"Yes",null,"Moderate",null,"Yes",null,"Yes",null,"Yes",null,"Type C2","Note 1","Humid",0.7,"Humid","Type W1h","Type W1h","Plant",0.5,0.5,"N/A","N/A","N/A","N/A","Yes","Yes","Humid","Humid","N/A","Suitable for heavy movable FF&E on castors ","Type L7.3","Type L7.3","Not required","Not required","N/A","N/A","N/A","N/A",0.3,"N/A",200,200,300,300,"N/A","N/A","N/A","N/A",25,25,"N/A","N/A",0.4,0.4,60,60,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","sw","No",null,"N/A","N/A",null,null,"Contractor to specify (CTS)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","Note 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","/=K188",null,null,null,"Contractor to specify (CTS)",null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A","N/A","N/A","CTS to suit M&E design proposed  ","CTS to suit M&E design proposed  ","CTS to suit M&E design proposed","CTS to suit M&E design proposed ","CTS","CTS","CTS","CTS","CTS","N/A","N/A","N/A","CTS","N/A","N/A","CTS","Fire Containment.","Contractor to Specify if provided",null,"Add here text to be included on sign","CTS","CTS","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","All FF&E shall be provided as Group 2 by the contractor in a suitable and safe layout which allows for easy access for future maintenance"]
["PLA02 (Server room)",null,null,null,"Server room","PLA02","Space for ICT servers","As SoA","m2","Server racks and switching with space for access and maintenance"," N/A ","N/A","N/A","Non-net","N/A","Non-net","None",7,"none","As SoA","Full disabled access not required","None","As SSDB","As SoA","As SoA",2400,2200,"N/A",null,"Not Required",null,"As existing","Contractor to specify if provided","Type D8","Note 1","Fire-resistant cupboard or plant",0,"  ",926,null,825,null,2000,null,3,null,4,null,60,null,"Yes",null,"No",null,"No",null,"Yes",null,"No",null,"Standard",null,"Yes",null,"No",null,"Pull face",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Door should open outwards and be unlockable from inside the room.","Type F2","Note 1","Light practical lino, resin, rubber or vinyl","Yes",null,"Commercial 33",null,"N/A",null,0.2,null,10,null,"N/A",null,"N/A",null,"Yes",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C2","Note 1","Humid",0.7,"Humid","Type W1h","Type W1h","Plant",0.5,0.5,"N/A","N/A","N/A","N/A","Yes","Yes","Humid","Humid","N/A"," All finishes shall be static resistant","Type L7.3","Type L7.3","Not required","Not required","N/A","N/A","N/A","N/A",0.3,"N/A",200,200,300,300,"N/A","N/A","N/A","N/A",25,25,"N/A","N/A",0.4,0.4,60,60,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","sw","No",null,"Type T8","Type T8","See note","See note","Contractor to specify (CTS)","See note","See note","See note","See note","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A",12,"N/A","Type V3b","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,2,null,"N/A","/=K188",null,null,null,"Contractor to specify (CTS)",null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A",null,null,"Minimum temperature in server room for legacy servers of 15oC. Temperatures above server racks to be below 27oC, with occasional temps of up to 200 hours at up to 30oC and up to a maximum air temperature of 35oC or higher temperatures as specified by manufacturer for new equipment. Air change rate for battery back up and filtration of fresh air to satisfy manufacturer's requirements.   ","None ","Power","None  ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Fire Containment.","Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","All fitted and fixed FF&E shall be provided as Group 2 by the contractor, using legacy items where appropriate, in a suitable and safe layout which allows for the preferences of the school and the ICT strategy"]
["RES00 (Group room)",null,null,null,"Group room","RES00","Room for assistance with individuals and groups","As SoA","m2","Individual/small group learning support. One to one counselling. Privacy required.","As SoA","N/A","/=ROUND(K14/4,0)","Learning resources","Zone B","General","None",4,"none","As SoA","Full disabled access required","Enclosed","As SSDB","As SoA","As SoA",2400,2400,"CTS",null,"Not Required ",null,"As existing","Contractor to specify if provided","Type D1.1v","Type D1.1v","General, with vision panel",30,30,926,926,825,825,2000,2000,5,5,3,3,30,30,"Yes","Yes","No","No","Yes","Yes","No","No","No","No","Standard","Standard","Yes","Yes","Yes","Yes","No","No","No","No",200,200,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Access control and hinge protection to be agreed with school if used by foundation stage pupils (nursery and reception)","Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.35/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,35,40,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.    ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'max group size' defined in the SoAs. "]
["SEN01 (SEN resource base)",null,null,null,"SEN resource base","SEN01","Small room for assistance with individuals and groups with SEN",16,"m2","Individual therapy and counselling. Individual/small group learning support. Staff meetings.",7,"N/A",3,"Learning resources","Zone C","General","None ",6,"none","As SoA","Full disabled access required","Enclosed","As SSDB",16,16,2400,2400,"CTS",null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.1v","Note 1","General, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A2.40/60","/=K188","Low","Low",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.    ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'max group size' defined in the SoA.  "]
["SEN06 (Inclusion immersion...)",null,null,null,"Inclusion/ immersion facilities","SEN06","Room for assistance of individuals and groups with SEN","As SoA","m2","Individual/ small group learning support. Private counselling.","As SoA","As SoA","varies","Learning resources","Zone B","General","None ",6,"none","As SoA","Full disabled access required","Enclosed","As SSDB",16,16,2400,2400,"N/A",null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A4.30/55","/=K188","Average","Low",null,"Contractor to specify (CTS)",null,30,35,55,60,38,35,45,40,37,37,"R04","R04","N/A","<=0.4","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.    ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["SEN11 (SEN therapy and MI r...",null,null,null,"SEN therapy/ MI room","SEN11","Room for physio- and other therapy and medical inspections",12,"m2","Administering drug treatments to pupils. Medical inspection by external practitioners. Physio- or speech therapy for pupils with special needs.",3,"N/A","/=ROUND(K14/4,0)","Staff and admin","N/A","General","Optional for multi-agency work",5,"none","As SoA","Full disabled access required","Enclosed","As SSDB",12,12,2400,2400,"CTS",null,"Not Required ",null,"As existing","Contractor to specify if provided","Type D1.1","Note 1","General, no vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"No",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W3n","Note 1","Jointless",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V6","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"A2.40/60","/=K188","Low","Low",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.    ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Cold, with hot and cold handwash  ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'max group size' defined in the SoA.  "]
["STH00 (PE store(s))",null,null,null,"PE store(s) (sports hall)","STH00","Storage for PE and sports equipment, including mats","As SoA","m2","Storing PE and sports equipment including trampolines, forms, racquets and balls."," N/A ","N/A"," N/A ","Storage (teaching)","N/A","General","Optional",3,"adjacent sports hall","As SoA, off hall postioned to allow access from any subdivisions of hall","Full disabled access not required","Enclosed or open to sports hall","As SSDB","As SoA","As SoA",2400,2200,5000,"preferred","Not Required ",null,"N/A","Contractor to specify if provided","Type DD9","Note 1","Hall store",0,"  ",926,null,"825 (1650)",null,"2000 (see note)",null,3,null,4,null,0,null,"Yes",null,"No",null,"No",null,"No",null,"No",null,"Standard",null,"Yes",null,"No",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Dimensions to suit equipment to be stored, particularly trampolines","Type F2","Note 1","Light practical lino, resin, rubber or vinyl","Yes",null,"Commercial 33",null,"N/A",null,0.2,null,10,null,"N/A",null,"N/A",null,"Yes",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L7.2c","Type L7.2c","Not required","Not required","N/A","N/A","N/A","N/A","N/A","N/A",100,100,150,150,"N/A","N/A","N/A","N/A",24,24,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V2b","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"N/A","/=K188",null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A",null,null,"     ","None","None","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Fire Containment. Separate mat storage required if mats not flame retardent.","Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Contractor to provide fitted shelves and hooks to suit storage of  items to be stored, in agreement with the school and taking account of legacy items. Loose FF&E to be stored in primary PE store to match generic list in HAL13 and/or legacy items."]
["STH05 (External PE store)",null,null,null,"External PE store","STH05","Store for external PE and sports activities",8,"m2","Storing equipment for outdoor sports including goals, nets, bats, racquets, balls."," N/A ","N/A"," N/A ","Storage (teaching)","N/A","General","Optional",3,"none","As SoA","Full disabled access not required","Enclosed","As SSDB",8,7,2400,2200,"CTS",null,"Double doors required ",null,"N/A","Contractor to specify if provided","N/A","Note 1","No internal door required",null,"  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F2","Note 1","Light practical lino, resin, rubber or vinyl","Yes",null,"Commercial 33",null,"N/A",null,0.2,null,10,null,"N/A",null,"N/A",null,"Yes",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W2h","Type W2h","Humid areas and toilets",0.5,0.5,"Yes","Yes","N/A","N/A","Yes","Yes","Humid","Humid","N/A"," ","Type L7.2c","Type L7.2c","Not required","Not required","N/A","N/A","N/A","N/A","N/A","N/A",100,100,150,150,"N/A","N/A","N/A","N/A",24,24,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No",null,"Type T9","Type T9",5,5,"Contractor to specify (CTS)","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","Type V2b","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"N/A","/=K188",null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A",null,null,"     ","None","None","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Fire Containment.","Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Contractor to provide fitted shelves and hooks to suit storage of  items to be stored, in agreement with the school and taking account of legacy items. "]
["STH10 (Furniture store)",null,null,null,"Furniture/ equipment store(s)","STH10","Storage for chairs and tables used in hall","As SoA","m2","Storage for chairs for assemblies, exams and performances, as well as dining (with tables if required) in an adjacent hall."," N/A ","N/A"," N/A ","Storage (non-teaching)","N/A","General","Optional",3,"dining area(s)","As SoA","Disabled access not required","Enclosed","As SSDB, directly off hall","As SoA","As SoA",2400,2200,1800,"minimum","None ",null,"N/A","Contractor to specify if provided","Type DD9","Note 1","Hall store",0,"  ",926,null,"825 (1650)",null,"2000 (see note)",null,3,null,4,null,0,null,"Yes",null,"No",null,"No",null,"No",null,"No",null,"Standard",null,"Yes",null,"No",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Dimensions to suit equipment to be stored, particularly folding dining tables","Type F2","Note 1","Light practical lino, resin, rubber or vinyl","Yes",null,"Commercial 33",null,"N/A",null,0.2,null,10,null,"N/A",null,"N/A",null,"Yes",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L7.2c","Type L7.2c","Not required","Not required","N/A","N/A","N/A","N/A","N/A","N/A",100,100,150,150,"N/A","N/A","N/A","N/A",24,24,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No",null,"Type T9","Type T9",5,5,"Contractor to specify (CTS)","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","Type V2b","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"N/A","/=K188",null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A",null,null,null,"None","None","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Fire Containment.","Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Dimensions of store to suit dimensions of chairs and tables (including trolleys)"]
["STN01 (Personal storage (cl...",null,null,null,"Personal storage (cloakrooms)","STN01","Coat hooks and shelving for bags off circulation areas for pupils",2.5,"m2","Storing pupils personal belongings (coats, bags, books, PE equipment etc)."," N/A ","N/A"," N/A ","Storage (non-teaching)","N/A","General","None",2,"none","As SoA","Disabled access to at least 25% of coat hooks  required","Open plan","As SSDB",2.5,2.5,2400,2200,750,null,"Not Required ",null,"N/A","Contractor to specify if provided","N/A","Note 1","No internal door required",null,"  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1d","Note 1","Durable carpet, lino, rubber or vinyl","Yes",null,"Commercial 33",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L7.3","Type L7.3","Not required","Not required","N/A","N/A","N/A","N/A",0.3,"N/A",200,200,300,300,"N/A","N/A","N/A","N/A",25,25,"N/A","N/A",0.4,0.4,60,60,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","sw","No",null,"Type T9","Type T9",5,5,"Contractor to specify (CTS)","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","Type V2b","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"N/A","/=K188",null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,"R15","R15","<=1.5","<=2.0","     ","None","None","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Allow enough space for safe access.","Contractor to Specify if provided",null,"N/A","N/A","N/A","N/A","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the required area defined in the SoA. "]
["STN02 (Personal storage (lo",null,null,null,"Personal storage (lockers)","STN02","Lockers off circulation areas for pupils, not including circulation",6,"m2","Storing pupils personal belongings (coats, bags, books, PE equipment etc)."," N/A ","N/A"," N/A ","Storage (non-teaching)","N/A","General","None",2,"none","As SoA","Disabled access to at least 25% of lockers required","Open plan","off circulation area. As SSDB","As SoA","As SoA",2400,2200,750,null,"Not Required unless for fire. CTS if provided ",null,"N/A","Contractor to specify if provided","N/A","Note 1","No internal door required",null,"  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1d","Type F1d","Durable carpet, lino, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A","0.2, 0.15 if carpet","0.2, 0.15 if carpet",10,10,"No","No","No","No","No","No","Yes","Yes","Moderate","Moderate","Yes","Yes","No","No","No","No","Type C1","Note 1","General",0.7,"Normal","Type W1n","Type W1n","General",0.5,0.5,"N/A","N/A","N/A","N/A","Yes","Yes","Normal","Normal","N/A"," ","Type L7.3","Type L7.3","Not required","Not required","N/A","N/A","N/A","N/A",0.3,"N/A",200,200,300,300,"N/A","N/A","N/A","N/A",25,25,"N/A","N/A",0.4,0.4,60,60,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","sw","No",null,"Type T7","Type T7",18,18,"Contractor to specify (CTS)",15,15,21,21,40,"N/A",6,"N/A",4,"N/A","N/A","N/A","N/A","N/A",200,200,12,12,"Type V2b","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"N/A","Note 1",null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,"R15","R15","<=1.5","<=2.0","     ","None","None","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Allow enough space for safe access.","Contractor to Specify",null,"N/A","N/A","N/A","N/A","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the required area defined in the SoA. Assumes lockers in a linear arrangement"]
["STN04 (Wheelchair and appli...",null,null,null,"Wheelchair/ appliances bay(s)","STN04","Space for wheelchairs and similar appliances, off circulation area ","CTS","m2","Space for appliances to be stored and charged where necessary. Space for wheelchairs."," N/A ","N/A"," N/A ","Storage (non-teaching)","N/A","General","None",2,"none","As SoA","Full disabled and trolley access required","Open plan","Off circulation area. As SSDB","As SoA","As SoA",2400,2200,750,null,"Not Required",null,"N/A",null,"N/A","Note 1","No internal door required",null,"  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1d","Note 1","Durable carpet, lino, rubber or vinyl","Yes",null,"Commercial 33",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L7.3","Type L7.3","Not required","Not required","N/A","N/A","N/A","N/A",0.3,"N/A",200,200,300,300,"N/A","N/A","N/A","N/A",25,25,"N/A","N/A",0.4,0.4,60,60,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","sw","No",null,"Type T7","Type T7",18,18,"Contractor to specify (CTS)",15,15,21,21,40,"N/A",6,"N/A",4,"N/A","N/A","N/A","N/A","N/A",200,200,12,12,"Type V2b","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"N/A","/=K188",null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,"R15","R20","<=1.5","<=2.0","If space is refurbished, see Note 2 in tech annexe.    ","None","Power socket for recharging where appropriate","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Allow enough space for safe access.","Contractor to Specify if provided",null,"N/A","N/A","N/A","N/A","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["STN21 (Secure and exam and ...",null,null,null,"Secure/ exam/ archive store","STN21","Secure store room for  storage of exam papers or archives",5,"m2","Storing examination papers, archived documents or other confidential items securely."," N/A ","N/A"," N/A ","Storage (non-teaching)","N/A","General","None",7,"all spaces used for exams, when exams needed","As SoA","Full disabled access not required","Securely enclosed","As SSDB",8,7,2400,2200,"CTS",null,"Not Required ",null,"N/A","Contractor to specify if provided","Type D7","Type D7","Fire-resistant, no vision panel",0,0,926,926,825,825,2000,2000,3,3,4,4,60,60,"Yes","Yes","No","No","No","No","No","No","No","No","Standard","Standard","Yes","Yes","Yes","Yes","No","No","No","No",200,200,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Secure locks and ironmongery. 5-lever mortice locks or key pad required","Type F2","Note 1","Light practical lino, resin, rubber or vinyl","Yes",null,"Commercial 33",null,"N/A",null,0.2,null,10,null,"N/A",null,"N/A",null,"Yes",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L7.2c","Type L7.2c","Not required","Not required","N/A","N/A","N/A","N/A","N/A","N/A",100,100,150,150,"N/A","N/A","N/A","N/A",24,24,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No",null,"Type T9","Type T9",5,5,"Contractor to specify (CTS)","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","Type V2b","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"N/A","/=K188",null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A",null,null,"     ","None","None","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Fire Containment.","Contractor to Specify if provided","High security containment","Add here text to be included on sign","N/A","N/A","N/A","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Area allocation assumes 5 shelves."]
["STN31 (Cleaners store)",null,null,null,"Cleaners store","STN31","Cleaners' store with sink",1.5,"m2","Filling and emptying buckets. Storing cleaning materials and equipment."," N/A ","N/A"," N/A ","Storage (non-teaching)","N/A","General","None ",2,"none","As SoA","Full disabled access not required ","Enclosed ","As SSDB",1.5,1.5,2100,2000,"CTS",null,"Not Required ",null,"N/A","Contractor to specify if provided","Type D8","Note 1","Fire-resistant cupboard or plant",0,"  ",926,null,825,null,2000,null,3,null,4,null,60,null,"Yes",null,"No",null,"No",null,"Yes",null,"No",null,"Standard",null,"Yes",null,"No",null,"Pull face",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Door should open outwards and be unlockable from inside the room.","Type F2sc","Type F2sc","Chemical resistant light practical non-slip lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","N/A","N/A","Yes","Yes","Yes","Yes","Moderate","Moderate","Yes","Yes","Yes","Yes","No","No","Type C1","Note 1","General",0.7,"Normal","Type W2h","Type W2h","Humid areas and toilets",0.5,0.5,"Yes","Yes","N/A","N/A","Yes","Yes","Humid","Humid","N/A","Suitable for heavy movable FF&E on castors ","Type L7.2c","Type L7.2c","Not required","Not required","N/A","N/A","N/A","N/A","N/A","N/A",100,100,150,150,"N/A","N/A","N/A","N/A",24,24,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No",null,"Type T9","Type T9",5,5,"Contractor to specify (CTS)","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","Type V2b","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"N/A","/=K188",null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A",null,null,null,"None","None","Hot and cold to belfast sink  ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Staff-only access. Fire Containment.","Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","N/A","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["STT05 (Specialist store)",null,null,null,"Specialist teaching store","STT05","Store room for light practical resources or work in progress",5,"m2","Storing teaching resources and materials relevant to the teaching space (eg. art, graphics or music) and/or work in progress. Storing teaching resources including books, files and CDs."," N/A ","N/A"," N/A ","Storage (teaching)","N/A","General","None",3,"any adjacent teaching space","As SoA","Disabled access not required","Enclosed","As SSDB, directly off teaching space if art or light practical",5,5,2400,2200,1500,null,"Not Required ",null,"N/A","Contractor to specify if provided","Type D6","Note 1","Store room",0,"  ",926,null,825,null,2000,null,3,null,3,null,30,null,"Yes",null,"No",null,"No",null,"No",null,"No",null,"Standard",null,"Yes",null,"No",null,"Pull face",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Door to open outwards if store opens off teaching space.","Type F2","Note 1","Light practical lino, resin, rubber or vinyl","Yes",null,"Commercial 33",null,"N/A",null,0.2,null,10,null,"N/A",null,"N/A",null,"Yes",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L7.2c","Type L7.2c","Not required","Not required","N/A","N/A","N/A","N/A","N/A","N/A",100,100,150,150,"N/A","N/A","N/A","N/A",24,24,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No",null,"T9","T9",5,5,"Contractor to specify (CTS)","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","Type V2b","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"N/A","/=K188",null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A",null,null,"     ","None","Power sockets for recharging laptops where approprate","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Fire Containment.","Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","N/A","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Area allocation assumes 5 shelves."]
["STT10 (General store)",null,null,null,"General store","STT10","Store room for general teaching or ICT resources",5,"m2","Storing teaching resources including books, files and digital equipment."," N/A ","N/A"," N/A ","Storage (teaching)","N/A","General","None",2,"any adjacent teaching space","As SoA","Disabled access not required","Enclosed","As SSDB","As SoA","As SoA",2400,2200,1700,"minimum if over 4m2","Not Required ",null,"N/A","Contractor to specify if provided","Type D6","Note 1","Store room",0,"  ",926,null,825,null,2000,null,3,null,3,null,30,null,"Yes",null,"No",null,"No",null,"No",null,"No",null,"Standard",null,"Yes",null,"No",null,"Pull face",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Door to open outwards if store is adjacent teaching space","Type F2","Note 1","Light practical lino, resin, rubber or vinyl","Yes",null,"Commercial 33",null,"N/A",null,0.2,null,10,null,"N/A",null,"N/A",null,"Yes",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L7.2c","Type L7.2c","Not required","Not required","N/A","N/A","N/A","N/A","N/A","N/A",100,100,150,150,"N/A","N/A","N/A","N/A",24,24,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No",null,"Type T9","Type T9",5,5,"Contractor to specify (CTS)","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","Type V2b","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"N/A","/=K188",null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A",null,null,"     ","None","Power sockets for recharging laptops where appropriate","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Fire Containment.","Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","N/A","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the required area defined in the SoA. Area allocation assumes 5 shelves."]
["SUP01 (Chapel)",null,null,null,"Chapel (or similar)","SUP01","Chapel or similar for small group prayer and reflection","As SoA","m2","Individual/small group prayer and reflection. Private counselling.","As SoA","N/A","N/A","Learning resources","Zone A","General","None",4,"None","As SoA","Disabled access into the space required ","Enclosed ","As SSDB","As SoA","As SoA",2700,2400,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1b","As existing","Preferred","Preferred",0.5,null,0.8,null,0.3,null,300,null,450,null,100,null,150,null,19,null,"0.3 to 0.5",null,0.6,null,80,null,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A2.40/60","/=K188","Low","Low",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.2","R08.2","0.8 - 1.2","0.8 - 1.2","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.    ","None","Power sockets as FOS where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","FF&E shall be as discussed with the school, taking account of legacy items (see legacy survey), in a suitable layout."]
["TOC03 (Hygiene rm (without",null,null,null,"Hygiene room (without shower)","TOC03","Hygiene room for disabled pupils' washdown ",9,"m2","Room for changing pupils, with bed against wall, and two doors: one to nursery playroom (where applicable) and one to rest of school.",1,"N/A",2,"Non-net","N/A","Non-net","None",5,"all SEN and nursery spaces","As SoA","Full disabled access required","Enclosed","As SSDB",9,8,2700,2400,2400,"minimum","Not Required ",null,"As existing","Contractor to specify if provided","Type D4.2","Note 1","Suitable for wet areas and durable",30,"  ",926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"Yes",null,"No",null,"No",null,"No",null,"Standard",null,"Deadlock only",null,"No",null,"Both faces",null,"Yes",null,450,null,"Type D4.2","Note 1","Suitable for wet areas and durable",30,null,926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"Yes",null,"No",null,"No",null,"No",null,"Standard",null,"Deadlock only",null,"No",null,"Both faces",null,"Yes",null,450,null,"2 doors: one to nursery playroom (where applicable) and one to rest of school. Access control and hinge protection to be agreed with school if used by foundation stage pupils (nursery and reception). Surface protection to limit wheelchair damage.  Handles ergonomic to suit limited dexterity and to be at the correct height to promote independence. Means to control access to be agreed with school.","Type F7","Type F7","Wet area ceramic, resin, rubber or vinyl","Yes for vinyl","Yes for vinyl","Commercial 34","Commercial 34","N/A","N/A",0.2,0.2,10,10,"Yes, see note","Yes, see note","Minimum SRV 36","Minimum SRV 36","Yes","Yes","Yes","Yes","High","High","No","No","Yes","Yes","No","No","Type C2","Note 1","Humid",0.7,"Humid","Type W3w","Type W2h","Wet areas",0.5,0.5,"Yes","Yes","Yes","N/A","Yes","Yes","Wet","Humid","N/A","Barefoot areas shall be barefoot slip resistance category B. Ceiling to take hoist tracking in both directions, avoiding light fittings","Type L7.2","Type L7.2","Preferred","Preferred","N/A","N/A","N/A","N/A",0.3,0.3,200,200,300,300,70,70,"N/A","N/A",22,22,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No","Water / moisture grade luminaires if shower bed provided. Avoid direct downlighting over changing bed","Type T7a","Type T7a",18,18,"Contractor to specify (CTS)",15,15,21,21,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A",12,12,"Type V3","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.15,null,"10 ach (see note)",null,"A3.50/65","Note 1","Average","Medium",null,"Contractor to specify (CTS)",null,50,50,65,65,"N/A","N/A","N/A","N/A","N/A","N/A","R15","R15","<=1.5","<=2.0","Intermittent extract of 6l/s per WC/urinal and 15l/s per shower/bath or 10ach whichever is greater   ","None  ","Power to hand dryer if provided","Hot and cold with single mixer extended lever spray tap to handwash basin. Water to whb to be pre-mixed max temperature 43 degrees. Cartridge-type lockable soap dispenser. High velocity electric hand dryer or paper towel dispenser, to be agreed with school.","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Emergency call system","Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","N/A","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["TOC04 (Hygiene room (with w",null,null,null,"Hygiene room (with shower)","TOC04","Hygiene room for disabled pupils' washdown and toileting",12,"m2","Assisted shower. Peninsular WC able to be accessed from either side. Room for changing pupils, with bed against wall."," N/A ",1,2,"Non-net","N/A","Non-net","None",5,"all SEN spaces","As SoA","Full disabled access required","Enclosed","As SSDB",12,12,2700,2400,2700,"minimum","Not Required ",null,"As existing","Contractor to specify if provided","Type D4.2","Note 1","Suitable for wet areas and durable",30,"  ",926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"Yes",null,"No",null,"No",null,"No",null,"Standard",null,"Deadlock only",null,"No",null,"Both faces",null,"Yes",null,450,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Surface protection to limit wheelchair damage.  Handles ergonomic to suit limited dexterity and to be at the correct height to promote independence. Means to control access to be agreed with school. Access control and hinge protection to be agreed with school if used by foundation stage pupils (nursery and reception). ","Type F7","Type F7","Wet area ceramic, resin, rubber or vinyl","Yes for vinyl","Yes for vinyl","Commercial 34","Commercial 34","N/A","N/A",0.2,0.2,10,10,"Yes, see note","Yes, see note","Minimum SRV 36","Minimum SRV 36","Yes","Yes","Yes","Yes","High","High","No","No","Yes","Yes","No","No","Type C2","Note 1","Humid",0.7,"Humid","Type W3w","Type W2h","Wet areas",0.5,0.5,"Yes","Yes","Yes","N/A","Yes","Yes","Wet","Humid","N/A","Barefoot areas shall be barefoot slip resistance category B Ceiling to take hoist tracking in both directions, avoiding light fittings","Type L7.2","Type L7.2","Preferred","Preferred","N/A","N/A","N/A","N/A",0.3,0.3,200,200,300,300,70,70,"N/A","N/A",22,22,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No","Water / moisture grade luminaires","Type T7a","Type T7a",18,18,"Contractor to specify (CTS)",15,15,21,21,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A",12,12,"Type V3","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.15,null,"10 ach (see note)",null,"A3.50/65","Note 1","Average","Medium",null,"Contractor to specify (CTS)",null,50,50,65,65,"N/A","N/A","N/A","N/A","N/A","N/A","R15","R15","<=1.5","<=2.0","Intermittent extract of 6l/s per WC/urinal and 15l/s per shower/bath or 10ach whichever is greater.   ","None","Power to hand dryer if provided","wc. Cold, with hot and cold handwash. Hot and cold with single mixer extended lever spray tap to handwash basin. Water to whb to be pre-mixed max temperature 43 degrees. WC and whb. Cartridge-type lockable soap dispenser.  High velocity electric hand dryer or paper towel dispenser, to be agreed with school.  Lockable sheet dispensing toilet paper holders. Mirror above wash hand basin","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Emergency call system","Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","N/A","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["TOC13 (Pupil toilet suite)",null,null,null,"Pupil toilet suite","TOC13","Pupils' toilet cubicles and shared hand-wash/ dry area","CTS","m2","Toilet cubicles with shared hand washing and drying facilities.","CTS","N/A","N/A","Non-net","N/A","Non-net","None ",3,"none if others available","As SoA","Disabled access not required","Enclosed","As SSDB","As SoA","As SoA",2700,2400,"CTS",null,"Not Required ",null,"As existing","Contractor to specify if provided","Type D4.1","Note 1","Suitable for wet areas",30,"  ",926,null,825,null,2000,null,8,null,3,null,30,null,"Yes",null,"Yes",null,"No",null,"No",null,"No",null,"Standard",null,"Deadlock only",null,"No",null,"Pull face",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"If cubicle doors open inwards it shall be openable outwards in an emergency. ","Type F2sch","Type F2sch","Light practical non-slip hygienic  lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","SRV36 + 20 microns","SRV36 + 20 microns","Yes","Yes","Yes","Yes","High","High","Yes","Yes","Yes","Yes","No","No","Type C2","Note 1","Humid",0.7,"Humid","Type W2h","Type W2h","Humid areas and toilets",0.5,0.5,"Yes","Yes","N/A","N/A","Yes","Yes","Humid","Humid","N/A"," Tiling or similar above wash-hand basin as a minimum","Type L7.2","Type L7.2","Preferred","Preferred","N/A","N/A","N/A","N/A",0.3,0.3,200,200,300,300,70,70,"N/A","N/A",22,22,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No",null,"Type T7a","Type T7a",18,18,"Contractor to specify (CTS)",15,15,21,21,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A",12,12,"Type V2d","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"A3.50/65","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,50,50,65,65,"N/A","N/A","N/A","N/A","N/A","N/A","R15","R15","<=1.5","<=2.0","  Intermittent extract of 6l/s per WC/urinal or 10ach whichever is greater. If space is refurbished, see Note 2 in tech annexe.    ","None","Power to hand dryer if provided","Cold, with hot and cold handwash. Water to whb to be pre-mixed max temperature 43 degrees with single mixer tap. Sanitary ware, including hand washing and drying, to suit the number of wcs provided and the age of pupils. Cartridge-type lockable soap dispenser.  High velocity electric hand dryer or paper towel dispenser, to be agreed with school.  Lockable sheet dispensing toilet paper holders","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","(sanitaryware including fittings covered under Specific wet services requirements)"]
["TOC15 (Individual toilet)",null,null,null,"Individual toilet","TOC15","Individual pupil's toilet, sink and hand-wash/ dry in one space",3,"m2","Toilet and wash hand basin for ambulant pupils or staff.",1,"N/A","N/A","Non-net","N/A","Non-net","None",3,"none if others available","As SoA","Disabled access not required","Enclosed","As SSDB",3,2.5,2400,2200,"CTS",null,"Not Required ",null,"As existing","Contractor to specify if provided","Type D4.1n","Note 1","Suitable for toilets",30,"  ",926,null,825,null,2000,null,8,null,3,null,30,null,"Yes",null,"Yes",null,"No",null,"No",null,"No",null,"See note",null,"Deadlock only",null,"No",null,"Pull face",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Door leaf shall open inwards but be openable outwards in an emergency","Type F2sch","Type F2sch","Light practical non-slip hygienic  lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","SRV36 + 20 microns","SRV36 + 20 microns","Yes","Yes","Yes","Yes","High","High","Yes","Yes","Yes","Yes","No","No","Type C2","Note 1","Humid",0.7,"Humid","Type W2h","Type W2h","Humid areas and toilets",0.5,0.5,"Yes","Yes","N/A","N/A","Yes","Yes","Humid","Humid","N/A"," ","Type L7.2","Type L7.2","Preferred","Preferred","N/A","N/A","N/A","N/A",0.3,0.3,200,200,300,300,70,70,"N/A","N/A",22,22,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No",null,"Type T7a","Type T7a",18,18,"Contractor to specify (CTS)",15,15,21,21,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A",12,12,"Type V2d","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"A3.50/65","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,50,50,65,65,"N/A","N/A","N/A","N/A","N/A","N/A","R15","R15","<=1.5","<=2.0","Intermittent extract of 6l/s per WC/urinal and 15l/s per shower/bath. If space is refurbished, see Note 2 in tech annexe.     ","None","Power to hand dryers if provided","Cold, with hot and cold handwash. Water to whb to be pre-mixed max temperature 43 degrees with single mixer tap. Sanitary ware, including hand washing and drying. Cartridge-type lockable soap dispenser.  High velocity electric hand dryer or paper towel dispenser, to be agreed with school.  Lockable sheet dispensing toilet paper holders . Mirror above wash hand basin","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","(sanitaryware including fittings covered under Specific wet services requirements)"]
["TOC21 (Staff and accessible...",null,null,null,"Staff/ accessible toilet","TOC21","Accessible toilets suitable for disabled pupils as well as any staff or visitors",3.5,"m2","Unisex toilet and wash hand basin for non-ambulant pupils/adults, or ambulant staff or visitors.",1,"N/A",1,"Non-net","N/A","Non-net","Optional",4,"all spaces within 40m if required by wheelchair users","As SoA","Full disabled access required","Enclosed","As SSDB",3.5,3.5,2400,2200,2300,"minimum","Not Required ",null,"As existing","Contractor to specify if provided","Type D4.2","Note 1","Suitable for wet areas and durable",30,"  ",926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"Yes",null,"No",null,"No",null,"No",null,"Standard",null,"Deadlock only",null,"No",null,"Both faces",null,"Yes",null,450,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Door leaf to open outwards. Surface protection to limit wheelchair damage.  Handles ergonomic to suit limited dexterity and to be at the correct height to promote independence. ","Type F2sch","Type F2sch","Light practical non-slip hygienic  lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","SRV36 + 20 microns","SRV36 + 20 microns","Yes","Yes","Yes","Yes","High","High","Yes","Yes","Yes","Yes","No","No","Type C2","Note 1","Humid",0.7,"Humid","Type W2h","Type W2h","Humid areas and toilets",0.5,0.5,"Yes","Yes","N/A","N/A","Yes","Yes","Humid","Humid","N/A"," Tiling or similar above wash-hand basin as a minimum","Type L7.2","Type L7.2","Preferred","Preferred","N/A","N/A","N/A","N/A",0.3,0.3,200,200,300,300,70,70,"N/A","N/A",22,22,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No",null,"Type T7a","Type T7a",18,18,"Contractor to specify (CTS)",15,15,21,21,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A",12,12,"Type V3","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.15,null,"10 ach (see note)",null,"A3.50/65","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,50,50,65,65,"N/A","N/A","N/A","N/A","N/A","N/A","R15","R15","<=1.5","<=2.0","Intermittent extract of 6l/s per WC/urinal or 10ach whichever is greater. If space is refurbished, see Note 2 in tech annexe.     ","None  ","Power to hand dryers if provided","Cold, with hot and cold handwash. Hot and cold with single mixer extended lever spray tap to handwash basin. Water to whb to be pre-mixed max temperature 43 degrees. WC and whb. Cartridge-type lockable soap dispenser.  High velocity electric hand dryer or paper towel dispenser, to be agreed with school.  Lockable sheet dis pensing toilet paper holders. Mirror above wash hand basin","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","(sanitaryware including fittings covered under Specific wet services requirements)"]
["TOC22 (Staff toilet suite)",null,null,null,"Staff toilet suite","TOC22","Staff toilet cubicles and shared hand-wash/ dry area","CTS","m2","Toilet cubicles with shared hand washing and drying facilities.","CTS","N/A","N/A","Non-net","N/A","Non-net","None ",3,"none if others available","As SoA","Disabled access not required","Enclosed","As SSDB","As SoA","As SoA",2700,2400,"CTS",null,"Not Required ",null,"As existing","Contractor to specify if provided","Type D4.1","Note 1","Suitable for wet areas",30,"  ",926,null,825,null,2000,null,8,null,3,null,30,null,"Yes",null,"Yes",null,"No",null,"No",null,"No",null,"Standard",null,"Deadlock only",null,"No",null,"Pull face",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"If cubicle doors open inwards it shall be openable outwards in an emergency. ","Type F2sch","Type F2sch","Light practical non-slip hygienic  lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","SRV36 + 20 microns","SRV36 + 20 microns","Yes","Yes","Yes","Yes","High","High","Yes","Yes","Yes","Yes","No","No","Type C2","Note 1","Humid",0.7,"Humid","Type W2h","Type W2h","Humid areas and toilets",0.5,0.5,"Yes","Yes","N/A","N/A","Yes","Yes","Humid","Humid","N/A"," Tiling or similar above wash-hand basin as a minimum","Type L7.2","Type L7.2","Preferred","Preferred","N/A","N/A","N/A","N/A",0.3,0.3,200,200,300,300,70,70,"N/A","N/A",22,22,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No",null,"Type T7a","Type T7a",18,18,"Contractor to specify (CTS)",15,15,21,21,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A",12,12,"Type V2d","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"A3.50/65","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,50,50,65,65,"N/A","N/A","N/A","N/A","N/A","N/A","R15","R15","<=1.5","<=2.0","Intermittent extract of 6l/s per WC/urinal or 10ach whichever is greater. If space is refurbished, see Note 2 in tech annexe.     ","None","Power to hand dryer if provided","Cold, with hot and cold handwash. Water to whb to be pre-mixed max temperature 43 degrees with single mixer tap. Sanitary ware, including hand washing and drying, to suit the number of wcs provided. Mirror. Cartridge-type lockable soap dispenser.  High velocity electric hand dryer or paper towel dispenser, to be agreed with school.  Lockable sheet dispensing toilet paper holders","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify if provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","(sanitaryware including fittings covered under Specific wet services requirements)"]
["TOC03 (Hygiene rm (without",null,null,null,"Hygiene room (without shower)","TOC03","Hygiene room for disabled pupils' washdown ",9,"m2","Room for changing pupils, with bed against wall, and two doors: one to nursery playroom (where applicable) and one to rest of school.",1,"N/A",2,"Non-net","N/A","Non-net","None",5,"all SEN and nursery spaces","As SoA","Full disabled access required","Enclosed","As SSDB",9,8,2700,2400,2400,"minimum","Not Required ",null,"As existing","Contractor to specify if provided","Type D4.2","Note 1","Suitable for wet areas and durable",30,"  ",926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"Yes",null,"No",null,"No",null,"No",null,"Standard",null,"Deadlock only",null,"No",null,"Both faces",null,"Yes",null,450,null,"Type D4.2","Note 1","Suitable for wet areas and durable",30,null,926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"Yes",null,"No",null,"No",null,"No",null,"Standard",null,"Deadlock only",null,"No",null,"Both faces",null,"Yes",null,450,null,"2 doors: one to nursery playroom (where applicable) and one to rest of school. Access control and hinge protection to be agreed with school if used by foundation stage pupils (nursery and reception). Surface protection to limit wheelchair damage.  Handles ergonomic to suit limited dexterity and to be at the correct height to promote independence. Means to control access to be agreed with school.","Type F7","Type F7","Wet area ceramic, resin, rubber or vinyl","Yes for vinyl","Yes for vinyl","Commercial 34","Commercial 34","N/A","N/A",0.2,0.2,10,10,"Yes, see note","Yes, see note","Minimum SRV 36","Minimum SRV 36","Yes","Yes","Yes","Yes","High","High","No","No","Yes","Yes","No","No","Type C2","Note 1","Humid",0.7,"Humid","Type W3w","Type W2h","Wet areas",0.5,0.5,"Yes","Yes","Yes","N/A","Yes","Yes","Wet","Humid","N/A","Barefoot areas shall be barefoot slip resistance category B. Ceiling to take hoist tracking in both directions, avoiding light fittings","Type L7.2","Type L7.2","Preferred","Preferred","N/A","N/A","N/A","N/A",0.3,0.3,200,200,300,300,70,70,"N/A","N/A",22,22,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No","Water / moisture grade luminaires if shower bed provided. Avoid direct downlighting over changing bed","Type T7a","Type T7a",18,18,"Contractor to specify (CTS)",15,15,21,21,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A",12,12,"Type V3","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.15,null,"10 ach (see note)",null,"A3.50/65","Note 1","Average","Medium",null,"Contractor to specify (CTS)",null,50,50,65,65,"N/A","N/A","N/A","N/A","N/A","N/A","R15","R15","<=1.5","<=2.0","Intermittent extract of 6l/s per WC/urinal and 15l/s per shower/bath or 10ach whichever is greater   ","None  ","Power to hand dryer if provided","Hot and cold with single mixer extended lever spray tap to handwash basin. Water to whb to be pre-mixed max temperature 43 degrees. Cartridge-type lockable soap dispenser. High velocity electric hand dryer or paper towel dispenser, to be agreed with school.","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Emergency call system","Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","N/A","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["HAL12 (Small hall)",null,null,null,"Small hall","HAL12","Primary school space for movement, dance, gymnastics and other PE activities and exams, but not dining",80,"m2","Dance. Gymnastics. Occasional use for exams and exhibitions. Table tennis. Trampolining. Exhibitions.  Music and drama rehearsal and performance. Parent evenings. Presentations. Assessment.",30,30,4,"Halls and dining","N/A","Large and performance","Yes","6 or 7 if used for exams","adjacent store(s)","As SoA","Full disabled access","Enclosed","As SSDB",80,80,4500,3500,7500,"minimum","Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type DD2v","Note 1","Double acoustic, with vision panel",35,"  ",926,null,"825 (1500)",null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type DD2v","Note 1","Double acoustic, with vision panel",35,null,926,null,"825 (1500)",null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,"Plain meeting stiles","Type F4","Note 1","Hall lino, rubber, timber, composition or vinyl","Yes for vinyl",null,"Commercial 34",null,"N/A",null,0.2,null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"No",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Suitable for heavy movable FF&E on castors.","Type L4","Type L4","Required","Preferred",0.5,"N/A",0.8,"N/A",0.6,0.6,300,300,450,450,100,100,"N/A","N/A",22,22,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","Yes","Default illuminance 300 lux, but option to switch to 500 lux for some sports useful, see LG5","Type T4","/=K165",21,21,"Contractor to specify (CTS)",19,19,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,16,16,"Type V2","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A7.35/60","/=K188","High","Low",null,"Contractor to specify (CTS)",null,35,40,60,65,38,35,45,40,37,37,"R08.2","R08.2","0.8 - 1.2","0.8 - 1.2","A means of increasing the air velocity during the summer shall be provided. Ventilation rate to suit occupancy. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","No projections, including opening doors, to avoid injury during activity.","Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control. Dim-out blinds for performances","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. FF&E to be agreed with school"]
["HAL13 (Main hall)",null,null,null,"Main hall (primary)","HAL13","Multi-purpose hall for assembly, PE, exams and dining in primary schools","As SoA ","m2","Assemblies. Assessment. Dining of hot and cold food from adjacent servery area(s). Exhibitions. Gymnastics. Music and drama rehearsal and performance. Parent evenings. Presentations.","As SoA ",30,"N/A","Halls and dining","N/A","Large and performance","Yes","6 or 7 if used for exams","adjacent store(s)","As SoA","Disabled access required to all areas except some seating","Enclosed","As SSDB","As SoA","As SoA",4500,4200,10000,"minimum","Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type DD2v","Note 1","Double acoustic, with vision panel",35,"  ",926,null,"825 (1500)",null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type DD2v","Note 1","Double acoustic, with vision panel",35,null,926,null,"825 (1500)",null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,"Plain meeting stiles","Type F4","Note 1","Hall lino, rubber, timber, composition or vinyl","Yes for vinyl",null,"Commercial 34",null,"N/A",null,0.2,null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"No",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1ns","Note 1","Acoustic",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"Contractor to identify","Suitable for heavy movable FF&E on castors ","Type L4","Type L4","Required","Preferred",0.5,"N/A",0.8,"N/A",0.6,0.6,300,300,450,450,100,100,"N/A","N/A",22,22,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","Yes",null,"Type T4","/=K165",21,21,"Contractor to specify (CTS)",19,19,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,16,16,"Type V2","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A7.35/60","/=K188","High","Low",null,"Contractor to specify (CTS)",null,35,40,60,65,38,35,45,40,37,37,"R08.2","R08.2","0.8 - 1.2","0.8 - 1.2","A means of increasing the air velocity during the summer shall be provided. Ventilation rate to suit occupancy. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets where appropriate, separate circuits at high level for projector etc., plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","No projections, including opening doors, to avoid injury during activity.","Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control. Dim-out blinds for performances","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["LIB01 (Library )",null,null,null,"Library ","LIB01","Primary school library for all pupils","As SoA ","m2","Discussion. Individual study (including use of ICT). Informal reading and use of reference resources. Reading. Storage of books and other printed material. Whole class presentations.","As SoA ","As SoA",2,"Learning resources","Zone B","Light practical","None",4,"none","As SoA","Full disabled access","Enclosed or semi-enclosed","As SSDB","As SoA","As SoA",2700,2400,"CTS",null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.1v","Note 1","General, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A1.40/60","/=K188","Low","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R06.1","R06.1","<=0.6","<=0.8","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'max group size' defined in the SoAs. "]
["PRA01 (ICT rich practical r...",null,null,null,"ICT rich practical room","PRA01","Primary school classroom used for fixed ICT devices for all workplaces with limited layout options",62,"m2","Independent study and research. Individual, group and whole class pupil led presentations and discussions using ICT devices and whiteboard. Teacher led presentations and briefings using ICT and the whiteboard.",30,21,3,"Basic teaching","Zone D","Specialist","None",6,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB","As SoA","As SoA",2700,2400,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.35/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,35,40,60,65,33,30,40,35,32,32,"R06.1","R06.1","<=0.6","<=0.8","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot and cold water to all sinks listed under FF&E, cold water to belfast sink","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. Some FF&E proportional to the 'max group size' defined in the SoAs. Worktop to be constructed to allow it to be re-used at standing height at a later date."]
["PRA11 (Food bay and practic...",null,null,null,"Food bay/ practical resources","PRA11","Bay for primary food preparation with a small group and pupil access to practical resources",13,"m2","Group discussion. Independent study and research. Making and tasting food. Presentations. Simple supervised experiments and evaluation exercises.",4,"N/A",1,"Basic teaching","Zone D","Specialist","None",6,"none","As SoA","Disabled access into the space required","Semi-enclosed ","As SSDB",13,13,2700,2400,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L2.1","Type L2.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,500,500,750,750,165,165,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No","300 lux as in classrooms can be used if a higher lighting level can be achieved by task lighting or dimming if required","Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.40/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=0.8","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["PRA12 (Food science DT art)",null,null,null,"Food/ science/ DT/ art area","PRA12","Specialist space for primary food preparation, science, art and Design Technology activities","As SoA ","m2","Group discussion. Independent study and research. Making and tasting food. Presentations. Simple supervised experiments and evaluation exercises. Using the whiteboard.","As SoA","As SoA","/=ROUNDUP(K14/8,0)","Basic teaching","Zone D","Specialist","None",6,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB","As SoA","As SoA",2700,2400,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.2vh","Note 1","Strong, with vision panel, humid areas",30,"  ",926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"Yes",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F2sh","Type F2sh","Light practical hygienic lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","N/A","N/A","Yes","Yes","Yes","Yes","High","High","Yes","Yes","No","No","No","No","Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Suitable for heavy movable FF&E on castors ","Type L1.1","Type L1.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.40/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=0.8","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot and cold water to all sinks listed under FF&E","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. Some FF&E proportional to the 'max group size' defined in the SoAs. Some FF&E required depending on activities (food, art or DT) and title of space"]
["PRI03 (Nursery playroom)",null,null,null,"Nursery playroom","PRI03","Primary school playroom for a range of FF&E layout options and activities for 3 to 4 year olds",55,"m2","Group discussion. Using the whiteboard. Role play. Range of play activities. Quiet time. Small group work. Sand and water play. Solitary play. Computer-based play.",26,"As SoA","/=ROUNDUP(K14/8,0)","Basic teaching","Zone D","General","None",5,"none","As SoA","Disabled access into the space required","semi-enclosed","As SSDB","As SoA","As SoA",2700,2400,"CTS",null,"Required ",null,"As existing","Contractor to specify if provided","Type D1.1vs","Note 1","Special general, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Protected",null,"Yes",null,"Yes",null,"No",null,"Yes",null,200,null,"Type D1.1vs","Note 1","Special general, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Protected",null,"Yes",null,"Yes",null,"No",null,"  Yes ",null,200,null,"Ergonomic handle and access control system to be agreed with school","Type F1p","Note 1","Primary carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Carpet to part of area to suit FF&E layout ","Type L1.2","Type L1.2","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.35/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,35,40,60,65,33,30,40,35,32,32,"R06.1","R06.1","<=0.6","<=0.8","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot and cold water to all sinks listed under FF&E","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. Some FF&E proportional to the 'max group size' defined in the SoAs."]
["PRI04 (Nursery 2 to 3 year old)",null,null,null,"Nursery playroom (2 to 3 year old)","PRI04","Primary school playroom for a range of FF&E layout options and activities for 2 to 3 year olds","As SoA ","m2","Group discussion. Using the whiteboard. Role play. Range of play activities. Quiet time. Small group work. Sand and water play. Solitary play. Computer-based play.","As SoA ","As SoA","/=ROUNDUP(K14/5,0)","Basic teaching","Zone E","General","None",5,"none","As SoA","Disabled access into the space required","semi-enclosed","As SSDB","As SoA","As SoA",2700,2400,"CTS",null,"Required ",null,"As existing","Contractor to specify if provided","Type D1.1vs","Note 1","Special general, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Protected",null,"Yes",null,"Yes",null,"No",null,"Yes",null,200,null,"Type D1.1vs","Note 1","Special general, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Protected",null,"Yes",null,"Yes",null,"No",null,"  Yes ",null,200,null,"Ergonomic handle and access control system to be agreed with school","Type F1p","Note 1","Primary carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Carpet to part of area to suit FF&E layout ","Type L1.2","Type L1.2","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.35/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,35,40,60,65,33,30,40,35,32,32,"R06.1","R06.1","<=0.6","<=0.8","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot and cold water to all sinks listed under FF&E","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. Equipment shall be as provided by the school (see legacy survey), in a suitable layout."]
["PRI13 (Reception classroom)",null,null,null,"Reception classroom","PRI13","Primary school classroom for a range of FF&E layout options and activities for reception pupils","As SoA ","m2","Computer based play. Group discussion. Quiet time. Range of play activities. Role play. Sand and water play. Small group work. Solitary play. Using the whiteboard.","As SoA ","As SoA","/=ROUNDUP(K14/8,0)","Basic teaching","Zone D","General","None",5,"none","As SoA","Disabled access into the space required","Enclosed or Semi-enclosed","As SSDB, may open onto adjacent reception or nursery class","As SoA","As SoA",2700,2400,"CTS",null,"Required ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type DD1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Parliament",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Doors to open 180o if between classrooms","Type F1p","Note 1","Primary carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Carpet to part of area to suit FF&E layout ","Type L1.1","Type L1.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.35/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,35,40,60,65,33,30,40,35,32,32,"R06.1","R06.1","<=0.6","<=0.8","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot and cold water to all sinks listed under FF&E","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. Some FF&E proportional to the 'max group size' defined in the SoA. Some FF&E proportional to the 'average area of space' defined in the SoA."]
["PRI22 (Classbase with sink)",null,null,null,"Classbase with sink","PRI22","Primary school classbase for limited primary activities including water-based, typically for infant (KS1), with easy access to a shared teaching area without sink",50,"m2","Activity based play (typically for infants). Circle time. Group discussion. Range of play activities including water-based. Small group teaching. Small group work. Using ICT devices. Using the whiteboard. Whole class shared activity.",30,30,"/=ROUNDUP(K14/10,0)","Basic teaching","Zone B","General","None",5,"none","As SoA","Disabled access into the space required","Semi-enclosed","As SSDB, must open onto shared teaching area",50,49,2700,2400,"CTS",null,"Required ",null,"As existing","Contractor to specify if provided","N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1p","Note 1","Primary carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Carpet to part of area to suit FF&E layout ","Type L1.1","Type L1.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.35/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,35,40,60,65,33,30,40,35,32,32,"R06.1","R06.1","<=0.6","<=0.8","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot and cold water to all sinks listed under FF&E","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. "]
["PRI23 (Infant classroom)",null,null,null,"Infant classroom","PRI23","Primary school classroom for a range of FF&E layout options and activities for Key Stage 1 pupils",55,"m2","Activity based play. Circle time. Group discussion. Range of play activities. Small group teaching. Small group work. Using ICT devices. Using the whiteboard. Whole class shared activity.",30,30,"/=ROUNDUP(K14/10,0)","Basic teaching","Zone C","General","None",5,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB","As SoA","As SoA",2700,2400,"CTS",null,"Required ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1p","Note 1","Primary carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Carpet to part of area to suit FF&E layout ","Type L1.1","Type L1.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.35/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,35,40,60,65,33,30,40,35,32,32,"R06.1","R06.1","<=0.6","<=0.8","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot and cold water to all sinks listed under FF&E","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. Some FF&E proportional to the 'max group size' defined in the SoA. Some FF&E proportional to the 'average area of space' defined in the SoA."]
["PRI26 (Shared without sink)",null,null,null,"Shared teaching area without sink","PRI26","Open plan teaching area shared by adjacent classbases with sinks to enhance the range of activities, typically infant (KS1) ","As SoA ","m2","Group activities. Group discussion. Independent study and research. Use of ICT. Small group work. ","As SoA ","As SoA","/=ROUNDUP(K14/5,0)","Basic teaching","Zone C","General","None",5,"none","As SoA","Disabled access into the space required","Open plan","As SSDB","As SoA","As SoA",2700,2400,"N/A",null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","N/A","N/A","No internal door required",null,"  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Type D1.1v","Note 1","General, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1a","Type L1.1a","Required","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,"N/A","N/A",19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.40/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R05","R05","<=0.5","<=0.5","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'max group size' defined in the SoAs."]
["PRI32 (Classbase without sink)",null,null,null,"Classbase without sink","PRI32","Primary school classbase for limited primary activities, typically for junior (KS2), with easy access to a shared teaching area with sink",50,"m2","Activity based play (typically for junior). Circle time. Group discussion. Range of play activities not including water-based. Small group teaching. Small group work. Using ICT devices. Using the whiteboard. Whole class shared activity.",30,30,"/=ROUNDUP(K14/10,0)","Basic teaching","Zone B","General","None",5,"none","As SoA","Disabled access into the space required","Semi-enclosed","As SSDB",50,49,2700,2400,"CTS",null,"Required ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1p","Note 1","Primary carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Carpet to part of area to suit FF&E layout ","Type L1.1","Type L1.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.35/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,35,40,60,65,33,30,40,35,32,32,"R06.1","R06.1","<=0.6","<=0.8","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot and cold water to all sinks listed under FF&E","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. "]
["PRI33 (Junior classroom)",null,null,null,"Junior classroom","PRI33","Primary school classroom for a range of FF&E layout options and activities for Key Stage 2 pupils",55,"m2","Group activities. Group discussion. Independent study and research. Presentations. Use of ICT. Using the whiteboard. ",30,30,"/=ROUNDUP(K14/10,0)","Basic teaching","Zone C","General","None",5,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB","As SoA","As SoA",2700,2400,"CTS",null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1p","Note 1","Primary carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Carpet to part of area to suit FF&E layout ","Type L1.1","Type L1.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.35/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,35,40,60,65,33,30,40,35,32,32,"R06.1","R06.1","<=0.6","<=0.8","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot and cold water to all sinks listed under FF&E","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. Some FF&E proportional to the 'max group size' defined in the SoA. Some FF&E proportional to the 'average area of space' defined in the SoA."]
["PRI36 (Shared teach with sink)",null,null,null,"Shared teaching area with sink","PRI36","Open plan teaching area shared by adjacent classbases without sinks to enhance the range of activities, typically junior (KS2) ","As SoA ","m2","Group discussion. Painting. Small group work. Simple science activities. Water-based arts and crafts.","As SoA ","As SoA","/=ROUNDUP(K14/5,0)","Basic teaching","Zone C","General","None",5,"none","As SoA","Disabled access into the space required","Open plan","As SSDB","As SoA","As SoA",2700,2400,"N/A",null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","N/A","N/A","No internal door required",null,"  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Type D1.1v","Note 1","General, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1a","Type L1.1a","Required","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,"N/A","N/A",19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.40/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R05","R05","<=0.5","<=0.5","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot and cold water to all sinks listed under FF&E","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'max group size' defined in the SoAs."]
["RES41 (Pupil changing (dry))",null,null,null,"Pupil changing (dry)","RES41","Pupil changing (dry)","As SoA","m2","Small group dry changing room",15,"N/A","N/A","Learning resources","Zone B","General","None",4,"none","As SoA","Disabled access not required","Enclosed","As SSDB","As SoA","As SoA",2700,2400,"CTS",null,"Not Required ",null,"As existing","Contractor to specify if provided","Type D4.1","Note 1","suitable for wet areas",30,null,926,null,825,null,2000,null,8,null,3,null,30,null,"yes",null,"yes",null,"no",null,"no",null,"no",null,"standard",null,"deadlock only",null,"no",null,"pull face",null,"no",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Hinge protection required. Access controlto be agreed with school.","Type F2sh","Note 1","light practical hygienic  lino, resin, rubber or vinyl","Yes",null,"Commercial 33",null,"N/A",null,0.2,null,10,null,"R10",null,"N/A",null,"Yes",null,"Yes",null,"High",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," Suitable for heavy movable FF&E on castors ","Type L7.2","Type L7.2","Preferred","Preferred","N/A","N/A","N/A","N/A",0.3,0.3,200,200,300,300,70,70,"N/A","N/A",22,22,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",55,null,55,"N/A","N/A","occ, sw","No",null,"Type T4","/=K165",21,21,"Contractor to specify (CTS)",19,19,26,26,40,null,6,null,4,null,"N/A",120,"N/A",5,200,200,16,16,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.35/60","/=K188","Average","Medium",45,null,40,35,40,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.        ","None","Cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'max group size' defined in the SoAs. "]
["STT03 (Teaching storage bay)",null,null,null,"Teaching storage bay","STT03","Storage bay off classroom or classbase for teaching resources",1.5,"m2","Storing teaching resources and equipment."," N/A ","N/A","N/A","Storage (teaching)","N/A","General","None",2,"Adjacent teaching space","As SoA","Disabled access not required","Semi-enclosed","As SSDB, directly off classroom or classbase",1.5,1.5,2400,2200,900,null,"Not Required ","/","N/A","N/A ","N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"curtain or similar across doorway","Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L7.2c","Type L7.2c","Not required","Not required","N/A","N/A","N/A","N/A","N/A","N/A",100,100,150,150,"N/A","N/A","N/A","N/A",24,24,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No",null,"T9","/=K165",5,5,"Contractor to specify (CTS)","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","Type V2b","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"N/A","/=K188",null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A",null,null,null,"None","None","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'max group size' defined in the SoAs."]
["TOC11 (Foundation toilets)",null,null,null,"Foundation toilets","TOC11","Pupils' toilets and hand-wash/ dry area for early years, easily supervisable","As SoA ","m2","Easily supervisable toilet cubicles with shared hand washing facility.","As SoA ","N/A","N/A","Non-net","N/A","Non-net","None",4,"adjacent nursery playroom","As SoA","None","Enclosed","As SSDB, off nursery playroom","As SoA","As SoA",2700,2400,"CTS",null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D4.1ns","Note 1","Special suitable for toilets",30,"  ",926,null,825,null,2000,null,8,null,3,null,30,null,"Yes",null,"Yes",null,"No",null,"No",null,"No",null,"Protected",null,"Deadlock only",null,"No",null,"Pull face",null,"Yes",null,450,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Door to toilet area may not be required. Access control system to be agreed with school. If door leaf opens inwards it shall be openable outwards in an emergency","Type F2sch","Type F2sch","Light practical non-slip hygienic  lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","SRV36 + 20 microns","SRV36 + 20 microns","Yes","Yes","Yes","Yes","High","High","Yes","Yes","Yes","Yes","No","No","Type C2","Note 1","Humid",0.7,"Humid","Type W2h","Note 1","Humid areas and toilets",0.5,null,"Yes",null,"N/A",null,"Yes",null,"Humid",null,"N/A"," Tiling or similar above wash-hand basin as a minimum","Type L7.2","Type L7.2","Preferred","Preferred","N/A","N/A","N/A","N/A",0.3,0.3,200,200,300,300,70,70,"N/A","N/A",22,22,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No",null,"Type T7a","/=K165",18,18,"Contractor to specify (CTS)",15,15,21,21,"N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A",12,12,"Type V2d","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"A3.50/65","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,50,50,65,65,"N/A","N/A","N/A","N/A","N/A","N/A","R15","R15","<=1.5","<=2.0","Intermittent extract of 6l/s per WC/urinal and 15l/s per shower/bath or 6ach whichever is greater. If space is refurbished, see Note 2 in tech annexe.       ","None  ","Power to hand dryers if provided","Cold, with hot and cold handwash. Water to whb to be pre-mixed max temperature 43 degrees with single mixer tap. Sanitary ware, including hand washing and drying, to suit the number of wcs provided and the age of pupils. Cartridge-type lockable soap dispenser.  High velocity electric hand dryer or paper towel dispenser, to be agreed with school.  Lockable sheet dispensing toilet paper holders","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["ACT01 (Dance studio)",null,null,null,"Dance studio","ACT01","Space for movement, dance, gymnastics and exams, but not dining",120,"m2","Dance. Gymnastics. Occasional use for exams and exhibitions. Table tennis.",30,30,4,"Halls and dining","N/A","Large and performance","Yes","6 or 7 if used for exams","none","As SoA","Disabled access into the space required","Enclosed","As SSDB",120,120,4500,3500,10000,"minimum","Not Required unless for fire. CTS if provided Contractor to specify if provided",null,"As existing","Contractor to specify if provided","Type DD3v","Note 1","Sports hall, with vison panels",30,"  ",926,null,"875 (1200)",null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes, with safety glass",null,"No",null,"No",null,"Standard",null,"Yes",null,"No",null,"Pull face",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Plain meeting stiles. Must open out from hall space. All surfaces must be flush with no projecting frames or ironmongery.","Type F5","Note 1","Semi-sprung timber floor","N/A",null,"N/A",null,"A3",null,0.2,null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"No",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," Floor to match limits of impact and fatigue on human body in DIN 18032: Part 2, and must be easy to clean","Type L4","Type L4","Required","Preferred",0.5,"N/A",0.8,"N/A",0.6,0.6,300,300,450,450,100,100,"N/A","N/A",22,22,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","Yes","Default illuminance 300 lux, but option to switch to 500 lux for some sports useful, see LG5","Type T4","/=K165",21,21,"Contractor to specify (CTS)",19,19,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,16,16,"Type V2","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A6.40/60","/=K188","High","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R12.1","R12.1","<=1.2","<=1.5","A means of increasing the air velocity during the summer shall be provided.  Ventilation rate to suit occupancy. If space is refurbished, see Note 2 in tech annexe.   ","None","Power sockets as FOS, at low level on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","No projections, including opening doors, to avoid injury during activity.","Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Flat mirrors with no distortion on full length of longer wall, between 0.15m and 2.3m high, and horizontal Barres on two other walls at two heights between 900 and 1100 from FFL to top of Barre."]
["ACT05 (Activity studio)",null,null,null,"Activity studio","ACT05","Space for movement, dance, gymnastics and other PE activities and exams, but not dining",150,"m2","Dance. Gymnastics. Occasional use for exams and exhibitions. Table tennis. Trampolining.",30,30,4,"Halls and dining","N/A","Large and performance","Yes","6 or 7 if used for exams","Adjacent store(s)","As SoA","Disabled access into the space required","Enclosed","As SSDB",30,30,4500,4200,10000,"minimum","Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type DD3v","Note 1","Sports hall, with vison panels",30,"  ",926,null,"875 (1200)",null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes, with safety glass",null,"No",null,"No",null,"Standard",null,"Yes",null,"No",null,"Pull face",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Plain meeting stiles. Must open out from hall space. All surfaces must be flush with no projecting frames or ironmongery","Type F5","Note 1","Semi-sprung timber floor","N/A",null,"N/A",null,"A3",null,0.2,null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"No",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L4","Type L4","Required","Preferred",0.5,"N/A",0.8,"N/A",0.6,0.6,300,300,450,450,100,100,"N/A","N/A",22,22,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","Yes","Default illuminance 300 lux, but option to switch to 500 lux for some sports useful, see LG5","Type T4","/=K165",21,21,"Contractor to specify (CTS)",19,19,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,16,16,"Type V2","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A7.35/60","/=K188","High","Low",null,"Contractor to specify (CTS)",null,35,40,60,65,38,35,45,40,37,37,"R12.1","R12.1","<=1.2","<=1.5","A means of increasing the air velocity during the summer shall be provided.  Ventilation rate to suit occupancy. If space is refurbished, see Note 2 in tech annexe.      ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","No projections, including opening doors, to avoid injury during activity.","Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Barres on one wall at two heights between 900 and 100 from FFL to top of barre"]
["ACT22 (Fitness exercise)",null,null,null,"Fitness/exercise studio","ACT22","Space for weights, fixed machine cardio vascular exercise, movement, and other PE activities.","As SoA","m2","Fixed machine cardio vascular exercise. Trampolining. Weights.","As SoA","As SoA","/=ROUNDUP(K14/10,0)","Basic teaching","Zone G","Large and performance","Yes",6,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB","As SoA","As SoA",2700,2700,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type DD3v","Note 1","Sports hall, with vison panels",30,"  ",926,null,"875 (1200)",null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes, with safety glass",null,"No",null,"No",null,"Standard",null,"Yes",null,"No",null,"Pull face",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Plain meeting stiles. Must open out from hall space. All surfaces must be flush with no projecting frames or ironmongery","Type F2s","Note 1","Light practical non-slip lino, resin, rubber or vinyl","Yes",null,"Commercial 33",null,"N/A",null,0.2,null,10,null,"R10",null,"N/A",null,"Yes",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Suitable for heavy movable FF&E on castors. Floor surface must be able to withstand live loads from users, accidental point load impact (e.g. dropping of free weights), and dynamic effects (harmonic vibration from users on machines). ","Type L4","Type L4","Required","Preferred",0.5,"N/A",0.8,"N/A",0.6,0.6,300,300,450,450,100,100,"N/A","N/A",22,22,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","Yes","Default illuminance 300 lux, but option to switch to 500 lux for some sports useful, see LG5","Type T6","/=K165",17,17,"Contractor to specify (CTS)",15,15,23,23,40,40,6,6,4,4,"N/A","N/A","N/A","N/A",200,200,12,12,"Type V2","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A6.40/60","/=K188","High","Medium",null,"Contractor to specify (CTS)",null,40,40,60,65,33,35,40,40,32,37,"R12.1","R12.1","<=1.2","<=1.5","A means of increasing the air velocity during the summer shall be provided.  Ventilation rate to suit occupancy. If space is refurbished, see Note 2 in tech annexe.      ","None","Power sockets for each cardio machine and other equipment, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","No projections, including opening doors, to avoid injury during activity.","Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Equipment shall be as provided by the school (see legacy survey), in a suitable layout which allows for the size of each piece of equipment and safe space around it."]
["CLA02 (Seminar room)",null,null,null,"Seminar room","CLA02","Seminar room for smaller 14-19 groups with a range of FF&E layout options and activities",41,"m2","Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Teacher led presentations and briefings using the whiteboard.",22,24,3,"Basic teaching","Zone C","General","None ",5,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB","As SoA","As SoA",2700,2700,"CTS",null,"Not Required ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1","Type L1.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.35/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,35,40,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.        ","None ","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. Some FF&E proportional to the 'max group size' in the SoA."]
["CLA12 (General classroom)",null,null,null,"General classroom","CLA12","Secondary school classroom for a range of FF&E layout options and activities",55,"m2","Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard.",30,30,3,"Basic teaching","Zone C","General","None",5,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB","As SoA","As SoA",2700,2700,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1","Type L1.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.35/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,35,40,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.        ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. Some FF&E proportional to the 'max group size' in the SoA."]
["CLA13 (Extensive classroom)",null,null,null,"Extensive classroom","CLA13","Secondary school classroom for all classroom FF&E layout options and activities",62,"m2","Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard.",30,30,3,"Basic teaching","Zone D","General","None",5,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB","As SoA","As SoA",2700,2700,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1","Type L1.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.35/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,35,40,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.        ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. Some FF&E proportional to the 'max group size' in the SoA."]
["CLA18 (Open learning area)",null,null,null,"Open learning area","CLA18","Secondary school semi-open plan learning area for a range of layout options and activities","As SoA","m2","Group discussion. Independent study and research. Presentations. Using the whiteboard.","As SoA","As SoA","/=ROUNDUP(K14/10,0)","Basic teaching","Zone C","General","None ",5,"none","As SoA","Disabled access into the space required ","Open-plan or partially enclosed ","As SSDB",55,55,2700,2700,"CTS",null,"Not Required ",null,"As existing","Contractor to specify if provided","N/A","Note 1","No internal door required",null,"  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1","Type L1.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.40/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R05","R05","<=0.5","<=0.5","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.        ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. Some FF&E proportional to the 'max group size' in the SoA."]
["CLA31 (Temporarily ICT-rich...)",null,null,null,"Temporarily ICT-rich classroom","CLA31","Secondary school classroom with fixed ICT devices for all workplaces and a range of FF&E layout options",55,"m2"," Independent study and research. Individual, group and whole class pupil led presentations and discussions using ICT devices and whiteboard. Teacher led presentations and briefings using ICT and the whiteboard.",30,30,3,"Basic teaching","Zone C","General","None",5,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB",55,55,2700,2700,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1","Type L1.1","Required","Required",0.5,"N/A",0.8,"N/A","N/A",0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,"N/A",200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.35/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,35,40,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.        ","None","Power sockets to suit ICT provision, within dado trunking on 4 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. "]
["CLA32 (ICT-rich classroom)",null,null,null,"ICT-rich classroom","CLA32","Secondary school classroom with fixed ICT devices for all workplaces and a range of FF&E layout options",62,"m2","Independent study and research. Individual, group and whole class pupil led presentations and discussions using ICT devices and whiteboard. Teacher led presentations and briefings using ICT and the whiteboard.",30,21,3,"Basic teaching","Zone D","Light practical","None",5,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB",62,62,2700,2700,"N/A",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1","Type L1.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.40/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,40,40,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.        ","None","Power sockets to suit ICT provision, within dado trunking on 4 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","All FF&E in this space to be provided by the Contractor. Some FF&E proportional to the 'max group size' defined in the SoAs. "]
["CLA35 (ICT-rich learning area)",null,null,null,"ICT-rich learning area","CLA35","Semi-open plan area with fixed ICT devices for all workplaces and a range of FF&E layout options",62,"m2","Group discussion. Independent study and research. Presentations. Using ICT devices . Using the whiteboard.",30,21,3,"Basic teaching","Zone as SoA","Light practical","None",5,"none","As SoA","Disabled access into the space required","Open-plan or partially enclosed","As SSDB",62,62,2700,2700,"N/A",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.40/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.        ","None","Power sockets to suit ICT provision, within dado trunking on all walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'Group size' defined in the SoAs. "]
["CLA41 (ICT and business stu...",null,null,null,"ICT/ business studies room","CLA41","Secondary school classroom with fixed ICT devices for half of the workplaces with business environment",62,"m2","Independent study and research. Individual, group and whole class pupil led presentations and discussions using ICT devices predominantly by 14-19 age group. Occasional need for some furniture re-arrangement. Teacher led presentations and briefings using ICT and the whiteboard.",30,21,3,"Basic teaching","Zone D","Light practical","None ",6,"none","As SoA","Disabled access into the space required ","Enclosed","As SSDB",62,62,2700,2700,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.1v","Note 1","General, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1","Type L1.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.35/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,35,40,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.        ","None","Power sockets to suit ICT provision, within dado trunking on 4 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. Some FF&E proportional to the 'max group size' in the SoA."]
["DAT02 (General art room)",null,null,null,"General art room","DAT02","Secondary school art room for a range of FF&E layout options and activities suitable for general 2D art","As SoA","m2","Individual and group 2D work (drawing, painting). Individual, group and whole class pupil led presentations and discussions using the whiteboard. Small scale 3D work using a range of materials including card, plastic and wood. Some pupil research occasionally using ICT. Teacher led presentations and briefings using the whiteboard.","As SoA","As SoA",3,"Basic teaching","Zone F","Light practical","None ",6,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB","As SoA","As SoA",2700,2700,"CTS",null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.1v","Note 1","General, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F2sc","Type F2sc","Chemical resistant light practical non-slip lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","N/A","N/A","Yes","Yes","Yes","Yes","Moderate","Moderate","Yes","Yes","Yes","Yes","No","No","Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Suitable for heavy movable FF&E on castors ","Type L2.1","Type L2.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,500,500,750,750,165,165,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No","300 lux as in classrooms can be used if a higher lighting level can be achieved by task lighting or dimming if required","Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.40/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided.  Local extract ventilation based on risk assessment when practical work involving fumes is planned. If space is refurbished, see Note 2 in tech annexe.      ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot and cold water to sinks listed under FF&E","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. Some FF&E proportional to the 'max group size' in the SoA."]
["DAT03 (3D Art room)",null,null,null,"3D Art room","DAT03","Secondary school art room for general and 3D art including clay work",97,"m2","Individual and group 2D work (drawing, painting). Individual, group and whole class pupil led presentations and discussions using the whiteboard. Large scale 3D work such as sculpture using a range of materials including card, wood, textile and basic clay techniques. Teacher led presentations and briefings using the whiteboard.",30,30,3,"Basic teaching","Zone G","Light practical","None",6,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB","As SoA","As SoA",2700,2700,7500,"minimum","Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.1v","Note 1","General, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F2sc","Type F2sc","Chemical resistant light practical non-slip lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","N/A","N/A","Yes","Yes","Yes","Yes","Moderate","Moderate","Yes","Yes","Yes","Yes","No","No","Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Suitable for heavy movable FF&E on castors ","Type L2.1","Type L2.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,500,500,750,750,165,165,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No","300 lux as in classrooms can be used if a higher lighting level can be achieved by task lighting or dimming if required","Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.40/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided.  Local extract ventilation based on risk assessment when practical work involving fumes is planned. If space is refurbished, see Note 2 in tech annexe.      ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot and cold water to sinks listed under FF&E  ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Need to be able to clean surfaces of clay dust; sufficient space must be allowed around pottery equipment.","Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. Some FF&E proportional to the 'max group size' in the SoA."]
["DAT04 (3D art room (ceramics))",null,null,null,"3D art room (ceramics)","DAT04","Secondary school art room for general and 3D art including clay",104,"m2","2D work (drawing, painting). Large scale 3D work with extensive use of clay, including using a wheel. Whole class presentations and discussions using the whiteboard.",32,30,3,"Basic teaching","Zone G","Light practical","None",6,"none","As SoA","Disabled access into the space required ","Enclosed","As SSDB",104,104,2700,2700,7500,"minimum","Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.1v","Note 1","General, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F2sc","Type F2sc","Chemical resistant light practical non-slip lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","N/A","N/A","Yes","Yes","Yes","Yes","Moderate","Moderate","Yes","Yes","Yes","Yes","No","No","Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Suitable for heavy movable FF&E on castors ","Type L2.1","Type L2.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,500,500,750,750,165,165,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No","300 lux as in classrooms can be used if a higher lighting level can be achieved by task lighting or dimming if required","Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1a","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.40/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided.  Local extract ventilation based on risk assessment when practical work involving fumes is planned. If space is refurbished, see Note 2 in tech annexe.      ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Cold, with hot and cold handwash  ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Need to be able to clean surfaces of clay dust; sufficient space must be allowed around pottery equipment.","Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. Some FF&E proportional to the 'max group size' in the SoA."]
["DAT05 (3D art room (textiles)",null,null,null,"3D art room (textiles)","DAT05","Secondary school art room for general artwork and printing techniques and 3D art ",104,"m2","2D work (drawing, painting). Printing techniques for 2D and 3D work. Whole class presentations and discussions using the whiteboard.",32,30,3,"Basic teaching","Zone G","Light practical","None",6,"none","As SoA","Disabled access into the space required ","Enclosed","As SSDB",104,104,2700,2700,7500,"minimum","Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.1v","Note 1","General, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F2sc","Type F2sc","Chemical resistant light practical non-slip lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","N/A","N/A","Yes","Yes","Yes","Yes","Moderate","Moderate","Yes","Yes","Yes","Yes","No","No","Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Suitable for heavy movable FF&E on castors","Type L2.1","Type L2.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,500,500,750,750,165,165,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No","300 lux as in classrooms can be used if a higher lighting level can be achieved by task lighting or dimming if required","Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1a","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.40/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided.  Local extract ventilation based on risk assessment when practical work involving fumes is planned. If space is refurbished, see Note 2 in tech annexe.      ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Cold, with hot and cold handwash  ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Need to be able to clean surfaces of clay dust; sufficient space must be allowed around pottery equipment.","Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. Some FF&E proportional to the 'max group size' in the SoA."]
["DAT12 (Hair and beauty salo",null,null,null,"Hair and beauty salon","DAT12","Secondary school salon for hair styling and beauty therapy",69,"m2","Individual and paired pupil practical work and teacher demonstration using specialist chairs, basins and beds. Occasional use of mobile tables and the whiteboard. Waiting area for those being treated.",16,"As SoA",3,"Basic teaching","Zone H","Heavy practical","None",6,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB","As SoA","As SoA",2700,2700,"CTS",null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.1v","Note 1","General, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F2","Type F2","Light practical lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"N/A","N/A","N/A","N/A","Yes","Yes","Yes","Yes","Moderate","Moderate","Yes","Yes","No","No","No","No","Type C1","Note 1","General",0.7,"Normal","Type W4","As existing","Rough",0.5,null,"N/A",null,"N/A",null,"N/A",null,"Normal",null,"N/A","Suitable for heavy movable FF&E on castors ","Type L2.1","Type L2.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,500,500,750,750,165,165,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No","300 lux as in classrooms can be used if a higher lighting level can be achieved by task lighting or dimming if required","Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1a","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A5.40/60","Note 1","High","High",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided.  Local extract ventilation based on risk assessment when practical work involving fumes is planned   ","Bottled gas only","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Cold, with hot and cold handwash  ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Safe distances around fixed equipment and workbenches","Contractor to Specify",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. Some FF&E proportional to the 'max group size' in the SoA."]
["DAT15 (Photography studio)",null,null,null,"Photography studio","DAT15","Secondary school studio for practical photography and editing","As SoA","m2","Individual and group photography, using a range of equipment including white background, lighting and tripod. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Photo editing and pupil research using ICT. Teacher led presentations and briefings using the whiteboard.","As SoA","As SoA",3,"Basic teaching","Zone F","Light practical","None ",6,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB","As SoA","As SoA",2700,2700,"N/A",null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.1v","Note 1","General, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F2sc","Type F2sc","Chemical resistant light practical non-slip lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","N/A","N/A","Yes","Yes","Yes","Yes","Moderate","Moderate","Yes","Yes","Yes","Yes","No","No","Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","At least one wall shall be clear and white. Suitable for heavy movable FF&E on castors ","Type L2.1","Type L2.1","Required","Required",0.5,"N/A",0.8,"N/A","N/A",0.3,500,500,750,750,165,165,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No","300 lux as in classrooms can be used if a higher lighting level can be achieved by task lighting or dimming if required","Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,"N/A",200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.40/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided.  Local extract ventilation based on risk assessment when practical work involving fumes is planned. If space is refurbished, see Note 2 in tech annexe.    ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot and cold water to sinks listed under FF&E","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows"]
["DAT22 (Graphic products)",null,null,null,"Graphic products","DAT22","Secondary school room for graphics and light, small scale product design",83,"m2","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Small scale making with card and some plastics. Traditional and computer based drawing and design.",25,30,3,"Basic teaching","Zone G","Light practical","None ",6,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB",83,80,2700,2700,"CTS",null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.1v","Note 1","General, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F2","Note 1","Light practical lino, resin, rubber or vinyl","Yes",null,"Commercial 33",null,"N/A",null,0.2,null,10,null,"N/A",null,"N/A",null,"Yes",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L2.1","Type L2.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,500,500,750,750,165,165,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No","300 lux as in classrooms can be used if a higher lighting level can be achieved by task lighting or dimming if required","Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.40/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided.  Local extract ventilation based on risk assessment when practical work involving fumes is planned. If space is refurbished, see Note 2 in tech annexe.    ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot and cold water to all sinks listed under FF&E  ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows"]
["DAT25 (Constructional texti...",null,null,null,"Constructional textiles","DAT25","Secondary school room for working with textiles",83,"m2","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making with textiles including traditional and computerised sewing and knitting machines. Traditional and computer based drawing and design.",25,30,3,"Basic teaching","Zone G","Light practical","None ",6,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB",83,80,2700,2700,"CTS",null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.1v","Note 1","General, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F2","Note 1","Light practical lino, resin, rubber or vinyl","Yes",null,"Commercial 33",null,"N/A",null,0.2,null,10,null,"N/A",null,"N/A",null,"Yes",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L2.1","Type L2.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,500,500,750,750,165,165,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No","300 lux as in classrooms can be used if a higher lighting level can be achieved by task lighting or dimming if required","Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.40/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided.  Local extract ventilation based on risk assessment when practical work involving fumes is planned. If space is refurbished, see Note 2 in tech annexe.    ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot and cold water to all sinks listed under FF&E","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows"]
["DAT28 (Electronics and cont...",null,null,null,"Electronics and control systems","DAT28","Secondary school room for electronics, pneumatics and light, small scale product design",83,"m2","Drawing. ICT based research and design. Incorporating electronic. Robotic and pneumatic techniques. Small scale making with card. Whole class presentations and discussions using the whiteboard. Wood and plastics.",25,30,3,"Basic teaching","Zone G","Light practical","None ",6,"none","As SoA","Disabled access into the space required ","Enclosed ","As SSDB",83,83,2700,2700,"CTS",null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.1v","Note 1","General, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F2","Note 1","Light practical lino, resin, rubber or vinyl","Yes",null,"Commercial 33",null,"N/A",null,0.2,null,10,null,"N/A",null,"N/A",null,"Yes",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L2.1","Type L2.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,500,500,750,750,165,165,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No","300 lux as in classrooms can be used if a higher lighting level can be achieved by task lighting or dimming if required","Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.40/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided.  Local extract ventilation based on risk assessment when practical work involving fumes is planned. If space is refurbished, see Note 2 in tech annexe.    ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Safe distances around machines.","Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows"]
["DAT32 (Food studio)",null,null,null,"Food studio","DAT32","Secondary school food room for demonstrations of food preparation",69,"m2","ICT based research and design. Making and tasting food. Teacher demonstrations. Using the whiteboard. Whole class presentations and discussions.",24,15,3,"Basic teaching","Zone F","Heavy practical","None ",6,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB","As SoA","As SoA",2700,2700,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.2vh","Note 1","Strong, with vision panel, humid areas",30,"  ",926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"Yes",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.2vh","Note 1","Strong, with vision panel, humid areas",30,null,926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"Yes",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F2sh","Type F2sh","Light practical hygienic lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","N/A","N/A","Yes","Yes","Yes","Yes","High","High","Yes","Yes","No","No","No","No","Type C2","Note 1","Humid",0.7,"Humid","Type W3h","Type W3h","Humid",0.5,0.5,"Yes","Yes","Yes","Yes","Yes","Yes","Humid","Humid","N/A","Suitable for heavy movable FF&E on castors ","Type L2.1e","Type L2.1e","Required","Required",0.5,0.5,0.8,0.8,0.3,0.3,500,500,750,750,165,165,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, sw, dim","Yes","300 lux as in classrooms can be used if a higher lighting level can be achieved by task lighting or dimming if required","Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1a","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.40/60","Note 1","Average","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided.  Local extract ventilation based on risk assessment when practical work involving fumes is planned   ","Yes, to gas ovens and hobs.   ","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot, and cold drinking water to all sinks, with hot and cold to handwash basin  ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Need to be able to clean surfaces thoroughly to maintain hygiene; safe distances around cookers.","Contractor to Specify",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows"]
["DAT35 (Food room)",null,null,null,"Food room","DAT35","Secondary school food room for non-vocational practical cookery activities by pupils in pairs",104,"m2","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making and tasting food. Teacher practical demonstrations. Traditional and computer based drawing and design of recipes etc.",24,"As SoA",3,"Basic teaching","Zone H","Heavy practical","None",6,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB","As SoA","As SoA",2700,2700,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.2vh","Note 1","Strong, with vision panel, humid areas",30,"  ",926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"Yes",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.2vh","Note 1","Strong, with vision panel, humid areas",30,null,926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"Yes",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F2sh","Type F2sh","Light practical hygienic lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","N/A","N/A","Yes","Yes","Yes","Yes","High","High","Yes","Yes","No","No","No","No","Type C2","Note 1","Humid",0.7,"Humid","Type W3h","Type W3h","Humid",0.5,0.5,"Yes","Yes","Yes","Yes","Yes","Yes","Humid","Humid","N/A","Suitable for heavy movable FF&E on castors ","Type L2.1e","Type L2.1e","Required","Required",0.5,0.5,0.8,0.8,0.3,0.3,500,500,750,750,165,165,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, sw, dim","Yes","300 lux as in classrooms can be used if a higher lighting level can be achieved by task lighting or dimming if required","Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1a","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.40/60","Note 1","Average","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided.  Local extract ventilation based on risk assessment when practical work involving fumes is planned   ","Yes, to gas ovens and hobs.   ","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot and cold water to all sinks listed under FF&E ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Need to be able to clean surfaces thoroughly to maintain hygiene; safe distances around cookers.","Contractor to Specify",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows"]
["DAT43 (Resistant materials ...",null,null,null,"Resistant materials workshop","DAT43","Secondary school workshop for working with resistant materials and electronics","As SoA","m2","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making with wood, plastics and some metals. Some electronics and control. Teacher demonstrations using machines and practical multibenches. Traditional and computer based drawing and design.","As SoA","As SoA",3,"Basic teaching","Zone H","Heavy practical","None",6,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB","As SoA","As SoA",2700,2700,7500,"minimum","Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.2v","Note 1","Strong, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.2v","Note 1","Strong, with vision panel",35,null,926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F3","Note 1","Heavy practical concrete, resin, rubber or vinyl","Yes for rubber or vinyl",null,"Commercial 34",null,"N/A",null,0.2,null,10,null,"R11",null,"Minimum SRV 36",null,"Yes",null,"Yes",null,"Moderate",null,"Yes",null,"Yes",null,"Yes",null,"Type C1","Note 1","General",0.7,"Normal","Type W4","Note 1","Rough",0.5,null,"N/A",null,"N/A",null,"N/A",null,"Normal",null,"N/A","Suitable for heavy movable FF&E on castors. Concrete or ceramic tiles floor required around any heat treatment equipment","Type L2.1e","Type L2.1e","Required","Required",0.5,0.5,0.8,0.8,0.3,0.3,500,500,750,750,165,165,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, sw, dim","Yes","300 lux as in classrooms can be used if a higher lighting level can be achieved by task lighting or dimming if required","Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1a","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A5.40/60","/=K188","High","High",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided.  Local extract ventilation based on risk assessment when practical work involving fumes is planned. If space is refurbished, see Note 2 in tech annexe. Ducting to specialist dust extraction unit in adjacent prep/store.   ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus sockets or 3-phase supply to suit equipment accommodated, and cleaners' SSSO at low level","Hot and cold water to all sinks listed under FF&E","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Lockable single switch disconnector for power and emergency stop system for fixed machinery; Safe distances around fixed equipment and workbenches.","Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. Ducting from all relevant equipment to dust extract unit in adjacent prep room"]
["DAT46 (RM with heat bay)",null,null,null,"RM workshop with heat bay","DAT46","Secondary school workshop for working with a range of resistant materials, including wood, metal and plastics",111,"m2","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making with wood, metals (including heat treatment) and some plastics. Some electronics and control. Teacher demonstrations using machines and practical multibenches. Traditional and computer based drawing and design.",24,27,3,"Basic teaching","Zone I","Heavy practical","None",6,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB",111,111,2700,2700,7500,"minimum","Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.2v","Note 1","Strong, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.2v","Note 1","Strong, with vision panel",35,null,926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F3","Note 1","Heavy practical concrete, resin, rubber or vinyl","Yes for rubber or vinyl",null,"Commercial 34",null,"N/A",null,0.2,null,10,null,"R11",null,"Minimum SRV 36",null,"Yes",null,"Yes",null,"Moderate",null,"Yes",null,"Yes",null,"Yes",null,"Type C1","Note 1","General",0.7,"Normal","Type W4","Note 1","Rough",0.5,null,"N/A",null,"N/A",null,"N/A",null,"Normal",null,"N/A","Suitable for heavy movable FF&E on castors. Concrete or ceramic tiles floor required around any heat treatment equipment","Type L2.1e","Type L2.1e","Required","Required",0.5,0.5,0.8,0.8,0.3,0.3,500,500,750,750,165,165,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, sw, dim","Yes","300 lux as in classrooms can be used if a higher lighting level can be achieved by task lighting or dimming if required","Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1a","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A5.40/60","/=K188","High","High",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided.  Local extract ventilation based on risk assessment when practical work involving fumes is planned. If space is refurbished, see Note 2 in tech annexe. Ducting to specialist dust extraction unit in adjacent prep/store.   ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus sockets or 3-phase supply to suit equipment accommodated, and cleaners' SSSO at low level","Hot and cold water to all sinks listed under FF&E ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Lockable single switch disconnector for power and emergency stop system for fixed machinery; Safe distances around fixed equipment and workbenches.","Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows"]
["DAT48 (Engineering workshop)",null,null,null,"Engineering workshop","DAT48","Secondary school workshop for vocational engineering courses ",97,"m2","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making with wood, metals (including heat treatment) and some plastics. Some electronics and control. Teacher demonstrations using machines and practical multibenches.",20,23,3,"Basic teaching","Zone I","Heavy practical","None",6,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB",97,96,2700,2700,7500,"minimum","Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.2v","Note 1","Strong, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.2v","Note 1","Strong, with vision panel",35,null,926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F3","Note 1","Heavy practical concrete, resin, rubber or vinyl","Yes for rubber or vinyl",null,"Commercial 34",null,"N/A",null,0.2,null,10,null,"R11",null,"Minimum SRV 36",null,"Yes",null,"Yes",null,"Moderate",null,"Yes",null,"Yes",null,"Yes",null,"Type C1","Note 1","General",0.7,"Normal","Type W4","Note 1","Rough",0.5,null,"N/A",null,"N/A",null,"N/A",null,"Normal",null,"N/A","Suitable for heavy movable FF&E on castors Concrete or ceramic tiles floor required around any heat treatment equipment","Type L2.1e","Type L2.1e","Required","Required",0.5,0.5,0.8,0.8,0.3,0.3,500,500,750,750,165,165,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, sw, dim","Yes","300 lux as in classrooms can be used if a higher lighting level can be achieved by task lighting or dimming if required","Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1a","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A5.40/60","/=K188","High","High",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided.  Local extract ventilation based on risk assessment when practical work involving fumes is planned. If space is refurbished, see Note 2 in tech annexe. Ducting to specialist dust extraction unit in adjacent prep/store.   ","Bottled gas only","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus sockets or 3-phase supply to suit equipment accommodated, and cleaners' SSSO at low level","Hot and cold water to all sinks listed under FF&E ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Lockable single switch disconnector for power and emergency stop system for fixed machinery; means to isolate and restore gas supply. Safe distances around fixed equipment and workbenches.","Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows"]
["DAT49 (Construction workshop)",null,null,null,"Construction workshop","DAT49","Secondary school workshop for vocational construction courses ",97,"m2","Construction skills including painting and decorating; plumbing and carpentry. Teacher demonstrations using machines and practical multibenches.",16,23,3,"Basic teaching","Zone J","Heavy practical","None",6,"none","As SoA","Disabled access into the space required ","Enclosed ","As SSDB",97,96,2700,2700,7500,"minimum","Required ",null,"As existing","Contractor to specify if provided","Type D1.2v","Note 1","Strong, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.2v","Note 1","Strong, with vision panel",35,null,926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F3","Note 1","Heavy practical concrete, resin, rubber or vinyl","Yes for rubber or vinyl",null,"Commercial 34",null,"N/A",null,0.2,null,10,null,"R11",null,"Minimum SRV 36",null,"Yes",null,"Yes",null,"Moderate",null,"Yes",null,"Yes",null,"Yes",null,"Type C1","Note 1","General",0.7,"Normal","Type W4","Note 1","Rough",0.5,null,"N/A",null,"N/A",null,"N/A",null,"Normal",null,"N/A","Suitable for heavy movable FF&E on castors. Concrete or ceramic tiles floor required around any heat treatment equipment","Type L2.1e","Type L2.1e","Required","Required",0.5,0.5,0.8,0.8,0.3,0.3,500,500,750,750,165,165,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, sw, dim","Yes","300 lux as in classrooms can be used if a higher lighting level can be achieved by task lighting or dimming if required","Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1a","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A5.40/60","/=K188","High","High",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided.  Local extract ventilation based on risk assessment when practical work involving fumes is planned. If space is refurbished, see Note 2 in tech annexe.   ","Bottled gas only","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus sockets or 3-phase supply to suit equipment accommodated, and cleaners' SSSO at low level","Cold, with hot and cold handwash  ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Lockable single switch disconnector for power and emergency stop system for fixed machinery; means to isolate and restore gas supply. Safe distances around fixed equipment and workbenches.","Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. Equipment shall be as provided by the school (see legacy survey), in a suitable layout which allows for the size of each piece of equipment and safe space around it."]
["DIN04 (Social space)",null,null,null,"Social space","DIN04","Specialist 'common room' for pupils to socialise, discuss and study in an informal setting","As SoA","m2","Can also be used for school events such as parents meetings/presentations, teacher consultations or whole school teacher meetings. Social area for specific group, typically sixth form pupils. Some study areas with use of ICT.","As SoA","As SoA","N/A","Halls and dining","Zone A","General","No",4,"none","As SoA","Disabled access into the space required","Enclosed, semi-enclosed or open plan","As SSDB","As SoA","As SoA",2700,2700,"CTS",null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.1v","Note 1","General, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,"Doors specified will only be applicable to enclosed social spaces","Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1","Type L1.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.45/65","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,"N/A","N/A","N/A","N/A","N/A","N/A","R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Optional for vending","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'max group size' defined in the SoAs. "]
["DIN05 (Sixth form social sp...",null,null,null,"Sixth form social space","DIN05","Specialist 'common room' for post-16 pupils to socialise, discuss and study in an informal setting","As SoA","m2","Can also be used for school events such as parents meetings/presentations, teacher consultations or whole school teacher meetings. Social area for sixth form pupils. Some study areas with use of ICT.","As SoA","As SoA","N/A","Halls and dining","Zone A","General","No",4,"none","As SoA","Disabled access into the space required","Enclosed, semi-enclosed or open plan","As SSDB","As SoA","As SoA",2700,2700,"CTS",null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.1v","Note 1","General, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,"Doors specified will only be applicable to enclosed social spaces","Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1","Type L1.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.45/65","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,"N/A","N/A","N/A","N/A","N/A","N/A","R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Optional for vending","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'max group size' defined in the SoAs. "]
["HAL01 (Main hall)",null,null,null,"Main hall (secondary)","HAL01","Multi-purpose hall for assembly, performance, PE, exams and cold dining, in secondary schools","As SoA","m2","Dining of cold food from nearby dining area. Music and drama rehearsals and performance. Parent evenings. School assemblies (various sizes) using PA system and whiteboard. Some gymnastic practise and performance, table tennis and trampolining. Whole year group examinations.","As SoA","As SoA","N/A","Halls and dining","N/A","Large and performance","Yes","6 or 7 if used for exams","adjacent store(s), control room","As SoA","Disabled access required to all areas except some seating","Enclosed","As SSDB","As SoA","As SoA",6900,4500,12000,"preferred","Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type DD2v","Note 1","Double acoustic, with vision panel",35,"  ",926,null,"825 (1500)",null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D2v","Note 1","Acoustic, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Plain meeting stiles. Main entrance doors to be at centre of side walls, between performance area and bleacher seating, where possible. Single-leaf doors to each corner of back wall behind performance space.","Type F4hw","Type F4hw","Hygienic waterproof lino, rubber, timber or vinyl","Yes for vinyl","Yes for vinyl","Commercial 34","Commercial 34","N/A","N/A",0.2,0.2,10,10,"No","No","No","No","Yes","Yes","Yes","Yes","High","High","No","No","No","No","No","No","Type C1","Note 1","General",0.7,"Normal","Type W2ns","Note 1","Dining",0.5,null,"Yes",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Suitable for movable bleacher seating to cover approximately half of the floor area, from adjacent bleacher seating store","Type L4","Type L4","Required","Preferred",0.5,"N/A",0.8,"N/A",0.6,0.6,300,300,450,450,100,100,"N/A","N/A",22,22,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","Yes","Default illuminance 300 lux, but option to switch to 500 lux for some sports (see LG5) and dimming for stage lighting required","Type T4","/=K165",21,21,"Contractor to specify (CTS)",19,19,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,16,16,"Type V2","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A7.35/60","/=K188","High","Low",null,"Contractor to specify (CTS)",null,35,40,60,65,38,35,45,40,37,37,"R08.2","R08.2","0.8 - 1.2","0.8 - 1.2","A means of increasing the air velocity during the summer shall be provided.  Ventilation rate to suit occupancy.  If space is refurbished, see Note 2 in tech annexe.   ","None","Power sockets where appropriate, separate circuits at high level for stage lighting etc., plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Fire escape should be planned based on maximum capacity being achieved when movable bleacher seating is fully extended.","Contractor to Specify where provided",null,"Add here text to be included on sign","CTS","CTS","Contractor to specify if provided for glare control. Dim-out blinds required for performances","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Drapes to provide proscenium arch at front of performance area, which should take up approximately one thrid of the floor area, opposite the bleacher seating."]
["LIB05 (Library resource cen",null,null,null,"Library resource centre","LIB05","Secondary school library and careers area",237,"m2","Individual study and research using books and ICT. Informal reading and use of reference resources. Lending books and PC resources. Whole class group for library skills.",65,"As SoA",4,"Learning resources","Zone F","Light practical","None",4,"none","As SoA","Disabled access required to all areas except some seating","Partially enclosed","As SSDB","As SoA","As SoA",2700,2700,7500,"minimum","Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.1v","Note 1","General, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F1","Type F1","General carpet, lino, rubber or vinyl","Yes","Yes","Commercial 32","Commercial 32","N/A","N/A","0.2, 0.15 if carpet","0.2, 0.15 if carpet",10,10,"No","No","No","No","No","No","Yes","Yes","Moderate","Moderate","Yes","Yes","No","No","No","No","Type C1","Note 1","General",0.7,"Normal","Type W1n","Type W1n","General",0.5,0.5,"N/A","N/A","N/A","N/A","Yes","Yes","Normal","Normal","N/A"," ","Type L1.1a","Type L1.1a","Required","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,"N/A","N/A",19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A3.40/60","Note 1","Average","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R10.1","R10.1","<=1.0","<=1.2","A means of increasing the air velocity during the summer shall be provided.     ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Specialist security barrier at all entrances and exits","Contractor to Specify",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'max group size' in the SoA. Group 3 FF&E indicative, to be agreed with school based on any legacy items."]
["LIB06 (Sixth form study are...",null,null,null,"Sixth form study area(s)","LIB06","Secondary school study area for sixth form pupils","As SoA","m2","Individual study (including use of ICT). Reading and use of reference resources. ","As SoA","As SoA","N/A","Learning resources","Zone B","Light practical","None ",4,"none","As SoA","Disabled access into the space required ","Partially enclosed","As SSDB","As SoA","As SoA",2700,2700,"CTS",null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.1v","Note 1","General, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L1.1a","Type L1.1a","Required","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,"N/A","N/A",19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A1.40/60","/=K188","Low","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'max group size' in the SoA."]
["PER01 (Music classroom)",null,null,null,"Music classroom","PER01","Secondary school music classroom for performance, composing and theory",62,"m2","Group and individual composing and music making using ICT, keyboards and percussion. Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Teacher led presentations and briefings using the whiteboard.",30,21,3,"Basic teaching","Zone D","Large and performance","None ",6,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB","As SoA","As SoA",2700,2700,"CTS",null,"Not Required ",null,"As existing","Contractor to specify if provided","Type D2v","Type D2v","Acoustic, with vision panel",35,35,926,926,825,825,2000,2000,5,5,3,3,30,30,"Yes","Yes","No","No","Yes","Yes","No","No","No","No","Standard","Standard","Yes","Yes","Yes","Yes","No","No","No","No",200,200,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1ns","Note 1","Acoustic",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"Contractor to identify"," Wall panels may be required to achieve required sound quality. ","Type L3","Type L3","Required","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,"N/A","N/A",19,19,"0.3 to 0.5","0.3 to 0.5","N/A","N/A",80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","Yes",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A8.35/55","/=K188","Very high","Low",null,"Contractor to specify (CTS)",null,35,40,55,65,38,35,45,40,37,37,"R10","R10","<=1.0","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. "]
["PER02 (Extensive music clas...",null,null,null,"Extensive music classroom","PER02","Secondary school music classroom for performance, composing and theory, with option of keyboards for all pupils",69,"m2","Group and individual composing and music making using ICT, keyboards and percussion. Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Teacher led presentations and briefings using the whiteboard.",30,24,3,"Basic teaching","Zone E","Large and performance","None",6,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB",69,69,2700,2700,"CTS",null,"Not Required ",null,"As existing","Contractor to specify if provided","Type D2v","Type D2v","Acoustic, with vision panel",35,35,926,926,825,825,2000,2000,5,5,3,3,30,30,"Yes","Yes","No","No","Yes","Yes","No","No","No","No","Standard","Standard","Yes","Yes","Yes","Yes","No","No","No","No",200,200,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1ns","Note 1","Acoustic",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"Contractor to identify","Wall panels may be required to achieve required sound quality. ","Type L3","Type L3","Required","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,"N/A","N/A",19,19,"0.3 to 0.5","0.3 to 0.5","N/A","N/A",80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","Yes",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A8.35/55","/=K188","Very high","Low",null,"Contractor to specify (CTS)",null,35,40,55,65,38,35,45,40,37,37,"R10","R10","<=1.0","<=1.0","A means of increasing the air velocity during the summer shall be provided.  If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. "]
["PER04 (Music recital and dr...",null,null,null,"Music recital/ drama studio","PER04","Studio space for drama and large music recital room combined",83,"m2","Group and individual composing and music making using ICT, keyboards and percussion. Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Pupil led performances to class. Teacher led presentations and briefings using the whiteboard.",30,27,3,"Basic teaching","Zone F","Large and performance","None ",6,"Hall if drama studio used as green room","As SoA","Disabled access into the space required","Enclosed","As SSDB",83,83,4500,4000,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D2v","Type D2v","Acoustic, with vision panel",35,35,926,926,825,825,2000,2000,5,5,3,3,30,30,"Yes","Yes","No","No","Yes","Yes","No","No","No","No","Standard","Standard","Yes","Yes","Yes","Yes","No","No","No","No",200,200,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F4","Note 1","Hall lino, rubber, timber, composition or vinyl","Yes for vinyl",null,"Commercial 34",null,"N/A",null,0.2,null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"No",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1ns","Note 1","Acoustic",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"Contractor to identify"," Wall panels may be required to achieve required sound quality.","Type L3","Type L3","Required","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,"N/A","N/A",19,19,"0.3 to 0.5","0.3 to 0.5","N/A","N/A",80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","Yes","options for lighting grid for stage lighting","Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A8.35/55","/=K188","Very high","Low",null,"Contractor to specify (CTS)",null,35,40,55,65,38,35,45,40,37,37,"R10.3","R10.3","<=1.0","<=1.5","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, on 2 walls where appropriate, plus sockets to suit school's lighting systems and cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows."]
["PER05 (Drama studio)",null,null,null,"Drama studio","PER05","Studio space for drama ",90,"m2","Drama workshops. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Pupil led rehearsals and performance to a small audience. Teacher led presentations and briefings occasionally with whiteboard.",30,27,3,"Basic teaching","Zone F","Large and performance","Yes ","6 or 7 if used for exams","Hall if drama studio used as green room","As SoA","Disabled access into the space required","Enclosed","As SSDB",90,83,4500,4000,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D2v","Type D2v","Acoustic, with vision panel",35,35,926,926,825,825,2000,2000,5,5,3,3,30,30,"Yes","Yes","No","No","Yes","Yes","No","No","No","No","Standard","Standard","Yes","Yes","Yes","Yes","No","No","No","No",200,200,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F4","Note 1","Hall lino, rubber, timber, composition or vinyl","Yes for vinyl",null,"Commercial 34",null,"N/A",null,0.2,null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"No",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1ns","Note 1","Acoustic",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"Contractor to identify","Wall panels may be required to achieve required sound quality.","Type L3","Type L3","Required","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,"N/A","N/A",19,19,"0.3 to 0.5","0.3 to 0.5","N/A","N/A",80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","Yes","options for lighting grid for stage lighting","Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A7.35/60","/=K188","High","Low",null,"Contractor to specify (CTS)",null,35,40,60,65,38,35,45,40,37,37,"R10.3","R10.3","<=1.0","<=1.5","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.   ","None","Power sockets as FOS, on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows."]
["RES12 (Music practice and g...",null,null,null,"Music practice/ group room","RES12","Room for music practice/ lessons",8,"m2","Individual music lessons. Individuals/small groups composing and practising music using a variety of percussion instruments and electronic keyboard.",3,"N/A",1,"Learning resources","Zone B","Large and performance","None ",4,"none","As SoA","Disabled access into the space preferred","Enclosed","As SSDB",8,7,2400,2400,"CTS",null,"Not Required ",null,"As existing","Contractor to specify if provided","Type D2v","Type D2v","Acoustic, with vision panel",35,35,926,926,825,825,2000,2000,5,5,3,3,30,30,"Yes","Yes","No","No","Yes","Yes","No","No","No","No","Standard","Standard","Yes","Yes","Yes","Yes","No","No","No","No",200,200,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Angled wall panels may be required to achieve required sound quality. ","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A8.35/55","/=K188","Very high","Low",null,"Contractor to specify (CTS)",null,35,40,55,65,38,35,45,40,37,37,"R06.1","R06.1","<=0.6","<=0.8","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Group 3 FF&E indicative. Likely to contain full drum kit if extensive group room"]
["RES13 (Extensive music prac)",null,null,null,"Extensive music practice room","RES13","Room for music practice/ lesson, including drums",16,"m2","Individual music lessons. Individual/small groups composing and practising music using a variety of percussion instruments, full drum kit and electronic keyboard.",7,"N/A",1,"Learning resources","Zone C","Large and performance","None ",4,"none","As SoA","Disabled access into the space preferred","Enclosed","As SSDB",16,15,2400,2400,"CTS",null,"Not Required ",null,"As existing","Contractor to specify if provided","Type D2v","Type D2v","Acoustic, with vision panel",35,35,926,926,825,825,2000,2000,5,5,3,3,30,30,"Yes","Yes","No","No","Yes","Yes","No","No","No","No","Standard","Standard","Yes","Yes","Yes","Yes","No","No","No","No",200,200,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Angled wall panels may be required to achieve required sound quality. ","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A8.35/55","/=K188","Very high","Low",null,"Contractor to specify (CTS)",null,35,40,55,65,38,35,45,40,37,37,"R06.1","R06.1","<=0.6","<=0.8","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Group 3 FF&E indicative. Likely to contain full drum kit if extensive group room"]
["RES14 (Control room for rec...",null,null,null,"Control room for recording","RES14","Room housing specialist recording equipment",8,"m2","Using analogue or digital equipment to record music played in adjacent space(s) and to create/edit digital music.",3,"N/A",1,"Learning resources","Zone B","Large and performance","None ",5,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB, directly adjacent to large music group room",8,7,2400,2400,"CTS",null,"Not Required ",null,"As existing","Contractor to specify if provided","Type D2v","Note 1","Acoustic, with vision panel",35,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D2v","Note 1","Acoustic, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,"glazed viewing screens to adjacent music spaces","Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1ns","Note 1","Acoustic",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"Contractor to identify","Angled wall panels and sound-absorbing panels may be required to achieve required sound quality. ","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A8.35/55","/=K188","Very high","Low",null,"Contractor to specify (CTS)",null,35,40,55,65,38,35,45,40,37,37,"R05","R05","<=0.5","<=0.5","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, within dado trunking on 2 walls to suit school's audio, visual and control equipment, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["RES16 (Lighting and audio c...",null,null,null,"Lighting/ audio control room","RES16","Room for controlling lighting and audio systems in adjacent performance space",6,"m2"," Using analogue or digital equipment to control stage lighting and sound system in adjacent hall.",2,"N/A",1,"Learning resources","Zone B","Light practical","None ",4,"none","As SoA","Disabled access into the space preferred ","Enclosed ","As SSDB",6,6,2400,2400,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D2","Note 1","Acoustic, with vision panel",35,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"No",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D2","Note 1","Acoustic, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"No",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F1","Note 1","General carpet, lino, rubber or vinyl","Yes",null,"Commercial 32",null,"N/A",null,"0.2, 0.15 if carpet",null,10,null,"No",null,"No",null,"No",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," Dark coloured wall finishes","Type L8","Type L8","None","None","N/A","N/A","N/A","N/A","N/A","N/A",100,100,150,150,"N/A","N/A","N/A","N/A",25,25,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","sw","Yes",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A1.40/60","/=K188","Low","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided. If space is refurbished, see Note 2 in tech annexe.     ","None","Power sockets as FOS, within dado trunking on 2 walls to suit school's audio, visual and control equipment, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["RES21 (Kiln room)",null,null,null,"Kiln room","RES21","Room for kiln(s) and drying racks",4,"m2","Firing and glazing articles in kiln(s). Storing clay articles awaiting firing."," N/A ","N/A","N/A","Learning resources","N/A","Light practical","None ",5,"none","As SoA","Disabled access not required, trolley access required ","Enclosed ","As SSDB, off 3D art room",4,4,2400,2100,1350,"minimum","Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D7","Note 1","Fire-resistant, no vision panel",0,"  ",926,null,825,null,2000,null,3,null,4,null,60,null,"Yes",null,"No",null,"No",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F3","Type F3","Heavy practical concrete, resin, rubber or vinyl","Yes for rubber or vinyl","Yes for rubber or vinyl","Commercial 34","Commercial 34","N/A","N/A",0.2,0.2,10,10,"R11","R11","Minimum SRV 36","Minimum SRV 36","Yes","Yes","Yes","Yes","Moderate","Moderate","Yes","Yes","Yes","Yes","Yes","Yes","Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Suitable for heavy movable FF&E on castors ","Type L7.3","Type L7.3","Not required","Not required","N/A","N/A","N/A","N/A",0.3,0.3,200,200,300,300,"N/A","N/A","N/A","N/A",25,25,"N/A","N/A",0.4,0.4,60,60,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","sw","No",null,"Type T9","/=K165",5,5,"Contractor to specify (CTS)","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","Type V3b","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,2,null,"N/A","/=K188",null,null,null,"Contractor to specify (CTS)",null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A",null,null,"Extract required for specialist equipment to satisfy manufacturer's requirements. Sufficient space around back of kiln to allow for air movement and servicing. If space is refurbished, see Note 2 in tech annexe.","No, unless legacy kiln is gas fired.  ","Power to suit kiln provided","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Warning light to indicate firing required; should not be possible to open kiln door during firing.","Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["RES22 (Dark room)",null,null,null,"Dark room","RES22","Specialist dark room for photograph developing","As SoA","m2","Processing and developing photographs using tradtional techniques.","As SoA","As SoA",1,"Learning resources","Zone B","Light practical","None ",4,"none","As SoA","Disabled access into the space preferred ","Enclosed ","As SSDB","As SoA","As SoA",2400,2200,2400,null,"Not Required unless for fire. CTS if provided ",null,"N/A","Contractor to specify if provided","Type D7","Note 1","Fire-resistant, no vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"No",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"All-round light-tight seals on door required in normal operation, to ensure no light leakage. Ironmongery to include internal escape mechanism","Type F2sc","/=K101","Chemical resistant light practical non-slip lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","N/A","N/A","Yes","Yes","Yes","Yes","Moderate","Moderate","Yes","Yes","Yes","Yes","No","No","Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Suitable for heavy movable FF&E on castors. Dark coloured wall finishes","Type L8","Type L8","None","None","N/A","N/A","N/A","N/A","N/A","N/A",100,100,150,150,"N/A","N/A","N/A","N/A",25,25,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","sw","Yes","Separately-switched photographic safe light(s) in room and indicator light on outside required","Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V3b","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,2,null,"A1.45/65","A1.45/65","Low","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,33,30,40,35,32,32,"R10","R10","<=1.0","<=1.0","Ventilation can be variable but must be able to extract at 5ach when required.  If space is refurbished, see Note 2 in tech annexe.","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot and cold water to sink listed under FF&E, in mixer tap.  Chemical resistant waste pipework","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Chemicals kept in locked cupboards","Contractor to Specify where provided","Sign to say 'Do not enter when red light is on'","Add here text to be included on sign","CTS","CTS","100% blackout blinds required if window provided","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["SCI02 (Science studio)",null,null,null,"Science studio","SCI02","Secondary school science room for demonstration and light experiments",69,"m2","Group discussion. Independent research and recording. Presentations. Simple supervised experiments and evaluation exercises. Teacher demonstration of experiments. Using the whiteboard.",30,24,3,"Basic teaching","Zone E","Light practical","None",5,"none","As SoA","Disabled access into the space required ","Enclosed","As SSDB",69,69,2700,2700,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.1v","Note 1","General, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F2sc","Type F2sc","Chemical resistant light practical non-slip lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","N/A","N/A","Yes","Yes","Yes","Yes","Moderate","Moderate","Yes","Yes","Yes","Yes","No","No","Type C1","Note 1","General",0.7,"Normal","Type W2n","Note 1","Science",0.5,null,"Yes",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Suitable for heavy movable FF&E on castors ","Type L2.1","Type L2.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,500,500,750,750,165,165,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No","300 lux as in classrooms can be used if a higher lighting level can be achieved by task lighting or dimming if required","Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1b","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,1.3,null,"N/A",null,"A3.35/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,35,40,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided.  Local extract ventilation to provide 5ach during science experiments involving fumes. If space is refurbished, see Note 2 in tech annexe.   ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Cold water to wet serviced bollards or similar listed under FF&E, hot and cold to belfast sink","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Means to isolate gas supply and isolate power. Alternative exit in emergency (e.g. to adjacent room).","Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control. 1 in every 3 science teaching spaces to have black-out blinds","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","All FF&E in this space to be provided by the Contractor. Some FF&E proportional to the 'max group size' defined in the SoAs. White board to be perpendicular to windows. Space for whole group to gather round demonstration desk should be allowed."]
["SCI05 (General science labo",null,null,null,"General science laboratory","SCI05","Secondary school science laboratory for demonstration and a wide range of  'hands on' experiments",83,"m2","Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of experiments. Using the whiteboard. Whole class presentations. Wide range of supervised experiments using gas, power and water.",30,30,3,"Basic teaching","Zone F","Light practical","None",6,"none","As SoA","Disabled access into the space required ","Enclosed ","As SSDB",83,83,2700,2700,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.1v","Note 1","General, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F2sc","Type F2sc","Chemical resistant light practical non-slip lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","N/A","N/A","Yes","Yes","Yes","Yes","Moderate","Moderate","Yes","Yes","Yes","Yes","No","No","Type C1","Note 1","General",0.7,"Normal","Type W2n","Type W2n","Science",0.5,0.5,"Yes","Yes","N/A","N/A","Yes","Yes","Normal","Normal","N/A","Suitable for heavy movable FF&E on castors ","Type L2.1","Type L2.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,500,500,750,750,165,165,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No","300 lux as in classrooms can be used if a higher lighting level can be achieved by task lighting or dimming if required","Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1b","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,1.3,null,"N/A",null,"A3.40/60","Note 1","Average","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided.  Local extract ventilation to provide 5ach during science experiments involving fumes.   ","4 double gas taps to all bollards listed on FF&E list and to side benching, or similar","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Cold water to wet serviced bollards or similar listed under FF&E, hot and cold to belfast sink","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Means to isolate gas supply and isolate power. Alternative exit in emergency (e.g. to adjacent room).","Contractor to Specify",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided. 1 in every 3 science teaching space to have black-out blinds","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","All FF&E in this space to be provided by the Contractor. Some FF&E proportional to the 'max group size' defined in the SoAs. White board to be perpendicular to windows. Space for whole group to gather round demonstration desk should be allowed."]
["SCI11 (Specialist sci lab)",null,null,null,"Specialist science laboratory","SCI11","Secondary school science laboratory for demonstration for all types of experiments, up to A-level ",90,"m2","Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of experiments. Using the whiteboard. Whole class presentations. Wide range of supervised experiments using gas, power and water.",30,"As SoA",3,"Basic teaching","Zone F","Light practical","None",6,"none","As SoA","Disabled access into the space required","Enclosed","As SSDB",90,90,2700,2700,"CTS",null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.1v","Note 1","General, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F2sc","Type F2sc","Chemical resistant light practical non-slip lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","N/A","N/A","Yes","Yes","Yes","Yes","Moderate","Moderate","Yes","Yes","Yes","Yes","No","No","Type C1","Note 1","General",0.7,"Normal","Type W2n","Type W2n","Science",0.5,0.5,"Yes","Yes","N/A","N/A","Yes","Yes","Normal","Normal","N/A","Suitable for heavy movable FF&E on castors ","Type L2.1","Type L2.1","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,500,500,750,750,165,165,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw, dim","No","300 lux as in classrooms can be used if a higher lighting level can be achieved by task lighting or dimming if required","Type T5","Type T5",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1b","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,1.3,null,"N/A",null,"A3.40/60","Note 1","Average","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R08.1","R08.1","<=0.8","<=1.0","A means of increasing the air velocity during the summer shall be provided.  Local extract ventilation to provide 5ach during science experiments involving fumes.   ","4 double gas taps to all bollards listed on FF&E list and to side benching, or similar","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Cold with swan neck at demo desk, side benching and service bollards, with hot and cold handwash","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Means to isolate gas supply and isolate power. Alternative exit in emergency (e.g. to adjacent room).","Contractor to Specify",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided. 1 in every 3 science teaching space to have black-out blinds","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","All FF&E in this space to be provided by the Contractor. Some FF&E proportional to the 'max group size' defined in the SoAs. White board to be perpendicular to windows. Space for whole group to gather round demonstration desk should be allowed."]
["SPH00 (school sports hall)",null,null,null,"School sports hall","SPH00","Sports hall for secondary school PE activities, exams and some recreational community use, using Sport England dimensions","As SoA","m2","Individual activities including Athletics (practice only) and gymnastics. Team games includng badminton; basketball; Five-A-Side football / futsal; indoor cricket; indoor tennis; judo; karate; korfball; mini handball; netball (practice only); short tennis; table tennis and volleyball.","As SoA","As SoA",6,"Halls and dining","N/A","Large and performance","Yes","6 or 7 if used for exams","none","As SoA","Disabled access into the space required","Enclosed","As SSDB","As SoA","As SoA",7500,7500,18000,null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type DD3v","Note 1","Sports hall, with vison panels",30,"  ",926,null,"875 (1200)",null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes, with safety glass",null,"No",null,"No",null,"Standard",null,"Yes",null,"No",null,"Pull face",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Plain meeting stiles. Must open out from hall space. All surfaces must be flush with no projecting frames or ironmongery","Type F6","Note 1","Sports hall floor","Yes for vinyl",null,"N/A",null,"P3",null,0.2,null,10,null,"Yes",null,"N/A",null,"Yes",null,"Yes",null,"Moderate",null,"No",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W3n","Note 1","Jointless",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Floor markings to be suitable for sports to be accommodated. Floor sockets to suit the sports hall floor. Division netting complete with roller hooks, telescopic roof and wall fixed support brackets and one wall fixed PVC storage pouch. Where dimensions allow Handball and Hockey: wall anchors to secure one pair of Handball goals, one pair of wall anchors to secure one pair of Hockey goals (may be able to re-use the anchors for five-a-side). For Indoor hockey the playing area is defined by the walls and/or perimeter boards used as rebound surfaces. Boards must be provided for this purpose to ensure a continuous perimeter to the playing area. Interlocking hockey side boards for use in sports halls with sloping face to keep hockey ball in play. One pair of wall anchors to secure one pair of five a side goals. ","Type L4","Type L4","Required","Preferred",0.5,"N/A",0.8,"N/A",0.6,0.6,300,300,450,450,100,100,"N/A","N/A",22,22,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","Yes","Default illuminance 300 lux, but option to switch to 500 lux for some sports useful, see LG5","Type T6","/=K165",17,17,"Contractor to specify (CTS)",15,15,23,23,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,12,12,"Type V2a","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A7.35/60","/=K188","High","Low",null,"Contractor to specify (CTS)",null,35,40,60,65,38,35,45,40,37,37,"R20","R20","<=2.0","<=2.0","A means of increasing the air velocity during the summer shall be provided.  Ventilation rate to suit occupancy. Maximum air velocity for badminton to be achievable when badminton is played. If space is refurbished, see Note 2 in tech annexe.   ","None","Power sockets as FOS, at low level on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","No projections, including opening doors, to avoid injury during activity.","Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Group 2 FF&E to be provided as shown. Group 3 FF&E listed indicative, and will vary depending on sports hall size and legacy items."]
["SPH20 (Community sports hall)",null,null,null,"Community sports hall","SPH20","Sports hall for secondary school PE activities and formal community use, using Sport England dimensions","As SoA","m2","2 net bays (36m wide). Badminton 4 courts. Basketball 1 court. Five-A-Side Football / Futsal 1 court. Indoor Cricket. Indoor Tennis. Judo. Karate. Korfball 1 court practice only. Mini Handball 1 court. Netball practice only. Short Tennis. Sports hall athletics practice only . Volleyball 1 court. Gymnastics. Table tennis.","As SoA","As SoA",6,"Halls and dining","N/A","Large and performance","Yes","6 or 7 if used for exams","none","As SoA","Disabled access into the space required","Enclosed","As SSDB","As SoA","As SoA",7500,7500,20000,null,"Optional. CTS if provided ",null,"As existing","Contractor to specify if provided","Type DD3v","Note 1","Sports hall, with vison panels",30,"  ",926,null,"875 (1200)",null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes, with safety glass",null,"No",null,"No",null,"Standard",null,"Yes",null,"No",null,"Pull face",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Plain meeting stiles. Must open out from hall space. All surfaces must be flush with no projecting frames or ironmongery","Type F6","Note 1","Sports hall floor","Yes for vinyl",null,"N/A",null,"P3",null,0.2,null,10,null,"Yes",null,"N/A",null,"Yes",null,"Yes",null,"Moderate",null,"No",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W3n","Note 1","Jointless",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Floor markings to be suitable for sports to be accommodated ","Type L4","Type L4","Required","Preferred",0.5,"N/A",0.8,"N/A",0.6,0.6,300,300,450,450,100,100,"N/A","N/A",22,22,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","Yes","Default illuminance 300 lux, but option to switch to 500 lux for some sports useful, see LG5","Type T6","/=K165",17,17,"Contractor to specify (CTS)",15,15,23,23,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,12,12,"Type V2a","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"A7.35/60","/=K188","High","Low",null,"Contractor to specify (CTS)",null,35,40,60,65,38,35,45,40,37,37,"R20","R20","<=2.0","<=2.0","A means of increasing the air velocity during the summer shall be provided.  Ventilation rate to suit occupancy. Maximum air velocity for badminton to be achievable when badminton is played. If space is refurbished, see Note 2 in tech annexe.   ","None","Power sockets as FOS, at low level on 2 walls where appropriate, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","No projections, including opening doors, to avoid injury during activity.","Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","White board to be perpendicular to windows. FF&E to be agreed with school"]
["STH20 (Bleacher seating)",null,null,null,"Bleacher seating storage","STH20","Storage area for retractable bleacher seating used in hall","As SoA","m2","Storage for retractable bleacher seating in an adjacent hall. Space required when bleacher seating is fully retracted"," N/A ","N/A"," N/A ","Storage (non-teaching)","N/A","General","Optional",3,"main hall","As SoA","N/A","semi-enclosed","As SSDB, directly off main hall","As SoA","As SoA","N/A","N/A","N/A","minimum","None ",null,"N/A","Contractor to specify if provided","N/A","N/A","No internal door required",null,"  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Dimensions to suit furniture to be stored","Type F4hw","Type F4hw","Hygienic waterproof lino, rubber, timber or vinyl","Yes for vinyl","Yes for vinyl","Commercial 34","Commercial 34","N/A","N/A",0.2,0.2,10,10,"No","No","No","No","Yes","Yes","Yes","Yes","High","High","No","No","No","No","No","No","Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","floor finish to match adjacent hall where required","N/A","N/A","Not required","Not required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No",null,"Type T9","/=K165",5,5,"Contractor to specify (CTS)","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","Type V2b","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"N/A","/=K188",null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A",null,null,null,"None","None","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","appropriate barriers to edge","Contractor to Specify where provided",null,"N/A","N/A","CTS","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Dimensions of store to suit dimensions of bleacher seating provided. Tiers to provide appropriately designed layout of bleacher seating to approximately half of the area of the adjacent main hall, providing, with additional chairs, seating for assembly to the number in the SoA for the main hall."]
["STT08 (Drama store (off room))",null,null,null,"Drama store (off room)","STT08","Store room for drama teaching resources and costumes",10,"m2","Storing drama teaching resources including costumes, props and some flats."," N/A ","N/A"," N/A ","Storage (teaching)","N/A","General","None",3,"adjacent teaching space","As SoA","Full disabled access not required","Enclosed","As SSDB",10,9,2200,2100,"CTS",null,"Not Required ",null,"N/A","Contractor to specify if provided","Type D6","Note 1","Store room",0,"  ",926,null,825,null,2000,null,3,null,3,null,30,null,"Yes",null,"No",null,"No",null,"No",null,"No",null,"Standard",null,"Yes",null,"No",null,"Pull face",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F2","Note 1","Light practical lino, resin, rubber or vinyl","Yes",null,"Commercial 33",null,"N/A",null,0.2,null,10,null,"N/A",null,"N/A",null,"Yes",null,"Yes",null,"Moderate",null,"Yes",null,"No",null,"No",null,"Type C1","Note 1","General",0.7,"Normal","Type W1n","Note 1","General",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A"," ","Type L7.3","Type L7.3","Not required","Not required","N/A","N/A","N/A","N/A",0.3,"N/A",200,200,300,300,"N/A","N/A","N/A","N/A",25,25,"N/A","N/A",0.4,0.4,60,60,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","sw","No",null,"Type T9","/=K165",5,5,"Contractor to specify (CTS)","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","Type V2b","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"N/A","/=K188",null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A",null,null,"     ","None","None","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Fire Containment.","Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["STT21 (Science prep room)",null,null,null,"Science prep room","STT21","Technician's preparation/ store room for all labs or studios in suite","As SoA","m2","Administrative tasks requiring ICT. Preparation of materials for practical activities. Stocktaking. Storing and cleaning equipment."," N/A ","N/A","As SoA","Storage (teaching)","N/A","Light practical","None",4,"all science laboratories and studios served by prep room","As SoA","Disabled and trolley access into the space required","Enclosed","As SSDB","As SoA","As SoA",2700,2700,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"As existing","Contractor to specify if provided","Type D1.1v","Note 1","General, with vision panel",30,"  ",926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D1.1v","Note 1","General, with vision panel",35,null,926,null,825,null,2000,null,5,null,3,null,30,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F2sc","Type F2sc","Chemical resistant light practical non-slip lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","N/A","N/A","Yes","Yes","Yes","Yes","Moderate","Moderate","Yes","Yes","Yes","Yes","No","No","Type C1","Note 1","General",0.7,"Normal","Type W2n","Note 1","Science",0.5,null,"Yes",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Suitable for heavy movable FF&E on castors ","Type L2.1e","Type L2.1e","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,500,500,750,750,165,165,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, sw, dim","Yes","300 lux as in classrooms can be used if a higher lighting level can be achieved by task lighting or dimming if required","Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V4","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,5,null,"A1.45/65","/=K188","Low","Medium",null,"Contractor to specify (CTS)",null,45,45,65,65,33,30,40,35,32,32,"R10","R10","<=1.0","<=1.0","A means of increasing the air velocity during the summer shall be provided.  Ventilation can be variable but must be able to extract at 5ach when required. If space is refurbished, see Note 2 in tech annexe.   ","Gas taps at preparation benching, minimum total one gas taps per technician","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Cold with swan neck taps at side benching plus hot and cold handwash   ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Fire Containment. Gas cylinders to be safely clamped. Radioactive cupboard should be fixed to a wall or bench 2m away from occpied areas","Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Some FF&E proportional to the 'Average Area of Space', required in the SoA."]
["STT23 (Chemical store)",null,null,null,"Chemical store","STT23","Chemical store asociated with science prep room",7,"m2","Storing chemicals, some hazardous. Not including radioactive materials, which should be stored separately. "," N/A ","N/A","N/A","Storage (teaching)","N/A","Light practical","None",4,"all science laboratories and studios","As SoA","Disabled access not required","Enclosed","As SSDB",7,7,2400,2400,"CTS",null,"Not Required ",null,"As existing","Contractor to specify if provided","Type D8h","Note 1","Fire-resistant cpd or plant, humid",0,"  ",926,null,825,null,2000,null,3,null,4,null,60,null,"Yes",null,"Yes",null,"No",null,"Yes",null,"No",null,"Standard",null,"Yes",null,"No",null,"Pull face",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Door should open outwards and be unlockable from  inside the room.","Type F2c","Type F2c","Chemical resistant lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"N/A","N/A","N/A","N/A","Yes","Yes","Yes","Yes","Moderate","Moderate","Yes","Yes","Yes","Yes","No","No","Type C1","Note 1","General",0.7,"Normal","Type W3n","Note 1","Jointless",0.5,null,"N/A",null,"N/A",null,"Yes",null,"Normal",null,"N/A","Suitable for heavy movable FF&E on castors. Floor should be bunded and impervious to chemicals. ","Type L7.3","Type L7.3","Not required","Not required","N/A","N/A","N/A","N/A",0.3,"N/A",200,200,300,300,"N/A","N/A","N/A","N/A",25,25,"N/A","N/A",0.4,0.4,60,60,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","sw","No",null,"Type T9","/=K165",5,5,"Contractor to specify (CTS)","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","Type V5","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,2,null,"N/A","/=K188",null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A",null,null,"Minimum temperature in chemical stores is 10oC. If space is refurbished, see Note 2 in tech annexe.  ","None","None","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Fire Containment. Staff only access, need to be able to open door from inside in emergency. Need fire resistant cupboard for highly flammable liquids within store and ideally separate store for most hazardous chemicals.","Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["STT32 (Multi-materials stor...",null,null,null,"Multi-materials store/ prep room","STT32","Technician's preparation/store room for all resistant materials rooms","As SoA","m2","Maintaining tools and equipment. Some administrative work requiring ICT. Storing and preparing resistant materials (wood, metal, plastics) and components for pupils' use.",2,"N/A",1,"Storage (teaching)","N/A","Heavy practical","None ",4,"all product design workshops","As SoA","Disabled access into the space required","Enclosed","As SSDB, off one workshop","As SoA","As SoA",2700,2700,4350,"minimum","Double doors for deliveries required ",null,"N/A","Contractor to specify if provided","Type D7v","Note 1","Fire-resistant, with vision panel",0,"  ",926,null,825,null,2000,null,3,null,4,null,60,null,"Yes",null,"No",null,"Yes",null,"No",null,"No",null,"No",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D7v","Note 1","Fire-resistant, with vision panel",0,null,926,null,825,null,2000,null,3,null,4,null,60,null,"Yes",null,"No",null,"Yes",null,"No",null,"  No ",null,"No",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F3","Note 1","Heavy practical concrete, resin, rubber or vinyl","Yes for rubber or vinyl",null,"Commercial 34",null,"N/A",null,0.2,null,10,null,"R11",null,"Minimum SRV 36",null,"Yes",null,"Yes",null,"Moderate",null,"Yes",null,"Yes",null,"Yes",null,"Type C1","Note 1","General",0.7,"Normal","Type W4","Note 1","Rough",0.5,null,"N/A",null,"N/A",null,"N/A",null,"Normal",null,"N/A","Suitable for heavy movable FF&E on castors ","Type L2.1e","Type L2.1e","Required","Required",0.5,"N/A",0.8,"N/A",0.3,0.3,500,500,750,750,165,165,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, sw, dim","Yes","300 lux as in classrooms can be used if a higher lighting level can be achieved by task lighting or dimming if required","Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V6","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"A5.40/60","/=K188","High","High",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"R10","R10","<=1.0","<=1.0","A means of increasing the air velocity during the  summer shall be provided. Specialist dust extraction to serve adjacent workshops. If space is refurbished, see Note 2 in tech annexe.   ","None","Power sockets and 3-phase supply to suit equipment accommodated, plus cleaners' SSSO at low level","Cold, with hot and cold handwash  ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Fire Containment. No access to pupils.","Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","Dust extraction unit connected to ducting to equipment in adjacent workshop(s)"]
["STT34 (Food store and prep ...",null,null,null,"Food store/ prep room","STT34","Technician's preparation/store room for all food rooms",10,"m2","Laundry of food room linen. Preparing food ingredients for lessons. Storing cooking equipment and ingredients.",2,"N/A",0,"Storage (teaching)","N/A","General","None ",4,"all food rooms and food studios","As SoA","Disabled access into the space required","Enclosed","As SSDB, off food room",10,9,2400,2400,1800,"minimum","Delivery entrance optional ",null,"N/A","Contractor to specify if provided","Type D7vh","Note 1","Fire-resistant, with vision panel, humid",0,"  ",926,null,825,null,2000,null,3,null,4,null,60,null,"Yes",null,"Yes",null,"Yes",null,"No",null,"No",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"No",null,200,null,"Type D7vh","Note 1","Fire-resistant, with vision panel, humid",0,null,926,null,825,null,2000,null,3,null,4,null,60,null,"Yes",null,"Yes",null,"Yes",null,"No",null,"  No ",null,"Standard",null,"Yes",null,"Yes",null,"No",null,"  No ",null,200,null,null,"Type F2sh","Type F2sh","Light practical hygienic lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","N/A","N/A","Yes","Yes","Yes","Yes","High","High","Yes","Yes","No","No","No","No","Type C1","Note 1","General",0.7,"Normal","Type W2h","Type W2h","Humid areas and toilets",0.5,0.5,"Yes","Yes","N/A","N/A","Yes","Yes","Humid","Humid","N/A","Suitable for heavy movable FF&E on castors ","Type L1.1b","Type L1.1b","Preferred","Preferred",0.5,"N/A",0.8,"N/A",0.3,0.3,300,300,450,450,100,100,150,150,19,19,"0.3 to 0.5","0.3 to 0.5",0.6,0.6,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","d, occ, sw","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V6","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"A3.40/60","/=K188","Average","Medium",null,"Contractor to specify (CTS)",null,40,45,60,65,33,30,40,35,32,32,"N/A","N/A",null,null,"A means of increasing the air velocity during the  summer shall be provided. If space is refurbished, see Note 2 in tech annexe.   ","None","Power sockets as FOS, within dado trunking on 2 walls where appropriate, plus cleaners' SSSO at low level","Hot and cold drinking water to sink, with hot and cold to handwash basin, dishwasher and washing machine.","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Fire Containment.","Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["STT35 (Food store (off food...",null,null,null,"Food store","STT35","Store room for food teaching resources including dry food",5,"m2","Storing dry food and cooking equipment."," N/A ","N/A","N/A","Storage (teaching)","N/A","N/A","None",3,"Adjacent food room","As SoA","Disabled access not required","Enclosed","As SSDB, off food room",5,5,2400,2200,"CTS",null,"Not Required unless for fire. CTS if provided ",null,"N/A","Contractor to specify if provided","Type D6h","Note 1","Store room in humid areas",0,"  ",926,null,825,null,2000,null,3,null,3,null,30,null,"Yes",null,"Yes",null,"No",null,"No",null,"No",null,"Standard",null,"Yes",null,"No",null,"Pull face",null,"No",null,200,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F2sh","Type F2sh","Light practical hygienic lino, resin, rubber or vinyl","Yes","Yes","Commercial 33","Commercial 33","N/A","N/A",0.2,0.2,10,10,"R10","R10","N/A","N/A","Yes","Yes","Yes","Yes","High","High","Yes","Yes","No","No","No","No","Type C2","Note 1","Humid",0.7,"Humid","Type W3h","Type W3h","Humid",0.5,0.5,"Yes","Yes","Yes","Yes","Yes","Yes","Humid","Humid","N/A","Suitable for heavy movable FF&E on castors ","Type L7.2c","Type L7.2c","Not required","Not required","N/A","N/A","N/A","N/A","N/A","N/A",100,100,150,150,"N/A","N/A","N/A","N/A",24,24,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No",null,"Type T5","/=K165",20,20,"Contractor to specify (CTS)",18,18,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,15,15,"Type V1a","Note 1",1000,null,1500,null,1500,null,2000,null,"N/A",null,0.3,null,"N/A",null,"N/A","/=K188",null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,"N/A","N/A",null,null,"A means of increasing the air velocity during the summer shall be provided.  If space is refurbished, see Note 2 in tech annexe.   ","None","Power sockets as PSBP ICT small power and data schedule, plus cleaners' SSSO at low level","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS","Fire Containment.","Contractor to Specify where provided",null,"Add here text to be included on sign","Contractor to specify particular appliances where appropriate","CTS","None","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["TOC01 (Pupil changing and s",null,null,null,"Pupil changing and showers","TOC01","Wet changing and shower cubicles for male or female pupils","As SoA","m2","Changing and showering for PE.","As SoA","N/A","N/A","Non-net","N/A","Non-net","Yes",3,"all indoor and outdoor sports facilities ","As SoA","Disabled access not required unless accessible changing to be part of the facility.","Enclosed","As SSDB","As SoA","As SoA",2700,2400,"CTS",null,"Required ",null,"As existing","Contractor to specify if provided","Type D4.1","Note 1","Suitable for wet areas",30,"  ",926,null,825,null,2000,null,8,null,3,null,30,null,"Yes",null,"Yes",null,"No",null,"No",null,"No",null,"Standard",null,"Deadlock only",null,"No",null,"Pull face",null,"No",null,200,null,"N/A","Note 1","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,"Type F7","Type F7","Wet area ceramic, resin, rubber or vinyl","Yes for vinyl","Yes for vinyl","Commercial 34","Commercial 34","N/A","N/A",0.2,0.2,10,10,"Yes, see note","Yes, see note","Minimum SRV 36","Minimum SRV 36","Yes","Yes","Yes","Yes","High","High","No","No","Yes","Yes","No","No","Type C2","Note 1","Humid",0.7,"Humid","Type W2h","Type W2h","Humid areas and toilets",0.5,0.5,"Yes","Yes","N/A","N/A","Yes","Yes","Humid","Humid","N/A","Barefoot areas shall be barefoot slip resistance category B Ceiling type C3 and wall type W3w in shower areas. Floor finish in shower areas to provide drainage ","Type L7.2","Type L7.2","Preferred","Preferred","N/A","N/A","N/A","N/A",0.3,0.3,200,200,300,300,70,70,"N/A","N/A",22,22,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No","Water / moisture grade luminaires. ","Type T4","Type T4",21,21,"Contractor to specify (CTS)",19,19,26,26,40,"N/A",6,"N/A",4,"N/A","N/A","N/A","N/A","N/A",200,200,16,16,"Type V2d","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"A5.50/65","Note 1","High","High",null,"Contractor to specify (CTS)",null,50,50,65,65,"N/A","N/A","N/A","N/A","N/A","N/A","R15","R15","<=1.5","<=2.0","A means of increasing the air velocity during the summer shall be provided.  Intermittent extract of 15l/s per shower/bath   ","None","Power to hand dryer if provided","Hot and cold to shower cubicles. One shower cubicle for every 8m2 of total changing area. Towel rails. Soap dish to each cubicle.","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["TOC02 (Accessible changing ...",null,null,null,"Accessible changing & showers","TOC02","Wet changing and shower cubicle for male or female staff, or for disabled or community users",6,"m2","Changing and showering for staff member or disabled pupil or visitor, for PE."," N/A ",1,1,"Non-net","N/A","Non-net","None",2,"all indoor and outdoor sports facilities ","As SoA","Full disabled access required","Enclosed","As SSDB",6,6,2700,2400,"CTS",null,"Not Required ",null,"As existing","Contractor to specify if provided","Type D4.2","Note 1","Suitable for wet areas and durable",30,"  ",926,null,825,null,2000,null,5,null,4,null,30,null,"Yes",null,"Yes",null,"No",null,"No",null,"No",null,"Standard",null,"Deadlock only",null,"No",null,"Both faces",null,"Yes",null,450,null,"N/A","Note 1","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Surface protection to limit wheelchair damage.  Handles ergonomic to suit limited dexterity and to be at the correct height to promote independence.","Type F7","Note 1","Wet area ceramic, resin, rubber or vinyl","Yes for vinyl",null,"Commercial 34",null,"N/A",null,0.2,null,10,null,"Yes, see note",null,"Minimum SRV 36",null,"Yes",null,"Yes",null,"High",null,"No",null,"Yes",null,"No",null,"Type C2","Note 1","Humid",0.7,"Humid","Type W2h","Type W2h","Humid areas and toilets",0.5,0.5,"Yes","Yes","N/A","N/A","Yes","Yes","Humid","Humid","N/A","Barefoot areas shall be barefoot slip resistance category B Ceiling type C3 and wall type W3w in shower areas. Floor finish in shower areas to provide drainage. Floor laid to simple falls to flush gully or grating","Type L7.2","Type L7.2","Preferred","Preferred","N/A","N/A","N/A","N/A",0.3,0.3,200,200,300,300,70,70,"N/A","N/A",22,22,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No","Water / moisture grade luminaires.","Type T4","/=K165",21,21,"Contractor to specify (CTS)",19,19,26,26,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,16,16,"Type V2d","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.3,null,"N/A",null,"A5.50/65","/=K188","High","High",null,"Contractor to specify (CTS)",null,50,50,65,65,"N/A","N/A","N/A","N/A","N/A","N/A","R15","R15","<=1.5","<=2.0","A means of increasing the air velocity during the summer shall be provided.  Intermittent extract of 15l/s per shower/bath. If space is refurbished, see Note 2 in tech annexe.      ","None  ","Power to hand dryer if provided","Hot and cold to shower area. Lever operated level entry shower to BS8300 with shower seat, fixed and drop down rails, half height folding shower door, shower controls to Part M. Towel rails. Soap dish.  ","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","N/A","CTS","CTS","CTS",null,"Contractor to Specify where provided",null,"Add here text to be included on sign","N/A","CTS","Contractor to specify if provided for glare control","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS","CTS"]
["TOC54 (Special hygiene faci -nf",null,null,null,"Special hygiene facilities - with wc","TOC54","Special school hygiene room for disabled pupils' wash-down (peninsular changing bed)",12,"m2"," Room for changing pupils, with bed against wall, assisted shower.",1,1,2,"Non-net","N/A","Non-net","None",5,"All SEN spaces","As SoA","Full disabled access required","Enclosed","As SSDB",12,12,"2700 (and to suit hoist)",2400,"N/A",null,"Lockable openable windows or vents to be provided. With restrictors. Window head height to be as close to ceiling as possible. controlled exit. weight of external door and ironmongery to enable operation by pupils (when permitted by staff). Hinges to protect fingers. Level threshold. External door handles warm to touch material.",null,"As existing","Contractor to specify if provided","Type D4.2s","Note 1","Special suitable for wet areas and durable",30,"  ",1026,null,925,null,2000,null,5,null,4,null,30,null,"Yes",null,"Yes",null,"No",null,"No",null,"No",null,"Protected",null,"Deadlock only",null,"No",null,"Both faces",null,"Yes",null,450,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"Surface protection to limit wheelchair damage.  Handles ergonomic to suit limited dexterity and to be at the correct height to promote independence. Means to control access to be agreed with school.","Type F7","Type F7","Wet area ceramic, resin, rubber or vinyl","Yes for vinyl","Yes for vinyl","Commercial 34","Commercial 34","N/A","N/A",0.2,0.2,10,10,"Yes, see note","Yes, see note","Minimum SRV 36","Minimum SRV 36","Yes","Yes","Yes","Yes","High","High","No","No","Yes","Yes","No","No","Type C2","Note 1","Humid",0.7,"Humid","Type W3w","Type W3w","Wet areas",0.5,0.5,"Yes","Yes","Yes","Yes","Yes","Yes","Wet","Wet","N/A","Barefoot areas shall be barefoot slip resistance category B Ceiling to take hoist tracking in both directions, avoiding light fittings","Type L7.2","Type L7.2","Preferred","Preferred","N/A","N/A","N/A","N/A",0.3,0.3,200,200,300,300,70,70,"N/A","N/A",22,22,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No","Water / moisture grade luminaires. avoid direct downlighting over changing bed","Type T3","Type T3",23,23,"Contractor to specify (CTS)",21,21,25,25,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,18,18,"Type V3","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.15,null,"10 ach (see note)",null,"A3.50/65","Note 1","Average","Medium",null,"Contractor to specify (CTS)",null,50,50,65,65,"N/A","N/A","N/A","N/A","N/A","N/A","R15","R15","<=1.5","<=2.0","A means of increasing the air velocity during the summer shall be provided.  In toilets and hygiene rooms: intermittent extract of 6l/s per WC/urinal and 15l/s per shower/bath or 10ach whichever is greater   ","None  ","Power to hand dryers if provided","Cold, with hot and cold handwash.  Adjustable height basin. Type of tap to be agreed with school. WC with drop down rails.  ","CTS","N/A","N/A","N/A","N/A","N/A","N/A","N/A","CTS","N/A","N/A","CTS",null,"Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["TOC53 (Special hygiene faci -nf",null,null,null,"Special hygiene facilities - without wc","TOC53","Special school hygiene room for disabled pupils' wash-down and use of WC",15,"m2"," Room for changing pupils, with peninsular shower bed.",1,1,2,"Non-net","N/A","Non-net","None",5,"All SEN spaces","As SoA","Full disabled access required","Enclosed","As SSDB",15,13,"2700 (and to suit hoist)",2400,"N/A",null,"Lockable openable windows or vents to be provided. With restrictors. Window head height to be as close to ceiling as possible. controlled exit. weight of external door and ironmongery to enable operation by pupils (when permitted by staff). Hinges to protect fingers. Level threshold. External door handles warm to touch material.",null,"As existing","Contractor to specify if provided","Type D4.2s","Note 1","Special suitable for wet areas and durable",30,"  ",1026,null,925,null,2000,null,5,null,4,null,30,null,"Yes",null,"Yes",null,"No",null,"No",null,"No",null,"Protected",null,"Deadlock only",null,"No",null,"Both faces",null,"Yes",null,450,null,"N/A","N/A","No internal door required",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   ",null,null,null,null,null,null,null,null,null,"   ",null,null,null,"If door to open out,  to have horizontal rail to enable closing. Surface protection to limit wheelchair damage.  Handles ergonomic to suit limited dexterity and to be at the correct height to promote independence. Means to control access to be agreed with school","Type F7","Type F7","Wet area ceramic, resin, rubber or vinyl","Yes for vinyl","Yes for vinyl","Commercial 34","Commercial 34","N/A","N/A",0.2,0.2,10,10,"Yes, see note","Yes, see note","Minimum SRV 36","Minimum SRV 36","Yes","Yes","Yes","Yes","High","High","No","No","Yes","Yes","No","No","Type C2","Note 1","Humid",0.7,"Humid","Type W3w","Type W3w","Wet areas",0.5,0.5,"Yes","Yes","Yes","Yes","Yes","Yes","Wet","Wet","N/A","Barefoot areas shall be barefoot slip resistance category B Ceiling to take hoist tracking in both directions, avoiding light fittings","Type L7.2","Type L7.2","Preferred","Preferred","N/A","N/A","N/A","N/A",0.3,0.3,200,200,300,300,70,70,"N/A","N/A",22,22,"N/A","N/A",0.4,0.4,80,80,"Contractor to specify (CTS)",null,"Contractor to specify (CTS)",null,"CTS","N/A","occ, sw","No","Water / moisture grade luminaires. Avoid direct downlighting over changing bed","Type T3","Type T3",23,23,"Contractor to specify (CTS)",21,21,25,25,40,"N/A",6,"N/A",4,"N/A","N/A",120,"N/A",5,200,200,18,18,"Type V3","Note 1","N/A",null,"N/A",null,"N/A",null,"N/A",null,"N/A",null,0.15,null,"10 ach (see note)",null,"A3.50/65","Note 1","Average","Medium",null,"Contractor to specify (CTS)",null,50,50,65,65,"N/A","N/A","N/A","N/A","N/A","N/A","R15","R15","<=1.5","<=2.0","A means of increasing the air velocity during the summer shall be provided.  In toilets and hygiene rooms: intermittent extract of 6l/s per WC/urinal and 15l/s per shower/bath or 10ach whichever is greater   ","None  ","Power to hand dryers if provided","Cold, with hot and cold handwash.  Water to whb to be pre-mixed max temperature 43 degrees.  Adjustable height whb, type of tap to be agreed with school. Floor mounted sluice. Cartridge-type lockable soap dispenser. High velocity electric hand dryer or hand towel dispenser. Lockable sheet dispensing toilet paper holders. Contrasting rails and fittings to meet Part M.  Mirror above each wash hand basin.","CTS","N/A","N/A","N/A","N/A","N/A","N/A","N/A","CTS","N/A","N/A","CTS",null,"Contractor to Specify",null,"Add here text to be included on sign","N/A","N/A","Contractor to specify if provided","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]

{"sheet":"(Manual) NotesLib","index":7,"n_rows":135,"n_cols":28,"rows_kept":135,"cut":false,"hidden":true,"merged":[]}
[]
[null,null,null,null,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24]
["ADM01 (Entrance and reception)","ADM01",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["ADM02 (Interview room)","ADM02",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 6m2 for 4","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["ADM03 (Sick bay)","ADM03",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 4m2 for 2","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["ADM04 (Sick room)","ADM04",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 6m2 for 3","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["ADM05 (General office)","ADM05",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["ADM06 (student services office)","ADM06",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["ADM08 (Reprographics room)","ADM08",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["ADM11 (Heads office)","ADM11",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 16m2 for 1 desk and 4 meeting","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["ADM13 (Office (PA to head))","ADM13",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 7m2 for 1","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["ADM20 (Kitchenette)","ADM20",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["ADM21 (Community entrance)","ADM21",null,null,"name of generic space type","reference code for generic space type",null,"As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["CIR00 (Circulation)","CIR00",null,null,null,null,"Varies. ","As SoA","based on teaching group size above",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:1997","Class defined in BS EN12400:2000","in FD##s BS476-22 or E##Sa BS EN1643-3:2001","security rating defined in LSP 1175",null,"Rw (db) to BS EN ISO717-1:1997","Class defined in BS EN12400:2000","in FD##s BS476-22 or E##Sa BS EN1643-3:2001","security rating defined in LSP 1175",null,"UDI-a to lie between 100 lux and 2000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["CIR01 (Corridor)","CIR01",null,null,null,null,"Varies. ","As SoA","based on teaching group size above",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:1997","Class defined in BS EN12400:2000","in FD##s BS476-22 or E##Sa BS EN1643-3:2001","security rating defined in LSP 1175",null,"Rw (db) to BS EN ISO717-1:1997","Class defined in BS EN12400:2000","in FD##s BS476-22 or E##Sa BS EN1643-3:2001","security rating defined in LSP 1175",null,"UDI-a to lie between 100 lux and 2000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["DIN01 (Dining area(s))","DIN01",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["KIT00 (School kitchen prep & s)","KIT00",null,null,"name of generic space type","reference code for generic space type","CTS within total school kitchen suite area in SoA","As SoA",null,null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["KIT01 (School kitchen prepa...","KIT01",null,null,"name of generic space type","reference code for generic space type","CTS within total school kitchen suite area in SoA","As SoA",null,null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["KIT02 (School kitchen serve...","KIT02",null,null,"name of generic space type","reference code for generic space type","CTS within total school kitchen suite area in SoA","As SoA",null,null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["KIT03 (School kitchen office)","KIT03",null,null,"name of generic space type","reference code for generic space type","CTS within total school kitchen suite area in SoA","As SoA",null,null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["KIT04 (School kitchen staff","KIT04",null,null,"name of generic space type","reference code for generic space type","CTS within total school kitchen suite area in SoA","As SoA",null,null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)","m length","Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["KIT05 (School kitchen store)","KIT05",null,null,"name of generic space type","reference code for generic space type","CTS within total school kitchen suite area in SoA","As SoA",null,null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["KIT06 (School kitchen dry s...","KIT06",null,null,"name of generic space type","reference code for generic space type","CTS within total school kitchen suite area in SoA","As SoA",null,null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93","m length","Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["KIT07 (School kitchen cold ...","KIT07",null,null,"name of generic space type","reference code for generic space type","CTS within total school kitchen suite area in SoA","As SoA",null,null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93","m length","Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["KIT08 (School kitchen freez...","KIT08",null,null,"name of generic space type","reference code for generic space type","CTS within total school kitchen suite area in SoA","As SoA",null,null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93","m length","Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["KIT09 (School kitchen toile...","KIT09",null,null,"name of generic space type","reference code for generic space type",null,"As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["OFF00 (Office only)","OFF00",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 7m2 for 1, 9m2 for 2","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["OFF10 (Office and meeting)","OFF10",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 13m2 for 2 plus 3 in meeting","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["OFF15 (Office and workroom)","OFF15",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["OFF20 (Office and pastoral)","OFF20",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["OFF31 (Staff room (prep social)","OFF31",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA",null,null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["OFF32 (Staff room social)","OFF32",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["OFF33 (Staff work room)","OFF33",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["OFF35 (Staff wk rm (with sink)","OFF35",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["OFF41 (Conference and meeti...","OFF41",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["OFF42 (Laundry)","OFF42",null,null,"name of generic space type","reference code for generic space type",null,null,null,null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours","within range ","In refurbishment","and for Nat Vent when nat vent paths are shut - see BB93","m length","Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["PLA01 (Plant room)","PLA01",null,null,null,null,"Varies","As SoA","based on teaching group size above",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:1997","Class defined in BS EN12400:2000","in FD##s BS476-22 or E##Sa BS EN1643-3:2001","security rating defined in LSP 1175",null,"Rw (db) to BS EN ISO717-1:1997","Class defined in BS EN12400:2000","in FD##s BS476-22 or E##Sa BS EN1643-3:2001","security rating defined in LSP 1175",null,"UDI-a to lie between 100 lux and 2000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["PLA02 (Server room)","PLA02",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA",null,null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["RES00 (Group room)","RES00",null,null,"name of generic space type","reference code for generic space type","As SoA. Small group room 9m2 for 3 incl wheelchair user","As SoA. Zone B unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["SEN01 (SEN resource base)","SEN01",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 16m2 for 7 including wheelchair user","As SoA. Zone C unless restrictive or extensive",null,null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["SEN06 (Inclusion immersion...)","SEN06",null,null,"name of generic space type","reference code for generic space type","typical area for group described","As SoA. Zone C unless restrictive or extensive",null,null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["SEN11 (SEN therapy and MI r...","SEN11",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 12m2 for 3 including wheelchair user","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["STH00 (PE store(s))","STH00",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 10% of hall served","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["STH05 (External PE store)","STH05",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 8m2","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["STH10 (Furniture store)","STH10",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["STN01 (Personal storage (cl...","STN01",null,null,"name of generic space type","reference code for generic space type","As SoA, not including circulation. Standard 2.5m2 for 30","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["STN02 (Personal storage (lo","STN02",null,null,"name of generic space type","reference code for generic space type","Contractor to Specify each set to match total area in SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["STN04 (Wheelchair and appli...","STN04",null,null,"name of generic space type","reference code for generic space type","Contractor to Specify each set to match total area in SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["STN21 (Secure and exam and ...","STN21",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 5m2","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["STN31 (Cleaners store)","STN31",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 1.5m2 in new build","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["STT05 (Specialist store)","STT05",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 5m2 in new build","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["STT10 (General store)","STT10",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 5m2 in new build","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["SUP01 (Chapel)","SUP01",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["TOC03 (Hygiene rm (without","TOC03",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 9m2 with 2 doors in new build","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["TOC04 (Hygiene room (with w","TOC04",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 12m2","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["TOC13 (Pupil toilet suite)","TOC13",null,null,"name of generic space type","reference code for generic space type","Contractor to Specify each suite to match total area in SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["TOC15 (Individual toilet)","TOC15",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 3m2 for 1 in new build","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["TOC21 (Staff and accessible...","TOC21",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 3.5m2 for 1 in new build","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["TOC22 (Staff toilet suite)","TOC22",null,null,"name of generic space type","reference code for generic space type","Contractor to Specify each suite to match total area in SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see BB93",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["HAL11 (Studio)","HAL11",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 55m2 for 30","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample F&E layouts. Contractor to reuse legacy items where possible."]
["HAL12 (Small hall)","HAL12",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 80m2 for 30","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample F&E layouts. Contractor to reuse legacy items where possible."]
["HAL13 (Main hall)","HAL13",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 150 or 180m2 for teaching group of 30","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample F&E layouts. Contractor to reuse legacy items where possible."]
["LIB01 (Library )","LIB01",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA. Zone B unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample F&E layouts. Contractor to reuse legacy items where possible."]
["PRA01 (ICT rich practical r...","PRA01",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 62m2 for 30","As SoA. Zone C unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample F&E layouts. Contractor to reuse legacy items where possible."]
["PRA11 (Food bay and practic...","PRA11",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 13m2 for up to 4","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample F&E layouts. Contractor to reuse legacy items where possible."]
["PRA12 (Food science DT art)","PRA12",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 34m2 for 15, 62m2 for 30","As SoA. Zone D unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample F&E layouts. Contractor to reuse legacy items where possible."]
["PRI03 (Nursery playroom)","PRI03",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 55m2 for 26","As SoA. Zone D unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample F&E layouts. Contractor to reuse legacy items where possible."]
["PRI04 (Nursery 2 to 3 year old)","PRI04",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 55m2 for 20","As SoA. Zone E as extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample F&E layouts. Contractor to reuse legacy items where possible."]
["PRI13 (Reception classroom)","PRI13",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 34m2 for 15, 62m2 for 30","As SoA. Zone D unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample F&E layouts. Contractor to reuse legacy items where possible."]
["PRI22 (Classbase with sink)","PRI22",null,null,"name of generic space type","reference code for generic space type","As SoA.Standard 50m2 for 30","As SoA. Zone B ","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample F&E layouts. Contractor to reuse legacy items where possible."]
["PRI23 (Infant classroom)","PRI23",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 55m2 for 30, 62m2 for 30 if extensive","As SoA. Zone C unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample F&E layouts. Contractor to reuse legacy items where possible."]
["PRI26 (Shared without sink)","PRI26",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA. Zone C unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample F&E layouts. Contractor to reuse legacy items where possible."]
["PRI32 (Classbase without sink)","PRI32",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 50m2 for 30","As SoA. Zone B unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample F&E layouts. Contractor to reuse legacy items where possible."]
["PRI33 (Junior classroom)","PRI33",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 55m2 for 30","As SoA. Zone C unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample F&E layouts. Contractor to reuse legacy items where possible."]
["PRI36 (Shared teach with sink)","PRI36",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA. Zone C unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample F&E layouts. Contractor to reuse legacy items where possible."]
["RES41 (Pupil changing (dry))","RES41",null,null,"name of generic space type","reference code for generic space type","As SoA. Small changing room incl wheelchair user","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample F&E layouts. Contractor to reuse legacy items where possible."]
["STT03 (Teaching storage bay)","STT03",null,null,null,null,"As SoA. Standard 1.5m2","As SoA","based on teaching group size above",null,"between internal faces of external and internal walls","Contractor to specify (CTS) ","Rw (db) to BS EN ISO717-1:1997","Class defined in BS EN12400:2000","in FD##s BS476-22 or E##Sa BS EN1643-3:2001","security rating defined in LSP 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Groups 1 and 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible"]
["TOC11 (Foundation toilets)","TOC11",null,null,"name of generic space type","reference code for generic space type","As SoA, typically based on 4m2 per wc","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample F&E layouts. Contractor to reuse legacy items where possible."]
["ACT01 (Dance studio)","ACT01",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 120m2 for 30","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["ACT05 (Activity studio)","ACT05",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 150m2 for 30","As SoA","As SoA","Minimum clear height","typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["ACT22 (Fitness exercise)","ACT22",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 69m2 for 20","As SoA","As SoA","Minimum clear height","typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["CLA02 (Seminar room)","CLA02",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 41m2 for 22","As SoA. Zone C unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["CLA12 (General classroom)","CLA12",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 55m2 for 30","As SoA. Zone C unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["CLA13 (Extensive classroom)","CLA13",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 62m2 for 30","As SoA. Zone D as extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["CLA18 (Open learning area)","CLA18",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 55m2 for 30","As SoA. Zone C unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["CLA31 (Temporarily ICT-rich...)","CLA31",null,null,"name of generic space type","reference code for generic space type",null,"As SoA. Zone D unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["CLA32 (ICT-rich classroom)","CLA32",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 62m2 for 30","As SoA. Zone D unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["CLA35 (ICT-rich learning area)","CLA35",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 62m2 for 30","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["CLA41 (ICT and business stu...","CLA41",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 62m2 for 30","As SoA. Zone D unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["DAT02 (General art room)","DAT02",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 83m2 for 30 or 90m2 for 32","As SoA. Zone F unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["DAT03 (3D Art room)","DAT03",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 97m2 for 30","As SoA. Zone G unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["DAT04 (3D art room (ceramics))","DAT04",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 104m2 for 32","As SoA. Zone G unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["DAT05 (3D art room (textiles)","DAT05",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 104m2 for 32","As SoA. Zone G unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["DAT12 (Hair and beauty salo","DAT12",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 69m2 for 16","As SoA. Zone H unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["DAT15 (Photography studio)","DAT15",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 83m2 for 30 or 90m2 for 32","As SoA. Zone F unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["DAT22 (Graphic products)","DAT22",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 83m2 for 25","As SoA. Zone G unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["DAT25 (Constructional texti...","DAT25",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 83m2 for 25","As SoA. Zone G unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["DAT28 (Electronics and cont...","DAT28",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 83m2 for 25","As SoA. Zone G unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["DAT32 (Food studio)","DAT32",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 69m2 for 24","As SoA. Zone F unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["DAT35 (Food room)","DAT35",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 97m2 if 2 rooms, 104m2 if 1","As SoA. Zone H unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["DAT43 (Resistant materials ...","DAT43",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 97m2 if 2 rooms, 104m2 if 1","As SoA. Zone H unless restrictive or extensive","As SoA","Minimum clear height","typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["DAT46 (RM with heat bay)","DAT46",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 111m2 for 24","As SoA. Zone I unless restrictive or extensive","As SoA","Minimum clear height","typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["DAT48 (Engineering workshop)","DAT48",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 97m2 for up to 20","As SoA. Zone I unless restrictive or extensive","As SoA","Minimum clear height","typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["DAT49 (Construction workshop)","DAT49",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 97m2 for 16","As SoA. Zone J unless restrictive or extensive","As SoA","Minimum clear height","typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["DIN04 (Social space)","DIN04",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["DIN05 (Sixth form social sp...","DIN05",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["HAL01 (Main hall)","HAL01",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 197, 226, 254, 282m2","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["LIB05 (Library resource cen","LIB05",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["LIB06 (Sixth form study are...","LIB06",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["PER01 (Music classroom)","PER01",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 62m2 for 30","As SoA. Zone D unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["PER02 (Extensive music clas...","PER02",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 69m2 for 30","As SoA. Zone E as extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["PER04 (Music recital and dr...","PER04",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 83m2 for 30","As SoA. Zone F unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["PER05 (Drama studio)","PER05",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 90m2 for 30","As SoA. Zone F unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["RES12 (Music practice and g...","RES12",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 8m2 for 3","As SoA. Zone B unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["RES13 (Extensive music prac)","RES13",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 16m2 for up to 7","As SoA. Zone C as extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["RES14 (Control room for rec...","RES14",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 8m2 for 3","As SoA. Zone B unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["RES16 (Lighting and audio c...","RES16",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 6m2 for 2","As SoA. Zone B unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["RES21 (Kiln room)","RES21",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 4m2 for new build.","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["RES22 (Dark room)","RES22",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 9m2 for up to 5","As SoA. Zone B unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["SCI02 (Science studio)","SCI02",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 69m2 in new build.","As SoA. Zone E unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["SCI05 (General science labo","SCI05",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 83m2 for 30 in new build.","As SoA. Zone F unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["SCI11 (Specialist sci lab)","SCI11",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 90m2 for up to 30 in new build.","As SoA. Zone F unless restrictive or extensive","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["SPH00 (school sports hall)","SPH00",null,null,"name of generic space type","reference code for generic space type","As SoA. 4-court 594m2 (18m x 33m) for up to 60","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["SPH20 (Community sports hall)","SPH20",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 20m x 34.5m for up to 60","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["STH20 (Bleacher seating)","STH20",null,null,"name of generic space type","reference code for generic space type","As SoA. Typically 16m2","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["STT08 (Drama store (off room))","STT08",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 10m2 in new build","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["STT21 (Science prep room)","STT21",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["STT23 (Chemical store)","STT23",null,null,"name of generic space type","reference code for generic space type","Typically 7m2 or 4m2 in small schools","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["STT32 (Multi-materials stor...","STT32",null,null,"name of generic space type","reference code for generic space type","typically 41m2 or 34m2 if 1 workshop","As SoA","As SoA","Minimum clear height","typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["STT34 (Food store and prep ...","STT34",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 10m2 for new build","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["STT35 (Food store (off food...","STT35",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 5m2","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["TOC01 (Pupil changing and s","TOC01",null,null,"name of generic space type","reference code for generic space type","As SoA","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["TOC02 (Accessible changing ...","TOC02",null,null,"name of generic space type","reference code for generic space type","As SoA. Standard 6m2","As SoA","As SoA",null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Group 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["TOC54 (Special hygiene faci -nf","TOC54",null,null,"name of generic space type","reference code for generic space type",null,null,null,null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Groups 1 and 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]
["TOC53 (Special hygiene faci -nf","TOC53",null,null,"name of generic space type","reference code for generic space type",null,null,null,null,"typically actual depth between internal faces of walls","Contractor to specify (CTS) dimension from FFL","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","Rw (db) to BS EN ISO717-1:2013","Class defined in BS EN12400:2002","in FD##s BS476-22:1987 or E##Sa to BS EN1643-3:2004","security rating defined in LPS 1175","to BS EN 50133-1:1997","UDI-a to lie between 100 lux and 3000 lux for percentage of core hours",null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,"Groups 1 and 2 FF&E shall be provided to allow the activities listed above to be carried out safely, effectively and efficiently by the maximum number of pupils and/or staff, using FF&E with attributes similar to the indicative FF&E listed below, as shown in sample FF&E layouts. Contractor to reuse legacy items where possible."]

{"sheet":"Individual Spaces","index":8,"n_rows":255,"n_cols":65,"rows_kept":255,"cut":false,"hidden":false,"merged":[]}
[null,null,null,null,null,null,null,null,null,null,null,null,"List generated at 18:43 on the 04/12/2023"]
["SCHOOL:",null,null,{"$f":"'Secondary SoA'!S2","v":"[Insert Project Code and Scheme Name here in title sheet]"},null,null,null,null,null,null,null,null,null,null,"RETAINED AREAS"]
["Parent ADS Code","Final ADS Code","Unique Room Code",null,"Unique room name",null,"Suite","Required Area (m2)","Employers Notes",null,"Proposed Area (m2)","Difference","Contractors Notes",null,"ER to New / Remodel / Keep","Existing Room","Existing Room Name","cell location on Secondary SoA",null,"CP to New / Remodel / Keep"]
["CLA02","CLA02",1001,"Seminar room 1",null,"Seminar room41","Mathematics",41,null,null,null,-41,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41,null,null,null,-41,null,null,null,null,null,null,null,"New Build"]
["CLA02","CLA02",1002,"Seminar room 2",null,"Seminar room41","English",41,null,null,null,-41,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41,null,null,null,-41,null,null,null,null,null,null,null,"New Build"]
["CLA02","CLA02",1003,"Seminar room 3",null,"Seminar room41","MFL",41,null,null,null,-41,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41,null,null,null,-41,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1004,"Classrooms (general) 1",null,"Classrooms (general)55","Mathematics",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1005,"Classrooms (general) 2",null,"Classrooms (general)55","Mathematics",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1006,"Classrooms (general) 3",null,"Classrooms (general)55","Mathematics",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1007,"Classrooms (general) 4",null,"Classrooms (general)55","Mathematics",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1008,"Classrooms (general) 5",null,"Classrooms (general)55","Mathematics",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1009,"Classrooms (general) 6",null,"Classrooms (general)55","Mathematics",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1010,"Classrooms (general) 7",null,"Classrooms (general)55","Mathematics",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1011,"Classrooms (general) 8",null,"Classrooms (general)55","Mathematics",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1012,"Classrooms (general) 9",null,"Classrooms (general)55","English",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1013,"Classrooms (general) 10",null,"Classrooms (general)55","English",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1014,"Classrooms (general) 11",null,"Classrooms (general)55","English",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1015,"Classrooms (general) 12",null,"Classrooms (general)55","English",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1016,"Classrooms (general) 13",null,"Classrooms (general)55","English",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1017,"Classrooms (general) 14",null,"Classrooms (general)55","English",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1018,"Classrooms (general) 15",null,"Classrooms (general)55","English",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1019,"Classrooms (general) 16",null,"Classrooms (general)55","English",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1020,"Classrooms (general) 17",null,"Classrooms (general)55","MFL",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1021,"Classrooms (general) 18",null,"Classrooms (general)55","MFL",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1022,"Classrooms (general) 19",null,"Classrooms (general)55","MFL",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1023,"Classrooms (general) 20",null,"Classrooms (general)55","MFL",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1024,"Classrooms (general) 21",null,"Classrooms (general)55","MFL",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1025,"Classrooms (general) 22",null,"Classrooms (general)55","MFL",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1026,"Classrooms (general) 23",null,"Classrooms (general)55","Humanities",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1027,"Classrooms (general) 24",null,"Classrooms (general)55","Humanities",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1028,"Classrooms (general) 25",null,"Classrooms (general)55","Humanities",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1029,"Classrooms (general) 26",null,"Classrooms (general)55","Humanities",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
["CLA12","CLA12",1030,"Classrooms (general) 27",null,"Classrooms (general)55","Humanities",55,null,null,null,-55,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,null,null,-55,null,null,null,null,null,null,null,"New Build"]
[null,null,null,null,"General Teaching Total : ",null,null,1608,null,null,0,-1608,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1608,null,null,0,-1608]
["CLA32","CLA32",1101,"ICT-rich classroom 1",null,"ICT-rich classroom69","ICT and Business Studies",69,null,null,null,-69,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,69,null,null,null,-69,null,null,null,null,null,null,null,"New Build"]
["CLA32","CLA32",1102,"ICT-rich classroom 2",null,"ICT-rich classroom69","ICT and Business Studies",69,null,null,null,-69,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,69,null,null,null,-69,null,null,null,null,null,null,null,"New Build"]
["CLA32","CLA32",1103,"ICT-rich classroom 3",null,"ICT-rich classroom69","ICT and Business Studies",69,null,null,null,-69,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,69,null,null,null,-69,null,null,null,null,null,null,null,"New Build"]
["CLA32","CLA42",1104,"ICT-rich classroom (business studies) 1",null,"ICT-rich classroom (business studies)69","ICT and Business Studies",69,null,null,null,-69,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,69,null,null,null,-69,null,null,null,null,null,null,null,"New Build"]
["SCI05","SCI05",1105,"Science laboratory 1",null,"Science laboratory83","Science",83,null,null,null,-83,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,83,null,null,null,-83,null,null,null,null,null,null,null,"New Build"]
["SCI05","SCI05",1106,"Science laboratory 2",null,"Science laboratory83","Science",83,null,null,null,-83,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,83,null,null,null,-83,null,null,null,null,null,null,null,"New Build"]
["SCI05","SCI05",1107,"Science laboratory 3",null,"Science laboratory83","Science",83,null,null,null,-83,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,83,null,null,null,-83,null,null,null,null,null,null,null,"New Build"]
["SCI05","SCI05",1108,"Science laboratory 4",null,"Science laboratory83","Science",83,null,null,null,-83,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,83,null,null,null,-83,null,null,null,null,null,null,null,"New Build"]
["SCI05","SCI05",1109,"Science laboratory 5",null,"Science laboratory83","Science",83,null,null,null,-83,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,83,null,null,null,-83,null,null,null,null,null,null,null,"New Build"]
["SCI05","SCI05",1110,"Science laboratory 6",null,"Science laboratory83","Science",83,null,null,null,-83,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,83,null,null,null,-83,null,null,null,null,null,null,null,"New Build"]
["SCI05","SCI05",1111,"Science laboratory 7",null,"Science laboratory83","Science",83,null,null,null,-83,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,83,null,null,null,-83,null,null,null,null,null,null,null,"New Build"]
["SCI05","SCI11",1112,"Science laboratory (specialist) 1",null,"Science laboratory (specialist)97","Science",97,null,null,null,-97,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,97,null,null,null,-97,null,null,null,null,null,null,null,"New Build"]
["SCI05","SCI11",1113,"Science laboratory (specialist) 2",null,"Science laboratory (specialist)97","Science",97,null,null,null,-97,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,97,null,null,null,-97,null,null,null,null,null,null,null,"New Build"]
["SCI05","SCI11",1114,"Science laboratory (specialist) 3",null,"Science laboratory (specialist)97","Science",97,null,null,null,-97,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,97,null,null,null,-97,null,null,null,null,null,null,null,"New Build"]
["DAT00","DAT02",1115,"Art room (general) 1",null,"Art room (general)83","DT/ Art",83,null,null,null,-83,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,83,null,null,null,-83,null,null,null,null,null,null,null,"New Build"]
["DAT00","DAT03",1116,"Art room (3D) 1",null,"Art room (3D)97","DT/ Art",97,null,null,null,-97,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,97,null,null,null,-97,null,null,null,null,null,null,null,"New Build"]
["DAT00","DAT03",1117,"Art room (3D) 2",null,"Art room (3D)97","DT/ Art",97,null,null,null,-97,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,97,null,null,null,-97,null,null,null,null,null,null,null,"New Build"]
["PER02","PER03",1118,"Music room (fitted, extensive) 1",null,"Music room (fitted, extensive)69","Perf arts, hall and dining",69,null,null,null,-69,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,69,null,null,null,-69,null,null,null,null,null,null,null,"New Build"]
["PER15","PER15",1119,"Drama studio 1",null,"Drama studio97","Perf arts, hall and dining",97,null,null,null,-97,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,97,null,null,null,-97,null,null,null,null,null,null,null,"New Build"]
["DAT43","DAT43",1120,"DT workshop 1",null,"DT workshop111","DT/ Art",111,null,null,null,-111,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,111,null,null,null,-111,null,null,null,null,null,null,null,"New Build"]
["DAT35","DAT35",1121,"Food room 1",null,"Food room97","DT/ Art",97,null,null,null,-97,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,97,null,null,null,-97,null,null,null,null,null,null,null,"New Build"]
["DAT20","DAT22",1122,"DT studio (graphic products) 1",null,"DT studio (graphic products)83","DT/ Art",83,null,null,null,-83,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,83,null,null,null,-83,null,null,null,null,null,null,null,"New Build"]
["DAT20","DAT25",1123,"DT studio (textiles) 1",null,"DT studio (textiles)83","DT/ Art",83,null,null,null,-83,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,83,null,null,null,-83,null,null,null,null,null,null,null,"New Build"]
[null,null,null,null,"Specialist Practical Total : ",null,null,1965,null,null,0,-1965,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1965,null,null,0,-1965]
["HAL01","HAL03",2001,"Assembly halls, secondary (with bleachers) 1",null,"Assembly halls, secondary (with bleachers)197","Perf arts, hall and dining",197,null,null,null,-197,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,197,null,null,null,-197,null,null,null,null,null,null,null,"New Build"]
["SPH00","SPH04",2002,"Sports hall, school (4-court) 1",null,"Sports hall, school (4-court)594","Sports/ PE",594,null,null,null,-594,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,594,null,null,null,-594,null,null,null,null,null,null,null,"New Build"]
["ACT05","ACT07",2003,"Activity studio (10 x 15) 1",null,"Activity studio (10 x 15)150","Sports/ PE",150,null,null,null,-150,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,null,null,null,-150,null,null,null,null,null,null,null,"New Build"]
["DIN01","DIN01",2004,"Dining hall 1",null,"Dining hall210","Perf arts, hall and dining",210,null,null,null,-210,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,210,null,null,null,-210,null,null,null,null,null,null,null,"New Build"]
["DIN02","DIN02",2005,"Informal dining space 1",null,"Informal dining space111","Balance",111,null,null,null,-111,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,111,null,null,null,-111,null,null,null,null,null,null,null,"New Build"]
[null,null,null,null,"Large Spaces Total : ",null,null,1262,null,null,0,-1262,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1262,null,null,0,-1262]
["LIB05","LIB05",3001,"Library resource centre (LRC) 1",null,"Library resource centre (LRC)146","Balance",146,null,null,null,-146,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,146,null,null,null,-146,null,null,null,null,null,null,null,"New Build"]
["LIB07","LIB06",3002,"Study space, room (sixth form) 1",null,"Study space, room (sixth form)69","Balance",69,null,null,null,-69,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,69,null,null,null,-69,null,null,null,null,null,null,null,"New Build"]
["RES21","RES21",3003,"Heavy practical resource (kiln) 1",null,"Heavy practical resource (kiln)4","DT/ Art",4,null,null,null,-4,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,-4,null,null,null,null,null,null,null,"New Build"]
["RES12","RES12",3004,"Music practice room 1",null,"Music practice room8","Perf arts, hall and dining",8,null,null,null,-8,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,-8,null,null,null,null,null,null,null,"New Build"]
["RES12","RES13",3005,"Music practice room (extensive) 1",null,"Music practice room (extensive)16","Perf arts, hall and dining",16,null,null,null,-16,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,null,null,null,-16,null,null,null,null,null,null,null,"New Build"]
["RES12","RES13",3006,"Music practice room (extensive) 2",null,"Music practice room (extensive)16","Perf arts, hall and dining",16,null,null,null,-16,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,null,null,null,-16,null,null,null,null,null,null,null,"New Build"]
["RES14","RES14",3007,"Recording control space 1",null,"Recording control space8","Perf arts, hall and dining",8,null,null,null,-8,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,-8,null,null,null,null,null,null,null,"New Build"]
["RES16","RES16",3008,"Lighting and audio control space 1",null,"Lighting and audio control space6","Perf arts, hall and dining",6,null,null,null,-6,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,-6,null,null,null,null,null,null,null,"New Build"]
["SEN02","SEN02",3009,"Medical treatment (MI) room 1",null,"Medical treatment (MI) room12","Balance",12,null,null,null,-12,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,null,-12,null,null,null,null,null,null,null,"New Build"]
["SEN20","SEN20",3010,"SEN resource space 1",null,"SEN resource space16","Balance",16,null,null,null,-16,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,null,null,null,-16,null,null,null,null,null,null,null,"New Build"]
["RES00","RES00",3011,"Small group room 1",null,"Small group room9","Balance",9,null,null,null,-9,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,null,null,null,-9,null,null,null,null,null,null,null,"New Build"]
["RES00","RES00",3012,"Small group room 2",null,"Small group room9","Balance",9,null,null,null,-9,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,null,null,null,-9,null,null,null,null,null,null,null,"New Build"]
["RES00","RES00",3013,"Small group room 3",null,"Small group room9","Balance",9,null,null,null,-9,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,null,null,null,-9,null,null,null,null,null,null,null,"New Build"]
["RES00","RES00",3014,"Small group room 4",null,"Small group room9","Balance",9,null,null,null,-9,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,null,null,null,-9,null,null,null,null,null,null,null,"New Build"]
["RES00","RES04",3015,"Small group room (large SEN etc.) 1",null,"Small group room (large SEN etc.)16","Balance",16,null,null,null,-16,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,null,null,null,-16,null,null,null,null,null,null,null,"New Build"]
[null,null,null,null,"Learning Resources Total : ",null,null,353,null,null,0,-353,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,353,null,null,0,-353]
["OFF30","OFF33",4001,"Staff workrooms (teaching staff) 1",null,"Staff workrooms (teaching staff)19","Mathematics",19,null,null,null,-19,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,null,null,null,-19,null,null,null,null,null,null,null,"New Build"]
["OFF30","OFF33",4002,"Staff workrooms (teaching staff) 2",null,"Staff workrooms (teaching staff)19","English",19,null,null,null,-19,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,null,null,null,-19,null,null,null,null,null,null,null,"New Build"]
["OFF30","OFF33",4003,"Staff workrooms (teaching staff) 3",null,"Staff workrooms (teaching staff)19","MFL",19,null,null,null,-19,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,null,null,null,-19,null,null,null,null,null,null,null,"New Build"]
["OFF30","OFF33",4004,"Staff workrooms (teaching staff) 4",null,"Staff workrooms (teaching staff)19","Science",19,null,null,null,-19,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,null,null,null,-19,null,null,null,null,null,null,null,"New Build"]
["OFF30","OFF33",4005,"Staff workrooms (teaching staff) 5",null,"Staff workrooms (teaching staff)19","DT/ Art",19,null,null,null,-19,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,null,null,null,-19,null,null,null,null,null,null,null,"New Build"]
["OFF30","OFF32",4006,"Staff workrooms (smaller teaching team) 1",null,"Staff workrooms (smaller teaching team)15","ICT and Business Studies",15,null,null,null,-15,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,null,null,-15,null,null,null,null,null,null,null,"New Build"]
["OFF30","OFF32",4007,"Staff workrooms (smaller teaching team) 2",null,"Staff workrooms (smaller teaching team)15","Humanities",15,null,null,null,-15,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,null,null,-15,null,null,null,null,null,null,null,"New Build"]
["OFF30","OFF32",4008,"Staff workrooms (smaller teaching team) 3",null,"Staff workrooms (smaller teaching team)15","Perf arts, hall and dining",15,null,null,null,-15,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,null,null,-15,null,null,null,null,null,null,null,"New Build"]
["OFF50","OFF52",4009,"Staff room (social) 1",null,"Staff room (social)41","Admin",41,null,null,null,-41,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41,null,null,null,-41,null,null,null,null,null,null,null,"New Build"]
["OFF40","OFF40",4010,"Meeting room (conference) 1",null,"Meeting room (conference)19","Admin",19,null,null,null,-19,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,null,null,null,-19,null,null,null,null,null,null,null,"New Build"]
["ADM32","ADM32",4011,"Reception area, community (50% circulation) 1",null,"Reception area, community (50% circulation)8","Sports/ PE",8,null,null,null,-8,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,-8,null,null,null,null,null,null,null,"New Build"]
["ADM22","ADM22",4012,"Kitchenette, bay 1",null,"Kitchenette, bay3","Admin",3,null,null,null,-3,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,-3,null,null,null,null,null,null,null,"New Build"]
["ADM22","ADM22",4013,"Kitchenette, bay 2",null,"Kitchenette, bay3","Admin",3,null,null,null,-3,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,-3,null,null,null,null,null,null,null,"New Build"]
["ADM22","ADM22",4014,"Kitchenette, bay 3",null,"Kitchenette, bay3","Admin",3,null,null,null,-3,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,-3,null,null,null,null,null,null,null,"New Build"]
["ADM22","ADM22",4015,"Kitchenette, bay 4",null,"Kitchenette, bay3","Admin",3,null,null,null,-3,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,-3,null,null,null,null,null,null,null,"New Build"]
["ADM22","ADM22",4016,"Kitchenette, bay 5",null,"Kitchenette, bay3","Admin",3,null,null,null,-3,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,-3,null,null,null,null,null,null,null,"New Build"]
["ADM10","ADM11",4017,"Enclosed office, admin (head) 1",null,"Enclosed office, admin (head)16","Admin",16,null,null,null,-16,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,null,null,null,-16,null,null,null,null,null,null,null,"New Build"]
["ADM10","ADM13",4018,"Enclosed office, admin (PA) 1",null,"Enclosed office, admin (PA)8","Admin",8,null,null,null,-8,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,-8,null,null,null,null,null,null,null,"New Build"]
["ADM08","ADM08",4019,"Reprographics room 1",null,"Reprographics room20","Admin",20,null,null,null,-20,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,null,null,null,-20,null,null,null,null,null,null,null,"New Build"]
["ADM05","ADM07",4020,"Enclosed office, with recep desk (and window) 1",null,"Enclosed office, with recep desk (and window)41","Admin",41,null,null,null,-41,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41,null,null,null,-41,null,null,null,null,null,null,null,"New Build"]
["ADM31","ADM31",4021,"Reception area, entrance (50% circulation) 1",null,"Reception area, entrance (50% circulation)24","Admin",24,null,null,null,-24,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,24,null,null,null,-24,null,null,null,null,null,null,null,"New Build"]
["ADM02","ADM02",4022,"Confidential meeting room (interview) 1",null,"Confidential meeting room (interview)6","Admin",6,null,null,null,-6,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,-6,null,null,null,null,null,null,null,"New Build"]
["ADM03","ADM03",4023,"First aid post (sick bay) 1",null,"First aid post (sick bay)6","Admin",6,null,null,null,-6,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,-6,null,null,null,null,null,null,null,"New Build"]
["OFF00","OFF01",4024,"Office (1-person) 1",null,"Office (1-person)7","Balance",7,null,null,null,-7,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,null,null,null,-7,null,null,null,null,null,null,null,"New Build"]
["OFF00","OFF01",4025,"Office (1-person) 2",null,"Office (1-person)7","Balance",7,null,null,null,-7,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,null,null,null,-7,null,null,null,null,null,null,null,"New Build"]
["OFF00","OFF01",4026,"Office (1-person) 3",null,"Office (1-person)7","Balance",7,null,null,null,-7,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,null,null,null,-7,null,null,null,null,null,null,null,"New Build"]
["OFF00","OFF01",4027,"Office (1-person) 4",null,"Office (1-person)7","Balance",7,null,null,null,-7,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,null,null,null,-7,null,null,null,null,null,null,null,"New Build"]
["OFF00","OFF01",4028,"Office (1-person) 5",null,"Office (1-person)7","Balance",7,null,null,null,-7,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,null,null,null,-7,null,null,null,null,null,null,null,"New Build"]
["OFF00","OFF11",4029,"Office (with meeting area, 1-person) 1",null,"Office (with meeting area, 1-person)9","Balance",9,null,null,null,-9,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,null,null,null,-9,null,null,null,null,null,null,null,"New Build"]
["OFF00","OFF11",4030,"Office (with meeting area, 1-person) 2",null,"Office (with meeting area, 1-person)9","Balance",9,null,null,null,-9,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,null,null,null,-9,null,null,null,null,null,null,null,"New Build"]
["OFF00","OFF11",4031,"Office (with meeting area, 1-person) 3",null,"Office (with meeting area, 1-person)9","Balance",9,null,null,null,-9,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,null,null,null,-9,null,null,null,null,null,null,null,"New Build"]
["OFF00","OFF11",4032,"Office (with meeting area, 1-person) 4",null,"Office (with meeting area, 1-person)9","Balance",9,null,null,null,-9,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,null,null,null,-9,null,null,null,null,null,null,null,"New Build"]
["OFF00","OFF11",4033,"Office (with meeting area, 1-person) 5",null,"Office (with meeting area, 1-person)9","Balance",9,null,null,null,-9,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,null,null,null,-9,null,null,null,null,null,null,null,"New Build"]
["OFF00","OFF11",4034,"Office (with meeting area, 1-person) 6",null,"Office (with meeting area, 1-person)9","Balance",9,null,null,null,-9,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,null,null,null,-9,null,null,null,null,null,null,null,"New Build"]
["OFF00","OFF11",4035,"Office (with meeting area, 1-person) 7",null,"Office (with meeting area, 1-person)9","Balance",9,null,null,null,-9,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,null,null,null,-9,null,null,null,null,null,null,null,"New Build"]
["OFF00","OFF11",4036,"Office (with meeting area, 1-person) 8",null,"Office (with meeting area, 1-person)9","Balance",9,null,null,null,-9,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,null,null,null,-9,null,null,null,null,null,null,null,"New Build"]
["OFF00","OFF06",4037,"Office (exams) 1",null,"Office (exams)9","-",9,null,null,null,-9,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,null,null,null,-9,null,null,null,null,null,null,null,"New Build"]
["OFF00","OFF23",4038,"Office (SENco, learning support) 1",null,"Office (SENco, learning support)11","-",11,null,null,null,-11,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11,null,null,null,-11,null,null,null,null,null,null,null,"New Build"]
["OFF30","OFF37",4039,"Staff workroom (ICT technicians) 1",null,"Staff workroom (ICT technicians)11","Balance",11,null,null,null,-11,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11,null,null,null,-11,null,null,null,null,null,null,null,"New Build"]
["OFF30","OFF38",4040,"Staff workroom (premises) 1",null,"Staff workroom (premises)11","Balance",11,null,null,null,-11,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11,null,null,null,-11,null,null,null,null,null,null,null,"New Build"]
[null,null,null,null,"Staff Spaces Total : ",null,null,493,null,null,0,-493,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,493,null,null,0,-493]
["STT10","STT13",5001,"Teaching resources store (IT/ GT off corridor) 1",null,"Teaching resources store (IT/ GT off corridor)5","Mathematics",5,null,null,null,-5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,-5,null,null,null,null,null,null,null,"New Build"]
["STT10","STT13",5002,"Teaching resources store (IT/ GT off corridor) 2",null,"Teaching resources store (IT/ GT off corridor)5","English",5,null,null,null,-5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,-5,null,null,null,null,null,null,null,"New Build"]
["STT10","STT13",5003,"Teaching resources store (IT/ GT off corridor) 3",null,"Teaching resources store (IT/ GT off corridor)5","MFL",5,null,null,null,-5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,-5,null,null,null,null,null,null,null,"New Build"]
["STT10","STT13",5004,"Teaching resources store (IT/ GT off corridor) 4",null,"Teaching resources store (IT/ GT off corridor)5","ICT and Business Studies",5,null,null,null,-5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,-5,null,null,null,null,null,null,null,"New Build"]
["STT10","STT13",5005,"Teaching resources store (IT/ GT off corridor) 5",null,"Teaching resources store (IT/ GT off corridor)5","Humanities",5,null,null,null,-5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,-5,null,null,null,null,null,null,null,"New Build"]
["STT10","STT13",5006,"Teaching resources store (IT/ GT off corridor) 6",null,"Teaching resources store (IT/ GT off corridor)5","Humanities",5,null,null,null,-5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,-5,null,null,null,null,null,null,null,"New Build"]
["STT20","STT21",5007,"Science prep room (central) 1",null,"Science prep room (central)111","Science",111,null,null,null,-111,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,111,null,null,null,-111,null,null,null,null,null,null,null,"New Build"]
["STT23","STT23",5008,"Chemicals store, science 1",null,"Chemicals store, science7","Science",7,null,null,null,-7,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,null,null,null,-7,null,null,null,null,null,null,null,"New Build"]
["STT10","STT16",5009,"Teaching resources store (off art room) 1",null,"Teaching resources store (off art room)5","DT/ Art",5,null,null,null,-5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,-5,null,null,null,null,null,null,null,"New Build"]
["STT10","STT16",5010,"Teaching resources store (off art room) 2",null,"Teaching resources store (off art room)5","DT/ Art",5,null,null,null,-5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,-5,null,null,null,null,null,null,null,"New Build"]
["STT10","STT16",5011,"Teaching resources store (off art room) 3",null,"Teaching resources store (off art room)5","DT/ Art",5,null,null,null,-5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,-5,null,null,null,null,null,null,null,"New Build"]
["STT10","STT16",5012,"Teaching resources store (off art room) 4",null,"Teaching resources store (off art room)5","DT/ Art",5,null,null,null,-5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,-5,null,null,null,null,null,null,null,"New Build"]
["STT10","STT16",5013,"Teaching resources store (off art room) 5",null,"Teaching resources store (off art room)5","DT/ Art",5,null,null,null,-5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,-5,null,null,null,null,null,null,null,"New Build"]
["STT10","STT16",5014,"Teaching resources store (off art room) 6",null,"Teaching resources store (off art room)5","DT/ Art",5,null,null,null,-5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,-5,null,null,null,null,null,null,null,"New Build"]
["STT32","STT32",5015,"DT prep room 1",null,"DT prep room34","DT/ Art",34,null,null,null,-34,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,34,null,null,null,-34,null,null,null,null,null,null,null,"New Build"]
["STT34","STT34",5016,"Food prep room 1",null,"Food prep room10","DT/ Art",10,null,null,null,-10,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,null,null,null,-10,null,null,null,null,null,null,null,"New Build"]
["STT10","STT18",5017,"Teaching resources store (off DT studio) 1",null,"Teaching resources store (off DT studio)5","DT/ Art",5,null,null,null,-5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,-5,null,null,null,null,null,null,null,"New Build"]
["STT10","STT18",5018,"Teaching resources store (off DT studio) 2",null,"Teaching resources store (off DT studio)5","DT/ Art",5,null,null,null,-5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,-5,null,null,null,null,null,null,null,"New Build"]
["STT10","STT18",5019,"Teaching resources store (off DT studio) 3",null,"Teaching resources store (off DT studio)5","DT/ Art",5,null,null,null,-5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,-5,null,null,null,null,null,null,null,"New Build"]
["STT10","STT18",5020,"Teaching resources store (off DT studio) 4",null,"Teaching resources store (off DT studio)5","DT/ Art",5,null,null,null,-5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,-5,null,null,null,null,null,null,null,"New Build"]
["STT10","STT17",5021,"Teaching resources store (music) 1",null,"Teaching resources store (music)5","Perf arts, hall and dining",5,null,null,null,-5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,-5,null,null,null,null,null,null,null,"New Build"]
["STT10","STT17",5022,"Teaching resources store (music) 2",null,"Teaching resources store (music)5","Perf arts, hall and dining",5,null,null,null,-5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,-5,null,null,null,null,null,null,null,"New Build"]
["STT08","STT08",5023,"Equipment store, drama 1",null,"Equipment store, drama10","Perf arts, hall and dining",10,null,null,null,-10,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,null,null,null,-10,null,null,null,null,null,null,null,"New Build"]
["STT10","STT41",5024,"Teaching resources store, room (off LRC) 1",null,"Teaching resources store, room (off LRC)3","Balance",3,null,null,null,-3,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,-3,null,null,null,null,null,null,null,"New Build"]
["STT00","STT42",5025,"Classroom store, room (off SEN room) 1",null,"Classroom store, room (off SEN room)5","Balance",5,null,null,null,-5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,-5,null,null,null,null,null,null,null,"New Build"]
["STH00","STH01",5026,"Sports equipment store, internal (sports hall) 1",null,"Sports equipment store, internal (sports hall)60","Sports/ PE",60,null,null,null,-60,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60,null,null,null,-60,null,null,null,null,null,null,null,"New Build"]
["STH00","STH02",5027,"Sports equipment store, internal (community) 1",null,"Sports equipment store, internal (community)4","Sports/ PE",4,null,null,null,-4,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,-4,null,null,null,null,null,null,null,"New Build"]
["STH00","STH03",5028,"Sports equipment store, internal (activity studio) 1",null,"Sports equipment store, internal (activity studio)15","Sports/ PE",15,null,null,null,-15,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,null,null,-15,null,null,null,null,null,null,null,"New Build"]
["STH05","STH05",5029,"Sports equipment store, external 1",null,"Sports equipment store, external8","Sports/ PE",8,null,null,null,-8,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,-8,null,null,null,null,null,null,null,"New Build"]
[null,null,null,null,"Teaching Storage Total : ",null,null,357,null,null,0,-357,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,357,null,null,0,-357]
["STH10","STH11",5101,"Furniture store (chair/ table, off hall) 1",null,"Furniture store (chair/ table, off hall)20","Perf arts, hall and dining",20,null,null,null,-20,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,null,null,null,-20,null,null,null,null,null,null,null,"New Build"]
["STN20","STN22",5102,"General storeroom (central stock) 1",null,"General storeroom (central stock)6","Balance",6,null,null,null,-6,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,-6,null,null,null,null,null,null,null,"New Build"]
["STN20","STN22",5103,"General storeroom (central stock) 2",null,"General storeroom (central stock)6","Balance",6,null,null,null,-6,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,-6,null,null,null,null,null,null,null,"New Build"]
["STN50","STN50",5104,"Secure storeroom 1",null,"Secure storeroom8","Admin",8,null,null,null,-8,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,-8,null,null,null,null,null,null,null,"New Build"]
["STN50","STN50",5105,"Secure storeroom 2",null,"Secure storeroom8","Admin",8,null,null,null,-8,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,-8,null,null,null,null,null,null,null,"New Build"]
["CIR06","CIR06",5106,"Equipment store, appliance bay 1",null,"Equipment store, appliance bay1.5","Balance",1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build"]
["CIR06","CIR06",5107,"Equipment store, appliance bay 2",null,"Equipment store, appliance bay1.5","Balance",1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build"]
["CIR06","CIR06",5108,"Equipment store, appliance bay 3",null,"Equipment store, appliance bay1.5","Balance",1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build"]
["CIR06","CIR06",5109,"Equipment store, appliance bay 4",null,"Equipment store, appliance bay1.5","Balance",1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build"]
["STH20","STH20",5110,"Retractable seating storage (off hall) 1",null,"Retractable seating storage (off hall)16","Perf arts, hall and dining",16,null,null,null,-16,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,null,null,null,-16,null,null,null,null,null,null,null,"New Build"]
["STN00","STN02",5111,"Coats and bag store (lockers) 1",null,"Coats and bag store (lockers)10","Mathematics",10,null,null,null,-10,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,null,null,null,-10,null,null,null,null,null,null,null,"New Build"]
["STN00","STN02",5112,"Coats and bag store (lockers) 2",null,"Coats and bag store (lockers)10","English",10,null,null,null,-10,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,null,null,null,-10,null,null,null,null,null,null,null,"New Build"]
["STN00","STN02",5113,"Coats and bag store (lockers) 3",null,"Coats and bag store (lockers)10","MFL",10,null,null,null,-10,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,null,null,null,-10,null,null,null,null,null,null,null,"New Build"]
["STN00","STN02",5114,"Coats and bag store (lockers) 4",null,"Coats and bag store (lockers)10","ICT and Business Studies",10,null,null,null,-10,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,null,null,null,-10,null,null,null,null,null,null,null,"New Build"]
["STN00","STN02",5115,"Coats and bag store (lockers) 5",null,"Coats and bag store (lockers)10","Humanities",10,null,null,null,-10,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,null,null,null,-10,null,null,null,null,null,null,null,"New Build"]
["STN00","STN02",5116,"Coats and bag store (lockers) 6",null,"Coats and bag store (lockers)10","Science",10,null,null,null,-10,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,null,null,null,-10,null,null,null,null,null,null,null,"New Build"]
["STN00","STN03",5117,"Coats and bag store (community lockers) 1",null,"Coats and bag store (community lockers)3","Sports/ PE",3,null,null,null,-3,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,-3,null,null,null,null,null,null,null,"New Build"]
["STN31","STN31",5118,"Cleaners' store 1",null,"Cleaners' store1.5","Balance",1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build"]
["STN31","STN31",5119,"Cleaners' store 2",null,"Cleaners' store1.5","Balance",1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build"]
["STN31","STN31",5120,"Cleaners' store 3",null,"Cleaners' store1.5","Balance",1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build"]
["STN31","STN31",5121,"Cleaners' store 4",null,"Cleaners' store1.5","Balance",1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build"]
["STN31","STN31",5122,"Cleaners' store 5",null,"Cleaners' store1.5","Balance",1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build"]
["STN31","STN31",5123,"Cleaners' store 6",null,"Cleaners' store1.5","Balance",1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build"]
["STN31","STN31",5124,"Cleaners' store 7",null,"Cleaners' store1.5","Balance",1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build"]
["STN31","STN31",5125,"Cleaners' store 8",null,"Cleaners' store1.5","Balance",1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,null,null,null,-1.5,null,null,null,null,null,null,null,"New Build"]
["STN32","STN32",5126,"Equipment store, maintenance 1",null,"Equipment store, maintenance8","Balance",8,null,null,null,-8,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,-8,null,null,null,null,null,null,null,"New Build"]
[null,null,null,null,"Non Teaching Storage Total : ",null,null,153,null,null,0,-153,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,153,null,null,0,-153]
["KIT00","KIT01",6001,"Food prep area, kitchen (servery & wash-up) 1",null,"Food prep area, kitchen (servery & wash-up)97","Perf arts, hall and dining",97,null,null,null,-97,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,97,null,null,null,-97,null,null,null,null,null,null,null,"New Build"]
["KIT11","KIT11",6002,"Office, kitchen 1",null,"Office, kitchen4","Perf arts, hall and dining",4,null,null,null,-4,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,-4,null,null,null,null,null,null,null,"New Build"]
["KIT20","KIT21",6003,"Food store, kitchen (dry) 1",null,"Food store, kitchen (dry)5","Perf arts, hall and dining",5,null,null,null,-5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,-5,null,null,null,null,null,null,null,"New Build"]
["KIT25","KIT25",6004,"Cold store, kitchen 1",null,"Cold store, kitchen4.5","Perf arts, hall and dining",4.5,null,null,null,-4.5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.5,null,null,null,-4.5,null,null,null,null,null,null,null,"New Build"]
["KIT25","KIT26",6005,"Cold store, kitchen (freezer) 1",null,"Cold store, kitchen (freezer)3.5","Perf arts, hall and dining",3.5,null,null,null,-3.5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.5,null,null,null,-3.5,null,null,null,null,null,null,null,"New Build"]
["KIT40","KIT40",6006,"Toilet, kitchen (with changing area) 1",null,"Toilet, kitchen (with changing area)6.5","Perf arts, hall and dining",6.5,null,null,null,-6.5,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6.5,null,null,null,-6.5,null,null,null,null,null,null,null,"New Build"]
["TOC01","TOC01",6007,"Changing room, with showers (pupils) 1",null,"Changing room, with showers (pupils)64","Sports/ PE",64,null,null,null,-64,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,64,null,null,null,-64,null,null,null,null,null,null,null,"New Build"]
["TOC01","TOC01",6008,"Changing room, with showers (pupils) 2",null,"Changing room, with showers (pupils)64","Sports/ PE",64,null,null,null,-64,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,64,null,null,null,-64,null,null,null,null,null,null,null,"New Build"]
["TOC02","TOC02",6009,"Accessible (and staff) changing room 1",null,"Accessible (and staff) changing room6","Sports/ PE",6,null,null,null,-6,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,-6,null,null,null,null,null,null,null,"New Build"]
["TOC02","TOC02",6010,"Accessible (and staff) changing room 2",null,"Accessible (and staff) changing room6","Sports/ PE",6,null,null,null,-6,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,-6,null,null,null,null,null,null,null,"New Build"]
["TOC04","TOC04",6011,"Hygiene room 1",null,"Hygiene room12","Balance",12,null,null,null,-12,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,null,-12,null,null,null,null,null,null,null,"New Build"]
["TOC10","TOC13",6012,"Toilets, suite (pupils) 1",null,"Toilets, suite (pupils)26","Balance",26,null,null,null,-26,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,null,null,null,-26,null,null,null,null,null,null,null,"New Build"]
["TOC10","TOC13",6013,"Toilets, suite (pupils) 2",null,"Toilets, suite (pupils)26","Balance",26,null,null,null,-26,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,null,null,null,-26,null,null,null,null,null,null,null,"New Build"]
["TOC10","TOC13",6014,"Toilets, suite (pupils) 3",null,"Toilets, suite (pupils)26","Balance",26,null,null,null,-26,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,null,null,null,-26,null,null,null,null,null,null,null,"New Build"]
["TOC10","TOC13",6015,"Toilets, suite (pupils) 4",null,"Toilets, suite (pupils)26","Balance",26,null,null,null,-26,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,null,null,null,-26,null,null,null,null,null,null,null,"New Build"]
["TOC10","TOC13",6016,"Toilets, suite (pupils) 5",null,"Toilets, suite (pupils)26","Balance",26,null,null,null,-26,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,null,null,null,-26,null,null,null,null,null,null,null,"New Build"]
["TOC10","TOC13",6017,"Toilets, suite (pupils) 6",null,"Toilets, suite (pupils)26","Balance",26,null,null,null,-26,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,null,null,null,-26,null,null,null,null,null,null,null,"New Build"]
["TOC10","TOC14",6018,"Toilets, suite (pupils, other) 1",null,"Toilets, suite (pupils, other)6","Sports/ PE",6,null,null,null,-6,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,-6,null,null,null,null,null,null,null,"New Build"]
["TOC10","TOC14",6019,"Toilets, suite (pupils, other) 2",null,"Toilets, suite (pupils, other)6","Sports/ PE",6,null,null,null,-6,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,-6,null,null,null,null,null,null,null,"New Build"]
["TOC10","TOC14",6020,"Toilets, suite (pupils, other) 3",null,"Toilets, suite (pupils, other)6","Balance",6,null,null,null,-6,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,-6,null,null,null,null,null,null,null,"New Build"]
["TOC15","TOC15",6021,"Toilet, individual (pupil) 1",null,"Toilet, individual (pupil)2","Balance",2,null,null,null,-2,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,-2,null,null,null,null,null,null,null,"New Build"]
["TOC15","TOC15",6022,"Toilet, individual (pupil) 2",null,"Toilet, individual (pupil)2","Balance",2,null,null,null,-2,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,-2,null,null,null,null,null,null,null,"New Build"]
["TOC15","TOC15",6023,"Toilet, individual (pupil) 3",null,"Toilet, individual (pupil)2","Balance",2,null,null,null,-2,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,-2,null,null,null,null,null,null,null,"New Build"]
["TOC10","TOC12",6024,"Toilets, suite (staff) 1",null,"Toilets, suite (staff)6","Admin",6,null,null,null,-6,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,-6,null,null,null,null,null,null,null,"New Build"]
["TOC10","TOC12",6025,"Toilets, suite (staff) 2",null,"Toilets, suite (staff)6","Admin",6,null,null,null,-6,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,-6,null,null,null,null,null,null,null,"New Build"]
["TOC21","TOC21",6026,"Accessible (and staff) toilet 1",null,"Accessible (and staff) toilet3.8","Balance",3.8,null,null,null,-3.8,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.8,null,null,null,-3.8,null,null,null,null,null,null,null,"New Build"]
["TOC21","TOC21",6027,"Accessible (and staff) toilet 2",null,"Accessible (and staff) toilet3.8","Balance",3.8,null,null,null,-3.8,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.8,null,null,null,-3.8,null,null,null,null,null,null,null,"New Build"]
["TOC21","TOC21",6028,"Accessible (and staff) toilet 3",null,"Accessible (and staff) toilet3.8","Balance",3.8,null,null,null,-3.8,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.8,null,null,null,-3.8,null,null,null,null,null,null,null,"New Build"]
["TOC21","TOC21",6029,"Accessible (and staff) toilet 4",null,"Accessible (and staff) toilet3.8","Balance",3.8,null,null,null,-3.8,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.8,null,null,null,-3.8,null,null,null,null,null,null,null,"New Build"]
["TOC21","TOC21",6030,"Accessible (and staff) toilet 5",null,"Accessible (and staff) toilet3.8","Balance",3.8,null,null,null,-3.8,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.8,null,null,null,-3.8,null,null,null,null,null,null,null,"New Build"]
["PLA10","PLA14",6031,"Server room (4-cabinet) 1",null,"Server room (4-cabinet)15.6","Balance",15.6,null,null,null,-15.6,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15.6,null,null,null,-15.6,null,null,null,null,null,null,null,"New Build"]
["PLA20","PLA21",6032,"Plant room (heat source) 1",null,"Plant room (heat source)32","Balance",32,null,null,null,-32,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,32,null,null,null,-32,null,null,null,null,null,null,null,"New Build"]
["PLA20","PLA23",6033,"Plant room (cold water tanks) 1",null,"Plant room (cold water tanks)28","Balance",28,null,null,null,-28,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,28,null,null,null,-28,null,null,null,null,null,null,null,"New Build"]
["PLA20","PLA25",6034,"Plant room (electrical intake) 1",null,"Plant room (electrical intake)28","Balance",28,null,null,null,-28,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,28,null,null,null,-28,null,null,null,null,null,null,null,"New Build"]
["PLA43","PLA43",6035,"Services shaft (enclosed electrical) 1",null,"Services shaft (enclosed electrical)1","Balance",1,null,null,null,-1,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,-1,null,null,null,null,null,null,null,"New Build"]
["PLA43","PLA43",6036,"Services shaft (enclosed electrical) 2",null,"Services shaft (enclosed electrical)1","Balance",1,null,null,null,-1,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,-1,null,null,null,null,null,null,null,"New Build"]
["PLA43","PLA43",6037,"Services shaft (enclosed electrical) 3",null,"Services shaft (enclosed electrical)1","Balance",1,null,null,null,-1,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,-1,null,null,null,null,null,null,null,"New Build"]
["PLA43","PLA43",6038,"Services shaft (enclosed electrical) 4",null,"Services shaft (enclosed electrical)1","Balance",1,null,null,null,-1,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,-1,null,null,null,null,null,null,null,"New Build"]
["PLA43","PLA43",6039,"Services shaft (enclosed electrical) 5",null,"Services shaft (enclosed electrical)1","Balance",1,null,null,null,-1,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,-1,null,null,null,null,null,null,null,"New Build"]
["PLA43","PLA43",6040,"Services shaft (enclosed electrical) 6",null,"Services shaft (enclosed electrical)1","Balance",1,null,null,null,-1,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,-1,null,null,null,null,null,null,null,"New Build"]
["PLA43","PLA43",6041,"Services shaft (enclosed electrical) 7",null,"Services shaft (enclosed electrical)1","Balance",1,null,null,null,-1,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,-1,null,null,null,null,null,null,null,"New Build"]
["PLA43","PLA43",6042,"Services shaft (enclosed electrical) 8",null,"Services shaft (enclosed electrical)1","Balance",1,null,null,null,-1,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,-1,null,null,null,null,null,null,null,"New Build"]
["PLA43","PLA43",6043,"Services shaft (enclosed electrical) 9",null,"Services shaft (enclosed electrical)1","Balance",1,null,null,null,-1,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,-1,null,null,null,null,null,null,null,"New Build"]
["PLA43","PLA43",6044,"Services shaft (enclosed electrical) 10",null,"Services shaft (enclosed electrical)1","Balance",1,null,null,null,-1,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,-1,null,null,null,null,null,null,null,"New Build"]
["PLA43","PLA43",6045,"Services shaft (enclosed electrical) 11",null,"Services shaft (enclosed electrical)1","Balance",1,null,null,null,-1,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,-1,null,null,null,null,null,null,null,"New Build"]
["PLA43","PLA43",6046,"Services shaft (enclosed electrical) 12",null,"Services shaft (enclosed electrical)1","Balance",1,null,null,null,-1,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,-1,null,null,null,null,null,null,null,"New Build"]
["PLA43","PLA43",6047,"Services shaft (enclosed electrical) 13",null,"Services shaft (enclosed electrical)1","Balance",1,null,null,null,-1,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,-1,null,null,null,null,null,null,null,"New Build"]
["PLA43","PLA43",6048,"Services shaft (enclosed electrical) 14",null,"Services shaft (enclosed electrical)1","Balance",1,null,null,null,-1,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,-1,null,null,null,null,null,null,null,"New Build"]
["PLA43","PLA43",6049,"Services shaft (enclosed electrical) 15",null,"Services shaft (enclosed electrical)1","Balance",1,null,null,null,-1,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,-1,null,null,null,null,null,null,null,"New Build"]
["PLA43","PLA43",6050,"Services shaft (enclosed electrical) 16",null,"Services shaft (enclosed electrical)1","Balance",1,null,null,null,-1,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,-1,null,null,null,null,null,null,null,"New Build"]
["PLA43","PLA43",6051,"Services shaft (enclosed electrical) 17",null,"Services shaft (enclosed electrical)1","Balance",1,null,null,null,-1,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,-1,null,null,null,null,null,null,null,"New Build"]
["PLA43","PLA43",6052,"Services shaft (enclosed electrical) 18",null,"Services shaft (enclosed electrical)1","Balance",1,null,null,null,-1,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,-1,null,null,null,null,null,null,null,"New Build"]
["PLA43","PLA43",6053,"Services shaft (enclosed electrical) 19",null,"Services shaft (enclosed electrical)1","Balance",1,null,null,null,-1,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,-1,null,null,null,null,null,null,null,"New Build"]
["PLA43","PLA43",6054,"Services shaft (enclosed electrical) 20",null,"Services shaft (enclosed electrical)1","Balance",1,null,null,null,-1,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,-1,null,null,null,null,null,null,null,"New Build"]
["CIR12","CIR12",6055,"Stairway 1",null,"Stairway324","Balance",27,null,null,null,-27,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,null,null,null,-27,null,null,null,null,null,null,null,"New Build"]
["CIR12","CIR12",6056,"Stairway 2",null,"Stairway324","Balance",27,null,null,null,-27,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,null,null,null,-27,null,null,null,null,null,null,null,"New Build"]
["CIR12","CIR12",6057,"Stairway 3",null,"Stairway324","Balance",27,null,null,null,-27,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,null,null,null,-27,null,null,null,null,null,null,null,"New Build"]
["CIR12","CIR12",6058,"Stairway 4",null,"Stairway324","Balance",27,null,null,null,-27,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,null,null,null,-27,null,null,null,null,null,null,null,"New Build"]
["CIR12","CIR12",6059,"Stairway 5",null,"Stairway324","Balance",27,null,null,null,-27,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,null,null,null,-27,null,null,null,null,null,null,null,"New Build"]
["CIR12","CIR12",6060,"Stairway 6",null,"Stairway324","Balance",27,null,null,null,-27,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,null,null,null,-27,null,null,null,null,null,null,null,"New Build"]
["CIR12","CIR12",6061,"Stairway 7",null,"Stairway324","Balance",27,null,null,null,-27,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,null,null,null,-27,null,null,null,null,null,null,null,"New Build"]
["CIR12","CIR12",6062,"Stairway 8",null,"Stairway324","Balance",27,null,null,null,-27,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,null,null,null,-27,null,null,null,null,null,null,null,"New Build"]
["CIR12","CIR12",6063,"Stairway 9",null,"Stairway324","Balance",27,null,null,null,-27,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,null,null,null,-27,null,null,null,null,null,null,null,"New Build"]
["CIR12","CIR12",6064,"Stairway 10",null,"Stairway324","Balance",27,null,null,null,-27,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,null,null,null,-27,null,null,null,null,null,null,null,"New Build"]
["CIR12","CIR12",6065,"Stairway 11",null,"Stairway324","Balance",27,null,null,null,-27,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,null,null,null,-27,null,null,null,null,null,null,null,"New Build"]
["CIR12","CIR12",6066,"Stairway 12",null,"Stairway324","Balance",27,null,null,null,-27,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,null,null,null,-27,null,null,null,null,null,null,null,"New Build"]
["CIR13","CIR13",6067,"Lift 1",null,"Lift36","Balance",6,null,null,null,-6,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,-6,null,null,null,null,null,null,null,"New Build"]
["CIR13","CIR13",6068,"Lift 2",null,"Lift36","Balance",6,null,null,null,-6,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,-6,null,null,null,null,null,null,null,"New Build"]
["CIR13","CIR13",6069,"Lift 3",null,"Lift36","Balance",6,null,null,null,-6,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,-6,null,null,null,null,null,null,null,"New Build"]
["CIR13","CIR13",6070,"Lift 4",null,"Lift36","Balance",6,null,null,null,-6,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,-6,null,null,null,null,null,null,null,"New Build"]
["CIR13","CIR13",6071,"Lift 5",null,"Lift36","Balance",6,null,null,null,-6,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,-6,null,null,null,null,null,null,null,"New Build"]
["CIR13","CIR13",6072,"Lift 6",null,"Lift36","Balance",6,null,null,null,-6,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,-6,null,null,null,null,null,null,null,"New Build"]
["CIR03","CIR03",6073,"Lobby 1",null,"Lobby12","Balance",6,null,null,null,-6,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,-6,null,null,null,null,null,null,null,"New Build"]
["CIR03","CIR03",6074,"Lobby 2",null,"Lobby12","Balance",6,null,null,null,-6,null,null,null,null,null,null,null,"New Build",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,-6,null,null,null,null,null,null,null,"New Build"]
[null,null,null,null,"Non-Net Total (except horizontal circulation or partitions) : ",null,null,{"$f":"SUM(INDIRECT(ADDRESS(ROW()-74,COLUMN())):INDIRECT(ADDRESS(ROW()-1,COLUMN())))","v":979.10000000000014},null,null,{"$f":"SUM(INDIRECT(ADDRESS(ROW()-74,COLUMN())):INDIRECT(ADDRESS(ROW()-1,COLUMN())))","v":0},{"$f":"SUM(INDIRECT(ADDRESS(ROW()-74,COLUMN())):INDIRECT(ADDRESS(ROW()-1,COLUMN())))","v":-979.10000000000014},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,979.10000000000014,null,null,0,-979.10000000000014]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Unallocated Spaces"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Keep",101,"classroom","$EY$9"]

{"sheet":"Project SoA","index":9,"n_rows":300,"n_cols":34,"rows_kept":300,"cut":false,"hidden":false,"merged":[]}
[null,null,1,2,3,4,null,null,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30]
["ADS cell reference",null,"$J$6","$H$6","$Q$6","$S$6","$J$10","$J$8","$H$8","$H$20",null,null,"$Q$20",null,"$Q$14","$Q$8","$H$10",null,null,null,null,"$Q$10","$H$22","$H$24","$H$26","$Q$26","$S$26","$H$12","$H$14","$H$16","$J$16","$H$18","$J$18","$H$28"]
["SCHOOL:",{"$f":"'[1]Primary SoA'!S2","v":"[Insert Project Code and Scheme Name here in title sheet]"},null,null,null,null,null,null,null,null,null,null,"CONTRACTOR :",null,null,null,"RETAINED AREAS"]
["Parent ADS Type Code","Final ADSCode","Unique Room Code","Unique room name","Contractor's room name","Contractor's room code (on drawings)","Uniclass code","Uniclass title","Suite","Required Area (m2)","Employers Notes",null,"Proposed Area (m2)","Difference","Contractors Notes","Contractors room code (on drwgs)","ER to New / Remodel / Keep","Existing Block - Room","Existing Room Name","cell location on Primary SoA",null,"CP to New / Remodel / Keep","Maximum group size, as SOA","Number of staff workstations","ER Maximum occupancy","CP Maximum occupancy","CP Age Range (for FF&E)","Summary description","Activities to be accomodated","Area Guidelines Category","Net Capacity Category","Area Guidelines Zone","Restrictive, standard or extensive","ER Third Party Use"]
[{"$f":"'Individual Spaces'!A4","v":"CLA02"},{"$f":"'Individual Spaces'!B4","v":"CLA02"},{"$f":"'Individual Spaces'!C4","v":1001},{"$f":"'Individual Spaces'!D4","v":"Seminar room 1"},{"$f":"'Individual Spaces'!E4","v":0},null,{"$f":"VLOOKUP($B5,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_78"},{"$f":"VLOOKUP($B5,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Seminar rooms"},{"$f":"'Individual Spaces'!G4","v":"Mathematics"},{"$f":"'Individual Spaces'!H4","v":41},null,null,null,{"$f":"M5-J5","v":-41},null,null,{"$f":"'Individual Spaces'!O4","v":0},{"$f":"'Individual Spaces'!P4","v":0},{"$f":"'Individual Spaces'!Q4","v":0},{"$f":"'Individual Spaces'!R4","v":0},null,{"$f":"Q5","v":0},{"$f":"IF(AF5=\"-\",0,ROUND((J5-VLOOKUP(B5,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B5,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":22},{"$f":"IF(VLOOKUP(B5,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B5,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J5-VLOOKUP(B5,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B5,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},{"$f":"IF(W5>200,ROUND(W5*1.05,0),ROUNDUP(W5*1.1,0))","v":25},null,null,{"$f":"VLOOKUP($B5,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Seminar room for smaller 14-19 groups with a range of layout options and activities"},{"$f":"VLOOKUP($B5,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B5,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B5,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B5,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B5,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B5,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A5","v":"CLA02"},{"$f":"'Individual Spaces'!B5","v":"CLA02"},{"$f":"'Individual Spaces'!C5","v":1002},{"$f":"'Individual Spaces'!D5","v":"Seminar room 2"},{"$f":"'Individual Spaces'!E5","v":0},null,{"$f":"VLOOKUP($B6,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_78"},{"$f":"VLOOKUP($B6,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Seminar rooms"},{"$f":"'Individual Spaces'!G5","v":"English"},{"$f":"'Individual Spaces'!H5","v":41},null,null,null,{"$f":"M6-J6","v":-41},null,null,{"$f":"'Individual Spaces'!O5","v":0},{"$f":"'Individual Spaces'!P5","v":0},{"$f":"'Individual Spaces'!Q5","v":0},{"$f":"'Individual Spaces'!R5","v":0},null,{"$f":"Q6","v":0},{"$f":"IF(AF6=\"-\",0,ROUND((J6-VLOOKUP(B6,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B6,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":22},{"$f":"IF(VLOOKUP(B6,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B6,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J6-VLOOKUP(B6,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B6,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},{"$f":"IF(W6>200,ROUND(W6*1.05,0),ROUNDUP(W6*1.1,0))","v":25},null,null,{"$f":"VLOOKUP($B6,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Seminar room for smaller 14-19 groups with a range of layout options and activities"},{"$f":"VLOOKUP($B6,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B6,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B6,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B6,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B6,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B6,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A6","v":"CLA02"},{"$f":"'Individual Spaces'!B6","v":"CLA02"},{"$f":"'Individual Spaces'!C6","v":1003},{"$f":"'Individual Spaces'!D6","v":"Seminar room 3"},{"$f":"'Individual Spaces'!E6","v":0},null,{"$f":"VLOOKUP($B7,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_78"},{"$f":"VLOOKUP($B7,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Seminar rooms"},{"$f":"'Individual Spaces'!G6","v":"MFL"},{"$f":"'Individual Spaces'!H6","v":41},null,null,null,-41,null,null,{"$f":"'Individual Spaces'!O6","v":0},{"$f":"'Individual Spaces'!P6","v":0},{"$f":"'Individual Spaces'!Q6","v":0},{"$f":"'Individual Spaces'!R6","v":0},null,0,{"$f":"IF(AF7=\"-\",0,ROUND((J7-VLOOKUP(B7,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B7,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":22},{"$f":"IF(VLOOKUP(B7,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B7,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J7-VLOOKUP(B7,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B7,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},25,null,null,{"$f":"VLOOKUP($B7,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Seminar room for smaller 14-19 groups with a range of layout options and activities"},{"$f":"VLOOKUP($B7,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B7,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B7,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B7,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B7,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B7,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A7","v":"CLA12"},{"$f":"'Individual Spaces'!B7","v":"CLA12"},{"$f":"'Individual Spaces'!C7","v":1004},{"$f":"'Individual Spaces'!D7","v":"Classrooms (general) 1"},{"$f":"'Individual Spaces'!E7","v":0},null,{"$f":"VLOOKUP($B8,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B8,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G7","v":"Mathematics"},{"$f":"'Individual Spaces'!H7","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O7","v":0},{"$f":"'Individual Spaces'!P7","v":0},{"$f":"'Individual Spaces'!Q7","v":0},{"$f":"'Individual Spaces'!R7","v":0},null,0,{"$f":"IF(AF8=\"-\",0,ROUND((J8-VLOOKUP(B8,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B8,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B8,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B8,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J8-VLOOKUP(B8,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B8,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B8,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B8,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B8,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B8,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B8,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B8,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B8,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A8","v":"CLA12"},{"$f":"'Individual Spaces'!B8","v":"CLA12"},{"$f":"'Individual Spaces'!C8","v":1005},{"$f":"'Individual Spaces'!D8","v":"Classrooms (general) 2"},{"$f":"'Individual Spaces'!E8","v":0},null,{"$f":"VLOOKUP($B9,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B9,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G8","v":"Mathematics"},{"$f":"'Individual Spaces'!H8","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O8","v":0},{"$f":"'Individual Spaces'!P8","v":0},{"$f":"'Individual Spaces'!Q8","v":0},{"$f":"'Individual Spaces'!R8","v":0},null,0,{"$f":"IF(AF9=\"-\",0,ROUND((J9-VLOOKUP(B9,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B9,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B9,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B9,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J9-VLOOKUP(B9,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B9,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B9,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B9,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B9,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B9,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B9,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B9,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B9,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A9","v":"CLA12"},{"$f":"'Individual Spaces'!B9","v":"CLA12"},{"$f":"'Individual Spaces'!C9","v":1006},{"$f":"'Individual Spaces'!D9","v":"Classrooms (general) 3"},{"$f":"'Individual Spaces'!E9","v":0},null,{"$f":"VLOOKUP($B10,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B10,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G9","v":"Mathematics"},{"$f":"'Individual Spaces'!H9","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O9","v":0},{"$f":"'Individual Spaces'!P9","v":0},{"$f":"'Individual Spaces'!Q9","v":0},{"$f":"'Individual Spaces'!R9","v":0},null,0,{"$f":"IF(AF10=\"-\",0,ROUND((J10-VLOOKUP(B10,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B10,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B10,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B10,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J10-VLOOKUP(B10,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B10,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B10,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B10,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B10,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B10,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B10,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B10,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B10,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A10","v":"CLA12"},{"$f":"'Individual Spaces'!B10","v":"CLA12"},{"$f":"'Individual Spaces'!C10","v":1007},{"$f":"'Individual Spaces'!D10","v":"Classrooms (general) 4"},{"$f":"'Individual Spaces'!E10","v":0},null,{"$f":"VLOOKUP($B11,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B11,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G10","v":"Mathematics"},{"$f":"'Individual Spaces'!H10","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O10","v":0},{"$f":"'Individual Spaces'!P10","v":0},{"$f":"'Individual Spaces'!Q10","v":0},{"$f":"'Individual Spaces'!R10","v":0},null,0,{"$f":"IF(AF11=\"-\",0,ROUND((J11-VLOOKUP(B11,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B11,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B11,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B11,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J11-VLOOKUP(B11,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B11,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B11,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B11,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B11,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B11,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B11,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B11,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B11,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A11","v":"CLA12"},{"$f":"'Individual Spaces'!B11","v":"CLA12"},{"$f":"'Individual Spaces'!C11","v":1008},{"$f":"'Individual Spaces'!D11","v":"Classrooms (general) 5"},{"$f":"'Individual Spaces'!E11","v":0},null,{"$f":"VLOOKUP($B12,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B12,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G11","v":"Mathematics"},{"$f":"'Individual Spaces'!H11","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O11","v":0},{"$f":"'Individual Spaces'!P11","v":0},{"$f":"'Individual Spaces'!Q11","v":0},{"$f":"'Individual Spaces'!R11","v":0},null,0,{"$f":"IF(AF12=\"-\",0,ROUND((J12-VLOOKUP(B12,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B12,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B12,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B12,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J12-VLOOKUP(B12,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B12,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B12,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B12,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B12,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B12,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B12,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B12,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B12,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A12","v":"CLA12"},{"$f":"'Individual Spaces'!B12","v":"CLA12"},{"$f":"'Individual Spaces'!C12","v":1009},{"$f":"'Individual Spaces'!D12","v":"Classrooms (general) 6"},{"$f":"'Individual Spaces'!E12","v":0},null,{"$f":"VLOOKUP($B13,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B13,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G12","v":"Mathematics"},{"$f":"'Individual Spaces'!H12","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O12","v":0},{"$f":"'Individual Spaces'!P12","v":0},{"$f":"'Individual Spaces'!Q12","v":0},{"$f":"'Individual Spaces'!R12","v":0},null,0,{"$f":"IF(AF13=\"-\",0,ROUND((J13-VLOOKUP(B13,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B13,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B13,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B13,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J13-VLOOKUP(B13,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B13,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B13,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B13,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B13,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B13,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B13,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B13,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B13,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A13","v":"CLA12"},{"$f":"'Individual Spaces'!B13","v":"CLA12"},{"$f":"'Individual Spaces'!C13","v":1010},{"$f":"'Individual Spaces'!D13","v":"Classrooms (general) 7"},{"$f":"'Individual Spaces'!E13","v":0},null,{"$f":"VLOOKUP($B14,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B14,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G13","v":"Mathematics"},{"$f":"'Individual Spaces'!H13","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O13","v":0},{"$f":"'Individual Spaces'!P13","v":0},{"$f":"'Individual Spaces'!Q13","v":0},{"$f":"'Individual Spaces'!R13","v":0},null,0,{"$f":"IF(AF14=\"-\",0,ROUND((J14-VLOOKUP(B14,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B14,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B14,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B14,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J14-VLOOKUP(B14,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B14,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B14,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B14,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B14,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B14,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B14,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B14,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B14,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A14","v":"CLA12"},{"$f":"'Individual Spaces'!B14","v":"CLA12"},{"$f":"'Individual Spaces'!C14","v":1011},{"$f":"'Individual Spaces'!D14","v":"Classrooms (general) 8"},{"$f":"'Individual Spaces'!E14","v":0},null,{"$f":"VLOOKUP($B15,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B15,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G14","v":"Mathematics"},{"$f":"'Individual Spaces'!H14","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O14","v":0},{"$f":"'Individual Spaces'!P14","v":0},{"$f":"'Individual Spaces'!Q14","v":0},{"$f":"'Individual Spaces'!R14","v":0},null,0,{"$f":"IF(AF15=\"-\",0,ROUND((J15-VLOOKUP(B15,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B15,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B15,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B15,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J15-VLOOKUP(B15,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B15,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B15,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B15,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B15,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B15,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B15,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B15,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B15,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A15","v":"CLA12"},{"$f":"'Individual Spaces'!B15","v":"CLA12"},{"$f":"'Individual Spaces'!C15","v":1012},{"$f":"'Individual Spaces'!D15","v":"Classrooms (general) 9"},{"$f":"'Individual Spaces'!E15","v":0},null,{"$f":"VLOOKUP($B16,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B16,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G15","v":"English"},{"$f":"'Individual Spaces'!H15","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O15","v":0},{"$f":"'Individual Spaces'!P15","v":0},{"$f":"'Individual Spaces'!Q15","v":0},{"$f":"'Individual Spaces'!R15","v":0},null,0,{"$f":"IF(AF16=\"-\",0,ROUND((J16-VLOOKUP(B16,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B16,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B16,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B16,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J16-VLOOKUP(B16,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B16,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B16,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B16,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B16,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B16,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B16,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B16,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B16,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A16","v":"CLA12"},{"$f":"'Individual Spaces'!B16","v":"CLA12"},{"$f":"'Individual Spaces'!C16","v":1013},{"$f":"'Individual Spaces'!D16","v":"Classrooms (general) 10"},{"$f":"'Individual Spaces'!E16","v":0},null,{"$f":"VLOOKUP($B17,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B17,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G16","v":"English"},{"$f":"'Individual Spaces'!H16","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O16","v":0},{"$f":"'Individual Spaces'!P16","v":0},{"$f":"'Individual Spaces'!Q16","v":0},{"$f":"'Individual Spaces'!R16","v":0},null,0,{"$f":"IF(AF17=\"-\",0,ROUND((J17-VLOOKUP(B17,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B17,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B17,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B17,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J17-VLOOKUP(B17,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B17,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B17,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B17,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B17,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B17,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B17,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B17,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B17,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A17","v":"CLA12"},{"$f":"'Individual Spaces'!B17","v":"CLA12"},{"$f":"'Individual Spaces'!C17","v":1014},{"$f":"'Individual Spaces'!D17","v":"Classrooms (general) 11"},{"$f":"'Individual Spaces'!E17","v":0},null,{"$f":"VLOOKUP($B18,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B18,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G17","v":"English"},{"$f":"'Individual Spaces'!H17","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O17","v":0},{"$f":"'Individual Spaces'!P17","v":0},{"$f":"'Individual Spaces'!Q17","v":0},{"$f":"'Individual Spaces'!R17","v":0},null,0,{"$f":"IF(AF18=\"-\",0,ROUND((J18-VLOOKUP(B18,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B18,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B18,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B18,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J18-VLOOKUP(B18,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B18,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B18,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B18,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B18,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B18,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B18,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B18,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B18,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A18","v":"CLA12"},{"$f":"'Individual Spaces'!B18","v":"CLA12"},{"$f":"'Individual Spaces'!C18","v":1015},{"$f":"'Individual Spaces'!D18","v":"Classrooms (general) 12"},{"$f":"'Individual Spaces'!E18","v":0},null,{"$f":"VLOOKUP($B19,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B19,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G18","v":"English"},{"$f":"'Individual Spaces'!H18","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O18","v":0},{"$f":"'Individual Spaces'!P18","v":0},{"$f":"'Individual Spaces'!Q18","v":0},{"$f":"'Individual Spaces'!R18","v":0},null,0,{"$f":"IF(AF19=\"-\",0,ROUND((J19-VLOOKUP(B19,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B19,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B19,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B19,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J19-VLOOKUP(B19,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B19,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B19,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B19,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B19,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B19,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B19,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B19,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B19,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A19","v":"CLA12"},{"$f":"'Individual Spaces'!B19","v":"CLA12"},{"$f":"'Individual Spaces'!C19","v":1016},{"$f":"'Individual Spaces'!D19","v":"Classrooms (general) 13"},{"$f":"'Individual Spaces'!E19","v":0},null,{"$f":"VLOOKUP($B20,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B20,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G19","v":"English"},{"$f":"'Individual Spaces'!H19","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O19","v":0},{"$f":"'Individual Spaces'!P19","v":0},{"$f":"'Individual Spaces'!Q19","v":0},{"$f":"'Individual Spaces'!R19","v":0},null,0,{"$f":"IF(AF20=\"-\",0,ROUND((J20-VLOOKUP(B20,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B20,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B20,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B20,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J20-VLOOKUP(B20,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B20,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B20,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B20,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B20,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B20,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B20,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B20,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B20,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A20","v":"CLA12"},{"$f":"'Individual Spaces'!B20","v":"CLA12"},{"$f":"'Individual Spaces'!C20","v":1017},{"$f":"'Individual Spaces'!D20","v":"Classrooms (general) 14"},{"$f":"'Individual Spaces'!E20","v":0},null,{"$f":"VLOOKUP($B21,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B21,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G20","v":"English"},{"$f":"'Individual Spaces'!H20","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O20","v":0},{"$f":"'Individual Spaces'!P20","v":0},{"$f":"'Individual Spaces'!Q20","v":0},{"$f":"'Individual Spaces'!R20","v":0},null,0,{"$f":"IF(AF21=\"-\",0,ROUND((J21-VLOOKUP(B21,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B21,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B21,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B21,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J21-VLOOKUP(B21,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B21,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B21,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B21,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B21,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B21,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B21,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B21,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B21,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A21","v":"CLA12"},{"$f":"'Individual Spaces'!B21","v":"CLA12"},{"$f":"'Individual Spaces'!C21","v":1018},{"$f":"'Individual Spaces'!D21","v":"Classrooms (general) 15"},{"$f":"'Individual Spaces'!E21","v":0},null,{"$f":"VLOOKUP($B22,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B22,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G21","v":"English"},{"$f":"'Individual Spaces'!H21","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O21","v":0},{"$f":"'Individual Spaces'!P21","v":0},{"$f":"'Individual Spaces'!Q21","v":0},{"$f":"'Individual Spaces'!R21","v":0},null,0,{"$f":"IF(AF22=\"-\",0,ROUND((J22-VLOOKUP(B22,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B22,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B22,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B22,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J22-VLOOKUP(B22,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B22,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B22,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B22,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B22,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B22,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B22,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B22,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B22,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A22","v":"CLA12"},{"$f":"'Individual Spaces'!B22","v":"CLA12"},{"$f":"'Individual Spaces'!C22","v":1019},{"$f":"'Individual Spaces'!D22","v":"Classrooms (general) 16"},{"$f":"'Individual Spaces'!E22","v":0},null,{"$f":"VLOOKUP($B23,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B23,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G22","v":"English"},{"$f":"'Individual Spaces'!H22","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O22","v":0},{"$f":"'Individual Spaces'!P22","v":0},{"$f":"'Individual Spaces'!Q22","v":0},{"$f":"'Individual Spaces'!R22","v":0},null,0,{"$f":"IF(AF23=\"-\",0,ROUND((J23-VLOOKUP(B23,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B23,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B23,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B23,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J23-VLOOKUP(B23,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B23,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B23,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B23,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B23,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B23,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B23,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B23,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B23,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A23","v":"CLA12"},{"$f":"'Individual Spaces'!B23","v":"CLA12"},{"$f":"'Individual Spaces'!C23","v":1020},{"$f":"'Individual Spaces'!D23","v":"Classrooms (general) 17"},{"$f":"'Individual Spaces'!E23","v":0},null,{"$f":"VLOOKUP($B24,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B24,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G23","v":"MFL"},{"$f":"'Individual Spaces'!H23","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O23","v":0},{"$f":"'Individual Spaces'!P23","v":0},{"$f":"'Individual Spaces'!Q23","v":0},{"$f":"'Individual Spaces'!R23","v":0},null,0,{"$f":"IF(AF24=\"-\",0,ROUND((J24-VLOOKUP(B24,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B24,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B24,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B24,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J24-VLOOKUP(B24,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B24,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B24,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B24,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B24,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B24,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B24,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B24,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B24,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A24","v":"CLA12"},{"$f":"'Individual Spaces'!B24","v":"CLA12"},{"$f":"'Individual Spaces'!C24","v":1021},{"$f":"'Individual Spaces'!D24","v":"Classrooms (general) 18"},{"$f":"'Individual Spaces'!E24","v":0},null,{"$f":"VLOOKUP($B25,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B25,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G24","v":"MFL"},{"$f":"'Individual Spaces'!H24","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O24","v":0},{"$f":"'Individual Spaces'!P24","v":0},{"$f":"'Individual Spaces'!Q24","v":0},{"$f":"'Individual Spaces'!R24","v":0},null,0,{"$f":"IF(AF25=\"-\",0,ROUND((J25-VLOOKUP(B25,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B25,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B25,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B25,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J25-VLOOKUP(B25,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B25,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B25,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B25,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B25,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B25,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B25,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B25,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B25,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A25","v":"CLA12"},{"$f":"'Individual Spaces'!B25","v":"CLA12"},{"$f":"'Individual Spaces'!C25","v":1022},{"$f":"'Individual Spaces'!D25","v":"Classrooms (general) 19"},{"$f":"'Individual Spaces'!E25","v":0},null,{"$f":"VLOOKUP($B26,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B26,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G25","v":"MFL"},{"$f":"'Individual Spaces'!H25","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O25","v":0},{"$f":"'Individual Spaces'!P25","v":0},{"$f":"'Individual Spaces'!Q25","v":0},{"$f":"'Individual Spaces'!R25","v":0},null,0,{"$f":"IF(AF26=\"-\",0,ROUND((J26-VLOOKUP(B26,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B26,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B26,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B26,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J26-VLOOKUP(B26,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B26,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B26,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B26,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B26,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B26,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B26,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B26,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B26,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A26","v":"CLA12"},{"$f":"'Individual Spaces'!B26","v":"CLA12"},{"$f":"'Individual Spaces'!C26","v":1023},{"$f":"'Individual Spaces'!D26","v":"Classrooms (general) 20"},{"$f":"'Individual Spaces'!E26","v":0},null,{"$f":"VLOOKUP($B27,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B27,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G26","v":"MFL"},{"$f":"'Individual Spaces'!H26","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O26","v":0},{"$f":"'Individual Spaces'!P26","v":0},{"$f":"'Individual Spaces'!Q26","v":0},{"$f":"'Individual Spaces'!R26","v":0},null,0,{"$f":"IF(AF27=\"-\",0,ROUND((J27-VLOOKUP(B27,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B27,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B27,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B27,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J27-VLOOKUP(B27,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B27,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B27,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B27,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B27,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B27,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B27,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B27,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B27,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A27","v":"CLA12"},{"$f":"'Individual Spaces'!B27","v":"CLA12"},{"$f":"'Individual Spaces'!C27","v":1024},{"$f":"'Individual Spaces'!D27","v":"Classrooms (general) 21"},{"$f":"'Individual Spaces'!E27","v":0},null,{"$f":"VLOOKUP($B28,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B28,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G27","v":"MFL"},{"$f":"'Individual Spaces'!H27","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O27","v":0},{"$f":"'Individual Spaces'!P27","v":0},{"$f":"'Individual Spaces'!Q27","v":0},{"$f":"'Individual Spaces'!R27","v":0},null,0,{"$f":"IF(AF28=\"-\",0,ROUND((J28-VLOOKUP(B28,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B28,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B28,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B28,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J28-VLOOKUP(B28,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B28,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B28,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B28,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B28,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B28,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B28,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B28,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B28,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A28","v":"CLA12"},{"$f":"'Individual Spaces'!B28","v":"CLA12"},{"$f":"'Individual Spaces'!C28","v":1025},{"$f":"'Individual Spaces'!D28","v":"Classrooms (general) 22"},{"$f":"'Individual Spaces'!E28","v":0},null,{"$f":"VLOOKUP($B29,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B29,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G28","v":"MFL"},{"$f":"'Individual Spaces'!H28","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O28","v":0},{"$f":"'Individual Spaces'!P28","v":0},{"$f":"'Individual Spaces'!Q28","v":0},{"$f":"'Individual Spaces'!R28","v":0},null,0,{"$f":"IF(AF29=\"-\",0,ROUND((J29-VLOOKUP(B29,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B29,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B29,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B29,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J29-VLOOKUP(B29,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B29,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B29,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B29,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B29,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B29,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B29,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B29,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B29,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A29","v":"CLA12"},{"$f":"'Individual Spaces'!B29","v":"CLA12"},{"$f":"'Individual Spaces'!C29","v":1026},{"$f":"'Individual Spaces'!D29","v":"Classrooms (general) 23"},{"$f":"'Individual Spaces'!E29","v":0},null,{"$f":"VLOOKUP($B30,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B30,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G29","v":"Humanities"},{"$f":"'Individual Spaces'!H29","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O29","v":0},{"$f":"'Individual Spaces'!P29","v":0},{"$f":"'Individual Spaces'!Q29","v":0},{"$f":"'Individual Spaces'!R29","v":0},null,0,{"$f":"IF(AF30=\"-\",0,ROUND((J30-VLOOKUP(B30,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B30,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B30,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B30,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J30-VLOOKUP(B30,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B30,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B30,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B30,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B30,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B30,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B30,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B30,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B30,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A30","v":"CLA12"},{"$f":"'Individual Spaces'!B30","v":"CLA12"},{"$f":"'Individual Spaces'!C30","v":1027},{"$f":"'Individual Spaces'!D30","v":"Classrooms (general) 24"},{"$f":"'Individual Spaces'!E30","v":0},null,{"$f":"VLOOKUP($B31,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B31,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G30","v":"Humanities"},{"$f":"'Individual Spaces'!H30","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O30","v":0},{"$f":"'Individual Spaces'!P30","v":0},{"$f":"'Individual Spaces'!Q30","v":0},{"$f":"'Individual Spaces'!R30","v":0},null,0,{"$f":"IF(AF31=\"-\",0,ROUND((J31-VLOOKUP(B31,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B31,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B31,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B31,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J31-VLOOKUP(B31,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B31,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B31,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B31,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B31,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B31,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B31,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B31,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B31,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A31","v":"CLA12"},{"$f":"'Individual Spaces'!B31","v":"CLA12"},{"$f":"'Individual Spaces'!C31","v":1028},{"$f":"'Individual Spaces'!D31","v":"Classrooms (general) 25"},{"$f":"'Individual Spaces'!E31","v":0},null,{"$f":"VLOOKUP($B32,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B32,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G31","v":"Humanities"},{"$f":"'Individual Spaces'!H31","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O31","v":0},{"$f":"'Individual Spaces'!P31","v":0},{"$f":"'Individual Spaces'!Q31","v":0},{"$f":"'Individual Spaces'!R31","v":0},null,0,{"$f":"IF(AF32=\"-\",0,ROUND((J32-VLOOKUP(B32,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B32,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B32,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B32,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J32-VLOOKUP(B32,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B32,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B32,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B32,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B32,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B32,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B32,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B32,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B32,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A32","v":"CLA12"},{"$f":"'Individual Spaces'!B32","v":"CLA12"},{"$f":"'Individual Spaces'!C32","v":1029},{"$f":"'Individual Spaces'!D32","v":"Classrooms (general) 26"},{"$f":"'Individual Spaces'!E32","v":0},null,{"$f":"VLOOKUP($B33,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B33,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G32","v":"Humanities"},{"$f":"'Individual Spaces'!H32","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O32","v":0},{"$f":"'Individual Spaces'!P32","v":0},{"$f":"'Individual Spaces'!Q32","v":0},{"$f":"'Individual Spaces'!R32","v":0},null,0,{"$f":"IF(AF33=\"-\",0,ROUND((J33-VLOOKUP(B33,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B33,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B33,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B33,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J33-VLOOKUP(B33,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B33,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B33,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B33,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B33,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B33,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B33,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B33,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B33,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A33","v":"CLA12"},{"$f":"'Individual Spaces'!B33","v":"CLA12"},{"$f":"'Individual Spaces'!C33","v":1030},{"$f":"'Individual Spaces'!D33","v":"Classrooms (general) 27"},{"$f":"'Individual Spaces'!E33","v":0},null,{"$f":"VLOOKUP($B34,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_14"},{"$f":"VLOOKUP($B34,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classrooms"},{"$f":"'Individual Spaces'!G33","v":"Humanities"},{"$f":"'Individual Spaces'!H33","v":55},null,null,null,-55,null,null,{"$f":"'Individual Spaces'!O33","v":0},{"$f":"'Individual Spaces'!P33","v":0},{"$f":"'Individual Spaces'!Q33","v":0},{"$f":"'Individual Spaces'!R33","v":0},null,0,{"$f":"IF(AF34=\"-\",0,ROUND((J34-VLOOKUP(B34,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B34,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B34,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B34,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J34-VLOOKUP(B34,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B34,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B34,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom for a range of layout options and activities"},{"$f":"VLOOKUP($B34,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B34,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B34,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B34,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B34,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B34,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A34","v":0},{"$f":"'Individual Spaces'!B34","v":0},{"$f":"'Individual Spaces'!C34","v":0},{"$f":"'Individual Spaces'!D34","v":0},{"$f":"'Individual Spaces'!E34","v":"General Teaching Total : "},null,{"$f":"VLOOKUP($B35,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B35,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G34","v":0},{"$f":"'Individual Spaces'!H34","v":1608},null,null,null,-1608,null,null,{"$f":"'Individual Spaces'!O34","v":0},{"$f":"'Individual Spaces'!P34","v":0},{"$f":"'Individual Spaces'!Q34","v":0},{"$f":"'Individual Spaces'!R34","v":0},null,0,{"$f":"IF(AF35=\"-\",0,ROUND((J35-VLOOKUP(B35,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B35,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B35,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B35,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J35-VLOOKUP(B35,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B35,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B35,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B35,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B35,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B35,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B35,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B35,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B35,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A35","v":"CLA32"},{"$f":"'Individual Spaces'!B35","v":"CLA32"},{"$f":"'Individual Spaces'!C35","v":1101},{"$f":"'Individual Spaces'!D35","v":"ICT-rich classroom 1"},{"$f":"'Individual Spaces'!E35","v":0},null,{"$f":"VLOOKUP($B36,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_41"},{"$f":"VLOOKUP($B36,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"ICT-rich classrooms"},{"$f":"'Individual Spaces'!G35","v":"ICT and Business Studies"},{"$f":"'Individual Spaces'!H35","v":69},null,null,null,-69,null,null,{"$f":"'Individual Spaces'!O35","v":0},{"$f":"'Individual Spaces'!P35","v":0},{"$f":"'Individual Spaces'!Q35","v":0},{"$f":"'Individual Spaces'!R35","v":0},null,0,{"$f":"IF(AF36=\"-\",0,ROUND((J36-VLOOKUP(B36,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B36,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":34},{"$f":"IF(VLOOKUP(B36,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B36,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J36-VLOOKUP(B36,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B36,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},38,null,null,{"$f":"VLOOKUP($B36,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom with fixed ICT devices for all workplaces and a range of layout options"},{"$f":"VLOOKUP($B36,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using ICT devices and whiteboard. Teacher led presentations and briefings using ICT and the whiteboard."},{"$f":"VLOOKUP($B36,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B36,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Fitted"},{"$f":"VLOOKUP($B36,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"D"},{"$f":"VLOOKUP($B36,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B36,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A36","v":"CLA32"},{"$f":"'Individual Spaces'!B36","v":"CLA32"},{"$f":"'Individual Spaces'!C36","v":1102},{"$f":"'Individual Spaces'!D36","v":"ICT-rich classroom 2"},{"$f":"'Individual Spaces'!E36","v":0},null,{"$f":"VLOOKUP($B37,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_41"},{"$f":"VLOOKUP($B37,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"ICT-rich classrooms"},{"$f":"'Individual Spaces'!G36","v":"ICT and Business Studies"},{"$f":"'Individual Spaces'!H36","v":69},null,null,null,-69,null,null,{"$f":"'Individual Spaces'!O36","v":0},{"$f":"'Individual Spaces'!P36","v":0},{"$f":"'Individual Spaces'!Q36","v":0},{"$f":"'Individual Spaces'!R36","v":0},null,0,{"$f":"IF(AF37=\"-\",0,ROUND((J37-VLOOKUP(B37,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B37,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":34},{"$f":"IF(VLOOKUP(B37,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B37,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J37-VLOOKUP(B37,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B37,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},38,null,null,{"$f":"VLOOKUP($B37,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom with fixed ICT devices for all workplaces and a range of layout options"},{"$f":"VLOOKUP($B37,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using ICT devices and whiteboard. Teacher led presentations and briefings using ICT and the whiteboard."},{"$f":"VLOOKUP($B37,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B37,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Fitted"},{"$f":"VLOOKUP($B37,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"D"},{"$f":"VLOOKUP($B37,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B37,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A37","v":"CLA32"},{"$f":"'Individual Spaces'!B37","v":"CLA32"},{"$f":"'Individual Spaces'!C37","v":1103},{"$f":"'Individual Spaces'!D37","v":"ICT-rich classroom 3"},{"$f":"'Individual Spaces'!E37","v":0},null,{"$f":"VLOOKUP($B38,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_41"},{"$f":"VLOOKUP($B38,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"ICT-rich classrooms"},{"$f":"'Individual Spaces'!G37","v":"ICT and Business Studies"},{"$f":"'Individual Spaces'!H37","v":69},null,null,null,-69,null,null,{"$f":"'Individual Spaces'!O37","v":0},{"$f":"'Individual Spaces'!P37","v":0},{"$f":"'Individual Spaces'!Q37","v":0},{"$f":"'Individual Spaces'!R37","v":0},null,0,{"$f":"IF(AF38=\"-\",0,ROUND((J38-VLOOKUP(B38,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B38,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":34},{"$f":"IF(VLOOKUP(B38,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B38,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J38-VLOOKUP(B38,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B38,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},38,null,null,{"$f":"VLOOKUP($B38,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom with fixed ICT devices for all workplaces and a range of layout options"},{"$f":"VLOOKUP($B38,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using ICT devices and whiteboard. Teacher led presentations and briefings using ICT and the whiteboard."},{"$f":"VLOOKUP($B38,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B38,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Fitted"},{"$f":"VLOOKUP($B38,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"D"},{"$f":"VLOOKUP($B38,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B38,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A38","v":"CLA32"},{"$f":"'Individual Spaces'!B38","v":"CLA42"},{"$f":"'Individual Spaces'!C38","v":1104},{"$f":"'Individual Spaces'!D38","v":"ICT-rich classroom (business studies) 1"},{"$f":"'Individual Spaces'!E38","v":0},null,{"$f":"VLOOKUP($B39,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_41"},{"$f":"VLOOKUP($B39,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"ICT-rich classrooms"},{"$f":"'Individual Spaces'!G38","v":"ICT and Business Studies"},{"$f":"'Individual Spaces'!H38","v":69},null,null,null,-69,null,null,{"$f":"'Individual Spaces'!O38","v":0},{"$f":"'Individual Spaces'!P38","v":0},{"$f":"'Individual Spaces'!Q38","v":0},{"$f":"'Individual Spaces'!R38","v":0},null,0,{"$f":"IF(AF39=\"-\",0,ROUND((J39-VLOOKUP(B39,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B39,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":34},{"$f":"IF(VLOOKUP(B39,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B39,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J39-VLOOKUP(B39,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B39,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},38,null,null,{"$f":"VLOOKUP($B39,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school classroom with fixed ICT devices for half workplaces with business environment"},{"$f":"VLOOKUP($B39,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research. Individual, group and whole class pupil led presentations and discussions using ICT devices predominantly by 14-19 age group. Occasional need for some furniture re-arrangement. Teacher led presentations and briefings using ICT and the whiteboard."},{"$f":"VLOOKUP($B39,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B39,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Fitted"},{"$f":"VLOOKUP($B39,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"D"},{"$f":"VLOOKUP($B39,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B39,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A39","v":"SCI05"},{"$f":"'Individual Spaces'!B39","v":"SCI05"},{"$f":"'Individual Spaces'!C39","v":1105},{"$f":"'Individual Spaces'!D39","v":"Science laboratory 1"},{"$f":"'Individual Spaces'!E39","v":0},null,{"$f":"VLOOKUP($B40,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_75"},{"$f":"VLOOKUP($B40,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Science laboratories"},{"$f":"'Individual Spaces'!G39","v":"Science"},{"$f":"'Individual Spaces'!H39","v":83},null,null,null,-83,null,null,{"$f":"'Individual Spaces'!O39","v":0},{"$f":"'Individual Spaces'!P39","v":0},{"$f":"'Individual Spaces'!Q39","v":0},{"$f":"'Individual Spaces'!R39","v":0},null,0,{"$f":"IF(AF40=\"-\",0,ROUND((J40-VLOOKUP(B40,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B40,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B40,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B40,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J40-VLOOKUP(B40,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B40,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B40,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school science laboratory for demonstration and 'hands on' experiments and fume cupboard"},{"$f":"VLOOKUP($B40,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of experiments. Using the whiteboard. Whole class presentations. Wide range of supervised experiments using gas, power and water."},{"$f":"VLOOKUP($B40,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B40,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Light practical (science)"},{"$f":"VLOOKUP($B40,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"F"},{"$f":"VLOOKUP($B40,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B40,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A40","v":"SCI05"},{"$f":"'Individual Spaces'!B40","v":"SCI05"},{"$f":"'Individual Spaces'!C40","v":1106},{"$f":"'Individual Spaces'!D40","v":"Science laboratory 2"},{"$f":"'Individual Spaces'!E40","v":0},null,{"$f":"VLOOKUP($B41,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_75"},{"$f":"VLOOKUP($B41,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Science laboratories"},{"$f":"'Individual Spaces'!G40","v":"Science"},{"$f":"'Individual Spaces'!H40","v":83},null,null,null,-83,null,null,{"$f":"'Individual Spaces'!O40","v":0},{"$f":"'Individual Spaces'!P40","v":0},{"$f":"'Individual Spaces'!Q40","v":0},{"$f":"'Individual Spaces'!R40","v":0},null,0,{"$f":"IF(AF41=\"-\",0,ROUND((J41-VLOOKUP(B41,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B41,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B41,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B41,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J41-VLOOKUP(B41,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B41,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B41,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school science laboratory for demonstration and 'hands on' experiments and fume cupboard"},{"$f":"VLOOKUP($B41,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of experiments. Using the whiteboard. Whole class presentations. Wide range of supervised experiments using gas, power and water."},{"$f":"VLOOKUP($B41,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B41,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Light practical (science)"},{"$f":"VLOOKUP($B41,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"F"},{"$f":"VLOOKUP($B41,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B41,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A41","v":"SCI05"},{"$f":"'Individual Spaces'!B41","v":"SCI05"},{"$f":"'Individual Spaces'!C41","v":1107},{"$f":"'Individual Spaces'!D41","v":"Science laboratory 3"},{"$f":"'Individual Spaces'!E41","v":0},null,{"$f":"VLOOKUP($B42,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_75"},{"$f":"VLOOKUP($B42,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Science laboratories"},{"$f":"'Individual Spaces'!G41","v":"Science"},{"$f":"'Individual Spaces'!H41","v":83},null,null,null,-83,null,null,{"$f":"'Individual Spaces'!O41","v":0},{"$f":"'Individual Spaces'!P41","v":0},{"$f":"'Individual Spaces'!Q41","v":0},{"$f":"'Individual Spaces'!R41","v":0},null,0,{"$f":"IF(AF42=\"-\",0,ROUND((J42-VLOOKUP(B42,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B42,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B42,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B42,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J42-VLOOKUP(B42,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B42,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B42,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school science laboratory for demonstration and 'hands on' experiments and fume cupboard"},{"$f":"VLOOKUP($B42,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of experiments. Using the whiteboard. Whole class presentations. Wide range of supervised experiments using gas, power and water."},{"$f":"VLOOKUP($B42,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B42,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Light practical (science)"},{"$f":"VLOOKUP($B42,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"F"},{"$f":"VLOOKUP($B42,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B42,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A42","v":"SCI05"},{"$f":"'Individual Spaces'!B42","v":"SCI05"},{"$f":"'Individual Spaces'!C42","v":1108},{"$f":"'Individual Spaces'!D42","v":"Science laboratory 4"},{"$f":"'Individual Spaces'!E42","v":0},null,{"$f":"VLOOKUP($B43,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_75"},{"$f":"VLOOKUP($B43,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Science laboratories"},{"$f":"'Individual Spaces'!G42","v":"Science"},{"$f":"'Individual Spaces'!H42","v":83},null,null,null,-83,null,null,{"$f":"'Individual Spaces'!O42","v":0},{"$f":"'Individual Spaces'!P42","v":0},{"$f":"'Individual Spaces'!Q42","v":0},{"$f":"'Individual Spaces'!R42","v":0},null,0,{"$f":"IF(AF43=\"-\",0,ROUND((J43-VLOOKUP(B43,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B43,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B43,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B43,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J43-VLOOKUP(B43,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B43,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B43,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school science laboratory for demonstration and 'hands on' experiments and fume cupboard"},{"$f":"VLOOKUP($B43,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of experiments. Using the whiteboard. Whole class presentations. Wide range of supervised experiments using gas, power and water."},{"$f":"VLOOKUP($B43,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B43,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Light practical (science)"},{"$f":"VLOOKUP($B43,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"F"},{"$f":"VLOOKUP($B43,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B43,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A43","v":"SCI05"},{"$f":"'Individual Spaces'!B43","v":"SCI05"},{"$f":"'Individual Spaces'!C43","v":1109},{"$f":"'Individual Spaces'!D43","v":"Science laboratory 5"},{"$f":"'Individual Spaces'!E43","v":0},null,{"$f":"VLOOKUP($B44,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_75"},{"$f":"VLOOKUP($B44,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Science laboratories"},{"$f":"'Individual Spaces'!G43","v":"Science"},{"$f":"'Individual Spaces'!H43","v":83},null,null,null,-83,null,null,{"$f":"'Individual Spaces'!O43","v":0},{"$f":"'Individual Spaces'!P43","v":0},{"$f":"'Individual Spaces'!Q43","v":0},{"$f":"'Individual Spaces'!R43","v":0},null,0,{"$f":"IF(AF44=\"-\",0,ROUND((J44-VLOOKUP(B44,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B44,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B44,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B44,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J44-VLOOKUP(B44,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B44,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B44,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school science laboratory for demonstration and 'hands on' experiments and fume cupboard"},{"$f":"VLOOKUP($B44,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of experiments. Using the whiteboard. Whole class presentations. Wide range of supervised experiments using gas, power and water."},{"$f":"VLOOKUP($B44,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B44,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Light practical (science)"},{"$f":"VLOOKUP($B44,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"F"},{"$f":"VLOOKUP($B44,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B44,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A44","v":"SCI05"},{"$f":"'Individual Spaces'!B44","v":"SCI05"},{"$f":"'Individual Spaces'!C44","v":1110},{"$f":"'Individual Spaces'!D44","v":"Science laboratory 6"},{"$f":"'Individual Spaces'!E44","v":0},null,{"$f":"VLOOKUP($B45,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_75"},{"$f":"VLOOKUP($B45,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Science laboratories"},{"$f":"'Individual Spaces'!G44","v":"Science"},{"$f":"'Individual Spaces'!H44","v":83},null,null,null,-83,null,null,{"$f":"'Individual Spaces'!O44","v":0},{"$f":"'Individual Spaces'!P44","v":0},{"$f":"'Individual Spaces'!Q44","v":0},{"$f":"'Individual Spaces'!R44","v":0},null,0,{"$f":"IF(AF45=\"-\",0,ROUND((J45-VLOOKUP(B45,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B45,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B45,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B45,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J45-VLOOKUP(B45,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B45,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B45,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school science laboratory for demonstration and 'hands on' experiments and fume cupboard"},{"$f":"VLOOKUP($B45,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of experiments. Using the whiteboard. Whole class presentations. Wide range of supervised experiments using gas, power and water."},{"$f":"VLOOKUP($B45,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B45,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Light practical (science)"},{"$f":"VLOOKUP($B45,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"F"},{"$f":"VLOOKUP($B45,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B45,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A45","v":"SCI05"},{"$f":"'Individual Spaces'!B45","v":"SCI05"},{"$f":"'Individual Spaces'!C45","v":1111},{"$f":"'Individual Spaces'!D45","v":"Science laboratory 7"},{"$f":"'Individual Spaces'!E45","v":0},null,{"$f":"VLOOKUP($B46,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_75"},{"$f":"VLOOKUP($B46,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Science laboratories"},{"$f":"'Individual Spaces'!G45","v":"Science"},{"$f":"'Individual Spaces'!H45","v":83},null,null,null,-83,null,null,{"$f":"'Individual Spaces'!O45","v":0},{"$f":"'Individual Spaces'!P45","v":0},{"$f":"'Individual Spaces'!Q45","v":0},{"$f":"'Individual Spaces'!R45","v":0},null,0,{"$f":"IF(AF46=\"-\",0,ROUND((J46-VLOOKUP(B46,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B46,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B46,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B46,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J46-VLOOKUP(B46,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B46,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B46,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school science laboratory for demonstration and 'hands on' experiments and fume cupboard"},{"$f":"VLOOKUP($B46,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of experiments. Using the whiteboard. Whole class presentations. Wide range of supervised experiments using gas, power and water."},{"$f":"VLOOKUP($B46,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B46,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Light practical (science)"},{"$f":"VLOOKUP($B46,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"F"},{"$f":"VLOOKUP($B46,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B46,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A46","v":"SCI05"},{"$f":"'Individual Spaces'!B46","v":"SCI11"},{"$f":"'Individual Spaces'!C46","v":1112},{"$f":"'Individual Spaces'!D46","v":"Science laboratory (specialist) 1"},{"$f":"'Individual Spaces'!E46","v":0},null,{"$f":"VLOOKUP($B47,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_75"},{"$f":"VLOOKUP($B47,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Science laboratories"},{"$f":"'Individual Spaces'!G46","v":"Science"},{"$f":"'Individual Spaces'!H46","v":97},null,null,null,-97,null,null,{"$f":"'Individual Spaces'!O46","v":0},{"$f":"'Individual Spaces'!P46","v":0},{"$f":"'Individual Spaces'!Q46","v":0},{"$f":"'Individual Spaces'!R46","v":0},null,0,{"$f":"IF(AF47=\"-\",0,ROUND((J47-VLOOKUP(B47,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B47,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":33},{"$f":"IF(VLOOKUP(B47,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B47,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J47-VLOOKUP(B47,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B47,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},37,null,null,{"$f":"VLOOKUP($B47,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school science laboratory for demonstration for all types of experiments, up to A-level "},{"$f":"VLOOKUP($B47,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of experiments. Using the whiteboard. Whole class presentations. Wide range of supervised experiments using gas, power and water."},{"$f":"VLOOKUP($B47,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B47,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Light practical (science)"},{"$f":"VLOOKUP($B47,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"F1"},{"$f":"VLOOKUP($B47,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"extensive"},{"$f":"VLOOKUP($B47,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A47","v":"SCI05"},{"$f":"'Individual Spaces'!B47","v":"SCI11"},{"$f":"'Individual Spaces'!C47","v":1113},{"$f":"'Individual Spaces'!D47","v":"Science laboratory (specialist) 2"},{"$f":"'Individual Spaces'!E47","v":0},null,{"$f":"VLOOKUP($B48,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_75"},{"$f":"VLOOKUP($B48,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Science laboratories"},{"$f":"'Individual Spaces'!G47","v":"Science"},{"$f":"'Individual Spaces'!H47","v":97},null,null,null,-97,null,null,{"$f":"'Individual Spaces'!O47","v":0},{"$f":"'Individual Spaces'!P47","v":0},{"$f":"'Individual Spaces'!Q47","v":0},{"$f":"'Individual Spaces'!R47","v":0},null,0,{"$f":"IF(AF48=\"-\",0,ROUND((J48-VLOOKUP(B48,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B48,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":33},{"$f":"IF(VLOOKUP(B48,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B48,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J48-VLOOKUP(B48,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B48,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},37,null,null,{"$f":"VLOOKUP($B48,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school science laboratory for demonstration for all types of experiments, up to A-level "},{"$f":"VLOOKUP($B48,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of experiments. Using the whiteboard. Whole class presentations. Wide range of supervised experiments using gas, power and water."},{"$f":"VLOOKUP($B48,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B48,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Light practical (science)"},{"$f":"VLOOKUP($B48,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"F1"},{"$f":"VLOOKUP($B48,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"extensive"},{"$f":"VLOOKUP($B48,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A48","v":"SCI05"},{"$f":"'Individual Spaces'!B48","v":"SCI11"},{"$f":"'Individual Spaces'!C48","v":1114},{"$f":"'Individual Spaces'!D48","v":"Science laboratory (specialist) 3"},{"$f":"'Individual Spaces'!E48","v":0},null,{"$f":"VLOOKUP($B49,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_75"},{"$f":"VLOOKUP($B49,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Science laboratories"},{"$f":"'Individual Spaces'!G48","v":"Science"},{"$f":"'Individual Spaces'!H48","v":97},null,null,null,-97,null,null,{"$f":"'Individual Spaces'!O48","v":0},{"$f":"'Individual Spaces'!P48","v":0},{"$f":"'Individual Spaces'!Q48","v":0},{"$f":"'Individual Spaces'!R48","v":0},null,0,{"$f":"IF(AF49=\"-\",0,ROUND((J49-VLOOKUP(B49,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B49,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":33},{"$f":"IF(VLOOKUP(B49,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B49,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J49-VLOOKUP(B49,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B49,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},37,null,null,{"$f":"VLOOKUP($B49,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school science laboratory for demonstration for all types of experiments, up to A-level "},{"$f":"VLOOKUP($B49,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of experiments. Using the whiteboard. Whole class presentations. Wide range of supervised experiments using gas, power and water."},{"$f":"VLOOKUP($B49,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B49,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Light practical (science)"},{"$f":"VLOOKUP($B49,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"F1"},{"$f":"VLOOKUP($B49,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"extensive"},{"$f":"VLOOKUP($B49,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A49","v":"DAT00"},{"$f":"'Individual Spaces'!B49","v":"DAT02"},{"$f":"'Individual Spaces'!C49","v":1115},{"$f":"'Individual Spaces'!D49","v":"Art room (general) 1"},{"$f":"'Individual Spaces'!E49","v":0},null,{"$f":"VLOOKUP($B50,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_04"},{"$f":"VLOOKUP($B50,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Art rooms"},{"$f":"'Individual Spaces'!G49","v":"DT/ Art"},{"$f":"'Individual Spaces'!H49","v":83},null,null,null,-83,null,null,{"$f":"'Individual Spaces'!O49","v":0},{"$f":"'Individual Spaces'!P49","v":0},{"$f":"'Individual Spaces'!Q49","v":0},{"$f":"'Individual Spaces'!R49","v":0},null,0,{"$f":"IF(AF50=\"-\",0,ROUND((J50-VLOOKUP(B50,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B50,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B50,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B50,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J50-VLOOKUP(B50,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B50,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B50,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school art room for a range of general art"},{"$f":"VLOOKUP($B50,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Individual and group 2D work (drawing, painting). Individual, group and whole class pupil led presentations and discussions using the whiteboard. Small scale 3D work using a range of materials including card, plastic and wood. Some pupil research occasionally using ICT. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B50,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B50,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Light practical"},{"$f":"VLOOKUP($B50,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"F"},{"$f":"VLOOKUP($B50,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B50,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A50","v":"DAT00"},{"$f":"'Individual Spaces'!B50","v":"DAT03"},{"$f":"'Individual Spaces'!C50","v":1116},{"$f":"'Individual Spaces'!D50","v":"Art room (3D) 1"},{"$f":"'Individual Spaces'!E50","v":0},null,{"$f":"VLOOKUP($B51,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_04"},{"$f":"VLOOKUP($B51,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Art rooms"},{"$f":"'Individual Spaces'!G50","v":"DT/ Art"},{"$f":"'Individual Spaces'!H50","v":97},null,null,null,-97,null,null,{"$f":"'Individual Spaces'!O50","v":0},{"$f":"'Individual Spaces'!P50","v":0},{"$f":"'Individual Spaces'!Q50","v":0},{"$f":"'Individual Spaces'!R50","v":0},null,0,{"$f":"IF(AF51=\"-\",0,ROUND((J51-VLOOKUP(B51,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B51,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B51,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B51,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J51-VLOOKUP(B51,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B51,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B51,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school art room for general and 3D art "},{"$f":"VLOOKUP($B51,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"2D work (drawing, painting). Small scale 3D work. Whole class presentations and discussions using the whiteboard."},{"$f":"VLOOKUP($B51,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B51,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Light practical"},{"$f":"VLOOKUP($B51,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"G"},{"$f":"VLOOKUP($B51,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"extensive"},{"$f":"VLOOKUP($B51,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A51","v":"DAT00"},{"$f":"'Individual Spaces'!B51","v":"DAT03"},{"$f":"'Individual Spaces'!C51","v":1117},{"$f":"'Individual Spaces'!D51","v":"Art room (3D) 2"},{"$f":"'Individual Spaces'!E51","v":0},null,{"$f":"VLOOKUP($B52,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_04"},{"$f":"VLOOKUP($B52,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Art rooms"},{"$f":"'Individual Spaces'!G51","v":"DT/ Art"},{"$f":"'Individual Spaces'!H51","v":97},null,null,null,-97,null,null,{"$f":"'Individual Spaces'!O51","v":0},{"$f":"'Individual Spaces'!P51","v":0},{"$f":"'Individual Spaces'!Q51","v":0},{"$f":"'Individual Spaces'!R51","v":0},null,0,{"$f":"IF(AF52=\"-\",0,ROUND((J52-VLOOKUP(B52,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B52,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B52,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B52,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J52-VLOOKUP(B52,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B52,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B52,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school art room for general and 3D art "},{"$f":"VLOOKUP($B52,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"2D work (drawing, painting). Small scale 3D work. Whole class presentations and discussions using the whiteboard."},{"$f":"VLOOKUP($B52,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B52,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Light practical"},{"$f":"VLOOKUP($B52,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"G"},{"$f":"VLOOKUP($B52,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"extensive"},{"$f":"VLOOKUP($B52,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A52","v":"PER02"},{"$f":"'Individual Spaces'!B52","v":"PER03"},{"$f":"'Individual Spaces'!C52","v":1118},{"$f":"'Individual Spaces'!D52","v":"Music room (fitted, extensive) 1"},{"$f":"'Individual Spaces'!E52","v":0},null,{"$f":"VLOOKUP($B53,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_55"},{"$f":"VLOOKUP($B53,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Music rooms"},{"$f":"'Individual Spaces'!G52","v":"Perf arts, hall and dining"},{"$f":"'Individual Spaces'!H52","v":69},null,null,null,-69,null,null,{"$f":"'Individual Spaces'!O52","v":0},{"$f":"'Individual Spaces'!P52","v":0},{"$f":"'Individual Spaces'!Q52","v":0},{"$f":"'Individual Spaces'!R52","v":0},null,0,{"$f":"IF(AF53=\"-\",0,ROUND((J53-VLOOKUP(B53,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B53,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(B53,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B53,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J53-VLOOKUP(B53,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B53,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},33,null,null,{"$f":"VLOOKUP($B53,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school music classroom for performance, composing and theory, with option of keyboards for all pupils"},{"$f":"VLOOKUP($B53,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Group and individual composing and music making using ICT, keyboards and percussion. Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Teacher led presentations and briefings using the whiteboard."},{"$f":"VLOOKUP($B53,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B53,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Fitted"},{"$f":"VLOOKUP($B53,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"E"},{"$f":"VLOOKUP($B53,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"extensive"},{"$f":"VLOOKUP($B53,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A53","v":"PER15"},{"$f":"'Individual Spaces'!B53","v":"PER15"},{"$f":"'Individual Spaces'!C53","v":1119},{"$f":"'Individual Spaces'!D53","v":"Drama studio 1"},{"$f":"'Individual Spaces'!E53","v":0},null,{"$f":"VLOOKUP($B54,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_24"},{"$f":"VLOOKUP($B54,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Drama studios"},{"$f":"'Individual Spaces'!G53","v":"Perf arts, hall and dining"},{"$f":"'Individual Spaces'!H53","v":97},null,null,null,-97,null,null,{"$f":"'Individual Spaces'!O53","v":0},{"$f":"'Individual Spaces'!P53","v":0},{"$f":"'Individual Spaces'!Q53","v":0},{"$f":"'Individual Spaces'!R53","v":0},null,0,{"$f":"IF(AF54=\"-\",0,ROUND((J54-VLOOKUP(B54,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B54,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":33},{"$f":"IF(VLOOKUP(B54,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B54,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J54-VLOOKUP(B54,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B54,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},37,null,null,{"$f":"VLOOKUP($B54,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school studio space for drama "},{"$f":"VLOOKUP($B54,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Drama workshops. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Pupil led rehearsals and performance to a small audience. Teacher led presentations and briefings occasionally with whiteboard."},{"$f":"VLOOKUP($B54,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B54,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Large"},{"$f":"VLOOKUP($B54,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"F1"},{"$f":"VLOOKUP($B54,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B54,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Yes "}]
[{"$f":"'Individual Spaces'!A54","v":"DAT43"},{"$f":"'Individual Spaces'!B54","v":"DAT43"},{"$f":"'Individual Spaces'!C54","v":1120},{"$f":"'Individual Spaces'!D54","v":"DT workshop 1"},{"$f":"'Individual Spaces'!E54","v":0},null,{"$f":"VLOOKUP($B55,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_40_23"},{"$f":"VLOOKUP($B55,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Design technology workshops"},{"$f":"'Individual Spaces'!G54","v":"DT/ Art"},{"$f":"'Individual Spaces'!H54","v":111},null,null,null,-111,null,null,{"$f":"'Individual Spaces'!O54","v":0},{"$f":"'Individual Spaces'!P54","v":0},{"$f":"'Individual Spaces'!Q54","v":0},{"$f":"'Individual Spaces'!R54","v":0},null,0,{"$f":"IF(AF55=\"-\",0,ROUND((J55-VLOOKUP(B55,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B55,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":29},{"$f":"IF(VLOOKUP(B55,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B55,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J55-VLOOKUP(B55,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B55,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},32,null,null,{"$f":"VLOOKUP($B55,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school workshop for working with all resistant materials, including wood, metal and plastics"},{"$f":"VLOOKUP($B55,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making with wood, plastics and some metals. Some electronics and control. Teacher demonstrations using machines and practical multibenches. Traditional and computer based drawing and design."},{"$f":"VLOOKUP($B55,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B55,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Heavy practical (workshop)"},{"$f":"VLOOKUP($B55,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"H"},{"$f":"VLOOKUP($B55,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B55,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A55","v":"DAT35"},{"$f":"'Individual Spaces'!B55","v":"DAT35"},{"$f":"'Individual Spaces'!C55","v":1121},{"$f":"'Individual Spaces'!D55","v":"Food room 1"},{"$f":"'Individual Spaces'!E55","v":0},null,{"$f":"VLOOKUP($B56,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_30"},{"$f":"VLOOKUP($B56,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Food rooms"},{"$f":"'Individual Spaces'!G55","v":"DT/ Art"},{"$f":"'Individual Spaces'!H55","v":97},null,null,null,-97,null,null,{"$f":"'Individual Spaces'!O55","v":0},{"$f":"'Individual Spaces'!P55","v":0},{"$f":"'Individual Spaces'!Q55","v":0},{"$f":"'Individual Spaces'!R55","v":0},null,0,{"$f":"IF(AF56=\"-\",0,ROUND((J56-VLOOKUP(B56,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B56,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":24},{"$f":"IF(VLOOKUP(B56,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B56,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J56-VLOOKUP(B56,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B56,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},27,null,null,{"$f":"VLOOKUP($B56,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school food room for a range of non-vocational practical cookery activities by pupils in pairs "},{"$f":"VLOOKUP($B56,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making and tasting food. Teacher practical demonstrations. Traditional and computer based design of recipes etc."},{"$f":"VLOOKUP($B56,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B56,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Heavy practical (clean)"},{"$f":"VLOOKUP($B56,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"H"},{"$f":"VLOOKUP($B56,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B56,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A56","v":"DAT20"},{"$f":"'Individual Spaces'!B56","v":"DAT22"},{"$f":"'Individual Spaces'!C56","v":1122},{"$f":"'Individual Spaces'!D56","v":"DT studio (graphic products) 1"},{"$f":"'Individual Spaces'!E56","v":0},null,{"$f":"VLOOKUP($B57,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_40_22"},{"$f":"VLOOKUP($B57,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Design Technology studios"},{"$f":"'Individual Spaces'!G56","v":"DT/ Art"},{"$f":"'Individual Spaces'!H56","v":83},null,null,null,-83,null,null,{"$f":"'Individual Spaces'!O56","v":0},{"$f":"'Individual Spaces'!P56","v":0},{"$f":"'Individual Spaces'!Q56","v":0},{"$f":"'Individual Spaces'!R56","v":0},null,0,{"$f":"IF(AF57=\"-\",0,ROUND((J57-VLOOKUP(B57,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B57,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":25},{"$f":"IF(VLOOKUP(B57,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B57,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J57-VLOOKUP(B57,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B57,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},28,null,null,{"$f":"VLOOKUP($B57,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school room for graphics and small scale product design"},{"$f":"VLOOKUP($B57,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Small scale making with card and some plastics. Traditional and computer based drawing and design."},{"$f":"VLOOKUP($B57,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B57,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Light practical"},{"$f":"VLOOKUP($B57,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"G"},{"$f":"VLOOKUP($B57,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B57,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A57","v":"DAT20"},{"$f":"'Individual Spaces'!B57","v":"DAT25"},{"$f":"'Individual Spaces'!C57","v":1123},{"$f":"'Individual Spaces'!D57","v":"DT studio (textiles) 1"},{"$f":"'Individual Spaces'!E57","v":0},null,{"$f":"VLOOKUP($B58,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_40_22"},{"$f":"VLOOKUP($B58,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Design Technology studios"},{"$f":"'Individual Spaces'!G57","v":"DT/ Art"},{"$f":"'Individual Spaces'!H57","v":83},null,null,null,-83,null,null,{"$f":"'Individual Spaces'!O57","v":0},{"$f":"'Individual Spaces'!P57","v":0},{"$f":"'Individual Spaces'!Q57","v":0},{"$f":"'Individual Spaces'!R57","v":0},null,0,{"$f":"IF(AF58=\"-\",0,ROUND((J58-VLOOKUP(B58,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B58,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":25},{"$f":"IF(VLOOKUP(B58,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B58,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J58-VLOOKUP(B58,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B58,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},28,null,null,{"$f":"VLOOKUP($B58,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school room for working with a range of 'dry' textiles"},{"$f":"VLOOKUP($B58,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making with textiles including traditional and computerised sewing and knitting machines. Traditional and computer based drawing and design."},{"$f":"VLOOKUP($B58,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Basic teaching"},{"$f":"VLOOKUP($B58,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Light practical"},{"$f":"VLOOKUP($B58,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"G"},{"$f":"VLOOKUP($B58,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B58,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A58","v":0},{"$f":"'Individual Spaces'!B58","v":0},{"$f":"'Individual Spaces'!C58","v":0},{"$f":"'Individual Spaces'!D58","v":0},{"$f":"'Individual Spaces'!E58","v":"Specialist Practical Total : "},null,{"$f":"VLOOKUP($B59,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B59,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G58","v":0},{"$f":"'Individual Spaces'!H58","v":1965},null,null,null,-1965,null,null,{"$f":"'Individual Spaces'!O58","v":0},{"$f":"'Individual Spaces'!P58","v":0},{"$f":"'Individual Spaces'!Q58","v":0},{"$f":"'Individual Spaces'!R58","v":0},null,0,{"$f":"IF(AF59=\"-\",0,ROUND((J59-VLOOKUP(B59,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B59,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B59,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B59,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J59-VLOOKUP(B59,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B59,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B59,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B59,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B59,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B59,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B59,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B59,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B59,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A59","v":"HAL01"},{"$f":"'Individual Spaces'!B59","v":"HAL03"},{"$f":"'Individual Spaces'!C59","v":2001},{"$f":"'Individual Spaces'!D59","v":"Assembly halls, secondary (with bleachers) 1"},{"$f":"'Individual Spaces'!E59","v":0},null,{"$f":"VLOOKUP($B60,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_05"},{"$f":"VLOOKUP($B60,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Assembly halls"},{"$f":"'Individual Spaces'!G59","v":"Perf arts, hall and dining"},{"$f":"'Individual Spaces'!H59","v":197},null,null,null,-197,null,null,{"$f":"'Individual Spaces'!O59","v":0},{"$f":"'Individual Spaces'!P59","v":0},{"$f":"'Individual Spaces'!Q59","v":0},{"$f":"'Individual Spaces'!R59","v":0},null,0,{"$f":"IF(AF60=\"-\",0,ROUND((J60-VLOOKUP(B60,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B60,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B60,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B60,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J60-VLOOKUP(B60,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B60,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B60,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Multi-purpose hall for assembly, PE and exams and cold food dining, in secondary schools, served by adjacent bleacher seating"},{"$f":"VLOOKUP($B60,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"School assemblies (various sizes) using PA system and whiteboard. Dining of cold food from nearby dining area. Music and drama rehearsals and performance. Parent evenings. Some gymnastic practise and performance, table tennis and recreational trampolining if 6.9m high. Whole year group examinations."},{"$f":"VLOOKUP($B60,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Halls and dining"},{"$f":"VLOOKUP($B60,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Large"},{"$f":"VLOOKUP($B60,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B60,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B60,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Yes"}]
[{"$f":"'Individual Spaces'!A60","v":"SPH00"},{"$f":"'Individual Spaces'!B60","v":"SPH04"},{"$f":"'Individual Spaces'!C60","v":2002},{"$f":"'Individual Spaces'!D60","v":"Sports hall, school (4-court) 1"},{"$f":"'Individual Spaces'!E60","v":0},null,{"$f":"VLOOKUP($B61,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_42_40_82"},{"$f":"VLOOKUP($B61,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Sports halls"},{"$f":"'Individual Spaces'!G60","v":"Sports/ PE"},{"$f":"'Individual Spaces'!H60","v":594},null,null,null,-594,null,null,{"$f":"'Individual Spaces'!O60","v":0},{"$f":"'Individual Spaces'!P60","v":0},{"$f":"'Individual Spaces'!Q60","v":0},{"$f":"'Individual Spaces'!R60","v":0},null,0,{"$f":"IF(AF61=\"-\",0,ROUND((J61-VLOOKUP(B61,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B61,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":331},{"$f":"IF(VLOOKUP(B61,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B61,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J61-VLOOKUP(B61,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B61,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},348,null,null,{"$f":"VLOOKUP($B61,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"18m x 33m sports hall for secondary school PE activities, exams and some recreational community use"},{"$f":"VLOOKUP($B61,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Individual activities including Athletics (practice only) and gymnastics. Team games including badminton; basketball; Five-A-Side football / futsal; indoor tennis; judo; karate; korfball; mini handball; netball (practice only); short tennis; table tennis and volleyball."},{"$f":"VLOOKUP($B61,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Halls and dining"},{"$f":"VLOOKUP($B61,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Large"},{"$f":"VLOOKUP($B61,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":0},{"$f":"VLOOKUP($B61,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B61,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Yes"}]
[{"$f":"'Individual Spaces'!A61","v":"ACT05"},{"$f":"'Individual Spaces'!B61","v":"ACT07"},{"$f":"'Individual Spaces'!C61","v":2003},{"$f":"'Individual Spaces'!D61","v":"Activity studio (10 x 15) 1"},{"$f":"'Individual Spaces'!E61","v":0},null,{"$f":"VLOOKUP($B62,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_01"},{"$f":"VLOOKUP($B62,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Activity studios"},{"$f":"'Individual Spaces'!G61","v":"Sports/ PE"},{"$f":"'Individual Spaces'!H61","v":150},null,null,null,-150,null,null,{"$f":"'Individual Spaces'!O61","v":0},{"$f":"'Individual Spaces'!P61","v":0},{"$f":"'Individual Spaces'!Q61","v":0},{"$f":"'Individual Spaces'!R61","v":0},null,0,{"$f":"IF(AF62=\"-\",0,ROUND((J62-VLOOKUP(B62,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B62,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":14},{"$f":"IF(VLOOKUP(B62,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B62,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J62-VLOOKUP(B62,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B62,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},16,null,null,{"$f":"VLOOKUP($B62,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"15m x 10m space for movement, dance, gymnastics and other PE activities, exams and optional community use, but not dining"},{"$f":"VLOOKUP($B62,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Dance. Gymnastics. Occasional use for exams and exhibitions. Table tennis."},{"$f":"VLOOKUP($B62,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Halls and dining"},{"$f":"VLOOKUP($B62,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Large"},{"$f":"VLOOKUP($B62,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":0},{"$f":"VLOOKUP($B62,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B62,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Yes"}]
[{"$f":"'Individual Spaces'!A62","v":"DIN01"},{"$f":"'Individual Spaces'!B62","v":"DIN01"},{"$f":"'Individual Spaces'!C62","v":2004},{"$f":"'Individual Spaces'!D62","v":"Dining hall 1"},{"$f":"'Individual Spaces'!E62","v":0},null,{"$f":"VLOOKUP($B63,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_40_20_22"},{"$f":"VLOOKUP($B63,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Dining halls"},{"$f":"'Individual Spaces'!G62","v":"Perf arts, hall and dining"},{"$f":"'Individual Spaces'!H62","v":210},null,null,null,-210,null,null,{"$f":"'Individual Spaces'!O62","v":0},{"$f":"'Individual Spaces'!P62","v":0},{"$f":"'Individual Spaces'!Q62","v":0},{"$f":"'Individual Spaces'!R62","v":0},null,0,{"$f":"IF(AF63=\"-\",0,ROUND((J63-VLOOKUP(B63,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B63,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B63,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B63,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J63-VLOOKUP(B63,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B63,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B63,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Large space permanently set out for dining"},{"$f":"VLOOKUP($B63,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Dining for hot and cold meals from servery area(s) within space or adjacent. Can also be used for school events such as parents meetings/presentations, teacher consultations or whole school teacher meetings. "},{"$f":"VLOOKUP($B63,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Halls and dining"},{"$f":"VLOOKUP($B63,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Large"},{"$f":"VLOOKUP($B63,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B63,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B63,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Optional "}]
[{"$f":"'Individual Spaces'!A63","v":"DIN02"},{"$f":"'Individual Spaces'!B63","v":"DIN02"},{"$f":"'Individual Spaces'!C63","v":2005},{"$f":"'Individual Spaces'!D63","v":"Informal dining space 1"},{"$f":"'Individual Spaces'!E63","v":0},null,{"$f":"VLOOKUP($B64,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_40_20_43"},{"$f":"VLOOKUP($B64,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Informal dining spaces"},{"$f":"'Individual Spaces'!G63","v":"Balance"},{"$f":"'Individual Spaces'!H63","v":111},null,null,null,-111,null,null,{"$f":"'Individual Spaces'!O63","v":0},{"$f":"'Individual Spaces'!P63","v":0},{"$f":"'Individual Spaces'!Q63","v":0},{"$f":"'Individual Spaces'!R63","v":0},null,0,{"$f":"IF(AF64=\"-\",0,ROUND((J64-VLOOKUP(B64,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B64,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":99},{"$f":"IF(VLOOKUP(B64,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B64,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J64-VLOOKUP(B64,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B64,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},109,null,null,{"$f":"VLOOKUP($B64,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Open area for pupils to socialise and eat snacks and sandwiches in secondary schools"},{"$f":"VLOOKUP($B64,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Socialising and dining of drinks and cold meals, typically from local servery area(s) within space or adjacent. Can also be used for school events such as parents meetings/presentations, teacher consultations or whole school teacher meetings. "},{"$f":"VLOOKUP($B64,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Halls and dining"},{"$f":"VLOOKUP($B64,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B64,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"A"},{"$f":"VLOOKUP($B64,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B64,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A64","v":0},{"$f":"'Individual Spaces'!B64","v":0},{"$f":"'Individual Spaces'!C64","v":0},{"$f":"'Individual Spaces'!D64","v":0},{"$f":"'Individual Spaces'!E64","v":"Large Spaces Total : "},null,{"$f":"VLOOKUP($B65,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B65,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G64","v":0},{"$f":"'Individual Spaces'!H64","v":1262},null,null,null,-1262,null,null,{"$f":"'Individual Spaces'!O64","v":0},{"$f":"'Individual Spaces'!P64","v":0},{"$f":"'Individual Spaces'!Q64","v":0},{"$f":"'Individual Spaces'!R64","v":0},null,0,{"$f":"IF(AF65=\"-\",0,ROUND((J65-VLOOKUP(B65,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B65,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B65,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B65,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J65-VLOOKUP(B65,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B65,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B65,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B65,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B65,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B65,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B65,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B65,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B65,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A65","v":"LIB05"},{"$f":"'Individual Spaces'!B65","v":"LIB05"},{"$f":"'Individual Spaces'!C65","v":3001},{"$f":"'Individual Spaces'!D65","v":"Library resource centre (LRC) 1"},{"$f":"'Individual Spaces'!E65","v":0},null,{"$f":"VLOOKUP($B66,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_75_45"},{"$f":"VLOOKUP($B66,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Learning resource centres"},{"$f":"'Individual Spaces'!G65","v":"Balance"},{"$f":"'Individual Spaces'!H65","v":146},null,null,null,-146,null,null,{"$f":"'Individual Spaces'!O65","v":0},{"$f":"'Individual Spaces'!P65","v":0},{"$f":"'Individual Spaces'!Q65","v":0},{"$f":"'Individual Spaces'!R65","v":0},null,0,{"$f":"IF(AF66=\"-\",0,ROUND((J66-VLOOKUP(B66,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B66,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":55},{"$f":"IF(VLOOKUP(B66,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B66,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J66-VLOOKUP(B66,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B66,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},61,null,null,{"$f":"VLOOKUP($B66,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school library and careers area"},{"$f":"VLOOKUP($B66,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Individual study and research using books and ICT. Informal reading and use of reference resources. Lending books and PC resources. Whole class group for library skills."},{"$f":"VLOOKUP($B66,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Learning resources"},{"$f":"VLOOKUP($B66,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Fitted"},{"$f":"VLOOKUP($B66,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"F"},{"$f":"VLOOKUP($B66,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B66,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A66","v":"LIB07"},{"$f":"'Individual Spaces'!B66","v":"LIB06"},{"$f":"'Individual Spaces'!C66","v":3002},{"$f":"'Individual Spaces'!D66","v":"Study space, room (sixth form) 1"},{"$f":"'Individual Spaces'!E66","v":0},null,{"$f":"VLOOKUP($B67,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_10_84"},{"$f":"VLOOKUP($B67,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Study spaces"},{"$f":"'Individual Spaces'!G66","v":"Balance"},{"$f":"'Individual Spaces'!H66","v":69},null,null,null,-69,null,null,{"$f":"'Individual Spaces'!O66","v":0},{"$f":"'Individual Spaces'!P66","v":0},{"$f":"'Individual Spaces'!Q66","v":0},{"$f":"'Individual Spaces'!R66","v":0},null,0,{"$f":"IF(AF67=\"-\",0,ROUND((J67-VLOOKUP(B67,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B67,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":42},{"$f":"IF(VLOOKUP(B67,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B67,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J67-VLOOKUP(B67,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B67,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},47,null,null,{"$f":"VLOOKUP($B67,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secondary school study area for sixth form pupils"},{"$f":"VLOOKUP($B67,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Individual study (including use of ICT). Reading and use of reference resources. "},{"$f":"VLOOKUP($B67,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Learning resources"},{"$f":"VLOOKUP($B67,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B67,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"B"},{"$f":"VLOOKUP($B67,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B67,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A67","v":"RES21"},{"$f":"'Individual Spaces'!B67","v":"RES21"},{"$f":"'Individual Spaces'!C67","v":3003},{"$f":"'Individual Spaces'!D67","v":"Heavy practical resource (kiln) 1"},{"$f":"'Individual Spaces'!E67","v":0},null,{"$f":"VLOOKUP($B68,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_75_37"},{"$f":"VLOOKUP($B68,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Heavy practical resource spaces"},{"$f":"'Individual Spaces'!G67","v":"DT/ Art"},{"$f":"'Individual Spaces'!H67","v":4},null,null,null,-4,null,null,{"$f":"'Individual Spaces'!O67","v":0},{"$f":"'Individual Spaces'!P67","v":0},{"$f":"'Individual Spaces'!Q67","v":0},{"$f":"'Individual Spaces'!R67","v":0},null,0,{"$f":"IF(AF68=\"-\",0,ROUND((J68-VLOOKUP(B68,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B68,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B68,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B68,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J68-VLOOKUP(B68,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B68,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B68,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Room for kiln(s) and drying racks"},{"$f":"VLOOKUP($B68,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Firing and glazing articles in kiln(s). Storing clay articles awaiting firing."},{"$f":"VLOOKUP($B68,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Learning resources"},{"$f":"VLOOKUP($B68,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Heavy practical (workshop)"},{"$f":"VLOOKUP($B68,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B68,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B68,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A68","v":"RES12"},{"$f":"'Individual Spaces'!B68","v":"RES12"},{"$f":"'Individual Spaces'!C68","v":3004},{"$f":"'Individual Spaces'!D68","v":"Music practice room 1"},{"$f":"'Individual Spaces'!E68","v":0},null,{"$f":"VLOOKUP($B69,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_75_55"},{"$f":"VLOOKUP($B69,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Music practice rooms"},{"$f":"'Individual Spaces'!G68","v":"Perf arts, hall and dining"},{"$f":"'Individual Spaces'!H68","v":8},null,null,null,-8,null,null,{"$f":"'Individual Spaces'!O68","v":0},{"$f":"'Individual Spaces'!P68","v":0},{"$f":"'Individual Spaces'!Q68","v":0},{"$f":"'Individual Spaces'!R68","v":0},null,0,{"$f":"IF(AF69=\"-\",0,ROUND((J69-VLOOKUP(B69,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B69,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(B69,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B69,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J69-VLOOKUP(B69,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B69,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},5,null,null,{"$f":"VLOOKUP($B69,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Room for music practice/ lessons"},{"$f":"VLOOKUP($B69,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Individual music lessons. Individuals/small groups composing and practising music using a variety of percussion instruments and electronic keyboard."},{"$f":"VLOOKUP($B69,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Learning resources"},{"$f":"VLOOKUP($B69,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B69,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"B"},{"$f":"VLOOKUP($B69,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B69,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A69","v":"RES12"},{"$f":"'Individual Spaces'!B69","v":"RES13"},{"$f":"'Individual Spaces'!C69","v":3005},{"$f":"'Individual Spaces'!D69","v":"Music practice room (extensive) 1"},{"$f":"'Individual Spaces'!E69","v":0},null,{"$f":"VLOOKUP($B70,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_75_55"},{"$f":"VLOOKUP($B70,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Music practice rooms"},{"$f":"'Individual Spaces'!G69","v":"Perf arts, hall and dining"},{"$f":"'Individual Spaces'!H69","v":16},null,null,null,{"$f":"M70-J70","v":-16},null,null,{"$f":"'Individual Spaces'!O69","v":0},{"$f":"'Individual Spaces'!P69","v":0},{"$f":"'Individual Spaces'!Q69","v":0},{"$f":"'Individual Spaces'!R69","v":0},null,{"$f":"Q70","v":0},{"$f":"IF(AF70=\"-\",0,ROUND((J70-VLOOKUP(B70,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B70,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":7},{"$f":"IF(VLOOKUP(B70,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B70,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J70-VLOOKUP(B70,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B70,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},{"$f":"IF(W70>200,ROUND(W70*1.05,0),ROUNDUP(W70*1.1,0))","v":8},null,null,{"$f":"VLOOKUP($B70,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Room for music practice/ lesson, including drums"},{"$f":"VLOOKUP($B70,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Individual music lessons. Individual/small groups composing and practising music using a variety of percussion instruments, full drum kit and electronic keyboard."},{"$f":"VLOOKUP($B70,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Learning resources"},{"$f":"VLOOKUP($B70,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B70,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B70,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"extensive"},{"$f":"VLOOKUP($B70,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A70","v":"RES12"},{"$f":"'Individual Spaces'!B70","v":"RES13"},{"$f":"'Individual Spaces'!C70","v":3006},{"$f":"'Individual Spaces'!D70","v":"Music practice room (extensive) 2"},{"$f":"'Individual Spaces'!E70","v":0},null,{"$f":"VLOOKUP($B71,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_75_55"},{"$f":"VLOOKUP($B71,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Music practice rooms"},{"$f":"'Individual Spaces'!G70","v":"Perf arts, hall and dining"},{"$f":"'Individual Spaces'!H70","v":16},null,null,null,-16,null,null,{"$f":"'Individual Spaces'!O70","v":0},{"$f":"'Individual Spaces'!P70","v":0},{"$f":"'Individual Spaces'!Q70","v":0},{"$f":"'Individual Spaces'!R70","v":0},null,0,{"$f":"IF(AF71=\"-\",0,ROUND((J71-VLOOKUP(B71,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B71,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":7},{"$f":"IF(VLOOKUP(B71,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B71,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J71-VLOOKUP(B71,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B71,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},8,null,null,{"$f":"VLOOKUP($B71,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Room for music practice/ lesson, including drums"},{"$f":"VLOOKUP($B71,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Individual music lessons. Individual/small groups composing and practising music using a variety of percussion instruments, full drum kit and electronic keyboard."},{"$f":"VLOOKUP($B71,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Learning resources"},{"$f":"VLOOKUP($B71,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B71,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B71,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"extensive"},{"$f":"VLOOKUP($B71,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A71","v":"RES14"},{"$f":"'Individual Spaces'!B71","v":"RES14"},{"$f":"'Individual Spaces'!C71","v":3007},{"$f":"'Individual Spaces'!D71","v":"Recording control space 1"},{"$f":"'Individual Spaces'!E71","v":0},null,{"$f":"VLOOKUP($B72,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_40_65_70"},{"$f":"VLOOKUP($B72,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Recording control spaces"},{"$f":"'Individual Spaces'!G71","v":"Perf arts, hall and dining"},{"$f":"'Individual Spaces'!H71","v":8},null,null,null,-8,null,null,{"$f":"'Individual Spaces'!O71","v":0},{"$f":"'Individual Spaces'!P71","v":0},{"$f":"'Individual Spaces'!Q71","v":0},{"$f":"'Individual Spaces'!R71","v":0},null,0,{"$f":"IF(AF72=\"-\",0,ROUND((J72-VLOOKUP(B72,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B72,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(B72,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B72,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J72-VLOOKUP(B72,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B72,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},5,null,null,{"$f":"VLOOKUP($B72,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Room housing specialist recording equipment"},{"$f":"VLOOKUP($B72,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Using analogue or digital equipment to record music played in adjacent space(s) and to create/edit digital music."},{"$f":"VLOOKUP($B72,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Learning resources"},{"$f":"VLOOKUP($B72,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Fitted"},{"$f":"VLOOKUP($B72,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"B"},{"$f":"VLOOKUP($B72,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B72,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A72","v":"RES16"},{"$f":"'Individual Spaces'!B72","v":"RES16"},{"$f":"'Individual Spaces'!C72","v":3008},{"$f":"'Individual Spaces'!D72","v":"Lighting and audio control space 1"},{"$f":"'Individual Spaces'!E72","v":0},null,{"$f":"VLOOKUP($B73,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_40_65_47"},{"$f":"VLOOKUP($B73,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Lighting and audio control spaces"},{"$f":"'Individual Spaces'!G72","v":"Perf arts, hall and dining"},{"$f":"'Individual Spaces'!H72","v":6},null,null,null,-6,null,null,{"$f":"'Individual Spaces'!O72","v":0},{"$f":"'Individual Spaces'!P72","v":0},{"$f":"'Individual Spaces'!Q72","v":0},{"$f":"'Individual Spaces'!R72","v":0},null,0,{"$f":"IF(AF73=\"-\",0,ROUND((J73-VLOOKUP(B73,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B73,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":3},{"$f":"IF(VLOOKUP(B73,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B73,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J73-VLOOKUP(B73,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B73,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},4,null,null,{"$f":"VLOOKUP($B73,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Room for controlling lighting and audio systems in adjacent performance space"},{"$f":"VLOOKUP($B73,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Using analogue or digital equipment to control stage lighting and sound system in adjacent hall."},{"$f":"VLOOKUP($B73,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Learning resources"},{"$f":"VLOOKUP($B73,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Fitted"},{"$f":"VLOOKUP($B73,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"B"},{"$f":"VLOOKUP($B73,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B73,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A73","v":"SEN02"},{"$f":"'Individual Spaces'!B73","v":"SEN02"},{"$f":"'Individual Spaces'!C73","v":3009},{"$f":"'Individual Spaces'!D73","v":"Medical treatment (MI) room 1"},{"$f":"'Individual Spaces'!E73","v":0},null,{"$f":"VLOOKUP($B74,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_10_53"},{"$f":"VLOOKUP($B74,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Medical treatment rooms"},{"$f":"'Individual Spaces'!G73","v":"Balance"},{"$f":"'Individual Spaces'!H73","v":12},null,null,null,-12,null,null,{"$f":"'Individual Spaces'!O73","v":0},{"$f":"'Individual Spaces'!P73","v":0},{"$f":"'Individual Spaces'!Q73","v":0},{"$f":"'Individual Spaces'!R73","v":0},null,0,{"$f":"IF(AF74=\"-\",0,ROUND((J74-VLOOKUP(B74,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B74,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":5},{"$f":"IF(VLOOKUP(B74,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B74,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J74-VLOOKUP(B74,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B74,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},6,null,null,{"$f":"VLOOKUP($B74,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Room for physio- and other therapy and medical inspections"},{"$f":"VLOOKUP($B74,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administering drug treatments to pupils. Medical inspection by external practitioners. Physio- or speech therapy for pupils with special needs and disabilities."},{"$f":"VLOOKUP($B74,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Learning resources"},{"$f":"VLOOKUP($B74,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B74,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B74,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B74,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Optional"}]
[{"$f":"'Individual Spaces'!A74","v":"SEN20"},{"$f":"'Individual Spaces'!B74","v":"SEN20"},{"$f":"'Individual Spaces'!C74","v":3010},{"$f":"'Individual Spaces'!D74","v":"SEN resource space 1"},{"$f":"'Individual Spaces'!E74","v":0},null,{"$f":"VLOOKUP($B75,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_75_82"},{"$f":"VLOOKUP($B75,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"SEN resource spaces"},{"$f":"'Individual Spaces'!G74","v":"Balance"},{"$f":"'Individual Spaces'!H74","v":16},null,null,null,-16,null,null,{"$f":"'Individual Spaces'!O74","v":0},{"$f":"'Individual Spaces'!P74","v":0},{"$f":"'Individual Spaces'!Q74","v":0},{"$f":"'Individual Spaces'!R74","v":0},null,0,{"$f":"IF(AF75=\"-\",0,ROUND((J75-VLOOKUP(B75,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B75,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":7},{"$f":"IF(VLOOKUP(B75,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B75,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J75-VLOOKUP(B75,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B75,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},8,null,null,{"$f":"VLOOKUP($B75,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Small room for assistance with individuals and groups with SEN"},{"$f":"VLOOKUP($B75,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Individual therapy and counselling. Individual/small group learning support. Staff meetings."},{"$f":"VLOOKUP($B75,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Learning resources"},{"$f":"VLOOKUP($B75,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B75,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B75,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B75,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A75","v":"RES00"},{"$f":"'Individual Spaces'!B75","v":"RES00"},{"$f":"'Individual Spaces'!C75","v":3011},{"$f":"'Individual Spaces'!D75","v":"Small group room 1"},{"$f":"'Individual Spaces'!E75","v":0},null,{"$f":"VLOOKUP($B76,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_75_80"},{"$f":"VLOOKUP($B76,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Small group rooms"},{"$f":"'Individual Spaces'!G75","v":"Balance"},{"$f":"'Individual Spaces'!H75","v":9},null,null,null,-9,null,null,{"$f":"'Individual Spaces'!O75","v":0},{"$f":"'Individual Spaces'!P75","v":0},{"$f":"'Individual Spaces'!Q75","v":0},{"$f":"'Individual Spaces'!R75","v":0},null,0,{"$f":"IF(AF76=\"-\",0,ROUND((J76-VLOOKUP(B76,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B76,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(B76,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B76,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J76-VLOOKUP(B76,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B76,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},5,null,null,{"$f":"VLOOKUP($B76,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Room for assistance with individuals and small groups "},{"$f":"VLOOKUP($B76,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Individual/ small group learning support. One to one counselling. Privacy required."},{"$f":"VLOOKUP($B76,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Learning resources"},{"$f":"VLOOKUP($B76,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B76,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"B"},{"$f":"VLOOKUP($B76,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B76,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A76","v":"RES00"},{"$f":"'Individual Spaces'!B76","v":"RES00"},{"$f":"'Individual Spaces'!C76","v":3012},{"$f":"'Individual Spaces'!D76","v":"Small group room 2"},{"$f":"'Individual Spaces'!E76","v":0},null,{"$f":"VLOOKUP($B77,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_75_80"},{"$f":"VLOOKUP($B77,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Small group rooms"},{"$f":"'Individual Spaces'!G76","v":"Balance"},{"$f":"'Individual Spaces'!H76","v":9},null,null,null,-9,null,null,{"$f":"'Individual Spaces'!O76","v":0},{"$f":"'Individual Spaces'!P76","v":0},{"$f":"'Individual Spaces'!Q76","v":0},{"$f":"'Individual Spaces'!R76","v":0},null,0,{"$f":"IF(AF77=\"-\",0,ROUND((J77-VLOOKUP(B77,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B77,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(B77,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B77,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J77-VLOOKUP(B77,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B77,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},5,null,null,{"$f":"VLOOKUP($B77,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Room for assistance with individuals and small groups "},{"$f":"VLOOKUP($B77,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Individual/ small group learning support. One to one counselling. Privacy required."},{"$f":"VLOOKUP($B77,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Learning resources"},{"$f":"VLOOKUP($B77,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B77,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"B"},{"$f":"VLOOKUP($B77,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B77,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A77","v":"RES00"},{"$f":"'Individual Spaces'!B77","v":"RES00"},{"$f":"'Individual Spaces'!C77","v":3013},{"$f":"'Individual Spaces'!D77","v":"Small group room 3"},{"$f":"'Individual Spaces'!E77","v":0},null,{"$f":"VLOOKUP($B78,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_75_80"},{"$f":"VLOOKUP($B78,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Small group rooms"},{"$f":"'Individual Spaces'!G77","v":"Balance"},{"$f":"'Individual Spaces'!H77","v":9},null,null,null,-9,null,null,{"$f":"'Individual Spaces'!O77","v":0},{"$f":"'Individual Spaces'!P77","v":0},{"$f":"'Individual Spaces'!Q77","v":0},{"$f":"'Individual Spaces'!R77","v":0},null,0,{"$f":"IF(AF78=\"-\",0,ROUND((J78-VLOOKUP(B78,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B78,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(B78,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B78,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J78-VLOOKUP(B78,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B78,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},5,null,null,{"$f":"VLOOKUP($B78,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Room for assistance with individuals and small groups "},{"$f":"VLOOKUP($B78,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Individual/ small group learning support. One to one counselling. Privacy required."},{"$f":"VLOOKUP($B78,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Learning resources"},{"$f":"VLOOKUP($B78,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B78,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"B"},{"$f":"VLOOKUP($B78,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B78,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A78","v":"RES00"},{"$f":"'Individual Spaces'!B78","v":"RES00"},{"$f":"'Individual Spaces'!C78","v":3014},{"$f":"'Individual Spaces'!D78","v":"Small group room 4"},{"$f":"'Individual Spaces'!E78","v":0},null,{"$f":"VLOOKUP($B79,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_75_80"},{"$f":"VLOOKUP($B79,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Small group rooms"},{"$f":"'Individual Spaces'!G78","v":"Balance"},{"$f":"'Individual Spaces'!H78","v":9},null,null,null,-9,null,null,{"$f":"'Individual Spaces'!O78","v":0},{"$f":"'Individual Spaces'!P78","v":0},{"$f":"'Individual Spaces'!Q78","v":0},{"$f":"'Individual Spaces'!R78","v":0},null,0,{"$f":"IF(AF79=\"-\",0,ROUND((J79-VLOOKUP(B79,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B79,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(B79,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B79,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J79-VLOOKUP(B79,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B79,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},5,null,null,{"$f":"VLOOKUP($B79,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Room for assistance with individuals and small groups "},{"$f":"VLOOKUP($B79,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Individual/ small group learning support. One to one counselling. Privacy required."},{"$f":"VLOOKUP($B79,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Learning resources"},{"$f":"VLOOKUP($B79,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B79,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"B"},{"$f":"VLOOKUP($B79,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B79,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A79","v":"RES00"},{"$f":"'Individual Spaces'!B79","v":"RES04"},{"$f":"'Individual Spaces'!C79","v":3015},{"$f":"'Individual Spaces'!D79","v":"Small group room (large SEN etc.) 1"},{"$f":"'Individual Spaces'!E79","v":0},null,{"$f":"VLOOKUP($B80,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_75_80"},{"$f":"VLOOKUP($B80,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Small group rooms"},{"$f":"'Individual Spaces'!G79","v":"Balance"},{"$f":"'Individual Spaces'!H79","v":16},null,null,null,-16,null,null,{"$f":"'Individual Spaces'!O79","v":0},{"$f":"'Individual Spaces'!P79","v":0},{"$f":"'Individual Spaces'!Q79","v":0},{"$f":"'Individual Spaces'!R79","v":0},null,0,{"$f":"IF(AF80=\"-\",0,ROUND((J80-VLOOKUP(B80,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B80,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":9},{"$f":"IF(VLOOKUP(B80,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B80,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J80-VLOOKUP(B80,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B80,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},10,null,null,{"$f":"VLOOKUP($B80,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Larger room for assistance with individuals and groups, typically with SEN"},{"$f":"VLOOKUP($B80,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Individual/ small group learning support. One to one counselling. Privacy required."},{"$f":"VLOOKUP($B80,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Learning resources"},{"$f":"VLOOKUP($B80,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B80,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"B"},{"$f":"VLOOKUP($B80,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"standard"},{"$f":"VLOOKUP($B80,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A80","v":0},{"$f":"'Individual Spaces'!B80","v":0},{"$f":"'Individual Spaces'!C80","v":0},{"$f":"'Individual Spaces'!D80","v":0},{"$f":"'Individual Spaces'!E80","v":"Learning Resources Total : "},null,{"$f":"VLOOKUP($B81,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B81,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G80","v":0},{"$f":"'Individual Spaces'!H80","v":353},null,null,null,-353,null,null,{"$f":"'Individual Spaces'!O80","v":0},{"$f":"'Individual Spaces'!P80","v":0},{"$f":"'Individual Spaces'!Q80","v":0},{"$f":"'Individual Spaces'!R80","v":0},null,0,{"$f":"IF(AF81=\"-\",0,ROUND((J81-VLOOKUP(B81,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B81,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B81,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B81,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J81-VLOOKUP(B81,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B81,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B81,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B81,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B81,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B81,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B81,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B81,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B81,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A81","v":"OFF30"},{"$f":"'Individual Spaces'!B81","v":"OFF33"},{"$f":"'Individual Spaces'!C81","v":4001},{"$f":"'Individual Spaces'!D81","v":"Staff workrooms (teaching staff) 1"},{"$f":"'Individual Spaces'!E81","v":0},null,{"$f":"VLOOKUP($B82,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_20_86"},{"$f":"VLOOKUP($B82,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Staff workrooms"},{"$f":"'Individual Spaces'!G81","v":"Mathematics"},{"$f":"'Individual Spaces'!H81","v":19},null,null,null,-19,null,null,{"$f":"'Individual Spaces'!O81","v":0},{"$f":"'Individual Spaces'!P81","v":0},{"$f":"'Individual Spaces'!Q81","v":0},{"$f":"'Individual Spaces'!R81","v":0},null,0,{"$f":"IF(AF82=\"-\",0,ROUND((J82-VLOOKUP(B82,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B82,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":7},{"$f":"IF(VLOOKUP(B82,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B82,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J82-VLOOKUP(B82,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B82,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":7},8,null,null,{"$f":"VLOOKUP($B82,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Space for staff for desk-based work and informal meetings or office/workroom, with space for repair of equipment"},{"$f":"VLOOKUP($B82,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Lesson preparation and research mainly using ICT with a hot desk arrangement. Marking and recording pupils work. Storage of some of staff's personal and teaching resources. Team meeting and discussions."},{"$f":"VLOOKUP($B82,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B82,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B82,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"D"},{"$f":"VLOOKUP($B82,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B82,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A82","v":"OFF30"},{"$f":"'Individual Spaces'!B82","v":"OFF33"},{"$f":"'Individual Spaces'!C82","v":4002},{"$f":"'Individual Spaces'!D82","v":"Staff workrooms (teaching staff) 2"},{"$f":"'Individual Spaces'!E82","v":0},null,{"$f":"VLOOKUP($B83,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_20_86"},{"$f":"VLOOKUP($B83,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Staff workrooms"},{"$f":"'Individual Spaces'!G82","v":"English"},{"$f":"'Individual Spaces'!H82","v":19},null,null,null,-19,null,null,{"$f":"'Individual Spaces'!O82","v":0},{"$f":"'Individual Spaces'!P82","v":0},{"$f":"'Individual Spaces'!Q82","v":0},{"$f":"'Individual Spaces'!R82","v":0},null,0,{"$f":"IF(AF83=\"-\",0,ROUND((J83-VLOOKUP(B83,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B83,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":7},{"$f":"IF(VLOOKUP(B83,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B83,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J83-VLOOKUP(B83,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B83,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":7},8,null,null,{"$f":"VLOOKUP($B83,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Space for staff for desk-based work and informal meetings or office/workroom, with space for repair of equipment"},{"$f":"VLOOKUP($B83,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Lesson preparation and research mainly using ICT with a hot desk arrangement. Marking and recording pupils work. Storage of some of staff's personal and teaching resources. Team meeting and discussions."},{"$f":"VLOOKUP($B83,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B83,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B83,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"D"},{"$f":"VLOOKUP($B83,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B83,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A83","v":"OFF30"},{"$f":"'Individual Spaces'!B83","v":"OFF33"},{"$f":"'Individual Spaces'!C83","v":4003},{"$f":"'Individual Spaces'!D83","v":"Staff workrooms (teaching staff) 3"},{"$f":"'Individual Spaces'!E83","v":0},null,{"$f":"VLOOKUP($B84,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_20_86"},{"$f":"VLOOKUP($B84,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Staff workrooms"},{"$f":"'Individual Spaces'!G83","v":"MFL"},{"$f":"'Individual Spaces'!H83","v":19},null,null,null,-19,null,null,{"$f":"'Individual Spaces'!O83","v":0},{"$f":"'Individual Spaces'!P83","v":0},{"$f":"'Individual Spaces'!Q83","v":0},{"$f":"'Individual Spaces'!R83","v":0},null,0,{"$f":"IF(AF84=\"-\",0,ROUND((J84-VLOOKUP(B84,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B84,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":7},{"$f":"IF(VLOOKUP(B84,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B84,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J84-VLOOKUP(B84,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B84,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":7},8,null,null,{"$f":"VLOOKUP($B84,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Space for staff for desk-based work and informal meetings or office/workroom, with space for repair of equipment"},{"$f":"VLOOKUP($B84,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Lesson preparation and research mainly using ICT with a hot desk arrangement. Marking and recording pupils work. Storage of some of staff's personal and teaching resources. Team meeting and discussions."},{"$f":"VLOOKUP($B84,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B84,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B84,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"D"},{"$f":"VLOOKUP($B84,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B84,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A84","v":"OFF30"},{"$f":"'Individual Spaces'!B84","v":"OFF33"},{"$f":"'Individual Spaces'!C84","v":4004},{"$f":"'Individual Spaces'!D84","v":"Staff workrooms (teaching staff) 4"},{"$f":"'Individual Spaces'!E84","v":0},null,{"$f":"VLOOKUP($B85,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_20_86"},{"$f":"VLOOKUP($B85,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Staff workrooms"},{"$f":"'Individual Spaces'!G84","v":"Science"},{"$f":"'Individual Spaces'!H84","v":19},null,null,null,-19,null,null,{"$f":"'Individual Spaces'!O84","v":0},{"$f":"'Individual Spaces'!P84","v":0},{"$f":"'Individual Spaces'!Q84","v":0},{"$f":"'Individual Spaces'!R84","v":0},null,0,{"$f":"IF(AF85=\"-\",0,ROUND((J85-VLOOKUP(B85,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B85,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":7},{"$f":"IF(VLOOKUP(B85,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B85,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J85-VLOOKUP(B85,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B85,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":7},8,null,null,{"$f":"VLOOKUP($B85,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Space for staff for desk-based work and informal meetings or office/workroom, with space for repair of equipment"},{"$f":"VLOOKUP($B85,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Lesson preparation and research mainly using ICT with a hot desk arrangement. Marking and recording pupils work. Storage of some of staff's personal and teaching resources. Team meeting and discussions."},{"$f":"VLOOKUP($B85,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B85,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B85,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"D"},{"$f":"VLOOKUP($B85,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B85,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A85","v":"OFF30"},{"$f":"'Individual Spaces'!B85","v":"OFF33"},{"$f":"'Individual Spaces'!C85","v":4005},{"$f":"'Individual Spaces'!D85","v":"Staff workrooms (teaching staff) 5"},{"$f":"'Individual Spaces'!E85","v":0},null,{"$f":"VLOOKUP($B86,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_20_86"},{"$f":"VLOOKUP($B86,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Staff workrooms"},{"$f":"'Individual Spaces'!G85","v":"DT/ Art"},{"$f":"'Individual Spaces'!H85","v":19},null,null,null,-19,null,null,{"$f":"'Individual Spaces'!O85","v":0},{"$f":"'Individual Spaces'!P85","v":0},{"$f":"'Individual Spaces'!Q85","v":0},{"$f":"'Individual Spaces'!R85","v":0},null,0,{"$f":"IF(AF86=\"-\",0,ROUND((J86-VLOOKUP(B86,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B86,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":7},{"$f":"IF(VLOOKUP(B86,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B86,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J86-VLOOKUP(B86,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B86,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":7},8,null,null,{"$f":"VLOOKUP($B86,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Space for staff for desk-based work and informal meetings or office/workroom, with space for repair of equipment"},{"$f":"VLOOKUP($B86,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Lesson preparation and research mainly using ICT with a hot desk arrangement. Marking and recording pupils work. Storage of some of staff's personal and teaching resources. Team meeting and discussions."},{"$f":"VLOOKUP($B86,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B86,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B86,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"D"},{"$f":"VLOOKUP($B86,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B86,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A86","v":"OFF30"},{"$f":"'Individual Spaces'!B86","v":"OFF32"},{"$f":"'Individual Spaces'!C86","v":4006},{"$f":"'Individual Spaces'!D86","v":"Staff workrooms (smaller teaching team) 1"},{"$f":"'Individual Spaces'!E86","v":0},null,{"$f":"VLOOKUP($B87,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_20_86"},{"$f":"VLOOKUP($B87,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Staff workrooms"},{"$f":"'Individual Spaces'!G86","v":"ICT and Business Studies"},{"$f":"'Individual Spaces'!H86","v":15},null,null,null,-15,null,null,{"$f":"'Individual Spaces'!O86","v":0},{"$f":"'Individual Spaces'!P86","v":0},{"$f":"'Individual Spaces'!Q86","v":0},{"$f":"'Individual Spaces'!R86","v":0},null,0,{"$f":"IF(AF87=\"-\",0,ROUND((J87-VLOOKUP(B87,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B87,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":5},{"$f":"IF(VLOOKUP(B87,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B87,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J87-VLOOKUP(B87,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B87,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":5},6,null,null,{"$f":"VLOOKUP($B87,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Space for staff for desk-based work and informal meetings or office/workroom, with space for repair of equipment"},{"$f":"VLOOKUP($B87,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Lesson preparation and research mainly using ICT with a hot desk arrangement. Marking and recording pupils work. Storage of some of staff's personal and teaching resources. Team meeting and discussions."},{"$f":"VLOOKUP($B87,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B87,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B87,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"D"},{"$f":"VLOOKUP($B87,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B87,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A87","v":"OFF30"},{"$f":"'Individual Spaces'!B87","v":"OFF32"},{"$f":"'Individual Spaces'!C87","v":4007},{"$f":"'Individual Spaces'!D87","v":"Staff workrooms (smaller teaching team) 2"},{"$f":"'Individual Spaces'!E87","v":0},null,{"$f":"VLOOKUP($B88,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_20_86"},{"$f":"VLOOKUP($B88,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Staff workrooms"},{"$f":"'Individual Spaces'!G87","v":"Humanities"},{"$f":"'Individual Spaces'!H87","v":15},null,null,null,-15,null,null,{"$f":"'Individual Spaces'!O87","v":0},{"$f":"'Individual Spaces'!P87","v":0},{"$f":"'Individual Spaces'!Q87","v":0},{"$f":"'Individual Spaces'!R87","v":0},null,0,{"$f":"IF(AF88=\"-\",0,ROUND((J88-VLOOKUP(B88,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B88,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":5},{"$f":"IF(VLOOKUP(B88,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B88,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J88-VLOOKUP(B88,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B88,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":5},6,null,null,{"$f":"VLOOKUP($B88,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Space for staff for desk-based work and informal meetings or office/workroom, with space for repair of equipment"},{"$f":"VLOOKUP($B88,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Lesson preparation and research mainly using ICT with a hot desk arrangement. Marking and recording pupils work. Storage of some of staff's personal and teaching resources. Team meeting and discussions."},{"$f":"VLOOKUP($B88,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B88,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B88,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"D"},{"$f":"VLOOKUP($B88,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B88,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A88","v":"OFF30"},{"$f":"'Individual Spaces'!B88","v":"OFF32"},{"$f":"'Individual Spaces'!C88","v":4008},{"$f":"'Individual Spaces'!D88","v":"Staff workrooms (smaller teaching team) 3"},{"$f":"'Individual Spaces'!E88","v":0},null,{"$f":"VLOOKUP($B89,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_20_86"},{"$f":"VLOOKUP($B89,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Staff workrooms"},{"$f":"'Individual Spaces'!G88","v":"Perf arts, hall and dining"},{"$f":"'Individual Spaces'!H88","v":15},null,null,null,-15,null,null,{"$f":"'Individual Spaces'!O88","v":0},{"$f":"'Individual Spaces'!P88","v":0},{"$f":"'Individual Spaces'!Q88","v":0},{"$f":"'Individual Spaces'!R88","v":0},null,0,{"$f":"IF(AF89=\"-\",0,ROUND((J89-VLOOKUP(B89,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B89,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":5},{"$f":"IF(VLOOKUP(B89,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B89,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J89-VLOOKUP(B89,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B89,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":5},6,null,null,{"$f":"VLOOKUP($B89,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Space for staff for desk-based work and informal meetings or office/workroom, with space for repair of equipment"},{"$f":"VLOOKUP($B89,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Lesson preparation and research mainly using ICT with a hot desk arrangement. Marking and recording pupils work. Storage of some of staff's personal and teaching resources. Team meeting and discussions."},{"$f":"VLOOKUP($B89,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B89,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B89,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"D"},{"$f":"VLOOKUP($B89,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B89,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A89","v":"OFF50"},{"$f":"'Individual Spaces'!B89","v":"OFF52"},{"$f":"'Individual Spaces'!C89","v":4009},{"$f":"'Individual Spaces'!D89","v":"Staff room (social) 1"},{"$f":"'Individual Spaces'!E89","v":0},null,{"$f":"VLOOKUP($B90,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_20_85"},{"$f":"VLOOKUP($B90,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Staff rooms"},{"$f":"'Individual Spaces'!G89","v":"Admin"},{"$f":"'Individual Spaces'!H89","v":41},null,null,null,-41,null,null,{"$f":"'Individual Spaces'!O89","v":0},{"$f":"'Individual Spaces'!P89","v":0},{"$f":"'Individual Spaces'!Q89","v":0},{"$f":"'Individual Spaces'!R89","v":0},null,0,{"$f":"IF(AF90=\"-\",0,ROUND((J90-VLOOKUP(B90,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B90,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":24},{"$f":"IF(VLOOKUP(B90,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B90,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J90-VLOOKUP(B90,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B90,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},27,null,null,{"$f":"VLOOKUP($B90,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Main space for any staff in school to meet and socialise, and to make tea and snacks"},{"$f":"VLOOKUP($B90,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Informal meeting and discussion during breaks. Limited ICT access. Receiving post/notices. Relaxing and taking refreshments."},{"$f":"VLOOKUP($B90,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B90,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B90,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"B"},{"$f":"VLOOKUP($B90,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B90,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A90","v":"OFF40"},{"$f":"'Individual Spaces'!B90","v":"OFF40"},{"$f":"'Individual Spaces'!C90","v":4010},{"$f":"'Individual Spaces'!D90","v":"Meeting room (conference) 1"},{"$f":"'Individual Spaces'!E90","v":0},null,{"$f":"VLOOKUP($B91,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_50"},{"$f":"VLOOKUP($B91,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Meeting rooms"},{"$f":"'Individual Spaces'!G90","v":"Admin"},{"$f":"'Individual Spaces'!H90","v":19},null,null,null,-19,null,null,{"$f":"'Individual Spaces'!O90","v":0},{"$f":"'Individual Spaces'!P90","v":0},{"$f":"'Individual Spaces'!Q90","v":0},{"$f":"'Individual Spaces'!R90","v":0},null,0,{"$f":"IF(AF91=\"-\",0,ROUND((J91-VLOOKUP(B91,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B91,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":9},{"$f":"IF(VLOOKUP(B91,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B91,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J91-VLOOKUP(B91,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B91,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},10,null,null,{"$f":"VLOOKUP($B91,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Conference or meeting room for meetings of staff, governors and other adults"},{"$f":"VLOOKUP($B91,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Meeting room for staff with internal and external visitors etc. Privacy important. Small scale presentations using ICT."},{"$f":"VLOOKUP($B91,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B91,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B91,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B91,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B91,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Optional "}]
[{"$f":"'Individual Spaces'!A91","v":"ADM32"},{"$f":"'Individual Spaces'!B91","v":"ADM32"},{"$f":"'Individual Spaces'!C91","v":4011},{"$f":"'Individual Spaces'!D91","v":"Reception area, community (50% circulation) 1"},{"$f":"'Individual Spaces'!E91","v":0},null,{"$f":"VLOOKUP($B92,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_71"},{"$f":"VLOOKUP($B92,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Reception areas"},{"$f":"'Individual Spaces'!G91","v":"Sports/ PE"},{"$f":"'Individual Spaces'!H91","v":8},null,null,null,-8,null,null,{"$f":"'Individual Spaces'!O91","v":0},{"$f":"'Individual Spaces'!P91","v":0},{"$f":"'Individual Spaces'!Q91","v":0},{"$f":"'Individual Spaces'!R91","v":0},null,0,{"$f":"IF(AF92=\"-\",0,ROUND((J92-VLOOKUP(B92,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B92,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":2},{"$f":"IF(VLOOKUP(B92,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B92,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J92-VLOOKUP(B92,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B92,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},3,null,null,{"$f":"VLOOKUP($B92,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Community entrance area, of which 50% is net area for vending and display, and 50% is circulation through the space"},{"$f":"VLOOKUP($B92,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Managing and controlling access to and from facilities used by the community such as sports halls."},{"$f":"VLOOKUP($B92,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B92,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B92,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":0},{"$f":"VLOOKUP($B92,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B92,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Yes "}]
[{"$f":"'Individual Spaces'!A92","v":"ADM22"},{"$f":"'Individual Spaces'!B92","v":"ADM22"},{"$f":"'Individual Spaces'!C92","v":4012},{"$f":"'Individual Spaces'!D92","v":"Kitchenette, bay 1"},{"$f":"'Individual Spaces'!E92","v":0},null,{"$f":"VLOOKUP($B93,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_60_45"},{"$f":"VLOOKUP($B93,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Kitchenettes"},{"$f":"'Individual Spaces'!G92","v":"Admin"},{"$f":"'Individual Spaces'!H92","v":3},null,null,null,-3,null,null,{"$f":"'Individual Spaces'!O92","v":0},{"$f":"'Individual Spaces'!P92","v":0},{"$f":"'Individual Spaces'!Q92","v":0},{"$f":"'Individual Spaces'!R92","v":0},null,0,{"$f":"IF(AF93=\"-\",0,ROUND((J93-VLOOKUP(B93,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B93,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(B93,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B93,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J93-VLOOKUP(B93,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B93,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},2,null,null,{"$f":"VLOOKUP($B93,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Small bay for staff to make drinks and snacks"},{"$f":"VLOOKUP($B93,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Making drinks and/or snacks for staff, pupils or visitors."},{"$f":"VLOOKUP($B93,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B93,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Light practical"},{"$f":"VLOOKUP($B93,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":0},{"$f":"VLOOKUP($B93,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B93,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A93","v":"ADM22"},{"$f":"'Individual Spaces'!B93","v":"ADM22"},{"$f":"'Individual Spaces'!C93","v":4013},{"$f":"'Individual Spaces'!D93","v":"Kitchenette, bay 2"},{"$f":"'Individual Spaces'!E93","v":0},null,{"$f":"VLOOKUP($B94,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_60_45"},{"$f":"VLOOKUP($B94,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Kitchenettes"},{"$f":"'Individual Spaces'!G93","v":"Admin"},{"$f":"'Individual Spaces'!H93","v":3},null,null,null,-3,null,null,{"$f":"'Individual Spaces'!O93","v":0},{"$f":"'Individual Spaces'!P93","v":0},{"$f":"'Individual Spaces'!Q93","v":0},{"$f":"'Individual Spaces'!R93","v":0},null,0,{"$f":"IF(AF94=\"-\",0,ROUND((J94-VLOOKUP(B94,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B94,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(B94,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B94,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J94-VLOOKUP(B94,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B94,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},2,null,null,{"$f":"VLOOKUP($B94,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Small bay for staff to make drinks and snacks"},{"$f":"VLOOKUP($B94,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Making drinks and/or snacks for staff, pupils or visitors."},{"$f":"VLOOKUP($B94,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B94,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Light practical"},{"$f":"VLOOKUP($B94,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":0},{"$f":"VLOOKUP($B94,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B94,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A94","v":"ADM22"},{"$f":"'Individual Spaces'!B94","v":"ADM22"},{"$f":"'Individual Spaces'!C94","v":4014},{"$f":"'Individual Spaces'!D94","v":"Kitchenette, bay 3"},{"$f":"'Individual Spaces'!E94","v":0},null,{"$f":"VLOOKUP($B95,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_60_45"},{"$f":"VLOOKUP($B95,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Kitchenettes"},{"$f":"'Individual Spaces'!G94","v":"Admin"},{"$f":"'Individual Spaces'!H94","v":3},null,null,null,-3,null,null,{"$f":"'Individual Spaces'!O94","v":0},{"$f":"'Individual Spaces'!P94","v":0},{"$f":"'Individual Spaces'!Q94","v":0},{"$f":"'Individual Spaces'!R94","v":0},null,0,{"$f":"IF(AF95=\"-\",0,ROUND((J95-VLOOKUP(B95,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B95,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(B95,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B95,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J95-VLOOKUP(B95,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B95,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},2,null,null,{"$f":"VLOOKUP($B95,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Small bay for staff to make drinks and snacks"},{"$f":"VLOOKUP($B95,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Making drinks and/or snacks for staff, pupils or visitors."},{"$f":"VLOOKUP($B95,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B95,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Light practical"},{"$f":"VLOOKUP($B95,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":0},{"$f":"VLOOKUP($B95,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B95,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A95","v":"ADM22"},{"$f":"'Individual Spaces'!B95","v":"ADM22"},{"$f":"'Individual Spaces'!C95","v":4015},{"$f":"'Individual Spaces'!D95","v":"Kitchenette, bay 4"},{"$f":"'Individual Spaces'!E95","v":0},null,{"$f":"VLOOKUP($B96,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_60_45"},{"$f":"VLOOKUP($B96,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Kitchenettes"},{"$f":"'Individual Spaces'!G95","v":"Admin"},{"$f":"'Individual Spaces'!H95","v":3},null,null,null,-3,null,null,{"$f":"'Individual Spaces'!O95","v":0},{"$f":"'Individual Spaces'!P95","v":0},{"$f":"'Individual Spaces'!Q95","v":0},{"$f":"'Individual Spaces'!R95","v":0},null,0,{"$f":"IF(AF96=\"-\",0,ROUND((J96-VLOOKUP(B96,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B96,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(B96,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B96,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J96-VLOOKUP(B96,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B96,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},2,null,null,{"$f":"VLOOKUP($B96,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Small bay for staff to make drinks and snacks"},{"$f":"VLOOKUP($B96,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Making drinks and/or snacks for staff, pupils or visitors."},{"$f":"VLOOKUP($B96,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B96,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Light practical"},{"$f":"VLOOKUP($B96,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":0},{"$f":"VLOOKUP($B96,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B96,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A96","v":"ADM22"},{"$f":"'Individual Spaces'!B96","v":"ADM22"},{"$f":"'Individual Spaces'!C96","v":4016},{"$f":"'Individual Spaces'!D96","v":"Kitchenette, bay 5"},{"$f":"'Individual Spaces'!E96","v":0},null,{"$f":"VLOOKUP($B97,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_60_45"},{"$f":"VLOOKUP($B97,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Kitchenettes"},{"$f":"'Individual Spaces'!G96","v":"Admin"},{"$f":"'Individual Spaces'!H96","v":3},null,null,null,-3,null,null,{"$f":"'Individual Spaces'!O96","v":0},{"$f":"'Individual Spaces'!P96","v":0},{"$f":"'Individual Spaces'!Q96","v":0},{"$f":"'Individual Spaces'!R96","v":0},null,0,{"$f":"IF(AF97=\"-\",0,ROUND((J97-VLOOKUP(B97,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B97,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(B97,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B97,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J97-VLOOKUP(B97,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B97,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},2,null,null,{"$f":"VLOOKUP($B97,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Small bay for staff to make drinks and snacks"},{"$f":"VLOOKUP($B97,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Making drinks and/or snacks for staff, pupils or visitors."},{"$f":"VLOOKUP($B97,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B97,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Light practical"},{"$f":"VLOOKUP($B97,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":0},{"$f":"VLOOKUP($B97,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B97,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A97","v":"ADM10"},{"$f":"'Individual Spaces'!B97","v":"ADM11"},{"$f":"'Individual Spaces'!C97","v":4017},{"$f":"'Individual Spaces'!D97","v":"Enclosed office, admin (head) 1"},{"$f":"'Individual Spaces'!E97","v":0},null,{"$f":"VLOOKUP($B98,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_27"},{"$f":"VLOOKUP($B98,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Enclosed offices"},{"$f":"'Individual Spaces'!G97","v":"Admin"},{"$f":"'Individual Spaces'!H97","v":16},null,null,null,-16,null,null,{"$f":"'Individual Spaces'!O97","v":0},{"$f":"'Individual Spaces'!P97","v":0},{"$f":"'Individual Spaces'!Q97","v":0},{"$f":"'Individual Spaces'!R97","v":0},null,0,{"$f":"IF(AF98=\"-\",0,ROUND((J98-VLOOKUP(B98,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B98,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":6},{"$f":"IF(VLOOKUP(B98,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B98,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J98-VLOOKUP(B98,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B98,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},7,null,null,{"$f":"VLOOKUP($B98,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Office for head or principal and meetings of staff, governors or other adults"},{"$f":"VLOOKUP($B98,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administrative tasks (including use of ICT) small group meetings and interviews. Privacy important."},{"$f":"VLOOKUP($B98,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B98,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B98,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"D"},{"$f":"VLOOKUP($B98,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B98,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A98","v":"ADM10"},{"$f":"'Individual Spaces'!B98","v":"ADM13"},{"$f":"'Individual Spaces'!C98","v":4018},{"$f":"'Individual Spaces'!D98","v":"Enclosed office, admin (PA) 1"},{"$f":"'Individual Spaces'!E98","v":0},null,{"$f":"VLOOKUP($B99,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_27"},{"$f":"VLOOKUP($B99,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Enclosed offices"},{"$f":"'Individual Spaces'!G98","v":"Admin"},{"$f":"'Individual Spaces'!H98","v":8},null,null,null,-8,null,null,{"$f":"'Individual Spaces'!O98","v":0},{"$f":"'Individual Spaces'!P98","v":0},{"$f":"'Individual Spaces'!Q98","v":0},{"$f":"'Individual Spaces'!R98","v":0},null,0,{"$f":"IF(AF99=\"-\",0,ROUND((J99-VLOOKUP(B99,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B99,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(B99,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B99,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J99-VLOOKUP(B99,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B99,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},2,null,null,{"$f":"VLOOKUP($B99,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Office for personal assistant to head or principal"},{"$f":"VLOOKUP($B99,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administrative tasks (including use of ICT) and filing."},{"$f":"VLOOKUP($B99,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B99,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B99,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"K"},{"$f":"VLOOKUP($B99,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B99,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A99","v":"ADM08"},{"$f":"'Individual Spaces'!B99","v":"ADM08"},{"$f":"'Individual Spaces'!C99","v":4019},{"$f":"'Individual Spaces'!D99","v":"Reprographics room 1"},{"$f":"'Individual Spaces'!E99","v":0},null,{"$f":"VLOOKUP($B100,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_73"},{"$f":"VLOOKUP($B100,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Reprographics rooms"},{"$f":"'Individual Spaces'!G99","v":"Admin"},{"$f":"'Individual Spaces'!H99","v":20},null,null,null,-20,null,null,{"$f":"'Individual Spaces'!O99","v":0},{"$f":"'Individual Spaces'!P99","v":0},{"$f":"'Individual Spaces'!Q99","v":0},{"$f":"'Individual Spaces'!R99","v":0},null,0,{"$f":"IF(AF100=\"-\",0,ROUND((J100-VLOOKUP(B100,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B100,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(B100,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B100,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J100-VLOOKUP(B100,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B100,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":2},5,null,null,{"$f":"VLOOKUP($B100,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Room for reprographics and photocopying machines"},{"$f":"VLOOKUP($B100,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administrative work. Collating, finishing, photocopying, printing, scanning. Storage of paper and printing resources."},{"$f":"VLOOKUP($B100,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B100,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B100,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"K"},{"$f":"VLOOKUP($B100,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B100,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A100","v":"ADM05"},{"$f":"'Individual Spaces'!B100","v":"ADM07"},{"$f":"'Individual Spaces'!C100","v":4020},{"$f":"'Individual Spaces'!D100","v":"Enclosed office, with recep desk (and window) 1"},{"$f":"'Individual Spaces'!E100","v":0},null,{"$f":"VLOOKUP($B101,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_27"},{"$f":"VLOOKUP($B101,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Enclosed offices"},{"$f":"'Individual Spaces'!G100","v":"Admin"},{"$f":"'Individual Spaces'!H100","v":41},null,null,null,-41,null,null,{"$f":"'Individual Spaces'!O100","v":0},{"$f":"'Individual Spaces'!P100","v":0},{"$f":"'Individual Spaces'!Q100","v":0},{"$f":"'Individual Spaces'!R100","v":0},null,0,{"$f":"IF(AF101=\"-\",0,ROUND((J101-VLOOKUP(B101,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B101,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":10},{"$f":"IF(VLOOKUP(B101,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B101,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J101-VLOOKUP(B101,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B101,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":10},11,null,null,{"$f":"VLOOKUP($B101,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Main office for administrative staff, with reception desk for visitors opening onto entrance/ reception area and reception window for pupils or students opening onto secure area"},{"$f":"VLOOKUP($B101,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Managing and controlling access to and from the school. Welcoming visitors and pupils at reception desk."},{"$f":"VLOOKUP($B101,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B101,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B101,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"K"},{"$f":"VLOOKUP($B101,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B101,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A101","v":"ADM31"},{"$f":"'Individual Spaces'!B101","v":"ADM31"},{"$f":"'Individual Spaces'!C101","v":4021},{"$f":"'Individual Spaces'!D101","v":"Reception area, entrance (50% circulation) 1"},{"$f":"'Individual Spaces'!E101","v":0},null,{"$f":"VLOOKUP($B102,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_71"},{"$f":"VLOOKUP($B102,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Reception areas"},{"$f":"'Individual Spaces'!G101","v":"Admin"},{"$f":"'Individual Spaces'!H101","v":24},null,null,null,-24,null,null,{"$f":"'Individual Spaces'!O101","v":0},{"$f":"'Individual Spaces'!P101","v":0},{"$f":"'Individual Spaces'!Q101","v":0},{"$f":"'Individual Spaces'!R101","v":0},null,0,{"$f":"IF(AF102=\"-\",0,ROUND((J102-VLOOKUP(B102,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B102,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":8},{"$f":"IF(VLOOKUP(B102,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B102,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J102-VLOOKUP(B102,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B102,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},9,null,null,{"$f":"VLOOKUP($B102,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Public side' of reception area, of which 50% is net area for waiting, seating and display, and 50% is circulation through the space"},{"$f":"VLOOKUP($B102,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"First point of contact for visitors to the school. Welcoming visitors."},{"$f":"VLOOKUP($B102,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B102,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B102,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":0},{"$f":"VLOOKUP($B102,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B102,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Yes "}]
[{"$f":"'Individual Spaces'!A102","v":"ADM02"},{"$f":"'Individual Spaces'!B102","v":"ADM02"},{"$f":"'Individual Spaces'!C102","v":4022},{"$f":"'Individual Spaces'!D102","v":"Confidential meeting room (interview) 1"},{"$f":"'Individual Spaces'!E102","v":0},null,{"$f":"VLOOKUP($B103,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_15"},{"$f":"VLOOKUP($B103,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Confidential meetings rooms"},{"$f":"'Individual Spaces'!G102","v":"Admin"},{"$f":"'Individual Spaces'!H102","v":6},null,null,null,-6,null,null,{"$f":"'Individual Spaces'!O102","v":0},{"$f":"'Individual Spaces'!P102","v":0},{"$f":"'Individual Spaces'!Q102","v":0},{"$f":"'Individual Spaces'!R102","v":0},null,0,{"$f":"IF(AF103=\"-\",0,ROUND((J103-VLOOKUP(B103,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B103,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(B103,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B103,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J103-VLOOKUP(B103,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B103,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},5,null,null,{"$f":"VLOOKUP($B103,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Room off reception area for meetings with visitors without the need to access the main school"},{"$f":"VLOOKUP($B103,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Interviews, some of which will be in private, with parents and visitors. Small group meetings for both staff and parents."},{"$f":"VLOOKUP($B103,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B103,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B103,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"A"},{"$f":"VLOOKUP($B103,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B103,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Optional "}]
[{"$f":"'Individual Spaces'!A103","v":"ADM03"},{"$f":"'Individual Spaces'!B103","v":"ADM03"},{"$f":"'Individual Spaces'!C103","v":4023},{"$f":"'Individual Spaces'!D103","v":"First aid post (sick bay) 1"},{"$f":"'Individual Spaces'!E103","v":0},null,{"$f":"VLOOKUP($B104,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_10_30"},{"$f":"VLOOKUP($B104,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"First aid posts"},{"$f":"'Individual Spaces'!G103","v":"Admin"},{"$f":"'Individual Spaces'!H103","v":6},null,null,null,-6,null,null,{"$f":"'Individual Spaces'!O103","v":0},{"$f":"'Individual Spaces'!P103","v":0},{"$f":"'Individual Spaces'!Q103","v":0},{"$f":"'Individual Spaces'!R103","v":0},null,0,{"$f":"IF(AF104=\"-\",0,ROUND((J104-VLOOKUP(B104,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B104,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":3},{"$f":"IF(VLOOKUP(B104,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B104,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J104-VLOOKUP(B104,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B104,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},4,null,null,{"$f":"VLOOKUP($B104,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Semi-open bay for pupils who are feeling unwell"},{"$f":"VLOOKUP($B104,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Passively supervised area for pupils who are ill, may need initial treatment and/or are waiting for parents/carers to pick them up."},{"$f":"VLOOKUP($B104,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B104,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B104,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"B"},{"$f":"VLOOKUP($B104,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B104,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A104","v":"OFF00"},{"$f":"'Individual Spaces'!B104","v":"OFF01"},{"$f":"'Individual Spaces'!C104","v":4024},{"$f":"'Individual Spaces'!D104","v":"Office (1-person) 1"},{"$f":"'Individual Spaces'!E104","v":0},null,{"$f":"VLOOKUP($B105,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_59"},{"$f":"VLOOKUP($B105,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Offices"},{"$f":"'Individual Spaces'!G104","v":"Balance"},{"$f":"'Individual Spaces'!H104","v":7},null,null,null,-7,null,null,{"$f":"'Individual Spaces'!O104","v":0},{"$f":"'Individual Spaces'!P104","v":0},{"$f":"'Individual Spaces'!Q104","v":0},{"$f":"'Individual Spaces'!R104","v":0},null,0,{"$f":"IF(AF105=\"-\",0,ROUND((J105-VLOOKUP(B105,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B105,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(B105,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B105,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J105-VLOOKUP(B105,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B105,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},2,null,null,{"$f":"VLOOKUP($B105,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Office for one member of staff with admin storage "},{"$f":"VLOOKUP($B105,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administrative tasks (including use of ICT) and filing."},{"$f":"VLOOKUP($B105,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B105,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B105,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"D"},{"$f":"VLOOKUP($B105,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B105,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A105","v":"OFF00"},{"$f":"'Individual Spaces'!B105","v":"OFF01"},{"$f":"'Individual Spaces'!C105","v":4025},{"$f":"'Individual Spaces'!D105","v":"Office (1-person) 2"},{"$f":"'Individual Spaces'!E105","v":0},null,{"$f":"VLOOKUP($B106,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_59"},{"$f":"VLOOKUP($B106,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Offices"},{"$f":"'Individual Spaces'!G105","v":"Balance"},{"$f":"'Individual Spaces'!H105","v":7},null,null,null,-7,null,null,{"$f":"'Individual Spaces'!O105","v":0},{"$f":"'Individual Spaces'!P105","v":0},{"$f":"'Individual Spaces'!Q105","v":0},{"$f":"'Individual Spaces'!R105","v":0},null,0,{"$f":"IF(AF106=\"-\",0,ROUND((J106-VLOOKUP(B106,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B106,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(B106,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B106,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J106-VLOOKUP(B106,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B106,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},2,null,null,{"$f":"VLOOKUP($B106,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Office for one member of staff with admin storage "},{"$f":"VLOOKUP($B106,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administrative tasks (including use of ICT) and filing."},{"$f":"VLOOKUP($B106,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B106,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B106,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"D"},{"$f":"VLOOKUP($B106,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B106,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A106","v":"OFF00"},{"$f":"'Individual Spaces'!B106","v":"OFF01"},{"$f":"'Individual Spaces'!C106","v":4026},{"$f":"'Individual Spaces'!D106","v":"Office (1-person) 3"},{"$f":"'Individual Spaces'!E106","v":0},null,{"$f":"VLOOKUP($B107,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_59"},{"$f":"VLOOKUP($B107,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Offices"},{"$f":"'Individual Spaces'!G106","v":"Balance"},{"$f":"'Individual Spaces'!H106","v":7},null,null,null,-7,null,null,{"$f":"'Individual Spaces'!O106","v":0},{"$f":"'Individual Spaces'!P106","v":0},{"$f":"'Individual Spaces'!Q106","v":0},{"$f":"'Individual Spaces'!R106","v":0},null,0,{"$f":"IF(AF107=\"-\",0,ROUND((J107-VLOOKUP(B107,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B107,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(B107,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B107,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J107-VLOOKUP(B107,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B107,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},2,null,null,{"$f":"VLOOKUP($B107,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Office for one member of staff with admin storage "},{"$f":"VLOOKUP($B107,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administrative tasks (including use of ICT) and filing."},{"$f":"VLOOKUP($B107,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B107,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B107,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"D"},{"$f":"VLOOKUP($B107,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B107,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A107","v":"OFF00"},{"$f":"'Individual Spaces'!B107","v":"OFF01"},{"$f":"'Individual Spaces'!C107","v":4027},{"$f":"'Individual Spaces'!D107","v":"Office (1-person) 4"},{"$f":"'Individual Spaces'!E107","v":0},null,{"$f":"VLOOKUP($B108,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_59"},{"$f":"VLOOKUP($B108,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Offices"},{"$f":"'Individual Spaces'!G107","v":"Balance"},{"$f":"'Individual Spaces'!H107","v":7},null,null,null,-7,null,null,{"$f":"'Individual Spaces'!O107","v":0},{"$f":"'Individual Spaces'!P107","v":0},{"$f":"'Individual Spaces'!Q107","v":0},{"$f":"'Individual Spaces'!R107","v":0},null,0,{"$f":"IF(AF108=\"-\",0,ROUND((J108-VLOOKUP(B108,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B108,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(B108,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B108,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J108-VLOOKUP(B108,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B108,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},2,null,null,{"$f":"VLOOKUP($B108,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Office for one member of staff with admin storage "},{"$f":"VLOOKUP($B108,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administrative tasks (including use of ICT) and filing."},{"$f":"VLOOKUP($B108,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B108,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B108,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"D"},{"$f":"VLOOKUP($B108,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B108,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A108","v":"OFF00"},{"$f":"'Individual Spaces'!B108","v":"OFF01"},{"$f":"'Individual Spaces'!C108","v":4028},{"$f":"'Individual Spaces'!D108","v":"Office (1-person) 5"},{"$f":"'Individual Spaces'!E108","v":0},null,{"$f":"VLOOKUP($B109,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_59"},{"$f":"VLOOKUP($B109,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Offices"},{"$f":"'Individual Spaces'!G108","v":"Balance"},{"$f":"'Individual Spaces'!H108","v":7},null,null,null,-7,null,null,{"$f":"'Individual Spaces'!O108","v":0},{"$f":"'Individual Spaces'!P108","v":0},{"$f":"'Individual Spaces'!Q108","v":0},{"$f":"'Individual Spaces'!R108","v":0},null,0,{"$f":"IF(AF109=\"-\",0,ROUND((J109-VLOOKUP(B109,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B109,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(B109,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B109,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J109-VLOOKUP(B109,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B109,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},2,null,null,{"$f":"VLOOKUP($B109,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Office for one member of staff with admin storage "},{"$f":"VLOOKUP($B109,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administrative tasks (including use of ICT) and filing."},{"$f":"VLOOKUP($B109,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B109,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B109,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"D"},{"$f":"VLOOKUP($B109,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B109,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A109","v":"OFF00"},{"$f":"'Individual Spaces'!B109","v":"OFF11"},{"$f":"'Individual Spaces'!C109","v":4029},{"$f":"'Individual Spaces'!D109","v":"Office (with meeting area, 1-person) 1"},{"$f":"'Individual Spaces'!E109","v":0},null,{"$f":"VLOOKUP($B110,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_59"},{"$f":"VLOOKUP($B110,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Offices"},{"$f":"'Individual Spaces'!G109","v":"Balance"},{"$f":"'Individual Spaces'!H109","v":9},null,null,null,-9,null,null,{"$f":"'Individual Spaces'!O109","v":0},{"$f":"'Individual Spaces'!P109","v":0},{"$f":"'Individual Spaces'!Q109","v":0},{"$f":"'Individual Spaces'!R109","v":0},null,0,{"$f":"IF(AF110=\"-\",0,ROUND((J110-VLOOKUP(B110,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B110,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":3},{"$f":"IF(VLOOKUP(B110,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B110,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J110-VLOOKUP(B110,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B110,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},4,null,null,{"$f":"VLOOKUP($B110,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Office for one member of staff, with space for meetings"},{"$f":"VLOOKUP($B110,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administrative tasks (including use of ICT). Small group meetings and interviews. "},{"$f":"VLOOKUP($B110,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B110,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B110,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B110,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B110,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A110","v":"OFF00"},{"$f":"'Individual Spaces'!B110","v":"OFF11"},{"$f":"'Individual Spaces'!C110","v":4030},{"$f":"'Individual Spaces'!D110","v":"Office (with meeting area, 1-person) 2"},{"$f":"'Individual Spaces'!E110","v":0},null,{"$f":"VLOOKUP($B111,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_59"},{"$f":"VLOOKUP($B111,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Offices"},{"$f":"'Individual Spaces'!G110","v":"Balance"},{"$f":"'Individual Spaces'!H110","v":9},null,null,null,-9,null,null,{"$f":"'Individual Spaces'!O110","v":0},{"$f":"'Individual Spaces'!P110","v":0},{"$f":"'Individual Spaces'!Q110","v":0},{"$f":"'Individual Spaces'!R110","v":0},null,0,{"$f":"IF(AF111=\"-\",0,ROUND((J111-VLOOKUP(B111,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B111,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":3},{"$f":"IF(VLOOKUP(B111,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B111,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J111-VLOOKUP(B111,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B111,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},4,null,null,{"$f":"VLOOKUP($B111,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Office for one member of staff, with space for meetings"},{"$f":"VLOOKUP($B111,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administrative tasks (including use of ICT). Small group meetings and interviews. "},{"$f":"VLOOKUP($B111,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B111,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B111,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B111,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B111,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A111","v":"OFF00"},{"$f":"'Individual Spaces'!B111","v":"OFF11"},{"$f":"'Individual Spaces'!C111","v":4031},{"$f":"'Individual Spaces'!D111","v":"Office (with meeting area, 1-person) 3"},{"$f":"'Individual Spaces'!E111","v":0},null,{"$f":"VLOOKUP($B112,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_59"},{"$f":"VLOOKUP($B112,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Offices"},{"$f":"'Individual Spaces'!G111","v":"Balance"},{"$f":"'Individual Spaces'!H111","v":9},null,null,null,-9,null,null,{"$f":"'Individual Spaces'!O111","v":0},{"$f":"'Individual Spaces'!P111","v":0},{"$f":"'Individual Spaces'!Q111","v":0},{"$f":"'Individual Spaces'!R111","v":0},null,0,{"$f":"IF(AF112=\"-\",0,ROUND((J112-VLOOKUP(B112,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B112,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":3},{"$f":"IF(VLOOKUP(B112,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B112,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J112-VLOOKUP(B112,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B112,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},4,null,null,{"$f":"VLOOKUP($B112,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Office for one member of staff, with space for meetings"},{"$f":"VLOOKUP($B112,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administrative tasks (including use of ICT). Small group meetings and interviews. "},{"$f":"VLOOKUP($B112,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B112,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B112,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B112,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B112,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A112","v":"OFF00"},{"$f":"'Individual Spaces'!B112","v":"OFF11"},{"$f":"'Individual Spaces'!C112","v":4032},{"$f":"'Individual Spaces'!D112","v":"Office (with meeting area, 1-person) 4"},{"$f":"'Individual Spaces'!E112","v":0},null,{"$f":"VLOOKUP($B113,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_59"},{"$f":"VLOOKUP($B113,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Offices"},{"$f":"'Individual Spaces'!G112","v":"Balance"},{"$f":"'Individual Spaces'!H112","v":9},null,null,null,-9,null,null,{"$f":"'Individual Spaces'!O112","v":0},{"$f":"'Individual Spaces'!P112","v":0},{"$f":"'Individual Spaces'!Q112","v":0},{"$f":"'Individual Spaces'!R112","v":0},null,0,{"$f":"IF(AF113=\"-\",0,ROUND((J113-VLOOKUP(B113,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B113,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":3},{"$f":"IF(VLOOKUP(B113,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B113,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J113-VLOOKUP(B113,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B113,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},4,null,null,{"$f":"VLOOKUP($B113,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Office for one member of staff, with space for meetings"},{"$f":"VLOOKUP($B113,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administrative tasks (including use of ICT). Small group meetings and interviews. "},{"$f":"VLOOKUP($B113,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B113,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B113,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B113,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B113,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A113","v":"OFF00"},{"$f":"'Individual Spaces'!B113","v":"OFF11"},{"$f":"'Individual Spaces'!C113","v":4033},{"$f":"'Individual Spaces'!D113","v":"Office (with meeting area, 1-person) 5"},{"$f":"'Individual Spaces'!E113","v":0},null,{"$f":"VLOOKUP($B114,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_59"},{"$f":"VLOOKUP($B114,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Offices"},{"$f":"'Individual Spaces'!G113","v":"Balance"},{"$f":"'Individual Spaces'!H113","v":9},null,null,null,-9,null,null,{"$f":"'Individual Spaces'!O113","v":0},{"$f":"'Individual Spaces'!P113","v":0},{"$f":"'Individual Spaces'!Q113","v":0},{"$f":"'Individual Spaces'!R113","v":0},null,0,{"$f":"IF(AF114=\"-\",0,ROUND((J114-VLOOKUP(B114,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B114,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":3},{"$f":"IF(VLOOKUP(B114,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B114,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J114-VLOOKUP(B114,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B114,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},4,null,null,{"$f":"VLOOKUP($B114,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Office for one member of staff, with space for meetings"},{"$f":"VLOOKUP($B114,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administrative tasks (including use of ICT). Small group meetings and interviews. "},{"$f":"VLOOKUP($B114,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B114,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B114,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B114,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B114,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A114","v":"OFF00"},{"$f":"'Individual Spaces'!B114","v":"OFF11"},{"$f":"'Individual Spaces'!C114","v":4034},{"$f":"'Individual Spaces'!D114","v":"Office (with meeting area, 1-person) 6"},{"$f":"'Individual Spaces'!E114","v":0},null,{"$f":"VLOOKUP($B115,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_59"},{"$f":"VLOOKUP($B115,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Offices"},{"$f":"'Individual Spaces'!G114","v":"Balance"},{"$f":"'Individual Spaces'!H114","v":9},null,null,null,-9,null,null,{"$f":"'Individual Spaces'!O114","v":0},{"$f":"'Individual Spaces'!P114","v":0},{"$f":"'Individual Spaces'!Q114","v":0},{"$f":"'Individual Spaces'!R114","v":0},null,0,{"$f":"IF(AF115=\"-\",0,ROUND((J115-VLOOKUP(B115,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B115,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":3},{"$f":"IF(VLOOKUP(B115,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B115,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J115-VLOOKUP(B115,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B115,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},4,null,null,{"$f":"VLOOKUP($B115,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Office for one member of staff, with space for meetings"},{"$f":"VLOOKUP($B115,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administrative tasks (including use of ICT). Small group meetings and interviews. "},{"$f":"VLOOKUP($B115,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B115,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B115,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B115,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B115,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A115","v":"OFF00"},{"$f":"'Individual Spaces'!B115","v":"OFF11"},{"$f":"'Individual Spaces'!C115","v":4035},{"$f":"'Individual Spaces'!D115","v":"Office (with meeting area, 1-person) 7"},{"$f":"'Individual Spaces'!E115","v":0},null,{"$f":"VLOOKUP($B116,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_59"},{"$f":"VLOOKUP($B116,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Offices"},{"$f":"'Individual Spaces'!G115","v":"Balance"},{"$f":"'Individual Spaces'!H115","v":9},null,null,null,-9,null,null,{"$f":"'Individual Spaces'!O115","v":0},{"$f":"'Individual Spaces'!P115","v":0},{"$f":"'Individual Spaces'!Q115","v":0},{"$f":"'Individual Spaces'!R115","v":0},null,0,{"$f":"IF(AF116=\"-\",0,ROUND((J116-VLOOKUP(B116,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B116,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":3},{"$f":"IF(VLOOKUP(B116,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B116,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J116-VLOOKUP(B116,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B116,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},4,null,null,{"$f":"VLOOKUP($B116,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Office for one member of staff, with space for meetings"},{"$f":"VLOOKUP($B116,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administrative tasks (including use of ICT). Small group meetings and interviews. "},{"$f":"VLOOKUP($B116,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B116,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B116,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B116,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B116,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A116","v":"OFF00"},{"$f":"'Individual Spaces'!B116","v":"OFF11"},{"$f":"'Individual Spaces'!C116","v":4036},{"$f":"'Individual Spaces'!D116","v":"Office (with meeting area, 1-person) 8"},{"$f":"'Individual Spaces'!E116","v":0},null,{"$f":"VLOOKUP($B117,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_59"},{"$f":"VLOOKUP($B117,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Offices"},{"$f":"'Individual Spaces'!G116","v":"Balance"},{"$f":"'Individual Spaces'!H116","v":9},null,null,null,-9,null,null,{"$f":"'Individual Spaces'!O116","v":0},{"$f":"'Individual Spaces'!P116","v":0},{"$f":"'Individual Spaces'!Q116","v":0},{"$f":"'Individual Spaces'!R116","v":0},null,0,{"$f":"IF(AF117=\"-\",0,ROUND((J117-VLOOKUP(B117,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B117,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":3},{"$f":"IF(VLOOKUP(B117,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B117,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J117-VLOOKUP(B117,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B117,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},4,null,null,{"$f":"VLOOKUP($B117,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Office for one member of staff, with space for meetings"},{"$f":"VLOOKUP($B117,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administrative tasks (including use of ICT). Small group meetings and interviews. "},{"$f":"VLOOKUP($B117,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B117,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B117,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B117,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B117,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A117","v":"OFF00"},{"$f":"'Individual Spaces'!B117","v":"OFF06"},{"$f":"'Individual Spaces'!C117","v":4037},{"$f":"'Individual Spaces'!D117","v":"Office (exams) 1"},{"$f":"'Individual Spaces'!E117","v":0},null,{"$f":"VLOOKUP($B118,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_59"},{"$f":"VLOOKUP($B118,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Offices"},{"$f":"'Individual Spaces'!G117","v":"-"},{"$f":"'Individual Spaces'!H117","v":9},null,null,null,-9,null,null,{"$f":"'Individual Spaces'!O117","v":0},{"$f":"'Individual Spaces'!P117","v":0},{"$f":"'Individual Spaces'!Q117","v":0},{"$f":"'Individual Spaces'!R117","v":0},null,0,{"$f":"IF(AF118=\"-\",0,ROUND((J118-VLOOKUP(B118,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B118,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":2},{"$f":"IF(VLOOKUP(B118,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B118,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J118-VLOOKUP(B118,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B118,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":2},3,null,null,{"$f":"VLOOKUP($B118,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"office for exams officer, with space for secure storage"},{"$f":"VLOOKUP($B118,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administrative tasks (including use of ICT) and confidential filing of secure documents."},{"$f":"VLOOKUP($B118,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B118,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B118,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"D"},{"$f":"VLOOKUP($B118,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B118,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A118","v":"OFF00"},{"$f":"'Individual Spaces'!B118","v":"OFF23"},{"$f":"'Individual Spaces'!C118","v":4038},{"$f":"'Individual Spaces'!D118","v":"Office (SENco, learning support) 1"},{"$f":"'Individual Spaces'!E118","v":0},null,{"$f":"VLOOKUP($B119,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_59"},{"$f":"VLOOKUP($B119,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Offices"},{"$f":"'Individual Spaces'!G118","v":"-"},{"$f":"'Individual Spaces'!H118","v":11},null,null,null,-11,null,null,{"$f":"'Individual Spaces'!O118","v":0},{"$f":"'Individual Spaces'!P118","v":0},{"$f":"'Individual Spaces'!Q118","v":0},{"$f":"'Individual Spaces'!R118","v":0},null,0,{"$f":"IF(AF119=\"-\",0,ROUND((J119-VLOOKUP(B119,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B119,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(B119,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B119,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J119-VLOOKUP(B119,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B119,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":2},5,null,null,{"$f":"VLOOKUP($B119,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Office for SENco and team, with space for informal meetings"},{"$f":"VLOOKUP($B119,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administrative tasks (including use of ICT) small informal meetings and interviews. Counselling."},{"$f":"VLOOKUP($B119,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B119,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B119,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"C"},{"$f":"VLOOKUP($B119,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B119,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A119","v":"OFF30"},{"$f":"'Individual Spaces'!B119","v":"OFF37"},{"$f":"'Individual Spaces'!C119","v":4039},{"$f":"'Individual Spaces'!D119","v":"Staff workroom (ICT technicians) 1"},{"$f":"'Individual Spaces'!E119","v":0},null,{"$f":"VLOOKUP($B120,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_20_86"},{"$f":"VLOOKUP($B120,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Staff workrooms"},{"$f":"'Individual Spaces'!G119","v":"Balance"},{"$f":"'Individual Spaces'!H119","v":11},null,null,null,-11,null,null,{"$f":"'Individual Spaces'!O119","v":0},{"$f":"'Individual Spaces'!P119","v":0},{"$f":"'Individual Spaces'!Q119","v":0},{"$f":"'Individual Spaces'!R119","v":0},null,0,{"$f":"IF(AF120=\"-\",0,ROUND((J120-VLOOKUP(B120,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B120,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":2},{"$f":"IF(VLOOKUP(B120,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B120,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J120-VLOOKUP(B120,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B120,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":2},3,null,null,{"$f":"VLOOKUP($B120,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Office/workroom for one or more ICT technicians, with space for repair of equipment"},{"$f":"VLOOKUP($B120,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administrative tasks (including use of ICT). Basic maintenance and repair of equipment. Storing small tools and items of equipment. Storing manuals and small maintenance equipment."},{"$f":"VLOOKUP($B120,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B120,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B120,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"E"},{"$f":"VLOOKUP($B120,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B120,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A120","v":"OFF30"},{"$f":"'Individual Spaces'!B120","v":"OFF38"},{"$f":"'Individual Spaces'!C120","v":4040},{"$f":"'Individual Spaces'!D120","v":"Staff workroom (premises) 1"},{"$f":"'Individual Spaces'!E120","v":0},null,{"$f":"VLOOKUP($B121,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_20_86"},{"$f":"VLOOKUP($B121,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Staff workrooms"},{"$f":"'Individual Spaces'!G120","v":"Balance"},{"$f":"'Individual Spaces'!H120","v":11},null,null,null,-11,null,null,{"$f":"'Individual Spaces'!O120","v":0},{"$f":"'Individual Spaces'!P120","v":0},{"$f":"'Individual Spaces'!Q120","v":0},{"$f":"'Individual Spaces'!R120","v":0},null,0,{"$f":"IF(AF121=\"-\",0,ROUND((J121-VLOOKUP(B121,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B121,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":2},{"$f":"IF(VLOOKUP(B121,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B121,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J121-VLOOKUP(B121,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B121,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":2},3,null,null,{"$f":"VLOOKUP($B121,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Office/workroom for one or more premises managers, caretakers, with space for repair of equipment"},{"$f":"VLOOKUP($B121,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administrative tasks (including use of ICT). Basic maintenance and repair of equipment. Storing small tools and items of equipment. Storing manuals and small maintenance equipment."},{"$f":"VLOOKUP($B121,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Staff and admin"},{"$f":"VLOOKUP($B121,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B121,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"E"},{"$f":"VLOOKUP($B121,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B121,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A121","v":0},{"$f":"'Individual Spaces'!B121","v":0},{"$f":"'Individual Spaces'!C121","v":0},{"$f":"'Individual Spaces'!D121","v":0},{"$f":"'Individual Spaces'!E121","v":"Staff Spaces Total : "},null,{"$f":"VLOOKUP($B122,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B122,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G121","v":0},{"$f":"'Individual Spaces'!H121","v":493},null,null,null,-493,null,null,{"$f":"'Individual Spaces'!O121","v":0},{"$f":"'Individual Spaces'!P121","v":0},{"$f":"'Individual Spaces'!Q121","v":0},{"$f":"'Individual Spaces'!R121","v":0},null,0,{"$f":"IF(AF122=\"-\",0,ROUND((J122-VLOOKUP(B122,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B122,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B122,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B122,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J122-VLOOKUP(B122,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B122,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B122,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B122,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B122,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B122,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B122,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B122,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B122,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A122","v":"STT10"},{"$f":"'Individual Spaces'!B122","v":"STT13"},{"$f":"'Individual Spaces'!C122","v":5001},{"$f":"'Individual Spaces'!D122","v":"Teaching resources store (IT/ GT off corridor) 1"},{"$f":"'Individual Spaces'!E122","v":0},null,{"$f":"VLOOKUP($B123,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_87"},{"$f":"VLOOKUP($B123,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Teaching resources stores"},{"$f":"'Individual Spaces'!G122","v":"Mathematics"},{"$f":"'Individual Spaces'!H122","v":5},null,null,null,-5,null,null,{"$f":"'Individual Spaces'!O122","v":0},{"$f":"'Individual Spaces'!P122","v":0},{"$f":"'Individual Spaces'!Q122","v":0},{"$f":"'Individual Spaces'!R122","v":0},null,0,{"$f":"IF(AF123=\"-\",0,ROUND((J123-VLOOKUP(B123,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B123,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B123,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B123,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J123-VLOOKUP(B123,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B123,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B123,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Store room for general teaching or ICT resources"},{"$f":"VLOOKUP($B123,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing teaching resources including books, files and digital equipment."},{"$f":"VLOOKUP($B123,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B123,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B123,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B123,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B123,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A123","v":"STT10"},{"$f":"'Individual Spaces'!B123","v":"STT13"},{"$f":"'Individual Spaces'!C123","v":5002},{"$f":"'Individual Spaces'!D123","v":"Teaching resources store (IT/ GT off corridor) 2"},{"$f":"'Individual Spaces'!E123","v":0},null,{"$f":"VLOOKUP($B124,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_87"},{"$f":"VLOOKUP($B124,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Teaching resources stores"},{"$f":"'Individual Spaces'!G123","v":"English"},{"$f":"'Individual Spaces'!H123","v":5},null,null,null,-5,null,null,{"$f":"'Individual Spaces'!O123","v":0},{"$f":"'Individual Spaces'!P123","v":0},{"$f":"'Individual Spaces'!Q123","v":0},{"$f":"'Individual Spaces'!R123","v":0},null,0,{"$f":"IF(AF124=\"-\",0,ROUND((J124-VLOOKUP(B124,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B124,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B124,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B124,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J124-VLOOKUP(B124,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B124,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B124,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Store room for general teaching or ICT resources"},{"$f":"VLOOKUP($B124,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing teaching resources including books, files and digital equipment."},{"$f":"VLOOKUP($B124,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B124,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B124,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B124,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B124,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A124","v":"STT10"},{"$f":"'Individual Spaces'!B124","v":"STT13"},{"$f":"'Individual Spaces'!C124","v":5003},{"$f":"'Individual Spaces'!D124","v":"Teaching resources store (IT/ GT off corridor) 3"},{"$f":"'Individual Spaces'!E124","v":0},null,{"$f":"VLOOKUP($B125,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_87"},{"$f":"VLOOKUP($B125,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Teaching resources stores"},{"$f":"'Individual Spaces'!G124","v":"MFL"},{"$f":"'Individual Spaces'!H124","v":5},null,null,null,-5,null,null,{"$f":"'Individual Spaces'!O124","v":0},{"$f":"'Individual Spaces'!P124","v":0},{"$f":"'Individual Spaces'!Q124","v":0},{"$f":"'Individual Spaces'!R124","v":0},null,0,{"$f":"IF(AF125=\"-\",0,ROUND((J125-VLOOKUP(B125,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B125,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B125,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B125,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J125-VLOOKUP(B125,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B125,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B125,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Store room for general teaching or ICT resources"},{"$f":"VLOOKUP($B125,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing teaching resources including books, files and digital equipment."},{"$f":"VLOOKUP($B125,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B125,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B125,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B125,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B125,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A125","v":"STT10"},{"$f":"'Individual Spaces'!B125","v":"STT13"},{"$f":"'Individual Spaces'!C125","v":5004},{"$f":"'Individual Spaces'!D125","v":"Teaching resources store (IT/ GT off corridor) 4"},{"$f":"'Individual Spaces'!E125","v":0},null,{"$f":"VLOOKUP($B126,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_87"},{"$f":"VLOOKUP($B126,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Teaching resources stores"},{"$f":"'Individual Spaces'!G125","v":"ICT and Business Studies"},{"$f":"'Individual Spaces'!H125","v":5},null,null,null,-5,null,null,{"$f":"'Individual Spaces'!O125","v":0},{"$f":"'Individual Spaces'!P125","v":0},{"$f":"'Individual Spaces'!Q125","v":0},{"$f":"'Individual Spaces'!R125","v":0},null,0,{"$f":"IF(AF126=\"-\",0,ROUND((J126-VLOOKUP(B126,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B126,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B126,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B126,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J126-VLOOKUP(B126,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B126,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B126,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Store room for general teaching or ICT resources"},{"$f":"VLOOKUP($B126,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing teaching resources including books, files and digital equipment."},{"$f":"VLOOKUP($B126,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B126,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B126,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B126,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B126,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A126","v":"STT10"},{"$f":"'Individual Spaces'!B126","v":"STT13"},{"$f":"'Individual Spaces'!C126","v":5005},{"$f":"'Individual Spaces'!D126","v":"Teaching resources store (IT/ GT off corridor) 5"},{"$f":"'Individual Spaces'!E126","v":0},null,{"$f":"VLOOKUP($B127,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_87"},{"$f":"VLOOKUP($B127,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Teaching resources stores"},{"$f":"'Individual Spaces'!G126","v":"Humanities"},{"$f":"'Individual Spaces'!H126","v":5},null,null,null,-5,null,null,{"$f":"'Individual Spaces'!O126","v":0},{"$f":"'Individual Spaces'!P126","v":0},{"$f":"'Individual Spaces'!Q126","v":0},{"$f":"'Individual Spaces'!R126","v":0},null,0,{"$f":"IF(AF127=\"-\",0,ROUND((J127-VLOOKUP(B127,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B127,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B127,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B127,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J127-VLOOKUP(B127,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B127,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B127,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Store room for general teaching or ICT resources"},{"$f":"VLOOKUP($B127,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing teaching resources including books, files and digital equipment."},{"$f":"VLOOKUP($B127,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B127,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B127,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B127,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B127,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A127","v":"STT10"},{"$f":"'Individual Spaces'!B127","v":"STT13"},{"$f":"'Individual Spaces'!C127","v":5006},{"$f":"'Individual Spaces'!D127","v":"Teaching resources store (IT/ GT off corridor) 6"},{"$f":"'Individual Spaces'!E127","v":0},null,{"$f":"VLOOKUP($B128,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_87"},{"$f":"VLOOKUP($B128,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Teaching resources stores"},{"$f":"'Individual Spaces'!G127","v":"Humanities"},{"$f":"'Individual Spaces'!H127","v":5},null,null,null,-5,null,null,{"$f":"'Individual Spaces'!O127","v":0},{"$f":"'Individual Spaces'!P127","v":0},{"$f":"'Individual Spaces'!Q127","v":0},{"$f":"'Individual Spaces'!R127","v":0},null,0,{"$f":"IF(AF128=\"-\",0,ROUND((J128-VLOOKUP(B128,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B128,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B128,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B128,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J128-VLOOKUP(B128,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B128,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B128,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Store room for general teaching or ICT resources"},{"$f":"VLOOKUP($B128,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing teaching resources including books, files and digital equipment."},{"$f":"VLOOKUP($B128,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B128,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B128,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B128,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B128,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A128","v":"STT20"},{"$f":"'Individual Spaces'!B128","v":"STT21"},{"$f":"'Individual Spaces'!C128","v":5007},{"$f":"'Individual Spaces'!D128","v":"Science prep room (central) 1"},{"$f":"'Individual Spaces'!E128","v":0},null,{"$f":"VLOOKUP($B129,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_80_75"},{"$f":"VLOOKUP($B129,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Science preparation rooms"},{"$f":"'Individual Spaces'!G128","v":"Science"},{"$f":"'Individual Spaces'!H128","v":111},null,null,null,-111,null,null,{"$f":"'Individual Spaces'!O128","v":0},{"$f":"'Individual Spaces'!P128","v":0},{"$f":"'Individual Spaces'!Q128","v":0},{"$f":"'Individual Spaces'!R128","v":0},null,0,{"$f":"IF(AF129=\"-\",0,ROUND((J129-VLOOKUP(B129,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B129,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":5},{"$f":"IF(VLOOKUP(B129,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B129,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J129-VLOOKUP(B129,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B129,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":2},6,null,null,{"$f":"VLOOKUP($B129,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Technician's preparation/ store room for all labs or studios in suite"},{"$f":"VLOOKUP($B129,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administrative tasks requiring ICT. Preparation of materials for practical activities. Stocktaking. Storing and cleaning equipment."},{"$f":"VLOOKUP($B129,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B129,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Light practical (science)"},{"$f":"VLOOKUP($B129,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":0},{"$f":"VLOOKUP($B129,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B129,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A129","v":"STT23"},{"$f":"'Individual Spaces'!B129","v":"STT23"},{"$f":"'Individual Spaces'!C129","v":5008},{"$f":"'Individual Spaces'!D129","v":"Chemicals store, science 1"},{"$f":"'Individual Spaces'!E129","v":0},null,{"$f":"VLOOKUP($B130,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_13"},{"$f":"VLOOKUP($B130,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Chemicals stores"},{"$f":"'Individual Spaces'!G129","v":"Science"},{"$f":"'Individual Spaces'!H129","v":7},null,null,null,-7,null,null,{"$f":"'Individual Spaces'!O129","v":0},{"$f":"'Individual Spaces'!P129","v":0},{"$f":"'Individual Spaces'!Q129","v":0},{"$f":"'Individual Spaces'!R129","v":0},null,0,{"$f":"IF(AF130=\"-\",0,ROUND((J130-VLOOKUP(B130,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B130,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B130,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B130,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J130-VLOOKUP(B130,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B130,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B130,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Chemical store associated with science prep room"},{"$f":"VLOOKUP($B130,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing chemicals, some hazardous."},{"$f":"VLOOKUP($B130,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B130,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B130,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B130,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B130,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A130","v":"STT10"},{"$f":"'Individual Spaces'!B130","v":"STT16"},{"$f":"'Individual Spaces'!C130","v":5009},{"$f":"'Individual Spaces'!D130","v":"Teaching resources store (off art room) 1"},{"$f":"'Individual Spaces'!E130","v":0},null,{"$f":"VLOOKUP($B131,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_87"},{"$f":"VLOOKUP($B131,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Teaching resources stores"},{"$f":"'Individual Spaces'!G130","v":"DT/ Art"},{"$f":"'Individual Spaces'!H130","v":5},null,null,null,-5,null,null,{"$f":"'Individual Spaces'!O130","v":0},{"$f":"'Individual Spaces'!P130","v":0},{"$f":"'Individual Spaces'!Q130","v":0},{"$f":"'Individual Spaces'!R130","v":0},null,0,{"$f":"IF(AF131=\"-\",0,ROUND((J131-VLOOKUP(B131,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B131,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B131,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B131,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J131-VLOOKUP(B131,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B131,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B131,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Store room for art teaching resources or work in progress"},{"$f":"VLOOKUP($B131,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing teaching resources and materials relevant to the teaching space (e.g. art, graphics or music) and/or work in progress. Storing teaching resources including books, files and equipment."},{"$f":"VLOOKUP($B131,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B131,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B131,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B131,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B131,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A131","v":"STT10"},{"$f":"'Individual Spaces'!B131","v":"STT16"},{"$f":"'Individual Spaces'!C131","v":5010},{"$f":"'Individual Spaces'!D131","v":"Teaching resources store (off art room) 2"},{"$f":"'Individual Spaces'!E131","v":0},null,{"$f":"VLOOKUP($B132,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_87"},{"$f":"VLOOKUP($B132,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Teaching resources stores"},{"$f":"'Individual Spaces'!G131","v":"DT/ Art"},{"$f":"'Individual Spaces'!H131","v":5},null,null,null,-5,null,null,{"$f":"'Individual Spaces'!O131","v":0},{"$f":"'Individual Spaces'!P131","v":0},{"$f":"'Individual Spaces'!Q131","v":0},{"$f":"'Individual Spaces'!R131","v":0},null,0,{"$f":"IF(AF132=\"-\",0,ROUND((J132-VLOOKUP(B132,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B132,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B132,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B132,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J132-VLOOKUP(B132,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B132,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B132,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Store room for art teaching resources or work in progress"},{"$f":"VLOOKUP($B132,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing teaching resources and materials relevant to the teaching space (e.g. art, graphics or music) and/or work in progress. Storing teaching resources including books, files and equipment."},{"$f":"VLOOKUP($B132,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B132,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B132,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B132,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B132,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A132","v":"STT10"},{"$f":"'Individual Spaces'!B132","v":"STT16"},{"$f":"'Individual Spaces'!C132","v":5011},{"$f":"'Individual Spaces'!D132","v":"Teaching resources store (off art room) 3"},{"$f":"'Individual Spaces'!E132","v":0},null,{"$f":"VLOOKUP($B133,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_87"},{"$f":"VLOOKUP($B133,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Teaching resources stores"},{"$f":"'Individual Spaces'!G132","v":"DT/ Art"},{"$f":"'Individual Spaces'!H132","v":5},null,null,null,-5,null,null,{"$f":"'Individual Spaces'!O132","v":0},{"$f":"'Individual Spaces'!P132","v":0},{"$f":"'Individual Spaces'!Q132","v":0},{"$f":"'Individual Spaces'!R132","v":0},null,0,{"$f":"IF(AF133=\"-\",0,ROUND((J133-VLOOKUP(B133,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B133,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B133,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B133,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J133-VLOOKUP(B133,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B133,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B133,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Store room for art teaching resources or work in progress"},{"$f":"VLOOKUP($B133,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing teaching resources and materials relevant to the teaching space (e.g. art, graphics or music) and/or work in progress. Storing teaching resources including books, files and equipment."},{"$f":"VLOOKUP($B133,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B133,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B133,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B133,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B133,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A133","v":"STT10"},{"$f":"'Individual Spaces'!B133","v":"STT16"},{"$f":"'Individual Spaces'!C133","v":5012},{"$f":"'Individual Spaces'!D133","v":"Teaching resources store (off art room) 4"},{"$f":"'Individual Spaces'!E133","v":0},null,{"$f":"VLOOKUP($B134,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_87"},{"$f":"VLOOKUP($B134,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Teaching resources stores"},{"$f":"'Individual Spaces'!G133","v":"DT/ Art"},{"$f":"'Individual Spaces'!H133","v":5},null,null,null,{"$f":"M134-J134","v":-5},null,null,{"$f":"'Individual Spaces'!O133","v":0},{"$f":"'Individual Spaces'!P133","v":0},{"$f":"'Individual Spaces'!Q133","v":0},{"$f":"'Individual Spaces'!R133","v":0},null,{"$f":"Q134","v":0},{"$f":"IF(AF134=\"-\",0,ROUND((J134-VLOOKUP(B134,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B134,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B134,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B134,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J134-VLOOKUP(B134,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B134,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},{"$f":"IF(W134>200,ROUND(W134*1.05,0),ROUNDUP(W134*1.1,0))","v":0},null,null,{"$f":"VLOOKUP($B134,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Store room for art teaching resources or work in progress"},{"$f":"VLOOKUP($B134,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing teaching resources and materials relevant to the teaching space (e.g. art, graphics or music) and/or work in progress. Storing teaching resources including books, files and equipment."},{"$f":"VLOOKUP($B134,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B134,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B134,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B134,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B134,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A134","v":"STT10"},{"$f":"'Individual Spaces'!B134","v":"STT16"},{"$f":"'Individual Spaces'!C134","v":5013},{"$f":"'Individual Spaces'!D134","v":"Teaching resources store (off art room) 5"},{"$f":"'Individual Spaces'!E134","v":0},null,{"$f":"VLOOKUP($B135,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_87"},{"$f":"VLOOKUP($B135,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Teaching resources stores"},{"$f":"'Individual Spaces'!G134","v":"DT/ Art"},{"$f":"'Individual Spaces'!H134","v":5},null,null,null,-5,null,null,{"$f":"'Individual Spaces'!O134","v":0},{"$f":"'Individual Spaces'!P134","v":0},{"$f":"'Individual Spaces'!Q134","v":0},{"$f":"'Individual Spaces'!R134","v":0},null,0,{"$f":"IF(AF135=\"-\",0,ROUND((J135-VLOOKUP(B135,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B135,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B135,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B135,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J135-VLOOKUP(B135,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B135,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B135,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Store room for art teaching resources or work in progress"},{"$f":"VLOOKUP($B135,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing teaching resources and materials relevant to the teaching space (e.g. art, graphics or music) and/or work in progress. Storing teaching resources including books, files and equipment."},{"$f":"VLOOKUP($B135,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B135,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B135,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B135,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B135,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A135","v":"STT10"},{"$f":"'Individual Spaces'!B135","v":"STT16"},{"$f":"'Individual Spaces'!C135","v":5014},{"$f":"'Individual Spaces'!D135","v":"Teaching resources store (off art room) 6"},{"$f":"'Individual Spaces'!E135","v":0},null,{"$f":"VLOOKUP($B136,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_87"},{"$f":"VLOOKUP($B136,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Teaching resources stores"},{"$f":"'Individual Spaces'!G135","v":"DT/ Art"},{"$f":"'Individual Spaces'!H135","v":5},null,null,null,-5,null,null,{"$f":"'Individual Spaces'!O135","v":0},{"$f":"'Individual Spaces'!P135","v":0},{"$f":"'Individual Spaces'!Q135","v":0},{"$f":"'Individual Spaces'!R135","v":0},null,0,{"$f":"IF(AF136=\"-\",0,ROUND((J136-VLOOKUP(B136,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B136,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B136,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B136,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J136-VLOOKUP(B136,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B136,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B136,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Store room for art teaching resources or work in progress"},{"$f":"VLOOKUP($B136,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing teaching resources and materials relevant to the teaching space (e.g. art, graphics or music) and/or work in progress. Storing teaching resources including books, files and equipment."},{"$f":"VLOOKUP($B136,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B136,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B136,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B136,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B136,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A136","v":"STT32"},{"$f":"'Individual Spaces'!B136","v":"STT32"},{"$f":"'Individual Spaces'!C136","v":5015},{"$f":"'Individual Spaces'!D136","v":"DT prep room 1"},{"$f":"'Individual Spaces'!E136","v":0},null,{"$f":"VLOOKUP($B137,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_80_85"},{"$f":"VLOOKUP($B137,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Design technology preparation rooms"},{"$f":"'Individual Spaces'!G136","v":"DT/ Art"},{"$f":"'Individual Spaces'!H136","v":34},null,null,null,-34,null,null,{"$f":"'Individual Spaces'!O136","v":0},{"$f":"'Individual Spaces'!P136","v":0},{"$f":"'Individual Spaces'!Q136","v":0},{"$f":"'Individual Spaces'!R136","v":0},null,0,{"$f":"IF(AF137=\"-\",0,ROUND((J137-VLOOKUP(B137,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B137,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(B137,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B137,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J137-VLOOKUP(B137,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B137,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},5,null,null,{"$f":"VLOOKUP($B137,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Technician's preparation/store room for all resistant materials rooms"},{"$f":"VLOOKUP($B137,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Maintaining tools and equipment. Some administrative work requiring ICT. Storing and preparing resistant materials (wood, metal, plastics) and components for pupils' use."},{"$f":"VLOOKUP($B137,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B137,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Heavy practical (workshop)"},{"$f":"VLOOKUP($B137,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"I"},{"$f":"VLOOKUP($B137,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B137,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A137","v":"STT34"},{"$f":"'Individual Spaces'!B137","v":"STT34"},{"$f":"'Individual Spaces'!C137","v":5016},{"$f":"'Individual Spaces'!D137","v":"Food prep room 1"},{"$f":"'Individual Spaces'!E137","v":0},null,{"$f":"VLOOKUP($B138,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_25_80_30"},{"$f":"VLOOKUP($B138,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Food preparation rooms"},{"$f":"'Individual Spaces'!G137","v":"DT/ Art"},{"$f":"'Individual Spaces'!H137","v":10},null,null,null,-10,null,null,{"$f":"'Individual Spaces'!O137","v":0},{"$f":"'Individual Spaces'!P137","v":0},{"$f":"'Individual Spaces'!Q137","v":0},{"$f":"'Individual Spaces'!R137","v":0},null,0,{"$f":"IF(AF138=\"-\",0,ROUND((J138-VLOOKUP(B138,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B138,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B138,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B138,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J138-VLOOKUP(B138,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B138,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B138,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Technician's preparation/store room for all food rooms"},{"$f":"VLOOKUP($B138,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Laundry of food room linen. Preparing food ingredients for lessons. Storing cooking equipment and ingredients."},{"$f":"VLOOKUP($B138,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B138,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Heavy practical (clean)"},{"$f":"VLOOKUP($B138,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B138,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B138,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A138","v":"STT10"},{"$f":"'Individual Spaces'!B138","v":"STT18"},{"$f":"'Individual Spaces'!C138","v":5017},{"$f":"'Individual Spaces'!D138","v":"Teaching resources store (off DT studio) 1"},{"$f":"'Individual Spaces'!E138","v":0},null,{"$f":"VLOOKUP($B139,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_87"},{"$f":"VLOOKUP($B139,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Teaching resources stores"},{"$f":"'Individual Spaces'!G138","v":"DT/ Art"},{"$f":"'Individual Spaces'!H138","v":5},null,null,null,-5,null,null,{"$f":"'Individual Spaces'!O138","v":0},{"$f":"'Individual Spaces'!P138","v":0},{"$f":"'Individual Spaces'!Q138","v":0},{"$f":"'Individual Spaces'!R138","v":0},null,0,{"$f":"IF(AF139=\"-\",0,ROUND((J139-VLOOKUP(B139,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B139,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B139,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B139,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J139-VLOOKUP(B139,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B139,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B139,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Store room opening off a teaching space for specialist teaching resources or work in progress"},{"$f":"VLOOKUP($B139,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing teaching resources and materials relevant to the teaching space (e.g. art, graphics or music) and/or work in progress. Storing teaching resources including books, files and equipment."},{"$f":"VLOOKUP($B139,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B139,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B139,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B139,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B139,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A139","v":"STT10"},{"$f":"'Individual Spaces'!B139","v":"STT18"},{"$f":"'Individual Spaces'!C139","v":5018},{"$f":"'Individual Spaces'!D139","v":"Teaching resources store (off DT studio) 2"},{"$f":"'Individual Spaces'!E139","v":0},null,{"$f":"VLOOKUP($B140,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_87"},{"$f":"VLOOKUP($B140,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Teaching resources stores"},{"$f":"'Individual Spaces'!G139","v":"DT/ Art"},{"$f":"'Individual Spaces'!H139","v":5},null,null,null,-5,null,null,{"$f":"'Individual Spaces'!O139","v":0},{"$f":"'Individual Spaces'!P139","v":0},{"$f":"'Individual Spaces'!Q139","v":0},{"$f":"'Individual Spaces'!R139","v":0},null,0,{"$f":"IF(AF140=\"-\",0,ROUND((J140-VLOOKUP(B140,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B140,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B140,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B140,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J140-VLOOKUP(B140,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B140,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B140,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Store room opening off a teaching space for specialist teaching resources or work in progress"},{"$f":"VLOOKUP($B140,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing teaching resources and materials relevant to the teaching space (e.g. art, graphics or music) and/or work in progress. Storing teaching resources including books, files and equipment."},{"$f":"VLOOKUP($B140,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B140,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B140,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B140,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B140,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A140","v":"STT10"},{"$f":"'Individual Spaces'!B140","v":"STT18"},{"$f":"'Individual Spaces'!C140","v":5019},{"$f":"'Individual Spaces'!D140","v":"Teaching resources store (off DT studio) 3"},{"$f":"'Individual Spaces'!E140","v":0},null,{"$f":"VLOOKUP($B141,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_87"},{"$f":"VLOOKUP($B141,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Teaching resources stores"},{"$f":"'Individual Spaces'!G140","v":"DT/ Art"},{"$f":"'Individual Spaces'!H140","v":5},null,null,null,-5,null,null,{"$f":"'Individual Spaces'!O140","v":0},{"$f":"'Individual Spaces'!P140","v":0},{"$f":"'Individual Spaces'!Q140","v":0},{"$f":"'Individual Spaces'!R140","v":0},null,0,{"$f":"IF(AF141=\"-\",0,ROUND((J141-VLOOKUP(B141,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B141,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B141,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B141,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J141-VLOOKUP(B141,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B141,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B141,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Store room opening off a teaching space for specialist teaching resources or work in progress"},{"$f":"VLOOKUP($B141,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing teaching resources and materials relevant to the teaching space (e.g. art, graphics or music) and/or work in progress. Storing teaching resources including books, files and equipment."},{"$f":"VLOOKUP($B141,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B141,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B141,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B141,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B141,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A141","v":"STT10"},{"$f":"'Individual Spaces'!B141","v":"STT18"},{"$f":"'Individual Spaces'!C141","v":5020},{"$f":"'Individual Spaces'!D141","v":"Teaching resources store (off DT studio) 4"},{"$f":"'Individual Spaces'!E141","v":0},null,{"$f":"VLOOKUP($B142,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_87"},{"$f":"VLOOKUP($B142,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Teaching resources stores"},{"$f":"'Individual Spaces'!G141","v":"DT/ Art"},{"$f":"'Individual Spaces'!H141","v":5},null,null,null,-5,null,null,{"$f":"'Individual Spaces'!O141","v":0},{"$f":"'Individual Spaces'!P141","v":0},{"$f":"'Individual Spaces'!Q141","v":0},{"$f":"'Individual Spaces'!R141","v":0},null,0,{"$f":"IF(AF142=\"-\",0,ROUND((J142-VLOOKUP(B142,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B142,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B142,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B142,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J142-VLOOKUP(B142,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B142,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B142,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Store room opening off a teaching space for specialist teaching resources or work in progress"},{"$f":"VLOOKUP($B142,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing teaching resources and materials relevant to the teaching space (e.g. art, graphics or music) and/or work in progress. Storing teaching resources including books, files and equipment."},{"$f":"VLOOKUP($B142,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B142,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B142,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B142,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B142,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A142","v":"STT10"},{"$f":"'Individual Spaces'!B142","v":"STT17"},{"$f":"'Individual Spaces'!C142","v":5021},{"$f":"'Individual Spaces'!D142","v":"Teaching resources store (music) 1"},{"$f":"'Individual Spaces'!E142","v":0},null,{"$f":"VLOOKUP($B143,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_87"},{"$f":"VLOOKUP($B143,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Teaching resources stores"},{"$f":"'Individual Spaces'!G142","v":"Perf arts, hall and dining"},{"$f":"'Individual Spaces'!H142","v":5},null,null,null,-5,null,null,{"$f":"'Individual Spaces'!O142","v":0},{"$f":"'Individual Spaces'!P142","v":0},{"$f":"'Individual Spaces'!Q142","v":0},{"$f":"'Individual Spaces'!R142","v":0},null,0,{"$f":"IF(AF143=\"-\",0,ROUND((J143-VLOOKUP(B143,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B143,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B143,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B143,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J143-VLOOKUP(B143,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B143,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B143,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Store room for music teaching resources or instruments"},{"$f":"VLOOKUP($B143,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing teaching resources including books, files and digital equipment."},{"$f":"VLOOKUP($B143,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B143,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B143,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B143,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B143,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A143","v":"STT10"},{"$f":"'Individual Spaces'!B143","v":"STT17"},{"$f":"'Individual Spaces'!C143","v":5022},{"$f":"'Individual Spaces'!D143","v":"Teaching resources store (music) 2"},{"$f":"'Individual Spaces'!E143","v":0},null,{"$f":"VLOOKUP($B144,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_87"},{"$f":"VLOOKUP($B144,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Teaching resources stores"},{"$f":"'Individual Spaces'!G143","v":"Perf arts, hall and dining"},{"$f":"'Individual Spaces'!H143","v":5},null,null,null,-5,null,null,{"$f":"'Individual Spaces'!O143","v":0},{"$f":"'Individual Spaces'!P143","v":0},{"$f":"'Individual Spaces'!Q143","v":0},{"$f":"'Individual Spaces'!R143","v":0},null,0,{"$f":"IF(AF144=\"-\",0,ROUND((J144-VLOOKUP(B144,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B144,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B144,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B144,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J144-VLOOKUP(B144,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B144,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B144,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Store room for music teaching resources or instruments"},{"$f":"VLOOKUP($B144,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing teaching resources including books, files and digital equipment."},{"$f":"VLOOKUP($B144,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B144,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B144,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B144,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B144,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A144","v":"STT08"},{"$f":"'Individual Spaces'!B144","v":"STT08"},{"$f":"'Individual Spaces'!C144","v":5023},{"$f":"'Individual Spaces'!D144","v":"Equipment store, drama 1"},{"$f":"'Individual Spaces'!E144","v":0},null,{"$f":"VLOOKUP($B145,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_27"},{"$f":"VLOOKUP($B145,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Equipment stores"},{"$f":"'Individual Spaces'!G144","v":"Perf arts, hall and dining"},{"$f":"'Individual Spaces'!H144","v":10},null,null,null,-10,null,null,{"$f":"'Individual Spaces'!O144","v":0},{"$f":"'Individual Spaces'!P144","v":0},{"$f":"'Individual Spaces'!Q144","v":0},{"$f":"'Individual Spaces'!R144","v":0},null,0,{"$f":"IF(AF145=\"-\",0,ROUND((J145-VLOOKUP(B145,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B145,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B145,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B145,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J145-VLOOKUP(B145,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B145,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B145,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Store room for drama teaching resources, opening off drama studio"},{"$f":"VLOOKUP($B145,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing drama teaching resources including costumes, props and some flats."},{"$f":"VLOOKUP($B145,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B145,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B145,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B145,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B145,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A145","v":"STT10"},{"$f":"'Individual Spaces'!B145","v":"STT41"},{"$f":"'Individual Spaces'!C145","v":5024},{"$f":"'Individual Spaces'!D145","v":"Teaching resources store, room (off LRC) 1"},{"$f":"'Individual Spaces'!E145","v":0},null,{"$f":"VLOOKUP($B146,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_87"},{"$f":"VLOOKUP($B146,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Teaching resources stores"},{"$f":"'Individual Spaces'!G145","v":"Balance"},{"$f":"'Individual Spaces'!H145","v":3},null,null,null,-3,null,null,{"$f":"'Individual Spaces'!O145","v":0},{"$f":"'Individual Spaces'!P145","v":0},{"$f":"'Individual Spaces'!Q145","v":0},{"$f":"'Individual Spaces'!R145","v":0},null,0,{"$f":"IF(AF146=\"-\",0,ROUND((J146-VLOOKUP(B146,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B146,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B146,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B146,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J146-VLOOKUP(B146,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B146,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B146,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Store room for teaching resources or materials"},{"$f":"VLOOKUP($B146,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing teaching resources including books, files and digital equipment."},{"$f":"VLOOKUP($B146,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B146,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B146,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B146,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B146,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A146","v":"STT00"},{"$f":"'Individual Spaces'!B146","v":"STT42"},{"$f":"'Individual Spaces'!C146","v":5025},{"$f":"'Individual Spaces'!D146","v":"Classroom store, room (off SEN room) 1"},{"$f":"'Individual Spaces'!E146","v":0},null,{"$f":"VLOOKUP($B147,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_18"},{"$f":"VLOOKUP($B147,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Classroom stores"},{"$f":"'Individual Spaces'!G146","v":"Balance"},{"$f":"'Individual Spaces'!H146","v":5},null,null,null,-5,null,null,{"$f":"'Individual Spaces'!O146","v":0},{"$f":"'Individual Spaces'!P146","v":0},{"$f":"'Individual Spaces'!Q146","v":0},{"$f":"'Individual Spaces'!R146","v":0},null,0,{"$f":"IF(AF147=\"-\",0,ROUND((J147-VLOOKUP(B147,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B147,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B147,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B147,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J147-VLOOKUP(B147,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B147,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B147,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Store room for teaching resources or materials"},{"$f":"VLOOKUP($B147,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing teaching resources including books, files and digital equipment."},{"$f":"VLOOKUP($B147,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B147,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B147,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B147,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B147,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A147","v":"STH00"},{"$f":"'Individual Spaces'!B147","v":"STH01"},{"$f":"'Individual Spaces'!C147","v":5026},{"$f":"'Individual Spaces'!D147","v":"Sports equipment store, internal (sports hall) 1"},{"$f":"'Individual Spaces'!E147","v":0},null,{"$f":"VLOOKUP($B148,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_82"},{"$f":"VLOOKUP($B148,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Sports equipment stores"},{"$f":"'Individual Spaces'!G147","v":"Sports/ PE"},{"$f":"'Individual Spaces'!H147","v":60},null,null,null,-60,null,null,{"$f":"'Individual Spaces'!O147","v":0},{"$f":"'Individual Spaces'!P147","v":0},{"$f":"'Individual Spaces'!Q147","v":0},{"$f":"'Individual Spaces'!R147","v":0},null,0,{"$f":"IF(AF148=\"-\",0,ROUND((J148-VLOOKUP(B148,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B148,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B148,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B148,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J148-VLOOKUP(B148,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B148,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B148,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Storage for PE and sports equipment, including mats"},{"$f":"VLOOKUP($B148,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing PE and sports equipment including trampolines, forms, racquets and balls."},{"$f":"VLOOKUP($B148,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B148,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B148,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B148,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B148,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Optional"}]
[{"$f":"'Individual Spaces'!A148","v":"STH00"},{"$f":"'Individual Spaces'!B148","v":"STH02"},{"$f":"'Individual Spaces'!C148","v":5027},{"$f":"'Individual Spaces'!D148","v":"Sports equipment store, internal (community) 1"},{"$f":"'Individual Spaces'!E148","v":0},null,{"$f":"VLOOKUP($B149,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_82"},{"$f":"VLOOKUP($B149,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Sports equipment stores"},{"$f":"'Individual Spaces'!G148","v":"Sports/ PE"},{"$f":"'Individual Spaces'!H148","v":4},null,null,null,-4,null,null,{"$f":"'Individual Spaces'!O148","v":0},{"$f":"'Individual Spaces'!P148","v":0},{"$f":"'Individual Spaces'!Q148","v":0},{"$f":"'Individual Spaces'!R148","v":0},null,0,{"$f":"IF(AF149=\"-\",0,ROUND((J149-VLOOKUP(B149,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B149,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B149,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B149,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J149-VLOOKUP(B149,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B149,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B149,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Storage for PE and sports equipment, including mats"},{"$f":"VLOOKUP($B149,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing PE and sports equipment including trampolines, forms, racquets and balls."},{"$f":"VLOOKUP($B149,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B149,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B149,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B149,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B149,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Yes"}]
[{"$f":"'Individual Spaces'!A149","v":"STH00"},{"$f":"'Individual Spaces'!B149","v":"STH03"},{"$f":"'Individual Spaces'!C149","v":5028},{"$f":"'Individual Spaces'!D149","v":"Sports equipment store, internal (activity studio) 1"},{"$f":"'Individual Spaces'!E149","v":0},null,{"$f":"VLOOKUP($B150,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_82"},{"$f":"VLOOKUP($B150,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Sports equipment stores"},{"$f":"'Individual Spaces'!G149","v":"Sports/ PE"},{"$f":"'Individual Spaces'!H149","v":15},null,null,null,-15,null,null,{"$f":"'Individual Spaces'!O149","v":0},{"$f":"'Individual Spaces'!P149","v":0},{"$f":"'Individual Spaces'!Q149","v":0},{"$f":"'Individual Spaces'!R149","v":0},null,0,{"$f":"IF(AF150=\"-\",0,ROUND((J150-VLOOKUP(B150,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B150,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B150,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B150,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J150-VLOOKUP(B150,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B150,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B150,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Storage for PE and sports equipment, including mats"},{"$f":"VLOOKUP($B150,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing PE and sports equipment including trampolines, forms, racquets and balls."},{"$f":"VLOOKUP($B150,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B150,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B150,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B150,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B150,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Optional"}]
[{"$f":"'Individual Spaces'!A150","v":"STH05"},{"$f":"'Individual Spaces'!B150","v":"STH05"},{"$f":"'Individual Spaces'!C150","v":5029},{"$f":"'Individual Spaces'!D150","v":"Sports equipment store, external 1"},{"$f":"'Individual Spaces'!E150","v":0},null,{"$f":"VLOOKUP($B151,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_82"},{"$f":"VLOOKUP($B151,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Sports equipment stores"},{"$f":"'Individual Spaces'!G150","v":"Sports/ PE"},{"$f":"'Individual Spaces'!H150","v":8},null,null,null,-8,null,null,{"$f":"'Individual Spaces'!O150","v":0},{"$f":"'Individual Spaces'!P150","v":0},{"$f":"'Individual Spaces'!Q150","v":0},{"$f":"'Individual Spaces'!R150","v":0},null,0,{"$f":"IF(AF151=\"-\",0,ROUND((J151-VLOOKUP(B151,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B151,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B151,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B151,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J151-VLOOKUP(B151,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B151,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B151,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Store for external PE and sports activities"},{"$f":"VLOOKUP($B151,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing equipment for outdoor sports including goals, nets, bats, racquets, balls."},{"$f":"VLOOKUP($B151,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (teaching)"},{"$f":"VLOOKUP($B151,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B151,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B151,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B151,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Optional"}]
[{"$f":"'Individual Spaces'!A151","v":0},{"$f":"'Individual Spaces'!B151","v":0},{"$f":"'Individual Spaces'!C151","v":0},{"$f":"'Individual Spaces'!D151","v":0},{"$f":"'Individual Spaces'!E151","v":"Teaching Storage Total : "},null,{"$f":"VLOOKUP($B152,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B152,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G151","v":0},{"$f":"'Individual Spaces'!H151","v":357},null,null,null,-357,null,null,{"$f":"'Individual Spaces'!O151","v":0},{"$f":"'Individual Spaces'!P151","v":0},{"$f":"'Individual Spaces'!Q151","v":0},{"$f":"'Individual Spaces'!R151","v":0},null,0,{"$f":"IF(AF152=\"-\",0,ROUND((J152-VLOOKUP(B152,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B152,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B152,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B152,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J152-VLOOKUP(B152,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B152,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B152,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B152,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B152,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B152,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B152,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B152,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B152,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A152","v":"STH10"},{"$f":"'Individual Spaces'!B152","v":"STH11"},{"$f":"'Individual Spaces'!C152","v":5101},{"$f":"'Individual Spaces'!D152","v":"Furniture store (chair/ table, off hall) 1"},{"$f":"'Individual Spaces'!E152","v":0},null,{"$f":"VLOOKUP($B153,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_32"},{"$f":"VLOOKUP($B153,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Furniture stores"},{"$f":"'Individual Spaces'!G152","v":"Perf arts, hall and dining"},{"$f":"'Individual Spaces'!H152","v":20},null,null,null,-20,null,null,{"$f":"'Individual Spaces'!O152","v":0},{"$f":"'Individual Spaces'!P152","v":0},{"$f":"'Individual Spaces'!Q152","v":0},{"$f":"'Individual Spaces'!R152","v":0},null,0,{"$f":"IF(AF153=\"-\",0,ROUND((J153-VLOOKUP(B153,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B153,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B153,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B153,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J153-VLOOKUP(B153,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B153,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B153,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Storage for chairs and tables used in hall"},{"$f":"VLOOKUP($B153,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storage for chairs for assemblies, exams and performances, as well as dining (with tables if required) in an adjacent hall."},{"$f":"VLOOKUP($B153,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B153,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B153,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B153,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B153,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Optional"}]
[{"$f":"'Individual Spaces'!A153","v":"STN20"},{"$f":"'Individual Spaces'!B153","v":"STN22"},{"$f":"'Individual Spaces'!C153","v":5102},{"$f":"'Individual Spaces'!D153","v":"General storeroom (central stock) 1"},{"$f":"'Individual Spaces'!E153","v":0},null,{"$f":"VLOOKUP($B154,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_35"},{"$f":"VLOOKUP($B154,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"General storerooms"},{"$f":"'Individual Spaces'!G153","v":"Balance"},{"$f":"'Individual Spaces'!H153","v":6},null,null,null,-6,null,null,{"$f":"'Individual Spaces'!O153","v":0},{"$f":"'Individual Spaces'!P153","v":0},{"$f":"'Individual Spaces'!Q153","v":0},{"$f":"'Individual Spaces'!R153","v":0},null,0,{"$f":"IF(AF154=\"-\",0,ROUND((J154-VLOOKUP(B154,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B154,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B154,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B154,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J154-VLOOKUP(B154,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B154,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B154,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Storage of stock and stationery"},{"$f":"VLOOKUP($B154,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing bulk items of paper or stock"},{"$f":"VLOOKUP($B154,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B154,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B154,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B154,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B154,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A154","v":"STN20"},{"$f":"'Individual Spaces'!B154","v":"STN22"},{"$f":"'Individual Spaces'!C154","v":5103},{"$f":"'Individual Spaces'!D154","v":"General storeroom (central stock) 2"},{"$f":"'Individual Spaces'!E154","v":0},null,{"$f":"VLOOKUP($B155,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_35"},{"$f":"VLOOKUP($B155,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"General storerooms"},{"$f":"'Individual Spaces'!G154","v":"Balance"},{"$f":"'Individual Spaces'!H154","v":6},null,null,null,-6,null,null,{"$f":"'Individual Spaces'!O154","v":0},{"$f":"'Individual Spaces'!P154","v":0},{"$f":"'Individual Spaces'!Q154","v":0},{"$f":"'Individual Spaces'!R154","v":0},null,0,{"$f":"IF(AF155=\"-\",0,ROUND((J155-VLOOKUP(B155,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B155,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B155,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B155,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J155-VLOOKUP(B155,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B155,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B155,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Storage of stock and stationery"},{"$f":"VLOOKUP($B155,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing bulk items of paper or stock"},{"$f":"VLOOKUP($B155,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B155,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B155,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B155,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B155,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A155","v":"STN50"},{"$f":"'Individual Spaces'!B155","v":"STN50"},{"$f":"'Individual Spaces'!C155","v":5104},{"$f":"'Individual Spaces'!D155","v":"Secure storeroom 1"},{"$f":"'Individual Spaces'!E155","v":0},null,{"$f":"VLOOKUP($B156,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_77"},{"$f":"VLOOKUP($B156,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Secure storerooms"},{"$f":"'Individual Spaces'!G155","v":"Admin"},{"$f":"'Individual Spaces'!H155","v":8},null,null,null,-8,null,null,{"$f":"'Individual Spaces'!O155","v":0},{"$f":"'Individual Spaces'!P155","v":0},{"$f":"'Individual Spaces'!Q155","v":0},{"$f":"'Individual Spaces'!R155","v":0},null,0,{"$f":"IF(AF156=\"-\",0,ROUND((J156-VLOOKUP(B156,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B156,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B156,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B156,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J156-VLOOKUP(B156,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B156,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B156,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secure storage of exam papers, archives or medical equipment and drugs"},{"$f":"VLOOKUP($B156,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing examination papers, archived documents or other confidential items securely."},{"$f":"VLOOKUP($B156,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B156,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B156,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B156,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B156,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A156","v":"STN50"},{"$f":"'Individual Spaces'!B156","v":"STN50"},{"$f":"'Individual Spaces'!C156","v":5105},{"$f":"'Individual Spaces'!D156","v":"Secure storeroom 2"},{"$f":"'Individual Spaces'!E156","v":0},null,{"$f":"VLOOKUP($B157,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_77"},{"$f":"VLOOKUP($B157,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Secure storerooms"},{"$f":"'Individual Spaces'!G156","v":"Admin"},{"$f":"'Individual Spaces'!H156","v":8},null,null,null,-8,null,null,{"$f":"'Individual Spaces'!O156","v":0},{"$f":"'Individual Spaces'!P156","v":0},{"$f":"'Individual Spaces'!Q156","v":0},{"$f":"'Individual Spaces'!R156","v":0},null,0,{"$f":"IF(AF157=\"-\",0,ROUND((J157-VLOOKUP(B157,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B157,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B157,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B157,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J157-VLOOKUP(B157,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B157,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B157,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Secure storage of exam papers, archives or medical equipment and drugs"},{"$f":"VLOOKUP($B157,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing examination papers, archived documents or other confidential items securely."},{"$f":"VLOOKUP($B157,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B157,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B157,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B157,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B157,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A157","v":"CIR06"},{"$f":"'Individual Spaces'!B157","v":"CIR06"},{"$f":"'Individual Spaces'!C157","v":5106},{"$f":"'Individual Spaces'!D157","v":"Equipment store, appliance bay 1"},{"$f":"'Individual Spaces'!E157","v":0},null,{"$f":"VLOOKUP($B158,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_27"},{"$f":"VLOOKUP($B158,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Equipment stores"},{"$f":"'Individual Spaces'!G157","v":"Balance"},{"$f":"'Individual Spaces'!H157","v":1.5},null,null,null,-1.5,null,null,{"$f":"'Individual Spaces'!O157","v":0},{"$f":"'Individual Spaces'!P157","v":0},{"$f":"'Individual Spaces'!Q157","v":0},{"$f":"'Individual Spaces'!R157","v":0},null,0,{"$f":"IF(AF158=\"-\",0,ROUND((J158-VLOOKUP(B158,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B158,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B158,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B158,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J158-VLOOKUP(B158,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B158,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B158,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Bay off circulation area for parking and charging a wheelchair or other appliances"},{"$f":"VLOOKUP($B158,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Space for appliances to be stored and charged where necessary. Space for wheelchairs."},{"$f":"VLOOKUP($B158,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B158,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B158,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B158,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B158,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A158","v":"CIR06"},{"$f":"'Individual Spaces'!B158","v":"CIR06"},{"$f":"'Individual Spaces'!C158","v":5107},{"$f":"'Individual Spaces'!D158","v":"Equipment store, appliance bay 2"},{"$f":"'Individual Spaces'!E158","v":0},null,{"$f":"VLOOKUP($B159,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_27"},{"$f":"VLOOKUP($B159,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Equipment stores"},{"$f":"'Individual Spaces'!G158","v":"Balance"},{"$f":"'Individual Spaces'!H158","v":1.5},null,null,null,-1.5,null,null,{"$f":"'Individual Spaces'!O158","v":0},{"$f":"'Individual Spaces'!P158","v":0},{"$f":"'Individual Spaces'!Q158","v":0},{"$f":"'Individual Spaces'!R158","v":0},null,0,{"$f":"IF(AF159=\"-\",0,ROUND((J159-VLOOKUP(B159,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B159,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B159,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B159,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J159-VLOOKUP(B159,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B159,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B159,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Bay off circulation area for parking and charging a wheelchair or other appliances"},{"$f":"VLOOKUP($B159,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Space for appliances to be stored and charged where necessary. Space for wheelchairs."},{"$f":"VLOOKUP($B159,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B159,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B159,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B159,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B159,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A159","v":"CIR06"},{"$f":"'Individual Spaces'!B159","v":"CIR06"},{"$f":"'Individual Spaces'!C159","v":5108},{"$f":"'Individual Spaces'!D159","v":"Equipment store, appliance bay 3"},{"$f":"'Individual Spaces'!E159","v":0},null,{"$f":"VLOOKUP($B160,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_27"},{"$f":"VLOOKUP($B160,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Equipment stores"},{"$f":"'Individual Spaces'!G159","v":"Balance"},{"$f":"'Individual Spaces'!H159","v":1.5},null,null,null,-1.5,null,null,{"$f":"'Individual Spaces'!O159","v":0},{"$f":"'Individual Spaces'!P159","v":0},{"$f":"'Individual Spaces'!Q159","v":0},{"$f":"'Individual Spaces'!R159","v":0},null,0,{"$f":"IF(AF160=\"-\",0,ROUND((J160-VLOOKUP(B160,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B160,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B160,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B160,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J160-VLOOKUP(B160,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B160,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B160,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Bay off circulation area for parking and charging a wheelchair or other appliances"},{"$f":"VLOOKUP($B160,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Space for appliances to be stored and charged where necessary. Space for wheelchairs."},{"$f":"VLOOKUP($B160,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B160,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B160,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B160,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B160,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A160","v":"CIR06"},{"$f":"'Individual Spaces'!B160","v":"CIR06"},{"$f":"'Individual Spaces'!C160","v":5109},{"$f":"'Individual Spaces'!D160","v":"Equipment store, appliance bay 4"},{"$f":"'Individual Spaces'!E160","v":0},null,{"$f":"VLOOKUP($B161,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_27"},{"$f":"VLOOKUP($B161,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Equipment stores"},{"$f":"'Individual Spaces'!G160","v":"Balance"},{"$f":"'Individual Spaces'!H160","v":1.5},null,null,null,-1.5,null,null,{"$f":"'Individual Spaces'!O160","v":0},{"$f":"'Individual Spaces'!P160","v":0},{"$f":"'Individual Spaces'!Q160","v":0},{"$f":"'Individual Spaces'!R160","v":0},null,0,{"$f":"IF(AF161=\"-\",0,ROUND((J161-VLOOKUP(B161,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B161,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B161,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B161,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J161-VLOOKUP(B161,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B161,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B161,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Bay off circulation area for parking and charging a wheelchair or other appliances"},{"$f":"VLOOKUP($B161,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Space for appliances to be stored and charged where necessary. Space for wheelchairs."},{"$f":"VLOOKUP($B161,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B161,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"General"},{"$f":"VLOOKUP($B161,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B161,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B161,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A161","v":"STH20"},{"$f":"'Individual Spaces'!B161","v":"STH20"},{"$f":"'Individual Spaces'!C161","v":5110},{"$f":"'Individual Spaces'!D161","v":"Retractable seating storage (off hall) 1"},{"$f":"'Individual Spaces'!E161","v":0},null,{"$f":"VLOOKUP($B162,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_73"},{"$f":"VLOOKUP($B162,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Retractable seating storage"},{"$f":"'Individual Spaces'!G161","v":"Perf arts, hall and dining"},{"$f":"'Individual Spaces'!H161","v":16},null,null,null,-16,null,null,{"$f":"'Individual Spaces'!O161","v":0},{"$f":"'Individual Spaces'!P161","v":0},{"$f":"'Individual Spaces'!Q161","v":0},{"$f":"'Individual Spaces'!R161","v":0},null,0,{"$f":"IF(AF162=\"-\",0,ROUND((J162-VLOOKUP(B162,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B162,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B162,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B162,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J162-VLOOKUP(B162,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B162,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B162,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"storage of retractable bleacher seating in hall"},{"$f":"VLOOKUP($B162,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storage for retractable bleacher seating in an adjacent hall. Space required when bleacher seating is fully retracted"},{"$f":"VLOOKUP($B162,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B162,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B162,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B162,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B162,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Optional"}]
[{"$f":"'Individual Spaces'!A162","v":"STN00"},{"$f":"'Individual Spaces'!B162","v":"STN02"},{"$f":"'Individual Spaces'!C162","v":5111},{"$f":"'Individual Spaces'!D162","v":"Coats and bag store (lockers) 1"},{"$f":"'Individual Spaces'!E162","v":0},null,{"$f":"VLOOKUP($B163,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_19"},{"$f":"VLOOKUP($B163,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Coats and bags stores"},{"$f":"'Individual Spaces'!G162","v":"Mathematics"},{"$f":"'Individual Spaces'!H162","v":10},null,null,null,-10,null,null,{"$f":"'Individual Spaces'!O162","v":0},{"$f":"'Individual Spaces'!P162","v":0},{"$f":"'Individual Spaces'!Q162","v":0},{"$f":"'Individual Spaces'!R162","v":0},null,0,{"$f":"IF(AF163=\"-\",0,ROUND((J163-VLOOKUP(B163,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B163,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B163,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B163,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J163-VLOOKUP(B163,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B163,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B163,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Space for lockers, and access to lockers, off circulation area"},{"$f":"VLOOKUP($B163,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing pupils personal belongings (coats, bags, books, PE equipment etc)."},{"$f":"VLOOKUP($B163,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B163,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B163,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B163,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B163,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A163","v":"STN00"},{"$f":"'Individual Spaces'!B163","v":"STN02"},{"$f":"'Individual Spaces'!C163","v":5112},{"$f":"'Individual Spaces'!D163","v":"Coats and bag store (lockers) 2"},{"$f":"'Individual Spaces'!E163","v":0},null,{"$f":"VLOOKUP($B164,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_19"},{"$f":"VLOOKUP($B164,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Coats and bags stores"},{"$f":"'Individual Spaces'!G163","v":"English"},{"$f":"'Individual Spaces'!H163","v":10},null,null,null,-10,null,null,{"$f":"'Individual Spaces'!O163","v":0},{"$f":"'Individual Spaces'!P163","v":0},{"$f":"'Individual Spaces'!Q163","v":0},{"$f":"'Individual Spaces'!R163","v":0},null,0,{"$f":"IF(AF164=\"-\",0,ROUND((J164-VLOOKUP(B164,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B164,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B164,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B164,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J164-VLOOKUP(B164,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B164,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B164,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Space for lockers, and access to lockers, off circulation area"},{"$f":"VLOOKUP($B164,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing pupils personal belongings (coats, bags, books, PE equipment etc)."},{"$f":"VLOOKUP($B164,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B164,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B164,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B164,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B164,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A164","v":"STN00"},{"$f":"'Individual Spaces'!B164","v":"STN02"},{"$f":"'Individual Spaces'!C164","v":5113},{"$f":"'Individual Spaces'!D164","v":"Coats and bag store (lockers) 3"},{"$f":"'Individual Spaces'!E164","v":0},null,{"$f":"VLOOKUP($B165,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_19"},{"$f":"VLOOKUP($B165,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Coats and bags stores"},{"$f":"'Individual Spaces'!G164","v":"MFL"},{"$f":"'Individual Spaces'!H164","v":10},null,null,null,-10,null,null,{"$f":"'Individual Spaces'!O164","v":0},{"$f":"'Individual Spaces'!P164","v":0},{"$f":"'Individual Spaces'!Q164","v":0},{"$f":"'Individual Spaces'!R164","v":0},null,0,{"$f":"IF(AF165=\"-\",0,ROUND((J165-VLOOKUP(B165,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B165,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B165,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B165,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J165-VLOOKUP(B165,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B165,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B165,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Space for lockers, and access to lockers, off circulation area"},{"$f":"VLOOKUP($B165,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing pupils personal belongings (coats, bags, books, PE equipment etc)."},{"$f":"VLOOKUP($B165,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B165,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B165,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B165,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B165,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A165","v":"STN00"},{"$f":"'Individual Spaces'!B165","v":"STN02"},{"$f":"'Individual Spaces'!C165","v":5114},{"$f":"'Individual Spaces'!D165","v":"Coats and bag store (lockers) 4"},{"$f":"'Individual Spaces'!E165","v":0},null,{"$f":"VLOOKUP($B166,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_19"},{"$f":"VLOOKUP($B166,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Coats and bags stores"},{"$f":"'Individual Spaces'!G165","v":"ICT and Business Studies"},{"$f":"'Individual Spaces'!H165","v":10},null,null,null,-10,null,null,{"$f":"'Individual Spaces'!O165","v":0},{"$f":"'Individual Spaces'!P165","v":0},{"$f":"'Individual Spaces'!Q165","v":0},{"$f":"'Individual Spaces'!R165","v":0},null,0,{"$f":"IF(AF166=\"-\",0,ROUND((J166-VLOOKUP(B166,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B166,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B166,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B166,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J166-VLOOKUP(B166,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B166,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B166,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Space for lockers, and access to lockers, off circulation area"},{"$f":"VLOOKUP($B166,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing pupils personal belongings (coats, bags, books, PE equipment etc)."},{"$f":"VLOOKUP($B166,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B166,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B166,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B166,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B166,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A166","v":"STN00"},{"$f":"'Individual Spaces'!B166","v":"STN02"},{"$f":"'Individual Spaces'!C166","v":5115},{"$f":"'Individual Spaces'!D166","v":"Coats and bag store (lockers) 5"},{"$f":"'Individual Spaces'!E166","v":0},null,{"$f":"VLOOKUP($B167,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_19"},{"$f":"VLOOKUP($B167,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Coats and bags stores"},{"$f":"'Individual Spaces'!G166","v":"Humanities"},{"$f":"'Individual Spaces'!H166","v":10},null,null,null,-10,null,null,{"$f":"'Individual Spaces'!O166","v":0},{"$f":"'Individual Spaces'!P166","v":0},{"$f":"'Individual Spaces'!Q166","v":0},{"$f":"'Individual Spaces'!R166","v":0},null,0,{"$f":"IF(AF167=\"-\",0,ROUND((J167-VLOOKUP(B167,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B167,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B167,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B167,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J167-VLOOKUP(B167,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B167,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B167,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Space for lockers, and access to lockers, off circulation area"},{"$f":"VLOOKUP($B167,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing pupils personal belongings (coats, bags, books, PE equipment etc)."},{"$f":"VLOOKUP($B167,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B167,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B167,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B167,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B167,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A167","v":"STN00"},{"$f":"'Individual Spaces'!B167","v":"STN02"},{"$f":"'Individual Spaces'!C167","v":5116},{"$f":"'Individual Spaces'!D167","v":"Coats and bag store (lockers) 6"},{"$f":"'Individual Spaces'!E167","v":0},null,{"$f":"VLOOKUP($B168,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_19"},{"$f":"VLOOKUP($B168,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Coats and bags stores"},{"$f":"'Individual Spaces'!G167","v":"Science"},{"$f":"'Individual Spaces'!H167","v":10},null,null,null,-10,null,null,{"$f":"'Individual Spaces'!O167","v":0},{"$f":"'Individual Spaces'!P167","v":0},{"$f":"'Individual Spaces'!Q167","v":0},{"$f":"'Individual Spaces'!R167","v":0},null,0,{"$f":"IF(AF168=\"-\",0,ROUND((J168-VLOOKUP(B168,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B168,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B168,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B168,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J168-VLOOKUP(B168,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B168,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B168,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Space for lockers, and access to lockers, off circulation area"},{"$f":"VLOOKUP($B168,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing pupils personal belongings (coats, bags, books, PE equipment etc)."},{"$f":"VLOOKUP($B168,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B168,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B168,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B168,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B168,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A168","v":"STN00"},{"$f":"'Individual Spaces'!B168","v":"STN03"},{"$f":"'Individual Spaces'!C168","v":5117},{"$f":"'Individual Spaces'!D168","v":"Coats and bag store (community lockers) 1"},{"$f":"'Individual Spaces'!E168","v":0},null,{"$f":"VLOOKUP($B169,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_19"},{"$f":"VLOOKUP($B169,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Coats and bags stores"},{"$f":"'Individual Spaces'!G168","v":"Sports/ PE"},{"$f":"'Individual Spaces'!H168","v":3},null,null,null,-3,null,null,{"$f":"'Individual Spaces'!O168","v":0},{"$f":"'Individual Spaces'!P168","v":0},{"$f":"'Individual Spaces'!Q168","v":0},{"$f":"'Individual Spaces'!R168","v":0},null,0,{"$f":"IF(AF169=\"-\",0,ROUND((J169-VLOOKUP(B169,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B169,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B169,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B169,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J169-VLOOKUP(B169,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B169,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B169,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Space for lockers, and access to lockers, off circulation areas, for community use outside school core hours"},{"$f":"VLOOKUP($B169,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing pupils personal belongings (coats, bags, books, PE equipment etc)."},{"$f":"VLOOKUP($B169,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B169,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B169,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B169,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B169,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Yes"}]
[{"$f":"'Individual Spaces'!A169","v":"STN31"},{"$f":"'Individual Spaces'!B169","v":"STN31"},{"$f":"'Individual Spaces'!C169","v":5118},{"$f":"'Individual Spaces'!D169","v":"Cleaners' store 1"},{"$f":"'Individual Spaces'!E169","v":0},null,{"$f":"VLOOKUP($B170,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_16"},{"$f":"VLOOKUP($B170,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Cleaners' stores"},{"$f":"'Individual Spaces'!G169","v":"Balance"},{"$f":"'Individual Spaces'!H169","v":1.5},null,null,null,-1.5,null,null,{"$f":"'Individual Spaces'!O169","v":0},{"$f":"'Individual Spaces'!P169","v":0},{"$f":"'Individual Spaces'!Q169","v":0},{"$f":"'Individual Spaces'!R169","v":0},null,0,{"$f":"IF(AF170=\"-\",0,ROUND((J170-VLOOKUP(B170,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B170,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B170,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B170,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J170-VLOOKUP(B170,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B170,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B170,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Cleaners' store with sink"},{"$f":"VLOOKUP($B170,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Filling and emptying buckets. Storing cleaning materials and equipment."},{"$f":"VLOOKUP($B170,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B170,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B170,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B170,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B170,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A170","v":"STN31"},{"$f":"'Individual Spaces'!B170","v":"STN31"},{"$f":"'Individual Spaces'!C170","v":5119},{"$f":"'Individual Spaces'!D170","v":"Cleaners' store 2"},{"$f":"'Individual Spaces'!E170","v":0},null,{"$f":"VLOOKUP($B171,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_16"},{"$f":"VLOOKUP($B171,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Cleaners' stores"},{"$f":"'Individual Spaces'!G170","v":"Balance"},{"$f":"'Individual Spaces'!H170","v":1.5},null,null,null,-1.5,null,null,{"$f":"'Individual Spaces'!O170","v":0},{"$f":"'Individual Spaces'!P170","v":0},{"$f":"'Individual Spaces'!Q170","v":0},{"$f":"'Individual Spaces'!R170","v":0},null,0,{"$f":"IF(AF171=\"-\",0,ROUND((J171-VLOOKUP(B171,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B171,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B171,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B171,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J171-VLOOKUP(B171,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B171,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B171,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Cleaners' store with sink"},{"$f":"VLOOKUP($B171,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Filling and emptying buckets. Storing cleaning materials and equipment."},{"$f":"VLOOKUP($B171,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B171,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B171,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B171,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B171,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A171","v":"STN31"},{"$f":"'Individual Spaces'!B171","v":"STN31"},{"$f":"'Individual Spaces'!C171","v":5120},{"$f":"'Individual Spaces'!D171","v":"Cleaners' store 3"},{"$f":"'Individual Spaces'!E171","v":0},null,{"$f":"VLOOKUP($B172,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_16"},{"$f":"VLOOKUP($B172,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Cleaners' stores"},{"$f":"'Individual Spaces'!G171","v":"Balance"},{"$f":"'Individual Spaces'!H171","v":1.5},null,null,null,-1.5,null,null,{"$f":"'Individual Spaces'!O171","v":0},{"$f":"'Individual Spaces'!P171","v":0},{"$f":"'Individual Spaces'!Q171","v":0},{"$f":"'Individual Spaces'!R171","v":0},null,0,{"$f":"IF(AF172=\"-\",0,ROUND((J172-VLOOKUP(B172,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B172,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B172,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B172,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J172-VLOOKUP(B172,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B172,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B172,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Cleaners' store with sink"},{"$f":"VLOOKUP($B172,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Filling and emptying buckets. Storing cleaning materials and equipment."},{"$f":"VLOOKUP($B172,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B172,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B172,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B172,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B172,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A172","v":"STN31"},{"$f":"'Individual Spaces'!B172","v":"STN31"},{"$f":"'Individual Spaces'!C172","v":5121},{"$f":"'Individual Spaces'!D172","v":"Cleaners' store 4"},{"$f":"'Individual Spaces'!E172","v":0},null,{"$f":"VLOOKUP($B173,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_16"},{"$f":"VLOOKUP($B173,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Cleaners' stores"},{"$f":"'Individual Spaces'!G172","v":"Balance"},{"$f":"'Individual Spaces'!H172","v":1.5},null,null,null,-1.5,null,null,{"$f":"'Individual Spaces'!O172","v":0},{"$f":"'Individual Spaces'!P172","v":0},{"$f":"'Individual Spaces'!Q172","v":0},{"$f":"'Individual Spaces'!R172","v":0},null,0,{"$f":"IF(AF173=\"-\",0,ROUND((J173-VLOOKUP(B173,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B173,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B173,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B173,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J173-VLOOKUP(B173,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B173,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B173,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Cleaners' store with sink"},{"$f":"VLOOKUP($B173,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Filling and emptying buckets. Storing cleaning materials and equipment."},{"$f":"VLOOKUP($B173,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B173,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B173,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B173,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B173,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A173","v":"STN31"},{"$f":"'Individual Spaces'!B173","v":"STN31"},{"$f":"'Individual Spaces'!C173","v":5122},{"$f":"'Individual Spaces'!D173","v":"Cleaners' store 5"},{"$f":"'Individual Spaces'!E173","v":0},null,{"$f":"VLOOKUP($B174,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_16"},{"$f":"VLOOKUP($B174,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Cleaners' stores"},{"$f":"'Individual Spaces'!G173","v":"Balance"},{"$f":"'Individual Spaces'!H173","v":1.5},null,null,null,-1.5,null,null,{"$f":"'Individual Spaces'!O173","v":0},{"$f":"'Individual Spaces'!P173","v":0},{"$f":"'Individual Spaces'!Q173","v":0},{"$f":"'Individual Spaces'!R173","v":0},null,0,{"$f":"IF(AF174=\"-\",0,ROUND((J174-VLOOKUP(B174,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B174,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B174,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B174,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J174-VLOOKUP(B174,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B174,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B174,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Cleaners' store with sink"},{"$f":"VLOOKUP($B174,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Filling and emptying buckets. Storing cleaning materials and equipment."},{"$f":"VLOOKUP($B174,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B174,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B174,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B174,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B174,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A174","v":"STN31"},{"$f":"'Individual Spaces'!B174","v":"STN31"},{"$f":"'Individual Spaces'!C174","v":5123},{"$f":"'Individual Spaces'!D174","v":"Cleaners' store 6"},{"$f":"'Individual Spaces'!E174","v":0},null,{"$f":"VLOOKUP($B175,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_16"},{"$f":"VLOOKUP($B175,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Cleaners' stores"},{"$f":"'Individual Spaces'!G174","v":"Balance"},{"$f":"'Individual Spaces'!H174","v":1.5},null,null,null,-1.5,null,null,{"$f":"'Individual Spaces'!O174","v":0},{"$f":"'Individual Spaces'!P174","v":0},{"$f":"'Individual Spaces'!Q174","v":0},{"$f":"'Individual Spaces'!R174","v":0},null,0,{"$f":"IF(AF175=\"-\",0,ROUND((J175-VLOOKUP(B175,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B175,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B175,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B175,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J175-VLOOKUP(B175,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B175,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B175,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Cleaners' store with sink"},{"$f":"VLOOKUP($B175,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Filling and emptying buckets. Storing cleaning materials and equipment."},{"$f":"VLOOKUP($B175,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B175,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B175,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B175,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B175,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A175","v":"STN31"},{"$f":"'Individual Spaces'!B175","v":"STN31"},{"$f":"'Individual Spaces'!C175","v":5124},{"$f":"'Individual Spaces'!D175","v":"Cleaners' store 7"},{"$f":"'Individual Spaces'!E175","v":0},null,{"$f":"VLOOKUP($B176,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_16"},{"$f":"VLOOKUP($B176,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Cleaners' stores"},{"$f":"'Individual Spaces'!G175","v":"Balance"},{"$f":"'Individual Spaces'!H175","v":1.5},null,null,null,-1.5,null,null,{"$f":"'Individual Spaces'!O175","v":0},{"$f":"'Individual Spaces'!P175","v":0},{"$f":"'Individual Spaces'!Q175","v":0},{"$f":"'Individual Spaces'!R175","v":0},null,0,{"$f":"IF(AF176=\"-\",0,ROUND((J176-VLOOKUP(B176,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B176,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B176,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B176,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J176-VLOOKUP(B176,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B176,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B176,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Cleaners' store with sink"},{"$f":"VLOOKUP($B176,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Filling and emptying buckets. Storing cleaning materials and equipment."},{"$f":"VLOOKUP($B176,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B176,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B176,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B176,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B176,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A176","v":"STN31"},{"$f":"'Individual Spaces'!B176","v":"STN31"},{"$f":"'Individual Spaces'!C176","v":5125},{"$f":"'Individual Spaces'!D176","v":"Cleaners' store 8"},{"$f":"'Individual Spaces'!E176","v":0},null,{"$f":"VLOOKUP($B177,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_16"},{"$f":"VLOOKUP($B177,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Cleaners' stores"},{"$f":"'Individual Spaces'!G176","v":"Balance"},{"$f":"'Individual Spaces'!H176","v":1.5},null,null,null,-1.5,null,null,{"$f":"'Individual Spaces'!O176","v":0},{"$f":"'Individual Spaces'!P176","v":0},{"$f":"'Individual Spaces'!Q176","v":0},{"$f":"'Individual Spaces'!R176","v":0},null,0,{"$f":"IF(AF177=\"-\",0,ROUND((J177-VLOOKUP(B177,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B177,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B177,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B177,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J177-VLOOKUP(B177,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B177,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B177,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Cleaners' store with sink"},{"$f":"VLOOKUP($B177,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Filling and emptying buckets. Storing cleaning materials and equipment."},{"$f":"VLOOKUP($B177,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B177,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B177,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B177,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B177,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A177","v":"STN32"},{"$f":"'Individual Spaces'!B177","v":"STN32"},{"$f":"'Individual Spaces'!C177","v":5126},{"$f":"'Individual Spaces'!D177","v":"Equipment store, maintenance 1"},{"$f":"'Individual Spaces'!E177","v":0},null,{"$f":"VLOOKUP($B178,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_27"},{"$f":"VLOOKUP($B178,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Equipment stores"},{"$f":"'Individual Spaces'!G177","v":"Balance"},{"$f":"'Individual Spaces'!H177","v":8},null,null,null,-8,null,null,{"$f":"'Individual Spaces'!O177","v":0},{"$f":"'Individual Spaces'!P177","v":0},{"$f":"'Individual Spaces'!Q177","v":0},{"$f":"'Individual Spaces'!R177","v":0},null,0,{"$f":"IF(AF178=\"-\",0,ROUND((J178-VLOOKUP(B178,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B178,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B178,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B178,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J178-VLOOKUP(B178,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B178,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B178,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"General storage of maintenance equipment and resources such as floor cleaners"},{"$f":"VLOOKUP($B178,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Filling and emptying buckets. Storing maintenance materials and equipment."},{"$f":"VLOOKUP($B178,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Storage (non-teaching)"},{"$f":"VLOOKUP($B178,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Storage"},{"$f":"VLOOKUP($B178,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B178,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B178,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A178","v":0},{"$f":"'Individual Spaces'!B178","v":0},{"$f":"'Individual Spaces'!C178","v":0},{"$f":"'Individual Spaces'!D178","v":0},{"$f":"'Individual Spaces'!E178","v":"Non Teaching Storage Total : "},null,{"$f":"VLOOKUP($B179,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B179,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G178","v":0},{"$f":"'Individual Spaces'!H178","v":153},null,null,null,-153,null,null,{"$f":"'Individual Spaces'!O178","v":0},{"$f":"'Individual Spaces'!P178","v":0},{"$f":"'Individual Spaces'!Q178","v":0},{"$f":"'Individual Spaces'!R178","v":0},null,0,{"$f":"IF(AF179=\"-\",0,ROUND((J179-VLOOKUP(B179,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B179,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B179,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B179,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J179-VLOOKUP(B179,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B179,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B179,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B179,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B179,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B179,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B179,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B179,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B179,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A179","v":"KIT00"},{"$f":"'Individual Spaces'!B179","v":"KIT01"},{"$f":"'Individual Spaces'!C179","v":6001},{"$f":"'Individual Spaces'!D179","v":"Food prep area, kitchen (servery & wash-up) 1"},{"$f":"'Individual Spaces'!E179","v":0},null,{"$f":"VLOOKUP($B180,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_60_30"},{"$f":"VLOOKUP($B180,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Food preparation areas"},{"$f":"'Individual Spaces'!G179","v":"Perf arts, hall and dining"},{"$f":"'Individual Spaces'!H179","v":97},null,null,null,-97,null,null,{"$f":"'Individual Spaces'!O179","v":0},{"$f":"'Individual Spaces'!P179","v":0},{"$f":"'Individual Spaces'!Q179","v":0},{"$f":"'Individual Spaces'!R179","v":0},null,0,{"$f":"IF(AF180=\"-\",0,ROUND((J180-VLOOKUP(B180,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B180,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":16},{"$f":"IF(VLOOKUP(B180,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B180,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J180-VLOOKUP(B180,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B180,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},18,null,null,{"$f":"VLOOKUP($B180,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Preparation, servery, wash-up and COSHH area of commercial kitchen for preparing and serving school meals"},{"$f":"VLOOKUP($B180,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Preparing, cooking and serving hot and cold meals for pupils and staff, as well as dishwashing and cleaning, by commercial catering staff. Also to include an area for administrative tasks (including use of ICT) by commercial catering staff."},{"$f":"VLOOKUP($B180,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B180,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B180,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"J"},{"$f":"VLOOKUP($B180,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B180,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A180","v":"KIT11"},{"$f":"'Individual Spaces'!B180","v":"KIT11"},{"$f":"'Individual Spaces'!C180","v":6002},{"$f":"'Individual Spaces'!D180","v":"Office, kitchen 1"},{"$f":"'Individual Spaces'!E180","v":0},null,{"$f":"VLOOKUP($B181,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_20_15_59"},{"$f":"VLOOKUP($B181,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Offices"},{"$f":"'Individual Spaces'!G180","v":"Perf arts, hall and dining"},{"$f":"'Individual Spaces'!H180","v":4},null,null,null,-4,null,null,{"$f":"'Individual Spaces'!O180","v":0},{"$f":"'Individual Spaces'!P180","v":0},{"$f":"'Individual Spaces'!Q180","v":0},{"$f":"'Individual Spaces'!R180","v":0},null,0,{"$f":"IF(AF181=\"-\",0,ROUND((J181-VLOOKUP(B181,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B181,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":2},{"$f":"IF(VLOOKUP(B181,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B181,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J181-VLOOKUP(B181,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B181,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":1},3,null,null,{"$f":"VLOOKUP($B181,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Chef's office or admin area within commercial kitchen for preparing and serving school meals"},{"$f":"VLOOKUP($B181,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Administrative tasks (including use of ICT) and filing by commercial catering staff."},{"$f":"VLOOKUP($B181,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B181,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B181,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"A"},{"$f":"VLOOKUP($B181,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B181,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A181","v":"KIT20"},{"$f":"'Individual Spaces'!B181","v":"KIT21"},{"$f":"'Individual Spaces'!C181","v":6003},{"$f":"'Individual Spaces'!D181","v":"Food store, kitchen (dry) 1"},{"$f":"'Individual Spaces'!E181","v":0},null,{"$f":"VLOOKUP($B182,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_29"},{"$f":"VLOOKUP($B182,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Food stores"},{"$f":"'Individual Spaces'!G181","v":"Perf arts, hall and dining"},{"$f":"'Individual Spaces'!H181","v":5},null,null,null,-5,null,null,{"$f":"'Individual Spaces'!O181","v":0},{"$f":"'Individual Spaces'!P181","v":0},{"$f":"'Individual Spaces'!Q181","v":0},{"$f":"'Individual Spaces'!R181","v":0},null,0,{"$f":"IF(AF182=\"-\",0,ROUND((J182-VLOOKUP(B182,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B182,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B182,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B182,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J182-VLOOKUP(B182,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B182,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B182,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Commercial kitchen dry store for use by school catering staff, as part of school kitchen suite"},{"$f":"VLOOKUP($B182,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing cold or dry foodstuffs for use by commercial catering staff, as part of school kitchen suite."},{"$f":"VLOOKUP($B182,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B182,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B182,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B182,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B182,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A182","v":"KIT25"},{"$f":"'Individual Spaces'!B182","v":"KIT25"},{"$f":"'Individual Spaces'!C182","v":6004},{"$f":"'Individual Spaces'!D182","v":"Cold store, kitchen 1"},{"$f":"'Individual Spaces'!E182","v":0},null,{"$f":"VLOOKUP($B183,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_15"},{"$f":"VLOOKUP($B183,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Cold stores"},{"$f":"'Individual Spaces'!G182","v":"Perf arts, hall and dining"},{"$f":"'Individual Spaces'!H182","v":4.5},null,null,null,-4.5,null,null,{"$f":"'Individual Spaces'!O182","v":0},{"$f":"'Individual Spaces'!P182","v":0},{"$f":"'Individual Spaces'!Q182","v":0},{"$f":"'Individual Spaces'!R182","v":0},null,0,{"$f":"IF(AF183=\"-\",0,ROUND((J183-VLOOKUP(B183,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B183,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B183,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B183,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J183-VLOOKUP(B183,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B183,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B183,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Commercial kitchen cold store for use by school catering staff, as part of school kitchen suite"},{"$f":"VLOOKUP($B183,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing refrigerated cold foodstuffs for use by commercial catering staff, as part of school kitchen suite."},{"$f":"VLOOKUP($B183,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B183,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B183,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B183,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B183,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A183","v":"KIT25"},{"$f":"'Individual Spaces'!B183","v":"KIT26"},{"$f":"'Individual Spaces'!C183","v":6005},{"$f":"'Individual Spaces'!D183","v":"Cold store, kitchen (freezer) 1"},{"$f":"'Individual Spaces'!E183","v":0},null,{"$f":"VLOOKUP($B184,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_50_15"},{"$f":"VLOOKUP($B184,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Cold stores"},{"$f":"'Individual Spaces'!G183","v":"Perf arts, hall and dining"},{"$f":"'Individual Spaces'!H183","v":3.5},null,null,null,-3.5,null,null,{"$f":"'Individual Spaces'!O183","v":0},{"$f":"'Individual Spaces'!P183","v":0},{"$f":"'Individual Spaces'!Q183","v":0},{"$f":"'Individual Spaces'!R183","v":0},null,0,{"$f":"IF(AF184=\"-\",0,ROUND((J184-VLOOKUP(B184,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B184,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B184,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B184,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J184-VLOOKUP(B184,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B184,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B184,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Commercial kitchen freezer store for use by school catering staff, as part of school kitchen suite"},{"$f":"VLOOKUP($B184,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Storing frozen foodstuffs for use by commercial catering staff, as part of school kitchen suite."},{"$f":"VLOOKUP($B184,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B184,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B184,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B184,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B184,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A184","v":"KIT40"},{"$f":"'Individual Spaces'!B184","v":"KIT40"},{"$f":"'Individual Spaces'!C184","v":6006},{"$f":"'Individual Spaces'!D184","v":"Toilet, kitchen (with changing area) 1"},{"$f":"'Individual Spaces'!E184","v":0},null,{"$f":"VLOOKUP($B185,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_89"},{"$f":"VLOOKUP($B185,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Toilets"},{"$f":"'Individual Spaces'!G184","v":"Perf arts, hall and dining"},{"$f":"'Individual Spaces'!H184","v":6.5},null,null,null,-6.5,null,null,{"$f":"'Individual Spaces'!O184","v":0},{"$f":"'Individual Spaces'!P184","v":0},{"$f":"'Individual Spaces'!Q184","v":0},{"$f":"'Individual Spaces'!R184","v":0},null,0,{"$f":"IF(AF185=\"-\",0,ROUND((J185-VLOOKUP(B185,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B185,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":2},{"$f":"IF(VLOOKUP(B185,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B185,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J185-VLOOKUP(B185,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B185,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},3,null,null,{"$f":"VLOOKUP($B185,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Toilet(s) for use by school catering staff, accessed from space for kitchen staff lockers and changing "},{"$f":"VLOOKUP($B185,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Toilet(s), wash hand basin and changing area for commercial catering staff, as part of school kitchen suite. Storage of personal belongings and clothing."},{"$f":"VLOOKUP($B185,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B185,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B185,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"T"},{"$f":"VLOOKUP($B185,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B185,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A185","v":"TOC01"},{"$f":"'Individual Spaces'!B185","v":"TOC01"},{"$f":"'Individual Spaces'!C185","v":6007},{"$f":"'Individual Spaces'!D185","v":"Changing room, with showers (pupils) 1"},{"$f":"'Individual Spaces'!E185","v":0},null,{"$f":"VLOOKUP($B186,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_20_13"},{"$f":"VLOOKUP($B186,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Changing rooms"},{"$f":"'Individual Spaces'!G185","v":"Sports/ PE"},{"$f":"'Individual Spaces'!H185","v":64},null,null,null,-64,null,null,{"$f":"'Individual Spaces'!O185","v":0},{"$f":"'Individual Spaces'!P185","v":0},{"$f":"'Individual Spaces'!Q185","v":0},{"$f":"'Individual Spaces'!R185","v":0},null,0,{"$f":"IF(AF186=\"-\",0,ROUND((J186-VLOOKUP(B186,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B186,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":56},{"$f":"IF(VLOOKUP(B186,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B186,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J186-VLOOKUP(B186,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B186,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},62,null,null,{"$f":"VLOOKUP($B186,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Wet changing and shower cubicles for male or female pupils"},{"$f":"VLOOKUP($B186,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Changing and showering for PE."},{"$f":"VLOOKUP($B186,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B186,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B186,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"A"},{"$f":"VLOOKUP($B186,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B186,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Yes"}]
[{"$f":"'Individual Spaces'!A186","v":"TOC01"},{"$f":"'Individual Spaces'!B186","v":"TOC01"},{"$f":"'Individual Spaces'!C186","v":6008},{"$f":"'Individual Spaces'!D186","v":"Changing room, with showers (pupils) 2"},{"$f":"'Individual Spaces'!E186","v":0},null,{"$f":"VLOOKUP($B187,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_20_13"},{"$f":"VLOOKUP($B187,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Changing rooms"},{"$f":"'Individual Spaces'!G186","v":"Sports/ PE"},{"$f":"'Individual Spaces'!H186","v":64},null,null,null,-64,null,null,{"$f":"'Individual Spaces'!O186","v":0},{"$f":"'Individual Spaces'!P186","v":0},{"$f":"'Individual Spaces'!Q186","v":0},{"$f":"'Individual Spaces'!R186","v":0},null,0,{"$f":"IF(AF187=\"-\",0,ROUND((J187-VLOOKUP(B187,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B187,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":56},{"$f":"IF(VLOOKUP(B187,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B187,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J187-VLOOKUP(B187,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B187,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},62,null,null,{"$f":"VLOOKUP($B187,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Wet changing and shower cubicles for male or female pupils"},{"$f":"VLOOKUP($B187,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Changing and showering for PE."},{"$f":"VLOOKUP($B187,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B187,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B187,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"A"},{"$f":"VLOOKUP($B187,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B187,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Yes"}]
[{"$f":"'Individual Spaces'!A187","v":"TOC02"},{"$f":"'Individual Spaces'!B187","v":"TOC02"},{"$f":"'Individual Spaces'!C187","v":6009},{"$f":"'Individual Spaces'!D187","v":"Accessible (and staff) changing room 1"},{"$f":"'Individual Spaces'!E187","v":0},null,{"$f":"VLOOKUP($B188,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_01"},{"$f":"VLOOKUP($B188,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Accessible changing rooms"},{"$f":"'Individual Spaces'!G187","v":"Sports/ PE"},{"$f":"'Individual Spaces'!H187","v":6},null,null,null,-6,null,null,{"$f":"'Individual Spaces'!O187","v":0},{"$f":"'Individual Spaces'!P187","v":0},{"$f":"'Individual Spaces'!Q187","v":0},{"$f":"'Individual Spaces'!R187","v":0},null,0,{"$f":"IF(AF188=\"-\",0,ROUND((J188-VLOOKUP(B188,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B188,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B188,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B188,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J188-VLOOKUP(B188,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B188,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B188,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Wet changing and shower cubicle for male or female staff, or for disabled or community users"},{"$f":"VLOOKUP($B188,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Changing and showering for staff member or disabled pupil or visitor, for PE."},{"$f":"VLOOKUP($B188,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B188,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B188,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B188,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B188,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Yes"}]
[{"$f":"'Individual Spaces'!A188","v":"TOC02"},{"$f":"'Individual Spaces'!B188","v":"TOC02"},{"$f":"'Individual Spaces'!C188","v":6010},{"$f":"'Individual Spaces'!D188","v":"Accessible (and staff) changing room 2"},{"$f":"'Individual Spaces'!E188","v":0},null,{"$f":"VLOOKUP($B189,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_01"},{"$f":"VLOOKUP($B189,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Accessible changing rooms"},{"$f":"'Individual Spaces'!G188","v":"Sports/ PE"},{"$f":"'Individual Spaces'!H188","v":6},null,null,null,-6,null,null,{"$f":"'Individual Spaces'!O188","v":0},{"$f":"'Individual Spaces'!P188","v":0},{"$f":"'Individual Spaces'!Q188","v":0},{"$f":"'Individual Spaces'!R188","v":0},null,0,{"$f":"IF(AF189=\"-\",0,ROUND((J189-VLOOKUP(B189,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B189,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B189,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B189,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J189-VLOOKUP(B189,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B189,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B189,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Wet changing and shower cubicle for male or female staff, or for disabled or community users"},{"$f":"VLOOKUP($B189,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Changing and showering for staff member or disabled pupil or visitor, for PE."},{"$f":"VLOOKUP($B189,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B189,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B189,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B189,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B189,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Yes"}]
[{"$f":"'Individual Spaces'!A189","v":"TOC04"},{"$f":"'Individual Spaces'!B189","v":"TOC04"},{"$f":"'Individual Spaces'!C189","v":6011},{"$f":"'Individual Spaces'!D189","v":"Hygiene room 1"},{"$f":"'Individual Spaces'!E189","v":0},null,{"$f":"VLOOKUP($B190,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_39"},{"$f":"VLOOKUP($B190,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Hygiene rooms"},{"$f":"'Individual Spaces'!G189","v":"Balance"},{"$f":"'Individual Spaces'!H189","v":12},null,null,null,-12,null,null,{"$f":"'Individual Spaces'!O189","v":0},{"$f":"'Individual Spaces'!P189","v":0},{"$f":"'Individual Spaces'!Q189","v":0},{"$f":"'Individual Spaces'!R189","v":0},null,0,{"$f":"IF(AF190=\"-\",0,ROUND((J190-VLOOKUP(B190,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B190,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B190,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B190,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J190-VLOOKUP(B190,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B190,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B190,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Hygiene room for disabled pupils' wash-down, showering and toileting using a ceiling-mounted hoist, with wc, wash-hand basin, shower and a shower-bed"},{"$f":"VLOOKUP($B190,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Assisted shower. Peninsular WC able to be accessed from either side. Room for changing pupils, with bed against wall."},{"$f":"VLOOKUP($B190,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B190,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B190,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B190,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B190,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A190","v":"TOC10"},{"$f":"'Individual Spaces'!B190","v":"TOC13"},{"$f":"'Individual Spaces'!C190","v":6012},{"$f":"'Individual Spaces'!D190","v":"Toilets, suite (pupils) 1"},{"$f":"'Individual Spaces'!E190","v":0},null,{"$f":"VLOOKUP($B191,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_89"},{"$f":"VLOOKUP($B191,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Toilets"},{"$f":"'Individual Spaces'!G190","v":"Balance"},{"$f":"'Individual Spaces'!H190","v":26},null,null,null,-26,null,null,{"$f":"'Individual Spaces'!O190","v":0},{"$f":"'Individual Spaces'!P190","v":0},{"$f":"'Individual Spaces'!Q190","v":0},{"$f":"'Individual Spaces'!R190","v":0},null,0,{"$f":"IF(AF191=\"-\",0,ROUND((J191-VLOOKUP(B191,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B191,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B191,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B191,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J191-VLOOKUP(B191,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B191,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B191,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Pupils' toilet cubicles and hand-wash/ dry area"},{"$f":"VLOOKUP($B191,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Suite of toilet cubicles and hand-wash/ dry area, for mainstream pupils"},{"$f":"VLOOKUP($B191,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B191,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B191,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B191,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B191,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A191","v":"TOC10"},{"$f":"'Individual Spaces'!B191","v":"TOC13"},{"$f":"'Individual Spaces'!C191","v":6013},{"$f":"'Individual Spaces'!D191","v":"Toilets, suite (pupils) 2"},{"$f":"'Individual Spaces'!E191","v":0},null,{"$f":"VLOOKUP($B192,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_89"},{"$f":"VLOOKUP($B192,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Toilets"},{"$f":"'Individual Spaces'!G191","v":"Balance"},{"$f":"'Individual Spaces'!H191","v":26},null,null,null,-26,null,null,{"$f":"'Individual Spaces'!O191","v":0},{"$f":"'Individual Spaces'!P191","v":0},{"$f":"'Individual Spaces'!Q191","v":0},{"$f":"'Individual Spaces'!R191","v":0},null,0,{"$f":"IF(AF192=\"-\",0,ROUND((J192-VLOOKUP(B192,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B192,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B192,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B192,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J192-VLOOKUP(B192,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B192,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B192,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Pupils' toilet cubicles and hand-wash/ dry area"},{"$f":"VLOOKUP($B192,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Suite of toilet cubicles and hand-wash/ dry area, for mainstream pupils"},{"$f":"VLOOKUP($B192,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B192,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B192,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B192,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B192,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A192","v":"TOC10"},{"$f":"'Individual Spaces'!B192","v":"TOC13"},{"$f":"'Individual Spaces'!C192","v":6014},{"$f":"'Individual Spaces'!D192","v":"Toilets, suite (pupils) 3"},{"$f":"'Individual Spaces'!E192","v":0},null,{"$f":"VLOOKUP($B193,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_89"},{"$f":"VLOOKUP($B193,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Toilets"},{"$f":"'Individual Spaces'!G192","v":"Balance"},{"$f":"'Individual Spaces'!H192","v":26},null,null,null,-26,null,null,{"$f":"'Individual Spaces'!O192","v":0},{"$f":"'Individual Spaces'!P192","v":0},{"$f":"'Individual Spaces'!Q192","v":0},{"$f":"'Individual Spaces'!R192","v":0},null,0,{"$f":"IF(AF193=\"-\",0,ROUND((J193-VLOOKUP(B193,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B193,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B193,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B193,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J193-VLOOKUP(B193,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B193,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B193,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Pupils' toilet cubicles and hand-wash/ dry area"},{"$f":"VLOOKUP($B193,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Suite of toilet cubicles and hand-wash/ dry area, for mainstream pupils"},{"$f":"VLOOKUP($B193,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B193,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B193,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B193,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B193,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A193","v":"TOC10"},{"$f":"'Individual Spaces'!B193","v":"TOC13"},{"$f":"'Individual Spaces'!C193","v":6015},{"$f":"'Individual Spaces'!D193","v":"Toilets, suite (pupils) 4"},{"$f":"'Individual Spaces'!E193","v":0},null,{"$f":"VLOOKUP($B194,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_89"},{"$f":"VLOOKUP($B194,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Toilets"},{"$f":"'Individual Spaces'!G193","v":"Balance"},{"$f":"'Individual Spaces'!H193","v":26},null,null,null,-26,null,null,{"$f":"'Individual Spaces'!O193","v":0},{"$f":"'Individual Spaces'!P193","v":0},{"$f":"'Individual Spaces'!Q193","v":0},{"$f":"'Individual Spaces'!R193","v":0},null,0,{"$f":"IF(AF194=\"-\",0,ROUND((J194-VLOOKUP(B194,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B194,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B194,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B194,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J194-VLOOKUP(B194,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B194,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B194,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Pupils' toilet cubicles and hand-wash/ dry area"},{"$f":"VLOOKUP($B194,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Suite of toilet cubicles and hand-wash/ dry area, for mainstream pupils"},{"$f":"VLOOKUP($B194,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B194,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B194,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B194,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B194,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A194","v":"TOC10"},{"$f":"'Individual Spaces'!B194","v":"TOC13"},{"$f":"'Individual Spaces'!C194","v":6016},{"$f":"'Individual Spaces'!D194","v":"Toilets, suite (pupils) 5"},{"$f":"'Individual Spaces'!E194","v":0},null,{"$f":"VLOOKUP($B195,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_89"},{"$f":"VLOOKUP($B195,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Toilets"},{"$f":"'Individual Spaces'!G194","v":"Balance"},{"$f":"'Individual Spaces'!H194","v":26},null,null,null,-26,null,null,{"$f":"'Individual Spaces'!O194","v":0},{"$f":"'Individual Spaces'!P194","v":0},{"$f":"'Individual Spaces'!Q194","v":0},{"$f":"'Individual Spaces'!R194","v":0},null,0,{"$f":"IF(AF195=\"-\",0,ROUND((J195-VLOOKUP(B195,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B195,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B195,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B195,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J195-VLOOKUP(B195,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B195,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B195,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Pupils' toilet cubicles and hand-wash/ dry area"},{"$f":"VLOOKUP($B195,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Suite of toilet cubicles and hand-wash/ dry area, for mainstream pupils"},{"$f":"VLOOKUP($B195,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B195,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B195,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B195,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B195,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A195","v":"TOC10"},{"$f":"'Individual Spaces'!B195","v":"TOC13"},{"$f":"'Individual Spaces'!C195","v":6017},{"$f":"'Individual Spaces'!D195","v":"Toilets, suite (pupils) 6"},{"$f":"'Individual Spaces'!E195","v":0},null,{"$f":"VLOOKUP($B196,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_89"},{"$f":"VLOOKUP($B196,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Toilets"},{"$f":"'Individual Spaces'!G195","v":"Balance"},{"$f":"'Individual Spaces'!H195","v":26},null,null,null,-26,null,null,{"$f":"'Individual Spaces'!O195","v":0},{"$f":"'Individual Spaces'!P195","v":0},{"$f":"'Individual Spaces'!Q195","v":0},{"$f":"'Individual Spaces'!R195","v":0},null,0,{"$f":"IF(AF196=\"-\",0,ROUND((J196-VLOOKUP(B196,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B196,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B196,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B196,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J196-VLOOKUP(B196,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B196,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B196,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Pupils' toilet cubicles and hand-wash/ dry area"},{"$f":"VLOOKUP($B196,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Suite of toilet cubicles and hand-wash/ dry area, for mainstream pupils"},{"$f":"VLOOKUP($B196,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B196,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B196,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B196,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B196,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A196","v":"TOC10"},{"$f":"'Individual Spaces'!B196","v":"TOC14"},{"$f":"'Individual Spaces'!C196","v":6018},{"$f":"'Individual Spaces'!D196","v":"Toilets, suite (pupils, other) 1"},{"$f":"'Individual Spaces'!E196","v":0},null,{"$f":"VLOOKUP($B197,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_89"},{"$f":"VLOOKUP($B197,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Toilets"},{"$f":"'Individual Spaces'!G196","v":"Sports/ PE"},{"$f":"'Individual Spaces'!H196","v":6},null,null,null,-6,null,null,{"$f":"'Individual Spaces'!O196","v":0},{"$f":"'Individual Spaces'!P196","v":0},{"$f":"'Individual Spaces'!Q196","v":0},{"$f":"'Individual Spaces'!R196","v":0},null,0,{"$f":"IF(AF197=\"-\",0,ROUND((J197-VLOOKUP(B197,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B197,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B197,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B197,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J197-VLOOKUP(B197,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B197,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B197,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Pupils' toilet cubicles and hand-wash/ dry area"},{"$f":"VLOOKUP($B197,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Suite of toilet cubicles and hand-wash/ dry area, for mainstream pupils"},{"$f":"VLOOKUP($B197,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B197,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B197,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B197,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B197,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A197","v":"TOC10"},{"$f":"'Individual Spaces'!B197","v":"TOC14"},{"$f":"'Individual Spaces'!C197","v":6019},{"$f":"'Individual Spaces'!D197","v":"Toilets, suite (pupils, other) 2"},{"$f":"'Individual Spaces'!E197","v":0},null,{"$f":"VLOOKUP($B198,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_89"},{"$f":"VLOOKUP($B198,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Toilets"},{"$f":"'Individual Spaces'!G197","v":"Sports/ PE"},{"$f":"'Individual Spaces'!H197","v":6},null,null,null,{"$f":"M198-J198","v":-6},null,null,{"$f":"'Individual Spaces'!O197","v":0},{"$f":"'Individual Spaces'!P197","v":0},{"$f":"'Individual Spaces'!Q197","v":0},{"$f":"'Individual Spaces'!R197","v":0},null,{"$f":"Q198","v":0},{"$f":"IF(AF198=\"-\",0,ROUND((J198-VLOOKUP(B198,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B198,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B198,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B198,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J198-VLOOKUP(B198,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B198,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},{"$f":"IF(W198>200,ROUND(W198*1.05,0),ROUNDUP(W198*1.1,0))","v":0},null,null,{"$f":"VLOOKUP($B198,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Pupils' toilet cubicles and hand-wash/ dry area"},{"$f":"VLOOKUP($B198,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Suite of toilet cubicles and hand-wash/ dry area, for mainstream pupils"},{"$f":"VLOOKUP($B198,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B198,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B198,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B198,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B198,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A198","v":"TOC10"},{"$f":"'Individual Spaces'!B198","v":"TOC14"},{"$f":"'Individual Spaces'!C198","v":6020},{"$f":"'Individual Spaces'!D198","v":"Toilets, suite (pupils, other) 3"},{"$f":"'Individual Spaces'!E198","v":0},null,{"$f":"VLOOKUP($B199,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_89"},{"$f":"VLOOKUP($B199,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Toilets"},{"$f":"'Individual Spaces'!G198","v":"Balance"},{"$f":"'Individual Spaces'!H198","v":6},null,null,null,-6,null,null,{"$f":"'Individual Spaces'!O198","v":0},{"$f":"'Individual Spaces'!P198","v":0},{"$f":"'Individual Spaces'!Q198","v":0},{"$f":"'Individual Spaces'!R198","v":0},null,0,{"$f":"IF(AF199=\"-\",0,ROUND((J199-VLOOKUP(B199,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B199,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B199,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B199,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J199-VLOOKUP(B199,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B199,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B199,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Pupils' toilet cubicles and hand-wash/ dry area"},{"$f":"VLOOKUP($B199,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Suite of toilet cubicles and hand-wash/ dry area, for mainstream pupils"},{"$f":"VLOOKUP($B199,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B199,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B199,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B199,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B199,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A199","v":"TOC15"},{"$f":"'Individual Spaces'!B199","v":"TOC15"},{"$f":"'Individual Spaces'!C199","v":6021},{"$f":"'Individual Spaces'!D199","v":"Toilet, individual (pupil) 1"},{"$f":"'Individual Spaces'!E199","v":0},null,{"$f":"VLOOKUP($B200,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_89"},{"$f":"VLOOKUP($B200,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Toilets"},{"$f":"'Individual Spaces'!G199","v":"Balance"},{"$f":"'Individual Spaces'!H199","v":2},null,null,null,-2,null,null,{"$f":"'Individual Spaces'!O199","v":0},{"$f":"'Individual Spaces'!P199","v":0},{"$f":"'Individual Spaces'!Q199","v":0},{"$f":"'Individual Spaces'!R199","v":0},null,0,{"$f":"IF(AF200=\"-\",0,ROUND((J200-VLOOKUP(B200,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B200,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B200,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B200,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J200-VLOOKUP(B200,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B200,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B200,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Individual pupils toilet, sink and hand-wash/ dry in one space"},{"$f":"VLOOKUP($B200,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Toilet and wash hand basin for mainstream pupils"},{"$f":"VLOOKUP($B200,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B200,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B200,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B200,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B200,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A200","v":"TOC15"},{"$f":"'Individual Spaces'!B200","v":"TOC15"},{"$f":"'Individual Spaces'!C200","v":6022},{"$f":"'Individual Spaces'!D200","v":"Toilet, individual (pupil) 2"},{"$f":"'Individual Spaces'!E200","v":0},null,{"$f":"VLOOKUP($B201,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_89"},{"$f":"VLOOKUP($B201,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Toilets"},{"$f":"'Individual Spaces'!G200","v":"Balance"},{"$f":"'Individual Spaces'!H200","v":2},null,null,null,-2,null,null,{"$f":"'Individual Spaces'!O200","v":0},{"$f":"'Individual Spaces'!P200","v":0},{"$f":"'Individual Spaces'!Q200","v":0},{"$f":"'Individual Spaces'!R200","v":0},null,0,{"$f":"IF(AF201=\"-\",0,ROUND((J201-VLOOKUP(B201,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B201,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B201,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B201,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J201-VLOOKUP(B201,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B201,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B201,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Individual pupils toilet, sink and hand-wash/ dry in one space"},{"$f":"VLOOKUP($B201,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Toilet and wash hand basin for mainstream pupils"},{"$f":"VLOOKUP($B201,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B201,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B201,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B201,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B201,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A201","v":"TOC15"},{"$f":"'Individual Spaces'!B201","v":"TOC15"},{"$f":"'Individual Spaces'!C201","v":6023},{"$f":"'Individual Spaces'!D201","v":"Toilet, individual (pupil) 3"},{"$f":"'Individual Spaces'!E201","v":0},null,{"$f":"VLOOKUP($B202,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_89"},{"$f":"VLOOKUP($B202,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Toilets"},{"$f":"'Individual Spaces'!G201","v":"Balance"},{"$f":"'Individual Spaces'!H201","v":2},null,null,null,-2,null,null,{"$f":"'Individual Spaces'!O201","v":0},{"$f":"'Individual Spaces'!P201","v":0},{"$f":"'Individual Spaces'!Q201","v":0},{"$f":"'Individual Spaces'!R201","v":0},null,0,{"$f":"IF(AF202=\"-\",0,ROUND((J202-VLOOKUP(B202,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B202,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B202,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B202,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J202-VLOOKUP(B202,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B202,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B202,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Individual pupils toilet, sink and hand-wash/ dry in one space"},{"$f":"VLOOKUP($B202,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Toilet and wash hand basin for mainstream pupils"},{"$f":"VLOOKUP($B202,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B202,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B202,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B202,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B202,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A202","v":"TOC10"},{"$f":"'Individual Spaces'!B202","v":"TOC12"},{"$f":"'Individual Spaces'!C202","v":6024},{"$f":"'Individual Spaces'!D202","v":"Toilets, suite (staff) 1"},{"$f":"'Individual Spaces'!E202","v":0},null,{"$f":"VLOOKUP($B203,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_89"},{"$f":"VLOOKUP($B203,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Toilets"},{"$f":"'Individual Spaces'!G202","v":"Admin"},{"$f":"'Individual Spaces'!H202","v":6},null,null,null,-6,null,null,{"$f":"'Individual Spaces'!O202","v":0},{"$f":"'Individual Spaces'!P202","v":0},{"$f":"'Individual Spaces'!Q202","v":0},{"$f":"'Individual Spaces'!R202","v":0},null,0,{"$f":"IF(AF203=\"-\",0,ROUND((J203-VLOOKUP(B203,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B203,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B203,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B203,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J203-VLOOKUP(B203,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B203,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B203,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Staff toilet cubicles and hand-wash/ dry area"},{"$f":"VLOOKUP($B203,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Suite of toilet cubicles and hand-wash/ dry area, for staff"},{"$f":"VLOOKUP($B203,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B203,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B203,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B203,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B203,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A203","v":"TOC10"},{"$f":"'Individual Spaces'!B203","v":"TOC12"},{"$f":"'Individual Spaces'!C203","v":6025},{"$f":"'Individual Spaces'!D203","v":"Toilets, suite (staff) 2"},{"$f":"'Individual Spaces'!E203","v":0},null,{"$f":"VLOOKUP($B204,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_89"},{"$f":"VLOOKUP($B204,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Toilets"},{"$f":"'Individual Spaces'!G203","v":"Admin"},{"$f":"'Individual Spaces'!H203","v":6},null,null,null,-6,null,null,{"$f":"'Individual Spaces'!O203","v":0},{"$f":"'Individual Spaces'!P203","v":0},{"$f":"'Individual Spaces'!Q203","v":0},{"$f":"'Individual Spaces'!R203","v":0},null,0,{"$f":"IF(AF204=\"-\",0,ROUND((J204-VLOOKUP(B204,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B204,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B204,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B204,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J204-VLOOKUP(B204,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B204,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B204,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Staff toilet cubicles and hand-wash/ dry area"},{"$f":"VLOOKUP($B204,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Suite of toilet cubicles and hand-wash/ dry area, for staff"},{"$f":"VLOOKUP($B204,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B204,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B204,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B204,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B204,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A204","v":"TOC21"},{"$f":"'Individual Spaces'!B204","v":"TOC21"},{"$f":"'Individual Spaces'!C204","v":6026},{"$f":"'Individual Spaces'!D204","v":"Accessible (and staff) toilet 1"},{"$f":"'Individual Spaces'!E204","v":0},null,{"$f":"VLOOKUP($B205,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_03"},{"$f":"VLOOKUP($B205,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Accessible toilets"},{"$f":"'Individual Spaces'!G204","v":"Balance"},{"$f":"'Individual Spaces'!H204","v":3.8},null,null,null,-3.8,null,null,{"$f":"'Individual Spaces'!O204","v":0},{"$f":"'Individual Spaces'!P204","v":0},{"$f":"'Individual Spaces'!Q204","v":0},{"$f":"'Individual Spaces'!R204","v":0},null,0,{"$f":"IF(AF205=\"-\",0,ROUND((J205-VLOOKUP(B205,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B205,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B205,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B205,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J205-VLOOKUP(B205,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B205,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B205,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Accessible toilets suitable for disabled pupils as well as any staff or visitors"},{"$f":"VLOOKUP($B205,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Unisex toilet and wash hand basin for non-ambulant pupils/adults, or ambulant staff or visitors."},{"$f":"VLOOKUP($B205,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B205,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B205,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B205,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B205,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Optional"}]
[{"$f":"'Individual Spaces'!A205","v":"TOC21"},{"$f":"'Individual Spaces'!B205","v":"TOC21"},{"$f":"'Individual Spaces'!C205","v":6027},{"$f":"'Individual Spaces'!D205","v":"Accessible (and staff) toilet 2"},{"$f":"'Individual Spaces'!E205","v":0},null,{"$f":"VLOOKUP($B206,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_03"},{"$f":"VLOOKUP($B206,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Accessible toilets"},{"$f":"'Individual Spaces'!G205","v":"Balance"},{"$f":"'Individual Spaces'!H205","v":3.8},null,null,null,-3.8,null,null,{"$f":"'Individual Spaces'!O205","v":0},{"$f":"'Individual Spaces'!P205","v":0},{"$f":"'Individual Spaces'!Q205","v":0},{"$f":"'Individual Spaces'!R205","v":0},null,0,{"$f":"IF(AF206=\"-\",0,ROUND((J206-VLOOKUP(B206,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B206,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B206,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B206,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J206-VLOOKUP(B206,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B206,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B206,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Accessible toilets suitable for disabled pupils as well as any staff or visitors"},{"$f":"VLOOKUP($B206,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Unisex toilet and wash hand basin for non-ambulant pupils/adults, or ambulant staff or visitors."},{"$f":"VLOOKUP($B206,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B206,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B206,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B206,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B206,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Optional"}]
[{"$f":"'Individual Spaces'!A206","v":"TOC21"},{"$f":"'Individual Spaces'!B206","v":"TOC21"},{"$f":"'Individual Spaces'!C206","v":6028},{"$f":"'Individual Spaces'!D206","v":"Accessible (and staff) toilet 3"},{"$f":"'Individual Spaces'!E206","v":0},null,{"$f":"VLOOKUP($B207,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_03"},{"$f":"VLOOKUP($B207,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Accessible toilets"},{"$f":"'Individual Spaces'!G206","v":"Balance"},{"$f":"'Individual Spaces'!H206","v":3.8},null,null,null,-3.8,null,null,{"$f":"'Individual Spaces'!O206","v":0},{"$f":"'Individual Spaces'!P206","v":0},{"$f":"'Individual Spaces'!Q206","v":0},{"$f":"'Individual Spaces'!R206","v":0},null,0,{"$f":"IF(AF207=\"-\",0,ROUND((J207-VLOOKUP(B207,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B207,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B207,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B207,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J207-VLOOKUP(B207,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B207,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B207,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Accessible toilets suitable for disabled pupils as well as any staff or visitors"},{"$f":"VLOOKUP($B207,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Unisex toilet and wash hand basin for non-ambulant pupils/adults, or ambulant staff or visitors."},{"$f":"VLOOKUP($B207,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B207,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B207,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B207,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B207,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Optional"}]
[{"$f":"'Individual Spaces'!A207","v":"TOC21"},{"$f":"'Individual Spaces'!B207","v":"TOC21"},{"$f":"'Individual Spaces'!C207","v":6029},{"$f":"'Individual Spaces'!D207","v":"Accessible (and staff) toilet 4"},{"$f":"'Individual Spaces'!E207","v":0},null,{"$f":"VLOOKUP($B208,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_03"},{"$f":"VLOOKUP($B208,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Accessible toilets"},{"$f":"'Individual Spaces'!G207","v":"Balance"},{"$f":"'Individual Spaces'!H207","v":3.8},null,null,null,-3.8,null,null,{"$f":"'Individual Spaces'!O207","v":0},{"$f":"'Individual Spaces'!P207","v":0},{"$f":"'Individual Spaces'!Q207","v":0},{"$f":"'Individual Spaces'!R207","v":0},null,0,{"$f":"IF(AF208=\"-\",0,ROUND((J208-VLOOKUP(B208,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B208,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B208,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B208,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J208-VLOOKUP(B208,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B208,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B208,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Accessible toilets suitable for disabled pupils as well as any staff or visitors"},{"$f":"VLOOKUP($B208,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Unisex toilet and wash hand basin for non-ambulant pupils/adults, or ambulant staff or visitors."},{"$f":"VLOOKUP($B208,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B208,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B208,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B208,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B208,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Optional"}]
[{"$f":"'Individual Spaces'!A208","v":"TOC21"},{"$f":"'Individual Spaces'!B208","v":"TOC21"},{"$f":"'Individual Spaces'!C208","v":6030},{"$f":"'Individual Spaces'!D208","v":"Accessible (and staff) toilet 5"},{"$f":"'Individual Spaces'!E208","v":0},null,{"$f":"VLOOKUP($B209,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_35_80_03"},{"$f":"VLOOKUP($B209,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Accessible toilets"},{"$f":"'Individual Spaces'!G208","v":"Balance"},{"$f":"'Individual Spaces'!H208","v":3.8},null,null,null,-3.8,null,null,{"$f":"'Individual Spaces'!O208","v":0},{"$f":"'Individual Spaces'!P208","v":0},{"$f":"'Individual Spaces'!Q208","v":0},{"$f":"'Individual Spaces'!R208","v":0},null,0,{"$f":"IF(AF209=\"-\",0,ROUND((J209-VLOOKUP(B209,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B209,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B209,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B209,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J209-VLOOKUP(B209,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B209,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B209,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Accessible toilets suitable for disabled pupils as well as any staff or visitors"},{"$f":"VLOOKUP($B209,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Unisex toilet and wash hand basin for non-ambulant pupils/adults, or ambulant staff or visitors."},{"$f":"VLOOKUP($B209,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B209,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B209,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B209,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B209,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"Optional"}]
[{"$f":"'Individual Spaces'!A209","v":"PLA10"},{"$f":"'Individual Spaces'!B209","v":"PLA14"},{"$f":"'Individual Spaces'!C209","v":6031},{"$f":"'Individual Spaces'!D209","v":"Server room (4-cabinet) 1"},{"$f":"'Individual Spaces'!E209","v":0},null,{"$f":"VLOOKUP($B210,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_77"},{"$f":"VLOOKUP($B210,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Server rooms"},{"$f":"'Individual Spaces'!G209","v":"Balance"},{"$f":"'Individual Spaces'!H209","v":15.6},null,null,null,-15.6,null,null,{"$f":"'Individual Spaces'!O209","v":0},{"$f":"'Individual Spaces'!P209","v":0},{"$f":"'Individual Spaces'!Q209","v":0},{"$f":"'Individual Spaces'!R209","v":0},null,0,{"$f":"IF(AF210=\"-\",0,ROUND((J210-VLOOKUP(B210,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B210,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B210,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B210,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J210-VLOOKUP(B210,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B210,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B210,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Specialist space for ICT servers "},{"$f":"VLOOKUP($B210,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Server racks and switching with space for access and maintenance"},{"$f":"VLOOKUP($B210,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B210,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B210,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B210,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B210,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A210","v":"PLA20"},{"$f":"'Individual Spaces'!B210","v":"PLA21"},{"$f":"'Individual Spaces'!C210","v":6032},{"$f":"'Individual Spaces'!D210","v":"Plant room (heat source) 1"},{"$f":"'Individual Spaces'!E210","v":0},null,{"$f":"VLOOKUP($B211,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_64"},{"$f":"VLOOKUP($B211,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Plant rooms"},{"$f":"'Individual Spaces'!G210","v":"Balance"},{"$f":"'Individual Spaces'!H210","v":32},null,null,null,-32,null,null,{"$f":"'Individual Spaces'!O210","v":0},{"$f":"'Individual Spaces'!P210","v":0},{"$f":"'Individual Spaces'!Q210","v":0},{"$f":"'Individual Spaces'!R210","v":0},null,0,{"$f":"IF(AF211=\"-\",0,ROUND((J211-VLOOKUP(B211,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B211,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B211,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B211,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J211-VLOOKUP(B211,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B211,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B211,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Internal room for heating source plant, including boilers"},{"$f":"VLOOKUP($B211,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Mechanical or electrical plant facilities"},{"$f":"VLOOKUP($B211,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B211,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B211,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B211,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B211,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A211","v":"PLA20"},{"$f":"'Individual Spaces'!B211","v":"PLA23"},{"$f":"'Individual Spaces'!C211","v":6033},{"$f":"'Individual Spaces'!D211","v":"Plant room (cold water tanks) 1"},{"$f":"'Individual Spaces'!E211","v":0},null,{"$f":"VLOOKUP($B212,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_64"},{"$f":"VLOOKUP($B212,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Plant rooms"},{"$f":"'Individual Spaces'!G211","v":"Balance"},{"$f":"'Individual Spaces'!H211","v":28},null,null,null,-28,null,null,{"$f":"'Individual Spaces'!O211","v":0},{"$f":"'Individual Spaces'!P211","v":0},{"$f":"'Individual Spaces'!Q211","v":0},{"$f":"'Individual Spaces'!R211","v":0},null,0,{"$f":"IF(AF212=\"-\",0,ROUND((J212-VLOOKUP(B212,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B212,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B212,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B212,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J212-VLOOKUP(B212,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B212,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B212,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Internal room for plant, including tanks"},{"$f":"VLOOKUP($B212,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Mechanical or electrical plant facilities"},{"$f":"VLOOKUP($B212,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B212,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B212,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B212,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B212,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A212","v":"PLA20"},{"$f":"'Individual Spaces'!B212","v":"PLA25"},{"$f":"'Individual Spaces'!C212","v":6034},{"$f":"'Individual Spaces'!D212","v":"Plant room (electrical intake) 1"},{"$f":"'Individual Spaces'!E212","v":0},null,{"$f":"VLOOKUP($B213,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_64"},{"$f":"VLOOKUP($B213,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Plant rooms"},{"$f":"'Individual Spaces'!G212","v":"Balance"},{"$f":"'Individual Spaces'!H212","v":28},null,null,null,-28,null,null,{"$f":"'Individual Spaces'!O212","v":0},{"$f":"'Individual Spaces'!P212","v":0},{"$f":"'Individual Spaces'!Q212","v":0},{"$f":"'Individual Spaces'!R212","v":0},null,0,{"$f":"IF(AF213=\"-\",0,ROUND((J213-VLOOKUP(B213,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B213,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(B213,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B213,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J213-VLOOKUP(B213,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B213,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":0},0,null,null,{"$f":"VLOOKUP($B213,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Internal room for electrical intake plant"},{"$f":"VLOOKUP($B213,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Mechanical or electrical plant facilities"},{"$f":"VLOOKUP($B213,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B213,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B213,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":"-"},{"$f":"VLOOKUP($B213,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":"-"},{"$f":"VLOOKUP($B213,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A213","v":"PLA43"},{"$f":"'Individual Spaces'!B213","v":"PLA43"},{"$f":"'Individual Spaces'!C213","v":6035},{"$f":"'Individual Spaces'!D213","v":"Services shaft (enclosed electrical) 1"},{"$f":"'Individual Spaces'!E213","v":0},null,{"$f":"VLOOKUP($B214,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_78"},{"$f":"VLOOKUP($B214,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Services shafts"},{"$f":"'Individual Spaces'!G213","v":"Balance"},{"$f":"'Individual Spaces'!H213","v":1},null,null,null,-1,null,null,{"$f":"'Individual Spaces'!O213","v":0},{"$f":"'Individual Spaces'!P213","v":0},{"$f":"'Individual Spaces'!Q213","v":0},{"$f":"'Individual Spaces'!R213","v":0},null,0,{"$f":"IF(AF214=\"-\",0,ROUND((J214-VLOOKUP(B214,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B214,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B214,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B214,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J214-VLOOKUP(B214,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B214,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B214,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Any vertical riser or duct space used for electrical plant, cabling or distribution boards"},{"$f":"VLOOKUP($B214,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Electrical plant facilities"},{"$f":"VLOOKUP($B214,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B214,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B214,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B214,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B214,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A214","v":"PLA43"},{"$f":"'Individual Spaces'!B214","v":"PLA43"},{"$f":"'Individual Spaces'!C214","v":6036},{"$f":"'Individual Spaces'!D214","v":"Services shaft (enclosed electrical) 2"},{"$f":"'Individual Spaces'!E214","v":0},null,{"$f":"VLOOKUP($B215,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_78"},{"$f":"VLOOKUP($B215,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Services shafts"},{"$f":"'Individual Spaces'!G214","v":"Balance"},{"$f":"'Individual Spaces'!H214","v":1},null,null,null,-1,null,null,{"$f":"'Individual Spaces'!O214","v":0},{"$f":"'Individual Spaces'!P214","v":0},{"$f":"'Individual Spaces'!Q214","v":0},{"$f":"'Individual Spaces'!R214","v":0},null,0,{"$f":"IF(AF215=\"-\",0,ROUND((J215-VLOOKUP(B215,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B215,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B215,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B215,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J215-VLOOKUP(B215,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B215,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B215,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Any vertical riser or duct space used for electrical plant, cabling or distribution boards"},{"$f":"VLOOKUP($B215,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Electrical plant facilities"},{"$f":"VLOOKUP($B215,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B215,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B215,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B215,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B215,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A215","v":"PLA43"},{"$f":"'Individual Spaces'!B215","v":"PLA43"},{"$f":"'Individual Spaces'!C215","v":6037},{"$f":"'Individual Spaces'!D215","v":"Services shaft (enclosed electrical) 3"},{"$f":"'Individual Spaces'!E215","v":0},null,{"$f":"VLOOKUP($B216,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_78"},{"$f":"VLOOKUP($B216,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Services shafts"},{"$f":"'Individual Spaces'!G215","v":"Balance"},{"$f":"'Individual Spaces'!H215","v":1},null,null,null,-1,null,null,{"$f":"'Individual Spaces'!O215","v":0},{"$f":"'Individual Spaces'!P215","v":0},{"$f":"'Individual Spaces'!Q215","v":0},{"$f":"'Individual Spaces'!R215","v":0},null,0,{"$f":"IF(AF216=\"-\",0,ROUND((J216-VLOOKUP(B216,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B216,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B216,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B216,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J216-VLOOKUP(B216,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B216,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B216,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Any vertical riser or duct space used for electrical plant, cabling or distribution boards"},{"$f":"VLOOKUP($B216,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Electrical plant facilities"},{"$f":"VLOOKUP($B216,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B216,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B216,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B216,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B216,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A216","v":"PLA43"},{"$f":"'Individual Spaces'!B216","v":"PLA43"},{"$f":"'Individual Spaces'!C216","v":6038},{"$f":"'Individual Spaces'!D216","v":"Services shaft (enclosed electrical) 4"},{"$f":"'Individual Spaces'!E216","v":0},null,{"$f":"VLOOKUP($B217,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_78"},{"$f":"VLOOKUP($B217,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Services shafts"},{"$f":"'Individual Spaces'!G216","v":"Balance"},{"$f":"'Individual Spaces'!H216","v":1},null,null,null,-1,null,null,{"$f":"'Individual Spaces'!O216","v":0},{"$f":"'Individual Spaces'!P216","v":0},{"$f":"'Individual Spaces'!Q216","v":0},{"$f":"'Individual Spaces'!R216","v":0},null,0,{"$f":"IF(AF217=\"-\",0,ROUND((J217-VLOOKUP(B217,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B217,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B217,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B217,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J217-VLOOKUP(B217,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B217,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B217,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Any vertical riser or duct space used for electrical plant, cabling or distribution boards"},{"$f":"VLOOKUP($B217,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Electrical plant facilities"},{"$f":"VLOOKUP($B217,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B217,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B217,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B217,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B217,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A217","v":"PLA43"},{"$f":"'Individual Spaces'!B217","v":"PLA43"},{"$f":"'Individual Spaces'!C217","v":6039},{"$f":"'Individual Spaces'!D217","v":"Services shaft (enclosed electrical) 5"},{"$f":"'Individual Spaces'!E217","v":0},null,{"$f":"VLOOKUP($B218,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_78"},{"$f":"VLOOKUP($B218,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Services shafts"},{"$f":"'Individual Spaces'!G217","v":"Balance"},{"$f":"'Individual Spaces'!H217","v":1},null,null,null,-1,null,null,{"$f":"'Individual Spaces'!O217","v":0},{"$f":"'Individual Spaces'!P217","v":0},{"$f":"'Individual Spaces'!Q217","v":0},{"$f":"'Individual Spaces'!R217","v":0},null,0,{"$f":"IF(AF218=\"-\",0,ROUND((J218-VLOOKUP(B218,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B218,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B218,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B218,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J218-VLOOKUP(B218,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B218,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B218,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Any vertical riser or duct space used for electrical plant, cabling or distribution boards"},{"$f":"VLOOKUP($B218,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Electrical plant facilities"},{"$f":"VLOOKUP($B218,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B218,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B218,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B218,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B218,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A218","v":"PLA43"},{"$f":"'Individual Spaces'!B218","v":"PLA43"},{"$f":"'Individual Spaces'!C218","v":6040},{"$f":"'Individual Spaces'!D218","v":"Services shaft (enclosed electrical) 6"},{"$f":"'Individual Spaces'!E218","v":0},null,{"$f":"VLOOKUP($B219,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_78"},{"$f":"VLOOKUP($B219,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Services shafts"},{"$f":"'Individual Spaces'!G218","v":"Balance"},{"$f":"'Individual Spaces'!H218","v":1},null,null,null,-1,null,null,{"$f":"'Individual Spaces'!O218","v":0},{"$f":"'Individual Spaces'!P218","v":0},{"$f":"'Individual Spaces'!Q218","v":0},{"$f":"'Individual Spaces'!R218","v":0},null,0,{"$f":"IF(AF219=\"-\",0,ROUND((J219-VLOOKUP(B219,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B219,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B219,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B219,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J219-VLOOKUP(B219,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B219,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B219,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Any vertical riser or duct space used for electrical plant, cabling or distribution boards"},{"$f":"VLOOKUP($B219,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Electrical plant facilities"},{"$f":"VLOOKUP($B219,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B219,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B219,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B219,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B219,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A219","v":"PLA43"},{"$f":"'Individual Spaces'!B219","v":"PLA43"},{"$f":"'Individual Spaces'!C219","v":6041},{"$f":"'Individual Spaces'!D219","v":"Services shaft (enclosed electrical) 7"},{"$f":"'Individual Spaces'!E219","v":0},null,{"$f":"VLOOKUP($B220,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_78"},{"$f":"VLOOKUP($B220,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Services shafts"},{"$f":"'Individual Spaces'!G219","v":"Balance"},{"$f":"'Individual Spaces'!H219","v":1},null,null,null,-1,null,null,{"$f":"'Individual Spaces'!O219","v":0},{"$f":"'Individual Spaces'!P219","v":0},{"$f":"'Individual Spaces'!Q219","v":0},{"$f":"'Individual Spaces'!R219","v":0},null,0,{"$f":"IF(AF220=\"-\",0,ROUND((J220-VLOOKUP(B220,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B220,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B220,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B220,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J220-VLOOKUP(B220,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B220,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B220,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Any vertical riser or duct space used for electrical plant, cabling or distribution boards"},{"$f":"VLOOKUP($B220,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Electrical plant facilities"},{"$f":"VLOOKUP($B220,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B220,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B220,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B220,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B220,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A220","v":"PLA43"},{"$f":"'Individual Spaces'!B220","v":"PLA43"},{"$f":"'Individual Spaces'!C220","v":6042},{"$f":"'Individual Spaces'!D220","v":"Services shaft (enclosed electrical) 8"},{"$f":"'Individual Spaces'!E220","v":0},null,{"$f":"VLOOKUP($B221,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_78"},{"$f":"VLOOKUP($B221,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Services shafts"},{"$f":"'Individual Spaces'!G220","v":"Balance"},{"$f":"'Individual Spaces'!H220","v":1},null,null,null,-1,null,null,{"$f":"'Individual Spaces'!O220","v":0},{"$f":"'Individual Spaces'!P220","v":0},{"$f":"'Individual Spaces'!Q220","v":0},{"$f":"'Individual Spaces'!R220","v":0},null,0,{"$f":"IF(AF221=\"-\",0,ROUND((J221-VLOOKUP(B221,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B221,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B221,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B221,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J221-VLOOKUP(B221,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B221,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B221,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Any vertical riser or duct space used for electrical plant, cabling or distribution boards"},{"$f":"VLOOKUP($B221,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Electrical plant facilities"},{"$f":"VLOOKUP($B221,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B221,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B221,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B221,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B221,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A221","v":"PLA43"},{"$f":"'Individual Spaces'!B221","v":"PLA43"},{"$f":"'Individual Spaces'!C221","v":6043},{"$f":"'Individual Spaces'!D221","v":"Services shaft (enclosed electrical) 9"},{"$f":"'Individual Spaces'!E221","v":0},null,{"$f":"VLOOKUP($B222,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_78"},{"$f":"VLOOKUP($B222,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Services shafts"},{"$f":"'Individual Spaces'!G221","v":"Balance"},{"$f":"'Individual Spaces'!H221","v":1},null,null,null,-1,null,null,{"$f":"'Individual Spaces'!O221","v":0},{"$f":"'Individual Spaces'!P221","v":0},{"$f":"'Individual Spaces'!Q221","v":0},{"$f":"'Individual Spaces'!R221","v":0},null,0,{"$f":"IF(AF222=\"-\",0,ROUND((J222-VLOOKUP(B222,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B222,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B222,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B222,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J222-VLOOKUP(B222,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B222,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B222,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Any vertical riser or duct space used for electrical plant, cabling or distribution boards"},{"$f":"VLOOKUP($B222,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Electrical plant facilities"},{"$f":"VLOOKUP($B222,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B222,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B222,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B222,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B222,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A222","v":"PLA43"},{"$f":"'Individual Spaces'!B222","v":"PLA43"},{"$f":"'Individual Spaces'!C222","v":6044},{"$f":"'Individual Spaces'!D222","v":"Services shaft (enclosed electrical) 10"},{"$f":"'Individual Spaces'!E222","v":0},null,{"$f":"VLOOKUP($B223,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_78"},{"$f":"VLOOKUP($B223,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Services shafts"},{"$f":"'Individual Spaces'!G222","v":"Balance"},{"$f":"'Individual Spaces'!H222","v":1},null,null,null,-1,null,null,{"$f":"'Individual Spaces'!O222","v":0},{"$f":"'Individual Spaces'!P222","v":0},{"$f":"'Individual Spaces'!Q222","v":0},{"$f":"'Individual Spaces'!R222","v":0},null,0,{"$f":"IF(AF223=\"-\",0,ROUND((J223-VLOOKUP(B223,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B223,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B223,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B223,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J223-VLOOKUP(B223,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B223,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B223,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Any vertical riser or duct space used for electrical plant, cabling or distribution boards"},{"$f":"VLOOKUP($B223,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Electrical plant facilities"},{"$f":"VLOOKUP($B223,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B223,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B223,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B223,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B223,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A223","v":"PLA43"},{"$f":"'Individual Spaces'!B223","v":"PLA43"},{"$f":"'Individual Spaces'!C223","v":6045},{"$f":"'Individual Spaces'!D223","v":"Services shaft (enclosed electrical) 11"},{"$f":"'Individual Spaces'!E223","v":0},null,{"$f":"VLOOKUP($B224,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_78"},{"$f":"VLOOKUP($B224,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Services shafts"},{"$f":"'Individual Spaces'!G223","v":"Balance"},{"$f":"'Individual Spaces'!H223","v":1},null,null,null,-1,null,null,{"$f":"'Individual Spaces'!O223","v":0},{"$f":"'Individual Spaces'!P223","v":0},{"$f":"'Individual Spaces'!Q223","v":0},{"$f":"'Individual Spaces'!R223","v":0},null,0,{"$f":"IF(AF224=\"-\",0,ROUND((J224-VLOOKUP(B224,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B224,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B224,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B224,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J224-VLOOKUP(B224,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B224,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B224,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Any vertical riser or duct space used for electrical plant, cabling or distribution boards"},{"$f":"VLOOKUP($B224,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Electrical plant facilities"},{"$f":"VLOOKUP($B224,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B224,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B224,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B224,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B224,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A224","v":"PLA43"},{"$f":"'Individual Spaces'!B224","v":"PLA43"},{"$f":"'Individual Spaces'!C224","v":6046},{"$f":"'Individual Spaces'!D224","v":"Services shaft (enclosed electrical) 12"},{"$f":"'Individual Spaces'!E224","v":0},null,{"$f":"VLOOKUP($B225,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_78"},{"$f":"VLOOKUP($B225,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Services shafts"},{"$f":"'Individual Spaces'!G224","v":"Balance"},{"$f":"'Individual Spaces'!H224","v":1},null,null,null,-1,null,null,{"$f":"'Individual Spaces'!O224","v":0},{"$f":"'Individual Spaces'!P224","v":0},{"$f":"'Individual Spaces'!Q224","v":0},{"$f":"'Individual Spaces'!R224","v":0},null,0,{"$f":"IF(AF225=\"-\",0,ROUND((J225-VLOOKUP(B225,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B225,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B225,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B225,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J225-VLOOKUP(B225,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B225,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B225,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Any vertical riser or duct space used for electrical plant, cabling or distribution boards"},{"$f":"VLOOKUP($B225,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Electrical plant facilities"},{"$f":"VLOOKUP($B225,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B225,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B225,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B225,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B225,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A225","v":"PLA43"},{"$f":"'Individual Spaces'!B225","v":"PLA43"},{"$f":"'Individual Spaces'!C225","v":6047},{"$f":"'Individual Spaces'!D225","v":"Services shaft (enclosed electrical) 13"},{"$f":"'Individual Spaces'!E225","v":0},null,{"$f":"VLOOKUP($B226,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_78"},{"$f":"VLOOKUP($B226,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Services shafts"},{"$f":"'Individual Spaces'!G225","v":"Balance"},{"$f":"'Individual Spaces'!H225","v":1},null,null,null,-1,null,null,{"$f":"'Individual Spaces'!O225","v":0},{"$f":"'Individual Spaces'!P225","v":0},{"$f":"'Individual Spaces'!Q225","v":0},{"$f":"'Individual Spaces'!R225","v":0},null,0,{"$f":"IF(AF226=\"-\",0,ROUND((J226-VLOOKUP(B226,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B226,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B226,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B226,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J226-VLOOKUP(B226,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B226,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B226,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Any vertical riser or duct space used for electrical plant, cabling or distribution boards"},{"$f":"VLOOKUP($B226,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Electrical plant facilities"},{"$f":"VLOOKUP($B226,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B226,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B226,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B226,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B226,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A226","v":"PLA43"},{"$f":"'Individual Spaces'!B226","v":"PLA43"},{"$f":"'Individual Spaces'!C226","v":6048},{"$f":"'Individual Spaces'!D226","v":"Services shaft (enclosed electrical) 14"},{"$f":"'Individual Spaces'!E226","v":0},null,{"$f":"VLOOKUP($B227,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_78"},{"$f":"VLOOKUP($B227,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Services shafts"},{"$f":"'Individual Spaces'!G226","v":"Balance"},{"$f":"'Individual Spaces'!H226","v":1},null,null,null,-1,null,null,{"$f":"'Individual Spaces'!O226","v":0},{"$f":"'Individual Spaces'!P226","v":0},{"$f":"'Individual Spaces'!Q226","v":0},{"$f":"'Individual Spaces'!R226","v":0},null,0,{"$f":"IF(AF227=\"-\",0,ROUND((J227-VLOOKUP(B227,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B227,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B227,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B227,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J227-VLOOKUP(B227,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B227,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B227,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Any vertical riser or duct space used for electrical plant, cabling or distribution boards"},{"$f":"VLOOKUP($B227,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Electrical plant facilities"},{"$f":"VLOOKUP($B227,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B227,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B227,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B227,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B227,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A227","v":"PLA43"},{"$f":"'Individual Spaces'!B227","v":"PLA43"},{"$f":"'Individual Spaces'!C227","v":6049},{"$f":"'Individual Spaces'!D227","v":"Services shaft (enclosed electrical) 15"},{"$f":"'Individual Spaces'!E227","v":0},null,{"$f":"VLOOKUP($B228,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_78"},{"$f":"VLOOKUP($B228,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Services shafts"},{"$f":"'Individual Spaces'!G227","v":"Balance"},{"$f":"'Individual Spaces'!H227","v":1},null,null,null,-1,null,null,{"$f":"'Individual Spaces'!O227","v":0},{"$f":"'Individual Spaces'!P227","v":0},{"$f":"'Individual Spaces'!Q227","v":0},{"$f":"'Individual Spaces'!R227","v":0},null,0,{"$f":"IF(AF228=\"-\",0,ROUND((J228-VLOOKUP(B228,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B228,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B228,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B228,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J228-VLOOKUP(B228,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B228,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B228,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Any vertical riser or duct space used for electrical plant, cabling or distribution boards"},{"$f":"VLOOKUP($B228,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Electrical plant facilities"},{"$f":"VLOOKUP($B228,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B228,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B228,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B228,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B228,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A228","v":"PLA43"},{"$f":"'Individual Spaces'!B228","v":"PLA43"},{"$f":"'Individual Spaces'!C228","v":6050},{"$f":"'Individual Spaces'!D228","v":"Services shaft (enclosed electrical) 16"},{"$f":"'Individual Spaces'!E228","v":0},null,{"$f":"VLOOKUP($B229,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_78"},{"$f":"VLOOKUP($B229,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Services shafts"},{"$f":"'Individual Spaces'!G228","v":"Balance"},{"$f":"'Individual Spaces'!H228","v":1},null,null,null,-1,null,null,{"$f":"'Individual Spaces'!O228","v":0},{"$f":"'Individual Spaces'!P228","v":0},{"$f":"'Individual Spaces'!Q228","v":0},{"$f":"'Individual Spaces'!R228","v":0},null,0,{"$f":"IF(AF229=\"-\",0,ROUND((J229-VLOOKUP(B229,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B229,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B229,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B229,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J229-VLOOKUP(B229,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B229,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B229,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Any vertical riser or duct space used for electrical plant, cabling or distribution boards"},{"$f":"VLOOKUP($B229,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Electrical plant facilities"},{"$f":"VLOOKUP($B229,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B229,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B229,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B229,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B229,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A229","v":"PLA43"},{"$f":"'Individual Spaces'!B229","v":"PLA43"},{"$f":"'Individual Spaces'!C229","v":6051},{"$f":"'Individual Spaces'!D229","v":"Services shaft (enclosed electrical) 17"},{"$f":"'Individual Spaces'!E229","v":0},null,{"$f":"VLOOKUP($B230,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_78"},{"$f":"VLOOKUP($B230,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Services shafts"},{"$f":"'Individual Spaces'!G229","v":"Balance"},{"$f":"'Individual Spaces'!H229","v":1},null,null,null,-1,null,null,{"$f":"'Individual Spaces'!O229","v":0},{"$f":"'Individual Spaces'!P229","v":0},{"$f":"'Individual Spaces'!Q229","v":0},{"$f":"'Individual Spaces'!R229","v":0},null,0,{"$f":"IF(AF230=\"-\",0,ROUND((J230-VLOOKUP(B230,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B230,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B230,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B230,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J230-VLOOKUP(B230,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B230,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B230,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Any vertical riser or duct space used for electrical plant, cabling or distribution boards"},{"$f":"VLOOKUP($B230,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Electrical plant facilities"},{"$f":"VLOOKUP($B230,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B230,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B230,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B230,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B230,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A230","v":"PLA43"},{"$f":"'Individual Spaces'!B230","v":"PLA43"},{"$f":"'Individual Spaces'!C230","v":6052},{"$f":"'Individual Spaces'!D230","v":"Services shaft (enclosed electrical) 18"},{"$f":"'Individual Spaces'!E230","v":0},null,{"$f":"VLOOKUP($B231,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_78"},{"$f":"VLOOKUP($B231,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Services shafts"},{"$f":"'Individual Spaces'!G230","v":"Balance"},{"$f":"'Individual Spaces'!H230","v":1},null,null,null,-1,null,null,{"$f":"'Individual Spaces'!O230","v":0},{"$f":"'Individual Spaces'!P230","v":0},{"$f":"'Individual Spaces'!Q230","v":0},{"$f":"'Individual Spaces'!R230","v":0},null,0,{"$f":"IF(AF231=\"-\",0,ROUND((J231-VLOOKUP(B231,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B231,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B231,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B231,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J231-VLOOKUP(B231,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B231,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B231,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Any vertical riser or duct space used for electrical plant, cabling or distribution boards"},{"$f":"VLOOKUP($B231,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Electrical plant facilities"},{"$f":"VLOOKUP($B231,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B231,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B231,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B231,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B231,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A231","v":"PLA43"},{"$f":"'Individual Spaces'!B231","v":"PLA43"},{"$f":"'Individual Spaces'!C231","v":6053},{"$f":"'Individual Spaces'!D231","v":"Services shaft (enclosed electrical) 19"},{"$f":"'Individual Spaces'!E231","v":0},null,{"$f":"VLOOKUP($B232,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_78"},{"$f":"VLOOKUP($B232,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Services shafts"},{"$f":"'Individual Spaces'!G231","v":"Balance"},{"$f":"'Individual Spaces'!H231","v":1},null,null,null,-1,null,null,{"$f":"'Individual Spaces'!O231","v":0},{"$f":"'Individual Spaces'!P231","v":0},{"$f":"'Individual Spaces'!Q231","v":0},{"$f":"'Individual Spaces'!R231","v":0},null,0,{"$f":"IF(AF232=\"-\",0,ROUND((J232-VLOOKUP(B232,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B232,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B232,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B232,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J232-VLOOKUP(B232,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B232,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B232,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Any vertical riser or duct space used for electrical plant, cabling or distribution boards"},{"$f":"VLOOKUP($B232,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Electrical plant facilities"},{"$f":"VLOOKUP($B232,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B232,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B232,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B232,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B232,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A232","v":"PLA43"},{"$f":"'Individual Spaces'!B232","v":"PLA43"},{"$f":"'Individual Spaces'!C232","v":6054},{"$f":"'Individual Spaces'!D232","v":"Services shaft (enclosed electrical) 20"},{"$f":"'Individual Spaces'!E232","v":0},null,{"$f":"VLOOKUP($B233,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_90_78"},{"$f":"VLOOKUP($B233,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Services shafts"},{"$f":"'Individual Spaces'!G232","v":"Balance"},{"$f":"'Individual Spaces'!H232","v":1},null,null,null,-1,null,null,{"$f":"'Individual Spaces'!O232","v":0},{"$f":"'Individual Spaces'!P232","v":0},{"$f":"'Individual Spaces'!Q232","v":0},{"$f":"'Individual Spaces'!R232","v":0},null,0,{"$f":"IF(AF233=\"-\",0,ROUND((J233-VLOOKUP(B233,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B233,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B233,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B233,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J233-VLOOKUP(B233,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B233,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B233,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Any vertical riser or duct space used for electrical plant, cabling or distribution boards"},{"$f":"VLOOKUP($B233,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Electrical plant facilities"},{"$f":"VLOOKUP($B233,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B233,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B233,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B233,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B233,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"None"}]
[{"$f":"'Individual Spaces'!A233","v":"CIR12"},{"$f":"'Individual Spaces'!B233","v":"CIR12"},{"$f":"'Individual Spaces'!C233","v":6055},{"$f":"'Individual Spaces'!D233","v":"Stairway 1"},{"$f":"'Individual Spaces'!E233","v":0},null,{"$f":"VLOOKUP($B234,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_10_87"},{"$f":"VLOOKUP($B234,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Stairways"},{"$f":"'Individual Spaces'!G233","v":"Balance"},{"$f":"'Individual Spaces'!H233","v":27},null,null,null,-27,null,null,{"$f":"'Individual Spaces'!O233","v":0},{"$f":"'Individual Spaces'!P233","v":0},{"$f":"'Individual Spaces'!Q233","v":0},{"$f":"'Individual Spaces'!R233","v":0},null,0,{"$f":"IF(AF234=\"-\",0,ROUND((J234-VLOOKUP(B234,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B234,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B234,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B234,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J234-VLOOKUP(B234,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B234,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B234,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Enclosed stairwell between floors, including stairs, landings and fire escape refuge areas"},{"$f":"VLOOKUP($B234,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Circulation of pupils and others between spaces."},{"$f":"VLOOKUP($B234,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B234,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B234,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B234,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B234,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"CTS"}]
[{"$f":"'Individual Spaces'!A234","v":"CIR12"},{"$f":"'Individual Spaces'!B234","v":"CIR12"},{"$f":"'Individual Spaces'!C234","v":6056},{"$f":"'Individual Spaces'!D234","v":"Stairway 2"},{"$f":"'Individual Spaces'!E234","v":0},null,{"$f":"VLOOKUP($B235,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_10_87"},{"$f":"VLOOKUP($B235,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Stairways"},{"$f":"'Individual Spaces'!G234","v":"Balance"},{"$f":"'Individual Spaces'!H234","v":27},null,null,null,-27,null,null,{"$f":"'Individual Spaces'!O234","v":0},{"$f":"'Individual Spaces'!P234","v":0},{"$f":"'Individual Spaces'!Q234","v":0},{"$f":"'Individual Spaces'!R234","v":0},null,0,{"$f":"IF(AF235=\"-\",0,ROUND((J235-VLOOKUP(B235,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B235,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B235,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B235,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J235-VLOOKUP(B235,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B235,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B235,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Enclosed stairwell between floors, including stairs, landings and fire escape refuge areas"},{"$f":"VLOOKUP($B235,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Circulation of pupils and others between spaces."},{"$f":"VLOOKUP($B235,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B235,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B235,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B235,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B235,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"CTS"}]
[{"$f":"'Individual Spaces'!A235","v":"CIR12"},{"$f":"'Individual Spaces'!B235","v":"CIR12"},{"$f":"'Individual Spaces'!C235","v":6057},{"$f":"'Individual Spaces'!D235","v":"Stairway 3"},{"$f":"'Individual Spaces'!E235","v":0},null,{"$f":"VLOOKUP($B236,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_10_87"},{"$f":"VLOOKUP($B236,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Stairways"},{"$f":"'Individual Spaces'!G235","v":"Balance"},{"$f":"'Individual Spaces'!H235","v":27},null,null,null,-27,null,null,{"$f":"'Individual Spaces'!O235","v":0},{"$f":"'Individual Spaces'!P235","v":0},{"$f":"'Individual Spaces'!Q235","v":0},{"$f":"'Individual Spaces'!R235","v":0},null,0,{"$f":"IF(AF236=\"-\",0,ROUND((J236-VLOOKUP(B236,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B236,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B236,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B236,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J236-VLOOKUP(B236,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B236,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B236,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Enclosed stairwell between floors, including stairs, landings and fire escape refuge areas"},{"$f":"VLOOKUP($B236,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Circulation of pupils and others between spaces."},{"$f":"VLOOKUP($B236,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B236,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B236,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B236,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B236,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"CTS"}]
[{"$f":"'Individual Spaces'!A236","v":"CIR12"},{"$f":"'Individual Spaces'!B236","v":"CIR12"},{"$f":"'Individual Spaces'!C236","v":6058},{"$f":"'Individual Spaces'!D236","v":"Stairway 4"},{"$f":"'Individual Spaces'!E236","v":0},null,{"$f":"VLOOKUP($B237,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_10_87"},{"$f":"VLOOKUP($B237,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Stairways"},{"$f":"'Individual Spaces'!G236","v":"Balance"},{"$f":"'Individual Spaces'!H236","v":27},null,null,null,-27,null,null,{"$f":"'Individual Spaces'!O236","v":0},{"$f":"'Individual Spaces'!P236","v":0},{"$f":"'Individual Spaces'!Q236","v":0},{"$f":"'Individual Spaces'!R236","v":0},null,0,{"$f":"IF(AF237=\"-\",0,ROUND((J237-VLOOKUP(B237,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B237,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B237,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B237,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J237-VLOOKUP(B237,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B237,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B237,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Enclosed stairwell between floors, including stairs, landings and fire escape refuge areas"},{"$f":"VLOOKUP($B237,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Circulation of pupils and others between spaces."},{"$f":"VLOOKUP($B237,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B237,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B237,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B237,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B237,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"CTS"}]
[{"$f":"'Individual Spaces'!A237","v":"CIR12"},{"$f":"'Individual Spaces'!B237","v":"CIR12"},{"$f":"'Individual Spaces'!C237","v":6059},{"$f":"'Individual Spaces'!D237","v":"Stairway 5"},{"$f":"'Individual Spaces'!E237","v":0},null,{"$f":"VLOOKUP($B238,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_10_87"},{"$f":"VLOOKUP($B238,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Stairways"},{"$f":"'Individual Spaces'!G237","v":"Balance"},{"$f":"'Individual Spaces'!H237","v":27},null,null,null,-27,null,null,{"$f":"'Individual Spaces'!O237","v":0},{"$f":"'Individual Spaces'!P237","v":0},{"$f":"'Individual Spaces'!Q237","v":0},{"$f":"'Individual Spaces'!R237","v":0},null,0,{"$f":"IF(AF238=\"-\",0,ROUND((J238-VLOOKUP(B238,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B238,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B238,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B238,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J238-VLOOKUP(B238,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B238,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B238,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Enclosed stairwell between floors, including stairs, landings and fire escape refuge areas"},{"$f":"VLOOKUP($B238,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Circulation of pupils and others between spaces."},{"$f":"VLOOKUP($B238,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B238,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B238,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B238,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B238,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"CTS"}]
[{"$f":"'Individual Spaces'!A238","v":"CIR12"},{"$f":"'Individual Spaces'!B238","v":"CIR12"},{"$f":"'Individual Spaces'!C238","v":6060},{"$f":"'Individual Spaces'!D238","v":"Stairway 6"},{"$f":"'Individual Spaces'!E238","v":0},null,{"$f":"VLOOKUP($B239,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_10_87"},{"$f":"VLOOKUP($B239,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Stairways"},{"$f":"'Individual Spaces'!G238","v":"Balance"},{"$f":"'Individual Spaces'!H238","v":27},null,null,null,-27,null,null,{"$f":"'Individual Spaces'!O238","v":0},{"$f":"'Individual Spaces'!P238","v":0},{"$f":"'Individual Spaces'!Q238","v":0},{"$f":"'Individual Spaces'!R238","v":0},null,0,{"$f":"IF(AF239=\"-\",0,ROUND((J239-VLOOKUP(B239,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B239,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B239,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B239,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J239-VLOOKUP(B239,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B239,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B239,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Enclosed stairwell between floors, including stairs, landings and fire escape refuge areas"},{"$f":"VLOOKUP($B239,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Circulation of pupils and others between spaces."},{"$f":"VLOOKUP($B239,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B239,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B239,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B239,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B239,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"CTS"}]
[{"$f":"'Individual Spaces'!A239","v":"CIR12"},{"$f":"'Individual Spaces'!B239","v":"CIR12"},{"$f":"'Individual Spaces'!C239","v":6061},{"$f":"'Individual Spaces'!D239","v":"Stairway 7"},{"$f":"'Individual Spaces'!E239","v":0},null,{"$f":"VLOOKUP($B240,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_10_87"},{"$f":"VLOOKUP($B240,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Stairways"},{"$f":"'Individual Spaces'!G239","v":"Balance"},{"$f":"'Individual Spaces'!H239","v":27},null,null,null,-27,null,null,{"$f":"'Individual Spaces'!O239","v":0},{"$f":"'Individual Spaces'!P239","v":0},{"$f":"'Individual Spaces'!Q239","v":0},{"$f":"'Individual Spaces'!R239","v":0},null,0,{"$f":"IF(AF240=\"-\",0,ROUND((J240-VLOOKUP(B240,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B240,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B240,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B240,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J240-VLOOKUP(B240,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B240,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B240,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Enclosed stairwell between floors, including stairs, landings and fire escape refuge areas"},{"$f":"VLOOKUP($B240,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Circulation of pupils and others between spaces."},{"$f":"VLOOKUP($B240,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B240,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B240,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B240,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B240,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"CTS"}]
[{"$f":"'Individual Spaces'!A240","v":"CIR12"},{"$f":"'Individual Spaces'!B240","v":"CIR12"},{"$f":"'Individual Spaces'!C240","v":6062},{"$f":"'Individual Spaces'!D240","v":"Stairway 8"},{"$f":"'Individual Spaces'!E240","v":0},null,{"$f":"VLOOKUP($B241,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_10_87"},{"$f":"VLOOKUP($B241,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Stairways"},{"$f":"'Individual Spaces'!G240","v":"Balance"},{"$f":"'Individual Spaces'!H240","v":27},null,null,null,-27,null,null,{"$f":"'Individual Spaces'!O240","v":0},{"$f":"'Individual Spaces'!P240","v":0},{"$f":"'Individual Spaces'!Q240","v":0},{"$f":"'Individual Spaces'!R240","v":0},null,0,{"$f":"IF(AF241=\"-\",0,ROUND((J241-VLOOKUP(B241,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B241,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B241,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B241,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J241-VLOOKUP(B241,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B241,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B241,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Enclosed stairwell between floors, including stairs, landings and fire escape refuge areas"},{"$f":"VLOOKUP($B241,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Circulation of pupils and others between spaces."},{"$f":"VLOOKUP($B241,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B241,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B241,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B241,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B241,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"CTS"}]
[{"$f":"'Individual Spaces'!A241","v":"CIR12"},{"$f":"'Individual Spaces'!B241","v":"CIR12"},{"$f":"'Individual Spaces'!C241","v":6063},{"$f":"'Individual Spaces'!D241","v":"Stairway 9"},{"$f":"'Individual Spaces'!E241","v":0},null,{"$f":"VLOOKUP($B242,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_10_87"},{"$f":"VLOOKUP($B242,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Stairways"},{"$f":"'Individual Spaces'!G241","v":"Balance"},{"$f":"'Individual Spaces'!H241","v":27},null,null,null,-27,null,null,{"$f":"'Individual Spaces'!O241","v":0},{"$f":"'Individual Spaces'!P241","v":0},{"$f":"'Individual Spaces'!Q241","v":0},{"$f":"'Individual Spaces'!R241","v":0},null,0,{"$f":"IF(AF242=\"-\",0,ROUND((J242-VLOOKUP(B242,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B242,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B242,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B242,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J242-VLOOKUP(B242,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B242,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B242,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Enclosed stairwell between floors, including stairs, landings and fire escape refuge areas"},{"$f":"VLOOKUP($B242,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Circulation of pupils and others between spaces."},{"$f":"VLOOKUP($B242,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B242,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B242,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B242,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B242,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"CTS"}]
[{"$f":"'Individual Spaces'!A242","v":"CIR12"},{"$f":"'Individual Spaces'!B242","v":"CIR12"},{"$f":"'Individual Spaces'!C242","v":6064},{"$f":"'Individual Spaces'!D242","v":"Stairway 10"},{"$f":"'Individual Spaces'!E242","v":0},null,{"$f":"VLOOKUP($B243,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_10_87"},{"$f":"VLOOKUP($B243,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Stairways"},{"$f":"'Individual Spaces'!G242","v":"Balance"},{"$f":"'Individual Spaces'!H242","v":27},null,null,null,-27,null,null,{"$f":"'Individual Spaces'!O242","v":0},{"$f":"'Individual Spaces'!P242","v":0},{"$f":"'Individual Spaces'!Q242","v":0},{"$f":"'Individual Spaces'!R242","v":0},null,0,{"$f":"IF(AF243=\"-\",0,ROUND((J243-VLOOKUP(B243,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B243,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B243,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B243,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J243-VLOOKUP(B243,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B243,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B243,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Enclosed stairwell between floors, including stairs, landings and fire escape refuge areas"},{"$f":"VLOOKUP($B243,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Circulation of pupils and others between spaces."},{"$f":"VLOOKUP($B243,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B243,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B243,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B243,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B243,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"CTS"}]
[{"$f":"'Individual Spaces'!A243","v":"CIR12"},{"$f":"'Individual Spaces'!B243","v":"CIR12"},{"$f":"'Individual Spaces'!C243","v":6065},{"$f":"'Individual Spaces'!D243","v":"Stairway 11"},{"$f":"'Individual Spaces'!E243","v":0},null,{"$f":"VLOOKUP($B244,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_10_87"},{"$f":"VLOOKUP($B244,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Stairways"},{"$f":"'Individual Spaces'!G243","v":"Balance"},{"$f":"'Individual Spaces'!H243","v":27},null,null,null,-27,null,null,{"$f":"'Individual Spaces'!O243","v":0},{"$f":"'Individual Spaces'!P243","v":0},{"$f":"'Individual Spaces'!Q243","v":0},{"$f":"'Individual Spaces'!R243","v":0},null,0,{"$f":"IF(AF244=\"-\",0,ROUND((J244-VLOOKUP(B244,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B244,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B244,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B244,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J244-VLOOKUP(B244,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B244,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B244,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Enclosed stairwell between floors, including stairs, landings and fire escape refuge areas"},{"$f":"VLOOKUP($B244,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Circulation of pupils and others between spaces."},{"$f":"VLOOKUP($B244,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B244,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B244,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B244,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B244,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"CTS"}]
[{"$f":"'Individual Spaces'!A244","v":"CIR12"},{"$f":"'Individual Spaces'!B244","v":"CIR12"},{"$f":"'Individual Spaces'!C244","v":6066},{"$f":"'Individual Spaces'!D244","v":"Stairway 12"},{"$f":"'Individual Spaces'!E244","v":0},null,{"$f":"VLOOKUP($B245,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_10_87"},{"$f":"VLOOKUP($B245,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Stairways"},{"$f":"'Individual Spaces'!G244","v":"Balance"},{"$f":"'Individual Spaces'!H244","v":27},null,null,null,-27,null,null,{"$f":"'Individual Spaces'!O244","v":0},{"$f":"'Individual Spaces'!P244","v":0},{"$f":"'Individual Spaces'!Q244","v":0},{"$f":"'Individual Spaces'!R244","v":0},null,0,{"$f":"IF(AF245=\"-\",0,ROUND((J245-VLOOKUP(B245,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B245,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B245,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B245,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J245-VLOOKUP(B245,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B245,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B245,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Enclosed stairwell between floors, including stairs, landings and fire escape refuge areas"},{"$f":"VLOOKUP($B245,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Circulation of pupils and others between spaces."},{"$f":"VLOOKUP($B245,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B245,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B245,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B245,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B245,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"CTS"}]
[{"$f":"'Individual Spaces'!A245","v":"CIR13"},{"$f":"'Individual Spaces'!B245","v":"CIR13"},{"$f":"'Individual Spaces'!C245","v":6067},{"$f":"'Individual Spaces'!D245","v":"Lift 1"},{"$f":"'Individual Spaces'!E245","v":0},null,{"$f":"VLOOKUP($B246,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_10_47"},{"$f":"VLOOKUP($B246,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Lifts"},{"$f":"'Individual Spaces'!G245","v":"Balance"},{"$f":"'Individual Spaces'!H245","v":6},null,null,null,-6,null,null,{"$f":"'Individual Spaces'!O245","v":0},{"$f":"'Individual Spaces'!P245","v":0},{"$f":"'Individual Spaces'!Q245","v":0},{"$f":"'Individual Spaces'!R245","v":0},null,0,{"$f":"IF(AF246=\"-\",0,ROUND((J246-VLOOKUP(B246,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B246,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B246,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B246,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J246-VLOOKUP(B246,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B246,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B246,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Lift enclosure and space to wait in front of doors"},{"$f":"VLOOKUP($B246,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Circulation of pupils and others between spaces."},{"$f":"VLOOKUP($B246,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B246,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B246,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B246,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B246,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"CTS"}]
[{"$f":"'Individual Spaces'!A246","v":"CIR13"},{"$f":"'Individual Spaces'!B246","v":"CIR13"},{"$f":"'Individual Spaces'!C246","v":6068},{"$f":"'Individual Spaces'!D246","v":"Lift 2"},{"$f":"'Individual Spaces'!E246","v":0},null,{"$f":"VLOOKUP($B247,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_10_47"},{"$f":"VLOOKUP($B247,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Lifts"},{"$f":"'Individual Spaces'!G246","v":"Balance"},{"$f":"'Individual Spaces'!H246","v":6},null,null,null,-6,null,null,{"$f":"'Individual Spaces'!O246","v":0},{"$f":"'Individual Spaces'!P246","v":0},{"$f":"'Individual Spaces'!Q246","v":0},{"$f":"'Individual Spaces'!R246","v":0},null,0,{"$f":"IF(AF247=\"-\",0,ROUND((J247-VLOOKUP(B247,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B247,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B247,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B247,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J247-VLOOKUP(B247,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B247,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B247,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Lift enclosure and space to wait in front of doors"},{"$f":"VLOOKUP($B247,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Circulation of pupils and others between spaces."},{"$f":"VLOOKUP($B247,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B247,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B247,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B247,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B247,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"CTS"}]
[{"$f":"'Individual Spaces'!A247","v":"CIR13"},{"$f":"'Individual Spaces'!B247","v":"CIR13"},{"$f":"'Individual Spaces'!C247","v":6069},{"$f":"'Individual Spaces'!D247","v":"Lift 3"},{"$f":"'Individual Spaces'!E247","v":0},null,{"$f":"VLOOKUP($B248,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_10_47"},{"$f":"VLOOKUP($B248,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Lifts"},{"$f":"'Individual Spaces'!G247","v":"Balance"},{"$f":"'Individual Spaces'!H247","v":6},null,null,null,-6,null,null,{"$f":"'Individual Spaces'!O247","v":0},{"$f":"'Individual Spaces'!P247","v":0},{"$f":"'Individual Spaces'!Q247","v":0},{"$f":"'Individual Spaces'!R247","v":0},null,0,{"$f":"IF(AF248=\"-\",0,ROUND((J248-VLOOKUP(B248,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B248,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B248,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B248,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J248-VLOOKUP(B248,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B248,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B248,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Lift enclosure and space to wait in front of doors"},{"$f":"VLOOKUP($B248,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Circulation of pupils and others between spaces."},{"$f":"VLOOKUP($B248,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B248,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B248,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B248,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B248,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"CTS"}]
[{"$f":"'Individual Spaces'!A248","v":"CIR13"},{"$f":"'Individual Spaces'!B248","v":"CIR13"},{"$f":"'Individual Spaces'!C248","v":6070},{"$f":"'Individual Spaces'!D248","v":"Lift 4"},{"$f":"'Individual Spaces'!E248","v":0},null,{"$f":"VLOOKUP($B249,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_10_47"},{"$f":"VLOOKUP($B249,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Lifts"},{"$f":"'Individual Spaces'!G248","v":"Balance"},{"$f":"'Individual Spaces'!H248","v":6},null,null,null,-6,null,null,{"$f":"'Individual Spaces'!O248","v":0},{"$f":"'Individual Spaces'!P248","v":0},{"$f":"'Individual Spaces'!Q248","v":0},{"$f":"'Individual Spaces'!R248","v":0},null,0,{"$f":"IF(AF249=\"-\",0,ROUND((J249-VLOOKUP(B249,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B249,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B249,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B249,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J249-VLOOKUP(B249,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B249,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B249,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Lift enclosure and space to wait in front of doors"},{"$f":"VLOOKUP($B249,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Circulation of pupils and others between spaces."},{"$f":"VLOOKUP($B249,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B249,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B249,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B249,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B249,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"CTS"}]
[{"$f":"'Individual Spaces'!A249","v":"CIR13"},{"$f":"'Individual Spaces'!B249","v":"CIR13"},{"$f":"'Individual Spaces'!C249","v":6071},{"$f":"'Individual Spaces'!D249","v":"Lift 5"},{"$f":"'Individual Spaces'!E249","v":0},null,{"$f":"VLOOKUP($B250,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_10_47"},{"$f":"VLOOKUP($B250,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Lifts"},{"$f":"'Individual Spaces'!G249","v":"Balance"},{"$f":"'Individual Spaces'!H249","v":6},null,null,null,-6,null,null,{"$f":"'Individual Spaces'!O249","v":0},{"$f":"'Individual Spaces'!P249","v":0},{"$f":"'Individual Spaces'!Q249","v":0},{"$f":"'Individual Spaces'!R249","v":0},null,0,{"$f":"IF(AF250=\"-\",0,ROUND((J250-VLOOKUP(B250,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B250,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B250,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B250,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J250-VLOOKUP(B250,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B250,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B250,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Lift enclosure and space to wait in front of doors"},{"$f":"VLOOKUP($B250,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Circulation of pupils and others between spaces."},{"$f":"VLOOKUP($B250,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B250,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B250,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B250,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B250,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"CTS"}]
[{"$f":"'Individual Spaces'!A250","v":"CIR13"},{"$f":"'Individual Spaces'!B250","v":"CIR13"},{"$f":"'Individual Spaces'!C250","v":6072},{"$f":"'Individual Spaces'!D250","v":"Lift 6"},{"$f":"'Individual Spaces'!E250","v":0},null,{"$f":"VLOOKUP($B251,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_10_47"},{"$f":"VLOOKUP($B251,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Lifts"},{"$f":"'Individual Spaces'!G250","v":"Balance"},{"$f":"'Individual Spaces'!H250","v":6},null,null,null,-6,null,null,{"$f":"'Individual Spaces'!O250","v":0},{"$f":"'Individual Spaces'!P250","v":0},{"$f":"'Individual Spaces'!Q250","v":0},{"$f":"'Individual Spaces'!R250","v":0},null,0,{"$f":"IF(AF251=\"-\",0,ROUND((J251-VLOOKUP(B251,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B251,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B251,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B251,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J251-VLOOKUP(B251,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B251,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B251,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Lift enclosure and space to wait in front of doors"},{"$f":"VLOOKUP($B251,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Circulation of pupils and others between spaces."},{"$f":"VLOOKUP($B251,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B251,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B251,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B251,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B251,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"CTS"}]
[{"$f":"'Individual Spaces'!A251","v":"CIR03"},{"$f":"'Individual Spaces'!B251","v":"CIR03"},{"$f":"'Individual Spaces'!C251","v":6073},{"$f":"'Individual Spaces'!D251","v":"Lobby 1"},{"$f":"'Individual Spaces'!E251","v":0},null,{"$f":"VLOOKUP($B252,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_10_51"},{"$f":"VLOOKUP($B252,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Lobbies"},{"$f":"'Individual Spaces'!G251","v":"Balance"},{"$f":"'Individual Spaces'!H251","v":6},null,null,null,-6,null,null,{"$f":"'Individual Spaces'!O251","v":0},{"$f":"'Individual Spaces'!P251","v":0},{"$f":"'Individual Spaces'!Q251","v":0},{"$f":"'Individual Spaces'!R251","v":0},null,0,{"$f":"IF(AF252=\"-\",0,ROUND((J252-VLOOKUP(B252,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B252,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B252,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B252,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J252-VLOOKUP(B252,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B252,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B252,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Lobby area between main external doors and internal lobby doors"},{"$f":"VLOOKUP($B252,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Circulation of pupils and others between spaces."},{"$f":"VLOOKUP($B252,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B252,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B252,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B252,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B252,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"CTS"}]
[{"$f":"'Individual Spaces'!A252","v":"CIR03"},{"$f":"'Individual Spaces'!B252","v":"CIR03"},{"$f":"'Individual Spaces'!C252","v":6074},{"$f":"'Individual Spaces'!D252","v":"Lobby 2"},{"$f":"'Individual Spaces'!E252","v":0},null,{"$f":"VLOOKUP($B253,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":"SL_90_10_51"},{"$f":"VLOOKUP($B253,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"Lobbies"},{"$f":"'Individual Spaces'!G252","v":"Balance"},{"$f":"'Individual Spaces'!H252","v":6},null,null,null,-6,null,null,{"$f":"'Individual Spaces'!O252","v":0},{"$f":"'Individual Spaces'!P252","v":0},{"$f":"'Individual Spaces'!Q252","v":0},{"$f":"'Individual Spaces'!R252","v":0},null,0,{"$f":"IF(AF253=\"-\",0,ROUND((J253-VLOOKUP(B253,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B253,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B253,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B253,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J253-VLOOKUP(B253,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B253,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B253,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":"Lobby area between main external doors and internal lobby doors"},{"$f":"VLOOKUP($B253,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":"Circulation of pupils and others between spaces."},{"$f":"VLOOKUP($B253,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B253,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":"Non-net"},{"$f":"VLOOKUP($B253,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B253,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B253,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":"CTS"}]
[{"$f":"'Individual Spaces'!A253","v":0},{"$f":"'Individual Spaces'!B253","v":0},{"$f":"'Individual Spaces'!C253","v":0},{"$f":"'Individual Spaces'!D253","v":0},{"$f":"'Individual Spaces'!E253","v":"Non-Net Total (except horizontal circulation or partitions) : "},null,{"$f":"VLOOKUP($B254,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B254,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G253","v":0},{"$f":"'Individual Spaces'!H253","v":979.10000000000014},null,null,null,-979.10000000000014,null,null,{"$f":"'Individual Spaces'!O253","v":0},{"$f":"'Individual Spaces'!P253","v":0},{"$f":"'Individual Spaces'!Q253","v":0},{"$f":"'Individual Spaces'!R253","v":0},null,0,{"$f":"IF(AF254=\"-\",0,ROUND((J254-VLOOKUP(B254,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B254,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B254,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B254,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J254-VLOOKUP(B254,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B254,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B254,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B254,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B254,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B254,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B254,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B254,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B254,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A254","v":0},{"$f":"'Individual Spaces'!B254","v":0},{"$f":"'Individual Spaces'!C254","v":0},{"$f":"'Individual Spaces'!D254","v":0},{"$f":"'Individual Spaces'!E254","v":0},null,{"$f":"VLOOKUP($B255,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B255,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G254","v":0},{"$f":"'Individual Spaces'!H254","v":0},null,null,null,{"$f":"M255-J255","v":0},null,null,{"$f":"'Individual Spaces'!O254","v":"Unallocated Spaces"},{"$f":"'Individual Spaces'!P254","v":0},{"$f":"'Individual Spaces'!Q254","v":0},{"$f":"'Individual Spaces'!R254","v":0},null,{"$f":"Q255","v":"Unallocated Spaces"},{"$f":"IF(AF255=\"-\",0,ROUND((J255-VLOOKUP(B255,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B255,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B255,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B255,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J255-VLOOKUP(B255,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B255,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$f":"IF(W255>200,ROUND(W255*1.05,0),ROUNDUP(W255*1.1,0))","v":{"$error":"#N/A"}},null,null,{"$f":"VLOOKUP($B255,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B255,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B255,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B255,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B255,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B255,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B255,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A255","v":0},{"$f":"'Individual Spaces'!B255","v":0},{"$f":"'Individual Spaces'!C255","v":0},{"$f":"'Individual Spaces'!D255","v":0},{"$f":"'Individual Spaces'!E255","v":0},null,{"$f":"VLOOKUP($B256,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B256,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G255","v":0},{"$f":"'Individual Spaces'!H255","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O255","v":"Keep"},{"$f":"'Individual Spaces'!P255","v":101},{"$f":"'Individual Spaces'!Q255","v":"classroom"},{"$f":"'Individual Spaces'!R255","v":"$EY$9"},null,"Keep",{"$f":"IF(AF256=\"-\",0,ROUND((J256-VLOOKUP(B256,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B256,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B256,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B256,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J256-VLOOKUP(B256,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B256,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B256,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B256,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B256,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B256,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B256,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B256,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B256,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A256","v":0},{"$f":"'Individual Spaces'!B256","v":0},{"$f":"'Individual Spaces'!C256","v":0},{"$f":"'Individual Spaces'!D256","v":0},{"$f":"'Individual Spaces'!E256","v":0},null,{"$f":"VLOOKUP($B257,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B257,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G256","v":0},{"$f":"'Individual Spaces'!H256","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O256","v":0},{"$f":"'Individual Spaces'!P256","v":0},{"$f":"'Individual Spaces'!Q256","v":0},{"$f":"'Individual Spaces'!R256","v":0},null,0,{"$f":"IF(AF257=\"-\",0,ROUND((J257-VLOOKUP(B257,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B257,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B257,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B257,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J257-VLOOKUP(B257,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B257,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B257,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B257,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B257,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B257,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B257,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B257,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B257,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A257","v":0},{"$f":"'Individual Spaces'!B257","v":0},{"$f":"'Individual Spaces'!C257","v":0},{"$f":"'Individual Spaces'!D257","v":0},{"$f":"'Individual Spaces'!E257","v":0},null,{"$f":"VLOOKUP($B258,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B258,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G257","v":0},{"$f":"'Individual Spaces'!H257","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O257","v":0},{"$f":"'Individual Spaces'!P257","v":0},{"$f":"'Individual Spaces'!Q257","v":0},{"$f":"'Individual Spaces'!R257","v":0},null,0,{"$f":"IF(AF258=\"-\",0,ROUND((J258-VLOOKUP(B258,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B258,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B258,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B258,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J258-VLOOKUP(B258,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B258,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B258,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B258,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B258,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B258,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B258,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B258,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B258,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A258","v":0},{"$f":"'Individual Spaces'!B258","v":0},{"$f":"'Individual Spaces'!C258","v":0},{"$f":"'Individual Spaces'!D258","v":0},{"$f":"'Individual Spaces'!E258","v":0},null,{"$f":"VLOOKUP($B259,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B259,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G258","v":0},{"$f":"'Individual Spaces'!H258","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O258","v":0},{"$f":"'Individual Spaces'!P258","v":0},{"$f":"'Individual Spaces'!Q258","v":0},{"$f":"'Individual Spaces'!R258","v":0},null,0,{"$f":"IF(AF259=\"-\",0,ROUND((J259-VLOOKUP(B259,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B259,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B259,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B259,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J259-VLOOKUP(B259,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B259,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B259,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B259,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B259,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B259,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B259,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B259,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B259,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A259","v":0},{"$f":"'Individual Spaces'!B259","v":0},{"$f":"'Individual Spaces'!C259","v":0},{"$f":"'Individual Spaces'!D259","v":0},{"$f":"'Individual Spaces'!E259","v":0},null,{"$f":"VLOOKUP($B260,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B260,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G259","v":0},{"$f":"'Individual Spaces'!H259","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O259","v":0},{"$f":"'Individual Spaces'!P259","v":0},{"$f":"'Individual Spaces'!Q259","v":0},{"$f":"'Individual Spaces'!R259","v":0},null,0,{"$f":"IF(AF260=\"-\",0,ROUND((J260-VLOOKUP(B260,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B260,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B260,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B260,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J260-VLOOKUP(B260,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B260,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B260,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B260,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B260,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B260,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B260,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B260,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B260,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A260","v":0},{"$f":"'Individual Spaces'!B260","v":0},{"$f":"'Individual Spaces'!C260","v":0},{"$f":"'Individual Spaces'!D260","v":0},{"$f":"'Individual Spaces'!E260","v":0},null,{"$f":"VLOOKUP($B261,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B261,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G260","v":0},{"$f":"'Individual Spaces'!H260","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O260","v":0},{"$f":"'Individual Spaces'!P260","v":0},{"$f":"'Individual Spaces'!Q260","v":0},{"$f":"'Individual Spaces'!R260","v":0},null,0,{"$f":"IF(AF261=\"-\",0,ROUND((J261-VLOOKUP(B261,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B261,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B261,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B261,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J261-VLOOKUP(B261,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B261,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B261,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B261,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B261,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B261,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B261,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B261,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B261,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A261","v":0},{"$f":"'Individual Spaces'!B261","v":0},{"$f":"'Individual Spaces'!C261","v":0},{"$f":"'Individual Spaces'!D261","v":0},{"$f":"'Individual Spaces'!E261","v":0},null,{"$f":"VLOOKUP($B262,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B262,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G261","v":0},{"$f":"'Individual Spaces'!H261","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O261","v":0},{"$f":"'Individual Spaces'!P261","v":0},{"$f":"'Individual Spaces'!Q261","v":0},{"$f":"'Individual Spaces'!R261","v":0},null,0,{"$f":"IF(AF262=\"-\",0,ROUND((J262-VLOOKUP(B262,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B262,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B262,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B262,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J262-VLOOKUP(B262,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B262,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B262,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B262,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B262,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B262,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B262,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B262,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B262,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A262","v":0},{"$f":"'Individual Spaces'!B262","v":0},{"$f":"'Individual Spaces'!C262","v":0},{"$f":"'Individual Spaces'!D262","v":0},{"$f":"'Individual Spaces'!E262","v":0},null,{"$f":"VLOOKUP($B263,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B263,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G262","v":0},{"$f":"'Individual Spaces'!H262","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O262","v":0},{"$f":"'Individual Spaces'!P262","v":0},{"$f":"'Individual Spaces'!Q262","v":0},{"$f":"'Individual Spaces'!R262","v":0},null,0,{"$f":"IF(AF263=\"-\",0,ROUND((J263-VLOOKUP(B263,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B263,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B263,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B263,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J263-VLOOKUP(B263,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B263,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B263,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B263,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B263,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B263,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B263,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B263,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B263,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A263","v":0},{"$f":"'Individual Spaces'!B263","v":0},{"$f":"'Individual Spaces'!C263","v":0},{"$f":"'Individual Spaces'!D263","v":0},{"$f":"'Individual Spaces'!E263","v":0},null,{"$f":"VLOOKUP($B264,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B264,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G263","v":0},{"$f":"'Individual Spaces'!H263","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O263","v":0},{"$f":"'Individual Spaces'!P263","v":0},{"$f":"'Individual Spaces'!Q263","v":0},{"$f":"'Individual Spaces'!R263","v":0},null,0,{"$f":"IF(AF264=\"-\",0,ROUND((J264-VLOOKUP(B264,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B264,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B264,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B264,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J264-VLOOKUP(B264,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B264,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B264,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B264,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B264,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B264,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B264,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B264,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B264,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A264","v":0},{"$f":"'Individual Spaces'!B264","v":0},{"$f":"'Individual Spaces'!C264","v":0},{"$f":"'Individual Spaces'!D264","v":0},{"$f":"'Individual Spaces'!E264","v":0},null,{"$f":"VLOOKUP($B265,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B265,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G264","v":0},{"$f":"'Individual Spaces'!H264","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O264","v":0},{"$f":"'Individual Spaces'!P264","v":0},{"$f":"'Individual Spaces'!Q264","v":0},{"$f":"'Individual Spaces'!R264","v":0},null,0,{"$f":"IF(AF265=\"-\",0,ROUND((J265-VLOOKUP(B265,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B265,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B265,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B265,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J265-VLOOKUP(B265,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B265,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B265,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B265,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B265,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B265,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B265,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B265,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B265,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A265","v":0},{"$f":"'Individual Spaces'!B265","v":0},{"$f":"'Individual Spaces'!C265","v":0},{"$f":"'Individual Spaces'!D265","v":0},{"$f":"'Individual Spaces'!E265","v":0},null,{"$f":"VLOOKUP($B266,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B266,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G265","v":0},{"$f":"'Individual Spaces'!H265","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O265","v":0},{"$f":"'Individual Spaces'!P265","v":0},{"$f":"'Individual Spaces'!Q265","v":0},{"$f":"'Individual Spaces'!R265","v":0},null,0,{"$f":"IF(AF266=\"-\",0,ROUND((J266-VLOOKUP(B266,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B266,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B266,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B266,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J266-VLOOKUP(B266,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B266,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B266,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B266,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B266,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B266,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B266,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B266,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B266,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A266","v":0},{"$f":"'Individual Spaces'!B266","v":0},{"$f":"'Individual Spaces'!C266","v":0},{"$f":"'Individual Spaces'!D266","v":0},{"$f":"'Individual Spaces'!E266","v":0},null,{"$f":"VLOOKUP($B267,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B267,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G266","v":0},{"$f":"'Individual Spaces'!H266","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O266","v":0},{"$f":"'Individual Spaces'!P266","v":0},{"$f":"'Individual Spaces'!Q266","v":0},{"$f":"'Individual Spaces'!R266","v":0},null,0,{"$f":"IF(AF267=\"-\",0,ROUND((J267-VLOOKUP(B267,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B267,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B267,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B267,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J267-VLOOKUP(B267,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B267,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B267,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B267,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B267,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B267,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B267,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B267,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B267,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A267","v":0},{"$f":"'Individual Spaces'!B267","v":0},{"$f":"'Individual Spaces'!C267","v":0},{"$f":"'Individual Spaces'!D267","v":0},{"$f":"'Individual Spaces'!E267","v":0},null,{"$f":"VLOOKUP($B268,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B268,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G267","v":0},{"$f":"'Individual Spaces'!H267","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O267","v":0},{"$f":"'Individual Spaces'!P267","v":0},{"$f":"'Individual Spaces'!Q267","v":0},{"$f":"'Individual Spaces'!R267","v":0},null,0,{"$f":"IF(AF268=\"-\",0,ROUND((J268-VLOOKUP(B268,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B268,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B268,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B268,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J268-VLOOKUP(B268,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B268,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B268,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B268,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B268,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B268,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B268,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B268,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B268,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A268","v":0},{"$f":"'Individual Spaces'!B268","v":0},{"$f":"'Individual Spaces'!C268","v":0},{"$f":"'Individual Spaces'!D268","v":0},{"$f":"'Individual Spaces'!E268","v":0},null,{"$f":"VLOOKUP($B269,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B269,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G268","v":0},{"$f":"'Individual Spaces'!H268","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O268","v":0},{"$f":"'Individual Spaces'!P268","v":0},{"$f":"'Individual Spaces'!Q268","v":0},{"$f":"'Individual Spaces'!R268","v":0},null,0,{"$f":"IF(AF269=\"-\",0,ROUND((J269-VLOOKUP(B269,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B269,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B269,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B269,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J269-VLOOKUP(B269,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B269,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B269,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B269,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B269,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B269,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B269,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B269,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B269,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A269","v":0},{"$f":"'Individual Spaces'!B269","v":0},{"$f":"'Individual Spaces'!C269","v":0},{"$f":"'Individual Spaces'!D269","v":0},{"$f":"'Individual Spaces'!E269","v":0},null,{"$f":"VLOOKUP($B270,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B270,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G269","v":0},{"$f":"'Individual Spaces'!H269","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O269","v":0},{"$f":"'Individual Spaces'!P269","v":0},{"$f":"'Individual Spaces'!Q269","v":0},{"$f":"'Individual Spaces'!R269","v":0},null,0,{"$f":"IF(AF270=\"-\",0,ROUND((J270-VLOOKUP(B270,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B270,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B270,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B270,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J270-VLOOKUP(B270,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B270,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B270,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B270,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B270,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B270,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B270,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B270,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B270,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A270","v":0},{"$f":"'Individual Spaces'!B270","v":0},{"$f":"'Individual Spaces'!C270","v":0},{"$f":"'Individual Spaces'!D270","v":0},{"$f":"'Individual Spaces'!E270","v":0},null,{"$f":"VLOOKUP($B271,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B271,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G270","v":0},{"$f":"'Individual Spaces'!H270","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O270","v":0},{"$f":"'Individual Spaces'!P270","v":0},{"$f":"'Individual Spaces'!Q270","v":0},{"$f":"'Individual Spaces'!R270","v":0},null,0,{"$f":"IF(AF271=\"-\",0,ROUND((J271-VLOOKUP(B271,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B271,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B271,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B271,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J271-VLOOKUP(B271,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B271,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B271,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B271,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B271,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B271,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B271,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B271,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B271,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A271","v":0},{"$f":"'Individual Spaces'!B271","v":0},{"$f":"'Individual Spaces'!C271","v":0},{"$f":"'Individual Spaces'!D271","v":0},{"$f":"'Individual Spaces'!E271","v":0},null,{"$f":"VLOOKUP($B272,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B272,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G271","v":0},{"$f":"'Individual Spaces'!H271","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O271","v":0},{"$f":"'Individual Spaces'!P271","v":0},{"$f":"'Individual Spaces'!Q271","v":0},{"$f":"'Individual Spaces'!R271","v":0},null,0,{"$f":"IF(AF272=\"-\",0,ROUND((J272-VLOOKUP(B272,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B272,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B272,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B272,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J272-VLOOKUP(B272,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B272,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B272,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B272,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B272,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B272,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B272,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B272,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B272,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A272","v":0},{"$f":"'Individual Spaces'!B272","v":0},{"$f":"'Individual Spaces'!C272","v":0},{"$f":"'Individual Spaces'!D272","v":0},{"$f":"'Individual Spaces'!E272","v":0},null,{"$f":"VLOOKUP($B273,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B273,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G272","v":0},{"$f":"'Individual Spaces'!H272","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O272","v":0},{"$f":"'Individual Spaces'!P272","v":0},{"$f":"'Individual Spaces'!Q272","v":0},{"$f":"'Individual Spaces'!R272","v":0},null,0,{"$f":"IF(AF273=\"-\",0,ROUND((J273-VLOOKUP(B273,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B273,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B273,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B273,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J273-VLOOKUP(B273,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B273,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B273,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B273,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B273,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B273,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B273,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B273,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B273,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A273","v":0},{"$f":"'Individual Spaces'!B273","v":0},{"$f":"'Individual Spaces'!C273","v":0},{"$f":"'Individual Spaces'!D273","v":0},{"$f":"'Individual Spaces'!E273","v":0},null,{"$f":"VLOOKUP($B274,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B274,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G273","v":0},{"$f":"'Individual Spaces'!H273","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O273","v":0},{"$f":"'Individual Spaces'!P273","v":0},{"$f":"'Individual Spaces'!Q273","v":0},{"$f":"'Individual Spaces'!R273","v":0},null,0,{"$f":"IF(AF274=\"-\",0,ROUND((J274-VLOOKUP(B274,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B274,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B274,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B274,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J274-VLOOKUP(B274,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B274,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B274,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B274,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B274,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B274,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B274,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B274,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B274,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A274","v":0},{"$f":"'Individual Spaces'!B274","v":0},{"$f":"'Individual Spaces'!C274","v":0},{"$f":"'Individual Spaces'!D274","v":0},{"$f":"'Individual Spaces'!E274","v":0},null,{"$f":"VLOOKUP($B275,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B275,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G274","v":0},{"$f":"'Individual Spaces'!H274","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O274","v":0},{"$f":"'Individual Spaces'!P274","v":0},{"$f":"'Individual Spaces'!Q274","v":0},{"$f":"'Individual Spaces'!R274","v":0},null,0,{"$f":"IF(AF275=\"-\",0,ROUND((J275-VLOOKUP(B275,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B275,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B275,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B275,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J275-VLOOKUP(B275,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B275,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B275,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B275,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B275,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B275,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B275,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B275,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B275,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A275","v":0},{"$f":"'Individual Spaces'!B275","v":0},{"$f":"'Individual Spaces'!C275","v":0},{"$f":"'Individual Spaces'!D275","v":0},{"$f":"'Individual Spaces'!E275","v":0},null,{"$f":"VLOOKUP($B276,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B276,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G275","v":0},{"$f":"'Individual Spaces'!H275","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O275","v":0},{"$f":"'Individual Spaces'!P275","v":0},{"$f":"'Individual Spaces'!Q275","v":0},{"$f":"'Individual Spaces'!R275","v":0},null,0,{"$f":"IF(AF276=\"-\",0,ROUND((J276-VLOOKUP(B276,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B276,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B276,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B276,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J276-VLOOKUP(B276,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B276,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B276,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B276,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B276,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B276,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B276,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B276,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B276,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A276","v":0},{"$f":"'Individual Spaces'!B276","v":0},{"$f":"'Individual Spaces'!C276","v":0},{"$f":"'Individual Spaces'!D276","v":0},{"$f":"'Individual Spaces'!E276","v":0},null,{"$f":"VLOOKUP($B277,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B277,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G276","v":0},{"$f":"'Individual Spaces'!H276","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O276","v":0},{"$f":"'Individual Spaces'!P276","v":0},{"$f":"'Individual Spaces'!Q276","v":0},{"$f":"'Individual Spaces'!R276","v":0},null,0,{"$f":"IF(AF277=\"-\",0,ROUND((J277-VLOOKUP(B277,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B277,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B277,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B277,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J277-VLOOKUP(B277,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B277,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B277,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B277,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B277,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B277,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B277,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B277,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B277,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A277","v":0},{"$f":"'Individual Spaces'!B277","v":0},{"$f":"'Individual Spaces'!C277","v":0},{"$f":"'Individual Spaces'!D277","v":0},{"$f":"'Individual Spaces'!E277","v":0},null,{"$f":"VLOOKUP($B278,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B278,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G277","v":0},{"$f":"'Individual Spaces'!H277","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O277","v":0},{"$f":"'Individual Spaces'!P277","v":0},{"$f":"'Individual Spaces'!Q277","v":0},{"$f":"'Individual Spaces'!R277","v":0},null,0,{"$f":"IF(AF278=\"-\",0,ROUND((J278-VLOOKUP(B278,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B278,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B278,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B278,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J278-VLOOKUP(B278,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B278,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B278,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B278,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B278,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B278,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B278,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B278,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B278,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A278","v":0},{"$f":"'Individual Spaces'!B278","v":0},{"$f":"'Individual Spaces'!C278","v":0},{"$f":"'Individual Spaces'!D278","v":0},{"$f":"'Individual Spaces'!E278","v":0},null,{"$f":"VLOOKUP($B279,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B279,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G278","v":0},{"$f":"'Individual Spaces'!H278","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O278","v":0},{"$f":"'Individual Spaces'!P278","v":0},{"$f":"'Individual Spaces'!Q278","v":0},{"$f":"'Individual Spaces'!R278","v":0},null,0,{"$f":"IF(AF279=\"-\",0,ROUND((J279-VLOOKUP(B279,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B279,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B279,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B279,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J279-VLOOKUP(B279,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B279,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B279,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B279,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B279,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B279,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B279,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B279,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B279,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A279","v":0},{"$f":"'Individual Spaces'!B279","v":0},{"$f":"'Individual Spaces'!C279","v":0},{"$f":"'Individual Spaces'!D279","v":0},{"$f":"'Individual Spaces'!E279","v":0},null,{"$f":"VLOOKUP($B280,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B280,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G279","v":0},{"$f":"'Individual Spaces'!H279","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O279","v":0},{"$f":"'Individual Spaces'!P279","v":0},{"$f":"'Individual Spaces'!Q279","v":0},{"$f":"'Individual Spaces'!R279","v":0},null,0,{"$f":"IF(AF280=\"-\",0,ROUND((J280-VLOOKUP(B280,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B280,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B280,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B280,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J280-VLOOKUP(B280,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B280,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B280,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B280,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B280,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B280,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B280,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B280,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B280,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A280","v":0},{"$f":"'Individual Spaces'!B280","v":0},{"$f":"'Individual Spaces'!C280","v":0},{"$f":"'Individual Spaces'!D280","v":0},{"$f":"'Individual Spaces'!E280","v":0},null,{"$f":"VLOOKUP($B281,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B281,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G280","v":0},{"$f":"'Individual Spaces'!H280","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O280","v":0},{"$f":"'Individual Spaces'!P280","v":0},{"$f":"'Individual Spaces'!Q280","v":0},{"$f":"'Individual Spaces'!R280","v":0},null,0,{"$f":"IF(AF281=\"-\",0,ROUND((J281-VLOOKUP(B281,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B281,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B281,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B281,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J281-VLOOKUP(B281,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B281,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B281,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B281,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B281,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B281,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B281,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B281,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B281,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A281","v":0},{"$f":"'Individual Spaces'!B281","v":0},{"$f":"'Individual Spaces'!C281","v":0},{"$f":"'Individual Spaces'!D281","v":0},{"$f":"'Individual Spaces'!E281","v":0},null,{"$f":"VLOOKUP($B282,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B282,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G281","v":0},{"$f":"'Individual Spaces'!H281","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O281","v":0},{"$f":"'Individual Spaces'!P281","v":0},{"$f":"'Individual Spaces'!Q281","v":0},{"$f":"'Individual Spaces'!R281","v":0},null,0,{"$f":"IF(AF282=\"-\",0,ROUND((J282-VLOOKUP(B282,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B282,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B282,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B282,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J282-VLOOKUP(B282,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B282,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B282,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B282,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B282,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B282,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B282,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B282,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B282,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A282","v":0},{"$f":"'Individual Spaces'!B282","v":0},{"$f":"'Individual Spaces'!C282","v":0},{"$f":"'Individual Spaces'!D282","v":0},{"$f":"'Individual Spaces'!E282","v":0},null,{"$f":"VLOOKUP($B283,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B283,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G282","v":0},{"$f":"'Individual Spaces'!H282","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O282","v":0},{"$f":"'Individual Spaces'!P282","v":0},{"$f":"'Individual Spaces'!Q282","v":0},{"$f":"'Individual Spaces'!R282","v":0},null,0,{"$f":"IF(AF283=\"-\",0,ROUND((J283-VLOOKUP(B283,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B283,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B283,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B283,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J283-VLOOKUP(B283,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B283,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B283,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B283,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B283,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B283,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B283,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B283,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B283,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A283","v":0},{"$f":"'Individual Spaces'!B283","v":0},{"$f":"'Individual Spaces'!C283","v":0},{"$f":"'Individual Spaces'!D283","v":0},{"$f":"'Individual Spaces'!E283","v":0},null,{"$f":"VLOOKUP($B284,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B284,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G283","v":0},{"$f":"'Individual Spaces'!H283","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O283","v":0},{"$f":"'Individual Spaces'!P283","v":0},{"$f":"'Individual Spaces'!Q283","v":0},{"$f":"'Individual Spaces'!R283","v":0},null,0,{"$f":"IF(AF284=\"-\",0,ROUND((J284-VLOOKUP(B284,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B284,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B284,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B284,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J284-VLOOKUP(B284,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B284,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B284,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B284,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B284,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B284,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B284,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B284,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B284,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A284","v":0},{"$f":"'Individual Spaces'!B284","v":0},{"$f":"'Individual Spaces'!C284","v":0},{"$f":"'Individual Spaces'!D284","v":0},{"$f":"'Individual Spaces'!E284","v":0},null,{"$f":"VLOOKUP($B285,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B285,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G284","v":0},{"$f":"'Individual Spaces'!H284","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O284","v":0},{"$f":"'Individual Spaces'!P284","v":0},{"$f":"'Individual Spaces'!Q284","v":0},{"$f":"'Individual Spaces'!R284","v":0},null,0,{"$f":"IF(AF285=\"-\",0,ROUND((J285-VLOOKUP(B285,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B285,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B285,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B285,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J285-VLOOKUP(B285,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B285,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B285,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B285,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B285,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B285,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B285,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B285,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B285,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A285","v":0},{"$f":"'Individual Spaces'!B285","v":0},{"$f":"'Individual Spaces'!C285","v":0},{"$f":"'Individual Spaces'!D285","v":0},{"$f":"'Individual Spaces'!E285","v":0},null,{"$f":"VLOOKUP($B286,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B286,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G285","v":0},{"$f":"'Individual Spaces'!H285","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O285","v":0},{"$f":"'Individual Spaces'!P285","v":0},{"$f":"'Individual Spaces'!Q285","v":0},{"$f":"'Individual Spaces'!R285","v":0},null,0,{"$f":"IF(AF286=\"-\",0,ROUND((J286-VLOOKUP(B286,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B286,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B286,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B286,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J286-VLOOKUP(B286,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B286,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B286,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B286,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B286,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B286,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B286,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B286,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B286,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A286","v":0},{"$f":"'Individual Spaces'!B286","v":0},{"$f":"'Individual Spaces'!C286","v":0},{"$f":"'Individual Spaces'!D286","v":0},{"$f":"'Individual Spaces'!E286","v":0},null,{"$f":"VLOOKUP($B287,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B287,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G286","v":0},{"$f":"'Individual Spaces'!H286","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O286","v":0},{"$f":"'Individual Spaces'!P286","v":0},{"$f":"'Individual Spaces'!Q286","v":0},{"$f":"'Individual Spaces'!R286","v":0},null,0,{"$f":"IF(AF287=\"-\",0,ROUND((J287-VLOOKUP(B287,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B287,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B287,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B287,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J287-VLOOKUP(B287,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B287,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B287,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B287,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B287,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B287,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B287,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B287,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B287,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A287","v":0},{"$f":"'Individual Spaces'!B287","v":0},{"$f":"'Individual Spaces'!C287","v":0},{"$f":"'Individual Spaces'!D287","v":0},{"$f":"'Individual Spaces'!E287","v":0},null,{"$f":"VLOOKUP($B288,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B288,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G287","v":0},{"$f":"'Individual Spaces'!H287","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O287","v":0},{"$f":"'Individual Spaces'!P287","v":0},{"$f":"'Individual Spaces'!Q287","v":0},{"$f":"'Individual Spaces'!R287","v":0},null,0,{"$f":"IF(AF288=\"-\",0,ROUND((J288-VLOOKUP(B288,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B288,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B288,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B288,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J288-VLOOKUP(B288,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B288,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B288,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B288,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B288,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B288,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B288,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B288,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B288,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A288","v":0},{"$f":"'Individual Spaces'!B288","v":0},{"$f":"'Individual Spaces'!C288","v":0},{"$f":"'Individual Spaces'!D288","v":0},{"$f":"'Individual Spaces'!E288","v":0},null,{"$f":"VLOOKUP($B289,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B289,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G288","v":0},{"$f":"'Individual Spaces'!H288","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O288","v":0},{"$f":"'Individual Spaces'!P288","v":0},{"$f":"'Individual Spaces'!Q288","v":0},{"$f":"'Individual Spaces'!R288","v":0},null,0,{"$f":"IF(AF289=\"-\",0,ROUND((J289-VLOOKUP(B289,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B289,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B289,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B289,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J289-VLOOKUP(B289,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B289,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B289,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B289,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B289,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B289,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B289,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B289,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B289,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A289","v":0},{"$f":"'Individual Spaces'!B289","v":0},{"$f":"'Individual Spaces'!C289","v":0},{"$f":"'Individual Spaces'!D289","v":0},{"$f":"'Individual Spaces'!E289","v":0},null,{"$f":"VLOOKUP($B290,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B290,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G289","v":0},{"$f":"'Individual Spaces'!H289","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O289","v":0},{"$f":"'Individual Spaces'!P289","v":0},{"$f":"'Individual Spaces'!Q289","v":0},{"$f":"'Individual Spaces'!R289","v":0},null,0,{"$f":"IF(AF290=\"-\",0,ROUND((J290-VLOOKUP(B290,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B290,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B290,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B290,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J290-VLOOKUP(B290,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B290,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B290,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B290,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B290,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B290,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B290,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B290,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B290,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A290","v":0},{"$f":"'Individual Spaces'!B290","v":0},{"$f":"'Individual Spaces'!C290","v":0},{"$f":"'Individual Spaces'!D290","v":0},{"$f":"'Individual Spaces'!E290","v":0},null,{"$f":"VLOOKUP($B291,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B291,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G290","v":0},{"$f":"'Individual Spaces'!H290","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O290","v":0},{"$f":"'Individual Spaces'!P290","v":0},{"$f":"'Individual Spaces'!Q290","v":0},{"$f":"'Individual Spaces'!R290","v":0},null,0,{"$f":"IF(AF291=\"-\",0,ROUND((J291-VLOOKUP(B291,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B291,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B291,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B291,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J291-VLOOKUP(B291,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B291,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B291,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B291,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B291,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B291,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B291,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B291,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B291,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A291","v":0},{"$f":"'Individual Spaces'!B291","v":0},{"$f":"'Individual Spaces'!C291","v":0},{"$f":"'Individual Spaces'!D291","v":0},{"$f":"'Individual Spaces'!E291","v":0},null,{"$f":"VLOOKUP($B292,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B292,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G291","v":0},{"$f":"'Individual Spaces'!H291","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O291","v":0},{"$f":"'Individual Spaces'!P291","v":0},{"$f":"'Individual Spaces'!Q291","v":0},{"$f":"'Individual Spaces'!R291","v":0},null,0,{"$f":"IF(AF292=\"-\",0,ROUND((J292-VLOOKUP(B292,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B292,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B292,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B292,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J292-VLOOKUP(B292,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B292,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B292,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B292,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B292,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B292,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B292,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B292,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B292,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A292","v":0},{"$f":"'Individual Spaces'!B292","v":0},{"$f":"'Individual Spaces'!C292","v":0},{"$f":"'Individual Spaces'!D292","v":0},{"$f":"'Individual Spaces'!E292","v":0},null,{"$f":"VLOOKUP($B293,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B293,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G292","v":0},{"$f":"'Individual Spaces'!H292","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O292","v":0},{"$f":"'Individual Spaces'!P292","v":0},{"$f":"'Individual Spaces'!Q292","v":0},{"$f":"'Individual Spaces'!R292","v":0},null,0,{"$f":"IF(AF293=\"-\",0,ROUND((J293-VLOOKUP(B293,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B293,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B293,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B293,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J293-VLOOKUP(B293,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B293,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B293,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B293,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B293,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B293,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B293,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B293,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B293,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A293","v":0},{"$f":"'Individual Spaces'!B293","v":0},{"$f":"'Individual Spaces'!C293","v":0},{"$f":"'Individual Spaces'!D293","v":0},{"$f":"'Individual Spaces'!E293","v":0},null,{"$f":"VLOOKUP($B294,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B294,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G293","v":0},{"$f":"'Individual Spaces'!H293","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O293","v":0},{"$f":"'Individual Spaces'!P293","v":0},{"$f":"'Individual Spaces'!Q293","v":0},{"$f":"'Individual Spaces'!R293","v":0},null,0,{"$f":"IF(AF294=\"-\",0,ROUND((J294-VLOOKUP(B294,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B294,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B294,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B294,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J294-VLOOKUP(B294,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B294,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B294,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B294,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B294,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B294,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B294,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B294,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B294,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A294","v":0},{"$f":"'Individual Spaces'!B294","v":0},{"$f":"'Individual Spaces'!C294","v":0},{"$f":"'Individual Spaces'!D294","v":0},{"$f":"'Individual Spaces'!E294","v":0},null,{"$f":"VLOOKUP($B295,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B295,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G294","v":0},{"$f":"'Individual Spaces'!H294","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O294","v":0},{"$f":"'Individual Spaces'!P294","v":0},{"$f":"'Individual Spaces'!Q294","v":0},{"$f":"'Individual Spaces'!R294","v":0},null,0,{"$f":"IF(AF295=\"-\",0,ROUND((J295-VLOOKUP(B295,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B295,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B295,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B295,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J295-VLOOKUP(B295,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B295,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B295,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B295,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B295,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B295,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B295,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B295,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B295,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A295","v":0},{"$f":"'Individual Spaces'!B295","v":0},{"$f":"'Individual Spaces'!C295","v":0},{"$f":"'Individual Spaces'!D295","v":0},{"$f":"'Individual Spaces'!E295","v":0},null,{"$f":"VLOOKUP($B296,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B296,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G295","v":0},{"$f":"'Individual Spaces'!H295","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O295","v":0},{"$f":"'Individual Spaces'!P295","v":0},{"$f":"'Individual Spaces'!Q295","v":0},{"$f":"'Individual Spaces'!R295","v":0},null,0,{"$f":"IF(AF296=\"-\",0,ROUND((J296-VLOOKUP(B296,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B296,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B296,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B296,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J296-VLOOKUP(B296,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B296,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B296,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B296,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B296,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B296,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B296,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B296,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B296,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A296","v":0},{"$f":"'Individual Spaces'!B296","v":0},{"$f":"'Individual Spaces'!C296","v":0},{"$f":"'Individual Spaces'!D296","v":0},{"$f":"'Individual Spaces'!E296","v":0},null,{"$f":"VLOOKUP($B297,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B297,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G296","v":0},{"$f":"'Individual Spaces'!H296","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O296","v":0},{"$f":"'Individual Spaces'!P296","v":0},{"$f":"'Individual Spaces'!Q296","v":0},{"$f":"'Individual Spaces'!R296","v":0},null,0,{"$f":"IF(AF297=\"-\",0,ROUND((J297-VLOOKUP(B297,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B297,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B297,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B297,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J297-VLOOKUP(B297,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B297,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B297,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B297,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B297,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B297,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B297,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B297,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B297,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A297","v":0},{"$f":"'Individual Spaces'!B297","v":0},{"$f":"'Individual Spaces'!C297","v":0},{"$f":"'Individual Spaces'!D297","v":0},{"$f":"'Individual Spaces'!E297","v":0},null,{"$f":"VLOOKUP($B298,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B298,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G297","v":0},{"$f":"'Individual Spaces'!H297","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O297","v":0},{"$f":"'Individual Spaces'!P297","v":0},{"$f":"'Individual Spaces'!Q297","v":0},{"$f":"'Individual Spaces'!R297","v":0},null,0,{"$f":"IF(AF298=\"-\",0,ROUND((J298-VLOOKUP(B298,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B298,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B298,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B298,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J298-VLOOKUP(B298,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B298,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B298,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B298,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B298,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B298,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B298,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B298,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B298,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A298","v":0},{"$f":"'Individual Spaces'!B298","v":0},{"$f":"'Individual Spaces'!C298","v":0},{"$f":"'Individual Spaces'!D298","v":0},{"$f":"'Individual Spaces'!E298","v":0},null,{"$f":"VLOOKUP($B299,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B299,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G298","v":0},{"$f":"'Individual Spaces'!H298","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O298","v":0},{"$f":"'Individual Spaces'!P298","v":0},{"$f":"'Individual Spaces'!Q298","v":0},{"$f":"'Individual Spaces'!R298","v":0},null,0,{"$f":"IF(AF299=\"-\",0,ROUND((J299-VLOOKUP(B299,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B299,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B299,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B299,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J299-VLOOKUP(B299,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B299,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B299,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B299,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B299,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B299,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B299,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B299,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B299,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]
[{"$f":"'Individual Spaces'!A299","v":0},{"$f":"'Individual Spaces'!B299","v":0},{"$f":"'Individual Spaces'!C299","v":0},{"$f":"'Individual Spaces'!D299","v":0},{"$f":"'Individual Spaces'!E299","v":0},null,{"$f":"VLOOKUP($B300,'Data Library'!$1:$522,MATCH(G$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B300,'Data Library'!$1:$522,MATCH(H$2,'Data Library'!$1:$1,0),0)","v":"-"},{"$f":"'Individual Spaces'!G299","v":0},{"$f":"'Individual Spaces'!H299","v":0},null,null,null,0,null,null,{"$f":"'Individual Spaces'!O299","v":0},{"$f":"'Individual Spaces'!P299","v":0},{"$f":"'Individual Spaces'!Q299","v":0},{"$f":"'Individual Spaces'!R299","v":0},null,0,{"$f":"IF(AF300=\"-\",0,ROUND((J300-VLOOKUP(B300,'Prog Assums'!$AP$7:$AU$292,4,FALSE))/VLOOKUP(B300,'Prog Assums'!$AP$7:$AU$292,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(B300,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=1,1,IF(VLOOKUP(B300,'Prog Assums'!$AP$7:$AW$292,7,FALSE)=0,0,ROUND((J300-VLOOKUP(B300,'Prog Assums'!$AP$7:$AW$292,6,FALSE))/VLOOKUP(B300,'Prog Assums'!$AP$7:$AW$292,7,FALSE),0)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"VLOOKUP($B300,'Data Library'!$1:$512,MATCH(AB$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B300,'Data Library'!$1:$512,MATCH(AC$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B300,'Data Library'!$1:$512,MATCH(AD$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B300,'Data Library'!$1:$512,MATCH(AE$2,'Data Library'!$1:$1,0),0)","v":0},{"$f":"VLOOKUP($B300,'Prog Assums'!$AP$7:$AV$292,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B300,'Prog Assums'!$AP$7:$AW$292,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($B300,'Data Library'!$1:$512,MATCH(AH$2,'Data Library'!$1:$1,0),0)","v":0}]

{"sheet":"Prog Assums","index":10,"n_rows":305,"n_cols":57,"rows_kept":305,"cut":false,"hidden":false,"merged":[]}
[]
[null,null,null,null,"Programme Assumptions"]
[null,"Drop Down Lists",null,null,"Characteristics",null,null,null,null,null,null,null,null,"space types",null,null,null,null,null,null,null,null,null,null,null,"recom'd zone if:",null,null,null,null,null,null,null,null,null,null,"(for description of space see data library)",null,null,null,null,null,null,null,"group size",null,"staff workstations"]
[null,null,null,null,"age ranges","rec/ KS1","KS2","KS3","KS4","post-16","middle or all-age","net capacity utilisation factor",null,"not including existing space types","zone","net cap","net cap","default size if new","storage (first if DT)","storage for other DT","Final ADS Code","existing","Parent ADS Code","minimum size if refurb",null,"restrictive","standard","extensive","for group of:","if smaller than minimum then:","min possible area","Min rec'd Area if restrictive (or 10%)","Min rec'd Area if standard","Min rec'd Area if extensive","max possible area","if larger than maximum then:","attributes","availability priority category","consequential unavailability ",null,null,"Final ADS Code","Furnished space type (singular)","zone","base area","area/ person","base area","area/ person","Restrictive, standard or extensive","Required Area (m2)","Total data points indicative","WiFi","Power sockets",null,"Maximum group size, as SOA","Number of staff workstations","ER Maximum occupancy"]
[null,"site",null,null,null,null,null,null,null,null,null,null,null,"secondary general ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AR5=\"-\",0,ROUND((AX5-VLOOKUP(AP5,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP5,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP5,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX5-VLOOKUP(AP5,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP5,'Prog Assums'!$AR$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(BC5>200,ROUND(BC5*1.05,0),ROUNDUP(BC5*1.1,0))","v":{"$error":"#N/A"}}]
[null,"sufficient",1,"OK",null,null,4,3,2,null,1,0.75,null,"-","-",null,null,null,null,null,"-",null,"-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-","-","-",null,null,null,0,null,null,null,null,null,null,{"$f":"IF(AR6=\"-\",0,ROUND((AX6-VLOOKUP(AP6,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP6,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(AP6,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX6-VLOOKUP(AP6,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP6,'Prog Assums'!$AR$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(BC6>200,ROUND(BC6*1.05,0),ROUNDUP(BC6*1.1,0))","v":0}]
[null,"restricted",1,"tight",null,null,2,2,null,null,1,0.83,null,{"$f":"IF(C$27=\"extg\",\"Seminar rooms (restrictive, extg)\",\"-\")","v":"Seminar rooms (restrictive, extg)"},"B",1.5,4,37,1,null,"CLA01",1,{"$f":"VLOOKUP(U7,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA02"},{"$f":"ROUND(VLOOKUP(O7,$E$38:$I$54,2,FALSE)+(AC7*VLOOKUP(O7,$E$38:$I$54,3,FALSE)),0)","v":37},"37m2 for 22","B","C","D",22,"group room",25,{"$f":"MINA(AG7*0.9,VLOOKUP(Z7,$E$38:$I$53,2)+(VLOOKUP(Z7,$E$38:$I$53,3,FALSE)*$AC7))","v":36.9},{"$f":"ROUND(VLOOKUP(AA7,$E$38:$I$53,2)+(VLOOKUP(AA7,$E$38:$I$53,3,FALSE)*$AC7),0)","v":41},{"$f":"VLOOKUP(AB7,$E$38:$I$53,2)+(VLOOKUP(AB7,$E$38:$I$53,3,FALSE)*$AC7)","v":46.8},50,"general classroom","existing enclosed","5","none",null,null,"CLA01",{"$f":"IF(C$27=\"extg\",\"Seminar room (restrictive, extg)\",\"-\")","v":"Seminar room (restrictive, extg)"},"B",{"$f":"VLOOKUP($AR7,$E$38:$G$54,2,FALSE)","v":2},{"$f":"VLOOKUP($AR7,$E$38:$G$54,3,FALSE)","v":1.6},null,1,"restrictive",35,10,2,6,null,{"$f":"IF(AX7=\"-\",0,ROUNDDOWN((AX7-VLOOKUP(AP7,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP7,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":20},{"$f":"IF(VLOOKUP(AP7,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX7-VLOOKUP(AP7,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP7,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},22]
[null,"sufficient split (2)",2,"OK","11-14",null,null,3,null,null,null,0.79,null,"Seminar rooms","C",1.5,4,41,1,null,"CLA02",null,{"$f":"VLOOKUP(U8,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA02"},{"$f":"ROUND(VLOOKUP(O8,$E$38:$I$54,2,FALSE)+(AC8*VLOOKUP(O8,$E$38:$I$54,3,FALSE)),0)","v":41},"41m2 for 22","B","C","D","22","group room",25,36.9,41,{"$f":"VLOOKUP(AB8,$E$38:$I$53,2)+(VLOOKUP(AB8,$E$38:$I$53,3,FALSE)*$AC8)","v":46.8},50,"general classroom","enclosed","5","none",null,null,"CLA02","Seminar room","C",4,1.7,null,1,"standard",41,10,2,8,null,{"$f":"IF(AX8=\"-\",0,ROUNDDOWN((AX8-VLOOKUP(AP8,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP8,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":21},{"$f":"IF(VLOOKUP(AP8,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX8-VLOOKUP(AP8,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP8,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},24]
[null,"restricted split (2)",2,"tight","11-16",null,null,3,2,null,null,0.75,null,{"$f":"IF(C$27=\"extg\",\"Seminar rooms (extensive, extg)\",\"-\")","v":"Seminar rooms (extensive, extg)"},"D",1.5,4,48,1,null,"CLA03",1,{"$f":"VLOOKUP(U9,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA02"},47,"48m2 for 22","B","C","D",22,"group room",25,36.9,41,48,50,"general classroom","existing enclosed","5","none",null,null,"CLA03",{"$f":"IF(C$27=\"extg\",\"Seminar room (extensive, extg)\",\"-\")","v":"Seminar room (extensive, extg)"},"D",5,1.9,null,1,"extensive",48,10,2,10,null,{"$f":"IF(AX9=\"-\",0,ROUNDDOWN((AX9-VLOOKUP(AP9,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP9,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":22},{"$f":"IF(VLOOKUP(AP9,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX9-VLOOKUP(AP9,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP9,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},25]
[null,"sufficient split (3)",3,"OK","12-16",null,null,2,2,null,null,0.73,null,{"$f":"IF(C$27=\"extg\",\"Classrooms (restrictive, extg)\",\"-\")","v":"Classrooms (restrictive, extg)"},"B",1.5,4,50,1,null,"CLA11",1,{"$f":"VLOOKUP(U10,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA12"},50,"49.5m2 for 30","B","C","D",30,"seminar room",25,49.5,55,{"$f":"VLOOKUP(AB10,$E$38:$I$53,2)+(VLOOKUP(AB10,$E$38:$I$53,3,FALSE)*$AC10)","v":62},95,"double classroom","existing enclosed","5","none",null,null,"CLA11",{"$f":"IF(C$27=\"extg\",\"Classroom (restrictive, extg)\",\"-\")","v":"Classroom (restrictive, extg)"},"B",2,1.6,null,1,"restrictive",50,9,2,8,null,{"$f":"IF(AX10=\"-\",0,ROUNDDOWN((AX10-VLOOKUP(AP10,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP10,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP10,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX10-VLOOKUP(AP10,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP10,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,"restricted split (3)",3,"tight","13-16",null,null,1,2,null,null,0.72,null,"Classrooms (general)","C",1.5,4,55,1,null,"CLA12",null,{"$f":"VLOOKUP(U11,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA12"},55,"55m2 for 30","B","C","D","30","seminar room",25,49.5,55,62,95,"double classroom","enclosed","5","none",null,null,"CLA12","Classrooms (general)","C",4,1.7,null,1,"standard",55,9,2,8,null,{"$f":"IF(AX11=\"-\",0,ROUNDDOWN((AX11-VLOOKUP(AP11,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP11,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP11,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX11-VLOOKUP(AP11,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP11,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,"sufficient split (4)",4,"OK","14-16",null,null,null,2,null,null,0.69,null,"Classrooms (extensive)","D",1.5,4,62,1,null,"CLA13",null,{"$f":"VLOOKUP(U12,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA12"},62,"62m2 for 30","B","C","D",30,"seminar room",25,49.5,55,62,95,"double classroom","existing enclosed","5","none",null,null,"CLA13","Classrooms (extensive)","D",5,1.9,null,1,"extensive",62,9,2,8,null,{"$f":"IF(AX12=\"-\",0,ROUNDDOWN((AX12-VLOOKUP(AP12,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP12,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP12,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX12-VLOOKUP(AP12,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP12,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,"restricted split (4)",4,"tight","11-18",null,null,3,2,2,null,0.71,null,{"$f":"IF(C$27=\"extg\",\"Classrooms, double (restrictive, extg)\",\"-\")","v":"Classrooms, double (restrictive, extg)"},"B",2.5,-20,97,2,null,"CLA14",1,{"$f":"VLOOKUP(U13,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA15"},98,"95.5m2 for 60","B","C","D",60,"general classroom",72,95.4,106,119,132,"split into more","existing enclosed","5","none",null,null,"CLA14",{"$f":"IF(C$27=\"extg\",\"Classroom, double (restrictive, extg)\",\"-\")","v":"Classroom, double (restrictive, extg)"},"B",2,1.6,null,1,"restrictive",104,20,4,16,null,{"$f":"IF(AX13=\"-\",0,ROUNDDOWN((AX13-VLOOKUP(AP13,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP13,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":63},{"$f":"IF(VLOOKUP(AP13,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX13-VLOOKUP(AP13,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP13,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},70]
[null,null,null,null,"12-18",null,null,2,2,2,null,0.7,null,"Classrooms, double","C",2.5,-20,111,2,null,"CLA15",null,{"$f":"VLOOKUP(U14,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA15"},106,"106m2 for 60","B","C","D","60","general classroom",72,95.4,106,119,132,"split into more","enclosed","5","none",null,null,"CLA15","Classroom, double","C",4,1.7,null,1,"standard",111,20,4,16,null,{"$f":"IF(AX14=\"-\",0,ROUNDDOWN((AX14-VLOOKUP(AP14,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP14,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":62},{"$f":"IF(VLOOKUP(AP14,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX14-VLOOKUP(AP14,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP14,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},69]
[null,null,null,null,"13-18",null,null,1,2,2,null,0.69,null,{"$f":"IF(C$27=\"extg\",\"Classrooms, double (extensive, extg)\",\"-\")","v":"Classrooms, double (extensive, extg)"},"D",2.5,-20,125,2,null,"CLA16",1,{"$f":"VLOOKUP(U15,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA15"},119,"119m2 for 60","B","C","D",60,"general classroom",72,95.4,106,119,132,"split into more","existing enclosed","5","none",null,null,"CLA16",{"$f":"IF(C$27=\"extg\",\"Classroom, double (extensive, extg)\",\"-\")","v":"Classroom, double (extensive, extg)"},"D",5,1.9,null,1,"extensive",125,20,4,16,null,{"$f":"IF(AX15=\"-\",0,ROUNDDOWN((AX15-VLOOKUP(AP15,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP15,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":63},{"$f":"IF(VLOOKUP(AP15,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX15-VLOOKUP(AP15,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP15,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},70]
[null,null,null,null,"14-18",null,null,null,2,2,null,0.67,null,{"$f":"IF(C$27=\"extg\",\"Semi-open classbases, home base (restrictive)\",\"-\")","v":"Semi-open classbases, home base (restrictive)"},"B",1.5,4,50,1,null,"CLA21",1,{"$f":"VLOOKUP(U16,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA22"},50,"50m2 for 30","B","C","D",30,"informal/ small group discussion",25,49.5,55,62,106,"split into more","existing enclosed","5","none",null,null,"CLA21",{"$f":"IF(C$27=\"extg\",\"Semi-open classbase, home base (restrictive)\",\"-\")","v":"Semi-open classbase, home base (restrictive)"},"B",2,1.6,null,1,"restrictive",50,10,2,8,null,{"$f":"IF(AX16=\"-\",0,ROUNDDOWN((AX16-VLOOKUP(AP16,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP16,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP16,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX16-VLOOKUP(AP16,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP16,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,"storeys","storeys",null,"16-18",null,null,null,null,2,null,0.63,null,"Semi-open classbases, home base","C",1.5,4,55,1,null,"CLA22",null,{"$f":"VLOOKUP(U17,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA22"},55,"55m2 for 30","B","C","D","30","informal/ small group discussion",25,49.5,55,62,106,"split into more","semi-open","5","none",null,null,"CLA22","Semi-open classbase, home base","C",4,1.7,null,1,"standard",55,10,4,10,null,{"$f":"IF(AX17=\"-\",0,ROUNDDOWN((AX17-VLOOKUP(AP17,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP17,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP17,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX17-VLOOKUP(AP17,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP17,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Semi-open classbases, home base (extensive)","D",1.5,4,62,1,null,"CLA23",null,{"$f":"VLOOKUP(U18,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA22"},62,"62m2 for 30","B","C","D",30,"informal/ small group discussion",25,49.5,55,62,106,"split into more","semi-open","5","none",null,null,"CLA23","Semi-open classbase, home base (extensive)","D",5,1.9,null,1,"extensive",62,10,6,12,null,{"$f":"IF(AX18=\"-\",0,ROUNDDOWN((AX18-VLOOKUP(AP18,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP18,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP18,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX18-VLOOKUP(AP18,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP18,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,"1 and 2-storey",2,"of net min circulation for 2 storeys",null,null,null,null,null,null,null,null,null,"Secondary SEN classrooms (ambulant)","G",1.5,4,41,1,null,"CLA60",null,{"$f":"VLOOKUP(U19,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA60"},39,"41m2 for 10","F","G","H","10","SEN resource",25,"-","AS SOA","-",75,"split into more","enclosed for SEN pupils",null,null,null,null,"CLA60","Secondary SEN classroom (ambulant)","G",10,2.9,null,1,"standard",34,18,2,16,null,{"$f":"IF(AX19=\"-\",0,ROUNDDOWN((AX19-VLOOKUP(AP19,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP19,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":8},{"$f":"IF(VLOOKUP(AP19,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX19-VLOOKUP(AP19,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP19,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},9]
[null,"2-storey",2,"of net min circulation for 2 storeys",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX20=\"-\",0,ROUNDDOWN((AX20-VLOOKUP(AP20,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP20,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP20,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX20-VLOOKUP(AP20,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP20,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,"3-storey",3,"of net min circulation for 3 storeys",null,null,null,null,null,null,null,null,null,"Classrooms (smaller group)","C",1.5,4,48,1,null,"CLA18",null,{"$f":"VLOOKUP(U21,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA12"},48,"48m2 for 26","B","C","D","26","seminar room",25,{"$f":"MINA(AG21*0.9,VLOOKUP(Z21,$E$38:$I$53,2)+(VLOOKUP(Z21,$E$38:$I$53,3,FALSE)*$AC21))","v":43.2},{"$f":"ROUND(VLOOKUP(AA21,$E$38:$I$53,2)+(VLOOKUP(AA21,$E$38:$I$53,3,FALSE)*$AC21),0)","v":48},{"$f":"VLOOKUP(AB21,$E$38:$I$53,2)+(VLOOKUP(AB21,$E$38:$I$53,3,FALSE)*$AC21)","v":54.4},55,"general classroom","enclosed","5","none",null,null,"CLA18","Classroom (smaller group)","C",{"$f":"VLOOKUP($AR21,$E$38:$G$54,2,FALSE)","v":4},{"$f":"VLOOKUP($AR21,$E$38:$G$54,3,FALSE)","v":1.7},null,1,"standard",48,9,2,8,null,{"$f":"IF(AX21=\"-\",0,ROUNDDOWN((AX21-VLOOKUP(AP21,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP21,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":25},{"$f":"IF(VLOOKUP(AP21,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX21-VLOOKUP(AP21,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP21,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},28]
[null,"4-storey",4,"of net min circulation for 4 storeys",null,null,null,null,null,null,null,null,null,"Classrooms (larger group)","C",1.5,4,62,1,null,"CLA19",null,{"$f":"VLOOKUP(U22,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA12"},62,"62m2 for 34","B","C","D","34","seminar room",25,{"$f":"MINA(AG22*0.9,VLOOKUP(Z22,$E$38:$I$53,2)+(VLOOKUP(Z22,$E$38:$I$53,3,FALSE)*$AC22))","v":55.800000000000004},{"$f":"ROUND(VLOOKUP(AA22,$E$38:$I$53,2)+(VLOOKUP(AA22,$E$38:$I$53,3,FALSE)*$AC22),0)","v":62},{"$f":"VLOOKUP(AB22,$E$38:$I$53,2)+(VLOOKUP(AB22,$E$38:$I$53,3,FALSE)*$AC22)","v":69.599999999999994},95,"double classroom","enclosed","5","none",null,null,"CLA19","Classroom (larger group)","C",{"$f":"VLOOKUP($AR22,$E$38:$G$54,2,FALSE)","v":4},{"$f":"VLOOKUP($AR22,$E$38:$G$54,3,FALSE)","v":1.7},null,1,"standard",62,9,2,8,null,{"$f":"IF(AX22=\"-\",0,ROUNDDOWN((AX22-VLOOKUP(AP22,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP22,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":34},{"$f":"IF(VLOOKUP(AP22,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX22-VLOOKUP(AP22,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP22,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},38]
[null,"5-storey",5,"of net min circulation for 5 storeys",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX23=\"-\",0,ROUNDDOWN((AX23-VLOOKUP(AP23,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP23,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP23,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX23-VLOOKUP(AP23,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP23,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"ICT/ business studies",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX24=\"-\",0,ROUNDDOWN((AX24-VLOOKUP(AP24,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP24,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP24,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX24-VLOOKUP(AP24,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP24,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX25=\"-\",0,ROUNDDOWN((AX25-VLOOKUP(AP25,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP25,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP25,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX25-VLOOKUP(AP25,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP25,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(C$27=\"extg\",\"ICT-rich classrooms (restrictive, extg)\",\"-\")","v":"ICT-rich classrooms (restrictive, extg)"},"C",2,4,55,1,null,"CLA31",1,{"$f":"VLOOKUP(U26,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA32"},55,"55m2 for 30","C","D","E","30","ICT-rich resource",45,{"$f":"MINA(AG26*0.9,VLOOKUP(Z26,$E$38:$I$53,2)+(VLOOKUP(Z26,$E$38:$I$53,3,FALSE)*$AC26))","v":55},{"$f":"ROUND(VLOOKUP(AA26,$E$38:$I$53,2)+(VLOOKUP(AA26,$E$38:$I$53,3,FALSE)*$AC26),0)","v":62},{"$f":"VLOOKUP(AB26,$E$38:$I$53,2)+(VLOOKUP(AB26,$E$38:$I$53,3,FALSE)*$AC26)","v":69},125,"split into more",null,"5","none",null,null,"CLA31",{"$f":"IF(AF$27=\"extg\",\"ICT-rich classroom (restrictive, extg)\",\"-\")","v":"-"},"C",{"$f":"VLOOKUP($AR26,$E$38:$G$54,2,FALSE)","v":4},{"$f":"VLOOKUP($AR26,$E$38:$G$54,3,FALSE)","v":1.7},null,1,"restrictive",55,46,2,20,null,{"$f":"IF(AX26=\"-\",0,ROUNDDOWN((AX26-VLOOKUP(AP26,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP26,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP26,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX26-VLOOKUP(AP26,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP26,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,"existing buildings",{"$f":"IF('Secondary SoA'!AO8=\"extg\",\"extg\",\"\")","v":"extg"},null,null,null,null,null,null,null,null,null,null,"ICT-rich classrooms","D",2,4,69,0.5,null,"CLA32",null,{"$f":"VLOOKUP(U27,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA32"},62,"62m2 for 30","C","D","E","30","ICT-rich resource",45,55,62,69,125,"split into more","enclosed with fixed ICT","5","none",null,null,"CLA32","ICT-rich classroom","D",5,1.9,null,1,"standard",62,46,2,38,null,{"$f":"IF(AX27=\"-\",0,ROUNDDOWN((AX27-VLOOKUP(AP27,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP27,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP27,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX27-VLOOKUP(AP27,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP27,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,"none (all new)",null,null,null,null,null,null,null,null,null,null,null,"ICT-rich classrooms (extensive)","E",2,4,69,0.5,null,"CLA33",null,{"$f":"VLOOKUP(U28,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA32"},69,"69m2 for 30","C","D","E","30","ICT-rich resource",45,55,62,69,125,"split into more",null,"5","none",null,null,"CLA33","ICT-rich classroom (extensive)","E",6,2.1,null,1,"extensive",69,46,2,38,null,{"$f":"IF(AX28=\"-\",0,ROUNDDOWN((AX28-VLOOKUP(AP28,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP28,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP28,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX28-VLOOKUP(AP28,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP28,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,"some retained","extg",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(C$27=\"extg\",\"ICT-rich classrooms, semi-open (restrictive, extg)\",\"-\")","v":"ICT-rich classrooms, semi-open (restrictive, extg)"},"C",2,4,55,0.5,null,"CLA34",1,{"$f":"VLOOKUP(U29,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA35"},55,"55m2 for 30","C","D","E","30","ICT-rich resource",45,55,62,69,125,"split into more",null,"5","none",null,null,"CLA34",{"$f":"IF(C$27=\"extg\",\"ICT-rich classroom, semi-open (restrictive, extg)\",\"-\")","v":"ICT-rich classroom, semi-open (restrictive, extg)"},"C",4,1.7,null,1,"restrictive",55,46,2,20,null,{"$f":"IF(AX29=\"-\",0,ROUNDDOWN((AX29-VLOOKUP(AP29,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP29,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP29,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX29-VLOOKUP(AP29,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP29,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,"some refurb'ed","extg",null,null,null,null,null,null,null,null,null,null,"ICT-rich classrooms, semi-open","D",2,4,62,0.5,null,"CLA35",null,{"$f":"VLOOKUP(U30,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA35"},62,"62m2 for 30","C","D","E","30","ICT-rich resource",45,55,62,69,125,"split into more","semi-open with fixed ICT","5","none",null,null,"CLA35","ICT-rich classroom, semi-open","D",5,1.9,null,1,"standard",62,46,2,38,null,{"$f":"IF(AX30=\"-\",0,ROUNDDOWN((AX30-VLOOKUP(AP30,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP30,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP30,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX30-VLOOKUP(AP30,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP30,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,"all existing","extg",null,null,null,null,null,null,null,null,null,null,"ICT-rich classrooms, semi-open (extensive)","E",2,4,69,0.5,null,"CLA36",null,{"$f":"VLOOKUP(U31,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA35"},69,"69m2 for 30","C","D","E","30","ICT-rich resource",45,55,62,69,125,"split into more",null,"5","none",null,null,"CLA36","ICT-rich classroom, semi-open (extensive)","E",6,2.1,null,1,"extensive",69,46,2,38,null,{"$f":"IF(AX31=\"-\",0,ROUNDDOWN((AX31-VLOOKUP(AP31,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP31,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP31,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX31-VLOOKUP(AP31,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP31,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Classrooms (temporarily ICT-rich)","C",2,4,55,0.5,null,"CLA41",null,{"$f":"VLOOKUP(U32,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA12"},55,"55m2 for 30","C","D","E","30","ICT-rich resource",45,55,62,69,125,"split into more","enclosed with 50% fixed ICT","6","none",null,null,"CLA41","Classroom (temporarily ICT-rich)","C",4,1.7,null,1,"restrictive",55,46,2,38,null,{"$f":"IF(AX32=\"-\",0,ROUNDDOWN((AX32-VLOOKUP(AP32,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP32,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP32,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX32-VLOOKUP(AP32,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP32,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"ICT-rich classrooms (business studies)","D",2,4,69,0.5,null,"CLA42",null,{"$f":"VLOOKUP(U33,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA32"},62,"62m2 for 30","C","D","E","30","ICT-rich resource",45,55,62,69,125,"split into more","enclosed with 50% fixed ICT","6","none",null,null,"CLA42","ICT-rich classroom (business studies)","D",5,1.9,null,1,"standard",62,46,2,38,null,{"$f":"IF(AX33=\"-\",0,ROUNDDOWN((AX33-VLOOKUP(AP33,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP33,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP33,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX33-VLOOKUP(AP33,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP33,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"ICT-rich classrooms (business studies, extensive)","E",2,4,69,0.5,null,"CLA43",null,{"$f":"VLOOKUP(U34,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA32"},69,"69m2 for 30","C","D","E","30","ICT-rich resource",45,55,62,69,125,"split into more",null,"6","none",null,null,"CLA43","ICT-rich classroom (business studies, extensive)","E",6,2.1,null,1,"extensive",69,46,2,38,null,{"$f":"IF(AX34=\"-\",0,ROUNDDOWN((AX34-VLOOKUP(AP34,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP34,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP34,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX34-VLOOKUP(AP34,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP34,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,null,null,null,"recommended area zones (BB103 figure 6)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX35=\"-\",0,ROUNDDOWN((AX35-VLOOKUP(AP35,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP35,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP35,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX35-VLOOKUP(AP35,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP35,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,"existing (if cell AO8=extg)",null,null,null,null,null,null,null,null,null,null,null,"science",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX36=\"-\",0,ROUNDDOWN((AX36-VLOOKUP(AP36,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP36,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP36,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX36-VLOOKUP(AP36,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP36,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,"zone","MIN",null,"MAX",null,null,null,null,null,"-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX37=\"-\",0,ROUNDDOWN((AX37-VLOOKUP(AP37,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP37,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP37,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX37-VLOOKUP(AP37,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP37,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,{"$f":"IF('Secondary SoA'!AO8=\"extg\",\"some retained\",\"\")","v":"some retained"},null,null,"-",0,0,0,0,0,0,null,null,{"$f":"IF(C$27=\"extg\",\"Science studios (restrictive, extg)\",\"-\")","v":"Science studios (restrictive, extg)"},"D",2.5,4,62,5,null,"SCI01",1,{"$f":"VLOOKUP(U38,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SCI02"},{"$f":"ROUND(VLOOKUP(O38,$E$38:$I$54,2,FALSE)+(AC38*VLOOKUP(O38,$E$38:$I$54,3,FALSE)),0)","v":62},"62m2 for 30","D","E","E1",30,"classroom",45,{"$f":"MINA(AG38*0.9,VLOOKUP(Z38,$E$38:$I$53,2)+(VLOOKUP(Z38,$E$38:$I$53,3,FALSE)*$AC38))","v":62},{"$f":"ROUND(VLOOKUP(AA38,$E$38:$I$53,2)+(VLOOKUP(AA38,$E$38:$I$53,3,FALSE)*$AC38),0)","v":69},{"$f":"VLOOKUP(AB38,$E$38:$I$53,2)+(VLOOKUP(AB38,$E$38:$I$53,3,FALSE)*$AC38)","v":76},125,"science large group/ demo",null,"6","none",null,null,"SCI01",{"$f":"IF(C$27=\"extg\",\"Science studio (restrictive, extg)\",\"-\")","v":"Science studio (restrictive, extg)"},"D",{"$f":"VLOOKUP($AR38,$E$38:$G$54,2,FALSE)","v":5},{"$f":"VLOOKUP($AR38,$E$38:$G$54,3,FALSE)","v":1.9},null,1,"restrictive",62,10,2,16,null,{"$f":"IF(AX38=\"-\",0,ROUNDDOWN((AX38-VLOOKUP(AP38,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP38,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP38,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX38-VLOOKUP(AP38,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP38,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,{"$f":"IF('Secondary SoA'!AO8=\"extg\",\"retained\",\"\")","v":"retained"},null,null,"A",2,1.1000000000000001,2,1.6,35,50,null,null,"Science studios","E",2.5,4,69,5,null,"SCI02",null,{"$f":"VLOOKUP(U39,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SCI02"},69,"69m2 for 30","D","E","E1","30","classroom",45,62,69,76,125,"science large group/ demo","less than 50% serviced benches or bollards","5","none",null,null,"SCI02","Science studio","E",6,2.1,null,1,"standard",69,10,2,16,null,{"$f":"IF(AX39=\"-\",0,ROUNDDOWN((AX39-VLOOKUP(AP39,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP39,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP39,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX39-VLOOKUP(AP39,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP39,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,{"$f":"IF('Secondary SoA'!AO8=\"extg\",\"refurb'ed\",\"\")","v":"refurb'ed"},null,null,"B",2,1.6,4,1.7,50,55,null,null,"Science studios (extensive)","E1",2.5,4,76,5,null,"SCI03",null,{"$f":"VLOOKUP(U40,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SCI02"},76,"76m2 for 30","D","E","E1",30,"classroom",45,62,69,76,125,"science large group/ demo",null,"6","none",null,null,"SCI03","Science studio (extensive)","E1",7,2.2999999999999998,null,1,"extensive",76,10,2,24,null,{"$f":"IF(AX40=\"-\",0,ROUNDDOWN((AX40-VLOOKUP(AP40,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP40,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP40,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX40-VLOOKUP(AP40,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP40,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,null,null,null,"C",4,1.7,5,1.9,55,62,null,null,{"$f":"IF(C$27=\"extg\",\"Science laboratories (restrictive, extg)\",\"-\")","v":"Science laboratories (restrictive, extg)"},"E1",2.5,4,76,10,null,"SCI04",1,{"$f":"VLOOKUP(U41,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SCI05"},76,"83m2 for 30","E1","F","F1","30","science studio",45,74.7,83,90,90,"split into more","more than 50% serviced benches or bollards","6","none",null,null,"SCI04",{"$f":"IF(C$27=\"extg\",\"Science laboratory (restrictive, extg)\",\"-\")","v":"Science laboratory (restrictive, extg)"},"E1",7,2.2999999999999998,null,1,"restrictive",76,12,2,24,null,{"$f":"IF(AX41=\"-\",0,ROUNDDOWN((AX41-VLOOKUP(AP41,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP41,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP41,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX41-VLOOKUP(AP41,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP41,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,null,null,null,"D",5,1.9,6,2.1,62,69,null,null,"Science laboratories","F",2.5,4,83,10,null,"SCI05",null,{"$f":"VLOOKUP(U42,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SCI05"},83,"90m2 for 30","E1","F","F1",30,"science studio",45,74.7,83,90,90,"specialist science lab",null,"6","none",null,null,"SCI05","Science laboratory","F",8,2.5,null,1,"standard",83,12,2,24,null,{"$f":"IF(AX42=\"-\",0,ROUNDDOWN((AX42-VLOOKUP(AP42,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP42,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP42,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX42-VLOOKUP(AP42,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP42,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,"curriculum model",null,null,"E",6,2.1,7,2.2999999999999998,69,76,null,null,"Science laboratories (specialist)","F1",2.5,4,97,12,null,"SCI11",null,{"$f":"VLOOKUP(U43,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SCI05"},90,"90m2 for 30","F","F1","G","30","general science lab",45,81,90,97,150,"split into more",null,"6","none",null,null,"SCI11","Science laboratory (specialist)","F1",9,2.7,null,1,"extensive",90,12,2,24,null,{"$f":"IF(AX43=\"-\",0,ROUNDDOWN((AX43-VLOOKUP(AP43,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP43,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP43,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX43-VLOOKUP(AP43,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP43,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,"-",null,null,"E1",7,2.2999999999999998,8,2.5,76,83,null,null,"Science laboratories (chemistry)","F1",2.5,4,97,12,null,"SCI12",null,{"$f":"VLOOKUP(U44,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SCI05"},90,"90m2 for 30","F","F1","G",30,"general science lab",45,81,90,97,150,"split into more","more than 50% serviced benches or bollards","6","none",null,null,"SCI12","Science laboratory (chemistry)","F1",9,2.7,null,1,"extensive",90,12,2,24,null,{"$f":"IF(AX44=\"-\",0,ROUNDDOWN((AX44-VLOOKUP(AP44,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP44,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP44,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX44-VLOOKUP(AP44,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP44,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,"A: vocational",null,null,"F",8,2.5,10,2.9,83,97,null,null,"Science laboratories (biology)","F1",2.5,4,97,12,null,"SCI13",null,{"$f":"VLOOKUP(U45,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SCI05"},90,"90m2 for 30","F","F1","G","30","general science lab",45,81,90,97,150,"split into more",null,"6","none",null,null,"SCI13","Science laboratory (biology)","F1",9,2.7,null,1,"extensive",90,12,2,24,null,{"$f":"IF(AX45=\"-\",0,ROUNDDOWN((AX45-VLOOKUP(AP45,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP45,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP45,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX45-VLOOKUP(AP45,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP45,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,"B: music/ sports",null,null,"F1",9,2.7,10,2.9,90,97,null,null,"Science laboratories (physics)","F1",2.5,4,97,12,null,"SCI14",null,{"$f":"VLOOKUP(U46,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SCI05"},90,"90m2 for 30","F","F1","G",30,"general science lab",45,81,90,97,150,"split into more",null,"6","none",null,null,"SCI14","Science laboratory (physics)","F1",9,2.7,null,1,"extensive",90,12,2,24,null,{"$f":"IF(AX46=\"-\",0,ROUNDDOWN((AX46-VLOOKUP(AP46,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP46,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP46,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX46-VLOOKUP(AP46,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP46,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,"C: typical",null,null,"G",10,2.9,14,3.4,79.599999999999994,95.6,null,null,"Science studios (large group/ demo)","A",2.5,4,69,5,null,"SCI21",null,{"$f":"VLOOKUP(U47,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SCI02"},68,"[69m2 for 30]","-","A","B","60","informal/ small group discussion",45,"-",69,"-",150,"split into more","semi-open","6","none",null,null,"SCI21","Science studio (large group/ demo)","A",2,1.1000000000000001,null,1,"standard",69,10,2,16,null,{"$f":"IF(AX47=\"-\",0,ROUNDDOWN((AX47-VLOOKUP(AP47,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP47,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":60},{"$f":"IF(VLOOKUP(AP47,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX47-VLOOKUP(AP47,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP47,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},66]
[null,"D: academic",null,null,"G1",11,3.1,14,3.4,85.4,95.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX48=\"-\",0,ROUNDDOWN((AX48-VLOOKUP(AP48,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP48,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP48,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX48-VLOOKUP(AP48,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP48,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,"H",14,3.4,18,3.9,95.6,111.6,null,null,"creative arts spaces",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX49=\"-\",0,ROUNDDOWN((AX49-VLOOKUP(AP49,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP49,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP49,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX49-VLOOKUP(AP49,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP49,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,"H1",15,3.7,18,3.9,103.80000000000001,111.6,null,null,"-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX50=\"-\",0,ROUNDDOWN((AX50-VLOOKUP(AP50,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP50,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP50,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX50-VLOOKUP(AP50,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP50,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,"I",18,3.9,24,4.5,111.6,132,null,null,{"$f":"IF(C$27=\"extg\",\"Art rooms (restrictive, extg)\",\"-\")","v":"Art rooms (restrictive, extg)"},"E1",2.5,4,76,10,null,"DAT01",1,{"$f":"VLOOKUP(U51,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT00"},{"$f":"ROUND(VLOOKUP(O51,$E$38:$I$54,2,FALSE)+(AC51*VLOOKUP(O51,$E$38:$I$54,3,FALSE)),0)","v":76},"76m2 for 30","E1","F","G","30","art/ design resource",45,76,{"$f":"ROUND(VLOOKUP(AA51,$E$38:$I$53,2)+(VLOOKUP(AA51,$E$38:$I$53,3,FALSE)*$AC51),0)","v":83},{"$f":"VLOOKUP(AB51,$E$38:$I$53,2)+(VLOOKUP(AB51,$E$38:$I$53,3,FALSE)*$AC51)","v":97},104,"3D art room",null,"6","none",null,null,"DAT01",{"$f":"IF(C$27=\"extg\",\"Art room (restrictive, extg)\",\"-\")","v":"Art room (restrictive, extg)"},"E1",{"$f":"VLOOKUP($AR51,$E$38:$G$54,2,FALSE)","v":7},{"$f":"VLOOKUP($AR51,$E$38:$G$54,3,FALSE)","v":2.2999999999999998},null,1,"restrictive",76,24,2,12,null,{"$f":"IF(AX51=\"-\",0,ROUNDDOWN((AX51-VLOOKUP(AP51,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP51,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP51,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX51-VLOOKUP(AP51,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP51,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,null,null,null,"J",24,4.5,30,5.0999999999999996,105,121.8,null,null,"Art rooms (general)","F",2.5,4,83,10,null,"DAT02",null,{"$f":"VLOOKUP(U52,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT00"},83,"83m2 for 30","E1","F","G","30","art/ design resource",45,{"$f":"MINA(AG52*0.9,VLOOKUP(Z52,$E$38:$I$53,2)+(VLOOKUP(Z52,$E$38:$I$53,3,FALSE)*$AC52))","v":74.7},{"$f":"ROUND(VLOOKUP(AA52,$E$38:$I$53,2)+(VLOOKUP(AA52,$E$38:$I$53,3,FALSE)*$AC52),0)","v":83},97,104,"3D art room","serviced space","6","none",null,null,"DAT02","Art room (general)","F",8,2.5,null,1,"standard",83,24,2,12,null,{"$f":"IF(AX52=\"-\",0,ROUNDDOWN((AX52-VLOOKUP(AP52,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP52,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP52,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX52-VLOOKUP(AP52,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP52,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,null,null,null,"K",4,3.7,14,3.4,null,null,null,null,"Art rooms (3D)","G",2.5,4,97,10,1,"DAT03",null,{"$f":"VLOOKUP(U53,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT00"},97,"97m2 for 30","F1","G","H","30","art room",45,87.3,{"$f":"ROUND(VLOOKUP(AA53,$E$38:$I$53,2)+(VLOOKUP(AA53,$E$38:$I$53,3,FALSE)*$AC53),0)","v":97},116,150,"split into more","serviced space","6","none",null,null,"DAT03","Art room (3D)","G",10,2.9,null,1,"extensive",97,22,2,12,null,{"$f":"IF(AX53=\"-\",0,ROUNDDOWN((AX53-VLOOKUP(AP53,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP53,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP53,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX53-VLOOKUP(AP53,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP53,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,null,null,null,"T",0.5,3,null,null,null,null,null,null,"Art rooms (ceramics)","G",2.5,4,97,10,1,"DAT04",null,{"$f":"VLOOKUP(U54,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT00"},97,"104m2 for 30","F1","G1","H","30","art room",45,90,{"$f":"ROUND(VLOOKUP(AA54,$E$38:$I$53,2)+(VLOOKUP(AA54,$E$38:$I$53,3,FALSE)*$AC54),0)","v":104},116,150,"split into more","serviced space","6","none",null,null,"DAT04","Art room (ceramics)","G1",11,3.1,null,1,"extensive",104,22,2,12,null,{"$f":"IF(AX54=\"-\",0,ROUNDDOWN((AX54-VLOOKUP(AP54,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP54,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP54,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX54-VLOOKUP(AP54,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP54,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Art rooms (textiles)","G1",2.5,4,111,10,null,"DAT05",null,{"$f":"VLOOKUP(U55,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT00"},104,"104m2 for 30","F1","G1","H","30","art room",45,90,{"$f":"ROUND(VLOOKUP(AA55,$E$38:$I$53,2)+(VLOOKUP(AA55,$E$38:$I$53,3,FALSE)*$AC55),0)","v":104},116,150,"split into more","serviced space","6","none",null,null,"DAT05","Art room (textiles)","G1",11,3.1,null,1,"extensive",104,22,2,12,null,{"$f":"IF(AX55=\"-\",0,ROUNDDOWN((AX55-VLOOKUP(AP55,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP55,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP55,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX55-VLOOKUP(AP55,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP55,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,"classroom options",null,null,"FE","min NOR","activity","sports","hall","yrs","with stage","hall dims",null,"Photography studios","F",2.5,4,69,10,null,"DAT15",null,{"$f":"VLOOKUP(U56,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT15"},68,"69m2 for 24","E1","F","G","24","art/ design resource",45,62.1,69,79.599999999999994,125,"split into more","serviced space","6","none",null,null,"DAT15","Photography studio","F",8,2.5,null,1,"standard",69,46,2,38,null,{"$f":"IF(AX56=\"-\",0,ROUNDDOWN((AX56-VLOOKUP(AP56,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP56,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":24},{"$f":"IF(VLOOKUP(AP56,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX56-VLOOKUP(AP56,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP56,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},27]
[null,"all standard except post-16",null,null,null,null,null,null,null,null,"with bleacher",null,null,{"$f":"IF(C$27=\"extg\",\"Music rooms (fitted, restrictive, extg)\",\"-\")","v":"Music rooms (fitted, restrictive, extg)"},"C",2,4,55,5,null,"PER01",1,{"$f":"VLOOKUP(U57,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PER02"},55,"55m2 for 30","C","D","E","30","Music practice/ group room",45,55,{"$f":"ROUND(VLOOKUP(AA57,$E$38:$I$53,2)+(VLOOKUP(AA57,$E$38:$I$53,3,FALSE)*$AC57),0)","v":62},69,75,"music recital room",null,null,null,null,null,"PER01",{"$f":"IF(C$27=\"extg\",\"Music room (fitted, restrictive, extg)\",\"-\")","v":"Music room (fitted, restrictive, extg)"},"C",4,1.7,null,1,"restrictive",55,40,null,12,null,{"$f":"IF(AX57=\"-\",0,ROUNDDOWN((AX57-VLOOKUP(AP57,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP57,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP57,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX57-VLOOKUP(AP57,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP57,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,"some extensive",null,{"$f":"100+(F58*0.1)","v":115},1,150,null,180,169,5,{"$f":"42+(F58/5*J58*1.05*0.63)","v":141.22499999999999},"11.75x14.4",null,"Music rooms (fitted)","D",2,4,62,5,null,"PER02",null,{"$f":"VLOOKUP(U58,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PER02"},62,"62m2 for 30","C","D","E","30","Music practice/ group room",45,55,62,69,75,"music recital room","acoustically discrete","6","none",null,null,"PER02","Music room (fitted)","D",5,1.9,null,1,"standard",62,40,2,12,null,{"$f":"IF(AX58=\"-\",0,ROUNDDOWN((AX58-VLOOKUP(AP58,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP58,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP58,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX58-VLOOKUP(AP58,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP58,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,"some variable",null,{"$f":"100+(F59*0.1)","v":130},2,300,null,306,169,3,{"$f":"42+(F59/5*J59*1.05*0.63)","v":161.07},null,null,"Music rooms (fitted, extensive)","E",2,4,69,5,null,"PER03",null,{"$f":"VLOOKUP(U59,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PER02"},69,"69m2 for 30","C","D","E","30","Music practice/ group room",45,55,62,69,75,"music recital room",null,"6","none",null,null,"PER03","Music room (fitted, extensive)","E",6,2.1,null,1,"extensive",69,40,2,16,null,{"$f":"IF(AX59=\"-\",0,ROUNDDOWN((AX59-VLOOKUP(AP59,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP59,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP59,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX59-VLOOKUP(AP59,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP59,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,null,null,145,3,450,null,306,197,2.5,{"$f":"42+(F60/5*J60*1.05*0.63)","v":190.83750000000001},"11.75x16.8",null,"Music and drama classrooms","F",1.5,4,83,5,null,"PER05",null,{"$f":"VLOOKUP(U60,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PER05"},83,"83m2 for 30","E1","F","G","30","Music room",75,"-",83,"-",150,"hall","acoustically discrete","6","none",null,null,"PER05","Music and drama classroom","F",8,2.5,null,1,"standard",83,10,2,16,null,{"$f":"IF(AX60=\"-\",0,ROUNDDOWN((AX60-VLOOKUP(AP60,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP60,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP60,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX60-VLOOKUP(AP60,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP60,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,null,null,160,4,600,null,504,197,2,{"$f":"42+(F61/5*J61*1.05*0.63)","v":200.76},null,null,"Music and drama classrooms (recital)","F",1.5,4,83,10,null,"PER08",null,{"$f":"VLOOKUP(U61,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PER05"},83,"83m2 for 30","E1","F","G","30","Music room",45,"-",83,"-",150,"hall","high space, acoustically discrete","6","Hall if drama studio used as green room",null,null,"PER08","Music and drama classroom (recital)","F",8,2.5,null,1,"standard",83,8,2,16,null,{"$f":"IF(AX61=\"-\",0,ROUNDDOWN((AX61-VLOOKUP(AP61,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP61,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP61,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX61-VLOOKUP(AP61,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP61,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,null,null,175,5,750,null,504,197,1.5,{"$f":"42+(F62/5*J62*1.05*0.63)","v":190.83750000000001},null,null,"Drama studios","F1",12.5,-20,97,10,null,"PER15",null,{"$f":"VLOOKUP(U62,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PER15"},90,"90m2 for 30","E1","F1","G","30","Extensive classroom",62,"-",90,"-",150,"hall","high space, acoustically discrete","6 or 7 if used for exams","Hall if drama studio used as green room",null,null,"PER15","Drama studio","F1",9,2.7,null,1,"standard",90,8,2,8,null,{"$f":"IF(AX62=\"-\",0,ROUNDDOWN((AX62-VLOOKUP(AP62,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP62,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP62,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX62-VLOOKUP(AP62,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP62,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,"science options",null,190,6,900,120,594,197,1.5,{"$f":"24+(F63/5*J63*1.05*0.58)","v":188.42999999999998},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX63=\"-\",0,ROUNDDOWN((AX63-VLOOKUP(AP63,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP63,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP63,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX63-VLOOKUP(AP63,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP63,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,"all standard labs + post-16",null,205,7,1050,120,594,226,1.5,{"$f":"24+(F64/5*J64*1.05*0.58)","v":215.83499999999998},"11.75x19.2",null,"design technology",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX64=\"-\",0,ROUNDDOWN((AX64-VLOOKUP(AP64,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP64,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP64,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX64-VLOOKUP(AP64,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP64,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,"3 specialist labs",null,220,8,1200,120,594,226,1,170.16,null,null,"-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX65=\"-\",0,ROUNDDOWN((AX65-VLOOKUP(AP65,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP65,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP65,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX65-VLOOKUP(AP65,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP65,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,"1 studio for every 2 spec labs",null,235,9,1350,120,594,226,1,188.42999999999998,null,null,"Hair and beauty training salons","H",2.5,4,69,10,10,"DAT12",null,{"$f":"VLOOKUP(U66,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT12"},{"$f":"ROUND(VLOOKUP(O66,$E$38:$I$54,2,FALSE)+(AC66*VLOOKUP(O66,$E$38:$I$54,3,FALSE)),0)","v":68},"69m2 for 14","G","H","I",16,"classroom",45,"-",69,"-",125,"split into more","serviced space","6","none",null,null,"DAT12","Hair and beauty training salon","H",{"$f":"VLOOKUP($AR66,$E$38:$G$54,2,FALSE)","v":14},{"$f":"VLOOKUP($AR66,$E$38:$G$54,3,FALSE)","v":3.4},null,1,"standard",69,12,2,8,null,{"$f":"IF(AX66=\"-\",0,ROUNDDOWN((AX66-VLOOKUP(AP66,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP66,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":16},{"$f":"IF(VLOOKUP(AP66,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX66-VLOOKUP(AP66,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP66,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},18]
[null,null,null,250,10,1500,120,594,254,1,206.7,"11.75x21.6",null,"DT studios","G",2.5,4,83,5,5,"DAT20",null,{"$f":"VLOOKUP(U67,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT20"},83,"83m2 for up to 24","F1","G","H","25","art/ design resource",45,{"$f":"MINA(AG67*0.9,VLOOKUP(Z67,$E$38:$I$53,2)+(VLOOKUP(Z67,$E$38:$I$53,3,FALSE)*$AC67))","v":74.7},{"$f":"ROUND(VLOOKUP(AA67,$E$38:$I$53,2)+(VLOOKUP(AA67,$E$38:$I$53,3,FALSE)*$AC67),0)","v":83},"-",150,"split into more","serviced space","6","none",null,null,"DAT20","DT studio","G",10,2.9,null,1,"standard",83,46,2,38,null,{"$f":"IF(AX67=\"-\",0,ROUNDDOWN((AX67-VLOOKUP(AP67,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP67,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":25},{"$f":"IF(VLOOKUP(AP67,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX67-VLOOKUP(AP67,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP67,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},28]
[null,"staff room options",null,265,11,1650,120,594,254,1,224.97,null,null,{"$f":"IF(C$27=\"extg\",\"DT studios (graphic products, restrictive, extg)\",\"-\")","v":"DT studios (graphic products, restrictive, extg)"},"F1",2.5,4,76,5,5,"DAT21",1,{"$f":"VLOOKUP(U68,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT20"},77,"76m2 for up to 24","F1","G","H",25,"art/ design resource",45,76,{"$f":"ROUND(VLOOKUP(AA68,$E$38:$I$53,2)+(VLOOKUP(AA68,$E$38:$I$53,3,FALSE)*$AC68),0)","v":83},"-",150,"split into more","serviced space","6","none",null,null,"DAT21",{"$f":"IF(C$27=\"extg\",\"DT studio (graphic products, restrictive, extg)\",\"-\")","v":"DT studio (graphic products, restrictive, extg)"},"F1",9,2.7,null,1,"restrictive",76,46,2,38,null,{"$f":"IF(AX68=\"-\",0,ROUNDDOWN((AX68-VLOOKUP(AP68,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP68,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":24},{"$f":"IF(VLOOKUP(AP68,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX68-VLOOKUP(AP68,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP68,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},27]
[null,"central staff room",null,280,12,1800,120,594,254,1,243.23999999999998,null,null,"DT studios (graphic products)","G",2.5,4,83,5,5,"DAT22",null,{"$f":"VLOOKUP(U69,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT20"},83,"83m2 for up to 24","F1","G","H","25","art/ design resource",45,{"$f":"MINA(AG69*0.9,VLOOKUP(Z69,$E$38:$I$53,2)+(VLOOKUP(Z69,$E$38:$I$53,3,FALSE)*$AC69))","v":74.7},83,"-",150,"split into more","serviced space","6","none",null,null,"DAT22","DT studio (graphic products)","G",10,2.9,null,1,"standard",83,46,2,38,null,{"$f":"IF(AX69=\"-\",0,ROUNDDOWN((AX69-VLOOKUP(AP69,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP69,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":25},{"$f":"IF(VLOOKUP(AP69,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX69-VLOOKUP(AP69,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP69,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},28]
[null,"staff social and work rooms",null,295,13,1950,120,594,282,1,261.51,"11.75x24.0",null,{"$f":"IF(C$27=\"extg\",\"DT studios (textiles, restrictive, extg)\",\"-\")","v":"DT studios (textiles, restrictive, extg)"},"F1",2.5,4,76,10,10,"DAT24",1,{"$f":"VLOOKUP(U70,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT20"},77,"76m2 for up to 24","F1","G","H",25,"art/ design resource",45,74.7,83,"-",150,"split into more","serviced space","6","none",null,null,"DAT24",{"$f":"IF(AF$27=\"extg\",\"DT studio (textiles, restrictive, extg)\",\"-\")","v":"-"},"F1",9,2.7,null,1,"restrictive",76,22,2,38,null,{"$f":"IF(AX70=\"-\",0,ROUNDDOWN((AX70-VLOOKUP(AP70,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP70,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":24},{"$f":"IF(VLOOKUP(AP70,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX70-VLOOKUP(AP70,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP70,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},{"$f":"IF(BC70>200,ROUND(BC70*1.05,0),ROUNDUP(BC70*1.1,0))","v":27}]
[null,"staff work rooms only",null,310,14,2100,120,594,282,1,279.77999999999997,null,null,"DT studios (textiles)","G",2.5,4,83,10,10,"DAT25",null,{"$f":"VLOOKUP(U71,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT20"},83,"83m2 for up to 24","F1","G","H","25","art/ design resource",45,74.7,83,"-",150,"split into more","serviced space","6","none",null,null,"DAT25","DT studio (textiles)","G",10,2.9,null,1,"standard",83,22,2,16,null,{"$f":"IF(AX71=\"-\",0,ROUNDDOWN((AX71-VLOOKUP(AP71,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP71,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":25},{"$f":"IF(VLOOKUP(AP71,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX71-VLOOKUP(AP71,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP71,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},28]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(C$27=\"extg\",\"DT studios (electronics & contol, restrictive, extg)\",\"-\")","v":"DT studios (electronics & contol, restrictive, extg)"},"F1",2.5,4,76,10,10,"DAT27",1,{"$f":"VLOOKUP(U72,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT20"},77,"76m2 for up to 24","F1","G","H",25,"art/ design resource",45,74.7,83,"-",150,"split into more","serviced space","6","none",null,null,"DAT27",{"$f":"IF(C$27=\"extg\",\"DT studio (electronics & contol, restrictive, extg)\",\"-\")","v":"DT studio (electronics & contol, restrictive, extg)"},"F1",9,2.7,null,1,"restrictive",76,31,2,38,null,{"$f":"IF(AX72=\"-\",0,ROUNDDOWN((AX72-VLOOKUP(AP72,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP72,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":24},{"$f":"IF(VLOOKUP(AP72,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX72-VLOOKUP(AP72,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP72,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"DT studios (electronics & control)","G",2.5,4,83,10,10,"DAT28",null,{"$f":"VLOOKUP(U73,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT20"},83,"83m2 for up to 24","F1","G","H","25","art/ design resource",45,74.7,83,"-",150,"split into more","serviced space","6","none",null,null,"DAT28","DT studio (electronics & control)","G",10,2.9,null,1,"standard",83,31,2,38,null,{"$f":"IF(AX73=\"-\",0,ROUNDDOWN((AX73-VLOOKUP(AP73,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP73,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":25},{"$f":"IF(VLOOKUP(AP73,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX73-VLOOKUP(AP73,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP73,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},28]
[null,"reception desk options",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(C$27=\"extg\",\"Food rooms (demonstration, restrictive, extg)\",\"-\")","v":"Food rooms (demonstration, restrictive, extg)"},"E1",3.5,4,62,5,5,"DAT31",1,{"$f":"VLOOKUP(U74,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT35"},62,"62m2 for up to 24","E1","F","H",24,"food store/ prep room",45,62.1,69,"-",97,"food room","serviced space with 1 or 2 cookers","6","none",null,null,"DAT31",{"$f":"IF(C$27=\"extg\",\"Food room (demonstration, restrictive, extg)\",\"-\")","v":"Food room (demonstration, restrictive, extg)"},"E1",7,2.2999999999999998,null,1,"restrictive",62,11,2,10,null,{"$f":"IF(AX74=\"-\",0,ROUNDDOWN((AX74-VLOOKUP(AP74,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP74,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":23},{"$f":"IF(VLOOKUP(AP74,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX74-VLOOKUP(AP74,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP74,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},26]
[null,"office with 2 recep desks",null,null,null,null,null,null,null,null,null,null,null,"Food rooms (demonstration)","F",3.5,4,69,5,5,"DAT32",null,{"$f":"VLOOKUP(U75,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT35"},68,"69m2 for up to 24","E1","F","H","24","food store/ prep room",45,62.1,69,"-",97,"food room","serviced space with 1 or 2 cookers","6","none",null,null,"DAT32","Food room (demonstration)","F",8,2.5,null,1,"standard",69,11,2,10,null,{"$f":"IF(AX75=\"-\",0,ROUNDDOWN((AX75-VLOOKUP(AP75,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP75,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":24},{"$f":"IF(VLOOKUP(AP75,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX75-VLOOKUP(AP75,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP75,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},27]
[null,"office with 1 recep desk only",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(C$27=\"extg\",\"Food rooms (restrictive, extg)\",\"-\")","v":"Food rooms (restrictive, extg)"},"G1",3.5,4,90,10,5,"DAT34",1,{"$f":"VLOOKUP(U76,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT35"},85,"85m2 for up to 24","G1","H","I",24,"food studio",67,85.4,{"$f":"ROUND(VLOOKUP(AA76,$E$38:$I$53,2)+(VLOOKUP(AA76,$E$38:$I$53,3,FALSE)*$AC76),0)","v":96},"-",150,"split into more","heavily serviced with many cookers","6","none",null,null,"DAT34",{"$f":"IF(C$27=\"extg\",\"Food room (restrictive, extg)\",\"-\")","v":"Food room (restrictive, extg)"},"G1",11,3.1,null,1,"restrictive",87,13,2,10,null,{"$f":"IF(AX76=\"-\",0,ROUNDDOWN((AX76-VLOOKUP(AP76,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP76,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":24},{"$f":"IF(VLOOKUP(AP76,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX76-VLOOKUP(AP76,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP76,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},27]
[null,"office and finance/student support",null,null,null,null,null,null,null,null,null,null,null,"Food rooms","H",3.5,4,97,10,5,"DAT35",null,{"$f":"VLOOKUP(U77,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT35"},96,"97m2 for up to 24","G1","H","I","24","food studio",67,85.4,97,"-",150,"split into more","heavily serviced with many cookers","6","none",null,null,"DAT35","Food room","H",14,3.4,null,1,"standard",104,13,2,16,null,{"$f":"IF(AX77=\"-\",0,ROUNDDOWN((AX77-VLOOKUP(AP77,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP77,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":26},{"$f":"IF(VLOOKUP(AP77,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX77-VLOOKUP(AP77,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP77,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},29]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(C$27=\"extg\",\"Food rooms (existing for 20)\",\"-\")","v":"Food rooms (existing for 20)"},"H1",3.5,4,97,10,5,"DAT36",1,{"$f":"VLOOKUP(U78,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT35"},89,"89m2 for up to 20","G1","H1","I",20,"food studio",67,73,{"$f":"ROUND(VLOOKUP(AA78,$E$38:$I$53,2)+(VLOOKUP(AA78,$E$38:$I$53,3,FALSE)*$AC78),0)","v":89},"-",150,"split into more","heavily serviced with many cookers","6","none",null,null,"DAT36",{"$f":"IF(C$27=\"extg\",\"Food room (existing for 20)\",\"-\")","v":"Food room (existing for 20)"},"H1",15,3.7,null,1,"standard",90,13,2,16,null,{"$f":"IF(AX78=\"-\",0,ROUNDDOWN((AX78-VLOOKUP(AP78,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP78,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":20},{"$f":"IF(VLOOKUP(AP78,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX78-VLOOKUP(AP78,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP78,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},22]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Food rooms (2 of 2)","H",3.5,4,97,10,5,"DAT37",null,{"$f":"VLOOKUP(U79,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT35"},96,"97m2 for up to 24","G1","H","I",24,"food studio",67,85.4,97,"-",150,"split into more","heavily serviced with many cookers","6","none",null,null,"DAT37","Food room (2 of 2)","H",14,3.4,null,1,"standard",97,13,2,16,null,{"$f":"IF(AX79=\"-\",0,ROUNDDOWN((AX79-VLOOKUP(AP79,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP79,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":24},{"$f":"IF(VLOOKUP(AP79,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX79-VLOOKUP(AP79,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP79,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Catering training kitchens","H1",3.5,4,97,10,5,"DAT39",null,{"$f":"VLOOKUP(U80,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT39"},104,"104m2 for up to 24","G1","H1","I","24","food studio",67,85.4,{"$f":"ROUND(VLOOKUP(AA80,$E$38:$I$53,2)+(VLOOKUP(AA80,$E$38:$I$53,3,FALSE)*$AC80),0)","v":104},"-",150,"split into more","specially serviced workstations","6","none",null,null,"DAT39","Catering training kitchen","H1",15,3.7,null,1,"standard",90,7,2,16,null,{"$f":"IF(AX80=\"-\",0,ROUNDDOWN((AX80-VLOOKUP(AP80,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP80,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":20},{"$f":"IF(VLOOKUP(AP80,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX80-VLOOKUP(AP80,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP80,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},22]
[null,"SEN resourced provision",null,null,"min net",null,"min gross",null,"max net",null,"max gross",null,null,{"$f":"IF(C$27=\"extg\",\"DT workshops (existing for 20)\",\"-\")","v":"DT workshops (existing for 20)"},"H1",3.5,4,97,34,7,"DAT41",1,{"$f":"VLOOKUP(U81,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT43"},89,"82m2 for up to 20","G1","H","I","20","art/ design resource",67,73,{"$f":"ROUND(VLOOKUP(AA81,$E$38:$I$53,2)+(VLOOKUP(AA81,$E$38:$I$53,3,FALSE)*$AC81),0)","v":82},"-",86,"split into more","heavily serviced workshop",null,null,null,null,"DAT41",{"$f":"IF(C$27=\"extg\",\"DT workshop (existing for 20)\",\"-\")","v":"DT workshop (existing for 20)"},"H1",15,3.7,null,1,"standard",90,12,2,16,null,{"$f":"IF(AX81=\"-\",0,ROUNDDOWN((AX81-VLOOKUP(AP81,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP81,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":20},{"$f":"IF(VLOOKUP(AP81,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX81-VLOOKUP(AP81,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP81,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},22]
[null,"-",0,null,0,0,0,0,0,0,0,null,null,{"$f":"IF(C$27=\"extg\",\"DT workshops (restrictive, extg)\",\"-\")","v":"DT workshops (restrictive, extg)"},"G1",3.5,4,90,34,7,"DAT42",1,{"$f":"VLOOKUP(U82,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT43"},85,"85m2 for up to 24","G1","H","I",24,"art/ design resource",67,85.4,97,"-",150,"split into more","heavily serviced workshop","6","none",null,null,"DAT42",{"$f":"IF(C$27=\"extg\",\"DT workshop (restrictive, extg)\",\"-\")","v":"DT workshop (restrictive, extg)"},"G1",11,3.1,null,1,"restrictive",87,12,2,16,null,{"$f":"IF(AX82=\"-\",0,ROUNDDOWN((AX82-VLOOKUP(AP82,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP82,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":24},{"$f":"IF(VLOOKUP(AP82,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX82-VLOOKUP(AP82,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP82,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},27]
[null,"integrated SRP for ambulant SEN","ARP","SRP",42,3.6,60,5,52,4.5999999999999996,6.5,null,null,"DT workshops","H",3.5,4,111,34,7,"DAT43",null,{"$f":"VLOOKUP(U83,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT43"},96,"104m2 for up to 24","G1","H","I","24","art/ design resource",67,85.4,97,"-",150,"split into more","heavily serviced workshop","6","none",null,null,"DAT43","DT workshop","H",14,3.4,null,1,"standard",104,12,2,16,null,{"$f":"IF(AX83=\"-\",0,ROUNDDOWN((AX83-VLOOKUP(AP83,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP83,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":26},{"$f":"IF(VLOOKUP(AP83,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX83-VLOOKUP(AP83,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP83,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},29]
[null,"integrated SRP for HI","ARP","SRP",42,3.6,60,5,52,4.5999999999999996,6.5,null,null,"DT workshops (2 of 2)","H",3.5,4,97,34,7,"DAT44",null,{"$f":"VLOOKUP(U84,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT43"},96,"97m2 for up to 24","G1","H","I","24","art/ design resource",67,85.4,97,"-",150,"split into more","heavily serviced workshop","6","none",null,null,"DAT44","DT workshop (2 of 2)","H",14,3.4,null,1,"standard",97,12,2,16,null,{"$f":"IF(AX84=\"-\",0,ROUNDDOWN((AX84-VLOOKUP(AP84,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP84,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":24},{"$f":"IF(VLOOKUP(AP84,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX84-VLOOKUP(AP84,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP84,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},27]
[null,"integrated SRP for VI","ARP","SRP",42,3.6,60,5,52,4.5999999999999996,6.5,null,null,"DT workshops (with heat bay)","I",3.5,4,111,34,7,"DAT46",null,{"$f":"VLOOKUP(U85,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT47"},112,"111m2 for up to 24","H1","I","J","24","art/ design resource",67,87.3,111,"-",150,"split into more","heavily serviced with heat bay","6","none",null,null,"DAT46","DT workshop (with heat bay)","I",18,3.9,null,1,"standard",118,12,2,16,null,{"$f":"IF(AX85=\"-\",0,ROUNDDOWN((AX85-VLOOKUP(AP85,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP85,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":25},{"$f":"IF(VLOOKUP(AP85,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX85-VLOOKUP(AP85,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP85,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},28]
[null,"integrated SRP for SLCN","ARP","SRP",42,3.6,60,5,52,4.5999999999999996,6.5,null,null,"Engineering workshops","I",3.5,4,97,34,7,"DAT47",null,{"$f":"VLOOKUP(U86,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT47"},96,"97m2 for up to 20","H1","I","-",20,"art/ design resource",67,"-",97,"-",150,"split into more","heavily serviced with heat bay","6","none",null,null,"DAT47","Engineering workshop","I",18,3.9,null,1,"standard",97,12,2,16,null,{"$f":"IF(AX86=\"-\",0,ROUNDDOWN((AX86-VLOOKUP(AP86,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP86,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":20},{"$f":"IF(VLOOKUP(AP86,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX86-VLOOKUP(AP86,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP86,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},22]
[null,"integrated SRP for ASD","ARP","SRP",42,3.6,60,5,52,4.5999999999999996,6.5,null,null,"Construction workshops","J",3.5,4,97,34,7,"DAT49",null,{"$f":"VLOOKUP(U87,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DAT49"},96,"97m2 for up to 16","I","J","-","16","art/ design resource",67,"-",97,"-",200,"split into more","accommodating construction","6","none",null,null,"DAT49","Construction workshop","J",24,4.5,null,1,"standard",97,10,2,16,null,{"$f":"IF(AX87=\"-\",0,ROUNDDOWN((AX87-VLOOKUP(AP87,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP87,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":16},{"$f":"IF(VLOOKUP(AP87,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX87-VLOOKUP(AP87,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP87,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},18]
[null,"integrated SRP for PD","ARP","SRP",30,3.6,60,5,40,4.4000000000000004,6.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX88=\"-\",0,ROUNDDOWN((AX88-VLOOKUP(AP88,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP88,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP88,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX88-VLOOKUP(AP88,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP88,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,"designated unit for HI","ARP","unit",42,7.6,60,10.5,52,8.8000000000000007,12.5,null,null,"PE general learning areas",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX89=\"-\",0,ROUNDDOWN((AX89-VLOOKUP(AP89,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP89,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP89,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX89-VLOOKUP(AP89,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP89,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,"designated unit for VI","ARP","unit",42,7.6,60,10.5,52,8.8000000000000007,12.5,null,null,"-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-","-","-","-",null,null,null,null,null,null,null,null,{"$f":"IF(AX90=\"-\",0,ROUNDDOWN((AX90-VLOOKUP(AP90,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP90,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP90,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX90-VLOOKUP(AP90,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP90,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,"designated unit for SLCN","ARP","unit",42,7.6,60,10.5,52,8.8000000000000007,12.5,null,null,"Classrooms (PE)","C",1.5,3,55,0,null,"CLA12",null,{"$f":"VLOOKUP(U91,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CLA12"},{"$f":"ROUND(VLOOKUP(O91,$E$38:$I$54,2,FALSE)+(AC91*VLOOKUP(O91,$E$38:$I$54,3,FALSE)),0)","v":55},"55m2 for 30","B","C","D","30","seminar room",25,{"$f":"MINA(AG91*0.9,VLOOKUP(Z91,$E$38:$I$53,2)+(VLOOKUP(Z91,$E$38:$I$53,3,FALSE)*$AC91))","v":49.5},{"$f":"ROUND(VLOOKUP(AA91,$E$38:$I$53,2)+(VLOOKUP(AA91,$E$38:$I$53,3,FALSE)*$AC91),0)","v":55},{"$f":"VLOOKUP(AB91,$E$38:$I$53,2)+(VLOOKUP(AB91,$E$38:$I$53,3,FALSE)*$AC91)","v":62},95,"double classroom","enclosed","5","none",null,null,"CLA12","Classroom (PE)","C",{"$f":"VLOOKUP($AR91,$E$38:$G$54,2,FALSE)","v":4},{"$f":"VLOOKUP($AR91,$E$38:$G$54,3,FALSE)","v":1.7},null,1,"standard",55,9,2,8,null,{"$f":"IF(AX91=\"-\",0,ROUNDDOWN((AX91-VLOOKUP(AP91,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP91,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":30},{"$f":"IF(VLOOKUP(AP91,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX91-VLOOKUP(AP91,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP91,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},33]
[null,"designated unit for ASD","ARP","unit",42,9,60,12.5,52,10,14.5,null,null,"Fitness rooms (exercise studio)","G",3.5,5,69,0,null,"ACT22",null,{"$f":"VLOOKUP(U92,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ACT22"},68,"69m2 for 20","F","G",null,"20","group room ",25,"-",69,"-",184,"split into more","accommodating fitness equipment","6","none",null,null,"ACT22","Fitness room (exercise studio)","G",{"$f":"VLOOKUP($AR92,$E$38:$G$54,2,FALSE)","v":10},{"$f":"VLOOKUP($AR92,$E$38:$G$54,3,FALSE)","v":2.9},null,1,"standard",69,22,2,16,null,{"$f":"IF(AX92=\"-\",0,ROUNDDOWN((AX92-VLOOKUP(AP92,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP92,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":20},{"$f":"IF(VLOOKUP(AP92,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX92-VLOOKUP(AP92,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP92,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},22]
[null,"designated unit for BD","ARP","unit",42,9,60,12.5,52,10,14.5,null,null,"Dining halls","-",12.5,-20,null,null,null,"DIN01",null,{"$f":"VLOOKUP(U93,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DIN01"},null,null,null,null,null,null,"too small",12,"-","AS SOA","-",600,"split into more","used predominantly for dining","4","none",null,null,"DIN01","Dining hall","-",2,0.95,null,0,"standard",80,8,6,12,null,{"$f":"IF(AX93=\"-\",0,ROUNDDOWN((AX93-VLOOKUP(AP93,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP93,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":82},{"$f":"IF(VLOOKUP(AP93,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX93-VLOOKUP(AP93,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP93,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},91]
[null,"designated unit for PD","ARP","unit",30,10.5,60,14.5,40,12,16.5,null,null,"-","-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-","-",{"$f":"VLOOKUP($AR94,$E$38:$G$54,2,FALSE)","v":0},{"$f":"VLOOKUP($AR94,$E$38:$G$54,3,FALSE)","v":0},null,null,"-",null,null,null,null,null,{"$f":"IF(AX94=\"-\",0,ROUNDDOWN((AX94-VLOOKUP(AP94,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP94,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP94,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX94-VLOOKUP(AP94,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP94,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Informal dining spaces","A",1.5,4,null,null,null,"DIN02",null,{"$f":"VLOOKUP(U95,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DIN02"},null,null,null,"A",null,null,"too small",12,"-",55,"-",600,"split into more",null,"4","none",null,null,"DIN02","Informal dining space","A",2,1.1000000000000001,null,0,"standard",8,5,2,8,null,{"$f":"IF(AX95=\"-\",0,ROUNDDOWN((AX95-VLOOKUP(AP95,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP95,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":5},{"$f":"IF(VLOOKUP(AP95,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX95-VLOOKUP(AP95,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP95,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Servery areas, meal collection","-",1.5,4,null,null,null,"DIN11",null,{"$f":"VLOOKUP(U96,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DIN11"},null,null,null,null,null,null,"too small",12,"-",25,"-",50,"dining area",null,"4","none",null,null,"DIN11","Servery area, meal collection","K",4,3.7,null,0,"standard",4,0,2,2,null,{"$f":"IF(AX96=\"-\",0,ROUNDDOWN((AX96-VLOOKUP(AP96,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP96,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(AP96,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX96-VLOOKUP(AP96,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP96,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},0]
[null,"dining",null,"sittings (assuming 33% hot meals)",null,null,null,null,null,null,null,null,null,"Servery areas, satellite","-",1.5,4,null,null,null,"DIN12",null,{"$f":"VLOOKUP(U97,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DIN12"},null,null,null,null,null,null,"too small",6,"-",12,"-",25,"dining area",null,"4","none",null,null,"DIN12","Servery area, satellite","K",4,3.7,null,0,"standard",4,2,2,2,null,{"$f":"IF(AX97=\"-\",0,ROUNDDOWN((AX97-VLOOKUP(AP97,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP97,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(AP97,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX97-VLOOKUP(AP97,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP97,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},0]
[null,"40 mins in dining area and hall","both",2.6700000000000004,"Dining halls",null,"space","of pupils in 2 hot, 3 cold sittings",null,null,null,null,null,"Social spaces","A",1.5,4,null,null,null,"DIN04",null,{"$f":"VLOOKUP(U98,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DIN04"},null,null,null,"A",null,null,"too small",12,"-",90,"-",600,"split into more","used predominantly for socialising","4","none",null,null,"DIN04","Social space","A",2,1.1000000000000001,null,0,"standard",7,5,2,6,null,{"$f":"IF(AX98=\"-\",0,ROUNDDOWN((AX98-VLOOKUP(AP98,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP98,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(AP98,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX98-VLOOKUP(AP98,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP98,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},5]
[null,"40 mins all in main hall","hall",2.6700000000000004,"Servery areas, meal collection",null,null,"of pupils in 2 hot, 3 cold sittings",null,null,null,null,null,"Social spaces (sixth form)","A",1.5,4,null,null,null,"DIN05",null,{"$f":"VLOOKUP(U99,'Data Library'!$A$4:$E$466,5,FALSE)","v":"DIN04"},null,null,null,"A",null,null,"too small",12,"-","AS SOA","-",600,"split into more",null,"4","none",null,null,"DIN05","Social space (sixth form)","A",2,1.1000000000000001,null,0,"standard",104,5,4,16,null,{"$f":"IF(AX99=\"-\",0,ROUNDDOWN((AX99-VLOOKUP(AP99,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP99,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":92},{"$f":"IF(VLOOKUP(AP99,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX99-VLOOKUP(AP99,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP99,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},102]
[null,"60 mins all in dining area (if pos)","dining",3.67,"Dining halls",null,"space","of pupils in 3 hot, 4 cold sittings",null,null,null,null,null,"Assembly halls, secondary (including stage)","-",12.5,-20,null,null,null,"HAL02",null,{"$f":"VLOOKUP(U100,'Data Library'!$A$4:$E$466,5,FALSE)","v":"HAL01"},null,null,null,null,null,null,"drama studio",120,"-","AS SOA","-",600,"sports hall","hign space suitable for performances","6 or 7 if used for exams","adjacent store(s), control room",null,null,"HAL02","Assembly hall, secondary (including stage)","-",45,0.6,null,0,"standard",null,14,null,null,null,{"$f":"IF(AX100=\"-\",0,ROUNDDOWN((AX100-VLOOKUP(AP100,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP100,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":-75},{"$f":"IF(VLOOKUP(AP100,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX100-VLOOKUP(AP100,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP100,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},-83]
[null,"80 mins split lunch in dining area","dining",4.67,"Dining halls",null,null,"of pupils in 2 hot, 3 cold sittings",null,null,null,null,null,"Assembly halls, secondary (with bleachers)","-",12.5,-20,null,null,null,"HAL03",null,{"$f":"VLOOKUP(U101,'Data Library'!$A$4:$E$466,5,FALSE)","v":"HAL01"},null,null,null,null,null,null,"drama studio",120,"-","AS SOA","-",600,"sports hall","hign space suitable for performances","6 or 7 if used for exams","adjacent store(s), control room",null,null,"HAL03","Assembly hall, secondary (with bleachers)","-",25,0.55000000000000004,null,0,"standard",306,14,4,12,null,{"$f":"IF(AX101=\"-\",0,ROUNDDOWN((AX101-VLOOKUP(AP101,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP101,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":510},{"$f":"IF(VLOOKUP(AP101,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX101-VLOOKUP(AP101,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP101,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},536]
[null,"60 mins in dining area and hall","both",3.67,"Dining halls",null,"space","of pupils in 2 hot, 3 cold sittings",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX102=\"-\",0,ROUNDDOWN((AX102-VLOOKUP(AP102,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP102,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP102,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX102-VLOOKUP(AP102,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP102,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,"60 mins all in main hall","hall",3.67,"Servery areas, meal collection",null,null,"of pupils in 2 hot, 3 cold sittings",null,null,null,null,null,"activity studios",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX103=\"-\",0,ROUNDDOWN((AX103-VLOOKUP(AP103,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP103,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP103,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX103-VLOOKUP(AP103,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP103,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX104=\"-\",0,ROUNDDOWN((AX104-VLOOKUP(AP104,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP104,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP104,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX104-VLOOKUP(AP104,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP104,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Dance studios",null,12.5,-20,120,null,null,"ACT01",null,{"$f":"VLOOKUP(U105,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ACT01"},null,"120m2 for 30",null,"-",null,"30","drama studio",105,"-",120,"-",200,"activity studio","hign space with 10 x 10 sprung floor or similar","6 or 7 if used for exams","none",null,null,"ACT01","Dance studio",null,-20,12.5,null,0,"standard",120,11,2,10,null,{"$f":"IF(AX105=\"-\",0,ROUNDDOWN((AX105-VLOOKUP(AP105,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP105,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":11},{"$f":"IF(VLOOKUP(AP105,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX105-VLOOKUP(AP105,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP105,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},13]
[null,"main hall options",null,null,null,null,null,null,null,null,null,null,null,"Activity studios",null,12.5,-20,null,null,null,"ACT05",null,{"$f":"VLOOKUP(U106,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ACT05"},null,"120m2 for 30",null,"-",null,"30","drama studio",105,"-",150,"-",300,"sports hall","hign space with sprung floor or similar","6 or 7 if used for exams","none",null,null,"ACT05","Activity studio",null,-20,12.5,null,0,"standard",150,12,2,10,null,{"$f":"IF(AX106=\"-\",0,ROUNDDOWN((AX106-VLOOKUP(AP106,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP106,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":13},{"$f":"IF(VLOOKUP(AP106,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX106-VLOOKUP(AP106,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP106,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},15]
[null,"hall including stage","Assembly halls, secondary (including stage)",null,null,null,null,null,null,null,null,null,null,"Activity studios (10 x 12)",null,12.5,-20,120,null,null,"ACT06",null,{"$f":"VLOOKUP(U107,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ACT05"},null,"120m2 for 30",null,"-",null,"30","drama studio",120,"-",120,"-",150,"activity studio",null,"6 or 7 if used for exams","none",null,null,"ACT06","Activity studio (10 x 12)",null,-20,12.5,null,0,"standard",120,12,2,10,null,{"$f":"IF(AX107=\"-\",0,ROUNDDOWN((AX107-VLOOKUP(AP107,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP107,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":11},{"$f":"IF(VLOOKUP(AP107,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX107-VLOOKUP(AP107,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP107,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},13]
[null,"hall with bleacher seating","Assembly halls, secondary (with bleachers)",null,null,null,null,null,null,null,null,null,null,"Activity studios (10 x 15)",null,12.5,-20,150,null,null,"ACT07",null,{"$f":"VLOOKUP(U108,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ACT05"},null,"150m2 for 30",null,"-",null,"30","activity studio",150,"-",150,"-",180,"activity studio",null,"6 or 7 if used for exams","none",null,null,"ACT07","Activity studio (10 x 15)",null,-20,12.5,null,0,"standard",150,12,2,10,null,{"$f":"IF(AX108=\"-\",0,ROUNDDOWN((AX108-VLOOKUP(AP108,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP108,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":13},{"$f":"IF(VLOOKUP(AP108,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX108-VLOOKUP(AP108,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP108,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},15]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Activity studios, 1-court",null,12.5,-20,180,null,null,"ACT10",null,{"$f":"VLOOKUP(U109,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ACT05"},null,"180m2",null,null,null,30,"activity studio",162,"-",180,"-",306,"school sports hall (2-court)",null,"6 or 7 if used for exams","none",null,null,"ACT10","Activity studio, 1-court",null,15,1.75,null,0,"standard",180,3,4,4,null,{"$f":"IF(AX109=\"-\",0,ROUNDDOWN((AX109-VLOOKUP(AP109,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP109,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":94},{"$f":"IF(VLOOKUP(AP109,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX109-VLOOKUP(AP109,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP109,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},104]
[null,"retained estate options",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($C$27=\"extg\",\"Gymnasiums (existing)\",\"-\")","v":"Gymnasiums (existing)"},null,12.5,-20,260,null,null,"ACT13",1,{"$f":"VLOOKUP(U110,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ACT11"},null,null,null,"-",null,"30","activity studio",200,"-",260,"-",300,"sports hall","hign space with sprung floor or similar","6 or 7 if used for exams","none",null,null,"ACT13",{"$f":"IF($C$27=\"extg\",\"Gymnasium (existing)\",\"-\")","v":"Gymnasium (existing)"},null,-20,12.5,null,0,"standard",260,12,0,0,null,{"$f":"IF(AX110=\"-\",0,ROUNDDOWN((AX110-VLOOKUP(AP110,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP110,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":22},{"$f":"IF(VLOOKUP(AP110,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX110-VLOOKUP(AP110,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP110,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},25]
[null,"General Teaching/ ICT","General_Learning",null,null,null,"General Teaching/ ICT",null,null,null,null,null,null,{"$f":"IF(C$27=\"extg\",\"Squash courts (existing)\",\"-\")","v":"Squash courts (existing)"},null,12.5,-20,58,null,null,"ACT15",1,{"$f":"VLOOKUP(U111,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ACT11"},null,null,null,"-",null,"2","too small",62,"-",62,"-",65,"activity studio","laid out for squash","6 or 7 if used for exams","none",null,null,"ACT15",{"$f":"IF($C$27=\"extg\",\"Squash court (existing)\",\"-\")","v":"Squash court (existing)"},null,-20,12.5,null,0,"standard",null,0,null,0,null,{"$f":"IF(AX111=\"-\",0,ROUNDDOWN((AX111-VLOOKUP(AP111,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP111,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(AP111,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX111-VLOOKUP(AP111,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP111,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},2]
[null,"Light Practical Teaching","Light_Practical_Learning",null,null,null,"Practical Teaching",null,null,null,null,null,null,{"$f":"IF(C$27=\"extg\",\"Indoor activity spaces, other (existing)\",\"-\")","v":"Indoor activity spaces, other (existing)"},null,12.5,-20,null,null,null,"ACT17",1,{"$f":"VLOOKUP(U112,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ACT11"},null,null,null,null,null,null,"PE classroom",62,"-",62,"-",300,"sports hall",null,null,null,null,null,"ACT17",{"$f":"IF($C$27=\"extg\",\"Indoor activity space, other (existing)\",\"-\")","v":"Indoor activity space, other (existing)"},null,-20,12.5,null,0,"standard",null,0,null,null,null,{"$f":"IF(AX112=\"-\",0,ROUNDDOWN((AX112-VLOOKUP(AP112,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP112,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(AP112,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX112-VLOOKUP(AP112,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP112,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},2]
[null,"Performance Teaching","Creative_Arts",null,null,null,"Large and Performance ",null,null,null,null,null,null,{"$f":"IF(C$27=\"extg\",\"Assembly halls, existing\",\"-\")","v":"Assembly halls, existing"},null,12.5,-20,null,null,null,"HAL21",1,{"$f":"VLOOKUP(U113,'Data Library'!$A$4:$E$466,5,FALSE)","v":"HAL21"},null,null,null,null,null,null,"drama studio",120,"-",250,"-",600,"split or supplementary",null,null,null,null,null,"HAL21",{"$f":"IF($C$27=\"extg\",\"Assembly hall, existing\",\"-\")","v":"Assembly hall, existing"},null,45,0.6,null,0,"standard",150,14,4,8,null,{"$f":"IF(AX113=\"-\",0,ROUNDDOWN((AX113-VLOOKUP(AP113,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP113,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":175},{"$f":"IF(VLOOKUP(AP113,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX113-VLOOKUP(AP113,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP113,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},193]
[null,"Heavy Practical Teaching","DnT",null,null,null,"Learning Resouces and supp",null,null,null,null,null,null,{"$f":"IF(C$27=\"extg\",\"Lecture theatres, existing\",\"-\")","v":"Lecture theatres, existing"},null,12.5,-20,null,null,null,"HAL22",1,{"$f":"VLOOKUP(U114,'Data Library'!$A$4:$E$466,5,FALSE)","v":"HAL22"},null,null,null,null,null,null,"too small",25,"-",62,"-",300,"split or supplementary",null,null,null,null,null,"HAL22",{"$f":"IF($C$27=\"extg\",\"Lecture theatre, existing\",\"-\")","v":"Lecture theatre, existing"},null,-20,12.5,null,0,"standard",null,9,null,null,null,{"$f":"IF(AX114=\"-\",0,ROUNDDOWN((AX114-VLOOKUP(AP114,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP114,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(AP114,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX114-VLOOKUP(AP114,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP114,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},2]
[null,"Large Spaces","Large_Spaces",null,null,null,"Administration Areas",null,null,null,null,null,null,{"$f":"IF(C$27=\"extg\",\"Indoor swimming pools (existing)\",\"-\")","v":"Indoor swimming pools (existing)"},null,12.5,-20,null,null,null,"ACT25",1,{"$f":"VLOOKUP(U115,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ACT25"},null,null,null,null,null,null,"too small",25,"-",500,"-",1500,"split or supplementary",null,null,null,null,null,"ACT25",{"$f":"IF($C$27=\"extg\",\"Indoor swimming pool (existing)\",\"-\")","v":"Indoor swimming pool (existing)"},null,-20,12.5,null,0,"standard",85,0,null,null,null,{"$f":"IF(AX115=\"-\",0,ROUNDDOWN((AX115-VLOOKUP(AP115,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP115,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":8},{"$f":"IF(VLOOKUP(AP115,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX115-VLOOKUP(AP115,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP115,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},9]
[null,"Library and Supplementary","lrc",null,null,null,"Staff Areas",null,null,null,null,null,null,"Climbing wall spaces (indoor)",null,12.5,-20,null,null,null,"ACT21",null,{"$f":"VLOOKUP(U116,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ACT21"},null,null,null,null,null,null,"too small",50,"-",62,"-",300,"activity studio","area with climbing wall","3","none",null,null,"ACT21","Climbing wall space (indoor)","C",{"$f":"VLOOKUP($AR116,$E$38:$G$54,2,FALSE)","v":4},{"$f":"VLOOKUP($AR116,$E$38:$G$54,3,FALSE)","v":1.7},null,0,"standard",25,0,0,0,null,{"$f":"IF(AX116=\"-\",0,ROUNDDOWN((AX116-VLOOKUP(AP116,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP116,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":12},{"$f":"IF(VLOOKUP(AP116,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX116-VLOOKUP(AP116,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP116,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},14]
[null,"Practical Resources","ArtsDnT",null,null,null,"Storage",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX117=\"-\",0,ROUNDDOWN((AX117-VLOOKUP(AP117,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP117,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP117,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX117-VLOOKUP(AP117,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP117,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,"SEN and support spaces","sen",null,null,null,"Non Net",null,null,null,null,null,null,"sports halls",null,"dims",null,"size",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX118=\"-\",0,ROUNDDOWN((AX118-VLOOKUP(AP118,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP118,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP118,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX118-VLOOKUP(AP118,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP118,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,"Administration Areas","admin",null,null,null,null,null,null,null,null,null,180,"Sports halls, school (1-court)",null,"18 x 10",null,180,null,null,"SPH01",null,{"$f":"VLOOKUP(U119,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SPH00"},null,"180m2",null,null,null,30,"activity studio",162,"-",180,"-",306,"school sports hall (2-court)",null,"6 or 7 if used for exams","none",null,null,"SPH01","Sports hall, school (1-court)",null,15,1.75,null,0,"standard",180,3,4,4,null,{"$f":"IF(AX119=\"-\",0,ROUNDDOWN((AX119-VLOOKUP(AP119,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP119,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":94},{"$f":"IF(VLOOKUP(AP119,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX119-VLOOKUP(AP119,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP119,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},104]
[null,"Staff Areas","staff",null,null,null,null,null,null,null,null,null,306,"Sports halls, school (2-court)",null,"18 x 17",null,306,null,null,"SPH02",null,{"$f":"VLOOKUP(U120,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SPH00"},null,"306m2",null,"-",null,"44","school sports hall (1-court)",306,"-",306,"-",450,"school sports hall (3-court)","sports hall","6 or 7 if used for exams","none",null,null,"SPH02","Sports hall, school (2-court)",null,15,1.75,null,0,"standard",306,10,4,4,null,{"$f":"IF(AX120=\"-\",0,ROUNDDOWN((AX120-VLOOKUP(AP120,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP120,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":166},{"$f":"IF(VLOOKUP(AP120,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX120-VLOOKUP(AP120,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP120,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},183]
[null,"General Storage","Gen_store",null,null,null,null,null,null,null,null,null,504,"Sports halls, school (3-court)",null,"18 x 28",null,504,null,null,"SPH03",null,{"$f":"VLOOKUP(U121,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SPH00"},null,"504m2",null,null,null,60,"school sports hall (2-court)",450,"-",504,"-",594,"school sports hall (4-court)",null,"6 or 7 if used for exams","none",null,null,"SPH03","Sports hall, school (3-court)",null,15,1.75,null,0,"standard",504,10,8,8,null,{"$f":"IF(AX121=\"-\",0,ROUNDDOWN((AX121-VLOOKUP(AP121,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP121,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":279},{"$f":"IF(VLOOKUP(AP121,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX121-VLOOKUP(AP121,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP121,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},293]
[null,"Practical Storage","prac_store",null,null,null,null,null,null,null,null,null,594,"Sports halls, school (4-court)",null,"18 x 33",null,594,null,null,"SPH04",null,{"$f":"VLOOKUP(U122,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SPH00"},null,"594m2",null,null,null,60,"school sports hall (3-court)",594,"-",594,"-",690,"community sports hall",null,"6 or 7 if used for exams","none",null,null,"SPH04","Sports hall, school (4-court)",null,15,1.75,null,0,"standard",594,10,8,8,null,{"$f":"IF(AX122=\"-\",0,ROUNDDOWN((AX122-VLOOKUP(AP122,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP122,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":330},{"$f":"IF(VLOOKUP(AP122,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX122-VLOOKUP(AP122,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP122,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},347]
[null,"Non Net","Non_Net",null,null,null,null,null,null,null,null,null,null,{"$f":"IF($C$27=\"extg\",\"Sports halls, school (multi-court, extg)\",\"-\")","v":"Sports halls, school (multi-court, extg)"},null,"as existing",null,544,null,null,"SPH31",1,{"$f":"VLOOKUP(U123,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SPH30"},null,"[500m2]",null,"-",null,"44","school gymnasium (existing)",300,"-",500,"-",690,"community sports hall (existing)","sports hall","6 or 7 if used for exams","none",null,null,"SPH31",{"$f":"IF($C$27=\"extg\",\"Sports hall, school (multi-court, extg)\",\"-\")","v":"Sports hall, school (multi-court, extg)"},null,15,1.75,null,0,"standard",544,10,8,8,null,{"$f":"IF(AX123=\"-\",0,ROUNDDOWN((AX123-VLOOKUP(AP123,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP123,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":302},{"$f":"IF(VLOOKUP(AP123,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX123-VLOOKUP(AP123,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP123,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},317]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($C$27=\"extg\",\"Sports halls, community (multi-court extg)\",\"-\")","v":"Sports halls, community (multi-court extg)"},null,"as existing",null,null,null,null,"SPH32",1,{"$f":"VLOOKUP(U124,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SPH30"},null,"[690m2]",null,null,null,60,"school sports hall (existing)",450,"-",690,"-",750,"split or supplementary","sports hall","6 or 7 if used for exams","none",null,null,"SPH32",{"$f":"IF($C$27=\"extg\",\"Sports hall, community (multi-court extg)\",\"-\")","v":"Sports hall, community (multi-court extg)"},null,15,1.75,null,0,"extensive",null,13,8,8,null,{"$f":"IF(AX124=\"-\",0,ROUNDDOWN((AX124-VLOOKUP(AP124,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP124,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":-8},{"$f":"IF(VLOOKUP(AP124,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX124-VLOOKUP(AP124,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP124,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},-9]
[null,"accom01",null,null,null,null,null,null,null,null,null,null,null,"Sports halls, community (multi-court)",null,null,null,null,null,null,"SPH20",null,{"$f":"VLOOKUP(U125,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SPH20"},null,"690m2",null,null,null,60,"activity studio",306,"-",690,"-",1800,"split or supplementary","sports hall",null,null,null,null,"SPH20","Sports hall, community (multi-court)",null,15,1.75,null,0,"extensive",null,13,8,8,null,{"$f":"IF(AX125=\"-\",0,ROUNDDOWN((AX125-VLOOKUP(AP125,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP125,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":-8},{"$f":"IF(VLOOKUP(AP125,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX125-VLOOKUP(AP125,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP125,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},-9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Sports halls, community (4-court)",null,"20 x 34.5",null,690,null,null,"SPH24",null,{"$f":"VLOOKUP(U126,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SPH20"},null,"690m2",null,null,null,60,"school sports hall",594,"-",690,"-",750,"split or supplementary","sports hall","6 or 7 if used for exams","none",null,null,"SPH24","Sports hall, community (4-court)",null,15,1.75,null,0,"extensive",690,13,8,10,null,{"$f":"IF(AX126=\"-\",0,ROUNDDOWN((AX126-VLOOKUP(AP126,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP126,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":385},{"$f":"IF(VLOOKUP(AP126,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX126-VLOOKUP(AP126,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP126,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},404]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Sports halls, community (5-court)",null,"21.35 x 40.6",null,867,null,null,"SPH25",null,{"$f":"VLOOKUP(U127,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SPH20"},null,"867m2",null,null,null,60,"community sports hall",731,"-",867,"-",900,"split or supplementary","sports hall","6 or 7 if used for exams","none",null,null,"SPH25","Sports hall, community (5-court)",null,15,1.75,null,0,"extensive",867,13,8,10,null,{"$f":"IF(AX127=\"-\",0,ROUNDDOWN((AX127-VLOOKUP(AP127,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP127,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":486},{"$f":"IF(VLOOKUP(AP127,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX127-VLOOKUP(AP127,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP127,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},510]
[null,"Remodel","room areas if 7.8 deep",null,null,null,null,null,null,null,null,null,null,"Sports halls, community (8-court)",null,"34.5 x 40.0",null,1380,null,null,"SPH27",null,{"$f":"VLOOKUP(U128,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SPH20"},null,"1380m2",null,null,null,90,"community sports hall",1188,"-",1380,"-",1435,"split or supplementary","sports hall","6 or 7 if used for exams","none",null,null,"SPH27","Sports hall, community (8-court)",null,15,1.75,null,0,"extensive",1241,13,10,16,null,{"$f":"IF(AX128=\"-\",0,ROUNDDOWN((AX128-VLOOKUP(AP128,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP128,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":700},{"$f":"IF(VLOOKUP(AP128,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX128-VLOOKUP(AP128,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP128,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},735]
[null,"Refurb",null,"area","realistic",null,null,null,null,null,null,null,null,"Sports halls, community (12-court)",null,"40.6 x 42.7",null,1733.6200000000001,null,null,"SPH28",null,{"$f":"VLOOKUP(U129,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SPH20"},null,"1734m2",null,null,null,90,"community sports hall",1538,"-",1734,"-",1800,"split or supplementary","sports hall",null,null,null,null,"SPH28","Sports hall, community (12-court)",null,15,1.75,null,0,"extensive",1258,13,12,16,null,{"$f":"IF(AX129=\"-\",0,ROUNDDOWN((AX129-VLOOKUP(AP129,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP129,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":710},{"$f":"IF(VLOOKUP(AP129,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX129-VLOOKUP(AP129,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP129,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},746]
[null,"Keep",null,"when","area,",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX130=\"-\",0,ROUNDDOWN((AX130-VLOOKUP(AP130,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP130,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP130,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX130-VLOOKUP(AP130,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP130,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,"recom-","allowing",null,null,null,null,null,null,null,null,"learning resources and supplementary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX131=\"-\",0,ROUNDDOWN((AX131-VLOOKUP(AP131,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP131,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP131,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX131-VLOOKUP(AP131,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP131,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,"space","mended","for parti-",null,null,null,null,null,null,null,null,"-",null,null,null,null,null,null,null,null,null,null,"[118m2]",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-","-","-","-",null,null,null,null,null,null,null,null,{"$f":"IF(AX132=\"-\",0,ROUNDDOWN((AX132-VLOOKUP(AP132,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP132,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP132,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX132-VLOOKUP(AP132,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP132,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,1,"size","width of","tions at",null,null,null,null,null,null,null,null,"Library resource centres (LRC)","F",2,4,null,null,null,"LIB05",null,{"$f":"VLOOKUP(U133,'Data Library'!$A$4:$E$466,5,FALSE)","v":"LIB05"},83,"[41m2]",null,"F",null,"30","too small",12,"-","AS SOA","-",250,"split into more",null,"4","none",null,null,"LIB05","Library resource centre (LRC)","F",{"$f":"VLOOKUP($AR133,$E$38:$G$54,2,FALSE)","v":8},{"$f":"VLOOKUP($AR133,$E$38:$G$54,3,FALSE)","v":2.5},null,1,"standard",180,28,2,39,null,{"$f":"IF(AX133=\"-\",0,ROUNDDOWN((AX133-VLOOKUP(AP133,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP133,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":68},{"$f":"IF(VLOOKUP(AP133,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX133-VLOOKUP(AP133,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP133,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},75]
[null,2,null,7.8,{"$f":"D134*0.15","v":1.17},null,null,null,null,null,null,null,null,"Study spaces, rooms (sixth form)","B",1.5,4,null,null,null,"LIB06",null,{"$f":"VLOOKUP(U134,'Data Library'!$A$4:$E$466,5,FALSE)","v":"LIB07"},34,"9m2 for up to 4",null,"B",null,"20","too small",12,"-","AS SOA","-",250,"split into more",null,"4","none",null,null,"LIB06","Study space, room (sixth form)","B",2,1.6,null,0,"standard",48,26,2,18,null,{"$f":"IF(AX134=\"-\",0,ROUNDDOWN((AX134-VLOOKUP(AP134,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP134,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":28},{"$f":"IF(VLOOKUP(AP134,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX134-VLOOKUP(AP134,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP134,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(BC134>200,ROUND(BC134*1.05,0),ROUNDUP(BC134*1.1,0))","v":31}]
[null,3,null,null,null,null,null,null,null,null,null,null,null,"Study spaces, rooms","B",1.5,4,null,null,null,"LIB07",null,{"$f":"VLOOKUP(U135,'Data Library'!$A$4:$E$466,5,FALSE)","v":"LIB07"},34,"[41m2]",null,"B",null,"20","too small",12,"-",{"$f":"ROUND(VLOOKUP(AA135,$E$38:$I$53,2)+(VLOOKUP(AA135,$E$38:$I$53,3,FALSE)*$AC135),0)","v":34},"-",250,"split into more",null,"4","none",null,null,"LIB07","Study space, room","B",2,1.6,null,0,"standard",48,26,2,8,null,{"$f":"IF(AX135=\"-\",0,ROUNDDOWN((AX135-VLOOKUP(AP135,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP135,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":28},{"$f":"IF(VLOOKUP(AP135,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX135-VLOOKUP(AP135,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP135,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},31]
[null,4,27,3.6,{"$f":"(D$134*D136)-E$134","v":26.909999999999997},null,null,null,null,null,null,null,null,"Faith spaces (chapel)","A",1.5,4,null,null,null,"SUP01",null,{"$f":"VLOOKUP(U136,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SUP00"},24,null,null,"A",null,"20","sacristy",12,"-",{"$f":"ROUND(VLOOKUP(AA136,$E$38:$I$53,2)+(VLOOKUP(AA136,$E$38:$I$53,3,FALSE)*$AC136),0)","v":24},"-",150,"hall",null,"2","none",null,null,"SUP01","Faith space (chapel)","A",2,1.1000000000000001,null,0,"standard",25,0,null,2,null,{"$f":"IF(AX136=\"-\",0,ROUNDDOWN((AX136-VLOOKUP(AP136,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP136,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":20},{"$f":"IF(VLOOKUP(AP136,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX136-VLOOKUP(AP136,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP136,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},22]
[null,5,34,4.5,33.93,null,null,null,null,null,null,null,null,"Faith spaces (prayer room)","A",1.5,4,null,null,null,"SUP01",null,{"$f":"VLOOKUP(U137,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SUP00"},24,null,null,"A",null,20,"too small",12,"-",{"$f":"ROUND(VLOOKUP(AA137,$E$38:$I$53,2)+(VLOOKUP(AA137,$E$38:$I$53,3,FALSE)*$AC137),0)","v":24},"-",150,"hall",null,"3","none",null,null,"SUP01","Faith space (prayer room)","A",2,1.1000000000000001,null,0,"standard",25,0,null,2,null,{"$f":"IF(AX137=\"-\",0,ROUNDDOWN((AX137-VLOOKUP(AP137,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP137,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":20},{"$f":"IF(VLOOKUP(AP137,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX137-VLOOKUP(AP137,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP137,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},22]
[null,6,41,5.4,40.950000000000003,null,null,null,null,null,null,null,null,"Staff workrooms (sacristy)","B",1.5,4,null,null,null,"SUP02",null,{"$f":"VLOOKUP(U138,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SUP00"},5,null,null,"B",null,"2","too small",6,"-",6,"-",50,"split into more",null,"2","none",null,null,"SUP01","Staff workroom (sacristy)","B",2,1.6,null,0,"standard",12,0,null,2,null,{"$f":"IF(AX138=\"-\",0,ROUNDDOWN((AX138-VLOOKUP(AP138,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP138,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":9},{"$f":"IF(VLOOKUP(AP138,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX138-VLOOKUP(AP138,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP138,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},10]
[null,null,48,6.3,47.97,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX139=\"-\",0,ROUNDDOWN((AX139-VLOOKUP(AP139,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP139,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP139,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX139-VLOOKUP(AP139,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP139,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,55,7.2,54.989999999999995,null,null,null,null,null,null,null,null,"Arts and DT learning resources",null,null,null,null,null,"group",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX140=\"-\",0,ROUNDDOWN((AX140-VLOOKUP(AP140,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP140,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP140,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX140-VLOOKUP(AP140,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP140,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,62,8.1,62.009999999999991,null,null,null,null,null,null,null,null,"-",null,null,null,null,null,"size",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX141=\"-\",0,ROUNDDOWN((AX141-VLOOKUP(AP141,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP141,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP141,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX141-VLOOKUP(AP141,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP141,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,69,9,69.03,null,null,null,null,null,null,null,null,"Music practice rooms","B",2,4,8,null,3,"RES12",null,{"$f":"VLOOKUP(U142,'Data Library'!$A$4:$E$466,5,FALSE)","v":"RES12"},7,"8m2 for up to 3","A","B","C","3","too small",6,"-",8,{"$f":"VLOOKUP(AB142,$E$38:$I$53,2)+(VLOOKUP(AB142,$E$38:$I$53,3,FALSE)*$AC142)","v":9.1},12,"extesive music practice","acoustically discrete","4","none",null,null,"RES12","Music practice room","B",{"$f":"VLOOKUP($AR142,$E$38:$G$54,2,FALSE)","v":2},{"$f":"VLOOKUP($AR142,$E$38:$G$54,3,FALSE)","v":1.6},null,0,"standard",4,3,0,4,null,{"$f":"IF(AX142=\"-\",0,ROUNDDOWN((AX142-VLOOKUP(AP142,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP142,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(AP142,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX142-VLOOKUP(AP142,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP142,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},2]
[null,null,76,9.9,76.05,null,null,null,null,null,null,null,null,"Music practice rooms (extensive)","C",2,4,16,null,7,"RES13",null,{"$f":"VLOOKUP(U143,'Data Library'!$A$4:$E$466,5,FALSE)","v":"RES12"},16,"16m2 for up to 7","A","B","C",7,"too small",12,"-",{"$f":"VLOOKUP(AA143,$E$38:$I$53,2)+(VLOOKUP(AA143,$E$38:$I$53,3,FALSE)*$AC143)","v":13.200000000000001},{"$f":"ROUND(VLOOKUP(AB143,$E$38:$I$53,2)+(VLOOKUP(AB143,$E$38:$I$53,3,FALSE)*$AC143),0)","v":16},45,"music classroom ",null,"5","none",null,null,"RES13","Music practice room (extensive)","C",4,1.7,null,0,"extensive",16,3,0,6,null,{"$f":"IF(AX143=\"-\",0,ROUNDDOWN((AX143-VLOOKUP(AP143,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP143,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":7},{"$f":"IF(VLOOKUP(AP143,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX143-VLOOKUP(AP143,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP143,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},8]
[null,null,83,10.8,83.070000000000007,null,null,null,null,null,null,null,null,"Recording control spaces","B",2,4,8,null,3,"RES14",null,{"$f":"VLOOKUP(U144,'Data Library'!$A$4:$E$466,5,FALSE)","v":"RES14"},7,"8m2 for up to 3","A","B","C","3","too small",6,"-",8,"-",45,"split into more","overseeing adjacent space","5","none",null,null,"RES14","Recording control space","B",2,1.6,null,0,"standard",8,11,2,4,null,{"$f":"IF(AX144=\"-\",0,ROUNDDOWN((AX144-VLOOKUP(AP144,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP144,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":3},{"$f":"IF(VLOOKUP(AP144,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX144-VLOOKUP(AP144,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP144,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},4]
[null,null,90,11.7,90.089999999999989,null,null,null,null,null,null,null,null,"Music practice rooms (recording)","B",2,4,9,null,4,"RES15",null,{"$f":"VLOOKUP(U145,'Data Library'!$A$4:$E$466,5,FALSE)","v":"RES12"},8,"9m2 for up to 4","A","B","C",4,"too small",6,"-",9,"-",45,"split into more",null,"5","control room for recording ",null,null,"RES15","Music practice room (recording)","B",2,1.6,null,0,"standard",12,11,2,4,null,{"$f":"IF(AX145=\"-\",0,ROUNDDOWN((AX145-VLOOKUP(AP145,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP145,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":6},{"$f":"IF(VLOOKUP(AP145,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX145-VLOOKUP(AP145,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP145,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},7]
[null,null,97,12.6,97.11,null,null,null,null,null,null,null,null,"Lighting and audio control spaces","B",2,4,6,null,2,"RES16",null,{"$f":"VLOOKUP(U146,'Data Library'!$A$4:$E$466,5,FALSE)","v":"RES16"},5,"6m2 for up to 2","A","B","C",2,"too small",4,"-",6,"-",45,"split into more",null,"4","none",null,null,"RES16","Lighting and audio control space","B",2,1.6,null,0,"standard",8,11,2,8,null,{"$f":"IF(AX146=\"-\",0,ROUNDDOWN((AX146-VLOOKUP(AP146,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP146,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":3},{"$f":"IF(VLOOKUP(AP146,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX146-VLOOKUP(AP146,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP146,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},4]
[null,null,104,13.5,104.13,null,null,null,null,null,null,null,null,"Heavy practical resource (kiln)","-",3.5,4,4,null,"-","RES21",null,{"$f":"VLOOKUP(U147,'Data Library'!$A$4:$E$466,5,FALSE)","v":"RES21"},null,"4m2","-","-","-","-","too small",4,"-",4,"-",25,"art/ design resource","acommodating kiln","5","none",null,null,"RES21","Heavy practical resource (kiln)","-",0,0,null,0,"standard",4,11,0,0,null,{"$f":"IF(AX147=\"-\",0,ROUNDDOWN((AX147-VLOOKUP(AP147,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP147,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP147,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX147-VLOOKUP(AP147,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP147,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,111,14.4,111.14999999999999,null,null,null,null,null,null,null,null,"Darkrooms","B",2.5,4,9,null,4,"RES22",null,{"$f":"VLOOKUP(U148,'Data Library'!$A$4:$E$466,5,FALSE)","v":"RES22"},8,"9m2 for up to 4","A","B","C","4","too small",6,"-",9,"-",45,"photography studio","dark but ventilated ","5","none",null,null,"RES22","Darkroom","B",2,1.6,null,0,"standard",9,3,2,4,null,{"$f":"IF(AX148=\"-\",0,ROUNDDOWN((AX148-VLOOKUP(AP148,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP148,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(AP148,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX148-VLOOKUP(AP148,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP148,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},5]
[null,null,118,15.3,118.17,null,null,null,null,null,null,null,null,"Light practical resource (art/ design)","F",2.5,4,41,null,13,"RES23",null,{"$f":"VLOOKUP(U149,'Data Library'!$A$4:$E$466,5,FALSE)","v":"RES23"},41,"[41m2]","E","F","G","13","too small",12,"-",41,"-",83,"general art room","semi-open resource ","5","none",null,null,"RES23","Light practical resource (art/ design)","F",8,2.5,null,0,"standard",41,16,2,8,null,{"$f":"IF(AX149=\"-\",0,ROUNDDOWN((AX149-VLOOKUP(AP149,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP149,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":13},{"$f":"IF(VLOOKUP(AP149,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX149-VLOOKUP(AP149,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP149,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},15]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Corridors (with art display)","-",1.5,4,4,null,"-","CIR05",null,{"$f":"VLOOKUP(U150,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CIR00"},0,null,"-","-","-",null,"too small",4,"-",12,"-",25,"art/ design resource",null,"2","none",null,null,"CIR05","Corridor (with art display)","-",0,0,null,0,"standard",4,0,0,2,null,{"$f":"IF(AX150=\"-\",0,ROUNDDOWN((AX150-VLOOKUP(AP150,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP150,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP150,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX150-VLOOKUP(AP150,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP150,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,"room size",3.6,{"$f":"D151*0.125","v":0.45},null,null,null,null,null,null,null,null,"ICT resource spaces, open","D",2,4,34,null,15,"RES31",null,{"$f":"VLOOKUP(U151,'Data Library'!$A$4:$E$466,5,FALSE)","v":"RES31"},34,null,"C","D","E","15","too small",6,"-",{"$f":"ROUND(VLOOKUP(AA151,$E$38:$I$53,2)+(VLOOKUP(AA151,$E$38:$I$53,3,FALSE)*$AC151),0)","v":34},"-",62,"ICT-rich learning area","semi-open resource ","4","none",null,null,"RES31","ICT resource space, open","D",5,1.9,null,0,"standard",41,32,2,12,null,{"$f":"IF(AX151=\"-\",0,ROUNDDOWN((AX151-VLOOKUP(AP151,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP151,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":18},{"$f":"IF(VLOOKUP(AP151,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX151-VLOOKUP(AP151,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP151,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},20]
[null,null,6,1.8,{"$f":"(D$151*D152)-E$151","v":6.03},null,null,null,null,null,null,null,null,"Heavy practical resource (heat treatment, extg)","F",3.5,4,12,null,2,"RES32",1,{"$f":"VLOOKUP(U152,'Data Library'!$A$4:$E$466,5,FALSE)","v":"RES32"},13,null,"E","F","G","2","too small",12,"-",{"$f":"ROUND(VLOOKUP(AA152,$E$38:$I$53,2)+(VLOOKUP(AA152,$E$38:$I$53,3,FALSE)*$AC152),0)","v":13},"-",67,"RM workshop with heat bay","acommodating heat treatment equipment","5","none",null,null,"RES32","Heavy practical resource (heat treatment, extg)","F",8,2.5,null,0,"standard",20,0,null,6,null,{"$f":"IF(AX152=\"-\",0,ROUNDDOWN((AX152-VLOOKUP(AP152,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP152,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(AP152,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX152-VLOOKUP(AP152,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP152,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},5]
[null,null,9,2.7,9.2700000000000014,null,null,null,null,null,null,null,null,"Heavy practical resource (CAD CAM, extg)","F",3.5,4,20,null,5,"RES33",1,{"$f":"VLOOKUP(U153,'Data Library'!$A$4:$E$466,5,FALSE)","v":"RES33"},21,null,"E","F","G","5","too small",12,"-",{"$f":"ROUND(VLOOKUP(AA153,$E$38:$I$53,2)+(VLOOKUP(AA153,$E$38:$I$53,3,FALSE)*$AC153),0)","v":21},"-",67,"resistant materials workshop","acommodating CAD CAM equipment","5","none",null,null,"RES33","Heavy practical resource (CAD CAM, extg)","F",8,2.5,null,0,"standard",20,0,2,18,null,{"$f":"IF(AX153=\"-\",0,ROUNDDOWN((AX153-VLOOKUP(AP153,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP153,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(AP153,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX153-VLOOKUP(AP153,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP153,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},5]
[null,null,13,3.6,12.510000000000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP(U154,'Data Library'!$A$4:$E$466,5,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX154=\"-\",0,ROUNDDOWN((AX154-VLOOKUP(AP154,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP154,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP154,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX154-VLOOKUP(AP154,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP154,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,16,4.5,15.75,null,null,null,null,null,null,null,null,"SEN and support spaces",null,null,null,null,null,null,null,null,{"$f":"VLOOKUP(U155,'Data Library'!$A$4:$E$466,5,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX155=\"-\",0,ROUNDDOWN((AX155-VLOOKUP(AP155,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP155,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP155,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX155-VLOOKUP(AP155,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP155,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,19,5.4,18.990000000000002,null,null,null,null,null,null,null,null,"-",null,null,null,null,null,null,null,null,{"$f":"VLOOKUP(U156,'Data Library'!$A$4:$E$466,5,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AX156=\"-\",0,ROUNDDOWN((AX156-VLOOKUP(AP156,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP156,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP156,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX156-VLOOKUP(AP156,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP156,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,22,6.3,22.23,null,null,null,null,null,null,null,null,"Small group rooms","B",1.5,4,9,null,4,"RES00",null,{"$f":"VLOOKUP(U157,'Data Library'!$A$4:$E$466,5,FALSE)","v":"RES00"},{"$f":"ROUND(VLOOKUP(O157,$E$38:$I$54,2,FALSE)+(AC157*VLOOKUP(O157,$E$38:$I$54,3,FALSE)),0)","v":8},"9m2 for up to 4","A","B","C",4,"too small",6,"-",9,"-",25,"large group room",null,"4","none",null,null,"RES00","Small group room","B",{"$f":"VLOOKUP($AR157,$E$38:$G$54,2,FALSE)","v":2},{"$f":"VLOOKUP($AR157,$E$38:$G$54,3,FALSE)","v":1.6},null,0,"standard",9,6,2,16,null,{"$f":"IF(AX157=\"-\",0,ROUNDDOWN((AX157-VLOOKUP(AP157,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP157,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(AP157,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX157-VLOOKUP(AP157,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP157,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},5]
[null,null,25,7.2,25.470000000000002,null,null,null,null,null,null,null,null,"Small group rooms (medium)","B",1.5,4,12,null,6,"RES03",null,{"$f":"VLOOKUP(U158,'Data Library'!$A$4:$E$466,5,FALSE)","v":"RES00"},12,"12m2 for up to 6","A","B","C","6","small group room",12,"-",{"$f":"ROUND(VLOOKUP(AA158,$E$38:$I$53,2)+(VLOOKUP(AA158,$E$38:$I$53,3,FALSE)*$AC158),0)","v":12},"-",25,"large group room","enclosed","4","none",null,null,"RES03","Small group room (medium)","B",2,1.6,null,0,"standard",12,6,2,12,null,{"$f":"IF(AX158=\"-\",0,ROUNDDOWN((AX158-VLOOKUP(AP158,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP158,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":6},{"$f":"IF(VLOOKUP(AP158,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX158-VLOOKUP(AP158,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP158,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},7]
[null,null,29,8.1,28.71,null,null,null,null,null,null,null,null,"Small group rooms (large SEN etc.)","B",1.5,4,16,null,9,"RES04",null,{"$f":"VLOOKUP(U159,'Data Library'!$A$4:$E$466,5,FALSE)","v":"RES00"},16,"16m2 for up to 9","A","B","C",9,"medium group room",16,"-",{"$f":"ROUND(VLOOKUP(AA159,$E$38:$I$53,2)+(VLOOKUP(AA159,$E$38:$I$53,3,FALSE)*$AC159),0)","v":16},"-",41,"seminar room",null,"4","none",null,null,"RES04","Small group room (large SEN etc.)","B",2,1.6,null,0,"standard",16,6,2,16,null,{"$f":"IF(AX159=\"-\",0,ROUNDDOWN((AX159-VLOOKUP(AP159,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP159,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":8},{"$f":"IF(VLOOKUP(AP159,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX159-VLOOKUP(AP159,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP159,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},9]
[null,null,32,9,31.95,null,null,null,null,null,null,null,null,"Shared teaching areas, secondary","B",1.5,4,16,null,9,"RES05",null,{"$f":"VLOOKUP(U160,'Data Library'!$A$4:$E$466,5,FALSE)","v":"RES05"},16,"16m2 for up to 9","A","B","C","9","small group room",12,"-",{"$f":"ROUND(VLOOKUP(AA160,$E$38:$I$53,2)+(VLOOKUP(AA160,$E$38:$I$53,3,FALSE)*$AC160),0)","v":16},"-",25,"open learning area","semi-open","4","none",null,null,"RES05","Shared teaching area, secondary","B",2,1.6,null,0,"standard",16,8,2,8,null,{"$f":"IF(AX160=\"-\",0,ROUNDDOWN((AX160-VLOOKUP(AP160,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP160,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":8},{"$f":"IF(VLOOKUP(AP160,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX160-VLOOKUP(AP160,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP160,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"SEN resource spaces","C",1.5,4,16,null,7,"SEN20",null,{"$f":"VLOOKUP(U161,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SEN20"},16,"16m2 for up to 7","B","C","D",7,"small group room",12,"-",{"$f":"ROUND(VLOOKUP(AA161,$E$38:$I$53,2)+(VLOOKUP(AA161,$E$38:$I$53,3,FALSE)*$AC161),0)","v":16},"-",41,"SEN classroom (ambulant)",null,"6","none",null,null,"SEN20","SEN resource space","C",4,1.7,null,0,"standard",16,8,2,16,null,{"$f":"IF(AX161=\"-\",0,ROUNDDOWN((AX161-VLOOKUP(AP161,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP161,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":7},{"$f":"IF(VLOOKUP(AP161,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX161-VLOOKUP(AP161,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP161,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Small group rooms (inclusion/ withdrawal)","B",1.5,4,16,null,7,"RES06",null,{"$f":"VLOOKUP(U162,'Data Library'!$A$4:$E$466,5,FALSE)","v":"RES00"},13,"16m2 for up to 7","B","C","D","7","small group room",12,"-",{"$f":"ROUND(VLOOKUP(AA162,$E$38:$I$53,2)+(VLOOKUP(AA162,$E$38:$I$53,3,FALSE)*$AC162),0)","v":16},null,41,"SEN classroom (ambulant)","enclosed for SEN pupils","6","none",null,null,"RES06","Small group room (inclusion/ withdrawal)","B",2,1.6,null,0,"standard",16,8,2,8,null,{"$f":"IF(AX162=\"-\",0,ROUNDDOWN((AX162-VLOOKUP(AP162,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP162,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":8},{"$f":"IF(VLOOKUP(AP162,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX162-VLOOKUP(AP162,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP162,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Medical treatment (MI) rooms","C",1.5,4,12,null,4,"SEN02",null,{"$f":"VLOOKUP(U163,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SEN02"},11,"12m2 for up to 4","B","C","D","4","too small",6,"-",12,"-",41,"SEN classroom (ambulant)","enclosed for MI","6","none",null,null,"SEN02","Medical treatment (MI) room","C",4,1.7,null,0,"standard",12,8,null,4,null,{"$f":"IF(AX163=\"-\",0,ROUNDDOWN((AX163-VLOOKUP(AP163,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP163,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(AP163,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX163-VLOOKUP(AP163,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP163,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Therapy rooms","C",1.5,4,9,null,3,"SEN12",null,{"$f":"VLOOKUP(U164,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SEN12"},9,"9m2 for up to 3","B","C","D",3,"too small",6,null,{"$f":"ROUND(VLOOKUP(AA164,$E$38:$I$53,2)+(VLOOKUP(AA164,$E$38:$I$53,3,FALSE)*$AC164),0)","v":9},"-",41,"SEN classroom (ambulant)",null,"6","none",null,null,"SEN12","Therapy room","C",4,1.7,null,0,"standard",9,3,null,8,null,{"$f":"IF(AX164=\"-\",0,ROUNDDOWN((AX164-VLOOKUP(AP164,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP164,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":2},{"$f":"IF(VLOOKUP(AP164,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX164-VLOOKUP(AP164,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP164,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"SEN resource spaces (ambulant support)","C",1.5,4,16,null,7,"SEN21",null,{"$f":"VLOOKUP(U165,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SEN20"},16,"16m2 for up to 7","B","C","D","7","small group room",12,"-",16,null,41,"SEN classroom (ambulant)","enclosed for SEN pupils","6","none",null,null,"SEN21","SEN resource space (ambulant support)","C",4,1.7,null,0,"standard",16,6,null,8,null,{"$f":"IF(AX165=\"-\",0,ROUNDDOWN((AX165-VLOOKUP(AP165,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP165,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":7},{"$f":"IF(VLOOKUP(AP165,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX165-VLOOKUP(AP165,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP165,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"SEN resource spaces (SLCN support)","C",1.5,4,16,null,7,"SEN22",null,{"$f":"VLOOKUP(U166,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SEN20"},16,"16m2 for up to 7","B","C","D","7","small group room",12,"-",16,null,41,"SEN classroom (ambulant)",null,"6","none",null,null,"SEN22","SEN resource space (SLCN support)","C",4,1.7,null,0,"standard",16,6,null,8,null,{"$f":"IF(AX166=\"-\",0,ROUNDDOWN((AX166-VLOOKUP(AP166,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP166,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":7},{"$f":"IF(VLOOKUP(AP166,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX166-VLOOKUP(AP166,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP166,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"SEN resource spaces (behaviour support)","C",1.5,4,16,null,7,"SEN23",null,{"$f":"VLOOKUP(U167,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SEN20"},16,"16m2 for up to 7","B","C","D","7","small group room",12,"-",16,null,41,"SEN classroom (ambulant)",null,"6","none",null,null,"SEN23","SEN resource space (behaviour support)","C",4,1.7,null,0,"standard",16,6,null,8,null,{"$f":"IF(AX167=\"-\",0,ROUNDDOWN((AX167-VLOOKUP(AP167,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP167,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":7},{"$f":"IF(VLOOKUP(AP167,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX167-VLOOKUP(AP167,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP167,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"SEN resource spaces (autism support)","C",1.5,4,16,null,7,"SEN24",null,{"$f":"VLOOKUP(U168,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SEN20"},16,"16m2 for up to 7","B","C","D","7","small group room",12,"-",16,null,41,"SEN classroom (ambulant)",null,"6","none",null,null,"SEN24","SEN resource space (autism support)","C",4,1.7,null,0,"standard",16,6,null,8,null,{"$f":"IF(AX168=\"-\",0,ROUNDDOWN((AX168-VLOOKUP(AP168,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP168,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":7},{"$f":"IF(VLOOKUP(AP168,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX168-VLOOKUP(AP168,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP168,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"SEN resource spaces (PD support)","C",1.5,4,16,null,7,"SEN25",null,{"$f":"VLOOKUP(U169,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SEN20"},16,"16m2 for up to 7","B","C","D","7","small group room",12,"-",16,null,41,"SEN classroom (ambulant)",null,"6","none",null,null,"SEN25","SEN resource space (PD support)","C",4,1.7,null,0,"standard",16,6,null,8,null,{"$f":"IF(AX169=\"-\",0,ROUNDDOWN((AX169-VLOOKUP(AP169,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP169,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":7},{"$f":"IF(VLOOKUP(AP169,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX169-VLOOKUP(AP169,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP169,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"SEN resource spaces (HI support)","C",1.5,4,16,null,7,"SEN26",null,{"$f":"VLOOKUP(U170,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SEN20"},16,"16m2 for up to 7","B","C","D","7","small group room",12,"-",16,null,41,"SEN classroom (ambulant)",null,"6","none",null,null,"SEN26","SEN resource space (HI support)","C",4,1.7,null,0,"standard",16,6,null,8,null,{"$f":"IF(AX170=\"-\",0,ROUNDDOWN((AX170-VLOOKUP(AP170,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP170,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":7},{"$f":"IF(VLOOKUP(AP170,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX170-VLOOKUP(AP170,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP170,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"SEN resource spaces (VI support)","C",1.5,4,16,null,7,"SEN27",null,{"$f":"VLOOKUP(U171,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SEN20"},16,"16m2 for up to 7","B","C","D","7","small group room",12,"-",{"$f":"ROUND(VLOOKUP(AA171,$E$38:$I$53,2)+(VLOOKUP(AA171,$E$38:$I$53,3,FALSE)*$AC171),0)","v":16},null,41,"SEN classroom (ambulant)",null,"6","none",null,null,"SEN27","SEN resource space (VI support)","C",4,1.7,null,0,"standard",16,6,null,8,null,{"$f":"IF(AX171=\"-\",0,ROUNDDOWN((AX171-VLOOKUP(AP171,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP171,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":7},{"$f":"IF(VLOOKUP(AP171,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX171-VLOOKUP(AP171,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP171,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Quiet calming spaces","C",1.5,4,6,null,1,"SEN30",null,{"$f":"VLOOKUP(U172,'Data Library'!$A$4:$E$466,5,FALSE)","v":"SEN30"},6,"6m2 for 1","B","C","D","1","too small",4,"-",6,"-",12,"small group room","enclosed for SEN pupils","6","none",null,null,"SEN30","Quiet calming space","C",4,1.7,null,0,"standard",6,4,null,8,null,{"$f":"IF(AX172=\"-\",0,ROUNDDOWN((AX172-VLOOKUP(AP172,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP172,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(AP172,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX172-VLOOKUP(AP172,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP172,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"-","-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-","-",0,0,null,null,null,null,null,null,null,null,{"$f":"IF(AX173=\"-\",0,ROUNDDOWN((AX173-VLOOKUP(AP173,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP173,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP173,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX173-VLOOKUP(AP173,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP173,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Confidential meetings rooms (interview)","A",1.5,4,6,null,3,"ADM02",null,{"$f":"VLOOKUP(U174,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ADM02"},5,"6m2 for 3",null,"A",null,"3","too small",4,"-",6,"-",25,"office/ meeting","enclosed for SEN pupils","4","none",null,null,"ADM02","Confidential meeting room (interview)","A",2,1.1000000000000001,null,0,"-",6,3,2,8,null,{"$f":"IF(AX174=\"-\",0,ROUNDDOWN((AX174-VLOOKUP(AP174,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP174,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":3},{"$f":"IF(VLOOKUP(AP174,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX174-VLOOKUP(AP174,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP174,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"First aid rooms (sick room)","B",1.5,4,6,null,2,"ADM04",null,{"$f":"VLOOKUP(U175,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ADM04"},5,"4 or 6m2",null,"B",null,"2","too small",4,"-",4,"-",25,"SEN therapy/ MI room",null,"2","none",null,null,"ADM04","First aid room (sick room)","B",2,1.6,null,0,"-",6,4,null,8,null,{"$f":"IF(AX175=\"-\",0,ROUNDDOWN((AX175-VLOOKUP(AP175,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP175,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":2},{"$f":"IF(VLOOKUP(AP175,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX175-VLOOKUP(AP175,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP175,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"First aid posts (sick bay)","B",1.5,4,4,null,2,"ADM03",null,{"$f":"VLOOKUP(U176,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ADM03"},5,"6m2",null,"B",null,"2","too small",4,"-",6,"-",25,"SEN therapy/ MI room",null,"2","none",null,null,"ADM03","First aid post (sick bay)","B",2,1.6,null,0,"-",4,0,0,8,null,{"$f":"IF(AX176=\"-\",0,ROUNDDOWN((AX176-VLOOKUP(AP176,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP176,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(AP176,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX176-VLOOKUP(AP176,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP176,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Enclosed offices, with recep desk (only)","K",1.5,4,"-",null,null,"ADM05",null,{"$f":"VLOOKUP(U177,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ADM05"},19,"varies",null,"K",null,"4","office",8,"-","AS SOA","-",50,"split into more","main central admin office","4","reception",null,null,"ADM05","Enclosed office, with recep desk (only)","K",4,3.7,4,3.7,"-",26,12,2,16,null,{"$f":"IF(AX177=\"-\",0,ROUNDDOWN((AX177-VLOOKUP(AP177,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP177,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":5},{"$f":"IF(VLOOKUP(AP177,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX177-VLOOKUP(AP177,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP177,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":6},6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Enclosed offices, with recep window","K",1.5,4,null,null,null,"ADM06",null,{"$f":"VLOOKUP(U178,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ADM06"},19,"varies",null,"K",null,4,"office",8,"-","AS SOA","-",50,"split into more",null,"4","none",null,null,"ADM06","Enclosed office, with recep window","K",4,3.7,4,3.7,"-",26,12,2,16,null,{"$f":"IF(AX178=\"-\",0,ROUNDDOWN((AX178-VLOOKUP(AP178,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP178,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":5},{"$f":"IF(VLOOKUP(AP178,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX178-VLOOKUP(AP178,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP178,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":6},6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Enclosed offices, with recep desk (and window)","K",1.5,4,null,null,null,"ADM07",null,{"$f":"VLOOKUP(U179,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ADM05"},34,"varies",null,"K",null,8,"office",8,"-","AS SOA","-",100,"split into more",null,"4","reception",null,null,"ADM07","Enclosed office, with recep desk (and window)","K",4,3.7,4,3.7,"-",39,12,2,16,null,{"$f":"IF(AX179=\"-\",0,ROUNDDOWN((AX179-VLOOKUP(AP179,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP179,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":9},{"$f":"IF(VLOOKUP(AP179,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX179-VLOOKUP(AP179,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP179,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":9},10]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Reprographics rooms","K",2,4,null,null,null,"ADM08",null,{"$f":"VLOOKUP(U180,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ADM08"},8,"varies",null,"G",null,"1","MFD bay",6,"-","AS SOA","-",100,"split into more","enclosed","4","none",null,null,"ADM08","Reprographics room","K",4,3.7,{"$f":"VLOOKUP($AR180,$E$38:$G$54,2,FALSE)","v":4},6.8,"-",13,15,2,24,null,{"$f":"IF(AX180=\"-\",0,ROUNDDOWN((AX180-VLOOKUP(AP180,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP180,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":2},{"$f":"IF(VLOOKUP(AP180,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX180-VLOOKUP(AP180,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP180,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Work booths, MFD","-",1.5,4,2,null,null,"CIR09",null,{"$f":"VLOOKUP(U181,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CIR09"},null,"2m2",null,"-",null,"-","too small",1.5,"-",2,"-",25,"reprographics room","semi-open","2","none",null,null,"CIR09","Work booth, MFD","-",0,0,null,0,"-",2,9,null,4,null,{"$f":"IF(AX181=\"-\",0,ROUNDDOWN((AX181-VLOOKUP(AP181,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP181,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP181,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX181-VLOOKUP(AP181,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP181,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Enclosed offices, admin (head)","D",1.5,4,16,null,5,"ADM11",null,{"$f":"VLOOKUP(U182,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ADM10"},15,"16m2",null,"D",null,"5","too small",9,"-",16,"-",41,"staff room (prep and social)","accommodating head","3","none",null,null,"ADM11","Enclosed office, admin (head)","D",5,1.9,null,1,"-",16,10,2,16,null,{"$f":"IF(AX182=\"-\",0,ROUNDDOWN((AX182-VLOOKUP(AP182,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP182,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":5},{"$f":"IF(VLOOKUP(AP182,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX182-VLOOKUP(AP182,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP182,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Enclosed offices, admin (PA)","K",1.5,4,8,null,1,"ADM13",null,{"$f":"VLOOKUP(U183,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ADM10"},8,"8m2",null,"K",null,"1","too small",7,"-",{"$f":"ROUND(VLOOKUP(AA183,$E$38:$I$53,2)+(VLOOKUP(AA183,$E$38:$I$53,3,FALSE)*$AC183),0)","v":8},"-",12,"general office","enclosed office used at all times","3","none",null,null,"ADM13","Enclosed office, admin (PA)","K",4,3.7,null,1,"-",9,4,0,16,null,{"$f":"IF(AX183=\"-\",0,ROUNDDOWN((AX183-VLOOKUP(AP183,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP183,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(AP183,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX183-VLOOKUP(AP183,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP183,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Kitchenettes, room","B",2.5,4,4,null,null,"ADM21",null,{"$f":"VLOOKUP(U184,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ADM21"},4,"4m2",null,"-",null,"-","too small",4,"-",4,"-",12,"staff work room (with sink)","set out as staff kitchen","2","none",null,null,"ADM21","Kitchenette, room",null,1,3,null,0,"-",4,2,0,16,null,{"$f":"IF(AX184=\"-\",0,ROUNDDOWN((AX184-VLOOKUP(AP184,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP184,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(AP184,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX184-VLOOKUP(AP184,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP184,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Kitchenettes, bay","B",2.5,4,4,null,null,"ADM22",null,{"$f":"VLOOKUP(U185,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ADM22"},null,"4m2",null,"-",null,"-","too small",4,"-",4,"-",12,"staff work room (with sink)","set out as staff kitchen","2","none",null,null,"ADM22","Kitchenette, bay",null,1,3,null,0,"-",null,0,null,8,null,{"$f":"IF(AX185=\"-\",0,ROUNDDOWN((AX185-VLOOKUP(AP185,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP185,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(AP185,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX185-VLOOKUP(AP185,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP185,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Reception areas, entrance (50% circulation)","-",1.5,4,"-",null,null,"ADM31",null,{"$f":"VLOOKUP(U186,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ADM31"},4,"[6m2]",null,"-",null,"-","too small",4,"-","AS SOA","-",25,"split into more","space with reception desk","4","interview room",null,null,"ADM31","Reception area, entrance (50% circulation)",null,1,3,null,0,"-",4,0,2,2,null,{"$f":"IF(AX186=\"-\",0,ROUNDDOWN((AX186-VLOOKUP(AP186,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP186,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(AP186,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX186-VLOOKUP(AP186,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP186,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Reception areas, community (50% circulation)","-",1.5,4,4,null,null,"ADM32",null,{"$f":"VLOOKUP(U187,'Data Library'!$A$4:$E$466,5,FALSE)","v":"ADM32"},null,"[4m2]",null,"-",null,null,"too small",4,"-",4,"-",25,"split into more",null,"2","none",null,null,"ADM32","Reception area, community (50% circulation)",null,1,3,null,0,"-",4,0,2,null,null,{"$f":"IF(AX187=\"-\",0,ROUNDDOWN((AX187-VLOOKUP(AP187,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP187,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(AP187,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX187-VLOOKUP(AP187,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP187,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Offices","D",1.5,4,"-",null,null,"OFF00",null,{"$f":"VLOOKUP(U188,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF00"},7,"varies",null,"D",null,"1","too small",6,"-",{"$f":"ROUND(VLOOKUP(AA188,$E$38:$I$53,2)+(VLOOKUP(AA188,$E$38:$I$53,3,FALSE)*$AC188),0)","v":7},"-",25,"general office","enclosed office","2","none",null,null,"OFF00","Office","D",{"$f":"VLOOKUP($AR188,$E$38:$G$54,2,FALSE)","v":5},{"$f":"VLOOKUP($AR188,$E$38:$G$54,3,FALSE)","v":1.9},{"$f":"VLOOKUP($AR188,$E$38:$G$54,2,FALSE)","v":5},{"$f":"VLOOKUP($AR188,$E$38:$G$54,3,FALSE)","v":1.9},"-",7,5,null,null,null,{"$f":"IF(AX188=\"-\",0,ROUNDDOWN((AX188-VLOOKUP(AP188,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP188,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(AP188,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX188-VLOOKUP(AP188,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP188,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Offices (1-person)","D",1.5,4,7,null,1,"OFF01",null,{"$f":"VLOOKUP(U189,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF00"},7,"7m2 for 1",null,"D",null,1,"too small",6,"-",7,"-",9,"office (2-person)",null,"2","none",null,null,"OFF01","Office (1-person)","D",5,1.9,5,1.9,"-",7,5,null,4,null,{"$f":"IF(AX189=\"-\",0,ROUNDDOWN((AX189-VLOOKUP(AP189,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP189,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(AP189,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX189-VLOOKUP(AP189,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP189,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Offices (2-person)","D",1.5,4,9,null,2,"OFF02",null,{"$f":"VLOOKUP(U190,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF00"},9,"9m2 for 2",null,"D",null,2,"too small",6,"-",9,"-",11,"office (3-person)",null,"2","none",null,null,"OFF02","Office (2-person)","D",5,1.9,5,1.9,"-",9,5,null,4,null,{"$f":"IF(AX190=\"-\",0,ROUNDDOWN((AX190-VLOOKUP(AP190,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP190,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":2},{"$f":"IF(VLOOKUP(AP190,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX190-VLOOKUP(AP190,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP190,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":2},3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Offices (3-person)","D",1.5,4,11,null,3,"OFF03",null,{"$f":"VLOOKUP(U191,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF00"},11,"11m2 for 3",null,"D",null,3,"too small",6,"-",11,"-",13,"office (4-person)",null,"2","none",null,null,"OFF03","Office (3-person)","D",5,1.9,5,1.9,"-",11,5,null,8,null,{"$f":"IF(AX191=\"-\",0,ROUNDDOWN((AX191-VLOOKUP(AP191,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP191,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":3},{"$f":"IF(VLOOKUP(AP191,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX191-VLOOKUP(AP191,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP191,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":3},4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Offices (4-person)","D",1.5,4,13,null,4,"OFF04",null,{"$f":"VLOOKUP(U192,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF00"},13,"13m2 for 4",null,"D",null,4,"too small",6,"-",13,"-",25,"office",null,"2","none",null,null,"OFF04","Office (4-person)","D",5,1.9,5,1.9,"-",13,5,2,12,null,{"$f":"IF(AX192=\"-\",0,ROUNDDOWN((AX192-VLOOKUP(AP192,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP192,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(AP192,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX192-VLOOKUP(AP192,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP192,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":4},5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Offices (exams)","D",1.5,4,9,null,2,"OFF06",null,{"$f":"VLOOKUP(U193,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF00"},9,"9m2 for 2",null,"D",null,2,"too small",6,"-",9,"-",25,"general office",null,"3","none",null,null,"OFF06","Office (exams)","D",5,1.9,5,1.9,"-",9,5,null,16,null,{"$f":"IF(AX193=\"-\",0,ROUNDDOWN((AX193-VLOOKUP(AP193,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP193,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":2},{"$f":"IF(VLOOKUP(AP193,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX193-VLOOKUP(AP193,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP193,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":2},3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Offices (with meeting area)","C",1.5,4,"-",null,null,"OFF10",null,{"$f":"VLOOKUP(U194,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF00"},9,"varies",null,"C",null,"3","too small",6,"-",9,"-",25,"staff work room","enclosed office/ meeting","3","none",null,null,"OFF10","Office (with meeting area)","C",4,1.7,4,{"$f":"(1.7*5)/2","v":4.25},"-",9,5,null,12,null,{"$f":"IF(AX194=\"-\",0,ROUNDDOWN((AX194-VLOOKUP(AP194,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP194,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":2},{"$f":"IF(VLOOKUP(AP194,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX194-VLOOKUP(AP194,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP194,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Offices (with meeting area, 1-person)","C",1.5,4,9,null,3,"OFF11",null,{"$f":"VLOOKUP(U195,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF00"},9,"9m2 for 1+2",null,"C",null,3,"too small",6,"-",9,"-",13,"office/ meeting (2-person)",null,"2","none",null,null,"OFF11","Office (with meeting area, 1-person)","C",4,1.7,4,{"$f":"(1.7*5)/2","v":4.25},"-",9,5,null,12,null,{"$f":"IF(AX195=\"-\",0,ROUNDDOWN((AX195-VLOOKUP(AP195,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP195,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":2},{"$f":"IF(VLOOKUP(AP195,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX195-VLOOKUP(AP195,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP195,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Offices (with meeting area, 2-person)","C",1.5,4,11,null,5,"OFF12",null,{"$f":"VLOOKUP(U196,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF00"},13,"13m2 for 2+3",null,"C",null,5,"too small",6,"-",13,"-",16,"office/ meeting (3-person)",null,"3","none",null,null,"OFF12","Office (with meeting area, 2-person)","C",4,1.7,4,4.25,"-",11,5,2,12,null,{"$f":"IF(AX196=\"-\",0,ROUNDDOWN((AX196-VLOOKUP(AP196,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP196,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(AP196,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX196-VLOOKUP(AP196,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP196,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":2},5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Offices (with meeting area, 3-person)","C",1.5,4,16,null,7,"OFF13",null,{"$f":"VLOOKUP(U197,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF00"},16,"16m2 for 3+4",null,"C",null,7,"too small",6,"-",16,"-",25,"office/ meeting",null,"3","none",null,null,"OFF13","Office (with meeting area, 3-person)","C",4,1.7,4,4.25,"-",16,5,2,16,null,{"$f":"IF(AX197=\"-\",0,ROUNDDOWN((AX197-VLOOKUP(AP197,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP197,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":7},{"$f":"IF(VLOOKUP(AP197,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX197-VLOOKUP(AP197,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP197,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":3},8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Staff workrooms (technical support staff)","E",1.5,4,"-",null,null,"OFF36",null,{"$f":"VLOOKUP(U198,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF30"},10,"varies",null,"E",null,"2","too small",8,"-",11,"-",25,"staff work room","space with workbench","3","none",null,null,"OFF36","Staff workroom (technical support staff)","E",6,2.1,6,2.1,"-",11,9,null,32,null,{"$f":"IF(AX198=\"-\",0,ROUNDDOWN((AX198-VLOOKUP(AP198,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP198,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":2},{"$f":"IF(VLOOKUP(AP198,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX198-VLOOKUP(AP198,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP198,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":2},{"$f":"IF(BC198>200,ROUND(BC198*1.05,0),ROUNDUP(BC198*1.1,0))","v":3}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Staff workrooms (ICT technicians)","E",1.5,4,11,null,2,"OFF37",null,{"$f":"VLOOKUP(U199,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF30"},10,"11m2 for 2",null,"E",null,2,"office",8,"-",11,"-",25,null,null,"4","none",null,null,"OFF37","Staff workroom (ICT technicians)","E",6,2.1,6,2.1,"-",11,9,null,12,null,{"$f":"IF(AX199=\"-\",0,ROUNDDOWN((AX199-VLOOKUP(AP199,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP199,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":2},{"$f":"IF(VLOOKUP(AP199,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX199-VLOOKUP(AP199,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP199,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":2},3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Staff workrooms (premises)","E",1.5,4,11,null,2,"OFF38",null,{"$f":"VLOOKUP(U200,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF30"},10,"11m2 for 2",null,"E",null,2,"office",8,"-",11,"-",25,null,null,"2","none",null,null,"OFF38","Staff workroom (premises)","E",6,2.1,6,2.1,"-",11,9,null,24,null,{"$f":"IF(AX200=\"-\",0,ROUNDDOWN((AX200-VLOOKUP(AP200,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP200,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":2},{"$f":"IF(VLOOKUP(AP200,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX200-VLOOKUP(AP200,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP200,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":2},3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Offices (pastoral)","C",1.5,4,"-",null,null,"OFF20",null,{"$f":"VLOOKUP(U201,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF00"},9,"varies",null,"C",null,"3","too small",6,"-",{"$f":"ROUND(VLOOKUP(AA201,$E$38:$I$53,2)+(VLOOKUP(AA201,$E$38:$I$53,3,FALSE)*$AC201),0)","v":9},"-",25,"staff room (social)","office with soft chairs","2","none",null,null,"OFF20","Office (pastoral)","C",4,1.7,4,{"$f":"(1.7*5)/2","v":4.25},"-",11,5,null,12,null,{"$f":"IF(AX201=\"-\",0,ROUNDDOWN((AX201-VLOOKUP(AP201,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP201,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(AP201,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX201-VLOOKUP(AP201,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP201,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":2},5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Offices (pastoral, 1-person)","C",1.5,4,11,null,4,"OFF21",null,{"$f":"VLOOKUP(U202,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF00"},11,"12m2 for 1+3",null,"C",null,4,"too small",6,"-",{"$f":"ROUND(VLOOKUP(AA202,$E$38:$I$53,2)+(VLOOKUP(AA202,$E$38:$I$53,3,FALSE)*$AC202),0)","v":11},"-",25,null,null,"2","none",null,null,"OFF21","Office (pastoral, 1-person)","C",4,1.7,4,{"$f":"(1.7*5)/2","v":4.25},"-",11,5,2,12,null,{"$f":"IF(AX202=\"-\",0,ROUNDDOWN((AX202-VLOOKUP(AP202,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP202,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(AP202,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX202-VLOOKUP(AP202,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP202,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":2},5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Offices (pastoral, 2-person)","C",1.5,4,13,null,5,"OFF22",null,{"$f":"VLOOKUP(U203,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF00"},13,"12m2 for 2+3",null,"C",null,5,"too small",6,"-",{"$f":"ROUND(VLOOKUP(AA203,$E$38:$I$53,2)+(VLOOKUP(AA203,$E$38:$I$53,3,FALSE)*$AC203),0)","v":13},"-",25,null,null,"2","none",null,null,"OFF22","Office (pastoral, 2-person)","C",4,1.7,4,4.25,"-",13,5,2,8,null,{"$f":"IF(AX203=\"-\",0,ROUNDDOWN((AX203-VLOOKUP(AP203,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP203,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":5},{"$f":"IF(VLOOKUP(AP203,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX203-VLOOKUP(AP203,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP203,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":2},6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Offices (SENco, learning support)","C",1.5,4,11,null,4,"OFF23",null,{"$f":"VLOOKUP(U204,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF00"},11,"12m2 for 1+3",null,"C",null,4,"too small",6,"-",{"$f":"ROUND(VLOOKUP(AA204,$E$38:$I$53,2)+(VLOOKUP(AA204,$E$38:$I$53,3,FALSE)*$AC204),0)","v":11},"-",25,null,null,"3","none",null,null,"OFF23","Office (SENco, learning support)","C",4,1.7,4,4.25,"-",11,5,2,12,null,{"$f":"IF(AX204=\"-\",0,ROUNDDOWN((AX204-VLOOKUP(AP204,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP204,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(AP204,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX204-VLOOKUP(AP204,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP204,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":2},5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Offices (visiting professionals)","D",1.5,4,"-",null,null,"OFF24",null,{"$f":"VLOOKUP(U205,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF00"},7,"varies",null,"D",null,"1","too small",6,"-",{"$f":"ROUND(VLOOKUP(AA205,$E$39:$I$54,2)+(VLOOKUP(AA205,$E$39:$I$54,3,FALSE)*$AC205),0)","v":7},"-",25,"general office","enclosed office","2","none",null,null,"OFF24","Office (visiting professionals)","D",{"$f":"VLOOKUP($AR205,$E$38:$H$54,2,FALSE)","v":5},{"$f":"VLOOKUP($AR205,$E$38:$H$54,3,FALSE)","v":1.9},null,0,"-",7,5,null,4,null,{"$f":"IF(AX205=\"-\",0,ROUNDDOWN((AX205-VLOOKUP(AP205,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP205,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(AP205,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX205-VLOOKUP(AP205,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP205,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Staff rooms (prep and social)","C",1.5,4,null,null,null,"OFF51",null,{"$f":"VLOOKUP(U206,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF50"},13,"varies",null,"C",null,"5","office",12,"-",{"$f":"ROUND(VLOOKUP(AA206,$E$38:$I$53,2)+(VLOOKUP(AA206,$E$38:$I$53,3,FALSE)*$AC206),0)","v":13},"-",150,"split into more","main staff space ","3","none",null,null,"OFF51","Staff room (prep and social)","C",{"$f":"VLOOKUP($AR206,$E$38:$G$54,2,FALSE)","v":4},{"$f":"VLOOKUP($AR206,$E$38:$G$54,3,FALSE)","v":1.7},{"$f":"VLOOKUP($AR206,$E$38:$G$54,2,FALSE)","v":4},{"$f":"(1.7*4)","v":6.8},"-",41,10,2,12,null,{"$f":"IF(AX206=\"-\",0,ROUNDDOWN((AX206-VLOOKUP(AP206,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP206,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":21},{"$f":"IF(VLOOKUP(AP206,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX206-VLOOKUP(AP206,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP206,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":5},24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Staff rooms (social)","B",1.5,4,null,null,null,"OFF52",null,{"$f":"VLOOKUP(U207,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF50"},40,"varies",null,"B",null,"24","office",12,"-","AS SOA","-",150,"split into more","staff space with soft chairs ","3","none",null,null,"OFF52","Staff room (social)","B",2,1.6,null,0,"-",41,8,2,48,null,{"$f":"IF(AX207=\"-\",0,ROUNDDOWN((AX207-VLOOKUP(AP207,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP207,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":24},{"$f":"IF(VLOOKUP(AP207,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX207-VLOOKUP(AP207,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP207,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Staff workrooms (smaller teaching team)","D",1.5,4,null,null,null,"OFF32",null,{"$f":"VLOOKUP(U208,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF30"},{"$f":"ROUND(VLOOKUP(O208,$E$38:$I$54,2,FALSE)+(AC208*VLOOKUP(O208,$E$38:$I$54,3,FALSE)),0)","v":18},"varies",null,"D",null,"7","office",9,"-","AS SOA","-",50,"staff room (prep and social)","local staff space ","3","none",null,null,"OFF32","Staff workrooms (smaller teaching team)","D",{"$f":"VLOOKUP($AR208,$E$38:$G$54,2,FALSE)","v":5},{"$f":"VLOOKUP($AR208,$E$38:$G$54,3,FALSE)","v":1.9},{"$f":"VLOOKUP($AR208,$E$38:$G$54,2,FALSE)","v":5},{"$f":"VLOOKUP($AR208,$E$38:$G$54,3,FALSE)","v":1.9},"-",20,7,2,24,null,{"$f":"IF(AX208=\"-\",0,ROUNDDOWN((AX208-VLOOKUP(AP208,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP208,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":7},{"$f":"IF(VLOOKUP(AP208,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX208-VLOOKUP(AP208,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP208,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":8},8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Staff workrooms (teaching staff)","D",1.5,4,null,null,null,"OFF33",null,{"$f":"VLOOKUP(U209,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF30"},18,"varies",null,"D",null,"7","office",9,"-","AS SOA","-",50,"staff room (prep and social)","local staff space ","3","none",null,null,"OFF33","Staff workrooms (teaching staff)","D",5,1.9,{"$f":"VLOOKUP($AR209,$E$38:$G$54,2,FALSE)","v":5},{"$f":"VLOOKUP($AR209,$E$38:$G$54,3,FALSE)","v":1.9},"-",20,7,2,24,null,{"$f":"IF(AX209=\"-\",0,ROUNDDOWN((AX209-VLOOKUP(AP209,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP209,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":7},{"$f":"IF(VLOOKUP(AP209,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX209-VLOOKUP(AP209,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP209,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":8},8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Staff workrooms (specially resourced)","D",1.5,4,null,null,null,"OFF34",null,{"$f":"VLOOKUP(U210,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF30"},13,"varies",null,"D",null,4,"office",9,"-","AS SOA","-",50,"staff room (prep and social)",null,"3","none",null,null,"OFF34","Staff workroom (specially resourced)","D",5,1.9,{"$f":"VLOOKUP($AR210,$E$38:$G$54,2,FALSE)","v":5},{"$f":"VLOOKUP($AR210,$E$38:$G$54,3,FALSE)","v":1.9},"-",13,7,2,24,null,{"$f":"IF(AX210=\"-\",0,ROUNDDOWN((AX210-VLOOKUP(AP210,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP210,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(AP210,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX210-VLOOKUP(AP210,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP210,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":4},5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Meeting rooms (conference)","C",1.5,4,null,null,null,"OFF40",null,{"$f":"VLOOKUP(U211,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF40"},18,"varies",null,"C",null,8,"office",12,"-","AS SOA","-",50,"staff room (prep and social)",null,"2","none",null,null,"OFF40","Meeting room (conference)","C",4,1.7,null,0,"-",20,9,2,24,null,{"$f":"IF(AX211=\"-\",0,ROUNDDOWN((AX211-VLOOKUP(AP211,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP211,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":9},{"$f":"IF(VLOOKUP(AP211,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX211-VLOOKUP(AP211,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP211,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},10]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Laundries","-",2.5,4,4,null,null,"OFF42",null,{"$f":"VLOOKUP(U212,'Data Library'!$A$4:$E$466,5,FALSE)","v":"OFF42"},4,"4m2",null,"-",null,"-","too small",2,"-",4,"-",12,"staff work room","set out as staff laundry","1","all SEN spaces",null,null,"OFF42","Laundry",null,1,3,null,0,"-",4,0,0,0,null,{"$f":"IF(AX212=\"-\",0,ROUNDDOWN((AX212-VLOOKUP(AP212,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP212,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(AP212,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX212-VLOOKUP(AP212,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP212,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"-","-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-","-",{"$f":"VLOOKUP($AR213,$E$38:$G$54,2,FALSE)","v":0},{"$f":"VLOOKUP($AR213,$E$38:$G$54,3,FALSE)","v":0},null,null,"-",null,null,null,null,null,{"$f":"IF(AX213=\"-\",0,ROUNDDOWN((AX213-VLOOKUP(AP213,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP213,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP213,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX213-VLOOKUP(AP213,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP213,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Classroom stores, room (off classroom)","-",2,4,3,null,null,"STT00",null,{"$f":"VLOOKUP(U214,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STT00"},3,"3m2",null,null,null,"-","too small",1.5,"-",3,"-",25,"split into more","store off teaching space","2","adjacent teaching space",null,null,"STT00","Classroom store, room (off classroom)","-",0,0,null,null,"-",4,0,null,2,null,{"$f":"IF(AX214=\"-\",0,ROUNDDOWN((AX214-VLOOKUP(AP214,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP214,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP214,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX214-VLOOKUP(AP214,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP214,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Classroom stores, bay (off classroom)","-",2,4,3,null,null,"STT09",null,{"$f":"VLOOKUP(U215,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STT09"},3,"3m2",null,null,null,"-","too small",1.5,"-",3,"-",25,"split into more","semi-open bay off teaching space","2","adjacent teaching space",null,null,"STT09","Classroom store, bay (off classroom)","-",0,0,null,null,"-",3,0,null,2,null,{"$f":"IF(AX215=\"-\",0,ROUNDDOWN((AX215-VLOOKUP(AP215,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP215,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP215,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX215-VLOOKUP(AP215,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP215,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Teaching resources stores (off DT studio)","-",2,4,5,null,null,"STT18",null,{"$f":"VLOOKUP(U216,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STT10"},5,"5m2",null,null,null,"-","too small",2,"-",5,"-",25,"split into more","store with wide shelves","3","adjacent teaching space",null,null,"STT18","Teaching resources store (off DT studio)","-",0,0,null,null,"-",6,0,null,4,null,{"$f":"IF(AX216=\"-\",0,ROUNDDOWN((AX216-VLOOKUP(AP216,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP216,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP216,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX216-VLOOKUP(AP216,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP216,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Teaching resources stores (off art room)","-",2,4,5,null,null,"STT16",null,{"$f":"VLOOKUP(U217,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STT10"},5,"5m2",null,null,null,null,"too small",2,"-",5,"-",25,"split into more","store with wide shelves","3","adjacent teaching space",null,null,"STT16","Teaching resources store (off art room)","-",0,0,null,null,"-",5,0,null,2,null,{"$f":"IF(AX217=\"-\",0,ROUNDDOWN((AX217-VLOOKUP(AP217,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP217,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP217,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX217-VLOOKUP(AP217,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP217,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Equipment stores, drama","-",2,4,10,null,null,"STT08",null,{"$f":"VLOOKUP(U218,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STT08"},10,"10m2",null,null,null,"-","store",6,"-",10,"-",25,"split into more","wide enough for drama","2","adjacent teaching space",null,null,"STT08","Equipment store, drama","-",0,0,null,null,"-",10,0,null,2,null,{"$f":"IF(AX218=\"-\",0,ROUNDDOWN((AX218-VLOOKUP(AP218,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP218,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP218,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX218-VLOOKUP(AP218,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP218,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"General storerooms (off corridor)","-",2,4,5,null,null,"STN20",null,{"$f":"VLOOKUP(U219,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STN20"},5,"5m2",null,null,null,"-","too small",2,"-",5,"-",25,"split into more","store off corridor","3","none",null,null,"STN20","General storeroom (off corridor)","-",0,0,null,null,"-",6,0,null,2,null,{"$f":"IF(AX219=\"-\",0,ROUNDDOWN((AX219-VLOOKUP(AP219,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP219,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP219,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX219-VLOOKUP(AP219,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP219,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Teaching resources stores (IT/ GT off corridor)","-",2,4,5,null,null,"STT13",null,{"$f":"VLOOKUP(U220,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STT10"},5,"5m2",null,null,null,null,"too small",2,"-",5,"-",25,"split into more","store off corridor","2","none",null,null,"STT13","Teaching resources store (IT/ GT off corridor)","-",0,0,null,null,"-",5,0,null,4,null,{"$f":"IF(AX220=\"-\",0,ROUNDDOWN((AX220-VLOOKUP(AP220,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP220,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP220,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX220-VLOOKUP(AP220,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP220,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Teaching resources stores (music)","-",2,4,5,null,null,"STT17",null,{"$f":"VLOOKUP(U221,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STT10"},5,"5m2",null,null,null,null,"too small",2,"-",5,"-",25,"split into more",null,"3","adjacent music space",null,null,"STT17","Teaching resources store (music)","-",0,0,null,null,"-",5,0,null,4,null,{"$f":"IF(AX221=\"-\",0,ROUNDDOWN((AX221-VLOOKUP(AP221,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP221,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP221,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX221-VLOOKUP(AP221,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP221,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Food stores, off food room","-",2,4,5,null,null,"STT35",null,{"$f":"VLOOKUP(U222,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STT35"},5,"5m2",null,null,null,"-","too small",2,"-",5,"-",9,"food store/ prep room","hygienic store","3","adjacent food room",null,null,"STT35","Food store, off food room","-",0,0,null,null,"-",5,0,null,4,null,{"$f":"IF(AX222=\"-\",0,ROUNDDOWN((AX222-VLOOKUP(AP222,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP222,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP222,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX222-VLOOKUP(AP222,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP222,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Teaching resources stores, room (off LRC)","-",2,4,3,null,null,"STT41",null,{"$f":"VLOOKUP(U223,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STT10"},3,"3m2",null,null,null,null,"too small",1.5,"-",3,"-",25,"split into more",null,"2","none",null,null,"STT41","Teaching resources store, room (off LRC)","-",0,0,null,null,"-",3,0,null,4,null,{"$f":"IF(AX223=\"-\",0,ROUNDDOWN((AX223-VLOOKUP(AP223,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP223,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP223,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX223-VLOOKUP(AP223,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP223,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Classroom stores, room (off SEN room)","-",2,4,5,null,null,"STT42",null,{"$f":"VLOOKUP(U224,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STT00"},5,"5m2",null,null,null,null,"too small",2,"-",5,"-",25,"split into more",null,"3","adjacent SEN room",null,null,"STT42","Classroom store, room (off SEN room)","-",0,0,null,null,"-",5,0,null,4,null,{"$f":"IF(AX224=\"-\",0,ROUNDDOWN((AX224-VLOOKUP(AP224,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP224,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP224,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX224-VLOOKUP(AP224,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP224,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Science prep rooms (central)","-",2.5,4,null,null,null,"STT21",null,{"$f":"VLOOKUP(U225,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STT20"},null,"varies",null,null,null,"-","specialist store",12,"-","AS SOA","-",150,"split into more","serviced store/ prep area","4","all science laboratories and studios served by prep room",null,null,"STT21","Science prep room (central)",null,0,22.5,0,50,"-",30,10,2,4,null,{"$f":"IF(AX225=\"-\",0,ROUNDDOWN((AX225-VLOOKUP(AP225,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP225,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(AP225,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX225-VLOOKUP(AP225,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP225,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Science prep rooms (satellite)","-",2.5,4,null,null,null,"STT22",null,{"$f":"VLOOKUP(U226,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STT20"},null,"varies",null,null,null,null,"specialist store",6,"-",12,"-",50,"split into more","serviced store/ prep area","4","all science laboratories and studios served by prep room",null,null,"STT22","Science prep room (satellite)","K",0,22.5,0,50,"-",26,9,2,4,null,{"$f":"IF(AX226=\"-\",0,ROUNDDOWN((AX226-VLOOKUP(AP226,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP226,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(AP226,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX226-VLOOKUP(AP226,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP226,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Chemicals stores, science","-",2,4,7,null,null,"STT23",null,{"$f":"VLOOKUP(U227,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STT23"},7,"7 or 10m2",null,null,null,"-","store",6,"-","AS SOA","-",25,"science prep room","specialist store for chemicals","4","all science laboratories and studios",null,null,"STT23","Chemicals store, science","-",{"$f":"VLOOKUP($AR227,$E$38:$G$54,2,FALSE)","v":0},{"$f":"VLOOKUP($AR227,$E$38:$G$54,3,FALSE)","v":0},null,0,"-",7,0,null,6,null,{"$f":"IF(AX227=\"-\",0,ROUNDDOWN((AX227-VLOOKUP(AP227,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP227,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP227,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX227-VLOOKUP(AP227,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP227,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"DT prep rooms","-",3.5,4,null,null,null,"STT32",null,{"$f":"VLOOKUP(U228,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STT32"},null,"34 or 41m2",null,null,null,"-","specialist store",34,"-","AS SOA","-",150,"split into more","prep area with machines","4","all product design workshops",null,null,"STT32","DT prep room","I",18,3.9,null,1,"-",26,3,null,2,null,{"$f":"IF(AX228=\"-\",0,ROUNDDOWN((AX228-VLOOKUP(AP228,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP228,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":2},{"$f":"IF(VLOOKUP(AP228,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX228-VLOOKUP(AP228,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP228,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Food prep rooms","-",3.5,4,10,null,null,"STT34",null,{"$f":"VLOOKUP(U229,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STT34"},10,"10m2",null,null,null,"-","food store",8,"-",10,"-",25,"science prep room","prep area for food area","4","all food rooms and food studios",null,null,"STT34","Food prep room","-",0,0,null,null,"-",10,0,null,2,null,{"$f":"IF(AX229=\"-\",0,ROUNDDOWN((AX229-VLOOKUP(AP229,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP229,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP229,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX229-VLOOKUP(AP229,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP229,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Sports equipment stores, internal","-",2,4,null,null,null,"STH00",null,{"$f":"VLOOKUP(U230,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STH00"},null,"10% of hall area",null,"-",null,"-","too small",2,"-",8,"-",150,"split or supplementary","off hall or in sports block","3","adjacent sports provision",null,null,"STH00","Sports equipment store, internal","-",0,0,null,null,"-",4,0,null,2,null,{"$f":"IF(AX230=\"-\",0,ROUNDDOWN((AX230-VLOOKUP(AP230,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP230,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP230,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX230-VLOOKUP(AP230,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP230,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Sports equipment stores, internal (sports hall)","-",2,4,null,null,null,"STH01",null,{"$f":"VLOOKUP(U231,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STH00"},null,"10% of hall area",null,"-",null,"-","PE store(s)",18,"-","AS SOA","-",150,"split or supplementary",null,"3","adjacent sports hall",null,null,"STH01","Sports equipment store, internal (sports hall)","-",0,0,null,null,"-",4,0,null,6,null,{"$f":"IF(AX231=\"-\",0,ROUNDDOWN((AX231-VLOOKUP(AP231,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP231,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP231,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX231-VLOOKUP(AP231,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP231,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Sports equipment stores, internal (community)","-",2,4,4,null,null,"STH02",null,{"$f":"VLOOKUP(U232,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STH00"},4,"10% of hall area",null,"-",null,"-","too small",2,"-",4,"-",50,"split or supplementary",null,"1","none",null,null,"STH02","Sports equipment store, internal (community)","-",0,0,null,null,"-",4,0,null,2,null,{"$f":"IF(AX232=\"-\",0,ROUNDDOWN((AX232-VLOOKUP(AP232,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP232,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP232,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX232-VLOOKUP(AP232,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP232,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Sports equipment stores, internal (activity studio)","-",2,4,null,null,null,"STH03",null,{"$f":"VLOOKUP(U233,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STH00"},null,"10% of studio area",null,"-",null,"-","PE store(s)",12,"-","AS SOA","-",50,"split or supplementary",null,"2","adjacent activity studio",null,null,"STH03","Sports equipment store, internal (activity studio)","-",0,0,null,null,"-",4,0,null,2,null,{"$f":"IF(AX233=\"-\",0,ROUNDDOWN((AX233-VLOOKUP(AP233,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP233,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP233,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX233-VLOOKUP(AP233,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP233,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Sports equipment stores, internal (off hall)","-",2,4,null,null,null,"STH04",null,{"$f":"VLOOKUP(U234,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STH00"},null,"10% of hall area",null,"-",null,"-","too small",12,"-",15,"-",50,"split or supplementary",null,"2","adjacent hall",null,null,"STH04","Sports equipment store, internal (off hall)","-",0,0,null,null,"-",4,0,null,2,null,{"$f":"IF(AX234=\"-\",0,ROUNDDOWN((AX234-VLOOKUP(AP234,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP234,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP234,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX234-VLOOKUP(AP234,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP234,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Sports equipment stores, external","-",2,4,8,null,null,"STH05",null,{"$f":"VLOOKUP(U235,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STH05"},8,"8m2",null,"-",null,"-","too small",2,"-",8,"-",25,"split or supplementary","direct access to outdoors","3","none",null,null,"STH05","Sports equipment store, external","-",0,0,null,null,"-",8,0,null,0,null,{"$f":"IF(AX235=\"-\",0,ROUNDDOWN((AX235-VLOOKUP(AP235,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP235,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP235,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX235-VLOOKUP(AP235,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP235,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Furniture stores","-",2,4,null,null,null,"STH10",null,{"$f":"VLOOKUP(U236,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STH10"},null,null,null,"-",null,"-","store",6,"-",20,"-",50,"split into more","wide enough for furniture","2"," adjacent hall",null,null,"STH10","Furniture store","-",0,0,null,null,"-",16,0,null,2,null,{"$f":"IF(AX236=\"-\",0,ROUNDDOWN((AX236-VLOOKUP(AP236,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP236,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP236,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX236-VLOOKUP(AP236,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP236,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Furniture stores (chair/ table, off hall)","-",2,4,null,null,null,"STH11",null,{"$f":"VLOOKUP(U237,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STH10"},null,null,null,"-",null,"-","store",6,"-","AS SOA","-",50,"split into more",null,"3","dining area(s)",null,null,"STH11","Furniture store (chair/ table, off hall)","-",0,0,null,null,"-",16,0,null,4,null,{"$f":"IF(AX237=\"-\",0,ROUNDDOWN((AX237-VLOOKUP(AP237,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP237,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP237,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX237-VLOOKUP(AP237,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP237,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Furniture stores (chair, off hall)","-",2,4,null,null,null,"STH12",null,{"$f":"VLOOKUP(U238,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STH10"},null,null,null,"-",null,"-","store",6,"-",20,"-",50,"split into more",null,"2"," adjacent hall",null,null,"STH12","Furniture store (chair, off hall)","-",0,0,null,null,"-",16,0,null,4,null,{"$f":"IF(AX238=\"-\",0,ROUNDDOWN((AX238-VLOOKUP(AP238,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP238,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP238,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX238-VLOOKUP(AP238,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP238,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"-","-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2"," adjacent hall",null,null,null,"-","-",0,0,null,null,"-",null,null,null,null,null,{"$f":"IF(AX239=\"-\",0,ROUNDDOWN((AX239-VLOOKUP(AP239,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP239,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP239,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX239-VLOOKUP(AP239,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP239,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Dining furniture stores, and servery","-",2,4,null,null,null,"STH15",null,{"$f":"VLOOKUP(U240,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STH15"},null,null,null,"-",null,"-","store",6,"-",20,"-",50,"split into more",null,"3","adjacent dining area",null,null,"STH15","Dining furniture store, and servery","-",0,0,null,null,"-",16,0,null,4,null,{"$f":"IF(AX240=\"-\",0,ROUNDDOWN((AX240-VLOOKUP(AP240,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP240,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP240,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX240-VLOOKUP(AP240,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP240,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Retractable seating storage (off hall)","-",2,4,16,null,null,"STH20",null,{"$f":"VLOOKUP(U241,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STH20"},16,"16m2",null,"-",null,"-","store",12,"-",16,"-",50,"split into more","specifically for movable bleachers","3","main hall",null,null,"STH20","Retractable seating storage (off hall)","-",0,0,null,null,"-",16,0,null,4,null,{"$f":"IF(AX241=\"-\",0,ROUNDDOWN((AX241-VLOOKUP(AP241,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP241,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP241,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX241-VLOOKUP(AP241,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP241,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Coats and bags stores (coat hooks)","-",2,4,null,null,null,"STN01",null,{"$f":"VLOOKUP(U242,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STN00"},null,"[15m2]",null,"-",null,"-","too small",1.5,"-",3,"-",25,"split into more","750 deep net area for coat hooks","3","none",null,null,"STN01","Coats and bag store (coat hooks)","-",0,0,null,null,"-",4,0,null,2,null,{"$f":"IF(AX242=\"-\",0,ROUNDDOWN((AX242-VLOOKUP(AP242,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP242,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP242,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX242-VLOOKUP(AP242,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP242,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Coats and bags stores (lockers)","-",2,4,null,null,null,"STN02",null,{"$f":"VLOOKUP(U243,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STN00"},null,"[1.5m2]",null,null,null,"-","too small",1.5,"-",4,"-",25,"split into more","750 deep net area for lockers","2","none",null,null,"STN02","Coats and bag store (lockers)","-",0,0,null,null,"-",4,0,null,4,null,{"$f":"IF(AX243=\"-\",0,ROUNDDOWN((AX243-VLOOKUP(AP243,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP243,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP243,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX243-VLOOKUP(AP243,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP243,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Coats and bags stores (community lockers)","-",2,4,4,null,null,"STN03",null,{"$f":"VLOOKUP(U244,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STN00"},4,"4m2",null,null,null,"-","too small",1.5,"-",4,"-",12,"split or supplementary",null,"1","none",null,null,"STN03","Coats and bag store (community lockers)","-",0,0,null,null,"-",4,0,null,2,null,{"$f":"IF(AX244=\"-\",0,ROUNDDOWN((AX244-VLOOKUP(AP244,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP244,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP244,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX244-VLOOKUP(AP244,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP244,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Equipment stores, appliance bay","-",2,4,1.5,null,null,"CIR06",null,{"$f":"VLOOKUP(U245,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CIR06"},1.5,"1.5m2",null,null,null,"-","too small",1.5,"-",1.5,"-",6,"split into more",null,"1","none",null,null,"CIR06","Equipment store, appliance bay","-",0,0,null,null,"-",1.5,2,0,2,null,{"$f":"IF(AX245=\"-\",0,ROUNDDOWN((AX245-VLOOKUP(AP245,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP245,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP245,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX245-VLOOKUP(AP245,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP245,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Secure storerooms","-",2,4,8,null,null,"STN50",null,{"$f":"VLOOKUP(U246,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STN50"},8,"8m2",null,null,null,"-","too small",1.5,"-",8,"-",25,"split into more","secure enclosure","7","all spaces used for exams, when exams needed",null,null,"STN50","Secure storeroom","-",0,0,null,null,"-",8,0,null,2,null,{"$f":"IF(AX246=\"-\",0,ROUNDDOWN((AX246-VLOOKUP(AP246,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP246,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP246,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX246-VLOOKUP(AP246,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP246,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"General storerooms (central stock)","-",2,4,8,null,null,"STN22",null,{"$f":"VLOOKUP(U247,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STN20"},8,"8m2",null,null,null,null,"too small",1.5,"-",8,"-",25,"split into more",null,"2","none",null,null,"STN22","General storeroom (central stock)","-",0,0,null,null,"-",8,0,null,4,null,{"$f":"IF(AX247=\"-\",0,ROUNDDOWN((AX247-VLOOKUP(AP247,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP247,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP247,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX247-VLOOKUP(AP247,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP247,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"General storerooms (community)","-",2,4,4,null,null,"STN25",null,{"$f":"VLOOKUP(U248,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STN20"},4,"4m2",null,null,null,null,"too small",1.5,"-",4,"-",12,"split or supplementary",null,"2","none",null,null,"STN25","General storeroom (community)","-",0,0,null,null,"-",null,0,null,4,null,{"$f":"IF(AX248=\"-\",0,ROUNDDOWN((AX248-VLOOKUP(AP248,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP248,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP248,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX248-VLOOKUP(AP248,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP248,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Cleaners' stores","-",2,4,1.5,null,null,"STN31",null,{"$f":"VLOOKUP(U249,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STN31"},1.5,"1.5m2",null,null,null,"-","too small",1.5,"-",1.5,"-",12,"split into more","store with mop sink","2","none",null,null,"STN31","Cleaners' store","-",0,0,null,null,"-",1.5,0,null,6,null,{"$f":"IF(AX249=\"-\",0,ROUNDDOWN((AX249-VLOOKUP(AP249,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP249,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP249,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX249-VLOOKUP(AP249,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP249,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Equipment stores, maintenance","-",2,4,8,null,null,"STN32",null,{"$f":"VLOOKUP(U250,'Data Library'!$A$4:$E$466,5,FALSE)","v":"STN32"},8,"8m2",null,null,null,null,"store",4,"-",8,"-",25,"split into more",null,"2","none",null,null,"STN32","Equipment store, maintenance","-",0,0,null,null,"-",8,0,null,2,null,{"$f":"IF(AX250=\"-\",0,ROUNDDOWN((AX250-VLOOKUP(AP250,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP250,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP250,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX250-VLOOKUP(AP250,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP250,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"-","-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-","-",0,0,null,null,"-",null,null,null,null,null,{"$f":"IF(AX251=\"-\",0,ROUNDDOWN((AX251-VLOOKUP(AP251,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP251,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP251,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX251-VLOOKUP(AP251,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP251,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Food prep areas, kitchen",null,null,null,null,null,null,"KIT00",null,{"$f":"VLOOKUP(U252,'Data Library'!$A$4:$E$466,5,FALSE)","v":"KIT00"},null,null,null,"-",null,"-","too small",25,"-","AS SOA","-",250,"split into more","specialist space","4","dining area and any servery areas",null,null,"KIT00","Food prep area, kitchen","J",24,4.5,null,1,"-",null,4,2,4,null,{"$f":"IF(AX252=\"-\",0,ROUNDDOWN((AX252-VLOOKUP(AP252,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP252,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":-5},{"$f":"IF(VLOOKUP(AP252,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX252-VLOOKUP(AP252,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP252,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},-6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Food prep areas, kitchen (servery & wash-up)",null,null,null,null,null,null,"KIT01",null,{"$f":"VLOOKUP(U253,'Data Library'!$A$4:$E$466,5,FALSE)","v":"KIT00"},null,null,null,"-",null,null,"too small",25,"-","AS SOA","-",250,"split into more","specialist space","4","dining area and any servery areas",null,null,"KIT01","Food prep area, kitchen (servery & wash-up)","J",24,4.5,null,null,"-",null,4,2,10,null,{"$f":"IF(AX253=\"-\",0,ROUNDDOWN((AX253-VLOOKUP(AP253,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP253,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":-5},{"$f":"IF(VLOOKUP(AP253,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX253-VLOOKUP(AP253,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP253,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},-6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Food prep areas, kitchen (prep/ servery suite)",null,null,null,null,null,null,"KIT02",null,{"$f":"VLOOKUP(U254,'Data Library'!$A$4:$E$466,5,FALSE)","v":"KIT00"},null,null,null,"-",null,null,"kitchen prep, servery & wash-up",32,"-","AS SOA","-",250,"split into more","specialist space","4","dining area and any servery areas",null,null,"KIT02","Food prep area, kitchen (prep/ servery suite)","J",24,4.5,null,1,"-",null,4,null,10,null,{"$f":"IF(AX254=\"-\",0,ROUNDDOWN((AX254-VLOOKUP(AP254,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP254,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":-5},{"$f":"IF(VLOOKUP(AP254,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX254-VLOOKUP(AP254,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP254,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},-6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Offices, kitchen",null,null,null,null,null,null,"KIT11",null,{"$f":"VLOOKUP(U255,'Data Library'!$A$4:$E$466,5,FALSE)","v":"KIT11"},null,null,null,"-",null,null,"too small",1.5,"-",3,"-",25,"split into more",null,"4","school kitchen areas",null,null,"KIT11","Office, kitchen","A",2,1.1000000000000001,null,1,"-",null,8,null,10,null,{"$f":"IF(AX255=\"-\",0,ROUNDDOWN((AX255-VLOOKUP(AP255,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP255,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":-1},{"$f":"IF(VLOOKUP(AP255,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX255-VLOOKUP(AP255,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP255,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":1},-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Food stores, kitchen",null,null,null,null,null,null,"KIT20",null,{"$f":"VLOOKUP(U256,'Data Library'!$A$4:$E$466,5,FALSE)","v":"KIT20"},null,null,null,"-",null,"-","too small",1.5,"-",5,"-",25,"split into more",null,"4","school kitchen areas",null,null,"KIT20","Food store, kitchen","-",0,0,null,null,"-",null,0,null,4,null,{"$f":"IF(AX256=\"-\",0,ROUNDDOWN((AX256-VLOOKUP(AP256,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP256,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP256,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX256-VLOOKUP(AP256,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP256,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Food stores, kitchen (dry)",null,null,null,null,null,null,"KIT21",null,{"$f":"VLOOKUP(U257,'Data Library'!$A$4:$E$466,5,FALSE)","v":"KIT20"},null,null,null,"-",null,null,"too small",1.5,"-",5,"-",25,"split into more",null,"4","school kitchen areas",null,null,"KIT21","Food store, kitchen (dry)","-",0,0,null,null,"-",null,0,null,null,null,{"$f":"IF(AX257=\"-\",0,ROUNDDOWN((AX257-VLOOKUP(AP257,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP257,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP257,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX257-VLOOKUP(AP257,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP257,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Cold stores, kitchen",null,null,null,null,null,null,"KIT25",null,{"$f":"VLOOKUP(U258,'Data Library'!$A$4:$E$466,5,FALSE)","v":"KIT25"},null,null,null,"-",null,null,"too small",1.5,"-",4,"-",25,"split into more","specialist store","4","school kitchen areas",null,null,"KIT25","Cold store, kitchen","-",0,0,null,null,"-",null,0,null,null,null,{"$f":"IF(AX258=\"-\",0,ROUNDDOWN((AX258-VLOOKUP(AP258,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP258,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP258,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX258-VLOOKUP(AP258,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP258,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Cold stores, kitchen (freezer)",null,null,null,null,null,null,"KIT26",null,{"$f":"VLOOKUP(U259,'Data Library'!$A$4:$E$466,5,FALSE)","v":"KIT25"},null,null,null,"-",null,null,"too small",1.5,"-",3,"-",25,"split into more","specialist store","4","school kitchen areas",null,null,"KIT26","Cold store, kitchen (freezer)","-",0,0,null,null,"-",null,0,null,8,null,{"$f":"IF(AX259=\"-\",0,ROUNDDOWN((AX259-VLOOKUP(AP259,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP259,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP259,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX259-VLOOKUP(AP259,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP259,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Toilets, kitchen (with changing area)",null,null,null,null,null,null,"KIT40",null,{"$f":"VLOOKUP(U260,'Data Library'!$A$4:$E$466,5,FALSE)","v":"KIT40"},null,"1.5 or 3m2",null,"-",null,null,"too small",1.5,"-",3,"-",12,"split into more","toilet and lobby","4","school kitchen areas",null,null,"KIT40","Toilet, kitchen (with changing area)","T",0.5,3,null,null,"-",null,0,null,4,null,{"$f":"IF(AX260=\"-\",0,ROUNDDOWN((AX260-VLOOKUP(AP260,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP260,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(AP260,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX260-VLOOKUP(AP260,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP260,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,null,null,"-",null,null,null,2,null,{"$f":"IF(AX261=\"-\",0,ROUNDDOWN((AX261-VLOOKUP(AP261,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP261,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP261,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX261-VLOOKUP(AP261,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP261,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Changing rooms, with showers (pupils)","A",null,null,null,null,null,"TOC01",null,{"$f":"VLOOKUP(U262,'Data Library'!$A$4:$E$466,5,FALSE)","v":"TOC01"},null,null,null,"A",null,"45","accessible/ staff toilet",12,"-","AS SOA","-",150,"split into more","specialist space","3","all indoor and outdoor sports facilities ",null,null,"TOC01","Changing room, with showers (pupils)","A",{"$f":"VLOOKUP($AR262,$E$38:$G$54,2,FALSE)","v":2},{"$f":"VLOOKUP($AR262,$E$38:$G$54,3,FALSE)","v":1.1000000000000001},null,null,"-",null,0,null,null,null,{"$f":"IF(AX262=\"-\",0,ROUNDDOWN((AX262-VLOOKUP(AP262,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP262,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":-1},{"$f":"IF(VLOOKUP(AP262,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX262-VLOOKUP(AP262,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP262,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(BC262>200,ROUND(BC262*1.05,0),ROUNDUP(BC262*1.1,0))","v":-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Accessible (and staff) changing rooms",null,null,null,6,null,null,"TOC02",null,{"$f":"VLOOKUP(U263,'Data Library'!$A$4:$E$466,5,FALSE)","v":"TOC02"},6,null,null,"-",null,"1","PE store",4,"-",6,"-",12,"split into more","specialist space","2","all indoor and outdoor sports facilities ",null,null,"TOC02","Accessible (and staff) changing room","-",0.5,3,null,null,"-",6,0,null,null,null,{"$f":"IF(AX263=\"-\",0,ROUNDDOWN((AX263-VLOOKUP(AP263,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP263,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":1},{"$f":"IF(VLOOKUP(AP263,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX263-VLOOKUP(AP263,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP263,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Changing rooms, ablutions and shoe space",null,null,null,null,null,null,"TOC03",null,{"$f":"VLOOKUP(U264,'Data Library'!$A$4:$E$466,5,FALSE)","v":"TOC03"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TOC03","Changing rooms, ablutions and shoe space","-",0.5,3,null,null,"-",null,null,null,2,null,{"$f":"IF(AX264=\"-\",0,ROUNDDOWN((AX264-VLOOKUP(AP264,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP264,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(AP264,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX264-VLOOKUP(AP264,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP264,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Hygiene rooms",null,null,null,12,null,null,"TOC04",null,{"$f":"VLOOKUP(U265,'Data Library'!$A$4:$E$466,5,FALSE)","v":"TOC04"},12,null,null,"-",null,"-","accessible/ staff toilet",9,"-",12,"-",25,"split into more","specialist space","5","all SEN spaces",null,null,"TOC04","Hygiene room","-",0.5,3,null,null,"-",12,0,null,4,null,{"$f":"IF(AX265=\"-\",0,ROUNDDOWN((AX265-VLOOKUP(AP265,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP265,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":3},{"$f":"IF(VLOOKUP(AP265,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX265-VLOOKUP(AP265,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP265,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Hygiene rooms (small 1 door)",null,null,null,8,null,null,"TOC05",null,{"$f":"VLOOKUP(U266,'Data Library'!$A$4:$E$466,5,FALSE)","v":"TOC04"},8,null,null,"-",null,"-","accessible/ staff toilet",7,"-",8,"-",25,"split into more","specialist space","5","all SEN spaces",null,null,"TOC05","Hygiene room (small 1 door)","-",0.5,3,null,null,"-",8,0,null,8,null,{"$f":"IF(AX266=\"-\",0,ROUNDDOWN((AX266-VLOOKUP(AP266,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP266,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":2},{"$f":"IF(VLOOKUP(AP266,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX266-VLOOKUP(AP266,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP266,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Hygiene rooms, small 2 doors",null,null,null,9,null,null,"TOC06",null,{"$f":"VLOOKUP(U267,'Data Library'!$A$4:$E$466,5,FALSE)","v":"TOC04"},9,null,null,"-",null,"-","accessible/ staff toilet",7,"-",9,"-",25,"split into more","specialist space","5","all SEN spaces",null,null,"TOC06","Hygiene room, small 2 doors","-",0.5,3,null,null,"-",9,0,null,8,null,{"$f":"IF(AX267=\"-\",0,ROUNDDOWN((AX267-VLOOKUP(AP267,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP267,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":2},{"$f":"IF(VLOOKUP(AP267,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX267-VLOOKUP(AP267,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP267,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Supervisable toilets (early years)",null,null,null,null,null,null,"TOC31",null,{"$f":"VLOOKUP(U268,'Data Library'!$A$4:$E$466,5,FALSE)","v":"TOC30"},null,null,null,"-",null,"-","individual toilet",2,"-",3,"-",6,"split into more","toilet","3","none if others available",null,null,"TOC31","Supervisable toilets (early years)","-",0.5,3,null,null,"-",15,0,null,null,null,{"$f":"IF(AX268=\"-\",0,ROUNDDOWN((AX268-VLOOKUP(AP268,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP268,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":4},{"$f":"IF(VLOOKUP(AP268,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX268-VLOOKUP(AP268,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP268,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Supervisable toilets (SEN)",null,null,null,null,null,null,"TOC32",null,{"$f":"VLOOKUP(U269,'Data Library'!$A$4:$E$466,5,FALSE)","v":"TOC30"},null,null,null,"-",null,"-","individual toilet",2,"-",3,"-",6,"split into more","toilet","3","none if others available",null,null,"TOC32","Supervisable toilets (SEN)","-",0.5,3,null,null,"-",null,0,null,null,null,{"$f":"IF(AX269=\"-\",0,ROUNDDOWN((AX269-VLOOKUP(AP269,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP269,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(AP269,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX269-VLOOKUP(AP269,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP269,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Toilets, suite (pupils)",null,null,null,null,null,null,"TOC13",null,{"$f":"VLOOKUP(U270,'Data Library'!$A$4:$E$466,5,FALSE)","v":"TOC10"},null,null,null,"-",null,"-","individual toilet",5,"-",19.5,"-",150,"split into more","toilet","3","none if others available",null,null,"TOC13","Toilets, suite (pupils)","-",0.5,3,null,null,"-",null,0,null,null,null,{"$f":"IF(AX270=\"-\",0,ROUNDDOWN((AX270-VLOOKUP(AP270,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP270,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(AP270,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX270-VLOOKUP(AP270,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP270,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Toilets, suite (pupils, other)",null,null,null,null,null,null,"TOC14",null,{"$f":"VLOOKUP(U271,'Data Library'!$A$4:$E$466,5,FALSE)","v":"TOC10"},null,null,null,"-",null,"-","individual toilet",5,"-",12,"-",150,"split into more","toilet","3","none if others available",null,null,"TOC14","Toilets, suite (pupils, other)","-",0.5,3,null,null,"-",null,0,null,null,null,{"$f":"IF(AX271=\"-\",0,ROUNDDOWN((AX271-VLOOKUP(AP271,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP271,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(AP271,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX271-VLOOKUP(AP271,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP271,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Toilets, individual (pupil)",null,null,null,2,null,null,"TOC15",null,{"$f":"VLOOKUP(U272,'Data Library'!$A$4:$E$466,5,FALSE)","v":"TOC15"},3,null,null,"-",null,"-","too small",2,"-",2,"-",6,"pupil toilet suite(s)","toilet","3","none if others available",null,null,"TOC15","Toilet, individual (pupil)","-",0.5,3,null,null,"-",2,0,null,null,null,{"$f":"IF(AX272=\"-\",0,ROUNDDOWN((AX272-VLOOKUP(AP272,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP272,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(AP272,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX272-VLOOKUP(AP272,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP272,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Toilets, individual (staff)",null,null,null,2,null,null,"TOC16",null,{"$f":"VLOOKUP(U273,'Data Library'!$A$4:$E$466,5,FALSE)","v":"TOC15"},3,null,null,"-",null,"-","too small",2,"-",2,"-",6,"staff toilet suite(s)","toilet","3","none if others available",null,null,"TOC16","Toilet, individual (staff)","-",0.5,3,null,null,"-",2,0,null,null,null,{"$f":"IF(AX273=\"-\",0,ROUNDDOWN((AX273-VLOOKUP(AP273,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP273,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(AP273,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX273-VLOOKUP(AP273,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP273,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Accessible (and staff) toilets",null,null,null,3.75,null,null,"TOC21",null,{"$f":"VLOOKUP(U274,'Data Library'!$A$4:$E$466,5,FALSE)","v":"TOC21"},3.5,null,null,"-",null,"-","individual toilet",3,"-",3.75,"-",12,"hygiene room","toilet","4","all spaces within 40m if required by wheelchair users",null,null,"TOC21","Accessible (and staff) toilet","-",0.5,3,null,null,"-",null,0,null,null,null,{"$f":"IF(AX274=\"-\",0,ROUNDDOWN((AX274-VLOOKUP(AP274,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP274,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(AP274,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX274-VLOOKUP(AP274,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP274,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Toilets, suite (staff)",null,null,null,null,null,null,"TOC12",null,{"$f":"VLOOKUP(U275,'Data Library'!$A$4:$E$466,5,FALSE)","v":"TOC10"},null,null,null,"-",null,"-","individual toilet",5,"-",12,"-",150,"split into more","toilet","3","none if others available",null,null,"TOC12","Toilets, suite (staff)","-",0.5,3,null,null,"-",null,0,null,null,null,{"$f":"IF(AX275=\"-\",0,ROUNDDOWN((AX275-VLOOKUP(AP275,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP275,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":0},{"$f":"IF(VLOOKUP(AP275,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX275-VLOOKUP(AP275,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP275,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,null,"-",null,null,null,null,null,{"$f":"IF(AX276=\"-\",0,ROUNDDOWN((AX276-VLOOKUP(AP276,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP276,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP276,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX276-VLOOKUP(AP276,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP276,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,0,"Server rooms",null,null,null,null,null,null,"PLA10",null,{"$f":"VLOOKUP(U277,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PLA10"},null,null,null,"-",null,"-","too small",3,"-","AS SOA","-",50,"split into more","specialist space","7","none",null,null,"PLA10","Server room","-",0,0,null,null,"-",null,0,null,null,null,{"$f":"IF(AX277=\"-\",0,ROUNDDOWN((AX277-VLOOKUP(AP277,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP277,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP277,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX277-VLOOKUP(AP277,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP277,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,1,"Server rooms (1-cabinet)",null,null,null,7.5,null,null,"PLA11",null,{"$f":"VLOOKUP(U278,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PLA10"},{"$f":"R278","v":7.5},null,null,"-",null,"-","too small",5,"-","AS SOA","-",50,"split into more","specialist space","7","none",null,null,"PLA11","Server room (1-cabinet)","-",0,0,null,null,"-",null,0,null,null,null,{"$f":"IF(AX278=\"-\",0,ROUNDDOWN((AX278-VLOOKUP(AP278,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP278,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP278,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX278-VLOOKUP(AP278,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP278,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,2,"Server rooms (2-cabinet)",null,null,null,10.199999999999999,null,null,"PLA12",null,{"$f":"VLOOKUP(U279,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PLA10"},{"$f":"R279","v":10.199999999999999},null,null,"-",null,"-","server room (1 cabinet)",7,"-","AS SOA","-",50,"split into more","specialist space","7","none",null,null,"PLA12","Server room (2-cabinet)","-",0,0,null,null,"-",null,0,null,null,null,{"$f":"IF(AX279=\"-\",0,ROUNDDOWN((AX279-VLOOKUP(AP279,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP279,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP279,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX279-VLOOKUP(AP279,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP279,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,3,"Server rooms (3-cabinet)",null,null,null,12.9,null,null,"PLA13",null,{"$f":"VLOOKUP(U280,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PLA10"},12.9,null,null,"-",null,"-","server room (2 cabinets)",9,"-","AS SOA","-",50,"split into more","specialist space","7","none",null,null,"PLA13","Server room (3-cabinet)","-",0,0,null,null,"-",null,0,null,null,null,{"$f":"IF(AX280=\"-\",0,ROUNDDOWN((AX280-VLOOKUP(AP280,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP280,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP280,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX280-VLOOKUP(AP280,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP280,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,4,"Server rooms (4-cabinet)",null,null,null,15.6,null,null,"PLA14",null,{"$f":"VLOOKUP(U281,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PLA10"},15.6,null,null,"-",null,"-","server room (3 cabinets)",11,"-","AS SOA","-",50,"split into more","specialist space","7","none",null,null,"PLA14","Server room (4-cabinet)","-",0,0,null,null,"-",null,0,null,null,null,{"$f":"IF(AX281=\"-\",0,ROUNDDOWN((AX281-VLOOKUP(AP281,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP281,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP281,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX281-VLOOKUP(AP281,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP281,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,5,"Server rooms (5-cabinet)",null,null,null,18.399999999999999,null,null,"PLA15",null,{"$f":"VLOOKUP(U282,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PLA10"},18.399999999999999,null,null,"-",null,"-","server room (4 cabinets)",13,"-","AS SOA","-",50,"split into more","specialist space","7","none",null,null,"PLA15","Server room (5-cabinet)","-",0,0,null,null,"-",null,0,null,null,null,{"$f":"IF(AX282=\"-\",0,ROUNDDOWN((AX282-VLOOKUP(AP282,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP282,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP282,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX282-VLOOKUP(AP282,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP282,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Server rooms (ICT hub)",null,null,null,7.5,null,null,"PLA18",null,{"$f":"VLOOKUP(U283,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PLA10"},7.5,null,null,"-",null,"-","too small",1,"-",2,"-",10,"server room","specialist space","7","none",null,null,"PLA18","Server room (ICT hub)","-",0,0,null,null,"-",null,0,null,null,null,{"$f":"IF(AX283=\"-\",0,ROUNDDOWN((AX283-VLOOKUP(AP283,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP283,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP283,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX283-VLOOKUP(AP283,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP283,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-","-",0,0,null,null,"-",null,null,null,null,null,{"$f":"IF(AX284=\"-\",0,ROUNDDOWN((AX284-VLOOKUP(AP284,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP284,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP284,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX284-VLOOKUP(AP284,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP284,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Plant rooms",null,null,null,null,null,null,"PLA20",null,{"$f":"VLOOKUP(U285,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PLA20"},null,null,null,"-",null,"-","too small",1,"-",50,"-",150,"split into more","boiler room or similar","7","none",null,null,"PLA20","Plant room","-",0,0,null,null,"-",null,2,0,0,null,{"$f":"IF(AX285=\"-\",0,ROUNDDOWN((AX285-VLOOKUP(AP285,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP285,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP285,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX285-VLOOKUP(AP285,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP285,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Plant rooms (heat source)",null,null,null,null,null,null,"PLA21",null,{"$f":"VLOOKUP(U286,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PLA20"},null,null,null,"-",null,"-","too small",1,"-",50,"-",150,"split into more","boiler room or similar","7","none",null,null,"PLA21","Plant room (heat source)","-",0,0,null,null,"-",null,2,null,null,null,{"$f":"IF(AX286=\"-\",0,ROUNDDOWN((AX286-VLOOKUP(AP286,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP286,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP286,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX286-VLOOKUP(AP286,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP286,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Plant rooms (ventilation)",null,null,null,null,null,null,"PLA22",null,{"$f":"VLOOKUP(U287,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PLA20"},null,null,null,"-",null,"-","too small",1,"-",50,"-",150,"split into more","boiler room or similar","7","none",null,null,"PLA22","Plant room (ventilation)","-",0,0,null,null,"-",null,2,null,null,null,{"$f":"IF(AX287=\"-\",0,ROUNDDOWN((AX287-VLOOKUP(AP287,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP287,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP287,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX287-VLOOKUP(AP287,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP287,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Plant rooms (cold water tanks)",null,null,null,null,null,null,"PLA23",null,{"$f":"VLOOKUP(U288,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PLA20"},null,null,null,"-",null,"-","too small",1,"-",50,"-",150,"split into more","boiler room or similar","7","none",null,null,"PLA23","Plant room (cold water tanks)","-",0,0,null,null,"-",null,2,null,null,null,{"$f":"IF(AX288=\"-\",0,ROUNDDOWN((AX288-VLOOKUP(AP288,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP288,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP288,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX288-VLOOKUP(AP288,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP288,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Plant rooms (sprinkler pumps)","CTS",null,null,null,null,null,"PLA24",null,{"$f":"VLOOKUP(U289,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PLA20"},null,null,null,"-",null,"-","too small",1,"-",50,"-",150,"split into more","boiler room or similar","7","none",null,null,"PLA24","Plant room (sprinkler pumps)","-",0,0,null,null,"-",null,2,null,null,null,{"$f":"IF(AX289=\"-\",0,ROUNDDOWN((AX289-VLOOKUP(AP289,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP289,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP289,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX289-VLOOKUP(AP289,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP289,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Plant rooms (electrical intake)","-",null,null,null,null,null,"PLA25",null,{"$f":"VLOOKUP(U290,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PLA20"},null,null,null,"-",null,"-","too small",1,"-",50,"-",150,"split into more","boiler room or similar","7","none",null,null,"PLA25","Plant room (electrical intake)","-",0,0,null,null,"-",null,2,null,null,null,{"$f":"IF(AX290=\"-\",0,ROUNDDOWN((AX290-VLOOKUP(AP290,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP290,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP290,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX290-VLOOKUP(AP290,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP290,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Services shafts (enclosed ventilation)","CTS",null,null,null,null,null,"PLA41",null,{"$f":"VLOOKUP(U291,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PLA40"},null,null,null,"-",null,"-","too small",1,"-",2,"-",10,"plant area",null,"7","none",null,null,"PLA41","Services shaft (enclosed ventilation)","-",0,0,null,null,"-",null,0,4,4,null,{"$f":"IF(AX291=\"-\",0,ROUNDDOWN((AX291-VLOOKUP(AP291,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP291,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP291,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX291-VLOOKUP(AP291,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP291,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Services shafts (enclosed daylit ventilation)","CTS",null,null,null,null,null,"PLA42",null,{"$f":"VLOOKUP(U292,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PLA40"},null,null,null,"-",null,"-","too small",1,"-",2,"-",10,"plant area","specialist space","7","none",null,null,"PLA42","Services shaft (enclosed daylit ventilation)","-",0,0,null,null,"-",null,0,null,null,null,{"$f":"IF(AX292=\"-\",0,ROUNDDOWN((AX292-VLOOKUP(AP292,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP292,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP292,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX292-VLOOKUP(AP292,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP292,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Services shafts (enclosed electrical)","-",null,null,null,null,null,"PLA43",null,{"$f":"VLOOKUP(U293,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PLA40"},null,null,null,"-",null,"-","too small",1,"-",2,"-",10,"plant area","specialist space","7","none",null,null,"PLA43","Services shaft (enclosed electrical)","-",0,0,null,null,"-",null,0,null,null,null,{"$f":"IF(AX293=\"-\",0,ROUNDDOWN((AX293-VLOOKUP(AP293,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP293,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP293,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX293-VLOOKUP(AP293,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP293,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Services shafts (enclosed other)","CTS",null,null,null,null,null,"PLA44",null,{"$f":"VLOOKUP(U294,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PLA40"},null,null,null,"-",null,"-","too small",1,"-",2,"-",10,"plant area","specialist space","7","none",null,null,"PLA44","Services shaft (enclosed other)","-",0,0,null,null,"-",null,0,null,null,null,{"$f":"IF(AX294=\"-\",0,ROUNDDOWN((AX294-VLOOKUP(AP294,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP294,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP294,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX294-VLOOKUP(AP294,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP294,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Light wells (open ventilation)","CTS",null,null,null,null,null,"PLA31",null,{"$f":"VLOOKUP(U295,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PLA30"},null,null,null,"-",null,"-","too small",1,"-",2,"-",10,"plant area","specialist space","7","none",null,null,"PLA31","Light well (open ventilation)","-",0,0,null,null,"-",null,0,null,null,null,{"$f":"IF(AX295=\"-\",0,ROUNDDOWN((AX295-VLOOKUP(AP295,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP295,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP295,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX295-VLOOKUP(AP295,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP295,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Light wells (open daylit ventilation)","CTS",null,null,null,null,null,"PLA32",null,{"$f":"VLOOKUP(U296,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PLA30"},null,null,null,"-",null,"-","too small",1,"-",2,"-",10,"plant area","specialist space","7","none",null,null,"PLA32","Light well (open daylit ventilation)","-",0,0,null,null,"-",null,0,null,null,null,{"$f":"IF(AX296=\"-\",0,ROUNDDOWN((AX296-VLOOKUP(AP296,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP296,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP296,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX296-VLOOKUP(AP296,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP296,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"-","-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-","-",0,0,null,null,"-",null,null,null,null,null,{"$f":"IF(AX297=\"-\",0,ROUNDDOWN((AX297-VLOOKUP(AP297,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP297,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#N/A"}},{"$f":"IF(VLOOKUP(AP297,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX297-VLOOKUP(AP297,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP297,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Stairways, plant","CTS",null,null,null,null,null,"PLA07",null,{"$f":"VLOOKUP(U298,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PLA20"},3,null,null,"-",null,"-","too small",1,"-",20,"-",150,"split into more","specialist space","7","none",null,null,"PLA07","Stairway, plant","-",0,0,null,null,"-",null,0,null,null,null,{"$f":"IF(AX298=\"-\",0,ROUNDDOWN((AX298-VLOOKUP(AP298,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP298,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP298,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX298-VLOOKUP(AP298,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP298,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Stairways, plant (to roof)","CTS",null,null,null,null,null,"PLA08",null,{"$f":"VLOOKUP(U299,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PLA20"},3,null,null,"-",null,"-","too small",1,"-",20,"-",150,"split into more","specialist space","7","none",null,null,"PLA08","Stairway, plant (to roof)","-",0,0,null,null,"-",null,0,null,null,null,{"$f":"IF(AX299=\"-\",0,ROUNDDOWN((AX299-VLOOKUP(AP299,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP299,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP299,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX299-VLOOKUP(AP299,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP299,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Stairways, plant (escape)","CTS",null,null,null,null,null,"PLA09",null,{"$f":"VLOOKUP(U300,'Data Library'!$A$4:$E$466,5,FALSE)","v":"PLA20"},3,null,null,"-",null,"-","too small",1,"-",20,"-",150,"split into more","specialist space","7","none",null,null,"PLA09","Stairway, plant (escape)","-",0,0,null,null,"-",null,0,null,null,null,{"$f":"IF(AX300=\"-\",0,ROUNDDOWN((AX300-VLOOKUP(AP300,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP300,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP300,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX300-VLOOKUP(AP300,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP300,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Circulation spaces (horizontal)",null,null,null,null,null,null,"CIR00",null,{"$f":"VLOOKUP(U301,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CIR00"},null,null,null,"-",null,"-","too small",1,"-",50,"-",500,"split into more","circulation to other spaces","3","none",null,null,"CIR00","Circulation space (horizontal)","-",0,0,null,null,"-",null,4,4,2,null,{"$f":"IF(AX301=\"-\",0,ROUNDDOWN((AX301-VLOOKUP(AP301,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP301,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP301,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX301-VLOOKUP(AP301,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP301,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Corridors",null,null,null,null,null,null,"CIR01",null,{"$f":"VLOOKUP(U302,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CIR00"},null,null,null,"-",null,"-","circulation area",5,"-",50,"-",500,"split into more","circulation to other spaces","3","none",null,null,"CIR01","Corridor","-",0,0,null,null,"-",null,1,4,6,null,{"$f":"IF(AX302=\"-\",0,ROUNDDOWN((AX302-VLOOKUP(AP302,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP302,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP302,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX302-VLOOKUP(AP302,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP302,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Stairways   (area per floor)",null,null,null,null,null,null,"CIR12",null,{"$f":"VLOOKUP(U303,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CIR12"},null,null,null,"-",null,"-","circulation area",5,"-",25,"-",50,"main circulation","circulation to other spaces","3","none",null,null,"CIR12","Stairway","-",0,0,null,null,"-",null,0,2,0,null,{"$f":"IF(AX303=\"-\",0,ROUNDDOWN((AX303-VLOOKUP(AP303,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP303,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP303,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX303-VLOOKUP(AP303,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP303,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Lifts           (area per floor, incl space to wait)",null,null,null,null,null,null,"CIR13",null,{"$f":"VLOOKUP(U304,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CIR13"},null,null,null,"-",null,"-","too small",2,"-",4,"-",10,"main circulation","lift","3","none",null,null,"CIR13","Lift","-",0,0,null,null,"-",null,0,null,null,null,{"$f":"IF(AX304=\"-\",0,ROUNDDOWN((AX304-VLOOKUP(AP304,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP304,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP304,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX304-VLOOKUP(AP304,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP304,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Lobbies",null,null,null,null,null,null,"CIR03",null,{"$f":"VLOOKUP(U305,'Data Library'!$A$4:$E$466,5,FALSE)","v":"CIR03"},null,null,null,"-",null,"-","circulation area",3,"-",6,"-",25,"main circulation","lobby","3","none",null,null,"CIR03","Lobby","-",0,0,null,null,"-",null,1,2,0,null,{"$f":"IF(AX305=\"-\",0,ROUNDDOWN((AX305-VLOOKUP(AP305,'Prog Assums'!$AP$7:$AV$305,4,FALSE))/VLOOKUP(AP305,'Prog Assums'!$AP$7:$AV$305,5,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$f":"IF(VLOOKUP(AP305,'Prog Assums'!$AP$7:$AX$305,7,FALSE)=1,1,ROUND((AX305-VLOOKUP(AP305,'Prog Assums'!$AP$7:$AX$305,6,FALSE))/VLOOKUP(AP305,'Prog Assums'!$AP$7:$AX$305,7,FALSE),0))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]

{"sheet":"Data Library","index":11,"n_rows":498,"n_cols":83,"rows_kept":498,"cut":false,"hidden":false,"merged":[]}
["Macro code","space types",null,null,null,"$H$10","$J$10","$J$8","$H$12","$H$14","$H$16","$J$16","  2023 NCA",null,"$H$18","$J$18","group size",null,"staff workstations",null,"$H$20","$H$22",null,"$H$24","$H$26","$J$26","$H$28","$H$33","$H$35","$H$37","$H$39","$J$39","$H$41","$H$45","$H$48","$H$50","$H$54","$H$56","$H$58","$H$60",null,"$H$62","$H$64","$H$66","$H$68","$H$70","$H$72","$H$74","$H$76","$H$80","$H$82","$H$83","$H$84","$H$85","$H$87","$H$91","$G$93","$H$95","$H$97","$H$106","$H$107","$H$109","$J$109","$H$111","$H$113","$H$115","$H$117","$H$127","$H$126","$H$120","$H$134"]
["Final ADS code","NEW name of individual space","previous name of individual space ","Previous Final ADS Code","parent ADS code","New build or existing","Uniclass code","Uniclass title","summary description","Activities to be accommodated","Area Guidelines Category/ Cobie Zone names","net capacity category","net cap","net cap","Area Guidelines (BB103/4) zone","restrictive/ standard/ extensive/ SEN","base area","area/ person","base area","area/ person","Required area (m2)","Max group size in SoA","Max group size from BB103/4 zone","no. of staff work-stations","Maximum occupancy","Age range","community use","access","Enclosure requirements","Adjacency requirements","minimum \nopen height / clear height \nif new","min open ht / clear ht \nif refurb","standard / minimum space depth","external doorset","min window sill ht (mm AFFL)","Specific external door or window requirements","Doorset from circulation","description","Doorset to adjacent space of similar type","description",null,"Specific doorset requirements","floor finish","description","ceiling finish","description","wall finish","description","Specific finishes requirements","Daylight and lighting requirements (code if new build)","Daylight Autonomy (sDA)","Useful Daylight Illuminance (UDI)","Daylight access","Visual connection to adjoining daylit spaces","Minimum horizontal/ task illuminance (lux)","Lighting controls","emergency lighting","Specific lighting requirements","Thermal comfort requirements","acoustics: Activity noise level","acoustics: Noise tolerance","reverberation time for new build","reverberation time for remodel or refurbishment","Specific environmental requirements","Gas services","Specific electrical services requirements","Specific wet services requirements","Total data points indicative","WiFi","Power sockets","Specific safety and security requirements"]
[]
["ACT01","Dance studios","Dance studios","ACT01","ACT01","New Build","SL_25_10_21","Dance studios","Secondary or tertiary space for movement, dance, gymnastics, exams and optional community use, but not dining","Dance. Gymnastics. Occasional use for exams and exhibitions. Table tennis.","Halls and dining","Large",12.5,-20,"H","-",16,3.3,null,0,120,30,32,0,36,"CTS","Yes","Disabled access into the space required","Enclosed",null,"4500 / 4500","3500 / 3500",10000,"Not required","CTS","","DD1.1kv","general double ","N/A","no internal doorset required",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards in Primary","F6.1","multi-purpose sport","C1.1","general","W1.1h","general","Floor to match limits of impact and fatigue on human body in DIN 18032: Part 2, and must be easy to clean","L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","if community use",null,"T2/T5","High","Medium","<=1.2","<=1.5",null,"None","Where required","None",11,2,10,"No projections, including opening doors, to avoid injury during activity."]
["ACT05","Activity studios","Activity studios","ACT05","ACT05","New Build","SL_25_10_01","Activity studios","Space for movement, dance, gymnastics and other PE activities, exams and optional community use, but not dining","Dance. Gymnastics. Occasional use for exams and exhibitions. Table tennis.","Halls and dining","Large",12.5,-20,"G","-",10,2.9,null,0,"As SoA",30,"As SoA",0,"As SoA","CTS","Yes","Disabled access into the space required","Enclosed",null,"5000 / 5000 (6900 of >180m2)","4500 / 4500","10650 / 7500","Optional","CTS","Contractor to Specify for approval if provided","DD1.1kv","general double ","N/A","no internal doorset required",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards in Primary","F6.1","multi-purpose sport","C1.1","general","W6.1h","general"," ","L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","if community use","Default illuminance 300 lux, but option to switch to 500 lux for some sports useful, see LG5","T2/T5","High","Medium","<=1.5","<=2.0",null,"None","Where required","None",12,2,10,"No projections, including opening doors, to avoid injury during activity."]
["ACT06","Activity studios (10 x 12)","Activity studios (10 x 12)","ACT06","ACT05","New Build","SL_25_10_01","Activity studios","12m x 10m space for movement, dance, gymnastics and other PE activities, exams and optional community use, but not dining","Dance. Gymnastics. Occasional use for exams and exhibitions. Table tennis.","Halls and dining","Large",12.5,-20,"G","-",10,2.9,null,0,120,30,38,0,42,"CTS","Yes","Disabled access into the space required","Enclosed",null,"5000 / 5000","4500 / 4500","10000 / 10000","Optional","CTS","Contractor to Specify for approval if provided","DD1.1kv","general double ","N/A","no internal doorset required",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards in Primary","F6.1","multi-purpose sport","C1.1","general","W6.1h","general",null,"L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","if community use","Default illuminance 300 lux, but option to switch to 500 lux for some sports useful, see LG5","T2/T5","High","Medium","<=1.5","<=2.0",null,"None","Where required","None",12,2,10,"No projections, including opening doors, to avoid injury during activity."]
["ACT07","Activity studios (10 x 15)","Activity studios (10 x 15)","ACT07","ACT05","New Build","SL_25_10_01","Activity studios","15m x 10m space for movement, dance, gymnastics and other PE activities, exams and optional community use, but not dining","Dance. Gymnastics. Occasional use for exams and exhibitions. Table tennis.","Halls and dining","Large",12.5,-20,"G","-",10,2.9,null,0,150,30,48,0,53,"CTS","Yes","Disabled access into the space required","Enclosed",null,"5000 / 5000","4500 / 4500","10000 / 10000","Optional","CTS","Contractor to Specify for approval if provided","DD1.1kv","general double ","N/A","no internal doorset required",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards in Primary","F6.1","multi-purpose sport","C1.1","general","W6.1h","general",null,"L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","if community use","Default illuminance 300 lux, but option to switch to 500 lux for some sports useful, see LG5","T2/T5","High","Medium","<=1.5","<=2.0",null,"None","Where required","None",12,2,10,"No projections, including opening doors, to avoid injury during activity."]
["ACT10","Activity studios, 1-court","Activity studios, 1-court","ACT10","ACT05","New Build","SL_25_10_01","Activity studios","18m x 10m space for badminton, movement, dance, gymnastics and other PE activities, exams and optional community use, but not dining","Individual activities including Athletics (practice only) and gymnastics. Recreational trampolining. Team games including badminton; judo; karate; indoor volleyball; table tennis.","Halls and dining","Large",12.5,-20,"S","standard",15,1.75,null,0,180,94,94,0,104,"N/A","Yes","Disabled access into the space required","Enclosed",null,"6900 / 6900","6900 / 6900","10000 / 10000","For fire only","CTS","Contractor to Specify for approval","DD1.1kv","general double ","N/A","no internal doorset required",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards in Primary","F6.1","multi-purpose sport","C1.1","general","W6.1h","sports","Floor markings to be suitable for sports to be accommodated. Floor sockets to suit the sports hall floor and FF&E provided. ","L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","if community use",null,"T2/T5","High","Medium","<=1.5","<=2.0","Ventilation as Tech Annex 2F 6.4.2","None","Where required","None",3,4,4,"No projections, including opening doors, to avoid injury during activity."]
["ACT11","Activity studios, 1-court (restrictive, extg)","Activity studios, 1-court (restrictive, extg)","ACT11","ACT11","Existing","SL_25_10_01","Activity studios","Existing space for badminton, movement, dance, gymnastics and other PE activities, exams and optional community use, but not dining","Individual activities including Athletics (practice only) and gymnastics. Recreational trampolining. Team games including badminton; judo; karate; indoor volleyball; table tennis.","Halls and dining","Large",12.5,-20,"S","restrictive",15,1.75,null,0,159,82,82,0,91,"N/A","Yes","Disabled access into the space required","Enclosed",null,"6700 / 6700","as existing","as existing","For fire only","CTS","Contractor to Specify for approval","DD1.1kv","general double ","N/A","no internal doorset required",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards in Primary","F6.1","multi-purpose sport","C1.1","general","W6.1h","sports","Floor markings to be suitable for sports to be accommodated. Floor sockets to suit the sports hall floor and FF&E provided. ","L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","if community use",null,"T2/T5","High","Medium","<=1.5","<=2.0","Ventilation as Tech Annex 2F 6.4.2","None","Where required","None",3,4,4,"No projections, including opening doors, to avoid injury during activity."]
["ACT13","Gymnasiums (existing)","Gymnasiums (existing)","ACT13","ACT11","Existing","SL_42_40_35","Gymnasiums","Existing gymnasium for movement, dance, gymnastics and other PE activities, exams and optional community use, but not dining","Dance. Gymnastics. Occasional use for exams and exhibitions. Table tennis. Recreational trampolining if over 6.7m high.","Halls and dining","Large",12.5,-20,"G","-",10,2.9,null,0,260,30,86,0,95,"CTS","Yes","Disabled access into the space required","Enclosed",null,"as existing","as existing","as existing","For fire only","CTS","Contractor to Specify for approval","DD1.1kv","general double ","N/A","no internal doorset required",null,"As existing","F6.1","multi-purpose sport","C1.1","general","W6.1h","sports","Floor markings to be suitable for sports to be accommodated. Floor sockets to suit the sports hall floor and FF&E provided. ","L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","if community use","Default illuminance 300 lux, but option to switch to 500 lux for some sports useful, see LG5","T2/T5","High","Medium","<=1.5","<=2.0",null,"None","Where required","None",12,2,10,"No projections, including opening doors, to avoid injury during activity."]
["ACT15","Squash courts (existing)","Squash courts (existing)","ACT15","ACT11","Existing","SL_42_40_83","Squash courts","Existing space designed as a squash court","Squash","Halls and dining","Large",12.5,-20,null,"-",0,30,null,0,58,2,2,0,3,"N/A","Yes","Disabled access into the space required","Enclosed",null,"as existing","as existing","as existing","For fire only","CTS","Contractor to Specify for approval","DD1.1kv","general double ","N/A","no internal doorset required",null,"As existing","F6.1","multi-purpose sport","C1.1","general","CTS","Contractor to specify for approval",null,"L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","if community use",null,"T2/T5","High","Medium","<=1.5","<=2.0",null,"None","Where required","None",12,2,10,"No projections, including opening doors, to avoid injury during activity."]
["ACT17","Indoor activity spaces, other (existing)","Indoor activity spaces, other (existing)","ACT17","ACT11","Existing","SL_42_40","Indoor activity spaces","Existing space designed for specific indoor sport","Indoor sports","Halls and dining","Large",12.5,-20,"G","-",10,2.9,null,0,"As SoA","As SoA","As SoA",0,"As SoA","N/A","Yes","Disabled access into the space required","Enclosed",null,"CTS","CTS","CTS","For fire only","CTS","Contractor to Specify for approval","DD1.1kv","general double ","N/A","no internal doorset required",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards in Primary","F6.1","multi-purpose sport","C1.1","general","W6.1h","sports",null,"L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","if community use",null,"T2/T5","High","Medium","<=1.5","<=2.0",null,"None","Where required","None",12,2,10,"No projections, including opening doors, to avoid injury during activity."]
["ACT21","Climbing wall spaces (indoor)","Climbing wall spaces (indoor)","ACT21","ACT21","New Build","SL_42_40_14","Climbing wall spaces","Space for specialist climbing wall and associated equipment","Climbing","Halls and dining","Large",12.5,-20,"C","-",4,1.7,null,0,"As SoA","As SoA","As SoA",0,"As SoA","N/A","Yes","Disabled access into the space required","Enclosed or semi-enclosed",null,"7500 / 7500","CTS","CTS","Not required","CTS","","DD1.1kv","general double ","N/A","no internal doorset required",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards in Primary","F6.1","multi-purpose sport","C1.1","general","CTS","Contractor to specify for approval",null,"L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","if community use",null,"T6","High","Medium","<=1.5","<=2.0",null,"None","Where required","None",0,0,0]
["ACT22","Fitness rooms (exercise studio)","Fitness rooms (exercise studio)","ACT22","ACT22","New Build","SL_42_40_30","Fitness rooms","Space for fitness and exercise equipment","Fixed machine cardio vascular exercise. Trampolining. Weights.","Basic teaching","Heavy practical (clean)",3.5,4,"G","-",10,2.9,null,0,69,20,20,0,22,"CTS","Yes","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7000","Not required","CTS","","DD1.1kv","general double ","N/A","no internal doorset required",null,null,"F6.1","multi-purpose sport","C1.1","general","W1.1h","general","Floor surface must be able to withstand live loads from users, accidental point load impact , and dynamic effects. ","L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","if community use",null,"T2","High","Medium","<=1.2","<=1.5",null,"None","To suit equipment","None",22,2,16]
["ACT25","Indoor swimming pools (existing)","Indoor swimming pools (existing)","ACT25","ACT25","Existing","SL_42_85_41","Indoor swimming pools","Internal space containing internal heated swimming pool and surrounding area","Swimming","Halls and dining","Large",12.5,-20,"G",null,10,2.9,null,0,"As SoA",30,"As SoA",0,"As SoA","N/A","Yes","Disabled access into the space required","Enclosed",null,"CTS","CTS","CTS","CTS","CTS","Contractor to Specify for approval","DD1.1kv","general double ","N/A","no internal doorset required",null,null,"F7.3h","wet area","C2.3","wet areas","W3.3","wet areas","Flooring in barefoot areas shall be 'barefoot slip resistance category B'. Walls to suit specialist requirements of pools. Ceiling to include hoist and track if SEN.","L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","if community use","IP rating for wet areas. Refer to SSB for any specialist lighting requirements","T9","High","High","<=1.5","<=2.0",null,"None","None","Heated and treated water"]
["ACT50","Activity studios (ambulant)","Activity studios (ambulant)","ACT50","ACT05","New Build","SL_25_10_01","Activity studios","Space for PE activities and exams, but not dining, for ambulant pupils needing additional support ","Gymnastics. Team games including basketball. Movement. Recreational trampolining if 6.9m high. Table tennis.","Halls and dining","Large",12.5,-20,"G","SEN",10,2.9,null,0,"As SoA",12,"As SoA",0,"As SoA","CTS","Yes","Disabled access into the space required","Enclosed",null,"5000 / 5000 (6900 if >180m2)","4500 / 4500","10200 / 7500","Optional","CTS","Contractor to Specify for approval if provided","DD1.1kv","general double ","N/A","no internal doorset required",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards","F6.1","multi-purpose sport","C1.1","general","W6.1h","general",null,"L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","if community use","Default illuminance 300 lux, but option to switch to 500 lux for some sports useful, see LG5","T2/T5","High","Medium","<=1.5","<=2.0",null,"None","Where required","None",6,2,10]
["ACT55","Activity studios, non-ambulant","Activity studios, non-ambulant","ACT55","ACT55","New Build","SL_25_10_01","Activity studios","Space for movement, dance, and other PE activities and exams, but not dining, for ambulant and non-ambulant pupils ","Gymnastics. Team games including basketball. Movement. Rebound therapy. Table tennis.","Halls and dining","Large",12.5,-20,"J","SEN",28,4.2,null,0,"As SoA",8,"As SoA",0,"As SoA","CTS","Yes","Disabled access into the space required","Enclosed",null,"5000 / 5000 (6900 if >180m2)","4500 / 4500","10200 / 7500","Optional","CTS","Contractor to Specify for approval if provided","DD1.1kv","general double ","N/A","no internal doorset required",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards","F6.1","multi-purpose sport","C1.1","general","W6.1h","general",null,"L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","if community use","Default illuminance 300 lux, but option to switch to 500 lux for some sports useful, see LG5","T2/T5","High","Medium","<=1.5","<=2.0",null,"None","Where required","None",6,2,10]
["ACT60","Fitness rooms (ambulant)","secondary fitness (ambulant)","ACT60","ACT22","New Build","SL_42_40_30","Fitness rooms","Space for fitness and exercise equipment for ambulant pupils needing additional support ","Fixed machine cardio vascular exercise. Weights.","Basic teaching","Heavy practical (clean)",3.5,4,"G","SEN",10,2.9,null,1,"As SoA",12,"As SoA",1,"As SoA","CTS","Yes","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7000","Not required","CTS","","DD1.1kv","general double ","N/A","no internal doorset required",null,"Finger guards","F6.1","multi-purpose sport","C1.1","general","W1.1h","general","Floor surface must be able to withstand live loads from users, accidental point load impact, and dynamic effects. ","L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","if community use",null,"T2","High","Medium","<=1.2","<=1.5",null,"None","To suit equipment","None",12,2,16]
["ACT65","Fitness rooms, non-ambulant","secondary fitness (non-ambulant)","ACT65","ACT65","New Build","SL_42_40_30","Fitness rooms","Space for fitness and exercise equipment including specialist equipment for non-ambulant pupils needing significant additional support ","Fixed machine cardio vascular exercise. Weights.","Basic teaching","Heavy practical (clean)",3.5,4,"J","SEN",28,4.2,null,1,"As SoA",8,"As SoA",1,"As SoA","CTS","Yes","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7000","Not required","CTS","","DD1.1kv","general double ","N/A","no internal doorset required",null,"Ergonomic handle. Finger guards","F6.1","multi-purpose sport","C1.1","general","W1.1h","general","Floor surface must be able to withstand live loads from users, accidental point load impact, and dynamic effects. Ceiling to include hoist tracking in both directions, avoiding light fittings","L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","if community use",null,"T5/T7","High","Medium","<=1.2","<=1.5",null,"None","To suit equipment","None",12,2,16]
["ADM02","Confidential meetings rooms (interview)","Confidential meetings rooms (interview)","ADM02","ADM02","New Build","SL_20_15_15","Confidential meetings rooms","Room off reception area for meetings with visitors without the need to access the main school","Interviews, some of which will be in private, with parents and visitors. Small group meetings for both staff and parents.","Staff and admin","General",1.5,4,"A","-",2,1.1000000000000001,null,0,6,4,4,0,5,"N/A","Optional ","Disabled access into the space required","Enclosed or semi-enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","D1.1av","general",null,"2 doors required, to allow second exit for staff, unless agreed otherwise","F1.1","general","C1.1","general","W1.1","general"," ","L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=0.8","<=0.8","Ventilation as Tech Annex 2F 6.2","None","Minimal","None",3,2,8]
["ADM03","First aid posts (sick bay)","First aid posts (sick bay)","ADM03","ADM03","New Build","SL_35_10_30","First aid posts","Semi-open bay for pupils who are feeling unwell","Passively supervised area for pupils who are ill, may need initial treatment and/or are waiting for parents/carers to pick them up.","Staff and admin","General",1.5,4,"B","-",2,1.6,null,0,4,1,1,0,2,"N/A","None","Disabled access into the area preferred","Semi-enclosed",null,"2700 / 2400","2400 / N/A","N/A / 750","Not required","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F3.4h","hygienic non-slip","C1.1","general","W3.2","humid","Flooring to be cleanable and not hold smells","L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T6","Low","Medium","<=0.8","<=1.0",null,"None","Minimal","None if toilet nearby",0,0,8,"Ability to supervise essential"]
["ADM04","First aid rooms (sick room)","First aid rooms (sick room)","ADM04","ADM04","New Build","SL_35_10_31","First aid rooms","Room for pupils who are feeling unwell","Supervised area for pupils who are ill, may need initial treatment and/or are waiting for parents/carers to pick them up.","Staff and admin","General",1.5,4,"B","-",2,1.6,null,0,6,3,3,0,4,"N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A",1700,"Not required","N/A","","D1.1av","general","N/A","no internal doorset required",null,"Finger guards if used by SEN, early years or KS1 pupils","F3.4h","hygienic non-slip","C1.1","general","W3.2","humid","Flooring to be cleanable and not hold smells","L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T6","Low","Medium","<=1.0","<=1.0",null,"None","Minimal","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",4,null,8,"Ability to supervise essential"]
["ADM05","Enclosed offices, with recep desk (only)","Enclosed offices, with recep desk (only)","ADM05","ADM05","New Build","SL_20_15_27","Enclosed offices","Main office for administrative staff, with reception desk for visitors opening onto entrance/ reception area","Administrative support to staff and welfare support to pupils. Managing and controlling access to and from the school. Welcoming visitors and pupils at reception desk.","Staff and admin","General",1.5,4,"K","-",4,3.7,4,3.7,"As SoA","As SoA","As SoA","As SoA","As SoA","N/A","None","Disabled access into the space required","Enclosed except reception desk","adjacent to Reception area, entrance","2700 / 2400 (3300 / 2700 if >27m2)","2400 / N/A","N/A / 3400","Not required","CTS","","D1.1a","private","N/A","no internal doorset required",null,"Accessible reception desk on one wall. See Annex 2D 4.2.1","F1.1","general","C1.1","general","W1.1","general"," ","L1.1k","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.0","Ventilation as Tech Annex 2F 6.2","None","Dado on 2 walls","None",12,2,16,"Means to keep sensitive documents securely"]
["ADM06","Enclosed offices, with recep window","Enclosed offices, with recep window","ADM06","ADM06","New Build","SL_20_15_27","Enclosed offices","Main office for finance staff, with reception window for pupils or students opening onto secure area","Administrative support to staff and welfare support to pupils. ","Staff and admin","General",1.5,4,"K","-",4,3.7,4,3.7,"As SoA","As SoA","As SoA","As SoA","As SoA","N/A","None","Disabled access into the space required","Enclosed except reception desk","adjacent to pupil circulation","2700 / 2400 (3300 / 2700 if >27m2)","2400 / N/A","N/A / 3400","Not required","CTS","","D1.1a","private","N/A","no internal doorset required",null,"Accessible reception window on one wall. See Annex 2D 4.2.2","F1.1","general","C1.1","general","W1.1","general"," ","L1.1k","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.0","Ventilation as Tech Annex 2F 6.2","None","Dado on 2 walls","None",12,2,16,"Means to keep sensitive documents securely"]
["ADM07","Enclosed offices, with recep desk (and window)","Enclosed offices, with recep desk (and window)","ADM07","ADM05","New Build","SL_20_15_27","Enclosed offices","Main office for administrative staff, with reception desk for visitors opening onto entrance/ reception area and reception window for pupils or students opening onto secure area","Managing and controlling access to and from the school. Welcoming visitors and pupils at reception desk.","Staff and admin","General",1.5,4,"K","-",4,3.7,4,3.7,"As SoA","As SoA","As SoA","As SoA","As SoA","N/A","None","Disabled access into the space required","Enclosed except reception desk","adjacent to Reception area, entrance","2700 / 2400 (3300 / 2700 if >27m2)","2400 / N/A","N/A / 3400","Not required","CTS","","D1.1a","private","N/A","no internal doorset required",null,"Accessible reception desk on one wall, and reception window. See Annex 2D 4.2.1","F1.1","general","C1.1","general","W1.1","general"," ","L1.1k","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.0","Ventilation as Tech Annex 2F 6.2","None","Dado on 2 walls","None",12,2,16,"Means to keep sensitive documents securely"]
["ADM08","Reprographics rooms","Reprographics rooms","ADM08","ADM08","New Build","SL_20_15_73","Reprographics rooms","Room for reprographics and photocopying machines","Administrative work. Collating, finishing, photocopying, printing, scanning. Storage of paper and printing resources.","Staff and admin","General",1.5,4,"K","-",4,3.7,4,6.8,"As SoA","As SoA","As SoA","As SoA","As SoA","N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400 (3300 / 2700 if >27m2)","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W1.1","general","Flooring suitable for heavy movable FF&E on castors ","L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.0","Ventilation to photocopiers and printers as Tech Annex 2F 6.3","None","To suit equipment","None",15,2,24]
["ADM11","Enclosed offices, admin (head/ principal)","Enclosed offices, admin (head/ principal)","ADM11","ADM10","New Build","SL_20_15_27","Enclosed offices","Office for head or principal and meetings of staff, governors or other adults","Administrative tasks (including use of ICT) small group meetings and interviews. Privacy important.","Staff and admin","General",1.5,4,"D","-",5,1.9,null,1,16,6,6,1,7,"N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1a","private","D1.1a","private",null,"See Annex 2D 4.2.1","F1.1","general","C1.1","general","W1.1","general"," ","L1.1k","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.0","Ventilation as Tech Annex 2F 6.2","None","Dado on 2 walls","None",10,2,16,"Means to keep sensitive documents securely"]
["ADM13","Enclosed offices, admin (PA)","Enclosed offices, admin (PA)","ADM13","ADM10","New Build","SL_20_15_27","Enclosed offices","Office for personal assistant to head or principal","Administrative tasks (including use of ICT) and filing.","Staff and admin","General",1.5,4,"K","-",4,3.7,null,1,8,1,1,1,2,"N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1a","private","D1.1a","private",null,"See Annex 2D 4.2.1","F1.1","general","C1.1","general","W1.1","general"," ","L1.1k","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.0","Ventilation as Tech Annex 2F 6.2","None","Dado on 2 walls","None",4,0,16,"Means to keep sensitive documents securely"]
["ADM21","Kitchenettes, room","Kitchenettes, room","ADM21","ADM21","New Build","SL_35_60_45","Kitchenettes","Small room for staff to make drinks and snacks","Making drinks and/or snacks for staff, pupils or visitors.","Staff and admin","Light practical",2.5,4,"B","-",2,1.6,null,0,4,1,1,0,2,"N/A","None","Disabled access into the space required","Enclosed ",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","N/A","","D2.2av","strong","N/A","no internal doorset required",null,null,"F3.4h","hygienic non-slip","C1.2","humid areas","W3.2","humid",null,"L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.0","Ventilation as Tech Annex 2F 6.3","None","To suit equipment","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",2,0,16,"Need to be able to clean surfaces thoroughly to maintain hygiene"]
["ADM22","Kitchenettes, bay","Kitchenettes, bay","ADM22","ADM22","New Build","SL_35_60_45","Kitchenettes","Small bay for staff to make drinks and snacks","Making drinks and/or snacks for staff, pupils or visitors.","Staff and admin","Light practical",2.5,4,"B","-",2,1.6,null,0,4,1,1,0,2,"N/A","None","Disabled access into the area preferred","Semi-enclosed","off a staff area","2700 / 2400","2400 / N/A","N/A / 750","Not required","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F3.4h","hygienic non-slip","C1.2","humid areas","W3.2","humid",null,"L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.0","Ventilation as Tech Annex 2F 6.3","None","To suit equipment","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",0,null,8,"Need to be able to clean surfaces thoroughly to maintain hygiene"]
["ADM23","Medical treatment rooms (nurse)","Medical treatment rooms (nurse)","ADM23","ADM23","New Build","SL_35_10_53","Medical treatment rooms","Room for storing and dispensing drugs, preparing feeds etc. ","Administrative tasks (including use of ICT). Preparing gastro tube feed. Possibly storing and dispensing drugs. Privacy and hygiene important.","Staff and admin","General",1.5,4,"K","-",4,3.7,4,6.8,12,2,2,1,3,"N/A","Optional ","Full disabled access required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1a","private","D1.1a","private",null,null,"F3.4h","hygienic non-slip","C1.1","general","W3.2","humid",null,"L3.1d","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, day dim, abs off","No",null,"T6","Low","Medium","<=1.0","<=1.0",null,"None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",8,null,4]
["ADM31","Reception areas, entrance (50% circulation)","Reception areas, entrance (50% circulation)","ADM31","ADM31","New Build","SL_20_15_71","Reception areas","Public side' of reception area, of which 50% is net area for waiting, seating and display, and 50% is circulation through the space","First point of contact for visitors to the school. Welcoming visitors.","Staff and admin","General",1.5,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","Yes ","Full disabled access required","Enclosed or semi-enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Entrance door or via lobby","N/A","Contractor to Specify for approval","DD1.1gv","general double ","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general","Including mat well unless adjacent draught lobby is provided","L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","If fire exit","300 available and limiting glare index of 19 to reception desk","T3","Average","Medium","<=1.5","<=2.0",null,"None","Minimal","None",0,2,2,"Secure supervised entrance; no unauthorised access to rest of school."]
["ADM32","Reception areas, community (50% circulation)","Reception areas, community (50% circulation)","ADM32","ADM32","New Build","SL_20_15_71","Reception areas","Community entrance area, of which 50% is net area for vending and display, and 50% is circulation through the space","Managing and controlling access to and from facilities used by the community such as sports halls.","Staff and admin","General",1.5,4,"-","-",0,0,null,0,4,"-","-",0,{"$error":"#VALUE!"},"N/A","Yes ","Full disabled access required","Enclosed or semi-enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Entrance door or via lobby","N/A","Contractor to Specify for approval","DD1.1gv","general double ","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general","Including mat well unless adjacent draught lobby is provided","L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","If fire exit","300 available and limiting glare index of 19 to reception desk if provided","T3","Average","Medium","<=1.5","<=2.0",null,"None","Minimal","None",0,2,2]
["CIR00","Circulation spaces (horizontal)","Circulation spaces (horizontal)","CIR00","CIR00","New Build","SL_90_10","Circulation spaces","Any circulation area or space off circulation except stairwells and lifts, including corridors, lobbies, balconies, circulation area within spaces and bays off corridors","Circulation of pupils and others between spaces.","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","CTS","Full disabled and trolley access required","Enclosed or semi-enclosed",null,"2400 / N/A","2400 / N/A","As GDB","Varies","N/A","Contractor to Specify for approval","varies","varies","varies","varies",null,"Finger guards if used by SEN, early years or KS1 pupils","F1.1","general","C1.1","general","W5.1h","circulation"," ","L4.3n","No requirement","No requirement","Required in upper floors and where possible elsewhere","n/a",100,"pres on, abs off, day off","If fire exit",null,"T3","Average","High","CTS","CTS","Ventilation as Tech Annex 2F 6.4.3 ","None","Minimal","Drinking water on each floor",4,4,2,"CTS if Fire Containment."]
["CIR01","Corridors","Corridors","CIR01","CIR00","New Build","SL_90_10_15","Corridors","Corridor space between rooms providing primary circulation for pupils","Circulation of pupils and others between spaces.","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","CTS","Full disabled and trolley access required","Enclosed",null,"2400 / N/A","2400 / N/A","As GDB","Not required","N/A","","N/A","no internal doorset required","DD1.1fv","general double ",null,"Finger guards if used by SEN, early years or KS1 pupils","F1.1","general","C1.1","general","W5.1h","circulation"," ","L4.3n","No requirement","No requirement","Required in upper floors and where possible elsewhere","n/a",100,"pres on, abs off, day off","If fire exit",null,"T3","Average","High","CTS","CTS","Ventilation as Tech Annex 2F 6.4.3 ","None","Minimal","Drinking water on each floor",1,4,6,"CTS if Fire Containment."]
["CIR03","Lobbies (main entrance)","Lobbies","CIR03","CIR03","New Build","SL_90_10_51","Lobbies","Lobby area between main external doors and internal lobby doors","Circulation of pupils and others between spaces.","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","CTS","Disabled access into the space required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / 2200","Entrance doors","N/A","Contractor to Specify for approval","DD1.1gv","general double ","DD1.1gv","general double ",null,"Finger guards if used by SEN, early years or KS1 pupils","F9.2","entrance","C1.1","general","W5.1h","circulation","including mat well ","L4.3n","No requirement","No requirement","Required in upper floors and where possible elsewhere","n/a",100,"pres on, abs off, day off","If fire exit",null,"T3","Average","Medium","<=1.5","<=2.0",null,"None","Minimal","None",1,2,0,"CTS if Fire Containment."]
["CIR04","Lobbies (alternative entrance)","Lobbies","CIR03","CIR03","New Build","SL_90_10_51","Lobbies","Lobby area between main external doors and internal lobby doors","Circulation of pupils and others between spaces.","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","CTS","Disabled access into the space required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / 2200","Entrance doors","N/A","Contractor to Specify for approval","DD1.1gv","general double ","DD1.1gv","general double ",null,"Finger guards if used by SEN, early years or KS1 pupils","F9.2","entrance","C1.1","general","W5.1h","circulation","including mat well ","L4.3n","No requirement","No requirement","Required in upper floors and where possible elsewhere","n/a",100,"pres on, abs off, day off","If fire exit",null,"T3","Average","Medium","<=1.5","<=2.0",null,"None","Minimal","None",1,2,0,"CTS if Fire Containment."]
["CIR05","Corridors (with art display)","Corridors (with art display)","CIR05","CIR00","New Build","SL_90_10_15","Corridors","Art display area off circulation area","Display of 2D and 3D artwork","Learning resources","General",1.5,4,"-","-",0,0,null,0,4,"-","-",0,{"$error":"#VALUE!"},"CTS","CTS","Disabled access into the space required","Enclosed or semi-enclosed",null,"2400 / N/A","2400 / N/A","As GDB","Varies","N/A","Contractor to Specify for approval","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W5.1h","circulation",null,"L4.3n","No requirement","No requirement","Required in upper floors and where possible elsewhere","n/a",100,"pres on, abs off, day off","If fire exit","Specialist lighting for illuminating displayed items","T3","Average","Medium","<=1.5","<=2.0",null,"None","Minimal. To suit display lighting","Drinking water on each floor",0,0,2]
["CIR06","Equipment stores, appliance bay","Equipment stores, appliance bay","CIR06","CIR06","New Build","SL_90_50_27","Equipment stores","Bay off circulation area for parking and charging a wheelchair or other appliances","Space for appliances to be stored and charged where necessary. Space for wheelchairs.","Storage (non-teaching)","General",1.5,4,"-","-",0,0,null,0,1.5,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled and trolley access required","Open-plan or semi-enclosed","off Corridor","2400 / N/A","2400 / N/A","N/A / 750","Not required","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W5.1h","general","A means to protect walls from wheelchair damage to be provided","L4.3n","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off, day off","No",null,"T3","Average","Medium","<=1.5","<=2.0",null,"None","Minimal. To recharge appliances","None",2,0,2,"Allow sufficient space for safe access."]
["CIR07","Work booths, phone","Work booths, phone","CIR07","CIR09","New Build","SL_90_10_15","Corridors","Bay off circulation area for making private phone calls","Space for phone booth to be located and connected to data/ telephony as required","Non-net","General",1.5,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access into the area preferred","Open-plan or semi-enclosed","off Corridor","2400 / N/A","2400 / N/A","N/A / 750","Varies","N/A","Contractor to Specify for approval","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W5.1h","circulation",null,"L4.3n","No requirement","No requirement","Required in upper floors and where possible elsewhere","n/a",100,"pres on, abs off, day off","No",null,"T3","Low","Medium","CTS","CTS","Ventilation as Tech Annex 2F 6.4.3 ","None","Minimal","None",1,null,1]
["CIR09","Work booths, MFD","Work booths, MFD","CIR09","CIR09","New Build","SL_90_20_98","Work booths","Bay for reprographics, photocopying or multi-function devices","Photocopying, printing, scanning. ","Staff and admin","General",1.5,4,"-","-",0,0,null,0,2,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access into the area preferred","Open-plan or semi-enclosed","off circulation or staff area","2700 / 2400","2400 / N/A","N/A / 750","Not required","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W1.1","general",null,"L4.3n","No requirement","No requirement","Required in upper floors and where possible elsewhere","n/a",300,"man on, abs off","No","Additional task lighting if required","T3","Low","Medium","<=1.0","<=1.0","Ventilation to photocopiers and printers as Tech Annex 2F 6.3","None","To suit equipment","None",9,null,4,null,null,null,null,null,null,null,"S",15,1.75,"for exams",null,36]
["CIR11","Stairways, AP","Stairways","CIR12","CIR12","New Build","SL_90_10_87","Stairways","Enclosed stairwell between floors, including stairs, landings and fire escape refuge areas","Circulation of pupils and others between spaces.","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","CTS","Disabled access into the space required","Enclosed",null,"N/A","N/A","7800 / 3400","Fire doors ","N/A","Contractor to Specify for approval","D1.1gv","n/a","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W5.1h","circulation",null,"L4.3n","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off, day off","If fire exit",null,"T3","Average","Medium","<=1.5","<=2.0","Ventilation as Tech Annex 2F 6.4.3 ","None","Minimal","None",0,2,0,"CTS if Fire Containment."]
["CIR12","Stairways","Stairways","CIR12","CIR12","New Build","SL_90_10_87","Stairways","Enclosed stairwell between floors, including stairs, landings and fire escape refuge areas","Circulation of pupils and others between spaces.","Non-net","Non-net",null,null,"-","-",0,0,null,0,27,"-","-",0,{"$error":"#VALUE!"},"N/A","CTS","Disabled access into the space required","Enclosed",null,"N/A","N/A","7800 / 3400","Fire doors ","N/A","Contractor to Specify for approval","DD1.1gv","general double ","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W5.1h","circulation",null,"L4.3n","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off, day off","If fire exit",null,"T3","Average","Medium","<=1.5","<=2.0","Ventilation as Tech Annex 2F 6.4.3 ","None","Minimal","None",0,2,0,"CTS if Fire Containment."]
["CIR13","Lifts","Lifts","CIR13","CIR13","New Build","SL_90_10_47","Lifts","Lift enclosure and space to wait in front of doors","Circulation of pupils and others between spaces.","Non-net","Non-net",null,null,"-","-",0,0,null,0,4,"-","-",0,{"$error":"#VALUE!"},"N/A","CTS","Full disabled and trolley access required","Enclosed",null,"N/A","N/A","N/A / 1400","Not required","N/A","","CTS","Contractor to specify for approval","N/A","no internal doorset required",null,null,"F1.1","general","N/A","not applicable","N/A","not applicable",null,"L4.3n","No requirement","No requirement","No requirement","Not applicable",100,"pres on, abs off, day off","No",null,"T3","Average","Medium","N/A","N/A",null,"None","N/A","None",0]
["CIR50","Circulation spaces (horizontal ambulant)","Circulation spaces (horizontal ambulant)","CIR50","CIR50","New Build","SL_90_10","Circulation spaces","Circulation areas including corridor space between rooms, stairwells and lobbies, some pupils using mobility aids","Horizontal circulation of ambulant pupils and others between spaces.","Non-net","Non-net",null,null,"-","SEN",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","CTS","Full disabled and trolley access required","Enclosed",null,"2400 / N/A","2400 / N/A","As GDB","Varies","N/A","Contractor to Specify for approval","DD1.1gv","general double ","DD1.1gv","general double ",null,"Finger guards.","F1.1","general","C1.1","general","W5.1h","general","A means to protect walls from wheelchair damage to be provided","L4.3n","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",100,"pres on, abs off, day off","If fire exit",null,"T3","Average","High","CTS","CTS","Ventilation as Tech Annex 2F 6.4.3 ","None","Minimal","Drinking water on each floor",2,null,2,"CTS if Fire Containment."]
["CIR51","Corridors (ambulant)",null,null,"CIR50","New Build","SL_90_10","Circulation spaces","Corridor space between rooms providing primary circulation for ambulant pupils needing additional support, some pupils using mobility aids","Horizontal circulation of ambulant pupils and others between spaces.","Non-net","Non-net",null,null,"-","SEN",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","CTS","Full disabled and trolley access required","Enclosed or semi-enclosed",null,"2400 / N/A","2400 / N/A","As GDB","Varies","N/A","Contractor to Specify for approval","DD1.1gv","general double ","DD1.1gv","general double ",null,"Finger guards.","F1.1","general","C1.1","general","W5.1h","general","A means to protect walls from wheelchair damage to be provided","L4.3n","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",100,"pres on, abs off, day off","If fire exit",null,"T3","Average","High","CTS","CTS","Ventilation as Tech Annex 2F 6.4.3 ","None","Minimal","Drinking water on each floor",2,null,2,"CTS if Fire Containment."]
["CIR53","Lifts (special)","Lifts (special)","CIR53","CIR53","New Build","SL_90_10_47","Lifts","Lift enclosure able to accommodate a side-lying frame as well as wheelchairs, and space to wait in front of doors","Vertical circulation of non-ambulant pupils and others between spaces.","Non-net","Non-net",null,null,"-","SEN",0,0,null,0,8,"-","-",0,{"$error":"#VALUE!"},"N/A","CTS","Full disabled and trolley access required","Enclosed",null,"N/A","N/A","N/A / 2000","Not required","N/A","","CTS","Contractor to specify for approval","N/A","no internal doorset required",null,"Lift doors colour contrast to surround","F1.1","general","N/A","not applicable","N/A","not applicable","A means to protect walls from wheelchair damage to be provided","L4.3n","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",100,"pres on, abs off, day off","No",null,"T3","Average","Medium","N/A","N/A",null,"None","N/A","None",0]
["CIR55","Corridors, non-ambulant","Corridors, non-ambulant","CIR55","CIR55","New Build","SL_90_10_15","Corridors","Corridor space between rooms providing primary circulation for ambulant pupils needing additional support, some pupils using mobility aids","Horizontal circulation of non-ambulant pupils and others between spaces.","Non-net","Non-net",null,null,"-","SEN",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","CTS","Full disabled and trolley access required","Enclosed or semi-enclosed",null,"2400 / N/A","2400 / N/A","As GDB","Not required","N/A","","N/A","no internal doorset required","DD6.1fv","special double",null,"Finger guards.","F1.1h","special general","C1.1","general","W5.1h","general","A means to protect walls from wheelchair damage to be provided","L4.3n","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",100,"pres on, abs off, day off","If fire exit",null,"T5/T7","Average","High","CTS","CTS","Ventilation as Tech Annex 2F 6.4.3 ","None","Minimal","Drinking water on each floor",2,null,2,"CTS if Fire Containment."]
["CIR56","Equipment stores, appliance bay (special)","Equipment stores, appliance bay (special)","CIR56","CIR06","New Build","SL_90_50_27","Equipment stores","Bay off circulation area for parking and charging several wheelchairs or other appliances","Space for appliances to be stored and charged where necessary. ","Storage (non-teaching)","Storage",2,4,"-","SEN",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled and trolley access required","Open plan","off Corridor","2400 / N/A","2400 / N/A","N/A / 1200","Not required","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W5.1h","general","A means to protect walls from wheelchair damage to be provided","L4.3n","No requirement","No requirement","Required in upper floors and where possible elsewhere","n/a",100,"pres on, abs off, day off","No",null,"T3","Average","Medium","<=1.5","<=2.0",null,"None","Minimal. To recharge appliances","None",2]
["CIR60","Lobbies (ambulant)",null,null,"CIR03","New Build","SL_90_10_51","Lobbies","Lobby area between main external doors and internal lobby doors for ambulant pupils needing additional support, some pupils using mobility aids","Circulation of pupils and others between spaces.","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","CTS","Disabled access into the space required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / 2200","Entrance doors","N/A","Contractor to Specify for approval","DD1.1gv","general double ","N/A","no internal doorset required",null,"Finger guards.","F9.2","entrance","C1.1","general","W5.1h","circulation","including appropriately designed mat well or similar","L4.3n","No requirement","No requirement","Required in upper floors and where possible elsewhere","n/a",100,"pres on, abs off, day off","If fire exit",null,"T3","Average","Medium","<=1.5","<=2.0",null,"None","Minimal","None",1,2,0,"CTS if Fire Containment."]
["CIR65","Lobbies (non-ambulant)",null,null,"CIR03","New Build","SL_90_10_51","Lobbies","Lobby area between main external doors and internal lobby doors for ambulant & non-ambulant pupils needing significant additional support and specialist equipment","Circulation of pupils and others between spaces.","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","CTS","Disabled access into the space required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / 2200","Entrance doors","N/A","Contractor to Specify for approval","DD1.1gv","general double ","N/A","no internal doorset required",null,"Finger guards.","F9.2","entrance","C1.1","general","W5.1h","circulation","including appropriately designed mat well or similar","L4.3n","No requirement","No requirement","Required in upper floors and where possible elsewhere","n/a",100,"pres on, abs off, day off","If fire exit",null,"T3","Average","Medium","<=1.5","<=2.0",null,"None","Minimal","None",1,2,0,"CTS if Fire Containment."]
["CLA01","Seminar rooms (restrictive, extg)","Seminar rooms (restrictive, extg)","CLA01","CLA02","Existing","SL_25_10_78","Seminar rooms","Existing seminar room for smaller 14-19 groups with limited layout options and activities ","Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"B","restrictive",2,1.6,null,1,37,22,22,1,25,"11-19","None","Full disabled access not required","Enclosed",null,"3300 / 2700","as existing","7800 / 7000","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","None",10,2,6]
["CLA02","Seminar rooms","Seminar rooms","CLA02","CLA02","New Build","SL_25_10_78","Seminar rooms","Seminar room for smaller 14-19 groups with a range of layout options and activities","Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"C","standard",4,1.7,null,1,41,22,22,1,25,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","None",10,2,8]
["CLA03","Seminar rooms (extensive, extg)","Seminar rooms (extensive, extg)","CLA03","CLA02","Existing","SL_25_10_78","Seminar rooms","Existing seminar room for smaller 14-19 groups suitable for all classrooms layout options and activities ","Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"D","extensive",5,1.9,null,1,48,22,23,1,26,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","as existing","7800 / 7000","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","None",10,2,10]
["CLA11","Classrooms (restrictive, extg)","Classrooms (restrictive, extg)","CLA11","CLA12","Existing","SL_25_10_14","Classrooms","Existing secondary school classroom for limited layout options and activities ","Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"B","restrictive",2,1.6,null,1,50,30,30,1,33,"11-19","None","Full disabled access not required","Enclosed",null,"3300 / 2700","as existing","7800 / 7000","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","None",9,2,8]
["CLA12","Classrooms (general)","Classrooms (general)","CLA12","CLA12","New Build","SL_25_10_14","Classrooms","Secondary school classroom for a range of layout options and activities","Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"C","standard",4,1.7,null,1,55,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general"," ","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","None",9,2,8]
["CLA12","Classrooms (PE)","Classrooms (PE)","CLA12","CLA12","New Build","SL_25_10_14","Classrooms","Secondary school classroom for a range of layout options and activities","Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"C","standard",4,1.7,null,1,55,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","None",9,2,8]
["CLA13","Classrooms (extensive)","Classrooms (extensive)","CLA13","CLA12","New Build","SL_25_10_14","Classrooms","Secondary school classroom suitable for all classroom layout options and activities","Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"D","extensive",5,1.9,null,1,62,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","None",9,2,8]
["CLA14","Classrooms, double (restrictive, extg)","Classrooms, double (restrictive, extg)","CLA14","CLA15","Existing","SL_25_10_14","Classrooms","Two linked secondary school classrooms for limited layout options and activities ","Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"B","restrictive",2,1.6,null,1,97,60,59,1,65,"11-19","None","Full disabled access not required","Enclosed",null,"3300 / 2700","as existing","7800 / 7000","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","None",20,4,16]
["CLA15","Classrooms, double","Classrooms, double","CLA15","CLA15","New Build","SL_25_10_14","Classrooms","Two linked secondary schools classrooms for a range of layout options and activities","Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"C","standard",4,1.7,null,1,111,60,60,1,66,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general"," ","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","None",20,4,16]
["CLA16","Classrooms, double (extensive, extg)","Classrooms, double (extensive, extg)","CLA16","CLA15","Existing","SL_25_10_14","Classrooms","Two existing linked secondary schools classrooms suitable for all classrooms layout options and activities","Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"D","extensive",5,1.9,null,1,125,60,60,1,66,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","as existing","7800 / 7000","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","None",20,4,16]
["CLA18","Classrooms (smaller group)","Classrooms (smaller group)","CLA18","CLA12","New Build","SL_25_10_14","Classrooms","Secondary school classroom for a range of layout options and activities","Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"C","standard",4,1.7,null,1,48,26,26,1,29,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","None",9,2,8]
["CLA19","Classrooms (larger group)","Classrooms (larger group)","CLA19","CLA12","New Build","SL_25_10_14","Classrooms","Secondary school classroom for a range of layout options and activities","Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"C","standard",4,1.7,null,1,62,34,34,1,38,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","None",9,2,8]
["CLA21","Semi-open classbases, home base (restrictive)","Semi-open classbases, home base (restrictive)","CLA21","CLA22","Existing","SL_25_10_77","Semi-open classbases","Existing secondary school semi-open plan learning area for limited layout options and activities ","Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"B","restrictive",2,1.6,null,1,50,30,30,1,33,"11-19","None","Full disabled access not required","Open-plan or semi-enclosed","off Corridor or Shared teaching area","3300 / 2700","2400 / N/A","7800 / 7000","Optional",1050,"Contractor to Specify for approval if provided","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold water to sink listed in School-specific SoA and ADS",10,2,8]
["CLA22","Semi-open classbases, home base","Semi-open classbases, home base","CLA22","CLA22","New Build","SL_25_10_77","Semi-open classbases","Secondary school semi-open plan learning area, used a registration 'home' base for a group of pupils","Group discussion. Independent study and research. Presentations. Using the whiteboard.","Basic teaching","General",1.5,4,"C","standard",4,1.7,null,1,55,30,30,1,33,"11-19","None","Disabled access into the space required","Open-plan or semi-enclosed","off Corridor or Shared teaching area","3300 / 2700","2400 / N/A","7800 / 7000","Optional",1050,"Contractor to Specify for approval if provided","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general"," ","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold water to sink listed in School-specific SoA and ADS",10,4,10]
["CLA23","Semi-open classbases, home base (extensive)","Semi-open classbases, home base (extensive)","CLA23","CLA22","New Build","SL_25_10_77","Semi-open classbases","Secondary school semi-open plan learning area suitable for all classrooms layout options and activities","Independent study and research. Individual, group and whole class pupil led presentations and discussions using ICT devices and whiteboard. Teacher led presentations and briefings using ICT and the whiteboard.","Basic teaching","General",1.5,4,"D","extensive",5,1.9,null,1,62,30,30,1,33,"11-19","None","Disabled access into the space required","Open-plan or semi-enclosed","off Corridor or Shared teaching area","3300 / 2700","2400 / N/A","7800 / 7000","Optional",1050,"Contractor to Specify for approval if provided","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold water to sink listed in School-specific SoA and ADS",10,6,12]
["CLA31","ICT-rich classrooms (restrictive, extg)","ICT-rich classrooms (restrictive, extg)","CLA31","CLA32","Existing","SL_25_10_41","ICT-rich classrooms","Secondary school classroom temporarily used as restrictive ICT-rich classroom","Independent study and research. Individual, group and whole class pupil led presentations and discussions using ICT devices and whiteboard. Teacher led presentations and briefings using ICT and the whiteboard.","Basic teaching","Fitted",2,4,"C","restrictive",4,1.7,null,1,55,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","as existing","7800 / 7200","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general"," ","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","To suit ICT","None",46,2,20]
["CLA32","ICT-rich classrooms","ICT-rich classrooms","CLA32","CLA32","New Build","SL_25_10_41","ICT-rich classrooms","Secondary school classroom with fixed ICT devices for all workplaces and a range of layout options","Independent study and research. Individual, group and whole class pupil led presentations and discussions using ICT devices and whiteboard. Teacher led presentations and briefings using ICT and the whiteboard.","Basic teaching","Fitted",2,4,"D","standard",5,1.9,null,1,62,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7200","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general"," ","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","To suit ICT","None",46,2,38]
["CLA33","ICT-rich classrooms (extensive)","ICT-rich classrooms (extensive)","CLA33","CLA32","New Build","SL_25_10_41","ICT-rich classrooms","Secondary school classroom with fixed ICT devices for all workplaces, and a wide range of layout options and activities","Independent study and research. Individual, group and whole class pupil led presentations and discussions using ICT devices and whiteboard. Teacher led presentations and briefings using ICT and the whiteboard.","Basic teaching","Fitted",2,4,"E","extensive",6,2.1,null,1,69,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7200","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","To suit ICT","None",46,2,38]
["CLA34","ICT-rich classrooms, semi-open (restrictive, extg)","ICT-rich classrooms, semi-open (restrictive, extg)","CLA34","CLA35","Existing","SL_25_10_41","ICT-rich classrooms","Semi-open plan area with fixed ICT devices for all workplaces with limited layout options","Group discussion. Independent study and research. Presentations. Using ICT devices . Using the whiteboard.","Basic teaching","Fitted",2,4,"C","restrictive",4,1.7,null,1,55,30,30,1,33,"11-19","None","Full disabled access not required","Open-plan or semi-enclosed","off Corridor or Shared teaching area","3300 / 2700","as existing","7800 / 7200","Not required",1050,"","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","To suit ICT","None",46,2,20]
["CLA35","ICT-rich classrooms, semi-open","ICT-rich classrooms, semi-open","CLA35","CLA35","New Build","SL_25_10_41","ICT-rich classrooms","Semi-open plan area with fixed ICT devices for all workplaces and a range of layout options","Group discussion. Independent study and research. Presentations. Using ICT devices . Using the whiteboard.","Basic teaching","Fitted",2,4,"D","standard",5,1.9,null,1,62,30,30,1,33,"11-19","None","Disabled access into the space required","Open-plan or semi-enclosed","off Corridor or Shared teaching area","3300 / 2700","2400 / N/A","7800 / 7200","Not required",1050,"","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general"," ","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","To suit ICT","None",46,2,38]
["CLA36","ICT-rich classrooms, semi-open (extensive)","ICT-rich classrooms, semi-open (extensive)","CLA36","CLA35","New Build","SL_25_10_41","ICT-rich classrooms","Semi-open plan area with fixed ICT devices for all workplaces, and a wide range of layout options and activities","Group discussion. Independent study and research. Presentations. Using ICT devices . Using the whiteboard.","Basic teaching","Fitted",2,4,"E","extensive",6,2.1,null,1,69,30,30,1,33,"11-19","None","Disabled access into the space required","Open-plan or semi-enclosed","off Corridor or Shared teaching area","3300 / 2700","2400 / N/A","7800 / 7200","Not required",1050,"","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","To suit ICT","None",46,2,38]
["CLA41","Classrooms (temporarily ICT-rich) ","Classrooms (temporarily ICT-rich) ","CLA41","CLA12","New Build","SL_25_10_14","Classrooms","Secondary school classroom temporarily used for fixed ICT devices for all workplaces with limited layout options","Group discussion. Independent study and research. Presentations. Using ICT devices . Using the whiteboard.","Basic teaching","Fitted",2,4,"C","restrictive",4,1.7,null,1,55,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7200","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","None",46,2,38]
["CLA42","ICT-rich classrooms (business studies)","ICT-rich classrooms (business studies)","CLA42","CLA32","New Build","SL_25_10_41","ICT-rich classrooms","Secondary school classroom with fixed ICT devices for half workplaces with business environment","Independent study and research. Individual, group and whole class pupil led presentations and discussions using ICT devices predominantly by 14-19 age group. Occasional need for some furniture re-arrangement. Teacher led presentations and briefings using ICT and the whiteboard.","Basic teaching","Fitted",2,4,"D","standard",5,1.9,null,1,69,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7200","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general"," ","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","To suit ICT","None",46,2,38]
["CLA43","ICT-rich classrooms (business studies, extensive)","ICT-rich classrooms (business studies, extensive)","CLA43","CLA32","New Build","SL_25_10_41","ICT-rich classrooms","Secondary school classroom with fixed ICT devices for half workplaces with business environment","Independent study and research. Individual, group and whole class pupil led presentations and discussions using ICT devices predominantly by 14-19 age group. Occasional need for some furniture re-arrangement. Teacher led presentations and briefings using ICT and the whiteboard.","Basic teaching","Fitted",2,4,"E","extensive",6,2.1,null,1,69,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7200","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 5.1","None","To suit ICT","None",46,2,38]
["CLA50","Sixth form SEN classrooms (ambulant)","Sixth form SEN classrooms (ambulant)","CLA50","CLA50","New Build","SL_25_10_81","Sixth form SEN classrooms","Secondary classroom for a range of FF&E layout options and activities for ambulant 16 to 19 year olds needing additional support ","Supported individual and group working including with ICT. Role play. Teacher led presentations using the whiteboard","Basic teaching","General",1.5,4,"G1","SEN",12,3.1,null,1,55,"As SoA",14,1,16,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,"Access control system to be agreed with school. Finger guards","F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,16]
["CLA51","Sixth form SEN classrooms (AP health)","Sixth form SEN classrooms (health)","CLA51","CLA50","New Build","SL_25_10_81","Sixth form SEN classrooms","Secondary classroom for a range of FF&E layout options and activities for ambulant 16 to 19 year olds needing additional support ","Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"F1","SEN",9,2.7,null,1,32,8,9,1,10,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,"Doorset, including ironmongery, finger guards and access control system to be agreed with school","F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,16]
["CLA52","Sixth form SEN classrooms (AP behaviour)","Sixth form SEN classrooms (behaviour)","CLA52","CLA50","New Build","SL_25_10_81","Sixth form SEN classrooms","Secondary classroom for a range of FF&E layout options and activities for ambulant 16 to 19 year olds needing additional support ","Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"G1","SEN",12,3.1,null,1,41,8,9,1,10,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,"Doorset, including ironmongery, finger guards and access control system, to be agreed with school","F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,16]
["CLA53","Sixth form SEN classrooms (with quiet space)","Sixth form SEN classrooms (with quiet bay off)","CLA53","CLA50","New Build","SL_25_10_81","Sixth form SEN classrooms","Secondary classroom for a range of FF&E layout options and activities for ambulant 16 to 19 year olds needing additional support and more ‘personal’ space","Supported individual and group working including with ICT. Role play. Teacher led presentations using the whiteboard","Basic teaching","General",1.5,4,"H","SEN",16,3.3,null,1,48,8,10,1,11,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,"Doorset, including ironmongery and access control system, to be agreed with school. Finger guards","F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,16]
["CLA54","Sixth form SEN classrooms (severe suite)","Sixth form SEN classrooms (in suite)","CLA54","CLA50","New Build","SL_25_10_81","Sixth form SEN classrooms","Secondary classroom for a range of FF&E layout options and activities for ambulant 16 to 19 year olds needing significant additional support and more ‘personal’ space","Supported individual and group working including with ICT. Role play. Teacher led presentations using the whiteboard","Basic teaching","General",1.5,4,"I","SEN",22,3.7,null,1,48,6,7,1,8,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,"Doorset, including ironmongery and access control system, to be agreed with school. Finger guards","F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,16]
["CLA55","Sixth form SEN classrooms, non-ambulant","post-16 classroom (non-ambulant)","CLA55","CLA55","New Build","SL_25_10_81","Sixth form SEN classrooms","Secondary classroom for a range of FF&E layout options and activities for ambulant and non-ambulant 16 to 19 year olds needing significant additional support and specialist equipment","Supported individual and group working including with ICT. Teacher led presentations using the whiteboard. Physiotherapy. Sensory experience. Rest and refreshments.","Basic teaching","General",1.5,4,"J1","SEN",32,4.4000000000000004,null,1,62,6,7,1,8,"11-19","None","Full disabled access required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Optional",1050,"Contractor to Specify for approval if provided","D6.1mv","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1","general","Ceiling to include hoist tracking in both directions, avoiding light fittings","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5/T7","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,16]
["CLA58","Sixth form SEN classrooms, PMLD suite",null,null,"CLA55","New Build","SL_25_10_81","Sixth form SEN classrooms","Secondary classroom for a range of FF&E layout options and activities for non-ambulant 16 to 19 year olds needing significant additional support and specialist equipment","Supported individual and group working including with ICT. Teacher led presentations using the whiteboard. Physiotherapy. Sensory experience. Rest and refreshments.","Basic teaching","General",1.5,4,"J1","SEN",32,4.4000000000000004,null,1,62,6,7,1,8,"11-19","None","Full disabled access required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Optional",1050,"Contractor to Specify for approval if provided","D6.1mv","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1","general","Ceiling to include hoist tracking in both directions, avoiding light fittings","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5/T7","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,16]
["CLA60","Secondary SEN classrooms (ambulant)","Secondary SEN classrooms (ambulant)","CLA60","CLA60","New Build","SL_25_10_76","Secondary SEN classrooms","Secondary classroom for a range of FF&E layout options and activities for ambulant 11 to 16 year olds needing additional support ","Supported individual and group working including with ICT. Role play. Teacher led presentations using the whiteboard","Basic teaching","General",1.5,4,"G1","SEN",12,3.1,null,1,55,"As SoA",14,1,16,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,"Access control system to be agreed with school. Finger guards","F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",18,2,16]
["CLA61","Secondary SEN classrooms (AP health)","Secondary SEN classrooms (health)","CLA61","CLA60","New Build","SL_25_10_76","Secondary SEN classrooms","Secondary classroom for a range of FF&E layout options and activities for ambulant 11 to 16 year olds needing additional support ","Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"F1","SEN",9,2.7,null,1,32,8,9,1,10,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,"Doorset, including ironmongery, finger guards and access control system to be agreed with school","F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,16]
["CLA62","Secondary SEN classrooms (AP behaviour)","Secondary SEN classrooms (behaviour)","CLA62","CLA60","New Build","SL_25_10_76","Secondary SEN classrooms","Secondary classroom for a range of FF&E layout options and activities for ambulant 11 to 16 year olds needing additional support ","Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"G1","SEN",12,3.1,null,1,41,8,9,1,10,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,"Doorset, including ironmongery, finger guards and access control system, to be agreed with school","F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,16]
["CLA63","Secondary SEN classrooms (with quiet space)","Secondary SEN classrooms (with quiet bay off)","CLA63","CLA60","New Build","SL_25_10_76","Secondary SEN classrooms","Secondary classroom for a range of FF&E layout options and activities for ambulant 11 to 16 year olds needing additional support and more ‘personal’ space","Supported individual and group working including with ICT. Role play. Teacher led presentations using the whiteboard","Basic teaching","General",1.5,4,"H","SEN",16,3.3,null,1,48,8,10,1,11,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,"Doorset, including ironmongery and access control system, to be agreed with school. Finger guards","F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,16]
["CLA64","Secondary SEN classrooms (severe suite)","Secondary SEN classrooms (in suite)","CLA64","CLA60","New Build","SL_25_10_76","Secondary SEN classrooms","Secondary classroom for a range of FF&E layout options and activities for ambulant 11 to 16 year olds needing significant additional support and more ‘personal’ space","Supported individual and group working including with ICT. Role play. Teacher led presentations using the whiteboard","Basic teaching","General",1.5,4,"I","SEN",22,3.7,null,1,48,6,7,1,8,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,"Doorset, including ironmongery and access control system, to be agreed with school. Finger guards","F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,16]
["CLA65","Secondary SEN classrooms, non-ambulant","secondary classroom (non-ambulant)","CLA65","CLA65","New Build","SL_25_10_76","Secondary SEN classrooms","Secondary classroom for a range of FF&E layout options and activities for ambulant & non-ambulant 11 to 16 year olds needing significant additional support and specialist equipment","Supported individual and group working including with ICT. Teacher led presentations using the whiteboard. Physiotherapy. Sensory experience. Rest and refreshments.","Basic teaching","General",1.5,4,"J1","SEN",32,4.4000000000000004,null,1,62,6,7,1,8,"11-19","None","Full disabled access required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Optional",1050,"Contractor to Specify for approval if provided","D6.1mv","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1","general","Ceiling to include hoist tracking in both directions, avoiding light fittings","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5/T7","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,16]
["CLA66","Semi-open classbases, home base (ambulant)","Semi-open classbases, homebase","CLA66","CLA66","New Build","SL_25_10_77","Semi-open classbases","Secondary semi-open plan learning area, used as a 'home' base for a group of ambulant pupils needing additional support","Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Role play. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"G1","SEN",12,3.1,null,1,55,12,14,1,16,"11-19","None","Disabled access into the space required","Enclosed","off Corridor or Shared teaching area","3300 / 2700","2400 / N/A","7800 / 7000","Optional",1050,"Contractor to Specify for approval if provided","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold water to sink listed in School-specific SoA and ADS",10,2,16]
["CLA68","Secondary SEN classrooms, PMLD suite",null,null,"CLA65","New Build","SL_25_10_76","Secondary SEN classrooms","Secondary classroom for a range of FF&E layout options and activities for non-ambulant 11 to 16 year olds needing significant additional support and specialist equipment","Supported individual and group working including with ICT. Teacher led presentations using the whiteboard. Physiotherapy. Sensory experience. Rest and refreshments.","Basic teaching","General",1.5,4,"J1","SEN",32,4.4000000000000004,null,1,62,6,7,1,8,"11-19","None","Full disabled access required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Optional",1050,"Contractor to Specify for approval if provided","D6.1mv","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1","general","Ceiling to include hoist tracking in both directions, avoiding light fittings","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5/T7","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,16]
["CLA70","ICT-rich classrooms (ambulant)","ICT-rich classrooms (ambulant)","CLA70","CLA32","New Build","SL_25_10_41","ICT-rich classrooms","Specialist secondary space with fixed ICT devices for all workplaces for ambulant pupils needing additional support  ","Independent study and research. Individual, group and whole class pupil led presentations and discussions using ICT devices and whiteboard. Teacher led presentations and briefings using ICT and the whiteboard.","Basic teaching","Fitted",2,4,"G1","SEN",12,3.1,null,1,55,"As SoA",14,1,16,"CTS","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7200","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,"Doorset, including ironmongery, finger guards and access control system, to be agreed with school","F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit ICT","None",38,0,38]
["CLA71","ICT-rich classrooms (AP)",null,null,"CLA32","New Build","SL_25_10_41","ICT-rich classrooms","Specialist secondary space with fixed ICT devices for all workplaces for ambulant pupils needing additional support  ","Independent study and research. Individual, group and whole class pupil led presentations and discussions using ICT devices and whiteboard. Teacher led presentations and briefings using ICT and the whiteboard.","Basic teaching","Fitted",2,4,"G1","SEN",12,3.1,null,1,41,8,"10",1,12,"CTS","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7200","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,"Doorset, including ironmongery, finger guards and access control system, to be agreed with school","F1.1","general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit ICT","None",38,0,38]
["CLA75","ICT-rich classrooms, non-ambulant","ICT-rich classrooms, non-ambulant","CLA75","CLA75","New Build","SL_25_10_41","ICT-rich classrooms","Specialist secondary space with fixed ICT devices for all workplaces for ambulant and non-ambulant 11 to 16 year olds needing significant additional support and specialist equipment","Independent study and research. Individual, group and whole class pupil led presentations and discussions using ICT devices and whiteboard. Teacher led presentations and briefings using ICT and the whiteboard.","Basic teaching","Fitted",2,4,"H - J","SEN",28,4.2,null,1,55,8,"12",1,14,"CTS","None","Full disabled access required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7200","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1","general",null,"L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5/T7","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit ICT","None",38,0,38]
["DAT00","Art rooms","Art rooms","DAT00","DAT00","New Build","SL_25_10_04","Art rooms","Secondary school art room for a range of general art","Individual and group 2D work (drawing, painting). Individual, group and whole class pupil led presentations and discussions using the whiteboard. Small scale 3D work using a range of materials including card, plastic and wood. Some pupil research occasionally using ICT. Teacher led presentations and briefings using the whiteboard.","Basic teaching","Light practical",2.5,4,"F","standard",8,2.5,null,1,83,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W1.1h","general","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.6 when practical work involving fumes is planned.","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",24,2,12]
["DAT01","Art rooms (restrictive, extg)","Art rooms (restrictive, extg)","DAT01","DAT00","Existing","SL_25_10_04","Art rooms","Existing secondary school art room for a limited range of general art","Individual and group 2D work (drawing, painting). Individual, group and whole class pupil led presentations and discussions using the whiteboard. Small scale 3D work using a range of materials including card, plastic and wood. Some pupil research occasionally using ICT. Teacher led presentations and briefings using the whiteboard.","Basic teaching","Light practical",2.5,4,"E1","restrictive",7,2.2999999999999998,null,1,76,30,30,1,33,"11-19","None","Full disabled access not required","Enclosed",null,"3300 / 2700","as existing","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W1.1h","general",null,"L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.6 when practical work involving fumes is planned.","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",24,2,12]
["DAT02","Art rooms (general)","Art rooms (general)","DAT02","DAT00","New Build","SL_25_10_04","Art rooms","Secondary school art room for a range of general art","Individual and group 2D work (drawing, painting). Individual, group and whole class pupil led presentations and discussions using the whiteboard. Small scale 3D work using a range of materials including card, plastic and wood. Some pupil research occasionally using ICT. Teacher led presentations and briefings using the whiteboard.","Basic teaching","Light practical",2.5,4,"F","standard",8,2.5,null,1,83,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W1.1h","general","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.6 when practical work involving fumes is planned.","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",24,2,12]
["DAT03","Art rooms (3D)","Art rooms (3D)","DAT03","DAT00","New Build","SL_25_10_04","Art rooms","Secondary school art room for general and 3D art ","2D work (drawing, painting). Small scale 3D work. Whole class presentations and discussions using the whiteboard.","Basic teaching","Light practical",2.5,4,"G","extensive",10,2.9,null,1,97,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W1.1h","general","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.6 when practical work involving fumes is planned.","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",22,2,12,"Need to be able to clean surfaces of clay dust; sufficient space must be allowed around pottery equipment."]
["DAT04","Art rooms (ceramics)","Art rooms (ceramics)","DAT04","DAT00","New Build","SL_25_10_04","Art rooms","Secondary school art room for general and 3D art including clay, typically using a potter's wheel","2D work (drawing, painting). Large scale 3D work with extensive use of clay, including using a wheel. Whole class presentations and discussions using the whiteboard.","Basic teaching","Light practical",2.5,4,"G1","extensive",12,3.1,null,1,97,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W1.1h","general","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.6 when practical work involving fumes is planned.","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",22,2,12,"Need to be able to clean surfaces of clay dust; sufficient space must be allowed around pottery equipment."]
["DAT05","Art rooms (textiles)","Art rooms (textiles)","DAT05","DAT00","New Build","SL_25_10_04","Art rooms","Secondary school art room for general art and making with textiles","2D work (drawing, painting). Printing techniques for 2D and 3D work. Whole class presentations and discussions using the whiteboard.","Basic teaching","Light practical",2.5,4,"G1","extensive",12,3.1,null,1,97,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W1.1h","general","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.6 when practical work involving fumes is planned.","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",22,2,12]
["DAT12","Hair and beauty training salons","Hair and beauty training salons","DAT12","DAT12","New Build","SL_25_40_36","Hair and beauty training salons","Secondary school salon for hair dressing and beauty therapy","Individual and paired pupil practical work and teacher demonstration using specialist chairs, basins and beds. Occasional use of mobile tables and the whiteboard. Waiting area for those being treated.","Basic teaching","Light practical",2.5,4,"H","standard",16,3.3,null,1,69,16,16,1,18,"11-19","Optional ","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Entrance door",1050,"Contractor to Specify for approval","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W1.1h","general","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.6 when practical work involving fumes is planned.","None","To suit equipment","Hot and cold water to all sinks listed under FF&E, cold water to other sinks or equipment",12,2,8]
["DAT15","Photography studios","Photography studios","DAT15","DAT15","New Build","SL_25_40_65","Photography studios","Secondary school studio for practical photography and editing","Individual and group photography, using a range of equipment including white background, lighting and tripod. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Photo editing and pupil research using ICT. Teacher led presentations and briefings using the whiteboard.","Basic teaching","Light practical",2.5,4,"F","standard",8,2.5,null,1,69,24,24,1,27,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7500","Not required",1050,"","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W1.1h","general","At least one wall shall be clear and white. Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.6 when practical work involving fumes is planned.","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",46,2,38]
["DAT20","DT studios","DT studios","DAT20","DAT20","New Build","SL_25_40_22","Design Technology studios","Secondary school room for design technology and small scale product design","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Small scale making. Traditional and computer based drawing and design.","Basic teaching","Light practical",2.5,4,"G","standard",10,2.9,null,1,83,24,25,1,28,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W1.1h","general","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.5.","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",46,2,38]
["DAT21","DT studios (graphic products, restrictive, extg)","DT studios (graphic products, restrictive, extg)","DAT21","DAT20","Existing","SL_25_40_22","Design Technology studios","Existing secondary school room for limited small scale product design","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Small scale making with card and some plastics. Traditional and computer based drawing and design.","Basic teaching","Light practical",2.5,4,"F1","restrictive",9,2.7,null,1,76,24,25,1,28,"11-19","None","Full disabled access not required","Enclosed",null,"3300 / 2700","as existing","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W1.1h","general","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.5.","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",46,2,38]
["DAT22","DT studios (graphic products)","DT studios (graphic products)","DAT22","DAT20","New Build","SL_25_40_22","Design Technology studios","Secondary school room for graphics and small scale product design","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Small scale making with card and some plastics. Traditional and computer based drawing and design.","Basic teaching","Light practical",2.5,4,"G","standard",10,2.9,null,1,83,24,25,1,28,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W1.1h","general","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.5.","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",46,2,38]
["DAT24","DT studios (textiles, restrictive, extg)","DT studios (textiles, restrictive, extg)","DAT24","DAT20","Existing","SL_25_40_22","Design Technology studios","Existing secondary school room for working with a limited range of 'dry' textiles","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making with textiles including traditional and computerised sewing and knitting machines. Traditional and computer based drawing and design.","Basic teaching","Light practical",2.5,4,"F1","restrictive",9,2.7,null,1,76,24,25,1,28,"11-19","None","Full disabled access not required","Enclosed",null,"3300 / 2700","as existing","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W1.1h","general","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.5.","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",22,2,38]
["DAT25","DT studios (textiles)","DT studios (textiles)","DAT25","DAT20","New Build","SL_25_40_22","Design Technology studios","Secondary school room for working with a range of 'dry' textiles","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making with textiles including traditional and computerised sewing and knitting machines. Traditional and computer based drawing and design.","Basic teaching","Light practical",2.5,4,"G","standard",10,2.9,null,1,83,24,25,1,28,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W1.1h","general","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.5.","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",22,2,16]
["DAT27","DT studios (electronics & control, restrictive, extg)","DT studios (electronics & control, restrictive, extg)","DAT27","DAT20","Existing","SL_25_40_22","Design Technology studios","Existing secondary school room for a limited range of electronics, pneumatics and light, small scale product design","Drawing. ICT based research and design. Incorporating electronic. Robotic and pneumatic techniques. Small scale making with card. Whole class presentations and discussions using the whiteboard. Wood and plastics.","Basic teaching","Light practical",2.5,4,"F1","restrictive",9,2.7,null,1,76,24,25,1,28,"11-19","None","Full disabled access not required","Enclosed",null,"3300 / 2700","as existing","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W1.1h","general","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.5.","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",31,2,38]
["DAT28","DT studios (electronics & control)","DT studios (electronics & control)","DAT28","DAT20","New Build","SL_25_40_22","Design Technology studios","Secondary school room for a range of  electronics, pneumatics and light, small scale product design","Drawing. ICT based research and design. Incorporating electronic. Robotic and pneumatic techniques. Small scale making with card. Whole class presentations and discussions using the whiteboard. Wood and plastics.","Basic teaching","Light practical",2.5,4,"G","standard",10,2.9,null,1,83,24,25,1,28,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,null,null,null,"C1.1","general","W1.1h","general","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.5.","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",31,2,38]
["DAT31","Food rooms (demonstration, restrictive, extg)","Food rooms (demonstration, restrictive, extg)","DAT31","DAT35","Existing","SL_25_10_30","Food rooms","Existing secondary school food room for demonstrations of food preparation, but no pupil practical","ICT based research and design. Making and tasting food. Teacher demonstrations. Using the whiteboard. Whole class presentations and discussions.","Basic teaching","Heavy practical (clean)",3.5,4,"E1","restrictive",7,2.2999999999999998,null,1,62,24,24,1,27,"11-19","None","Full disabled access not required","Enclosed",null,"2700 / 2700","as existing","7800 / 7500","Not required",1050,"","D2.2av","strong","D2.2av","strong",null,null,"F3.4h","hygienic non-slip","C1.2","humid areas","W3.2","humid","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","Average","Medium","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.3","Gas supply to any gas ovens, hobs and other appliances","To suit equipment","Hot and cold drinking water to all sinks, equipment and appliances",11,2,10,"Need to be able to clean surfaces thoroughly to maintain hygiene; safe distances around cookers."]
["DAT32","Food rooms (demonstration)","Food rooms (demonstration)","DAT32","DAT35","New Build","SL_25_10_30","Food rooms","Secondary school food room for demonstrations of food preparation, but limited pupil practical","ICT based research and design. Making and tasting food. Teacher demonstrations. Using the whiteboard. Whole class presentations and discussions.","Basic teaching","Heavy practical (clean)",3.5,4,"F","standard",8,2.5,null,1,69,24,24,1,27,"11-19","None","Disabled access into the space required","Enclosed",null,"2700 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D2.2av","strong","D2.2av","strong",null,null,"F3.4h","hygienic non-slip","C1.2","humid areas","W3.2","humid","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","Average","Medium","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.3","Gas supply to any gas ovens, hobs and other appliances","To suit equipment","Hot and cold drinking water to all sinks, equipment and appliances",11,2,10,"Need to be able to clean surfaces thoroughly to maintain hygiene; safe distances around cookers."]
["DAT34","Food rooms (restrictive, extg)","Food rooms (restrictive, extg)","DAT34","DAT35","Existing","SL_25_10_30","Food rooms","Secondary school food room for non-vocational practical cookery activities by pupil groups of 2 or 3","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making and tasting food. Teacher practical demonstrations. Traditional and computer based design of recipes etc.","Basic teaching","Heavy practical (clean)",3.5,4,"G1","restrictive",12,3.1,null,1,90,24,24,1,27,"11-19","None","Full disabled access not required","Enclosed",null,"2700 / 2700","as existing","7800 / 7500","Not required",1050,"","D2.2av","strong","D2.2av","strong",null,null,"F3.4h","hygienic non-slip","C1.2","humid areas","W3.2","humid","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","Average","Medium","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.3","Gas supply to any gas ovens, hobs and other appliances","To suit equipment","Hot and cold drinking water to all sinks, equipment and appliances",13,2,16,"Need to be able to clean surfaces thoroughly to maintain hygiene; safe distances around cookers."]
["DAT35","Food rooms","Food rooms","DAT35","DAT35","New Build","SL_25_10_30","Food rooms","Secondary school food room for a range of non-vocational practical cookery activities by pupils in pairs ","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making and tasting food. Teacher practical demonstrations. Traditional and computer based design of recipes etc.","Basic teaching","Heavy practical (clean)",3.5,4,"H","standard",16,3.3,null,1,97,24,27,1,30,"11-19","None","Disabled access into the space required","Enclosed",null,"2700 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D2.2av","strong","D2.2av","strong",null,null,"F3.4h","hygienic non-slip","C1.2","humid areas","W3.2","humid","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","Average","Medium","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.3","Gas supply to any gas ovens, hobs and other appliances","To suit equipment","Hot and cold drinking water to all sinks, equipment and appliances",13,2,16,"Need to be able to clean surfaces thoroughly to maintain hygiene; safe distances around cookers."]
["DAT36","Food rooms (existing for 20)","Food rooms (existing for 20)","DAT36","DAT35","Existing","SL_25_10_30","Food rooms","Secondary school food room for a range of non-vocational practical cookery activities by pupils in pairs ","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making and tasting food. Teacher practical demonstrations. Traditional and computer based design of recipes etc.","Basic teaching","Heavy practical (clean)",3.5,4,"H1","standard",18,3.5,null,1,90,20,21,1,24,"11-19","None","Disabled access into the space required","Enclosed",null,"2700 / 2700","as existing","7800 / 7500","Not required",1050,"","D2.2av","strong","D2.2av","strong",null,null,"F3.4h","hygienic non-slip","C1.2","humid areas","W3.2","humid","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","Average","Medium","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.3","Gas supply to any gas ovens, hobs and other appliances","To suit equipment","Hot and cold drinking water to all sinks, equipment and appliances",13,2,16,"Need to be able to clean surfaces thoroughly to maintain hygiene; safe distances around cookers."]
["DAT37","Food rooms (2 of 2)","Food rooms (2 of 2)","DAT37","DAT35","New Build","SL_25_10_30","Food rooms","Second of 2 or more secondary school food rooms for a range of non-vocational practical cookery activities by pupils in pairs ","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making and tasting food. Teacher practical demonstrations. Traditional and computer based design of recipes etc.","Basic teaching","Heavy practical (clean)",3.5,4,"H","standard",16,3.3,null,1,97,24,25,1,28,"11-19","None","Disabled access into the space required","Enclosed",null,"2700 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D2.2av","strong","D2.2av","strong",null,null,"F3.4h","hygienic non-slip","C1.2","humid areas","W3.2","humid","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","Average","Medium","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.3","Gas supply to any gas ovens, hobs and other appliances","To suit equipment","Hot and cold drinking water to all sinks, equipment and appliances",13,2,16,"Need to be able to clean surfaces thoroughly to maintain hygiene; safe distances around cookers."]
["DAT39","Catering training kitchens","Catering training kitchens","DAT39","DAT39","New Build","SL_25_40_11","Catering training kitchens","Secondary school food room for vocational courses in catering","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making and tasting food using commercial catering equipment. Teacher practical demonstrations. ","Basic teaching","Heavy practical (clean)",3.5,4,"H1","standard",18,3.5,null,1,97,20,21,1,24,"11-19","None","Disabled access into the space required","Enclosed",null,"2700 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D2.2av","strong","D2.2av","strong",null,null,"F3.4h","hygienic non-slip","C1.2","humid areas","W3.2","humid","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","Average","Medium","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.3","Gas supply to any gas ovens, hobs and other appliances","To suit equipment","Hot and cold drinking water to all sinks, equipment and appliances",7,2,16,"Need to be able to clean surfaces thoroughly to maintain hygiene; safe distances around cookers."]
["DAT41","DT workshops (existing for 20)","DT workshops (existing for 20)","DAT41","DAT43","Existing","SL_25_40_23","Design technology workshops","Existing secondary school workshop for working with resistant materials, with limited group size","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making with wood, plastics and some metals. Some electronics and control. Teacher demonstrations using machines and practical multibenches. Traditional and computer based drawing and design.","Basic teaching","Heavy practical (workshop)",3.5,4,"H1","standard",18,3.5,null,1,97,20,21,1,24,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","as existing","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D2.1av","strong","D2.1av","strong",null,"Access control system to be agreed with school. ","F5.4","heavy practical","C1.1","general","W4.1","rough","Flooring suitable for heavy movable FF&E on castors. Concrete or ceramic tiles floor required around any heat treatment equipment","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","High","High","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.5 and 7.6","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",12,2,16,"Lockable single switch disconnector for power and emergency stop system for fixed machinery; Safe distances around fixed equipment and workbenches."]
["DAT42","DT workshops (restrictive, extg)","DT workshops (restrictive, extg)","DAT42","DAT43","Existing","SL_25_40_23","Design technology workshops","Existing secondary school workshop for working with resistant materials, with limited machines","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making with wood, plastics and some metals. Some electronics and control. Teacher demonstrations using machines and practical multibenches. Traditional and computer based drawing and design.","Basic teaching","Heavy practical (workshop)",3.5,4,"G1","restrictive",12,3.1,null,1,90,24,24,1,27,"11-19","None","Full disabled access not required","Enclosed",null,"3300 / 2700","as existing","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D2.1av","strong","D2.1av","strong",null,"Access control system to be agreed with school. ","F5.4","heavy practical","C1.1","general","W4.1","rough","Flooring suitable for heavy movable FF&E on castors. Concrete or ceramic tiles floor required around any heat treatment equipment","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","High","High","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.5 and 7.6","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",12,2,16,"Lockable single switch disconnector for power and emergency stop system for fixed machinery; Safe distances around fixed equipment and workbenches."]
["DAT43","DT workshops","DT workshops","DAT43","DAT43","New Build","SL_25_40_23","Design technology workshops","Secondary school workshop for working with all resistant materials, including wood, metal and plastics","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making with wood, plastics and some metals. Some electronics and control. Teacher demonstrations using machines and practical multibenches. Traditional and computer based drawing and design.","Basic teaching","Heavy practical (workshop)",3.5,4,"H","standard",16,3.3,null,1,111,24,27,1,30,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2700","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D2.1av","strong","D2.1av","strong",null,"Access control system to be agreed with school. ","F5.4","heavy practical","C1.1","general","W4.1","rough","Flooring suitable for heavy movable FF&E on castors. Concrete or ceramic tiles floor required around any heat treatment equipment","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","High","High","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.5 and 7.6","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",12,2,16,"Lockable single switch disconnector for power and emergency stop system for fixed machinery; Safe distances around fixed equipment and workbenches."]
["DAT44","DT workshops (2 of 2)","DT workshops (2 of 2)","DAT44","DAT43","New Build","SL_25_40_23","Design technology workshops","Second of two or more secondary school workshops for working with timber and plastics or with metal","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making with wood, plastics and some metals. Some electronics and control. Teacher demonstrations using machines and practical multibenches. Traditional and computer based drawing and design.","Basic teaching","Heavy practical (workshop)",3.5,4,"H","standard",16,3.3,null,1,97,24,25,1,28,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2700","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D2.1av","strong","D2.1av","strong",null,"Access control system to be agreed with school. ","F5.4","heavy practical","C1.1","general","W4.1","rough","Flooring suitable for heavy movable FF&E on castors. Concrete or ceramic tiles floor required around any heat treatment equipment","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","High","High","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.5 and 7.6","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",12,2,16,"Lockable single switch disconnector for power and emergency stop system for fixed machinery; Safe distances around fixed equipment and workbenches."]
["DAT46","DT workshops (with heat bay)","DT workshops (with heat bay)","DAT46","DAT47","New Build","SL_25_40_23","Design technology workshops","Secondary school workshop for working with a range of resistant materials, with heat bay area","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making with wood, plastics and some metals. Some electronics and control. Teacher demonstrations using machines and practical multibenches. Traditional and computer based drawing and design.","Basic teaching","Heavy practical (workshop)",3.5,4,"I","standard",22,3.7,null,1,111,24,26,1,29,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2700","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D2.1av","strong","D2.1av","strong",null,"Access control system to be agreed with school. ","F5.4","heavy practical","C1.1","general","W4.1","rough","Flooring suitable for heavy movable FF&E on castors. Concrete or ceramic tiles floor required around any heat treatment equipment","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","High","High","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.5 and 7.6","Bottled gas only","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",12,2,16,"Lockable single switch disconnector for power and emergency stop system for fixed machinery; Safe distances around fixed equipment and workbenches."]
["DAT47","Engineering workshops","Engineering workshops","DAT47","DAT47","New Build","SL_25_40_27","Engineering workshops","Secondary school workshop for vocational engineering courses, with heat bay area","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making with wood, metals (including heat treatment) and some plastics. Some electronics and control. Teacher demonstrations using machines and practical multibenches.","Basic teaching","Heavy practical (workshop)",3.5,4,"I","standard",22,3.7,null,1,97,20,20,1,22,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2700","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D2.1av","strong","D2.1av","strong",null,"Access control system to be agreed with school. ","F5.4","heavy practical","C1.1","general","W4.1","rough","Flooring suitable for heavy movable FF&E on castors. Concrete or ceramic tiles floor required around any heat treatment equipment","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","High","High","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.5 and 7.6","Bottled gas only","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",12,2,16,"Lockable single switch disconnector for power and emergency stop system for fixed machinery; means to isolate and restore gas supply. Safe distances around fixed equipment and workbenches."]
["DAT49","Construction workshops","Construction workshops","DAT49","DAT49","New Build","SL_25_40_15","Construction workshops","Secondary school workshop for vocational construction courses ","Construction skills including painting and decorating; plumbing and carpentry. Teacher demonstrations using machines and practical multibenches.","Basic teaching","Heavy practical (workshop)",3.5,4,"J","standard",28,4.2,null,1,111,16,16,1,18,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2700","7800 / 7500","Double doors",1050,"Contractor to Specify for approval","D2.1av","strong","D2.1av","strong",null,"Access control system to be agreed with school. ","F5.4","heavy practical","C1.1","general","W4.1","rough","Flooring suitable for heavy movable FF&E on castors. Concrete or ceramic tiles floor required around any heat treatment equipment","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","High","High","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.5 and 7.6","Bottled gas only","To suit equipment","Cold water to wet serviced bollards or similar listed under FF&E, hot and cold to belfast or hand wash sink; chemically resistance drainage.",10,2,16,"Lockable single switch disconnector for power and emergency stop system for fixed machinery; means to isolate and restore gas supply. Safe distances around fixed equipment and workbenches."]
["DAT50","Art rooms (ambulant)","Art rooms (ambulant)","DAT50","DAT00","New Build","SL_25_10_04","Art rooms","Secondary room for a range of general art activities for ambulant pupils needing additional support","2D work (drawing, painting). Small scale 3D work. Whole class presentations and discussions using the whiteboard.","Basic teaching","Light practical",2.5,4,"H - I","SEN",16,3.3,null,1,55,12,"12",1,14,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,"Access control system to be agreed with school. Finger guards","F3.4","chemical resistant non-slip","C1.1","general","W1.1h","general","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",4,2,16]
["DAT51","Art rooms (AP)",null,null,"DAT00","New Build","SL_25_10_04","Art rooms","Secondary room for a range of general art activities for ambulant pupils needing additional support","2D work (drawing, painting). Small scale 3D work. Whole class presentations and discussions using the whiteboard.","Basic teaching","Light practical",2.5,4,"G1","SEN",12,3.1,null,1,41,8,"10",1,12,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,"Doorset, including ironmongery, finger guards and access control system to be agreed with school","F3.4","chemical resistant non-slip","C1.1","general","W1.1h","general","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",4,2,16]
["DAT55","Art rooms, non-ambulant","secondary art room (non-ambulant)","DAT55","DAT55","New Build","SL_25_10_04","Art rooms","Secondary room for a range of general art activities for ambulant and non-ambulant pupils needing significant additional support and specialist equipment","2D work (drawing, painting). Small scale 3D work. Whole class presentations and discussions using the whiteboard.","Basic teaching","Light practical",2.5,4,"J1","SEN",32,4.4000000000000004,null,1,62,6,7,1,8,"11-19","None","Full disabled access required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D6.1mv","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F3.4","chemical resistant non-slip","C1.1","general","W1.1h","general",null,"L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5/T7","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",4,2,16]
["DAT60","DT studios (ambulant art and design)","DT studios (ambulant art and design)","DAT60","DAT20","New Build","SL_25_40_22","Design technology studios","Secondary room for a range of art and D&T activities for ambulant pupils needing additional support","2D work (drawing, painting). Small scale 3D work including some use of machines. Whole class presentations and discussions using the whiteboard. ","Basic teaching","Light practical",2.5,4,"H - I","SEN",16,3.3,null,1,55,8,"12",1,14,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,"Access control system to be agreed with school. Finger guards","F3.4","chemical resistant non-slip","C1.1","general","W1.1h","general","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",4,2,16]
["DAT61","DT studios (AP art and design)",null,null,"DAT20","New Build","SL_25_40_22","Design technology studios","Secondary room for a range of art and D&T activities for ambulant pupils needing additional support","2D work (drawing, painting). Small scale 3D work including some use of machines. Whole class presentations and discussions using the whiteboard. ","Basic teaching","Light practical",2.5,4,"H - I","SEN",16,3.3,null,1,41,8,"12",1,14,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,"Doorset, including ironmongery, finger guards and access control system to be agreed with school","F3.4","chemical resistant non-slip","C1.1","general","W1.1h","general","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",4,2,16]
["DAT65","DT studios, non-ambulant (art and design)","secondary art and design studio (non-ambulant)","DAT65","DAT65","New Build","SL_25_40_22","Design technology studios","Secondary room for a range of art and D&T activities for ambulant & non-ambulant pupils needing significant additional support and specialist equipment","2D work (drawing, painting). Small scale 3D work including some use of machines. Whole class presentations and discussions using the whiteboard. ","Basic teaching","Light practical",2.5,4,"J1","SEN",32,4.4000000000000004,null,1,62,6,7,1,8,"11-19","None","Full disabled access required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D6.1mv","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F3.4h","hygienic non-slip","C1.1","general","W1.1h","general",null,"L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5/T7","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",4,2,16]
["DAT70","Hair and beauty training salons (ambulant)","Hair and beauty training salons (ambulant)","DAT70","DAT15","New Build","SL_25_40_36","Hair and beauty training salons","Secondary salon for hair dressing and beauty therapy for ambulant pupils needing additional support ","Individual and paired pupil practical work and teacher demonstration using specialist chairs, basins and beds. Occasional use of mobile tables and the whiteboard. Waiting area for those being treated.","Basic teaching","Light practical",2.5,4,"I","SEN",22,3.7,null,1,55,8,9,1,12,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Entrance door",1050,"Contractor to Specify for approval","D1.1av","general","D1.1av","general",null,"Access control system to be agreed with school. Finger guards","F3.4","chemical resistant non-slip","C1.1","general","W1.1h","general","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit equipment","Hot and cold water to all sinks listed under FF&E, cold water to other sinks or equipment",4,2,16]
["DAT75","Hair and beauty training salons, non-ambulant","hair and beauty (non-ambulant)","DAT75","DAT75","New Build","SL_25_40_36","Hair and beauty training salons","Secondary salon for hair dressing and beauty therapy for ambulant & non-ambulant pupils needing significant additional support and specialist equipment","Individual and paired pupil practical work and teacher demonstration using specialist chairs, basins and beds. Occasional use of mobile tables and the whiteboard. Waiting area for those being treated.","Basic teaching","Light practical",2.5,4,"J1","SEN",32,4.4000000000000004,null,1,62,6,7,1,8,"11-19","None","Full disabled access required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7000","Not required",1050,"","D6.1mv","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F3.4h","hygienic non-slip","C1.1","general","W1.1h","general",null,"L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5/T7","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",4,2,16]
["DAT80","Food rooms (ambulant)","Food rooms (ambulant)","DAT80","DAT35","New Build","SL_25_10_30","Food rooms","Secondary room for a range of non-vocational practical cookery activities for ambulant pupils needing additional support ","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making and tasting food. Teacher practical demonstrations. Traditional and computer based design of recipes etc.","Basic teaching","Heavy practical (clean)",3.5,4,"I1","SEN",25,3.9,null,1,"As SoA","As SoA","As SoA",1,"As SoA","11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D2.1av","strong","D2.1av","strong",null,"Doorset, including ironmongery, finger guards and access control system to be agreed with school","F3.4h","hygienic non-slip","C1.2","humid areas","W3.2","humid","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.3 and 7.8 Table 7-4. *Acoustics: see BB93 0.4","Gas supply to any gas ovens, hobs and other appliances","To suit equipment","Hot and cold drinking water to all sinks, equipment and appliances",4,2,16,"Need to be able to clean surfaces thoroughly to maintain hygiene; safe distances around cookers."]
["DAT83","Food rooms (ambulant up to 8)",null,null,"DAT35","New Build","SL_25_10_30","Food rooms","Secondary room for a range of non-vocational practical cookery activities for ambulant pupils needing additional support ","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making and tasting food. Teacher practical demonstrations. Traditional and computer based design of recipes etc.","Basic teaching","Heavy practical (clean)",3.5,4,"I1","SEN",25,3.9,null,1,55,8,"8",1,9,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D2.1av","strong","D2.1av","strong",null,"Doorset, including ironmongery, finger guards and access control system to be agreed with school","F3.4h","hygienic non-slip","C1.2","humid areas","W3.2","humid","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.3 and 7.8 Table 7-4. *Acoustics: see BB93 0.4","Gas supply to any gas ovens, hobs and other appliances","To suit equipment","Hot and cold drinking water to all sinks, equipment and appliances",4,2,16,"Need to be able to clean surfaces thoroughly to maintain hygiene; safe distances around cookers."]
["DAT84","Food rooms (ambulant up to 12)",null,null,"DAT35","New Build","SL_25_10_30","Food rooms","Secondary room for a range of non-vocational practical cookery activities for ambulant pupils needing additional support ","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making and tasting food. Teacher practical demonstrations. Traditional and computer based design of recipes etc.","Basic teaching","Heavy practical (clean)",3.5,4,"I1","SEN",25,3.9,null,1,69,12,"12",1,13,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D2.1av","strong","D2.1av","strong",null,"Doorset, including ironmongery, finger guards and access control system to be agreed with school","F3.4h","hygienic non-slip","C1.2","humid areas","W3.2","humid","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.3 and 7.8 Table 7-4. *Acoustics: see BB93 0.4","Gas supply to any gas ovens, hobs and other appliances","To suit equipment","Hot and cold drinking water to all sinks, equipment and appliances",4,2,16,"Need to be able to clean surfaces thoroughly to maintain hygiene; safe distances around cookers."]
["DAT85","Food rooms, non-ambulant","secondary food room (non-ambulant)","DAT85","DAT85","New Build","SL_25_10_30","Food rooms","Secondary room for a range of non-vocational practical cookery activities for ambulant and non-ambulant pupils needing significant additional support and specialist equipment","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making and tasting food. Teacher practical demonstrations. Traditional and computer based design of recipes etc.","Basic teaching","Heavy practical (clean)",3.5,4,"J1","SEN",32,4.4000000000000004,null,1,62,6,7,1,8,"11-19","None","Full disabled access required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D6.2mv","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F3.4h","hygienic non-slip","C1.2","humid areas","W3.2","humid",null,"L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5/T7","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.3 and 7.8 Table 7-4. *Acoustics: see BB93 0.4","Gas supply to any gas ovens, hobs and other appliances","To suit equipment","Hot and cold drinking water to all sinks, equipment and appliances",4,2,16]
["DAT87","Catering training kitchens (ambulant)","Catering training kitchens (ambulant)","DAT87","DAT39","New Build","SL_25_40_11","Catering training kitchens","Secondary food room for vocational courses in catering for ambulant pupils needing additional support ","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making and tasting food using commercial catering equipment. Teacher practical demonstrations. ","Basic teaching","Heavy practical (clean)",3.5,4,"J1","SEN",32,4.4000000000000004,null,1,69,6,7,1,8,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D2.2av","strong","D2.2av","strong",null,"Doorset, including ironmongery, finger guards and access control system to be agreed with school","F3.4h","hygienic non-slip","C1.2","humid areas","W3.2","humid","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","Average","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.3 and 7.8 Table 7-4. *Acoustics: see BB93 0.4","Gas supply to any gas ovens, hobs and other appliances","To suit equipment","Hot and cold drinking water to all sinks, equipment and appliances",7,2,16,"Need to be able to clean surfaces thoroughly to maintain hygiene; safe distances around cookers."]
["DAT90","DT workshops (ambulant)","DT workshops (ambulant)","DAT90","DAT43","New Build","SL_25_40_23","Design technology workshops","Secondary workshop for working with a range of resistant materials, for ambulant pupils needing additional support ","Independent study and research with some use of ICT. Individual, group and whole class pupil led presentations and discussions. Making with a range of materials. Some electronics and control. Teacher demonstrations using machines and practical multibenches. Traditional and computer based drawing and design.","Basic teaching","Heavy practical (workshop)",3.5,4,"I1","SEN",25,3.9,null,1,69,10,11,1,13,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2700","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D2.1av","strong","D2.1av","strong",null,"Doorset, including ironmongery, finger guards and access control system to be agreed with school","F5.4","heavy practical","C1.1","general","W4.1","rough","Flooring suitable for heavy movable FF&E on castors. Concrete or ceramic tiles floor required around any heat treatment equipment","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation based on Tech Annex 2F 7.5, 7.6 and 7.8. *Acoustics: see BB93 0.4","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",4,2,16]
["DAT96","Construction workshops (ambulant)","Construction workshops (ambulant)","DAT96","DAT49","New Build","SL_25_40_15","Construction workshops","Secondary workshop for vocational construction courses for ambulant pupils needing additional support ","Construction skills including painting and decorating; plumbing and carpentry. Teacher demonstrations using machines and practical multibenches.","Basic teaching","Heavy practical (workshop)",3.5,4,"J1","SEN",32,4.4000000000000004,null,1,69,7,7,1,8,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2700","7800 / 7500","Double doors",1050,"Contractor to Specify for approval","D2.1av","strong","D2.1av","strong",null,"Doorset, including ironmongery, finger guards and access control system to be agreed with school","F5.4","heavy practical","C1.1","general","W4.1","rough","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation based on Tech Annex 2F 7.5, 7.6 and 7.8. *Acoustics: see BB93 0.4","Bottled gas only","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",4,2,16]
["DAT97","Vehicle workshops","Vehicle workshops (ambulant)","DAT97","DAT97","New Build","SL_25_40_94","Vehicle workshops","Secondary workshop for vocational vehicle maintenance courses","Vehicle maintenance skills including engineering and bodywork. Teacher demonstrations using machines, vehicles and vehicle parts and practical multibenches.","Basic teaching","Heavy practical (workshop)",3.5,4,"J1","SEN",32,4.4000000000000004,null,1,69,7,7,1,8,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2700","7800 / 7500","Garage doors",1050,"Contractor to Specify for approval","D2.1av","strong","D2.1av","strong",null,"Doorset, including ironmongery, finger guards and access control system to be agreed with school","F5.4","heavy practical","C1.1","general","W4.1","rough","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation based on Tech Annex 2F 7.5, 7.6 and 7.8. *Acoustics: see BB93 0.4","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",4,2,16]
[0,"-","-",0,null,null,null,"-",null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,"Contractor to Specify for approval"]
["DIN01","Dining halls","Dining halls","DIN01","DIN01","New Build","SL_40_20_22","Dining halls","Large space permanently set out for dining","Dining for hot and cold meals from servery area(s) within space or adjacent. Can also be used for school events such as parents meetings/presentations, teacher consultations or whole school teacher meetings. ","Halls and dining","Large",12.5,-20,null,"-",3,0.95,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","Optional ","Disabled access required to all areas except some  seating","Enclosed, semi-enclosed or open plan","adjacent to school kitchen suite","3300 / 2700","2700 / 2400","10650 / 3400","Optional","CTS","Contractor to Specify for approval if provided","DD1.1av","general double ","DD1.1av","general double ",null,"Plain meeting stiles","F4.2h","dining","C1.1","general","W2.1h","science",null,"L2.6h","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",200,"key on, day dim, abs off","If fire exit",null,"T5","High","High","<=1.0","<=1.5","Ventilation as Tech Annex 2F 6.4.4","None","Where required","Drinking water outlet",8,6,12]
["DIN02","Informal dining spaces","Informal dining spaces","DIN02","DIN02","New Build","SL_40_20_43","Informal dining spaces","Open area for pupils to socialise and eat snacks and sandwiches in secondary schools","Socialising and dining of drinks and cold meals, typically from local servery area(s) within space or adjacent. Can also be used for school events such as parents meetings/presentations, teacher consultations or whole school teacher meetings. ","Halls and dining","General",1.5,4,"A","-",2,1.1000000000000001,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access into the space required","Enclosed, semi-enclosed or open plan",null,"3300 / 2700","2700 / 2400","7800 / 3400","Optional","CTS","Contractor to Specify for approval if provided","DD1.1av","general double ","DD1.1av","general double ",null,null,"F4.2h","dining","C1.1","general","W2.1h","science",null,"L2.6h","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",200,"key on, day dim, abs off","If fire exit",null,"T5","High","High","<=1.0","<=1.5","Ventilation as Tech Annex 2F 6.4.4","None","Where required","Optional for vending",5,2,8]
["DIN04","Social spaces","Social spaces","DIN04","DIN04","New Build","SL_90_20_80","Social spaces","Open area for pupils to socialise but not to eat","Social area for specific group, typically sixth form pupils. Some study areas with use of ICT. Can also be used for school events such as parents meetings/presentations, teacher consultations or whole school teacher meetings. ","Halls and dining","General",1.5,4,"A","-",2,1.1000000000000001,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access into the space required","Enclosed, semi-enclosed or open plan",null,"3300 / 2700","2700 / 2400","7800 / 3400","Optional","CTS","Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,null,"F1.1h","special general","C1.1","general","W1.1h","general"," ","L2.6h","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",200,"key on, day dim, abs off","If fire exit",null,"T5","Average","Medium","<=0.8","<=1.0",null,"None","Where required","Optional for vending",5,2,6]
["DIN05","Social spaces (sixth form)","Social spaces (sixth form)","DIN05","DIN04","New Build","SL_90_20_80","Social spaces","Specialist 'common room' for post-16 pupils to socialise, discuss and study in an informal setting","Social area for sixth form pupils. Some study areas with use of ICT. Can also be used for school events such as parents meetings/presentations, teacher consultations or whole school teacher meetings. ","Halls and dining","General",1.5,4,"A","-",2,1.1000000000000001,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access into the space required","Enclosed, semi-enclosed or open plan",null,"3300 / 2700","2700 / 2400","7800 / 3400","Optional","CTS","Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,null,"F1.1h","special general","C1.1","general","W1.1h","general",null,"L2.6h","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",200,"key on, day dim, abs off","If fire exit",null,"T5","Average","Medium","<=0.8","<=1.0",null,"None","Where required","Optional for vending",5,4,16]
["DIN11","Servery areas, meal collection","Servery areas, meal collection","DIN11","DIN11","New Build","SL_35_60_78","Servery areas","Area in front of school kitchen servery for collection of food and payment","Serving and collection of food and payment","Halls and dining","General",1.5,4,"A","-",2,1.1000000000000001,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access into the space required","Semi-enclosed or open plan",null,"2700 / 2400 (3300 / 2700 if >27m2)","2700 / 2400","N/A / 1700","Not required","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F4.2h","dining","C1.1","general","W2.1h","science",null,"L2.6h","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",200,"key on, day dim, abs off","If fire exit",null,"T5","High","High","<=1.0","<=1.5",null,"None","Where required","To suit equipment",0,2,2]
["DIN12","Servery areas, satellite","Servery areas, satellite","DIN12","DIN12","New Build","SL_35_60_78","Servery areas","Separate servery area for snacks, drink and/ or cold foods prepared in main kitchen","Serving and collection of food and payment","Halls and dining","General",1.5,4,"A","-",2,1.1000000000000001,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access into the space required","Semi-enclosed or open plan",null,"2700 / 2400 (3300 / 2700 if >27m2)","2700 / 2400","N/A / 1700","Not required","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F4.2h","dining","C1.1","general","W2.1h","science",null,"L2.6h","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",200,"key on, day dim, abs off","If fire exit",null,"T5","High","High","<=1.0","<=1.5",null,"None","Where required","To suit equipment",2,2,2]
["DIN50","Dining halls (ambulant)","Dining halls (ambulant)","DIN50","DIN01","New Build","SL_40_20_22","Dining halls","Space primarily for dining, also meetings and drama, for ambulant pupils","Dining for hot and cold meals from servery area(s) within space or adjacent. Can also be used for school events such as parents meetings/presentations, teacher consultations or whole school teacher meetings. ","Halls and dining","Large",12.5,-20,null,"SEN",5,1.2,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","Optional ","Disabled access into the space required","Enclosed, semi-enclosed or open plan","adjacent to school kitchen suite","3300 / 2700","2700 / 2400","10200 / 3400","Optional","CTS","Contractor to Specify for approval if provided","DD1.1av","general double ","DD1.1av","general double ",null,"Plain meeting stiles. Doorset, including ironmongery, finger guards and access control system to be agreed with school","F4.2h","dining","C1.1","general","W2.1h","science",null,"L2.6h","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",200,"key on, day dim, abs off","If fire exit",null,"T5","Average","Medium","<=1.0","<=1.5","Ventilation as Tech Annex 2F Section 7.8 Table 7-4","None","Where required","Drinking water outlet",0,2,2]
["DIN55","Dining halls, non-ambulant","dining area (non-ambulant)","DIN55","DIN55","New Build","SL_40_20_22","Dining halls","Space primarily for dining, also meetings and drama, for ambulant and non-ambulant pupils","Dining for hot and cold meals from servery area(s) within space or adjacent. Can also be used for school events such as parents meetings/presentations, teacher consultations or whole school teacher meetings. ","Halls and dining","Large",12.5,-20,"J","SEN",28,4.2,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","Optional ","Full disabled access required","Enclosed, semi-enclosed or open plan","adjacent to school kitchen suite","3300 / 2700","2700 / 2400","7800 / 3400","Optional","CTS","Contractor to Specify for approval if provided","DD1.1av","general double ","DD1.1av","general double ",null,"Plain meeting stiles. Doorset, including ergonomic handle, ironmongery, finger guards and access control system to be agreed with school","F4.2h","dining","C1.1","general","W2.1h","science",null,"L2.6h","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",200,"key on, day dim, abs off","If fire exit",null,"T5/T7","Average","Medium","<=1.0","<=1.5","Ventilation as Tech Annex 2F Section 7.8 Table 7-4","None","Where required","Drinking water outlet",0,2,2]
["DIN60","Informal dining spaces (ambulant)","Informal dining spaces (ambulant)","DIN60","DIN60","New Build","SL_40_20_43","Informal dining spaces","Open area for ambulant pupils to socialise and eat snacks and sandwiches","Socialising and dining of drinks and cold meals, typically from local servery area(s) within space or adjacent. Can also be used for school events such as parents meetings/presentations, teacher consultations or whole school teacher meetings. ","Halls and dining","General",1.5,4,"G","SEN",10,2.9,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access into the space required","Enclosed, semi-enclosed or open plan",null,"3300 / 2700","2700 / 2400","7800 / 3400","Optional","CTS","Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,"Doorset, including ironmongery, finger guards and access control system to be agreed with school","F4.2h","dining","C1.1","general","W2.1h","science",null,"L2.6h","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",200,"key on, day dim, abs off","If fire exit",null,"T5","Average","Medium","<=1.0","<=1.5","Ventilation as Tech Annex 2F Section 7.8 Table 7-4","None","Where required","Optional for vending",0,2,8]
["DIN63","Informal dining spaces (independent living)",null,null,"DIN60","New Build","SL_40_20_43","Informal dining spaces","Space primarily for dining, but also for learning cooking and washing in a domestic environment, for ambulant pupils","Dining of drinks and cold meals. Pupil practice in life skills including cleaning ","Halls and dining","General",1.5,4,"G","SEN",10,2.9,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access into the space required","Enclosed, semi-enclosed or open plan",null,"3300 / 2700","2700 / 2400","7800 / 3400","Optional","CTS","Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,"Doorset, including ironmongery, finger guards and access control system to be agreed with school","F4.2h","dining","C1.1","general","W2.1h","science",null,"L2.6h","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",200,"key on, day dim, abs off","If fire exit",null,"T5","Average","Medium","<=1.0","<=1.5","Ventilation as Tech Annex 2F Section 7.8 Table 7-4","None","To suit equipment","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",2,0,16,"Need to be able to clean surfaces thoroughly to maintain hygiene"]
["DIN65","Informal dining spaces, non-ambulant","social and sandwich area (non-ambulant)","DIN65","DIN65","New Build","SL_40_20_43","Informal dining spaces","Open area for non-ambulant pupils to socialise and eat snacks and sandwiches","Socialising and dining of drinks and cold meals, typically from local servery area(s) within space or adjacent. Can also be used for school events such as parents meetings/presentations, teacher consultations or whole school teacher meetings. ","Halls and dining","General",1.5,4,"J","SEN",28,4.2,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Full disabled access required","Enclosed, semi-enclosed or open plan",null,"3300 / 2700","2700 / 2400","7800 / 3400","Optional","CTS","Contractor to Specify for approval if provided","D6.1mv","special wide","D6.1mv","special wide",null,"Doorset, including ergonomic handle, ironmongery and access control system to be agreed with school","F4.2h","dining","C1.1","general","W2.1h","science",null,"L2.6h","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",200,"key on, day dim, abs off","If fire exit",null,"T5/T7","Average","Medium","<=1.0","<=1.5","Ventilation as Tech Annex 2F Section 7.8 Table 7-4","None","Where required","Optional dispenser",0,2,8]
["DIN70","Social spaces (ambulant)","Social spaces (ambulant)","DIN70","DIN04","New Build","SL_90_20_80","Social spaces","Open area for pupils to socialise and play games, for ambulant pupils","Social area. Some study areas with use of ICT. Can also be used for cold food dining, school events such as meetings/presentations. ","Halls and dining","General",1.5,4,"G","SEN",10,2.9,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access into the space required","Enclosed, semi-enclosed or open plan",null,"3300 / 2700","2700 / 2400","7800 / 3400","Optional","CTS","Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,"Doorset, including ironmongery, finger guards and access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1h","general",null,"L2.6h","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",200,"key on, day dim, abs off","If fire exit",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F Section 7.8 Table 7-4","None","Where required","Optional for vending",0,2,12]
["DIN75","Social spaces, non-ambulant","social space (non-ambulant)","DIN75","DIN75","New Build","SL_90_20_80","Social spaces","Open area for pupils to socialise and play games, for ambulant and non-ambulant pupils","Social area. Some study areas with use of ICT. Can also be used for cold food dining, school events such as meetings/presentations. ","Halls and dining","General",1.5,4,"J","SEN",28,4.2,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Full disabled access required","Enclosed, semi-enclosed or open plan",null,"3300 / 2700","2700 / 2400","7800 / 3400","Optional","CTS","Contractor to Specify for approval if provided","D6.1mv","special wide","N/A","no internal doorset required",null,"Ergonomic handle, and access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1h","science",null,"L2.6h","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",200,"key on, day dim, abs off","If fire exit",null,"T5/T7","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F Section 7.8 Table 7-4","None","Where required","Optional dispenser",0,2,12]
["DIN80","Social spaces (ambulant sixth form)","social space (sixth form ambulant)","DIN80","DIN04","New Build","SL_90_20_80","Social spaces","Specialist 'common room' for post-16 pupils to socialise, discuss, study, and possibly eat, in an informal setting, for ambulant pupils","Social area for sixth form pupils. Some study areas with use of ICT. Can also be used for cold food dining, school events such as meetings/presentations. ","Halls and dining","General",1.5,4,"G","SEN",10,2.9,null,0,"As SoA","As SoA","As SoA",0,"As SoA","16-19","None","Disabled access into the space required","Enclosed, semi-enclosed or open plan",null,"3300 / 2700","2700 / 2400","7800 / 3400","Optional","CTS","Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,"Doorset, including ironmongery, finger guards and access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1h","general",null,"L2.6h","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",200,"key on, day dim, abs off","If fire exit",null,"T5","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F Section 7.8 Table 7-4","None","Where required","Optional for vending",10,2,12]
["DIN85","Social spaces, non-ambulant (sixth form)","social space (sixth form non-ambulant)","DIN85","DIN75","New Build","SL_90_20_80","Social spaces","Specialist 'common room' for post-16 pupils to socialise, discuss, study, and possibly eat, in an informal setting, for ambulant and non-ambulant pupils","Social area for sixth form pupils. Some study areas with use of ICT. Can also be used for cold food dining, school events such as meetings/presentations. ","Halls and dining","General",1.5,4,"J","SEN",28,4.2,null,0,"As SoA","As SoA","As SoA",0,"As SoA","16-19","None","Full disabled access required","Enclosed, semi-enclosed or open plan",null,"3300 / 2700","2700 / 2400","7800 / 3400","Optional","CTS","Contractor to Specify for approval if provided","D6.1mv","special wide","N/A","no internal doorset required",null,"Doorset, including ergonomic handle, ironmongery, finger guards and access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1h","general",null,"L2.6h","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",200,"key on, day dim, abs off","If fire exit",null,"T5/T7","Average","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F Section 7.8 Table 7-4","None","Where required","Optional dispenser",10,2,12]
["HAL02","Assembly halls, secondary (including stage)","Assembly halls, secondary (including stage)","HAL02","HAL01","New Build","SL_25_10_05","Assembly halls","Multi-purpose hall for assembly, PE and exams and cold food dining, in secondary schools, including stage area","School assemblies (various sizes) using PA system and whiteboard. Dining of cold food from nearby dining area. Music and drama rehearsals and performance. Parent evenings. Some gymnastic practise and performance, table tennis and recreational trampolining if 6.9m high. Whole year group examinations.","Halls and dining","Large",12.5,-20,null,"-",45,0.6,null,0,"As SoA","As SoA","As SoA",0,"As SoA","11-19","Yes","Disabled access required to all areas except some seating","Enclosed",null,"6900 / 6900 (5000 if <180m2)","as existing","12450 / 12000","Optional","CTS","Contractor to Specify for approval if provided","DD1.1hv","general double ","DD1.1hv","general double ",null,"Plain meeting stiles","F6.2h","multi-purpose hall","C1.1","general","W2.1h","science",null,"L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","Yes","Dimming for stage lighting required","T2/T5","High","Low","0.8 - 1.2","0.8 - 1.5","Ventilation as Tech Annex 2F 6.4.2","None","To suit equipment","None",14,4,12,"Fire escape should be planned based on maximum capacity being achieved when movable bleacher seating is fully extended."]
["HAL03","Assembly halls, secondary (with bleachers)","Assembly halls, secondary (with bleachers)","HAL03","HAL01","New Build","SL_25_10_05","Assembly halls","Multi-purpose hall for assembly, PE and exams and cold food dining, in secondary schools, served by adjacent bleacher seating","School assemblies (various sizes) using PA system and whiteboard. Dining of cold food from nearby dining area. Music and drama rehearsals and performance. Parent evenings. Some gymnastic practise and performance, table tennis and recreational trampolining if 6.9m high. Whole year group examinations.","Halls and dining","Large",12.5,-20,null,"-",25,0.55000000000000004,null,0,"As SoA","As SoA","As SoA",0,"As SoA","11-19","Yes","Disabled access required to all areas except some seating","Enclosed","adjacent to Retractable seating storage","6900 / 6900 (5000 if <180m2)","as existing","12450 / 12000","Optional","CTS","Contractor to Specify for approval if provided","DD1.1hv","general double ","DD1.1hv","general double ",null,"Plain meeting stiles","F6.2h","multi-purpose hall","C1.1","general","W2.1h","science","Suitable for retractable bleacher seating to cover approximately half of the floor area","L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","Yes","Dimming for stage lighting required","T2/T5","High","Low","0.8 - 1.2","0.8 - 1.5","Ventilation as Tech Annex 2F 6.4.2","None","To suit equipment","None",14,4,12,"Fire escape should be planned based on maximum capacity being achieved when movable bleacher seating is fully extended."]
["HAL12","Activity studios (small hall)","Activity studios (small hall)","HAL12","ACT05","New Build","SL_25_10_01","Activity studios","Primary school space for music, movement, dance, gymnastics and exams, but not dining","Dance. Gymnastics. Occasional use for exams and exhibitions. Table tennis. Trampolining. Exhibitions.  Music and drama rehearsal and performance. Parent evenings. Presentations. Assessment.","Halls and dining","Large",12.5,-20,"A","-",2,1.1000000000000001,null,0,85,60,75,0,"As SoA","4-11","Optional ","Disabled access into the space required","Enclosed",null,"5000 / 5000 (6900 if >180m2)","as existing","10650 / 7500 ","Optional","CTS","Contractor to Specify for approval if provided","DD1.1kv","general double ","N/A","no internal doorset required",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards in Primary","F6.1","multi-purpose sport","C1.1","general","W1.1h","general","Flooring suitable for heavy movable FF&E on castors ","L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","if community use",null,"T2/T5","High","Low","0.8 - 1.2","0.8 - 1.5",null,"None","Where required","None",13,2,16,"No projections, including opening doors, to avoid injury during activity."]
["HAL13","Assembly halls, primary","Assembly halls, primary","HAL13","HAL13","New Build","SL_25_10_05","Assembly halls","Multi-purpose hall for assembly, PE, exams and dining in primary schools","Assemblies. Assessment. Dining of hot and cold food from adjacent servery area(s). Exhibitions. Gymnastics. Music and drama rehearsal and performance. Parent evenings. Presentations.","Halls and dining","Large",12.5,-20,null,"-",15,0.5,null,0,"As SoA","As SoA","As SoA",0,"As SoA","4-11","Yes","Disabled access required to all areas except some seating","Enclosed",null,"5000 / 5000 (6900 if >180m2)","as existing","10650 / 10000","Optional","CTS","Contractor to Specify for approval if provided","DD1.1hv","general double ","DD1.1hv","general double ",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards required","F6.2h","multi-purpose hall","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","Yes","Dimming for stage lighting required","T2/T5","High","Low","0.8 - 1.2","0.8 - 1.5","Ventilation as Tech Annex 2F 6.4.2","None","Where required","None",12,4,16,"No projections, including opening doors, to avoid injury during activity."]
["HAL21","Assembly halls, existing","Assembly halls, existing","HAL21","HAL21","Existing","SL_25_10_05","Assembly halls","Multi-purpose hall for assembly, PE and exams and cold food dining","Assemblies. Assessment. Dining of hot and cold food from adjacent servery area(s). Exhibitions. Gymnastics. Music and drama rehearsal and performance. Parent evenings. Presentations. Recreational trampolining if over 6.7m high","Halls and dining","Large",12.5,-20,null,"-",25,0.55000000000000004,null,0,"As SoA","As SoA","As SoA",0,"As SoA","4-11","Yes","Disabled access required to all areas except some seating","Enclosed",null,"5000 / 5000 (6900 if >180m2)","as existing","as existing","As existing","CTS","Contractor to Specify for approval","DD1.1hv","general double ","DD1.1hv","general double ",null,"As existing","F6.2h","multi-purpose hall","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","Yes","Dimming for stage lighting required","T2/T5","High","Low","0.8 - 1.2","0.8 - 1.5","Ventilation as Tech Annex 2F 6.4.2","None","Where required","None",14,4,16]
["HAL22","Lecture theatres, existing","Lecture theatres, existing","HAL22","HAL22","Existing","SL_25_10_47","Lecture theatres","Existing space designed for lectures","Lectures, demonstrations and meetings.","Halls and dining","Large",12.5,-20,"B","-",2,1.6,null,0,"As SoA","As SoA","As SoA",0,"As SoA","11-19","None ","Disabled access into the space required","Enclosed",null,"CTS","as existing","CTS","As existing","CTS","Contractor to Specify for approval","DD1.1hv","general double ","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1h","general",null,"L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","Yes",null,"T5","Average","Medium","<=0.8 or <=1.0","<=1.0",null,"None","Where required","None",9,2,12]
["HAL50","Assembly halls, ambulant","Assembly halls, ambulant","HAL50","HAL50","New Build","SL_25_10_05","Assembly halls","Multi-purpose primary/secondary hall for assembly, PE, and dining (and possibly music and movement) for ambulant pupils","Assemblies. Assessment (examinations). Dining of hot and cold food. Exhibitions. Gymnastics. Team games. Movement. Recreational trampolining if 6.9m high. Music and drama rehearsal and performance. Parent evenings. Presentations.","Halls and dining","Large",12.5,-20,null,"SEN",12,1.2,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","Yes","Disabled access into the space required","Enclosed",null,"5000 / 5000 (6900 if >180m2)","as existing","10200 / 10000","Optional","CTS","Contractor to Specify for approval if provided","DD1.1hv","general double ","DD1.1hv","general double ",null,"Plain meeting stiles. Doorset, including ironmongery, finger guards and access control system to be agreed with school","F6.2h","multi-purpose hall","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","Yes","Dimming for stage lighting required","T5","High","Low","0.8 - 1.2","0.8 - 1.5","Ventilation as Tech Annex 2F Section 7.8 Table 7-4","None","Where required","None",4,2,12]
["HAL55","Assembly halls, non-ambulant","Assembly halls, non-ambulant","HAL55","HAL55","New Build","SL_25_10_05","Assembly halls","Multi-purpose primary/secondary hall for assembly, PE, and dining (and possibly music and movement) for ambulant and non-ambulant pupils","Assemblies. Assessment (examinations). Dining of hot and cold food. Exhibitions. Gymnastics. Team games. Movement. Rebound therapy. Recreational trampolining if 6.9m high. Music and drama rehearsal and performance. Parent evenings. Presentations.","Halls and dining","Large",12.5,-20,null,"SEN",20,2.4,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","Yes","Full disabled access required","Enclosed",null,"5000 / 5000 (6900 if >180m2)","as existing","10200 / 10000","Optional","CTS","Contractor to Specify for approval if provided","DD6.1hv","special double ","DD1.1hv","general double ",null,"Plain meeting stiles. Doorset, including ergonomic handle, ironmongery, finger guards and access control system to be agreed with school","F6.2h","multi-purpose hall","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","Yes","Dimming for stage lighting required","T5/T7","High","Low","0.8 - 1.2","0.8 - 1.5","Ventilation as Tech Annex 2F Section 7.8 Table 7-4","None","Where required","None",4,2,12]
["KIT00","Food prep areas, kitchen","Food prep areas, kitchen","KIT00","KIT00","New Build","SL_35_60_30","Food preparation areas","Preparation, servery, wash-up and COSHH area of commercial kitchen for preparing and serving school meals","Preparing, cooking and serving hot and cold meals for pupils and staff, as well as dishwashing and cleaning, by commercial catering staff. Also to include an area for administrative tasks (including use of ICT) by commercial catering staff.","Non-net","Non-net",null,null,"J","-",28,4.2,null,0,"As SoA","As SoA","As SoA",0,"As SoA","N/A","None","Disabled and trolley access into the area required","Enclosed",null,"2700 / 2400","2400 / 2400","7800 / 7000","Required","CTS","Contractor to Specify for approval","D5.2av","strong, with vision panel","N/A","no internal doorset required",null,null,"F8.4h","kitchen","C1.2","humid areas","W3.2","humid"," ","L4.1m","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",500,"man on, abs off","Yes",null,"T4","High","High","<=1.5","<=2.0","Kitchen ventilation system as Tech Annex 2F 7.2","Gas supply to any gas ovens, hobs and other appliances","To suit equipment","Hot and cold drinking water to all sinks, equipment and appliances",4,2,10,"Fire Containment."]
["KIT01","Food prep areas, kitchen (servery & wash-up)","Food prep areas, kitchen (servery & wash-up)","KIT01","KIT00","New Build","SL_35_60_30","Food preparation areas","Preparation, servery, wash-up and COSHH area of commercial kitchen for preparing and serving school meals","Preparing, cooking and serving hot and cold meals for pupils and staff, as well as dishwashing and cleaning, by commercial catering staff. Also to include an area for administrative tasks (including use of ICT) by commercial catering staff.","Non-net","Non-net",null,null,"J","-",28,4.2,null,0,"As SoA","As SoA","As SoA",0,"As SoA","N/A","None","Disabled and trolley access into the area required","Enclosed",null,"2700 / 2400","2400 / 2400","7800 / 7000","Required","CTS","Contractor to Specify for approval","D5.2av","strong, with vision panel","N/A","no internal doorset required",null,null,"F8.4h","kitchen","C1.2","humid areas","W3.2","humid"," ","L4.1m","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",500,"man on, abs off","Yes",null,"T4","High","High","<=1.5","<=2.0","Kitchen ventilation system as Tech Annex 2F 7.2","Gas supply to any gas ovens, hobs and other appliances","To suit equipment","Hot and cold drinking water to all sinks, equipment and appliances",4,2,10,"Fire Containment."]
["KIT02","Food prep areas, kitchen (prep/ servery suite)","Food prep areas, kitchen (prep/ servery suite)","KIT02","KIT00","New Build","SL_35_60_30","Food preparation areas","Preparation, servery, wash-up, COSHH area, fridge, freezer and admin area of commercial kitchen for preparing and serving school meals","Preparing, cooking and serving hot and cold meals for pupils and staff, as well as dishwashing and cleaning, by commercial catering staff. ","Non-net","Non-net",null,null,"J","-",28,4.2,null,1,"As SoA","As SoA","As SoA",1,"As SoA","N/A","None","Disabled and trolley access into the area required","Semi-enclosed",null,"2700 / 2400","2400 / 2400","7800 / 7000","Required","CTS","Contractor to Specify for approval","D5.2av","strong, with vision panel","N/A","no internal doorset required",null,null,"F8.4h","kitchen","C1.2","humid areas","W3.2","humid"," ","L4.1m","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",500,"man on, abs off","Yes",null,"T4","High","High","<=1.5","<=2.0","Kitchen ventilation system as Tech Annex 2F 7.2","Gas supply to any gas ovens, hobs and other appliances","To suit equipment","Hot and cold drinking water to all sinks, equipment and appliances",4,null,10,"Fire Containment."]
["KIT11","Offices, kitchen ","Offices, kitchen ","KIT11","KIT11","New Build","SL_20_15_59","Offices","Chef's office or admin area within commercial kitchen for preparing and serving school meals","Administrative tasks (including use of ICT) and filing by commercial catering staff.","Non-net","Non-net",null,null,"A","-",2,1.1000000000000001,null,1,"As SoA","As SoA","As SoA",1,"As SoA","N/A","None","Disabled access into the area required","Enclosed or semi-enclosed",null,"2400 / N/A","2400 / 2400","N/A / CTS","Not required","N/A","","D2.2av","strong","N/A","no internal doorset required",null,null,"F3.4h","hygienic non-slip","C1.2","humid areas","W2.2h","humid areas and toilets"," ","L4.1m","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",500,"man on, abs off","If fire exit",null,"T4","Low","Medium","<=1.0","<=1.0",null,"None","Minimal","None",8,null,10,"CTS if Fire Containment."]
["KIT20","Food stores, kitchen","Food stores, kitchen","KIT20","KIT20","New Build","SL_90_50_29","Food stores","Commercial kitchen dry store for use by school catering staff, as part of school kitchen suite","Storing cold or dry foodstuffs for use by commercial catering staff, as part of school kitchen suite.","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,"As SoA","N/A","None","Disabled and trolley access into the area required","Enclosed","off kitchen Food prep area","2400 / N/A","2400 / 2400","N/A / CTS","Not required","N/A","","D4.2a","food store","N/A","no internal doorset required",null,null,"F3.4h","hygienic non-slip","C1.2","humid areas","W2.2h","humid areas and toilets"," ","L5.3l","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off, day off","No",null,"T1","N/A","N/A","N/A","N/A","Contractor to specify to suit best practice standards and guidance. ","None","Minimal","None",0,null,4]
["KIT21","Food stores, kitchen (dry)","Food stores, kitchen (dry)","KIT21","KIT20","New Build","SL_90_50_29","Food stores","Commercial kitchen dry store for use by school catering staff, as part of school kitchen suite","Storing cold or dry foodstuffs for use by commercial catering staff, as part of school kitchen suite.","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,"As SoA","N/A","None","Disabled and trolley access into the area required","Enclosed","off kitchen Food prep area","2400 / N/A","2400 / 2400","N/A / CTS","Not required","N/A","","D4.2a","food store","N/A","no internal doorset required",null,null,"F3.4h","hygienic non-slip","C1.2","humid areas","W2.2h","humid areas and toilets",null,"L5.3l","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off, day off","No",null,"T1","N/A","N/A","N/A","N/A","Contractor to specify to suit best practice standards and guidance. ","None","Minimal","None",0]
["KIT25","Cold stores, kitchen","Cold stores, kitchen","KIT25","KIT25","New Build","SL_90_50_15","Cold stores","Commercial kitchen cold store for use by school catering staff, as part of school kitchen suite","Storing refrigerated cold foodstuffs for use by commercial catering staff, as part of school kitchen suite.","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,"As SoA","N/A","None","Disabled and trolley access into the area required","Enclosed","off kitchen Food prep area","2400 / N/A","2400 / 2400","N/A / CTS","Not required","N/A","","CTS","Contractor to specify for approval","N/A","no internal doorset required",null,"Door to be designed to suit refrigerated facility as specified by the Contractor","CTS","Contractor to specify for approval","CTS","Contractor to specify for approval","CTS","Contractor to specify for approval","Contractor to specify to suit best practice standards and guidance ","L5.3l","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off, day off","No","Contractor to specify to suit best practice standards and guidance","CTS","N/A","N/A","N/A","N/A","Contractor to specify to suit best practice standards and guidance. ","Contractor to Specify for approval","CTS","None",0]
["KIT26","Cold stores, kitchen (freezer)","Cold stores, kitchen (freezer)","KIT26","KIT25","New Build","SL_90_50_15","Cold stores","Commercial kitchen freezer store for use by school catering staff, as part of school kitchen suite","Storing frozen foodstuffs for use by commercial catering staff, as part of school kitchen suite.","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,"As SoA","N/A","None","Disabled and trolley access into the area required","Enclosed","off kitchen Food prep area","2400 / N/A","2400 / 2400","N/A / CTS","Not required","N/A","","CTS","Contractor to specify for approval","N/A","no internal doorset required",null,"Door to be designed to suit refrigerated facility as specified by the Contractor","CTS","Contractor to specify for approval","CTS","Contractor to specify for approval","CTS","Contractor to specify for approval","Contractor to specify to suit best practice standards and guidance ","L5.3l","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off","No","Contractor to specify to suit best practice standards and guidance","CTS","N/A","N/A","N/A","N/A","Contractor to specify to suit best practice standards and guidance. ","Contractor to Specify for approval","CTS","None",0,null,8]
["KIT40","Toilets, kitchen (with changing area)","Toilets, kitchen (with changing area)","KIT40","KIT40","New Build","SL_35_80_89","Toilets","Toilet(s) for use by school catering staff, accessed from space for kitchen staff lockers and changing ","Toilet(s), wash hand basin and changing area for commercial catering staff, as part of school kitchen suite. Storage of personal belongings and clothing.","Non-net","Non-net",null,null,"T","-",0.5,3,null,0,"As SoA","As SoA","As SoA",0,"As SoA","N/A","None","Disabled and trolley access into the area required","Enclosed",null,"2400 / N/A","2200 / N/A","N/A / CTS","Not required","N/A","","D3.2b","toilets","N/A","no internal doorset required",null,"Additional indicator bolt required","F7.3h","wet area","C2.2","humid areas","W2.2h","humid areas and toilets",null,"L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off","No",null,"T3","Average","High","<=1.5","<=2.0","A locally controlled extract system shall be provided as specified in Tech Annex 2F 4.3.7 and 6.3","None","Hand dryers","Hot and cold water to all sinks listed under FF&E, cold water to other sinks or equipment",0,null,4]
["LIB01","School libraries (primary)","School libraries (primary)","LIB01","LIB01","New Build","SL_25_75_76","School libraries","Primary school library for all pupils","Discussion. Individual study (including use of ICT). Informal reading and use of reference resources. Reading. Storage of books and other printed material. Whole class presentations.","Learning resources","General",1.5,4,"B","-",2,1.6,null,0,"As SoA","As SoA","As SoA",0,"As SoA","4-11","None","Disabled access into the space required","Enclosed or semi-enclosed",null,"2700 / 2400 (3300 / 2700 if >27m2)","2400 / N/A","7800 / 2700","Optional","CTS","Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,null,"F1.1","general","C1.1","general","W1.1","general"," ","L2.1a","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=0.6","<=0.8",null,"None","Where required","None",15,2,32]
["LIB02","School libraries (infant)","School libraries (infant)","LIB02","LIB01","New Build","SL_25_75_76","School libraries","Primary school library for infant pupils","Discussion. Individual study (including use of ICT). Informal reading and use of reference resources. Reading. Storage of books and other printed material. Whole class presentations.","Learning resources","General",1.5,4,"B","-",2,1.6,null,0,"As SoA","As SoA","As SoA",0,"As SoA","4-7","None","Disabled access into the space required","Enclosed or semi-enclosed",null,"2700 / 2400 (3300 / 2700 if >27m2)","2400 / N/A","7800 / 2700","Optional","CTS","Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L2.1a","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=0.6","<=0.8",null,"None","Where required","None",15,2,32]
["LIB03","School libraries (junior)","School libraries (junior)","LIB03","LIB01","New Build","SL_25_75_76","School libraries","Primary school library for junior pupils","Discussion. Individual study (including use of ICT). Informal reading and use of reference resources. Reading. Storage of books and other printed material. Whole class presentations.","Learning resources","General",1.5,4,"B","-",2,1.6,null,0,"As SoA","As SoA","As SoA",0,"As SoA","7-11","None","Disabled access into the space required","Enclosed or semi-enclosed",null,"2700 / 2400 (3300 / 2700 if >27m2)","2400 / N/A","7800 / 2700","Optional","CTS","Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L2.1a","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=0.6","<=0.8",null,"None","Where required","None",15,2,48]
["LIB05","Library resource centres (LRC)","Library resource centres (LRC)","LIB05","LIB05","New Build","SL_25_75_45","Learning resource centres","Secondary school library and careers area","Individual study and research using books and ICT. Informal reading and use of reference resources. Lending books and PC resources. Whole class group for library skills.","Learning resources","Fitted",2,4,"F","-",8,2.5,null,1,"As SoA","As SoA","As SoA",1,"As SoA","11-19","None","Disabled access required to all areas except some seating","Enclosed or semi-enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Optional","CTS","Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,null,"F1.1","general","C1.1","general","W1.1","general"," ","L2.6d","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=1.0","<=1.2",null,"None","To suit ICT","None",28,2,39,"Specialist security barrier at all entrances and exits"]
["LIB06","Study spaces, rooms (sixth form)","Study spaces, rooms (sixth form)","LIB06","LIB07","New Build","SL_25_10_84","Study spaces","Secondary school study area for sixth form pupils","Individual study (including use of ICT). Reading and use of reference resources. ","Learning resources","General",1.5,4,"B","-",2,1.6,null,0,"As SoA","As SoA","As SoA",0,"As SoA","16-19","None","Disabled access into the space required","Enclosed or semi-enclosed",null,"3300 / 2700 (2700 / 2400 if <27m2)","2700 / 2400","7800 / 7000","Optional","CTS","Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,null,"F1.1","general","C1.1","general","W1.1","general"," ","L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, day dim, abs off","No",null,"T5","Low","Medium","<=0.8","<=1.0",null,"None","Dado on 2 walls","None",26,2,18]
["LIB07","Study spaces, rooms","Study spaces, rooms","LIB07","LIB07","New Build","SL_25_10_84","Study spaces","Secondary school study area for pupils","Individual study (including use of ICT). Reading and use of reference resources. ","Learning resources","General",1.5,4,"B","-",2,1.6,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access into the space required","Enclosed or semi-enclosed",null,"3300 / 2700 (2700 / 2400 if <27m2)","2700 / 2400","7800 / 7000","Optional","CTS","Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, day dim, abs off","No",null,"T5","Low","Medium","<=0.8","<=1.0",null,"None","Dado on 2 walls","None",26,2,8]
["LIB50","School libraries (ambulant)","School libraries, ambulant","LIB50","LIB50","New Build","SL_25_75_76","School libraries","Library for ambulant pupils of any age","Individual study and research using books and ICT. Informal reading and use of reference resources. Lending books and PC resources. Whole class group for library skills.","Learning resources","General",1.5,4,"D","SEN",5,1.9,null,0,"As SoA","As SoA","As SoA",0,"As SoA","5-19","None","Disabled access into the space required","Semi-enclosed or open plan",null,"2700 / 2400 (3300 / 2700 if >27m2)","2400 / N/A","7800 / 2700","Optional","CTS","Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,"Access control system and finger guards to be agreed with school","F1.1h","special general","C1.1","general","W1.1","general",null,"L2.1d","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Where required","None",22,2,32]
["LIB51","School libraries (ambulant, primary)","School libraries (ambulant, primary)","LIB51","LIB50","New Build","SL_25_75_76","School libraries","Library for ambulant pupils of primary age","Discussion. Individual study (including use of ICT). Informal reading and use of reference resources. Reading. Storage of books and other printed material. Whole class presentations.","Learning resources","General",1.5,4,"C","SEN",4,1.7,null,0,"As SoA","As SoA","As SoA",0,"As SoA","4-11","None","Disabled access into the space required","Semi-enclosed or open plan",null,"2700 / 2400 (3300 / 2700 if >27m2)","2400 / N/A","7800 / 2700","Optional","CTS","Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,"Access control system to be agreed with school. Finger guards","F1.1h","special general","C1.1","general","W1.1","general",null,"L2.1d","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Where required","None",10,2,32]
["LIB52","School libraries (ambulant, secondary)","School libraries (ambulant, secondary)","LIB52","LIB50","New Build","SL_25_75_76","School libraries","Library for ambulant pupils of secondary age","Individual study and research using books and ICT. Informal reading and use of reference resources. Lending books and PC resources. Whole class group for library skills.","Learning resources","General",1.5,4,"D","SEN",5,1.9,null,0,"As SoA","As SoA","As SoA",0,"As SoA","11-19","None","Disabled access into the space required","Semi-enclosed or open plan",null,"2700 / 2400 (3300 / 2700 if >27m2)","2400 / N/A","7800 / 2700","Optional","CTS","Contractor to Specify for approval if provided","D1.1av","general","D1.1av","general",null,"Access control system to be agreed with school. Finger guards","F1.1h","special general","C1.1","general","W1.1","general",null,"L2.1d","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Where required","None",10,2,32]
["LIB55","School libraries, non-ambulant","School libraries, non-ambulant","LIB55","LIB55","New Build","SL_25_75_76","School libraries","Library for ambulant and non-ambulant pupils of any age","Individual study and research using books and ICT. Informal reading and use of reference resources. Lending books and PC resources. Whole class group for library skills.","Learning resources","General",1.5,4,"F","SEN",8,2.5,null,0,"As SoA","As SoA","As SoA",0,"As SoA","11-19","None","Full disabled access required","Semi-enclosed or open plan",null,"2700 / 2400 (3300 / 2700 if >27m2)","2400 / N/A","7800 / 2700","Optional","CTS","Contractor to Specify for approval if provided","D6.1mv","special wide","N/A","no internal doorset required",null,"Ergonomic handle, and access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1","general",null,"L2.1d","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"man on, abs off","No",null,"T5/T7","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit ICT","None",10,2,32]
["LIB56","School libraries, non-ambulant (primary)","School libraries, non-ambulant (primary)","LIB56","LIB55","New Build","SL_25_75_76","School libraries","Library for ambulant and non-ambulant pupils of primary age","Discussion. Individual study (including use of ICT). Informal reading and use of reference resources. Reading. Storage of books and other printed material. Whole class presentations.","Learning resources","General",1.5,4,"F","SEN",8,2.5,null,0,"As SoA","As SoA","As SoA",0,"As SoA","4-11","None","Full disabled access required","Semi-enclosed or open plan",null,"2700 / 2400 (3300 / 2700 if >27m2)","2400 / N/A","7800 / 2700","Optional","CTS","Contractor to Specify for approval if provided","D6.1mv","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school. Finger guards","F1.1h","special general","C1.1","general","W1.1","general",null,"L2.1d","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"man on, abs off","No",null,"T5/T7","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit ICT","None",10,2,32]
["LIB57","School libraries, non-ambulant (secondary)","School libraries, non-ambulant (secondary)","LIB57","LIB55","New Build","SL_25_75_76","School libraries","Library for ambulant and non-ambulant pupils of secondary age","Individual study and research using books and ICT. Informal reading and use of reference resources. Lending books and PC resources. Whole class group for library skills.","Learning resources","General",1.5,4,"F","SEN",8,2.5,null,0,"As SoA","As SoA","As SoA",0,"As SoA","11-19","None","Full disabled access required","Semi-enclosed or open plan",null,"2700 / 2400 (3300 / 2700 if >27m2)","2700 / 2400","7800 / 2700","Optional","CTS","Contractor to Specify for approval if provided","D6.1mv","special wide","N/A","no internal doorset required",null,"Ergonomic handle, and access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1","general",null,"L2.1d","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"man on, abs off","No",null,"T5/T7","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit ICT","None",10,2,32]
["OFF00","Offices","Offices","OFF00","OFF00","New Build","SL_20_15_59","Offices","Office for one or more members of staff with admin storage ","Administrative tasks (including use of ICT) and filing.","Staff and admin","General",1.5,4,"D","-",5,1.9,5,1.9,"As SoA","As SoA","As SoA","As SoA","As SoA","N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general"," ","L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","Dado on 2 walls","None",5,null,4]
["OFF01","Offices (1-person)","Offices (1-person)","OFF01","OFF00","New Build","SL_20_15_59","Offices","Office for one member of staff with admin storage ","Administrative tasks (including use of ICT) and filing.","Staff and admin","General",1.5,4,"D","-",5,1.9,5,1.9,7,1,1,1,2,"N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","Dado on 2 walls","None",5,null,4]
["OFF02","Offices (2-person)","Offices (2-person)","OFF02","OFF00","New Build","SL_20_15_59","Offices","Office for two members of staff with admin storage ","Administrative tasks (including use of ICT) and filing.","Staff and admin","General",1.5,4,"D","-",5,1.9,5,1.9,9,2,2,2,3,"N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","Dado on 2 walls","None",5,null,4]
["OFF03","Offices (3-person)","Offices (3-person)","OFF03","OFF00","New Build","SL_20_15_59","Offices","Office for three members of staff with admin storage ","Administrative tasks (including use of ICT) and filing.","Staff and admin","General",1.5,4,"D","-",5,1.9,5,1.9,11,3,3,3,4,"N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","Dado on 2 walls","None",5,null,8]
["OFF04","Offices (4-person)","Offices (4-person)","OFF04","OFF00","New Build","SL_20_15_59","Offices","Office for four members of staff with admin storage ","Administrative tasks (including use of ICT) and filing.","Staff and admin","General",1.5,4,"D","-",5,1.9,5,1.9,13,4,4,4,5,"N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","Dado on 2 walls","None",5,2,12]
["OFF06","Offices (exams)","Offices (exams)","OFF06","OFF00","New Build","SL_20_15_59","Offices","office for exams officer, with space for secure storage","Administrative tasks (including use of ICT) and confidential filing of secure documents.","Staff and admin","General",1.5,4,"D","-",5,1.9,5,1.9,9,2,2,2,3,"N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","Dado on 2 walls","None",5,null,16,"Means to keep sensitive documents securely"]
["OFF10","Offices (with meeting area)","Offices (with meeting area)","OFF10","OFF00","New Build","SL_20_15_59","Offices","Office for one or more members of staff, with space for meetings","Administrative tasks (including use of ICT). Small group meetings and interviews. ","Staff and admin","General",1.5,4,"C","-",4,1.7,4,4.25,"As SoA","As SoA","As SoA","As SoA","As SoA","N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general"," ","L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","Dado on 2 walls","None",5,null,12]
["OFF11","Offices (with meeting area, 1-person)","Offices (with meeting area, 1-person)","OFF11","OFF00","New Build","SL_20_15_59","Offices","Office for one member of staff, with space for meetings","Administrative tasks (including use of ICT). Small group meetings and interviews. ","Staff and admin","General",1.5,4,"C","-",4,1.7,4,4.25,9,3,3,1,4,"N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","Dado on 2 walls","None",5,null,12]
["OFF12","Offices (with meeting area, 2-person)","Offices (with meeting area, 2-person)","OFF12","OFF00","New Build","SL_20_15_59","Offices","Office for two members of staff, with space for meetings","Administrative tasks (including use of ICT). Small group meetings and interviews. ","Staff and admin","General",1.5,4,"C","-",4,1.7,4,4.25,11,4,4,2,5,"N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","Dado on 2 walls","None",5,2,16]
["OFF13","Offices (with meeting area, 3-person)","Offices (with meeting area, 3-person)","OFF13","OFF00","New Build","SL_20_15_59","Offices","Office for three members of staff, with space for meetings","Administrative tasks (including use of ICT). Small group meetings and interviews. ","Staff and admin","General",1.5,4,"C","-",4,1.7,4,4.25,16,7,7,3,8,"N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","Dado on 2 walls","None",5,2,20]
["OFF20","Offices (pastoral)","Offices (pastoral)","OFF20","OFF00","New Build","SL_20_15_59","Offices","Office for one or more staff, with space for informal meetings","Administrative tasks (including use of ICT) small informal meetings and interviews. Counselling.","Staff and admin","General",1.5,4,"C","-",4,1.7,4,4.25,"As SoA","As SoA","As SoA","As SoA","As SoA","N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general"," ","L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","Dado on 2 walls","None",5,null,12]
["OFF21","Offices (pastoral, 1-person)","Offices (pastoral, 1-person)","OFF21","OFF00","New Build","SL_20_15_59","Offices","Office for one member of staff, with space for informal meetings","Administrative tasks (including use of ICT) small informal meetings and interviews. Counselling.","Staff and admin","General",1.5,4,"C","-",4,1.7,4,4.25,11,4,4,2,5,"N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","Dado on 2 walls","None",5,2,12]
["OFF22","Offices (pastoral, 2-person)","Offices (pastoral, 2-person)","OFF22","OFF00","New Build","SL_20_15_59","Offices","Office for two staff, with space for informal meetings","Administrative tasks (including use of ICT) small informal meetings and interviews. Counselling.","Staff and admin","General",1.5,4,"C","-",4,1.7,4,4.25,13,5,5,2,6,"N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","Dado on 2 walls","None",5,2,8]
["OFF23","Offices (SENco, learning support)","Offices (SENco, learning support)","OFF23","OFF00","New Build","SL_20_15_59","Offices","Office for SENco and team, with space for informal meetings","Administrative tasks (including use of ICT) small informal meetings and interviews. Counselling.","Staff and admin","General",1.5,4,"C","-",4,1.7,4,4.25,11,4,4,2,5,"N/A","None","Full disabled access required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","Dado on 2 walls","None",5,2,12]
["OFF24","Offices (visiting professionals)","Offices (visiting professionals)","OFF24","OFF00","New Build","SL_20_15_59","Offices","Office for visiting professionals and team, with space for informal meetings","Administrative tasks (including use of ICT) small informal meetings and interviews. Counselling.","Staff and admin","General",1.5,4,"C","SEN",4,1.7,4,4.25,"As SoA","As SoA","As SoA","As SoA","As SoA","N/A","None","Full disabled access required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","Dado on 2 walls","None",2,null,8]
["OFF32","Staff workrooms (smaller teaching team)","Staff workrooms (smaller teaching team)","OFF32","OFF30","New Build","SL_90_20_86","Staff workrooms","Space for staff for desk-based work and informal meetings or office/workroom, with space for repair of equipment","Lesson preparation and research mainly using ICT with a hot desk arrangement. Marking and recording pupils work. Storage of some of staff's personal and teaching resources. Team meeting and discussions.","Staff and admin","General",1.5,4,"D","-",5,1.9,5,1.9,"As SoA","As SoA","As SoA","As SoA","As SoA","N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","7800 / 3400","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general"," ","L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","To suit ICT","None",9,2,24]
["OFF33","Staff workrooms (teaching staff)","Staff workrooms (teaching staff)","OFF33","OFF30","New Build","SL_90_20_86","Staff workrooms","Space for staff for desk-based work and informal meetings or office/workroom, with space for repair of equipment","Lesson preparation and research mainly using ICT with a hot desk arrangement. Marking and recording pupils work. Storage of some of staff's personal and teaching resources. Team meeting and discussions.","Staff and admin","General",1.5,4,"D","-",5,1.9,5,1.9,"As SoA","As SoA","As SoA","As SoA","As SoA","N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","7800 / 3400","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general"," ","L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","To suit ICT","None",9,2,24]
["OFF34","Staff workrooms (specially resourced)","Staff workrooms (specially resourced)","OFF34","OFF30","New Build","SL_90_20_86","Staff workrooms","Space for staff in a school or a suite for desk-based work and informal meetings","Lesson preparation and research mainly using ICT with a hot desk arrangement. Marking and recording pupils work. Storage of some of staff's personal and teaching resources. Team meeting and discussions.","Staff and admin","General",1.5,4,"D","-",5,1.9,5,1.9,"As SoA","As SoA","As SoA","As SoA","As SoA","N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","To suit ICT","None",9,2,24]
["OFF36","Staff workrooms (technical support staff)","Staff workrooms (technical support staff)","OFF36","OFF30","New Build","SL_90_20_86","Staff workrooms","Office/workroom for one or more premises managers, caretakers or ICT technicians, with space for repair of equipment","Administrative tasks (including use of ICT). Basic maintenance and repair of equipment. Storing small tools and items of equipment. Storing manuals and small maintenance equipment.","Staff and admin","General",1.5,4,"E","-",6,2.1,6,2.1,11,2,2,2,3,"N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general"," ","L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","To suit ICT","None",9,2,24]
["OFF37","Staff workrooms (ICT technicians)","Staff workrooms (ICT technicians)","OFF37","OFF30","New Build","SL_90_20_86","Staff workrooms","Office/workroom for one or more ICT technicians, with space for repair of equipment","Administrative tasks (including use of ICT). Basic maintenance and repair of equipment. Storing small tools and items of equipment. Storing manuals and small maintenance equipment.","Staff and admin","General",1.5,4,"E","-",6,2.1,6,2.1,11,2,2,2,3,"N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","To suit ICT","None",9,2,24]
["OFF38","Staff workrooms (premises)","Staff workrooms (premises)","OFF38","OFF30","New Build","SL_90_20_86","Staff workrooms","Office/workroom for one or more premises managers, caretakers, with space for repair of equipment","Administrative tasks (including use of ICT). Basic maintenance and repair of equipment. Storing small tools and items of equipment. Storing manuals and small maintenance equipment.","Staff and admin","General",1.5,4,"E","-",6,2.1,6,2.1,11,2,2,2,3,"N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","To suit ICT","None",9,2,24]
["OFF40","Meeting rooms (conference)","Meeting rooms (conference)","OFF40","OFF40","New Build","SL_20_15_50","Meeting rooms","Conference or meeting room for meetings of staff, governors and other adults","Meeting room for staff with internal and external visitors etc. Privacy important. Small scale presentations using ICT.","Staff and admin","General",1.5,4,"C","-",4,1.7,null,0,"As SoA","As SoA","As SoA",0,"As SoA","N/A","Optional ","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 3400","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general"," ","L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","Dado on 2 walls","None",9,2,24]
["OFF42","Laundries","Laundries","OFF42","OFF42","New Build","SL_30_60_47","Laundries","Room for washing, drying and sorting pupils clothes","Washing, drying and sorting pupils clothes.","Staff and admin","General",1.5,4,"-","-",0,0,null,0,16,"-","-",0,"As SoA","N/A","None","Disabled access into the space required","Enclosed",null,"2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","D5.2av","strong, with vision panel","N/A","no internal doorset required",null,null,"F7.3h","wet area","C1.2","humid areas","W3.2","humid",null,"L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Average","Medium","<=1.5","<=2.0","Extract as Tech Annex 2F 6.3","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",0,0,0]
["OFF45","Meeting rooms (training)",null,null,"OFF40","New Build","SL_20_15_50","Meeting rooms","Conference or meeting room for meetings of staff, governors and other adults","Meeting room for staff with internal and external visitors etc. Privacy important. Small scale presentations using ICT.","Staff and admin","General",1.5,4,"C","-",4,1.7,null,0,"As SoA","As SoA","As SoA",0,"As SoA","N/A","Optional ","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 3400","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general"," ","L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","Dado on 2 walls","None",9,2,24]
["OFF50","Staff rooms","Staff rooms","OFF50","OFF50","New Build","SL_90_20_85","Staff rooms","Main space for any staff in school to work, meet and socialise, including preparation of teaching resources","Informal meeting and discussion during breaks. Lesson preparation and research mainly using tables. Limited ICT access. Marking and recording pupils work. Receiving post. Relaxing and taking refreshments.","Staff and admin","General",1.5,4,"C","-",4,1.7,4,6.8,"As SoA","As SoA","As SoA","As SoA","As SoA","N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400 (3300 / 2700 if >27m2)","2400 / N/A","7800 / 3400","Optional","CTS","Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1m","mixed general","C1.1","general","W1.1","general"," ","L1.1k","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","To suit ICT","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,12]
["OFF51","Staff rooms (prep and social)","Staff rooms (prep and social)","OFF51","OFF50","New Build","SL_90_20_85","Staff rooms","Main space for any staff in school to work, meet and socialise, including preparation of teaching resources","Informal meeting and discussion during breaks. Lesson preparation and research mainly using tables. Limited ICT access. Marking and recording pupils work. Receiving post. Relaxing and taking refreshments.","Staff and admin","General",1.5,4,"C","-",4,1.7,4,6.8,"As SoA","As SoA","As SoA","As SoA","As SoA","N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400 (3300 / 2700 if >27m2)","2400 / N/A","7800 / 3400","Optional","CTS","Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1m","mixed general","C1.1","general","W1.1","general"," ","L1.1k","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","To suit ICT","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,12]
["OFF52","Staff rooms (social)","Staff rooms (social)","OFF52","OFF50","New Build","SL_90_20_85","Staff rooms","Main space for any staff in school to meet and socialise, and to make tea and snacks","Informal meeting and discussion during breaks. Limited ICT access. Receiving post/notices. Relaxing and taking refreshments.","Staff and admin","General",1.5,4,"B","-",2,1.6,null,0,"As SoA","As SoA","As SoA","As SoA","As SoA","N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400 (3300 / 2700 if >27m2)","2400 / N/A","7800 / 3400","Optional","CTS","Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1m","mixed general","C1.1","general","W1.1","general"," ","L1.1k","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.2","Ventilation as Tech Annex 2F 6.2","None","To suit ICT","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",8,2,48]
["OFF53","Staff rooms (parents) ","Staff rooms (parents) ","OFF53","OFF50","New Build","SL_90_20_85","Staff rooms","Room for informal meetings and preparing drinks","Small group meetings and socialising of parents, carers and other visitors. Making drinks and/or snacks.","Staff and admin","General",1.5,4,"C","-",4,1.7,null,0,"As SoA","As SoA","As SoA","As SoA","As SoA","N/A","Yes ","Disabled access into the area preferred","Enclosed or semi-enclosed",null,"2700 / 2400 (3300 / 2700 if >27m2)","2400 / N/A","7800 / 3400","Optional","CTS","Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L1.1k","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.0","Ventilation as Tech Annex 2F 6.2","None","Where required","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,12]
["PER01","Music rooms (fitted, restrictive, extg)","Music rooms (fitted, restrictive, extg)","PER01","PER02","Existing","SL_25_10_55","Music rooms","Secondary school music classroom for limited performance, composing and theory","Group and individual composing and music making using ICT, keyboards and percussion. Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Teacher led presentations and briefings using the whiteboard.","Basic teaching","Fitted",2,4,"C","restrictive",4,1.7,null,1,55,30,30,1,33,"11-19","None","Full disabled access not required","Enclosed",null,"3300 / 2700","as existing","7800 / 7000","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general","Wall panels may be required to achieve required sound quality ","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","if community use",null,"T5","Very high","Low","<=1.0","<=1.0",null,"None","Dado on 2 walls","None",40,null,12]
["PER02","Music rooms (fitted)","Music rooms (fitted)","PER02","PER02","New Build","SL_25_10_55","Music rooms","Secondary school music classroom for performance, composing and theory","Group and individual composing and music making using ICT, keyboards and percussion. Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Teacher led presentations and briefings using the whiteboard.","Basic teaching","Fitted",2,4,"D","standard",5,1.9,null,1,62,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7000","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general","Wall panels may be required to achieve required sound quality ","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","if community use",null,"T5","Very high","Low","<=1.0","<=1.0",null,"None","Dado on 2 walls","None",40,2,12]
["PER03","Music rooms (fitted, extensive)","Music rooms (fitted, extensive)","PER03","PER02","New Build","SL_25_10_55","Music rooms","Secondary school music classroom for performance, composing and theory, with option of keyboards for all pupils","Group and individual composing and music making using ICT, keyboards and percussion. Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Teacher led presentations and briefings using the whiteboard.","Basic teaching","Fitted",2,4,"E","extensive",6,2.1,null,1,69,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7000","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general","Wall panels may be required to achieve required sound quality ","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","if community use",null,"T5","Very high","Low","<=1.0","<=1.0",null,"None","Dado on 2 walls","None",40,2,16]
["PER05","Music and drama classrooms","Music and drama classrooms","PER05","PER05","New Build","SL_25_10_54","Music and drama classrooms","Secondary school music room with space for performances to a small audience","Group and individual composing and music making using ICT, keyboards and percussion. Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"F","standard",8,2.5,null,1,83,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7000","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general","Wall panels may be required to achieve required sound quality. Flooring suitable for heavy movable FF&E on castors ","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","if community use",null,"T5","Very high","Low","<=1.0","<=1.0",null,"None","To suit equipment","None",10,2,16]
["PER08","Music and drama classrooms (recital)","Music and drama classrooms (recital)","PER08","PER05","New Build","SL_25_10_54","Music and drama classrooms","Secondary school studio space for drama and large music recital room combined","Group and individual composing and music making using ICT, keyboards and percussion. Independent study and research. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Pupil led performances to class. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"F","standard",8,2.5,null,1,83,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7000","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,null,"F6.1","multi-purpose sport","C1.1","general","W1.1","general","Wall panels may be required to achieve required sound quality. Flooring suitable for heavy movable FF&E on castors ","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","if community use",null,"T5","Very high","Low","<=1.0","<=1.5",null,"None","To suit equipment","None",8,2,16]
["PER11","Music and drama classrooms, studio","Music and drama classrooms, studio","PER11","PER11","New Build","SL_25_10_54","Music and drama classrooms","Primary school space for music, movement, dance and drama","Dance. Gymnastics. Occasional use for exams and exhibitions. Table tennis. Trampolining. Exhibitions.  Music and drama rehearsal and performance. Parent evenings. Presentations. Assessment.","Halls and dining","General",1.5,4,"C","-",4,1.7,null,0,55,30,30,0,33,"4-11","Optional ","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7000","Optional","CTS","Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,null,"F6.1","multi-purpose sport","C1.1","general","W1.1h","general","Wall panels may be required to achieve required sound quality. Flooring suitable for heavy movable FF&E on castors ","L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","if community use",null,"T5","High","Medium","<=1.0","<=1.0",null,"None","To suit equipment","None",8,2,16]
["PER15","Drama studios","Drama studios","PER15","PER15","New Build","SL_25_10_24","Drama studios","Secondary school studio space for drama ","Drama workshops. Individual, group and whole class pupil led presentations and discussions using the whiteboard. Pupil led rehearsals and performance to a small audience. Teacher led presentations and briefings occasionally with whiteboard.","Basic teaching","Large",12.5,-20,"F1","standard",9,2.7,null,1,97,30,30,1,33,"11-19","Yes ","Disabled access into the space required","Enclosed","adjacent to Assembly hall, via storage","4500 / 4500","3300 / 2700","7800 / 7000","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,"Finger guards if in a special school or AP","F6.1","multi-purpose sport","C1.1","general","W1.1h","general","Wall panels may be required to achieve required sound quality","L6.2i","Daylight to be excluded or blinds provided or blinds provided","Daylight to be excluded or blinds provided","Not applicable","Not applicable",300,"man on, day dim, abs off","if community use",null,"T5","High","Low","<=1.0","<=1.0",null,"None","To suit equipment","None",8,2,8]
["PER50","Music rooms (fitted, ambulant)","Music rooms (fitted, ambulant)","PER50","PER02","New Build","SL_25_10_55","Music rooms","Classroom for music making and music therapy for ambulant pupils needing additional support ","Group and individual composing and music making using instruments and specialist equipment. Teacher led presentations and briefings using the whiteboard.","Basic teaching","Fitted",2,-20,"G1","SEN",12,3.1,null,1,55,12,14,1,16,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7000","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,"Access control system and finger guards to be agreed with school","F1.1","general","C1.1","general","W1.1","general","Wall panels may be required to achieve required sound quality ","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","if community use",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","None",24,0,32]
["PER51","Music rooms (fitted, AP)",null,null,"PER02","New Build","SL_25_10_55","Music rooms","Classroom for music making and music therapy for ambulant pupils needing additional support ","Group and individual composing and music making using instruments and specialist equipment. Teacher led presentations and briefings using the whiteboard.","Basic teaching","Fitted",2,-20,"G1","SEN",12,3.1,null,1,41,12,14,1,16,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7000","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,"Access control system and finger guards to be agreed with school","F1.1","general","C1.1","general","W1.1","general","Wall panels may be required to achieve required sound quality ","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","if community use",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","None",24,0,32]
["PER55","Music rooms (fitted), non-ambulant","music classroom (non-ambulant) ","PER55","PER55","New Build","SL_25_10_55","Music rooms","Classroom for music making and music therapy for ambulant and non-ambulant pupils needing significant additional support and specialist equipment","Group and individual composing and music making using instruments and specialist equipment. Teacher led presentations and briefings using the whiteboard.","Basic teaching","Fitted",2,-20,"J1","SEN",32,4.4000000000000004,null,1,62,6,7,1,8,"11-19","None","Full disabled access required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,"Ergonomic handle, finger guards and access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1","general","Wall panels may be required to achieve required sound quality ","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","if community use",null,"T5/T7","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","None",24,0,32]
["PER60","Music and drama classrooms (ambulant)","Music and drama classrooms (ambulant)","PER60","PER05","New Build","SL_25_10_54","Music and drama classrooms","Secondary studio space for music making and drama for ambulant pupils needing additional support ","Group and individual composing and music making using instruments and specialist equipment. Drama workshops, rehearsals and performance to a small audience. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"G1","SEN",12,3.1,null,1,55,12,14,1,16,"11-19","Optional ","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7000","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,"Access control system and finger guards to be agreed with school","F1.1","general","C1.1","general","W1.1","general","Wall panels may be required to achieve required sound quality","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","if community use",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit equipment","None",24,0,32]
["PER61","Music and drama classrooms (AP)",null,null,"PER05","New Build","SL_25_10_54","Music and drama classrooms","Secondary studio space for music making and drama for ambulant pupils needing additional support ","Group and individual composing and music making using instruments and specialist equipment. Drama workshops, rehearsals and performance to a small audience. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"G1","SEN",12,3.1,null,1,41,8,"10",1,12,"11-19","Optional ","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7000","Not required",1050,"","D1.1av","general","N/A","no internal doorset required",null,"Access control system and finger guards to be agreed with school","F1.1","general","C1.1","general","W1.1","general","Wall panels may be required to achieve required sound quality","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","if community use",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit equipment","None",24,0,32]
["PER65","Music and drama classrooms, non-ambulant","music/ drama studio (non-ambulant)","PER65","PER65","New Build","SL_25_10_54","Music and drama classrooms","Secondary studio space for drama and music making and therapy for ambulant and non-ambulant pupils needing significant additional support and specialist equipment","Group and individual composing and music making using instruments and specialist equipment. Drama workshops, rehearsals and performance to a small audience. Teacher led presentations and briefings using the whiteboard.","Basic teaching","General",1.5,4,"J1","SEN",32,4.4000000000000004,null,1,62,6,7,1,8,"11-19","Optional ","Full disabled access required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D6.1mv","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1h","general","Wall panels may be required to achieve required sound quality","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","if community use",null,"T5/T7","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit equipment","None",24,0,32]
["PLA02","Plant and control spaces","Plant and control spaces","PLA02","PLA02","New Build","SL_90_90","Plant and control spaces","Any enclosure used for plant, including central ventilation or sprinkler tanks","Mechanical or electrical plant facilities","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed",null,"N/A","N/A","N/A / CTS","Optional","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"N/A","not applicable","N/A","not applicable","N/A","not applicable",null,"L5.5p","No requirement","No requirement","Not applicable","Not applicable",200,"man on, man off","No",null,"N/A","N/A","N/A","N/A","N/A",null,"N/A","N/A","N/A"]
["PLA05","Switch rooms, distribution boards","Switch rooms, distribution boards","PLA05","PLA05","New Build","SL_90_90_85","Switch rooms","Cupboard for electrical distribution board","Electrical plant facilities","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed",null,"N/A","N/A","N/A / CTS","Not required","N/A","","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room","N/A","not applicable","N/A","not applicable","W4.1","rough",null,"N/A","Not applicable","Not applicable","Not applicable","Not applicable","-","n/a","N/A",null,"N/A","N/A","N/A","N/A","N/A","Ventilation as Tech Annex 2F 4.3.11","N/A","N/A","N/A"]
["PLA07","Stairways, plant","Stairways, plant","PLA07","PLA20","New Build","SL_90_10_87","Stairways","Enclosure for stairway to rooftop or other plant ","Access to other plant facilities","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed",null,"N/A","N/A","N/A / CTS","Optional","N/A","Contractor to Specify for approval if provided","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room","N/A","not applicable","N/A","not applicable","W4.1","rough",null,"L5.5p","No requirement","No requirement","Not applicable","Not applicable","-","n/a","N/A",null,"N/A","N/A","N/A","N/A","N/A",null,"N/A","N/A","None"]
["PLA08","Stairways, plant (to roof)","Stairways, plant","PLA07","PLA20","New Build","SL_90_10_87","Stairways","Enclosure or extension to stairs for stairway to rooftop","Access to other plant facilities","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed",null,"N/A","N/A","N/A / CTS","Required","N/A","Contractor to Specify for approval","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room","N/A","not applicable","N/A","not applicable","W4.1","rough",null,"L5.5p","No requirement","No requirement","Not applicable","Not applicable","-","n/a","N/A",null,"N/A","N/A","N/A","N/A","N/A",null,"N/A","N/A","None"]
["PLA09","Stairways, plant (escape)","Stairways, plant","PLA07","PLA20","New Build","SL_90_10_87","Stairways","Enclosure for escape from rooftop or other plant, typically using a fixed ladder","Access to other plant facilities","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed",null,"N/A","N/A","N/A / CTS","Required","N/A","Contractor to Specify for approval","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room","N/A","not applicable","N/A","not applicable","W4.1","rough",null,"L5.5p","No requirement","No requirement","Not applicable","Not applicable","-","n/a","N/A",null,"N/A","N/A","N/A","N/A","N/A",null,"N/A","N/A","None"]
["PLA10","Server rooms","Server rooms","PLA10","PLA10","New Build","SL_90_90_77","Server rooms","Specialist space for ICT servers ","Server racks and switching with space for access and maintenance","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled access not required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / 3400","Not required","N/A","","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room","F2.1","stores","C3.2","humid areas","W1.1","general","All finishes shall be static resistant","L5.5p","No requirement","No requirement","Not applicable","Not applicable",200,"man on, man off","No",null,"see TA 2F","N/A","N/A","N/A","N/A","Ventilation and temperature control as Tech Annex 2F 7.4","None","To suit equipment","None"]
["PLA11","Server rooms (1-cabinet)","Server rooms (1-cabinet)","PLA11","PLA10","New Build","SL_90_90_77","Server rooms","Specialist space for ICT servers ","Server racks and switching with space for access and maintenance","Non-net","Non-net",null,null,"-","-",0,0,null,0,7.5,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled access not required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / 3400","Not required","N/A","","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room","F2.1","stores","C3.2","humid areas","W1.1","general","All finishes shall be static resistant","L5.5p","No requirement","No requirement","Not applicable","Not applicable",200,"man on, man off","No",null,"see TA 2F","N/A","N/A","N/A","N/A","Ventilation and temperature control as Tech Annex 2F 7.4","None","To suit equipment","None"]
["PLA12","Server rooms (2-cabinet)","Server rooms (2-cabinet)","PLA12","PLA10","New Build","SL_90_90_77","Server rooms","Specialist space for ICT servers ","Server racks and switching with space for access and maintenance","Non-net","Non-net",null,null,"-","-",0,0,null,0,10.199999999999999,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled access not required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / 3400","Not required","N/A","","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room","F2.1","stores","C3.2","humid areas","W1.1","general","All finishes shall be static resistant","L5.5p","No requirement","No requirement","Not applicable","Not applicable",200,"man on, man off","No",null,"see TA 2F","N/A","N/A","N/A","N/A","Ventilation and temperature control as Tech Annex 2F 7.4","None","To suit equipment","None"]
["PLA13","Server rooms (3-cabinet)","Server rooms (3-cabinet)","PLA13","PLA10","New Build","SL_90_90_77","Server rooms","Specialist space for ICT servers ","Server racks and switching with space for access and maintenance","Non-net","Non-net",null,null,"-","-",0,0,null,0,12.9,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled access not required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / 3400","Not required","N/A","","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room","F2.1","stores","C3.2","humid areas","W1.1","general","All finishes shall be static resistant","L5.5p","No requirement","No requirement","Not applicable","Not applicable",200,"man on, man off","No",null,"see TA 2F","N/A","N/A","N/A","N/A","Ventilation and temperature control as Tech Annex 2F 7.4","None","To suit equipment","None"]
["PLA14","Server rooms (4-cabinet)","Server rooms (4-cabinet)","PLA14","PLA10","New Build","SL_90_90_77","Server rooms","Specialist space for ICT servers ","Server racks and switching with space for access and maintenance","Non-net","Non-net",null,null,"-","-",0,0,null,0,15.6,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled access not required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / 3400","Not required","N/A","","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room","F2.1","stores","C3.2","humid areas","W1.1","general","All finishes shall be static resistant","L5.5p","No requirement","No requirement","Not applicable","Not applicable",200,"man on, man off","No",null,"see TA 2F","N/A","N/A","N/A","N/A","Ventilation and temperature control as Tech Annex 2F 7.4","None","To suit equipment","None"]
["PLA15","Server rooms (5-cabinet)","Server rooms (5-cabinet)","PLA15","PLA10","New Build","SL_90_90_77","Server rooms","Specialist space for ICT servers ","Server racks and switching with space for access and maintenance","Non-net","Non-net",null,null,"-","-",0,0,null,0,18.399999999999999,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled access not required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / 3400","Not required","N/A","","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room","F2.1","stores","C3.2","humid areas","W1.1","general","All finishes shall be static resistant","L5.5p","No requirement","No requirement","Not applicable","Not applicable",200,"man on, man off","No",null,"see TA 2F","N/A","N/A","N/A","N/A","Ventilation and temperature control as Tech Annex 2F 7.4","None","To suit equipment","None"]
["PLA18","Server rooms (ICT hub)","Server rooms (ICT hub)","PLA18","PLA10","New Build","SL_90_90_77","Server rooms","Specialist space for ICT hub","Rack and switching with space for access and maintenance","Non-net","Non-net",null,null,"-","-",0,0,null,0,7.5,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled access not required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / 3400","Not required","N/A","","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room","F2.1","stores","C3.2","humid areas","W1.1","general","All finishes shall be static resistant","L5.5p","No requirement","No requirement","Not applicable","Not applicable",200,"man on, man off","No",null,"see TA 2F","N/A","N/A","N/A","N/A","Ventilation and temperature control as Tech Annex 2F 7.4","None","To suit equipment","None"]
["PLA20","Plant rooms","Plant rooms","PLA20","PLA20","New Build","SL_90_90_64","Plant rooms","Internal room for mechanical or electrical plant, including boilers and tanks","Mechanical or electrical plant facilities","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed",null,"N/A","N/A","N/A / CTS","Double doors","N/A","Contractor to Specify for approval","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room","F5.4","heavy practical","C3.2","humid areas","W4.1","rough","Flooring suitable for heavy movable FF&E on castors ","L5.5p","No requirement","No requirement","Not applicable","Not applicable",200,"man on, man off","No",null,"N/A","N/A","N/A","N/A","N/A","Ventilation as Tech Annex 2F 4.3.11","N/A","N/A","N/A",2,null,null,"Fire Containment."]
["PLA21","Plant rooms (heat source)","Plant rooms (heat source)","PLA21","PLA20","New Build","SL_90_90_64","Plant rooms","Internal room for heating source plant, including boilers","Mechanical or electrical plant facilities","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed",null,"N/A","N/A","N/A / CTS","Double doors","N/A","Contractor to Specify for approval","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room","F5.4","heavy practical","C3.2","humid areas","W4.1","rough","Flooring suitable for heavy movable FF&E on castors ","L5.5p","No requirement","No requirement","Not applicable","Not applicable",200,"man on, man off","No",null,"N/A","N/A","N/A","N/A","N/A","Ventilation as Tech Annex 2F 4.3.11","N/A","N/A","N/A",2,null,null,"Fire Containment."]
["PLA22","Plant rooms (ventilation)","Plant rooms (ventilation)","PLA22","PLA20","New Build","SL_90_90_64","Plant rooms","Internal room for mechanical ventilation plant","Mechanical or electrical plant facilities","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed",null,"N/A","N/A","N/A / CTS","Double doors","N/A","Contractor to Specify for approval","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room","F5.4","heavy practical","C3.2","humid areas","W4.1","rough","Flooring suitable for heavy movable FF&E on castors ","L5.5p","No requirement","No requirement","Not applicable","Not applicable",200,"man on, man off","No",null,"N/A","N/A","N/A","N/A","N/A","Ventilation as Tech Annex 2F 4.3.11","N/A","N/A","N/A",2,null,null,"Fire Containment."]
["PLA23","Plant rooms (cold water tanks)","Plant rooms (cold water tanks)","PLA23","PLA20","New Build","SL_90_90_64","Plant rooms","Internal room for plant, including tanks","Mechanical or electrical plant facilities","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed",null,"N/A","N/A","N/A / CTS","Double doors","N/A","Contractor to Specify for approval","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room","F5.4","heavy practical","C3.2","humid areas","W4.1","rough","Flooring suitable for heavy movable FF&E on castors ","L5.5p","No requirement","No requirement","Not applicable","Not applicable",200,"man on, man off","No",null,"N/A","N/A","N/A","N/A","N/A","Ventilation as Tech Annex 2F 4.3.11","N/A","N/A","N/A",2,null,null,"Fire Containment."]
["PLA24","Plant rooms (sprinkler pumps)","Plant rooms (sprinkler pumps)","PLA24","PLA20","New Build","SL_90_90_64","Plant rooms","Internal room for mechanical plant, including sprinkler pumps","Mechanical or electrical plant facilities","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed",null,"N/A","N/A","N/A / CTS","Double doors","N/A","Contractor to Specify for approval","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room","F5.4","heavy practical","C3.2","humid areas","W4.1","rough","Flooring suitable for heavy movable FF&E on castors ","L5.5p","No requirement","No requirement","Not applicable","Not applicable",200,"man on, man off","No",null,"N/A","N/A","N/A","N/A","N/A","Ventilation as Tech Annex 2F 4.3.11","N/A","N/A","N/A",2,null,null,"Fire Containment."]
["PLA25","Plant rooms (electrical intake)","Plant rooms (electrical intake)","PLA25","PLA20","New Build","SL_90_90_64","Plant rooms","Internal room for electrical intake plant","Mechanical or electrical plant facilities","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed",null,"N/A","N/A","N/A / CTS","Double doors","N/A","Contractor to Specify for approval","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room","F5.4","heavy practical","C3.2","humid areas","W4.1","rough","Flooring suitable for heavy movable FF&E on castors ","L5.5p","No requirement","No requirement","Not applicable","Not applicable",200,"man on, man off","No",null,"N/A","N/A","N/A","N/A","N/A","Ventilation as Tech Annex 2F 4.3.11","N/A","N/A","N/A",2,null,null,"Fire Containment."]
["PLA30","Light wells (open)","Light wells","PLA30","PLA30","New Build","SL_90_60_51","Light wells","Any void for vertical ventilation that is open to adjacent spaces or circulation","Air movement","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Open plan","adjacent to circulation","N/A","N/A","N/A / CTS","Not required","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"N/A","not applicable","N/A","not applicable","CTS","Contractor to specify for approval",null,"N/A","Not applicable","Not applicable","Not applicable","Required to some adjoining spaces","-","n/a","N/A",null,"N/A","N/A","N/A","N/A","N/A",null,"N/A","N/A","N/A",0]
["PLA31","Light wells (open ventilation)",null,null,"PLA30","New Build","SL_90_90_78","Services shafts","Any void for vertical ventilation that is open to adjacent spaces or circulation but not providing daylight via rooflights","Air movement","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Open plan","adjacent to circulation","N/A","N/A","N/A / CTS","Not required","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"N/A","not applicable","N/A","not applicable","CTS","Contractor to specify for approval",null,"N/A","Not applicable","Not applicable","Not applicable","Required to some adjoining spaces","-","n/a","N/A",null,"N/A","N/A","N/A","N/A","N/A",null,"N/A","N/A","N/A"]
["PLA32","Light wells (open daylit ventilation)",null,null,"PLA30","New Build","SL_90_90_78","Services shafts","Any void for vertical ventilation that is open to adjacent spaces or circulation and provides daylight via rooflights","Air movement","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Open plan","adjacent to circulation","N/A","N/A","N/A / CTS","Not required","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"N/A","not applicable","N/A","not applicable","CTS","Contractor to specify for approval",null,"N/A","Not applicable","Not applicable","Not applicable","Required to some adjoining spaces","-","n/a","N/A",null,"N/A","N/A","N/A","N/A","N/A",null,"N/A","N/A","N/A"]
["PLA40","Services shafts (enclosed risers, flues and ducts)","Services shafts (risers, flues and ducts)","PLA06","PLA40","New Build","SL_90_90_78","Services shafts","Any vertical riser or duct space used for plant","Mechanical or electrical plant facilities","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed",null,"N/A","N/A","N/A / CTS","Not required","N/A","","CTS","Contractor to specify for approval","N/A","no internal doorset required",null,"Door or hatch if needed for access","N/A","not applicable","N/A","not applicable","N/A","not applicable",null,"N/A","Not applicable","Not applicable","Not applicable","Not applicable","-","n/a","N/A",null,"N/A","N/A","N/A","N/A","N/A",null,"N/A","N/A","N/A",null,null,null,"Fire Containment."]
["PLA41","Services shaft (enclosed ventilation)",null,null,"PLA40","New Build","SL_90_90_78","Services shafts","Any vertical riser or duct space used for concealed ventilation","Air movement","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed",null,"N/A","N/A","N/A","Not required","N/A","","CTS","Contractor to specify for approval","N/A","no internal doorset required",null,"Door or hatch if needed for access","N/A","not applicable","N/A","not applicable","N/A","not applicable",null,"N/A","Not applicable","Not applicable","Not applicable","Not applicable","-","n/a","N/A",null,"N/A","N/A","N/A","N/A","N/A",null,"N/A","N/A","N/A",null,null,null,"Fire Containment."]
["PLA42","Services shafts (enclosed daylit ventilation)",null,null,"PLA40","New Build","SL_90_90_78","Services shafts","Any vertical riser or duct space used for ventilation but also providing daylight via rooflights and internal glazing","Air movement","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed",null,"N/A","N/A","N/A","Not required","N/A","","CTS","Contractor to specify for approval","N/A","no internal doorset required",null,"Door or hatch if needed for access","N/A","not applicable","N/A","not applicable","N/A","not applicable",null,"N/A","Not applicable","Not applicable","Not applicable","Required to some adjoining spaces","-","n/a","N/A",null,"N/A","N/A","N/A","N/A","N/A",null,"N/A","N/A","N/A",null,null,null,"Fire Containment."]
["PLA43","Services shafts (enclosed electrical)",null,null,"PLA40","New Build","SL_90_90_78","Services shafts","Any vertical riser or duct space used for electrical plant, cabling or distribution boards","Electrical plant facilities","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed",null,"N/A","N/A","N/A","Not required","N/A","","CTS","Contractor to specify for approval","N/A","no internal doorset required",null,"Door or hatch if needed for access","N/A","not applicable","N/A","not applicable","N/A","not applicable",null,"N/A","Not applicable","Not applicable","Not applicable","Not applicable","-","n/a","N/A",null,"N/A","N/A","N/A","N/A","N/A",null,"N/A","N/A","N/A",null,null,null,"Fire Containment."]
["PLA44","Services shafts (enclosed other)",null,null,"PLA40","New Build","SL_90_90_78","Services shafts","Any vertical riser or duct space used for mechanical plant, pipework or similar","Mechanical plant facilities","Non-net","Non-net",null,null,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed",null,"N/A","N/A","N/A","Not required","N/A","","CTS","Contractor to specify for approval","N/A","no internal doorset required",null,"Door or hatch if needed for access","N/A","not applicable","N/A","not applicable","N/A","not applicable",null,"N/A","Not applicable","Not applicable","Not applicable","Not applicable","-","n/a","N/A",null,"N/A","N/A","N/A","N/A","N/A",null,"N/A","N/A","N/A",null,null,null,"Fire Containment."]
["PLA50","Plant rooms, pool","Plant rooms, pool","PLA50","PLA50","New Build","SL_90_90_64","Plant rooms","Internal room for plant associated with heating and treating pool water","Mechanical or electrical plant facilities","Non-net","Non-net",null,null,"-","SEN",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Required","N/A","Contractor to Specify for approval","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room","F5.4","heavy practical","C3.2","humid areas","W4.1","rough","Bunded floor for water treatment plant.","L5.5p","No requirement","No requirement","Not applicable","Not applicable",200,"man on, man off","No",null,"To suit equipment","N/A","N/A","N/A","N/A",null,"N/A","N/A","N/A"]
["PRA01","ICT-rich classrooms (extg primary)","ICT-rich classrooms (extg primary)","PRA01","CLA32","Existing","SL_25_10_41","ICT-rich classrooms","Primary school classroom used for fixed ICT devices for all workplaces with limited layout options","Independent study and research. Individual, group and whole class pupil led presentations and discussions using ICT devices and whiteboard. Teacher led presentations and briefings using ICT and the whiteboard.","Basic teaching","Fitted",2,4,"D","standard",5,1.9,null,1,55,26,26,1,29,"4-11","Optional ","Full disabled access not required","Enclosed",null,"3300 / 2700","as existing","7800 / 7200","Not required",750,"","D1.1av","general","N/A","no internal doorset required",null,"Access control and hinge protection/ finger guards to be agreed with school if used by Early Years or Infant pupils","F1.1","general","C1.1","general","W1.1","general"," ","L1.2b","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","To suit ICT","None",27,2,72]
["PRA02","Primary practical, temporarily ICT-rich","Primary practical, temporarily ICT-rich","PRA02","PRA02","New Build","SL_25_10_67","Primary practical rooms","Specialist space with fixed ICT devices for all workplaces, sink and wet services for use as practical in future","Independent study and research. Individual, group and whole class pupil led presentations and discussions using ICT devices and whiteboard. Teacher led presentations and briefings using ICT and the whiteboard.","Basic teaching","Fitted",2,4,"D","standard",5,1.9,null,1,62,30,30,1,33,"4-11","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7200","Not required",750,"","D2.2av","strong","N/A","no internal doorset required",null,"Access control and hinge protection/ finger guards to be agreed with school if used by Early Years or Infant pupils","F3.4h","hygienic non-slip","C1.2","humid areas","W1.1","general","Flooring suitable for heavy movable FF&E on castors ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","To suit ICT","Hot and cold water to all sinks listed under FF&E, cold water to other sinks or equipment",27,2,32]
["PRA10","Primary practical rooms","Primary practical rooms","PRA10","PRA10","New Build","SL_25_10_67","Primary practical rooms","Specialist space for primary food preparation, science, art and/or Design and Technology activities","Group discussion. Independent study and research. Making and tasting food. Presentations. Simple supervised experiments and evaluation exercises. Using the whiteboard.","Basic teaching","Light practical",2.5,4,"D","standard",5,1.9,null,1,"As SoA","As SoA","As SoA",1,"As SoA","4-11","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7200","Not required",750,"","D2.2av","strong","N/A","no internal doorset required",null,"Access control and hinge protection/ finger guards to be agreed with school if used by Early Years or Infant pupils","F3.4h","hygienic non-slip","C1.2","humid areas","W1.1","general","Flooring suitable for heavy movable FF&E on castors ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold water to all sinks listed under FF&E, cold water to other sinks or equipment",12,2,20]
["PRA12","Primary practical (food/ science/ DT)","Primary practical (food/ science/ DT)","PRA12","PRA10","New Build","SL_25_10_67","Primary practical rooms","Specialist space for primary food preparation, science, art and Design and Technology activities","Group discussion. Independent study and research. Making and tasting food. Presentations. Simple supervised experiments and evaluation exercises. Using the whiteboard.","Basic teaching","Light practical",2.5,4,"D","standard",5,1.9,null,1,"As SoA","As SoA","As SoA",1,"As SoA","4-11","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7200","Not required",750,"","D2.2av","strong","N/A","no internal doorset required",null,"Access control and hinge protection/ finger guards to be agreed with school if used by Early Years or Infant pupils","F3.4h","hygienic non-slip","C1.2","humid areas","W1.1","general","Flooring suitable for heavy movable FF&E on castors ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold water to all sinks listed under FF&E, cold water to other sinks or equipment",12,2,20]
["PRA13","Primary practical (infant food/ science/ DT)","Primary practical (infant food/ science/ DT)","PRA13","PRA10","New Build","SL_25_10_67","Primary practical rooms","Specialist space for primary food preparation, early years science, art and Design and Technology activities","Group discussion. Independent study and research. Making and tasting food. Presentations. Simple supervised experiments and evaluation exercises. Using the whiteboard.","Basic teaching","Light practical",2.5,4,"D","standard",5,1.9,null,1,69,30,30,1,33,"4-7","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7200","Not required",750,"","D2.2av","strong","N/A","no internal doorset required",null,"Access control and hinge protection/ finger guards to be agreed with school","F3.4h","hygienic non-slip","C1.2","humid areas","W1.1","general","Flooring suitable for heavy movable FF&E on castors ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","if community use",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold water to all sinks listed under FF&E, cold water to other sinks or equipment",12,2,32]
["PRA14","Primary practical (junior food/ science/ DT)","Primary practical (junior food/ science/ DT)","PRA14","PRA10","New Build","SL_25_10_67","Primary practical rooms","Specialist space for primary food preparation, Key Stage 2 science, art and Design and Technology activities","Group discussion. Independent study and research. Making and tasting food. Presentations. Simple supervised experiments and evaluation exercises. Using the whiteboard.","Basic teaching","Light practical",2.5,4,"D","standard",5,1.9,null,1,69,30,30,1,33,"7-11","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7200","Not required",750,"","D2.2av","strong","N/A","no internal doorset required",null,null,"F3.4h","hygienic non-slip","C1.2","humid areas","W1.1","general","Flooring suitable for heavy movable FF&E on castors ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","if community use",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold water to all sinks listed under FF&E, cold water to other sinks or equipment",12,2,32]
["PRA15","Primary practical (food/ science)","Primary practical (food/ science)","PRA15","PRA10","New Build","SL_25_10_67","Primary practical rooms","Specialist space for primary food preparation","Group discussion. Independent study and research. Making and tasting food. Presentations. Simple supervised experiments and evaluation exercises. Using the whiteboard.","Basic teaching","Light practical",2.5,4,"D","standard",5,1.9,null,1,69,30,30,1,33,"4-11","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7200","Not required",750,"","D2.2av","strong","N/A","no internal doorset required",null,"Access control and hinge protection/ finger guards to be agreed with school if used by Early Years or Infant pupils","F3.4h","hygienic non-slip","C1.2","humid areas","W1.1","general","Flooring suitable for heavy movable FF&E on castors ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","if community use",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold water to all sinks listed under FF&E, cold water to other sinks or equipment",12,2,16]
["PRA16","Primary practical (art/ DT)","Primary practical (art/ DT)","PRA16","PRA10","New Build","SL_25_10_67","Primary practical rooms","Specialist space for primary art and Design and Technology activities","Group discussion. Independent study and research. Presentations. Simple supervised experiments and evaluation exercises. Using the whiteboard.","Basic teaching","Light practical",2.5,4,"D","standard",5,1.9,null,1,34,15,15,1,17,"4-11","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7200","Not required",750,"","D2.2av","strong","N/A","no internal doorset required",null,"Access control and hinge protection/ finger guards to be agreed with school if used by Early Years or Infant pupils","F3.4h","hygienic non-slip","C1.2","humid areas","W1.1","general","Flooring suitable for heavy movable FF&E on castors ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","if community use",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold water to all sinks listed under FF&E, cold water to other sinks or equipment",12,2,20]
["PRA17","Primary practical (nurture)","Primary practical (nurture)","PRA17","PRA10","New Build","SL_25_10_67","Primary practical rooms","Specialist space for teaching primary core skills though art, play, food making and/or eating activities","Group discussion. Independent study and research. Making and tasting food. Presentations. Using the whiteboard.","Basic teaching","Light practical",2.5,4,"F1","standard",9,2.7,null,1,34,9,9,1,10,"4-11","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7200","Not required",750,"","D2.2av","strong","N/A","no internal doorset required",null,"Access control and hinge protection/ finger guards to be agreed with school if used by Early Years or Infant pupils","F3.4h","hygienic non-slip","C1.2","humid areas","W1.1","general","Flooring suitable for heavy movable FF&E on castors ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","if community use",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold water to all sinks listed under FF&E, cold water to other sinks or equipment",12,2,20]
["PRA31","Kitchenettes, food bay","Kitchenettes, food bay","PRA31","PRA31","New Build","SL_35_60_45","Kitchenettes","Bay for primary food preparation with a small group and pupil access to practical resources","Making food. Simple supervised exercises.","Basic teaching","Light practical",2.5,4,"D","standard",5,1.9,null,1,"As SoA","As SoA","As SoA",1,"As SoA","4-11","None","Disabled access into the space required","Semi-enclosed",null,"2700 / 2400","2400 / N/A","7800 / 1700","Not required","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F3.4h","hygienic non-slip","C1.2","humid areas","W1.1","general",null,"L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold water to all sinks listed under FF&E, cold water to other sinks or equipment",0,null,4]
["PRA41","Shared teaching areas, primary","Shared teaching areas, primary","PRA41","PRA41","New Build","SL_25_10_79","Shared teaching areas","Open plan teaching area shared by adjacent classbases with sinks to enhance the range of activities","Group activities. Group discussion. Independent study and research. Use of ICT. Small group work. ","Basic teaching","General",1.5,4,"C","standard",4,1.7,null,1,"As SoA","As SoA","As SoA",1,"As SoA","4-11","None","Disabled access into the space required","Open plan","adjacent to Semi-open classbases","3300 / 2700","2400 / N/A","N/A / 2700","Not required","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general"," ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.5","<=0.5","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","None",6,2,32]
["PRA50","Shared teaching areas (ambulant)","Shared teaching areas (ambulant)","PRA50","PRA41","New Build","SL_25_10_79","Shared teaching areas","Open plan teaching area for ambulant pupils needing additional support, shared by adjacent classbases with sinks to enhance the range of activities","Group activities. Group discussion. Independent study and research. Use of ICT. Small group work. ","Basic teaching","General",1.5,4,"G","SEN",10,2.9,null,0,"As SoA","As SoA","As SoA",0,"As SoA","4-11","None","Disabled access into the space required","Semi-enclosed or open plan","adjacent to Semi-open classbases","3300 / 2700","2400 / N/A","N/A / 2700","Not required","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","None",4,2,32]
["PRA70","Primary practical rooms (ambulant, food)","Primary practical rooms (ambulant, food)","PRA70","PRA10","New Build","SL_25_10_67","Primary practical rooms","Specialist space for primary food preparation with a small group of ambulant pupils needing additional support ","Group discussion. Independent study and research. Making and tasting food. Presentations. Simple supervised experiments and evaluation exercises. Using the whiteboard.","Basic teaching","Light practical",2.5,4,"G1","SEN",12,3.1,null,1,28,6,6,1,8,"4-11","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Not required",750,"","D2.2av","strong","N/A","no internal doorset required",null,"Access control system and hinge protection/ finger guards to be agreed with school","F3.4h","hygienic non-slip","C1.2","humid areas","W1.1","general","Flooring suitable for heavy movable FF&E on castors ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold water to all sinks listed under FF&E, cold water to other sinks or equipment",0,0,16]
["PRA75","Primary practical rooms, non-ambulant (food)","primary food room (non-ambulant)","PRA75","PRA75","New Build","SL_25_10_67","Primary practical rooms","Specialist space for primary food preparation with a small group of ambulant and non-ambulant ambulant pupils, needing significant additional support and specialist equipment","Group discussion. Independent study and research. Making and tasting food. Presentations. Simple supervised experiments and evaluation exercises. Using the whiteboard.","Basic teaching","Light practical",2.5,4,"H1","SEN",18,3.5,null,1,34,5,5,1,8,"4-11","None","Full disabled access required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Not required",750,"","D6.2mv","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F3.4h","hygienic non-slip","C1.2","humid areas","W1.1","general",null,"L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5/T7","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks, equipment and appliances",0,0,16]
["PRA80","Primary practical rooms (ambulant)","primary practical room (ambulant)","PRA80","PRA10","New Build","SL_25_10_67","Primary practical rooms","Specialist space for primary art, science and D&T activities with a small group of ambulant pupils needing additional support ","Group discussion. Independent study and research. Presentations. Simple supervised experiments and evaluation exercises. Using the whiteboard.","Basic teaching","Light practical",2.5,4,"G1","SEN",12,3.1,null,1,"As SoA","As SoA","As SoA",1,"As SoA","4-11","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7200","Not required",750,"","D2.2av","strong","N/A","no internal doorset required",null,"Access control system and hinge protection/ finger guards to be agreed with school","F3.4h","hygienic non-slip","C1.2","humid areas","W1.1","general","Flooring suitable for heavy movable FF&E on castors ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold water to all sinks listed under FF&E, cold water to other sinks or equipment",4,0,8]
["PRA83","Primary practical rooms (ambulant up to 6)",null,null,"PRA10","New Build","SL_25_10_67","Primary practical rooms","Specialist space for primary art, science and D&T activities with a small group of ambulant pupils needing additional support ","Group discussion. Independent study and research. Presentations. Simple supervised experiments and evaluation exercises. Using the whiteboard.","Basic teaching","Light practical",2.5,4,"G1","SEN",12,3.1,null,1,30,6,6,1,8,"4-11","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7200","Not required",750,"","D2.2av","strong","N/A","no internal doorset required",null,"Access control system and hinge protection/ finger guards to be agreed with school","F3.4h","hygienic non-slip","C1.2","humid areas","W1.1","general","Flooring suitable for heavy movable FF&E on castors ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold water to all sinks listed under FF&E, cold water to other sinks or equipment",4,0,8]
["PRA84","Primary practical rooms (ambulant up to 12)",null,null,"PRA10","New Build","SL_25_10_67","Primary practical rooms","Specialist space for primary art, science and D&T activities with a small group of ambulant pupils needing additional support ","Group discussion. Independent study and research. Presentations. Simple supervised experiments and evaluation exercises. Using the whiteboard.","Basic teaching","Light practical",2.5,4,"G1","SEN",12,3.1,null,1,55,12,14,1,16,"4-11","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7200","Not required",750,"","D2.2av","strong","N/A","no internal doorset required",null,"Access control system and hinge protection/ finger guards to be agreed with school","F3.4h","hygienic non-slip","C1.2","humid areas","W1.1","general","Flooring suitable for heavy movable FF&E on castors ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold water to all sinks listed under FF&E, cold water to other sinks or equipment",4,0,8]
["PRA85","Primary practical rooms, non-ambulant","primary practical room (non-ambulant)","PRA85","PRA85","New Build","SL_25_10_67","Primary practical rooms","Specialist space for primary art, science and D&T activities with a small group of ambulant and non-ambulant ambulant pupils, needing significant additional support and specialist equipment","Group discussion. Independent study and research. Presentations. Simple supervised experiments and evaluation exercises. Using the whiteboard.","Basic teaching","Light practical",2.5,4,"H1","SEN",18,3.5,null,1,34,5,5,1,6,"4-11","None","Full disabled access required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Not required",750,"","D6.1mv","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F3.4h","hygienic non-slip","C1.2","humid areas","W1.1","general",null,"L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5/T7","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks, equipment and appliances",4,0,8]
["PRI01","Nursery playrooms (restrictive, extg)","Nursery playrooms (restrictive, extg)","PRI01","PRI03","Existing","SL_25_10_57","Nursery playrooms","Existing primary school playroom for limited layout options and activities for 3 to 4 year olds","Group discussion. Using the whiteboard. Role play. Range of play activities. Quiet time. Small group work. Sand and water play. Solitary play. Computer-based play.","Basic teaching","General",1.5,4,"C","restrictive",4,1.7,null,1,48,26,26,1,29,"3-5","None","Full disabled access not required","Enclosed or semi-enclosed",null,"3300 / 2700","as existing","7800 / 7000","Required, fully glazed",750,"Contractor to Specify for approval","D1.1ev","early years","D1.1ev","early years",null,"Access control system to be agreed with school","F3.2i","classroom non-slip","C1.1","general","W1.1","general","Carpet mat to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",8,2,16]
["PRI03","Nursery playrooms","Nursery playrooms","PRI03","PRI03","New Build","SL_25_10_57","Nursery playrooms","Primary school playroom for a range of FF&E layout options and activities for 3 to 4 year olds","Group discussion. Using the whiteboard. Role play. Range of play activities. Quiet time. Small group work. Sand and water play. Solitary play. Computer-based play.","Basic teaching","General",1.5,4,"D","standard",5,1.9,null,1,55,26,26,1,29,"3-5","None","Disabled access into the space required","Enclosed or semi-enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Required, fully glazed",750,"Contractor to Specify for approval","D1.1ev","early years","D1.1ev","early years",null,"Access control system to be agreed with school","F3.2i","classroom non-slip","C1.1","general","W1.1","general","Carpet mat to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",8,2,16]
["PRI04","Nursery playrooms (2 to 3 year olds)","Nursery playrooms (2 to 3 year olds)","PRI04","PRI03","New Build","SL_25_10_57","Nursery playrooms","Primary school playroom for a range of layout options and activities for 2 to 3 year olds","Group discussion. Using the whiteboard. Role play. Range of play activities. Quiet time. Small group work. Sand and water play. Solitary play. Computer-based play.","Basic teaching","General",1.5,4,"E","standard",6,2.1,null,1,55,23,23,1,26,"2-3","None","Disabled access into the space required","Enclosed or semi-enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Required, fully glazed",750,"Contractor to Specify for approval","D1.1ev","early years","D1.1ev","early years",null,"Access control system to be agreed with school","F3.2i","classroom non-slip","C1.1","general","W1.1","general","Carpet mat to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",8,2,16]
["PRI05","Nursery playrooms (extensive)","Nursery playrooms (extensive)","PRI05","PRI03","New Build","SL_25_10_57","Nursery playrooms","Primary school playroom suitable for all playroom layout options and activities for 3 to 4 year olds","Group discussion. Using the whiteboard. Role play. Range of play activities. Quiet time. Small group work. Sand and water play. Solitary play. Computer-based play.","Basic teaching","General",1.5,4,"E","extensive",6,2.1,null,1,62,27,27,1,30,"3-4","None","Disabled access into the space required","Enclosed or semi-enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Required, fully glazed",750,"Contractor to Specify for approval","D1.1ev","early years","D1.1ev","early years",null,"Access control system to be agreed with school","F3.2i","classroom non-slip","C1.1","general","W1.1","general","Carpet mat to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",8,2,16]
["PRI11","Reception classrooms (restrictive, extg)","Reception classrooms (restrictive, extg)","PRI11","PRI13","Existing","SL_25_10_72","Reception classrooms","Existing primary school classroom for limited layout options and activities for Reception pupils","Computer based play. Group discussion. Quiet time. Range of play activities. Role play. Sand and water play. Small group work. Solitary play. Using the whiteboard.","Basic teaching","General",1.5,4,"C","restrictive",4,1.7,null,1,55,30,30,1,33,"4-5","None","Full disabled access not required","Enclosed or semi-enclosed",null,"3300 / 2700","as existing","7800 / 7000","Required",750,"Contractor to Specify for approval","D1.1ev","early years","D1.1ev","early years",null,"Access control system to be agreed with school","F3.2i","classroom non-slip","C1.1","general","W1.1","general","Carpet mat to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,16]
["PRI13","Reception classrooms","Reception classrooms","PRI13","PRI13","New Build","SL_25_10_72","Reception classrooms","Primary school classroom for a range of FF&E layout options and activities for Reception pupils","Computer based play. Group discussion. Quiet time. Range of play activities. Role play. Sand and water play. Small group work. Solitary play. Using the whiteboard.","Basic teaching","General",1.5,4,"D","standard",5,1.9,null,1,62,30,30,1,33,"4-5","None","Disabled access into the space required","Enclosed or semi-enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Required",750,"Contractor to Specify for approval","D1.1ev","early years","D1.1ev","early years",null,"Access control system to be agreed with school","F3.2i","classroom non-slip","C1.1","general","W1.1","general","Carpet mat to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,16]
["PRI15","Reception classrooms (extensive)","Reception classrooms (extensive)","PRI15","PRI13","New Build","SL_25_10_72","Reception classrooms","Primary school classroom suitable for all classroom layout options and activities for Reception pupils","Computer based play. Group discussion. Quiet time. Range of play activities. Role play. Sand and water play. Small group work. Solitary play. Using the whiteboard.","Basic teaching","General",1.5,4,"E","extensive",6,2.1,null,1,69,30,30,1,33,"4-5","None","Disabled access into the space required","Enclosed or semi-enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Required",750,"Contractor to Specify for approval","D1.1ev","early years","D1.1ev","early years",null,"Access control system to be agreed with school","F3.2i","classroom non-slip","C1.1","general","W1.1","general","Carpet mat to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,16]
["PRI21","Infant classrooms (restrictive, extg)","Infant classrooms (restrictive, extg)","PRI21","PRI23","Existing","SL_25_10_39","Infant classrooms","Existing primary school classroom for limited layout options and activities for infant (Key Stage 1) pupils","Activity based play. Circle time. Group discussion. Range of play activities. Small group teaching. Small group work. Using ICT devices. Using the whiteboard. Whole class shared activity.","Basic teaching","General",1.5,4,"B","restrictive",2,1.6,null,1,50,30,30,1,33,"5-7","None","Full disabled access not required","Enclosed",null,"3300 / 2700","as existing","7800 / 7000","Required",750,"Contractor to Specify for approval","D1.1ev","early years","N/A","no internal doorset required",null,null,"F3.2i","classroom non-slip","C1.1","general","W1.1","general","Carpet mat to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,16]
["PRI23","Infant classrooms","Infant classrooms","PRI23","PRI23","New Build","SL_25_10_39","Infant classrooms","Primary school classroom for a range of FF&E layout options and activities for infant (Key Stage 1) pupils","Activity based play. Circle time. Group discussion. Range of play activities. Small group teaching. Small group work. Using ICT devices. Using the whiteboard. Whole class shared activity.","Basic teaching","General",1.5,4,"C","standard",4,1.7,null,1,55,30,30,1,33,"5-7","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Required",750,"Contractor to Specify for approval","D1.1ev","early years","N/A","no internal doorset required",null,null,"F3.2i","classroom non-slip","C1.1","general","W1.1","general","Carpet mat to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,16]
["PRI25","Infant classrooms (extensive)","Infant classrooms (extensive)","PRI25","PRI23","New Build","SL_25_10_39","Infant classrooms","Primary school classroom suitable for all classroom layout options and wet and dry activities for infant (Key Stage 1) pupils","Activity based play. Circle time. Group discussion. Range of play activities. Small group teaching. Small group work. Using ICT devices. Using the whiteboard. Whole class shared activity.","Basic teaching","General",1.5,4,"D","extensive",5,1.9,null,1,62,30,30,1,33,"5-7","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Required",750,"Contractor to Specify for approval","D1.1ev","early years","N/A","no internal doorset required",null,null,"F3.2i","classroom non-slip","C1.1","general","W1.1","general","Carpet mat to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,32]
["PRI31","Junior classrooms (restrictive, extg)","Junior classrooms (restrictive, extg)","PRI31","PRI33","Existing","SL_25_10_44","Junior classrooms","Primary school classroom for limited layout options and activities for junior (Key Stage 2) pupils","Group activities. Group discussion. Independent study and research. Presentations. Use of ICT. Using the whiteboard. ","Basic teaching","General",1.5,4,"B","restrictive",2,1.6,null,1,50,30,30,1,33,"7-11","None","Full disabled access not required","Enclosed",null,"3300 / 2700","as existing","7800 / 7000","Not required",750,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1m","mixed general","C1.1","general","W1.1","general","Carpet to part of area to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,32]
["PRI33","Junior classrooms","Junior classrooms","PRI33","PRI33","New Build","SL_25_10_44","Junior classrooms","Primary school classroom for a range of FF&E layout options and wet and dry activities for junior (Key Stage 2) pupils","Group activities. Group discussion. Independent study and research. Presentations. Use of ICT. Using the whiteboard. ","Basic teaching","General",1.5,4,"C","standard",4,1.7,null,1,55,30,30,1,33,"7-11","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Not required",750,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1m","mixed general","C1.1","general","W1.1","general","Carpet to part of area to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,32]
["PRI35","Junior classrooms (extensive)","Junior classrooms (extensive)","PRI35","PRI33","New Build","SL_25_10_44","Junior classrooms","Primary school classroom suitable for all classroom layout options and activities for junior (Key Stage 2) pupils","Group activities. Group discussion. Independent study and research. Presentations. Use of ICT. Using the whiteboard. ","Basic teaching","General",1.5,4,"C","extensive",4,1.7,null,1,62,34,34,1,38,"7-11","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Not required",750,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1m","mixed general","C1.1","general","W1.1","general","Carpet to part of area to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",10,2,32]
["PRI37","Junior classrooms (group rooms)","Junior classrooms (group rooms)","PRI37","PRI33","New Build","SL_25_10_44","Junior classrooms","Room for assistance with individuals and small groups, and for table-based activities in larger groups","Group activities. Group discussion. Independent study and research. Presentations. Use of ICT. Using the whiteboard. ","Basic teaching","General",1.5,4,"B","standard",2,1.6,null,1,34,20,20,1,22,"7-11","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Not required",750,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general","Carpet to part of area to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",8,2,12]
["PRI38","Junior classrooms (without sink)","Junior classrooms (without sink)","PRI38","PRI33","New Build","SL_25_10_44","Junior classrooms","Primary school classroom for a range of FF&E layout options and dry activities for junior (Key Stage 2) pupils","Group activities. Group discussion. Independent study and research. Presentations. Use of ICT. Using the whiteboard. ","Basic teaching","General",1.5,4,"D","standard",5,1.9,null,1,55,26,26,1,29,"7-11","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Not required",750,"","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general","Carpet to part of area to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","No sink but hot and cold drinking water supply capped off for future use",10,2,32]
["PRI41","Semi-open classbases, infant","Semi-open classbases, infant","PRI41","PRI41","New Build","SL_25_10_77","Semi-open classbases","Primary school semi-open classbase for limited activities including water-based, typically for infant (KS1), with easy access to a shared teaching area without sink","Activity based play (typically for infants). Circle time. Group discussion. Range of play activities including water-based. Small group teaching. Small group work. Using ICT devices. Using the whiteboard. Whole class shared activity.","Basic teaching","General",1.5,4,"B","standard",2,1.6,null,1,50,30,30,1,33,"4-7","None","Disabled access into the space required","Semi-enclosed","adjacent to Shared teaching area","3300 / 2700","2400 / N/A","7800 / 7000","Required",750,"Contractor to Specify for approval","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F3.2i","classroom non-slip","C1.1","general","W1.1","general","Carpet mat to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","Hot and cold water to sink listed in School-specific SoA and ADS",10,2,32]
["PRI43","Semi-open classbases (junior, extg)","Semi-open classbases (junior, extg)","PRI43","PRI41","Existing","SL_25_10_77","Semi-open classbases","Primary school semi-open classbase for limited activities, for junior (KS2), with easy access to a shared teaching area with sink","Activity based play (typically for junior). Circle time. Group discussion. Range of play activities not including water-based. Small group teaching. Small group work. Using ICT devices. Using the whiteboard. Whole class shared activity.","Basic teaching","General",1.5,4,"B","standard",2,1.6,null,1,50,30,30,1,33,"7-11","None","Disabled access into the space required","Semi-enclosed","adjacent to Shared teaching area","3300 / 2700","as existing","7800 / 7000","Required",750,"Contractor to Specify for approval","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F3.2i","classroom non-slip","C1.1","general","W1.1","general","Carpet mat to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","as existing",10,2,32]
["PRI50","Nursery playrooms (ambulant)","Nursery playrooms (ambulant)","PRI50","PRI03","New Build","SL_25_10_57","Nursery playrooms","Primary playroom for a range of FF&E layout options and activities for ambulant 3 to 4 year olds needing additional support","Group discussion. Using the whiteboard. Role play. Range of play activities. Quiet time. Small group work. Sand and water play. Solitary play. Computer-based play.","Basic teaching","General",1.5,4,"H","SEN",16,3.3,null,1,55,12,12,1,14,"3-4","None","Disabled access into the space required","Enclosed or semi-enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Required, fully glazed",750,"Contractor to Specify for approval","D1.1ev","early years","D1.1ev","early years",null,"Access control system to be agreed with school","F3.2i","classroom non-slip","C1.1","general","W1.1","general","Carpet mat to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",4,0,32]
["PRI55","Nursery playrooms, non-ambulant","nursery playroom (non-ambulant)","PRI55","PRI55","New Build","SL_25_10_57","Nursery playrooms","Primary playroom for a range of FF&E layout options and activities for ambulant and non-ambulant 3 to 4 year olds needing significant additional support and specialist equipment","Group discussion. Using the whiteboard. Role play. Range of play activities. Quiet time. Small group work. Sand and water play. Solitary play. Computer-based play.","Basic teaching","General",1.5,4,"J","SEN",28,4.2,null,1,62,8,8,1,9,"3-4","None","Full disabled access required","Enclosed or semi-enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Required",750,"Contractor to Specify for approval","D6.1mv","special wide","D6.1mv","special wide",null,"Ergonomic handle and access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1","general","Ceiling to include hoist tracking in both directions, avoiding light fittings","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5/T7","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",4,0,32]
["PRI60","Reception classrooms (ambulant)","reception classroom (ambulant)","PRI60","PRI13","New Build","SL_25_10_72","Reception classrooms","Primary classroom for a range of FF&E layout options and activities for ambulant Reception pupils needing additional support","Supported individual and group play including computer based. Role play. Sand and water play. Using the whiteboard.","Basic teaching","General",1.5,4,"H","SEN",16,3.3,null,1,55,12,12,1,14,"4-5","None","Disabled access into the space required","Enclosed or semi-enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Required",750,"Contractor to Specify for approval","D1.1ev","early years","D1.1ev","early years",null,"Access control system to be agreed with school","F3.2i","classroom non-slip","C1.1","general","W1.1","general","Carpet mat to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",4,0,32]
["PRI65","Reception classrooms, non-ambulant","reception classroom (non-ambulant)","PRI65","PRI65","New Build","SL_25_10_72","Reception classrooms","Primary playroom for a range of FF&E layout options and activities for ambulant and non-ambulant Reception pupils needing significant additional support and specialist equipment","Supported individual and group play including computer based. Role play. Sand and water play. Using the whiteboard.","Basic teaching","General",1.5,4,"J","SEN",28,4.2,null,1,62,8,8,1,9,"4-5","None","Full disabled access required","Enclosed or semi-enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Required",750,"Contractor to Specify for approval","D6.1mv","special wide","D6.1mv","special wide",null,"Ergonomic handle and access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1","general","Ceiling to include hoist tracking in both directions, avoiding light fittings","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5/T7","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",6,0,32]
["PRI70","Primary SEN classrooms (ambulant)","Primary SEN classrooms (ambulant)","PRI70","PRI70","New Build","SL_25_10_68","Primary SEN classrooms","Primary classroom for a range of FF&E layout options and activities for ambulant pupils needing additional support ","Supported individual and group working including with ICT. Role play. Using the whiteboard.","Basic teaching","General",1.5,4,"G1","SEN",12,3.1,null,1,55,"As SoA",14,1,16,"4-11","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Optional",750,"Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,"Access control system to be agreed with school. Finger guards","F3.2i","classroom non-slip","C1.1","general","W1.1","general","Carpet mat to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",6,0,32]
["PRI71","Primary SEN classrooms (AP health)","Primary SEN classrooms (health)","PRI71","PRI70","New Build","SL_25_10_68","Primary SEN classrooms","Primary classroom for a range of FF&E layout options and activities for ambulant pupils needing additional support ","Supported individual and group working including with ICT. Role play. Using the whiteboard.","Basic teaching","General",1.5,4,"F1","SEN",9,2.7,null,1,32,8,9,1,10,"4-11","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Optional",750,"Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,"Doorset, including ironmongery, finger guards and access control system to be agreed with school","F3.2i","classroom non-slip","C1.1","general","W1.1","general","Carpet mat to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",6,0,32]
["PRI72","Primary SEN classrooms (AP behaviour)","Primary SEN classrooms (behaviour)","PRI72","PRI70","New Build","SL_25_10_68","Primary SEN classrooms","Primary classroom for a range of FF&E layout options and activities for ambulant pupils needing additional support ","Supported individual and group working including with ICT. Role play. Using the whiteboard.","Basic teaching","General",1.5,4,"G1","SEN",12,3.1,null,1,41,8,9,1,10,"4-11","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Optional",750,"Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,"Doorset, including ironmongery, finger guards and access control system, to be agreed with school","F3.2i","classroom non-slip","C1.1","general","W1.1","general","Carpet mat to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",6,0,32]
["PRI73","Primary SEN classrooms (with quiet space)","Primary SEN classrooms (with quiet bay off)","PRI73","PRI70","New Build","SL_25_10_68","Primary SEN classrooms","Primary classroom for a range of FF&E layout options and activities for ambulant pupils needing additional support ","Supported individual and group working including with ICT. Role play. Using the whiteboard.","Basic teaching","General",1.5,4,"H","SEN",16,3.3,null,1,48,8,10,1,11,"4-11","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Optional",750,"Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,"Doorset, including ironmongery and access control system, to be agreed with school. Finger guards","F3.2i","classroom non-slip","C1.1","general","W1.1","general","Carpet mat to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",6,0,32]
["PRI74","Primary SEN classrooms (severe suite)","Primary SEN classrooms (in suite)","PRI74","PRI70","New Build","SL_25_10_68","Primary SEN classrooms","Primary classroom for a range of FF&E layout options and activities for ambulant pupils needing additional support ","Supported individual and group working including with ICT. Role play. Using the whiteboard.","Basic teaching","General",1.5,4,"I","SEN",22,3.7,null,1,48,6,7,1,8,"4-11","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Optional",750,"Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,"Doorset, including ironmongery and access control system, to be agreed with school. Finger guards","F3.2i","classroom non-slip","C1.1","general","W1.1","general","Carpet mat to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",6,0,32]
["PRI75","Primary SEN classrooms, non-ambulant","primary classroom (non-ambulant)","PRI75","PRI75","New Build","SL_25_10_68","Primary SEN classrooms","Primary classroom for a range of FF&E layout options and activities for ambulant and non-ambulant pupils needing significant additional support and specialist equipment","Supported individual and group working including with ICT. Role play. Using the whiteboard.","Basic teaching","General",1.5,4,"J1","SEN",32,4.4000000000000004,null,1,62,6,7,1,8,"4-11","None","Full disabled access required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Optional",750,"Contractor to Specify for approval if provided","D6.1mv","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1","general","Ceiling to include hoist tracking in both directions, avoiding light fittings","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5/T7","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",6,0,32]
["PRI78","Primary SEN classrooms, PMLD suite",null,null,"PRI75","New Build","SL_25_10_68","Primary SEN classrooms","Primary classroom for a range of FF&E layout options and activities for non-ambulant pupils needing significant additional support and specialist equipment","Supported individual and group working including with ICT. Role play. Using the whiteboard.","Basic teaching","General",1.5,4,"J1","SEN",32,4.4000000000000004,null,1,62,6,7,1,8,"4-11","None","Full disabled access required","Enclosed",null,"3300 / 2700","2400 / N/A","7800 / 7000","Optional",750,"Contractor to Specify for approval if provided","D6.1mv","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school. Finger guards","F1.1h","special general","C1.1","general","W1.1","general","Ceiling to include hoist tracking in both directions, avoiding light fittings","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5/T7","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",6,0,32]
["PRI80","Semi-open classbases, ambulant","Semi-open classbases, ambulant","PRI80","PRI80","New Build","SL_25_10_77","Semi-open classbases","Primary semi-open classbase for ambulant pupils, for limited activities including water-based, with easy access to a shared teaching area without sink, typically for infant (KS1)","Supported individual and group working including with ICT. Role play. Using the whiteboard.","Basic teaching","General",1.5,4,"G1","SEN",12,3.1,null,1,55,12,14,1,16,"4-11","None","Disabled access into the space required","Semi-enclosed","adjacent to Shared teaching area","3300 / 2700","2400 / N/A","7800 / 7000","Optional",750,"Contractor to Specify for approval if provided","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F3.2i","classroom non-slip","C1.1","general","W1.1","general","Carpet mat to suit FF&E layout ","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold water to sink listed in School-specific SoA and ADS",6,0,32]
["PRI85","Semi-open classbases, non-ambulant","Semi-open classbases, non-ambulant","PRI85","PRI85","New Build","SL_25_10_77","Semi-open classbases","Primary semi-open classbase for ambulant and non-ambulant pupils needing significant additional support and specialist equipment, for limited activities, with easy access to a shared teaching area with sink","Supported individual and group working including with ICT. Role play. Using the whiteboard.","Basic teaching","General",1.5,4,"J1","SEN",32,4.4000000000000004,null,1,62,6,7,1,8,"4-11","None","Full disabled access required","Semi-enclosed","adjacent to Shared teaching area","3300 / 2700","2400 / N/A","7800 / 7000","Optional",750,"Contractor to Specify for approval if provided","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F1.1h","special general","C1.1","general","W1.1","general","Ceiling to include hoist tracking in both directions, avoiding light fittings","L1.2a","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",300,"man on, day dim, abs off","No",null,"T5/T7","Average*","Low*","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold water to sink listed in School-specific SoA and ADS",6,0,32]
["RES00","Small group rooms","Small group rooms","RES00","RES00","New Build","SL_25_75_80","Small group rooms","Room for assistance with individuals and small groups ","Individual/ small group learning support. One to one counselling. Privacy required.","Learning resources","General",1.5,4,"B","standard",2,1.6,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,"Finger guards if used by Early Years or infant pupils, or pupils with SEN","F1.1","general","C1.1","general","W1.1","general","Floor to be hygienic if used by Early Years pupils or pupil with SEN","L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","None",6,2,16]
["RES01","Small group rooms (nursery)","Small group rooms (nursery)","RES01","RES00","New Build","SL_25_75_80","Small group rooms","Small room for assistance with individuals and small groups ","Individual/ small group learning support. One to one counselling. ","Learning resources","General",1.5,4,"B","standard",2,1.6,null,0,9,4,4,0,5,"2-4","None","Disabled access into the space required","Enclosed","adjacent to Nursery playroom(s)","2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,"Finger guards if used by Early Years or infant pupils, or pupils with SEN","F1.1","general","C1.1","general","W1.1","general","Floor to be hygienic if used by Early Years pupils or pupil with SEN","L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","None",6,2,8]
["RES03","Small group rooms (medium)","Small group rooms (medium)","RES03","RES00","New Build","SL_25_75_80","Small group rooms","Room for assistance with individuals and groups needing support","Individual/ small group learning support. One to one counselling. Privacy required.","Learning resources","General",1.5,4,"B","standard",2,1.6,null,0,12,6,6,0,7,"CTS","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,"Finger guards if used by Early Years or infant pupils, or pupils with SEN","F1.1","general","C1.1","general","W1.1","general","Floor to be hygienic if used by Early Years pupils or pupil with SEN","L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","None",6,2,12]
["RES04","Small group rooms (large SEN etc.)","Small group rooms (large SEN etc.)","RES04","RES00","New Build","SL_25_75_80","Small group rooms","Larger room for assistance with individuals and groups, typically with SEN","Individual/ small group learning support. One to one counselling. Privacy required.","Learning resources","General",1.5,4,"B","standard",2,1.6,null,0,16,9,9,0,10,"CTS","None","Full disabled access required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,"Finger guards if used by Early Years or infant pupils, or pupils with SEN","F1.1","general","C1.1","general","W1.1","general","Floor to be hygienic if used by Early Years pupils or pupil with SEN","L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","None",6,2,16]
["RES05","Shared teaching areas, secondary","Shared teaching areas, secondary","RES05","RES05","New Build","SL_25_10_79","Shared teaching areas","Open area for assistance with individuals and groups  ","Individual/ small group learning support. Optional role play","Learning resources","General",1.5,4,"B","standard",2,1.6,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access into the space required","Semi-enclosed or open plan","adjacent to Semi-open classbases","2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Average","Medium","<=0.5","<=0.5","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","None",8,2,8]
["RES06","Small group room (inclusion/ withdrawal)","Small group room (inclusion/ withdrawal)","RES06","RES00","New Build","SL_25_75_80","Small group rooms","Small room for assistance with individuals and groups with SEN ","Individual therapy and counselling. Individual/small group learning support. Staff meetings.","Learning resources","General",1.5,4,"B","-",2,1.6,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access into the space required","Enclosed or semi-enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","N/A","","D1.1av","general","D1.1av","general",null,"Finger guards if used by Early Years or infant pupils, or pupils with SEN","F1.1","general","C1.1","general","W1.1","general","Floor to be hygienic if used by Early Years pupils or pupil with SEN","L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Average","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Dado on 2 walls","None",8,2,8]
["RES12","Music practice rooms","Music practice rooms","RES12","RES12","New Build","SL_25_75_55","Music practice rooms","Room for music practice/ lessons","Individual music lessons. Individuals/small groups composing and practising music using a variety of percussion instruments and electronic keyboard.","Learning resources","General",1.5,4,"B","standard",2,1.6,null,0,8,4,4,0,5,"11-19","None","Disabled access into the space required","Enclosed","in Music practice suite","2400 / N/A","2400 / N/A","N/A / 1700","Not required","N/A","","D1.1av","general","N/A","no internal doorset required",null,"Finger guards if used by Early Years or infant pupils, or pupils with SEN","F1.1","general","C1.1","general","W1.1","general","Angled wall panels may be required to achieve required sound quality. ","L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Very high","Low","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Where required","None",3,0,4]
["RES13","Music practice rooms (extensive)","Music practice rooms (extensive)","RES13","RES12","New Build","SL_25_75_55","Music practice rooms","Room for music practice/ lesson, including drums","Individual music lessons. Individual/small groups composing and practising music using a variety of percussion instruments, full drum kit and electronic keyboard.","Learning resources","General",1.5,4,"C","extensive",4,1.7,null,0,16,7,7,0,8,"11-19","None","Disabled access into the space required","Enclosed","in Music practice suite","2400 / N/A","2400 / N/A","N/A / 1700","Not required","N/A","","D1.1av","general","N/A","no internal doorset required",null,"Finger guards if used by Early Years or infant pupils, or pupils with SEN","F1.1","general","C1.1","general","W1.1","general","Angled wall panels may be required to achieve required sound quality. ","L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Very high","Low","<=0.6","<=0.8","Ventilation as Tech Annex 2F 5.1","None","Where required","None",3,0,6]
["RES14","Recording control spaces","Recording control spaces","RES14","RES14","New Build","SL_40_65_70","Recording control spaces","Room housing specialist recording equipment","Using analogue or digital equipment to record music played in adjacent space(s) and to create/edit digital music.","Learning resources","Fitted",2,4,"B","standard",2,1.6,null,0,8,4,4,0,5,"11-19","None","Disabled access into the space required","Enclosed","adjacent to music room(s)","2400 / N/A","2400 / N/A","N/A / 1700","Not required","N/A","","D1.1av","general","D1.1av","general",null,"Optional internal window to be provided to adjacent recording space (music room or recording studio). Finger guards if used by pupils with SEN","F1.1","general","C1.1","general","W1.1","general","Angled wall panels and sound-absorbing panels may be required to achieve required sound quality. ","L6.5g","Daylight to be excluded or blinds provided","Daylight to be excluded or blinds provided","Not applicable","Not applicable",300,"man on, man off","No",null,"T5","High","Low","<=0.5","<=0.6",null,"None","To suit equipment","None",11,2,4]
["RES15","Music practice rooms (recording)","Music practice rooms (recording)","RES15","RES12","New Build","SL_25_75_55","Music practice rooms","Room for recording music and music practice/ lessons","Using analogue or digital equipment to record sound in adjacent space.","Learning resources","Fitted",2,4,"B","standard",2,1.6,null,0,9,4,4,0,5,"11-19","None","Disabled access into the space required","Enclosed","adjacent to Recording control space","2400 / N/A","2400 / N/A","N/A / 1700","Not required","N/A","","D1.1av","general","N/A","no internal doorset required",null,"Finger guards if used by Early Years or infant pupils, or pupils with SEN","F1.1","general","C1.1","general","W1.1","general","Angled wall panels may be required to achieve required sound quality. ","L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Very high","Low","0.6 - 1.2","0.6 - 1.2",null,"None","Where required","None",11,2,4]
["RES16","Lighting and audio control spaces","Lighting and audio control spaces","RES16","RES16","New Build","SL_40_65_47","Lighting and audio control spaces","Room for controlling lighting and audio systems in adjacent performance space","Using analogue or digital equipment to control stage lighting and sound system in adjacent hall.","Learning resources","Fitted",2,4,"B","standard",2,1.6,null,0,6,3,3,0,4,"11-19","None","Disabled access into the space preferred","Enclosed","at back of Assembly hall","2400 / N/A","2400 / N/A","N/A / 1700","Not required","N/A","","D1.1av","general","D1.1av","general",null,"Glazed viewing screen to be provided to allow view of performance area in adjacent main hall. Finger guards if used by pupils with SEN","F1.1","general","C1.1","general","W1.1","general","Dark coloured wall finishes","L6.5g","Daylight to be excluded or blinds provided","Daylight to be excluded or blinds provided","Not applicable","Not applicable",300,"man on, man off","Yes",null,"T5","Average","Medium","<=0.8","<=1.0",null,"None","To suit equipment","None",11,2,8]
["RES21","Heavy practical resource (kiln)","Heavy practical resource (kiln)","RES21","RES21","New Build","SL_25_75_37","Heavy practical resource spaces","Room for kiln(s) and drying racks","Firing and glazing articles in kiln(s). Storing clay articles awaiting firing.","Learning resources","Heavy practical (workshop)",3.5,4,"-","standard",0,0,null,0,4,"-","-",0,"As SoA","11-19","None","Disabled access not required, trolley access required","Enclosed","off Art room","2400 / N/A","2400 / N/A","N/A / 1350","Not required","N/A","","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room. Finger guards if used by pupils with SEN","F5.4","heavy practical","C1.1","general","W4.1","rough","Flooring suitable for heavy movable FF&E on castors ","L5.5b","No requirement","No requirement","Not applicable","Not applicable",300,"man on, man off","No",null,"T5","N/A","N/A","N/A","N/A","Extract required for specialist equipment to satisfy manufacturer's requirements. Sufficient space around back of kiln to allow for air movement and servicing. ","Optional","To suit equipment","To suit equipment",11,0,0,"Warning light to indicate firing required; should not be possible to open kiln door during firing."]
["RES22","Darkrooms","Darkrooms","RES22","RES22","New Build","SL_25_30_21","Darkrooms","Specialist light-tight dark room for photograph developing","Processing and developing photographs using traditional techniques.","Learning resources","Light practical",2.5,4,"B","standard",2,1.6,null,0,9,4,4,0,5,"11-19","None","Disabled access into the space preferred","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / 2400","Not required","N/A","","D4.1a","store room","N/A","no internal doorset required",null,"All-round light-tight seals on door required in normal operation, to ensure no light leakage. Ironmongery to include internal escape mechanism","F3.4","chemical resistant non-slip","C1.1","general","W1.1","general","Flooring suitable for heavy movable FF&E on castors. Dark coloured wall finishes","L6.5e","Daylight to be excluded or blinds provided","Daylight to be excluded or blinds provided","Not applicable","Not applicable",300,"man on, man off","Yes","Separately-switched photographic safe light(s) in room and indicator light on outside required","T5","Low","Medium","<=1.0","<=1.0","Ventilation can be variable but must be able to extract at 5ach when required.  ","None","To suit equipment","Cold water to wet serviced bollards or similar listed under FF&E, hot and cold to belfast or hand wash sink; chemically resistance drainage.",3,2,4,"Locked cupboards to be provided for chemicals"]
["RES23","Light practical resource (art/ design)","Light practical resource (art/ design)","RES23","RES23","New Build","SL_25_75_47","Light practical resource spaces","Art resource room for sixth form pupils and display","Individual and group 2D work (drawing, painting). Individual and group pupil led discussions. Small scale 3D work using a range of materials including card, plastic and wood. Some pupil research occasionally using ICT. ","Learning resources","Light practical",2.5,4,"F","standard",8,2.5,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access into the space preferred","Enclosed or semi-enclosed",null,"2700 / 2400 (3300 / 2700 if >27m2)","2400 / N/A","N/A / 3400","Optional","N/A","Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,"Finger guards if used by Early Years or infant pupils, or pupils with SEN","F3.4","chemical resistant non-slip","C1.1","general","W1.1","general",null,"L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=0.8","<=1.0",null,"None","Where required","To suit equipment",16,2,8]
["RES31","ICT resource spaces, open","ICT resource spaces, open","RES31","RES31","New Build","SL_25_75_40","ICT resource spaces","Shared resource area for the design and technology suite","Individual and group work. Small scale 3D work using a range of materials including card, plastic and wood. Some pupil research occasionally using ICT. ","Learning resources","Fitted",2,4,"D","standard",5,1.9,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access into the space preferred","Enclosed or semi-enclosed",null,"2700 / 2400 (3300 / 2700 if >27m2)","2400 / N/A","N/A / 3400","Optional","N/A","Contractor to Specify for approval if provided","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W1.1","general",null,"L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=0.8","<=1.0",null,"None","To suit ICT","None",32,2,12]
["RES32","Heavy practical resource (heat treatment, extg)","Heavy practical resource (heat treatment, extg)","RES32","RES32","Existing","SL_25_75_37","Heavy practical resource spaces","Existing space for heat treatment equipment, associated with workshop(s)","Making with metals (including heat treatment). Teacher demonstrations using equipment.","Learning resources","Heavy practical (workshop)",3.5,4,"F","standard",8,2.5,null,0,"As SoA","As SoA","As SoA",0,"As SoA","11-19","None","Full disabled access not required","Enclosed or semi-enclosed",null,"3300 / 2700","as existing","as existing","Not required","N/A","","D2.1av","strong","N/A","no internal doorset required",null,"Finger guards if used by Early Years or infant pupils, or pupils with SEN","F5.4","heavy practical","C1.1","general","W4.1","rough",null,"L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","High","High","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.5 and 7.6","Bottled gas only","To suit equipment","To suit equipment",0,null,6]
["RES33","Heavy practical resource (CAD CAM, extg)","Heavy practical resource (CAD CAM, extg)","RES33","RES33","Existing","SL_25_75_37","Heavy practical resource spaces","Existing space for CADCAM machines, associated with workshop(s)","Making and teacher demonstrations with CAD CAM machines, linked to computer based design.","Learning resources","Heavy practical (workshop)",3.5,4,"F","standard",8,2.5,null,0,"As SoA","As SoA","As SoA",0,"As SoA","11-19","None","Full disabled access not required","Enclosed or semi-enclosed",null,"3300 / 2700","as existing","as existing","Not required","N/A","","D2.1av","strong","N/A","no internal doorset required",null,"Finger guards if used by Early Years or infant pupils, or pupils with SEN","F5.4","heavy practical","C1.1","general","W4.1","rough",null,"L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","Yes",null,"T5","High","High","<=0.8","<=1.0","Extract ventilation based on Tech Annex 2F 7.5 and 7.6","None","To suit equipment","To suit equipment",0,2,18]
["RES50","Small group rooms (ambulant)","Small group rooms (ambulant)","RES50","RES00","New Build","SL_25_75_80","Small group rooms","Room for assistance with individuals or small groups or for individual 'time out', for ambulant pupils","Individual/ small group learning support. One to one counselling. Privacy required.","Learning resources","General",1.5,4,"B","SEN",2,1.6,null,1,"As SoA","As SoA","As SoA",1,"As SoA","CTS","None","Disabled access into the space required","Enclosed",null,"2700 / 2400",2400,"N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,"Finger guards if used by Early Years or infant pupils, or pupils with SEN","F1.1","general","C1.1","general","W1.1","general","Floor to be hygienic if used by Early Years pupils or pupils with SEN","L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","None",6,2,16]
["RES55","Small group rooms (non-ambulant)","group room (non-ambulant)","RES55","RES55","New Build","SL_25_75_80","Small group rooms","Room for assistance with individuals or small groups or for individual 'time out', for ambulant and non-ambulant pupils","Individual/ small group learning support. One to one counselling. Privacy required.","Learning resources","General",1.5,4,"G","SEN",10,2.9,null,0,15,2,2,0,3,"CTS","None","Full disabled access required","Enclosed",null,"2700 / 2400","2700 / 2400","N/A / 1700","Not required","CTS","","D6.1mv","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1","general",null,"L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5/T7","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","None",6,2,16]
["RES56","Shared teaching areas, secondary (ambulant)","Shared teaching areas, secondary (ambulant)","RES56","RES05","New Build","SL_25_10_79","Shared teaching areas","Open area for assistance with individuals and groups  ","Individual/ small group learning support. One to one counselling. Privacy required.","Learning resources","General",1.5,4,"B","SEN",2,1.6,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access into the space preferred","Semi-enclosed or open plan",null,"2700 / 2400",2400,"N/A / 1700","Not required","CTS","","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","None",6,2,16]
["RES60","Independent life skills rooms (ambulant)","Independent life skills rooms (ambulant)","RES60","RES60","New Build","SL_25_40_42","Independent life skills rooms","Room for learning domestic skills including bed-making, cleaning, cooking and washing in a domestic environment, for secondary-age ambulant pupils","Pupil practice in life skills including cleaning and bedmaking","Learning resources","Light practical",2.5,4,"F","SEN",8,2.5,null,0,18,4,4,0,5,"11-19","None","Disabled access into the space required","Enclosed or semi-enclosed",null,"2700 / 2400",2400,"7800 / 7000","Optional","CTS","Contractor to Specify for approval if provided","D2.2av","strong","N/A","no internal doorset required",null,"Access control system and finger guards to be agreed with school.","F3.4h","hygienic non-slip","C1.2","humid areas","W3.2","humid","Flooring to suit range of activities ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","Appliances","To suit equipment","Hot and cold drinking water to all sinks, equipment and appliances",2,null,4]
["RES65","Independent life skills rooms, non-ambulant","life skills kitchen/ living room (non-ambulant)","RES65","RES65","New Build","SL_25_40_42","Independent life skills rooms","Room for learning domestic skills including bed-making, cleaning, cooking and washing in a domestic environment, for secondary-age ambulant and non-ambulant pupils","Pupil practice in life skills including cleaning and bedmaking","Learning resources","Light practical",2.5,4,"H","SEN",16,3.3,null,0,25,3,3,0,4,"11-19","None","Full disabled access required","Enclosed or semi-enclosed",null,"2700 / 2400",2400,"7800 / 7000","Optional","CTS","Contractor to Specify for approval if provided","D6.2mv","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F3.4h","hygienic non-slip","C1.2","humid areas","W3.2","humid","Flooring to suit range of activities ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5/T7","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","Appliances","To suit equipment","Hot and cold drinking water to all sinks, equipment and appliances",2,null,4]
["RES80","SEN resource spaces, role play","SEN resource spaces, role play","RES80","RES80","New Build","SL_25_75_82","SEN resource spaces","Room suitable to be used for role play for ambulant pupils","Individual/ small group learning support. Role play such as shop or doctor's surgery.","Learning resources","General",1.5,4,"C","SEN",4,1.7,null,0,12,5,5,0,6,"CTS","None","Disabled access into the space required","Enclosed or semi-enclosed",null,"2700 / 2400",2400,"N/A / 1700","Not required","CTS","","D1.1ev","early years","N/A","no internal doorset required",null,"Access control system to be agreed with school. Option of shop window","F1.1h","special general","C1.1","general","W1.1","general","Flooring to suit range of activities ","L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No","Manual dimming to main lighting required.","T5","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit equipment","Hot and cold drinking water to all sinks, equipment and appliances",2,null,4]
["SCI01","Science studios (restrictive, extg)","Science studios (restrictive, extg)","SCI01","SCI02","Existing","SL_25_10_74","Science studios","Existing secondary school science classroom for demonstration and classwork","Group discussion. Independent research and recording. Presentations. Simple supervised experiments and evaluation exercises. Teacher demonstration of experiments. Using the whiteboard.","Basic teaching","Light practical (science)",2.5,4,"D","restrictive",5,1.9,null,1,62,30,30,1,33,"11-19","None","Full disabled access not required","Enclosed",null,"3300 / 2700","as existing","7800 / 7500","Not required",1050,"","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Low","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 7.7","Double gas taps to all bollards listed on FF&E list (as specified in Annex 3: FF&E)","Dado on 2 walls","Cold water to wet serviced bollards or similar listed under FF&E, hot and cold to belfast or hand wash sink; chemically resistance drainage.",10,2,16,"Means to isolate gas supply and isolate power. Alternative exit in emergency (e.g. to adjacent room)."]
["SCI02","Science studios","Science studios","SCI02","SCI02","New Build","SL_25_10_74","Science studios","Secondary school science room for demonstration and light experiments","Group discussion. Independent research and recording. Presentations. Simple supervised experiments and evaluation exercises. Teacher demonstration of experiments. Using the whiteboard.","Basic teaching","Light practical (science)",2.5,4,"E","standard",6,2.1,null,1,69,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Low","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 7.7","Double gas taps to all bollards listed on FF&E list (as specified in Annex 3: FF&E)","Dado on 2 walls","Cold water to wet serviced bollards or similar listed under FF&E, hot and cold to belfast or hand wash sink; chemically resistance drainage.",10,2,16,"Means to isolate gas supply and isolate power. Alternative exit in emergency (e.g. to adjacent room)."]
["SCI03","Science studios (extensive)","Science studios (extensive)","SCI03","SCI02","New Build","SL_25_10_74","Science studios","Secondary school science laboratory for demonstration and limited 'hands on' experiments","Group discussion. Independent research and recording. Presentations. Simple supervised experiments and evaluation exercises. Teacher demonstration of experiments. Using the whiteboard.","Basic teaching","Light practical (science)",2.5,4,"E1","extensive",7,2.2999999999999998,null,1,76,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Low","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 7.7","Double gas taps to all bollards listed on FF&E list (as specified in Annex 3: FF&E)","Dado on 2 walls","Cold water to wet serviced bollards or similar listed under FF&E, hot and cold to belfast or hand wash sink; chemically resistance drainage.",10,2,24,"Means to isolate gas supply and isolate power. Alternative exit in emergency (e.g. to adjacent room)."]
["SCI04","Science laboratories (restrictive, extg)","Science laboratories (restrictive, extg)","SCI04","SCI05","Existing","SL_25_10_75","Science laboratories","Existing secondary school science laboratory for demonstration and a wide range of 'hands on' experiments","Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of experiments. Using the whiteboard. Whole class presentations. Wide range of supervised experiments using gas, power and water.","Basic teaching","Light practical (science)",2.5,4,"E1","restrictive",7,2.2999999999999998,null,1,76,30,30,1,33,"11-19","None","Full disabled access not required","Enclosed",null,"3300 / 2700","as existing","7800 / 7500","Not required",1050,"","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Low","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 7.7","Double gas taps to all bollards listed on FF&E list (as specified in Annex 3: FF&E)","Dado on 2 walls","Cold water to wet serviced bollards or similar listed under FF&E, hot and cold to belfast or hand wash sink; chemically resistance drainage.",12,2,24,"Means to isolate gas supply and isolate power. Alternative exit in emergency (e.g. to adjacent room)."]
["SCI05","Science laboratories","Science laboratories","SCI05","SCI05","New Build","SL_25_10_75","Science laboratories","Secondary school science laboratory for demonstration and 'hands on' experiments and fume cupboard","Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of experiments. Using the whiteboard. Whole class presentations. Wide range of supervised experiments using gas, power and water.","Basic teaching","Light practical (science)",2.5,4,"F","standard",8,2.5,null,1,83,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Low","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 7.7","Double gas taps to all bollards listed on FF&E list (as specified in Annex 3: FF&E)","Dado on 2 walls","Cold water to wet serviced bollards or similar listed under FF&E, hot and cold to belfast or hand wash sink; chemically resistance drainage.",12,2,24,"Means to isolate gas supply and isolate power. Alternative exit in emergency (e.g. to adjacent room)."]
["SCI11","science laboratories (specialist)","science laboratories (specialist)","SCI11","SCI05","New Build","SL_25_10_75","Science laboratories","Secondary school science laboratory for demonstration for all types of experiments, up to A-level ","Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of experiments. Using the whiteboard. Whole class presentations. Wide range of supervised experiments using gas, power and water.","Basic teaching","Light practical (science)",2.5,4,"F1","extensive",9,2.7,null,1,97,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Low","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 7.7","Double gas taps to all bollards listed on FF&E list (as specified in Annex 3: FF&E)","Dado on 2 walls","Cold water to wet serviced bollards or similar listed under FF&E, hot and cold to belfast or hand wash sink; chemically resistance drainage.",12,2,24,"Means to isolate gas supply and isolate power. Alternative exit in emergency (e.g. to adjacent room)."]
["SCI12","science laboratories (chemistry)","science laboratories (chemistry)","SCI12","SCI05","New Build","SL_25_10_75","Science laboratories","Secondary school science laboratory for demonstration for all types of chemistry experiments, up to A-level ","Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of experiments. Using the whiteboard. Whole class presentations. Wide range of supervised experiments using gas, power and water.","Basic teaching","Light practical (science)",2.5,4,"F1","extensive",9,2.7,null,1,97,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Low","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 7.7","Double gas taps to all bollards listed on FF&E list (as specified in Annex 3: FF&E)","Dado on 2 walls","Cold water to wet serviced bollards or similar listed under FF&E, hot and cold to belfast or hand wash sink; chemically resistance drainage.",12,2,24,"Means to isolate gas supply and isolate power. Alternative exit in emergency (e.g. to adjacent room)."]
["SCI13","science laboratories (biology)","science laboratories (biology)","SCI13","SCI05","New Build","SL_25_10_75","Science laboratories","Secondary school science laboratory for demonstration for all types of biology experiments, up to A-level ","Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of experiments. Using the whiteboard. Whole class presentations. Wide range of supervised experiments using gas, power and water.","Basic teaching","Light practical (science)",2.5,4,"F1","extensive",9,2.7,null,1,97,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Low","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 7.7","Double gas taps to all bollards listed on FF&E list (as specified in Annex 3: FF&E)","Dado on 2 walls","Cold water to wet serviced bollards or similar listed under FF&E, hot and cold to belfast or hand wash sink; chemically resistance drainage.",12,2,24,"Means to isolate gas supply and isolate power. Alternative exit in emergency (e.g. to adjacent room)."]
["SCI14","science laboratories (physics)","science laboratories (physics)","SCI14","SCI05","New Build","SL_25_10_75","Science laboratories","Secondary school science laboratory for demonstration for all types of physics experiments, up to A-level ","Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of experiments. Using the whiteboard. Whole class presentations. Wide range of supervised experiments using gas, power and water.","Basic teaching","Light practical (science)",2.5,4,"F1","extensive",9,2.7,null,1,97,30,30,1,33,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Low","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 7.7","Double gas taps to all bollards listed on FF&E list (as specified in Annex 3: FF&E)","Dado on 2 walls","Cold water to wet serviced bollards or similar listed under FF&E, hot and cold to belfast or hand wash sink; chemically resistance drainage.",12,2,24,"Means to isolate gas supply and isolate power. Alternative exit in emergency (e.g. to adjacent room)."]
["SCI21","Science studios (large group/ demo)","Science studios (large group/ demo)","SCI21","SCI02","New Build","SL_25_10_74","Science studios","Secondary school science room for demonstration and light experiments","Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of simple experiments. Using the whiteboard. Whole class presentations. ","Basic teaching","Light practical (science)",2.5,4,"A","standard",2,1.1000000000000001,null,1,69,61,61,1,68,"11-19","None","Disabled access into the space required","Enclosed or semi-enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Low","Medium","<=0.8","<=1.0","Ventilation as Tech Annex 2F 7.7","Double gas taps to all bollards listed on FF&E list (as specified in Annex 3: FF&E)","Dado on 2 walls","Cold water to wet serviced bollards or similar listed under FF&E, hot and cold to belfast or hand wash sink; chemically resistance drainage.",10,2,16,"Means to isolate gas supply and isolate power. Alternative exit in emergency (e.g. to adjacent room)."]
["SCI50","Science laboratories (ambulant)","Science laboratories (ambulant)","SCI50","SCI50","New Build","SL_25_10_75","Science laboratories","Specialist secondary space for a range of science activities, for ambulant pupils needing additional support ","Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of simple experiments. Using the whiteboard. Whole class presentations. ","Basic teaching","Light practical (science)",2.5,4,"H","SEN",16,3.3,null,1,"As SoA","As SoA","As SoA",1,"As SoA","11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D1.1av","general","D1.1av","general",null,"Doorset, including ironmongery, finger guards and access control system to be agreed with school","F3.4h","hygienic non-slip","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F 7.7 and 7.8. *Acoustics: see BB93 0.4","Double gas taps to fixed work surfaces listed on FF&E list","Dado on 2 walls","Cold water to wet serviced bollards or similar listed under FF&E, hot and cold to belfast or hand wash sink; chemically resistance drainage.",4,null,16]
["SCI53","Science laboratories (ambulant, fixed)","Science laboratories (autism or SEMH)","SCI53","SCI50","New Build","SL_25_10_75","Science laboratories","Specialist secondary space for a range of science activities, for ambulant pupils needing additional support ","Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of simple experiments. Using the whiteboard. Whole class presentations. ","Basic teaching","Light practical (science)",2.5,4,"I","SEN",22,3.7,null,1,55,8,9,1,10,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D1.1av","general","D1.1av","general",null,"Doorset, including ironmongery, finger guards and access control system to be agreed with school","F3.4h","hygienic non-slip","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F 7.7 and 7.8. *Acoustics: see BB93 0.4","Double gas taps to fixed work surfaces listed on FF&E list","Dado on 2 walls","Cold water to wet serviced bollards or similar listed under FF&E, hot and cold to belfast or hand wash sink; chemically resistance drainage.",4,null,16]
["SCI54","Science laboratories (ambulant, flexible)",null,null,"SCI50","New Build","SL_25_10_75","Science laboratories","Specialist secondary space for a range of science activities, for ambulant pupils needing additional support ","Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of simple experiments. Using the whiteboard. Whole class presentations. ","Basic teaching","Light practical (science)",2.5,4,"H","SEN",16,3.3,null,1,55,12,14,1,16,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D1.1av","general","D1.1av","general",null,"Doorset, including ironmongery, finger guards and access control system to be agreed with school","F3.4h","hygienic non-slip","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F 7.7 and 7.8. *Acoustics: see BB93 0.4","Double gas taps to fixed work surfaces listed on FF&E list","Dado on 2 walls","Cold water to wet serviced bollards or similar listed under FF&E, hot and cold to belfast or hand wash sink; chemically resistance drainage.",4,null,16]
["SCI55","Science studios, non-ambulant","secondary science studio (non-ambulant)","SCI55","SCI55","New Build","SL_25_10_74","Science studios","Specialist secondary space for a range of science activities, for ambulant pupils needing additional support ","Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of simple experiments. Using the whiteboard. Whole class presentations. ","Basic teaching","Light practical (science)",2.5,4,"J1","SEN",32,4.4000000000000004,null,1,62,6,7,1,8,"11-19","None","Full disabled access required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Not required",1050,"","D6.1mv","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F3.4h","hygienic non-slip","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5/T7","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F 7.7 and 7.8. *Acoustics: see BB93 0.4","Double gas taps to all bollards listed on FF&E list (as specified in Annex 3: FF&E)","Dado on 2 walls","Cold water to wet serviced bollards or similar listed under FF&E, hot and cold to belfast or hand wash sink; chemically resistance drainage.",4,null,16]
["SCI60","Multi-purpose practical rooms (ambulant)","Multi-purpose practical rooms (ambulant)","SCI60","SCI60","New Build","SL_25_10_53","Multi-purpose practical rooms","Specialist space for secondary art, science and D&T activities with a small group of ambulant pupils, needing additional support","Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of simple experiments. Using the whiteboard. Whole class presentations. Optional animal care or horticulture preparation.","Basic teaching","Light practical (science)",2.5,4,"H","SEN",16,3.3,null,1,55,12,14,1,16,"11-19","None","Disabled access into the space required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,"Doorset, including ironmongery, finger guards and access control system to be agreed with school","F3.4h","hygienic non-slip","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F 7.7 and 7.8. *Acoustics: see BB93 0.4","Optional","Dado on 2 walls","Cold water to wet serviced bollards or similar listed under FF&E, hot and cold to belfast or hand wash sink; chemically resistance drainage.",4,null,16]
["SCI65","Multi-purpose practical rooms, non-ambulant","secondary multi-purpose practical (non-ambulant)","SCI65","SCI65","New Build","SL_25_10_53","Multi-purpose practical rooms","Specialist space for secondary art, science and D&T activities with a small group of ambulant and non-ambulant pupils, needing significant additional support and specialist equipment","Briefing. Evaluation. Group and class discussion. Independent research and recording using ICT. Teacher demonstration of simple experiments. Using the whiteboard. Whole class presentations. ","Basic teaching","Light practical (science)",2.5,4,"J1","SEN",32,4.4000000000000004,null,1,62,6,7,1,8,"11-19","None","Full disabled access required","Enclosed",null,"3300 / 2700","2700 / 2400","7800 / 7500","Optional",1050,"Contractor to Specify for approval if provided","D6.1mv","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F3.4h","hygienic non-slip","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L1.2c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, day dim, abs off","No",null,"T5/T7","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F 7.7 and 7.8. *Acoustics: see BB93 0.4","Optional","Dado on 2 walls","Cold water to wet serviced bollards or similar listed under FF&E, hot and cold to belfast or hand wash sink; chemically resistance drainage.",4,null,16]
["SEN02","Medical treatment (MI) rooms","Medical treatment (MI) rooms","SEN02","SEN02","New Build","SL_35_10_53","Medical treatment rooms","Room for physio- and other therapy and medical inspections","Administering drug treatments to pupils. Medical inspection by external practitioners. Physio- or speech therapy for pupils with special needs and disabilities.","Learning resources","General",1.5,4,"C","-",4,1.7,null,1,12,5,5,1,6,"CTS","Optional","Full disabled access required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1a","private","N/A","no internal doorset required",null,"See Annex 2D 4.2.4. Finger guards if used by early years or in a special school or AP","F3.4h","hygienic non-slip","C1.1","general","W3.2","humid","Flooring to be cleanable and not hold smells","L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T6","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",8,null,4]
["SEN05","Medical treatment rooms, non-ambulant","Medical treatment rooms, non-ambulant","SEN05","SEN05","New Build","SL_35_10_53","Medical treatment rooms","Room for medical treatment/consultation for non-ambulant pupils","Medical treatment /consultation including with visiting medical staff, for non-ambulant pupils.","Learning resources","General",1.5,4,"E","SEN",6,2.1,null,0,16,3,3,0,4,"CTS","Optional","Full disabled access required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / CTS","Not required","CTS","","D6.1m","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F1.1h","special general","C1.1","general","W3.2","humid","Flooring suitable for wheelchairs, readily cleanable and not hold smells, no transition strips. Ceiling to include hoist tracking in both directions, avoiding light fittings","L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T6","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",1,null,8]
["SEN12","Therapy rooms","Therapy rooms","SEN12","SEN12","New Build","SL_35_10_88","Therapy rooms","Room for therapy ","Therapy and counselling for pupils with special needs; and related admin work.","Learning resources","General",1.5,4,"C","-",4,1.7,null,1,"As SoA","As SoA","As SoA",1,"As SoA","CTS","Optional","Full disabled access required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1a","private","N/A","no internal doorset required",null,"See Annex 2D 4.2.4. Finger guards if used by early years or in a special school or AP","F1.1","general","C1.1","general","W1.1","general",null,"L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No","refer to SSB for any specialist lighting requirements","T5","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","None",3,null,8]
["SEN13","Therapy rooms (speech & language)","Therapy rooms (speech & language)","SEN13","SEN12","New Build","SL_35_10_88","Therapy rooms","Room for speech therapy ","Speech therapy for pupils with special needs; and related admin work.","Learning resources","General",1.5,4,"C","-",4,1.7,null,1,"As SoA","As SoA","As SoA",1,"As SoA","CTS","Optional","Full disabled access required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1a","private","N/A","no internal doorset required",null,"See Annex 2D 4.2.4. Finger guards if used by early years or in a special school or AP","F1.1","general","C1.1","general","W1.1","general",null,"L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No","refer to SSB for any specialist lighting requirements","T5","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","None",3,null,8]
["SEN14","Therapy rooms (ambulant, physio)","Therapy rooms (ambulant, physio)","SEN14","SEN12","New Build","SL_35_10_88","Therapy rooms","Room for physiotherapy ","Physiotherapy with a range of equipment for pupils with special needs and disabilities.","Learning resources","General",1.5,4,"H","-",16,3.3,null,1,20,3,3,1,4,"CTS","Optional","Full disabled access required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1a","private","N/A","no internal doorset required",null,"See Annex 2D 4.2.4. Finger guards if used by early years or in a special school or AP","F1.1","general","C1.1","general","W1.1","general",null,"L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No","refer to SSB for any specialist lighting requirements","T5","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","None",1,null,8]
["SEN15","Therapy rooms, non-ambulant (physio)","Therapy rooms, non-ambulant","SEN15","SEN15","New Build","SL_35_10_88","Therapy rooms","Room for therapy ","Therapy and counselling for pupils with special needs; and related admin work.","Learning resources","General",1.5,4,"E","-",6,2.1,null,1,27,3,3,1,4,"CTS","Optional","Full disabled access required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / CTS","Not required","CTS","","D6.1m","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F1.1","general","C1.1","general","W1.1","general",null,"L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No","refer to SSB for any specialist lighting requirements","T5/T7","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","Optional, refer to SSB",1,null,8]
["SEN16","Therapy rooms, rebound","Therapy rooms, rebound","SEN16","SEN16","New Build","SL_35_10_88","Therapy rooms","Room for rebound therapy ","Rebound therapy for pupils with special needs and disabilities.","Learning resources","General",1.5,4,"H","-",16,3.3,null,1,20,1,1,1,2,"CTS","Optional","Full disabled access required","Enclosed or semi-enclosed",null,"3300 / 2700","2400 / N/A","N/A / CTS","Not required","CTS","","D1.1a","private","N/A","no internal doorset required",null,"Access control system to be agreed with school. Finger guards","F1.1","general","C1.1","general","W1.1","general","Monolithic ceiling. Padding on walls if required in SSB. Ceiling to include hoist and track. Trampoline to be recessed within floor to be at FFL.","L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No","refer to SSB for any specialist lighting requirements","T5","Low","Medium","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","None",1,null,8]
["SEN20","SEN resource spaces","SEN resource spaces","SEN20","SEN20","New Build","SL_25_75_82","SEN resource spaces","Small room for assistance with individuals and groups with SEN","Individual therapy and counselling. Individual/small group learning support. Staff meetings.","Learning resources","General",1.5,4,"C","-",4,1.7,null,0,16,7,7,0,8,"CTS","None","Full disabled access required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","N/A","","D1.1ev","early years","D1.1av","general",null,null,"F1.1","general","C1.1","general","W1.1","general"," ","L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=0.8","<=1.0",null,"None","Dado on 2 walls","None",8,2,16]
["SEN21","SEN resource spaces (ambulant support)","SEN resource spaces (ambulant support)","SEN21","SEN20","New Build","SL_25_75_82","SEN resource spaces","Room for assistance with individuals and groups with specific ambulant SEN or disabilities","Individual therapy and counselling. Individual/small group learning support. Staff meetings.","Learning resources","General",1.5,4,"C","SEN",4,1.7,null,0,"As SoA","As SoA","As SoA",1,"As SoA","CTS","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1ev","early years","N/A","no internal doorset required",null,"Access control system to be agreed with school","F1.1","general","C1.1","general","W1.1","general",null,"L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Average ","Low","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","None",6,null,8]
["SEN22","SEN resource spaces (SLCN support)","SEN resource spaces (SLCN support)","SEN22","SEN20","New Build","SL_25_75_82","SEN resource spaces","Room for assistance with individuals and groups with Speech, Language and Communication Needs","Individual therapy and counselling. Individual/small group learning support. Staff meetings.","Learning resources","General",1.5,4,"C","SEN",4,1.7,null,0,16,7,7,0,8,"CTS","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1ev","early years","N/A","no internal doorset required",null,"Access control system to be agreed with school","F1.1","general","C1.1","general","W1.1","general",null,"L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Average ","Low","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","None",6,null,8]
["SEN23","SEN resource spaces (behaviour support)","SEN resource spaces (behaviour support)","SEN23","SEN20","New Build","SL_25_75_82","SEN resource spaces","Room for assistance with individuals and groups with Behaviour Difficulties","Individual therapy and counselling. Individual/small group learning support. Staff meetings.","Learning resources","General",1.5,4,"E","-",6,2.1,null,0,16,5,5,0,6,"CTS","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1ev","early years","N/A","no internal doorset required",null,"Access control system to be agreed with school","F1.1","general","C1.1","general","W1.1","general",null,"L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Average ","Low","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","None",6,null,8]
["SEN24","SEN resource spaces (autism support)","SEN resource spaces (autism support)","SEN24","SEN20","New Build","SL_25_75_82","SEN resource spaces","Room for assistance with individuals and groups with Severe Autism","Individual therapy and counselling. Individual/small group learning support. Staff meetings.","Learning resources","General",1.5,4,"E","-",6,2.1,null,0,16,5,5,0,6,"CTS","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1ev","early years","N/A","no internal doorset required",null,"Access control system to be agreed with school","F1.1","general","C1.1","general","W1.1","general",null,"L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Average ","Low","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","None",6,null,8]
["SEN25","SEN resource spaces (PD support)","SEN resource spaces (PD support)","SEN25","SEN20","New Build","SL_25_75_82","SEN resource spaces","Room for assistance with individuals and groups with Physical Difficulties","Individual therapy and counselling. Individual/small group learning support. Staff meetings.","Learning resources","General",1.5,4,"F","-",8,2.5,null,0,16,3,3,0,4,"CTS","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1ev","early years","N/A","no internal doorset required",null,"Doorset, including ironmongery and access control system, to be agreed with school","F1.1","general","C1.1","general","W1.1","general",null,"L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Average ","Low","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","None",6,null,8]
["SEN26","SEN resource spaces (HI support)","SEN resource spaces (HI support)","SEN26","SEN20","New Build","SL_25_75_82","SEN resource spaces","Room for assistance with individuals and groups with Hearing Impairment","Individual therapy and counselling. Individual/small group learning support. Staff meetings.","Learning resources","General",1.5,4,"E","-",6,2.1,null,0,16,5,5,0,6,"CTS","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1ev","early years","N/A","no internal doorset required",null,"Access control system to be agreed with school","F1.1","general","C1.1","general","W1.1","general",null,"L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Average ","Low","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","None",6,null,8]
["SEN27","SEN resource spaces (VI support)","SEN resource spaces (VI support)","SEN27","SEN20","New Build","SL_25_75_82","SEN resource spaces","Room for assistance with individuals and groups with Visual Impairment","Individual therapy and counselling. Individual/small group learning support. Staff meetings.","Learning resources","General",1.5,4,"E","-",6,2.1,null,0,16,5,5,0,6,"CTS","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1ev","early years","N/A","no internal doorset required",null,"Access control system to be agreed with school","F1.1","general","C1.1","general","W1.1","general",null,"L3.1b","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Average ","Low","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","Dado on 2 walls","None",6,null,8]
["SEN30","Quiet calming spaces, room","Quiet calming spaces","SEN30","SEN30","New Build","SL_35_50_69","Quiet calming spaces","Room for an individual pupil to be withdrawn and avoid damage to themselves or building fabric","Calming of pupils with special needs.","Learning resources","General",1.5,4,"D","-",5,1.9,null,0,7,1,1,0,2,"CTS","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1400","Not required","CTS","","D1.1ev","early years","N/A","no internal doorset required",null,"Access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1","general","Monolithic ceiling. Padding on walls if required in SSB","L3.5f","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No","Specialist controls including dimming. Fittings to be tamper proof","T5","Average ","Low","<=0.6","<=0.8","Ventilation as Tech Annex 2F Section 7.8 Table 7-4","None","None","None",1]
["SEN31","Quiet calming spaces, bay (off classroom)","Quiet calming spaces, bay (off classroom)","SEN31","SEN31","New Build","SL_35_50_69","Quiet calming spaces","Bay for pupil self-referral or assistance (before they become dysregulated), off a SEN classroom","Independent working. One to one learning support and counselling. Privacy required.","Learning resources","General",1.5,4,"D","-",2,1.6,null,0,5,2,2,0,3,"CTS","None","Disabled access into the space required","Semi-enclosed or open plan","off SEN classroom","2400 / N/A",2400,"N/A / 1400","Optional","CTS","Contractor to Specify for approval if provided","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general","Monolithic ceiling. Padding on walls if required in SSB","L3.5f","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No","Specialist controls including dimming. Fittings to be tamper proof","T5","Low","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F Section 7.8 Table 7-4","None","None","None"]
["SEN32","Quiet calming spaces, room (off classroom)","Quiet calming spaces (room off classroom)","SEN32","SEN30","New Build","SL_35_50_69","Quiet calming spaces","Small room for pupil self-referral or assistance (before they become dysregulated), off a SEN classroom","Independent working. One to one learning support and counselling. Privacy required.","Learning resources","General",1.5,4,"D","-",2,1.6,null,0,5,2,2,0,3,"CTS","None","Disabled access into the space preferred","Enclosed","off SEN classroom","2700 / 2400",2400,"N/A / 1400","Not required","CTS","","D1.1ev","early years","N/A","no internal doorset required",null,"Access control system to be agreed with school","F1.1","general","C1.1","general","W1.1","general","Monolithic ceiling. Padding on walls if required in SSB","L3.5f","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No","Specialist controls including dimming. Fittings to be tamper proof","T5","Low","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F Section 7.8 Table 7-4","None","None","None",1]
["SEN33","Quiet calming spaces, bay (near classroom)",null,null,"SEN31","New Build","SL_35_50_69","Quiet calming spaces","Bay for pupil self-referral or assistance (before they become dysregulated), off a corridor near an SEN classroom","Independent working. One to one learning support and counselling. Privacy required.","Learning resources","General",1.5,4,"D","-",2,1.6,null,0,5,2,2,0,3,"CTS","None","Disabled access into the space required","Semi-enclosed or open plan","off SEN classroom","2400 / N/A",2400,"N/A / 1400","Optional","CTS","Contractor to Specify for approval if provided","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general","Monolithic ceiling. Padding on walls if required in SSB","L3.5f","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No","Specialist controls including dimming. Fittings to be tamper proof","T5","Low","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F Section 7.8 Table 7-4","None","None","None"]
["SEN34","Quiet calming spaces, room (near classroom)",null,null,"SEN30","New Build","SL_35_50_69","Quiet calming spaces","Small room for pupil self-referral or assistance (before they become dysregulated), off a corridor near an SEN classroom","Independent working. One to one learning support and counselling. Privacy required.","Learning resources","General",1.5,4,"D","-",2,1.6,null,0,5,2,2,0,3,"CTS","None","Disabled access into the space preferred","Enclosed","off SEN classroom","2700 / 2400",2400,"N/A / 1400","Not required","CTS","","D1.1ev","early years","N/A","no internal doorset required",null,"Access control system to be agreed with school","F1.1","general","C1.1","general","W1.1","general","Monolithic ceiling. Padding on walls if required in SSB","L3.5f","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No","Specialist controls including dimming. Fittings to be tamper proof","T5","Low","Medium","<=0.6","<=0.8","Ventilation as Tech Annex 2F Section 7.8 Table 7-4","None","None","None",1]
["SEN38","Quiet calming spaces (calming)","Quiet calming spaces (fitted)","SEN38","SEN30","New Build","SL_35_50_69","Quiet calming spaces","Room for an individual pupil who has become dysregulated and may pose a risk of harm to themselves or others","Calming of pupils with special needs.","Learning resources","General",1.5,4,"C","-",4,1.7,null,0,6,1,1,0,2,"CTS","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1400","Not required","CTS","","D1.1ev","early years","N/A","no internal doorset required",null,"Access control system to be agreed with school","F1.1","general","C1.1","general","W1.1","general","Monolithic ceiling. Padding on walls if required in SSB","L3.5f","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No","Specialist controls including dimming. Fittings to be tamper proof","T5","High","Low","<=0.6","<=0.8","Ventilation as Tech Annex 2F Section 7.8 Table 7-4","None","None","None",4,null,8]
["SEN40","Sensory rooms (ambulant)","Sensory rooms (ambulant)","SEN40","SEN40","New Build","SL_35_50_78","Sensory rooms","Specially equipped room for light and sound therapy, ambulant","Use of specialist projection equipment to simulate a range of environment for pupils with special needs","Learning resources","Fitted",2,4,"F","SEN",8,2.5,null,0,16,2,2,0,3,"CTS","None","Disabled access into the space required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Not required","CTS","","D1.1a","private","N/A","no internal doorset required",null,"Access control system to be agreed with school. Finger guards","F1.1","general","C1.1","general","W1.1","general",null,"L6.5f","No requirement","No requirement","Not applicable","Not applicable",300,"man on, abs off","No","Refer to SSB for any specialist lighting requirements","T5","Average ","Low","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit equipment","None",2,null,4]
["SEN45","Sensory rooms, non-ambulant","Sensory rooms, non-ambulant","SEN45","SEN45","New Build","SL_35_50_78","Sensory rooms","Specially equipped room for light and sound therapy, non-ambulant","Use of specialist projection equipment to simulate a range of environment for pupils with special needs","Learning resources","Fitted",2,4,"G","SEN",10,2.9,null,0,20,3,3,0,4,"CTS","None","Full disabled access required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / CTS","Not required","CTS","","D6.1m","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1","general",null,"L6.5f","No requirement","No requirement","Not applicable","Not applicable",300,"man on, abs off","No","Refer to SSB for any specialist lighting requirements","T5/T7","Average ","Low","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit equipment","None",2,null,4]
["SEN50","Sensory rooms (ambulant, immersion)","Sensory rooms (ambulant, immersion)","SEN50","SEN40","New Build","SL_35_50_78","Sensory rooms","Specially equipped 'immersive' room for small groups, ambulant","Use of specialist projection equipment to simulate a range of environment for pupils with special needs","Learning resources","Fitted",2,4,"D","SEN",5,1.9,null,0,16,4,4,0,5,"CTS","None","Disabled access into the space required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Not required","CTS","","D1.1a","private","N/A","no internal doorset required",null,"Access control system to be agreed with school. Finger guards","F1.1h","special general","C1.1","general","W1.1","general",null,"L6.5f","No requirement","No requirement","Not applicable","Not applicable",300,"man on, abs off","No","Refer to SSB for any specialist lighting requirements","T5","Average ","Low","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit equipment","None",2,null,4]
["SEN55","Sensory rooms, non-ambulant (immersion)","Sensory rooms, non-ambulant (immersion)","SEN55","SEN45","New Build","SL_35_50_78","Sensory rooms","Specially equipped 'immersive' room for small groups, non-ambulant","Use of specialist projection equipment to simulate a range of environment for pupils with special needs","Learning resources","Fitted",2,4,"E","SEN",6,2.1,null,0,16,4,4,0,5,"CTS","None","Full disabled access required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / CTS","Not required","CTS","","D6.1m","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1","general",null,"L6.5f","No requirement","No requirement","Not applicable","Not applicable",300,"man on, abs off","No","Refer to SSB for any specialist lighting requirements","T5/T7","Average ","Low","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit equipment","None",2,null,4]
["SEN60","Soft play rooms (ambulant)","Soft play rooms (ambulant)","SEN60","SEN60","New Build","SL_40_05_81","Soft play rooms","A room for movement therapy on padded surfaces, ambulant.","Use of soft play equipment by pupils with special needs","Learning resources","Fitted",2,4,"D","SEN",5,1.9,null,0,20,8,8,0,9,"CTS","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","7800 / CTS","Not required","CTS","","D1.1ev","early years","N/A","no internal doorset required",null,"Access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1","general","Suitable for padding to be fitted on floor and walls","L5.5f","No requirement","No requirement","Not applicable","Not applicable",300,"man on, abs off","No",null,"T5","High","Low","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","None","None"]
["SEN65","Soft play rooms, non-ambulant","Soft play rooms, non-ambulant","SEN65","SEN65","New Build","SL_40_05_81","Soft play rooms","A room for movement therapy on padded surfaces, non-ambulant.","Use of soft play equipment by pupils with special needs","Learning resources","Fitted",2,4,"E","SEN",6,2.1,null,0,27,7,7,0,8,"CTS","None","Full disabled access required","Enclosed",null,"2700 / 2400","2400 / N/A","7800 / CTS","Not required","CTS","","D6.1m","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1","general","Suitable for padding to be fitted on floor and walls. Ceiling to include hoist and track.","L5.5f","No requirement","No requirement","Not applicable","Not applicable",300,"man on, abs off","No",null,"T5/T7","High","Low","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","None","None"]
["SEN70","Sensory rooms (ambulant, with soft play)","Sensory rooms (ambulant, with soft play)","SEN70","SEN40","New Build","SL_35_50_78","Sensory rooms","A room for movement therapy on padded surfaces, non-ambulant.","Use of sensory and soft play equipment by pupils with special needs","Learning resources","Fitted",2,4,"D","SEN",5,1.9,null,0,20,8,8,0,9,"CTS","None","Disabled access into the space required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Not required","CTS","","D1.1a","private","N/A","no internal doorset required",null,"Access control system to be agreed with school. Finger guards","F1.1h","special general","C1.1","general","W1.1","general",null,"L6.5f","No requirement","No requirement","Not applicable","Not applicable",300,"man on, abs off","No","Refer to SSB for any specialist lighting requirements","T5","High","High","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit equipment","None"]
["SEN75","Sensory rooms, non-ambulant (with soft play)","Sensory rooms, non-ambulant (with soft play)","SEN75","SEN45","New Build","SL_35_50_78","Sensory rooms","A room for movement therapy on padded surfaces, non-ambulant.","Use of sensory and soft play equipment by pupils with special needs","Learning resources","Fitted",2,4,"E","SEN",6,2.1,null,0,27,7,7,0,8,"CTS","None","Full disabled access required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / CTS","Not required","CTS","","D6.1m","special wide","N/A","no internal doorset required",null,"Ergonomic handle and access control system to be agreed with school","F1.1h","special general","C1.1","general","W1.1","general",null,"L6.5f","No requirement","No requirement","Not applicable","Not applicable",300,"man on, abs off","No","Refer to SSB for any specialist lighting requirements","T5/T7","High","High","<=0.4*","<=0.4*","Ventilation as Tech Annex 2F Section 7.8 Table 7-4. *Acoustics: see BB93 0.4","None","To suit equipment","None"]
["SEN80","Warm water pools","Warm water pools","SEN80","SEN80","New Build","SL_35_10_97","Warm water pools","Pool for warm water therapy and recreational activity","Hydrotherapy for pupils with special needs","Learning resources","Large",12.5,-20,"J","SEN",28,4.2,null,0,150,29,29,0,32,"N/A","Optional","Full disabled access required","Enclosed",null,"CTS","CTS","N/A / CTS","Not required","CTS","","DD6.1hv","special double","N/A","no internal doorset required",null,"Ergonomic handle and access control system. Override to hold open device to be provided in an access restricted location. Finger guards","F7.3h","wet area","C2.3","wet areas","W3.3","wet areas","Flooring in barefoot areas shall be 'barefoot slip resistance category B'. Walls to suit specialist requirements of pools. ceiling to include hoist and track.","L5.5i","No requirement","No requirement","Not applicable","Not applicable",300,"man on, man off","No","IP rating for wet areas. Refer to SSB for any specialist lighting requirements","T9","High","High","<=1.5","<=2.0",null,"None","None","Heated and treated"]
["SEN85","Hydrotherapy pools","Hydrotherapy pools","SEN85","SEN85","New Build","SL_35_10_39","Hydrotherapy pools","Pool for warm water therapy ","Hydrotherapy for pupils with special needs","Learning resources","Large",12.5,-20,"J","SEN",28,4.2,null,0,85,14,14,0,16,"N/A","Optional","Full disabled access required","Enclosed",null,"CTS","CTS","N/A / CTS","Not required","CTS","","DD6.1hv","special double","N/A","no internal doorset required",null,"Ergonomic handle and access control system. Override to hold open device to be provided in an access restricted location. Finger guards","F7.3h","wet area","C2.3","wet areas","W3.3","wet areas","Flooring in barefoot areas shall be 'barefoot slip resistance category B'. Walls to suit specialist requirements of pools. ceiling to include hoist and track.","L5.5i","No requirement","No requirement","Not applicable","Not applicable",300,"man on, man off","No","IP rating for wet areas. Refer to SSB for any specialist lighting requirements","T9","High","High","<=1.5","<=2.0",null,"None","None","Heated and treated"]
["SPH01","Sports halls, school (1-court)",null,null,"SPH00","New Build","SL_42_40_82","Sports halls","18m wide sports hall for school PE activities, exams and some community use","Athletics (practice only) and gymnastics; badminton; basketball; Five-A-Side football / futsal; indoor tennis; judo; karate; korfball; mini handball; netball (practice only); short tennis; table tennis; trampolining; volleyball.","Halls and dining","Large",12.5,-20,"S","standard",15,1.75,null,0,180,94,"94",0,110,"N/A","Yes","Disabled access into the space required","Enclosed",null,"7500 / 7500","7500 / 7500","18000 / 18000","For fire only","CTS","Contractor to Specify for approval","DD1.1kv","general double ","N/A","no internal doorset required",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards in Primary and SEN","F6.1","multi-purpose sport","C1.1","general","W6.1h","sports","Floor markings to be suitable for sports to be accommodated. Floor sockets to suit the sports hall floor and FF&E provided. ","L2.6j","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement","500 switchable to 300","key on, day dim, abs off","Yes",null,"T2/T5","High","Medium","<=2.0","<=2.0","Ventilation as Tech Annex 2F 6.4.2","None","Where required","None",10,4,4,"No projections, including opening doors, to avoid injury during activity."]
["SPH02","Sports halls, school (2-court)","Sports halls, school (2-court)","SPH02","SPH00","New Build","SL_42_40_82","Sports halls","18m wide sports hall for secondary school PE activities, exams and some community use","Individual activities including Athletics (practice only) and gymnastics. Team games including badminton; basketball; Five-A-Side football / futsal; indoor tennis; judo; karate; korfball; mini handball; netball (practice only); short tennis; table tennis and volleyball.","Halls and dining","Large",12.5,-20,"S","standard",15,1.75,null,0,306,166,166,0,183,"N/A","Yes","Disabled access into the space required","Enclosed",null,"7500 / 7500","7500 / 7500","18000 / 18000","For fire only","CTS","Contractor to Specify for approval","DD1.1kv","general double ","N/A","no internal doorset required",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards in Primary","F6.1","multi-purpose sport","C1.1","general","W6.1h","sports","Floor markings to be suitable for sports to be accommodated. Floor sockets to suit the sports hall floor and FF&E provided. ","L2.6j","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement","500 switchable to 300","key on, day dim, abs off","Yes",null,"T2/T5","High","Medium","<=2.0","<=2.0","Ventilation as Tech Annex 2F 6.4.2","None","Where required","None",10,4,4,"No projections, including opening doors, to avoid injury during activity."]
["SPH03","Sports halls, school (3-court)","Sports halls, school (3-court)","SPH03","SPH00","New Build","SL_42_40_82","Sports halls","18m x 28m sports hall for secondary school PE activities, exams and some community use","Individual activities including Athletics (practice only) and gymnastics. Team games including badminton; basketball; Five-A-Side football / futsal; indoor tennis; judo; karate; korfball; mini handball; netball (practice only); short tennis; table tennis and volleyball.","Halls and dining","Large",12.5,-20,"S","standard",15,1.75,null,0,504,279,279,0,293,"N/A","Yes","Disabled access into the space required","Enclosed",null,"7500 / 7500","7500 / 7500","18000 / 18000","For fire only","CTS","Contractor to Specify for approval","DD1.1kv","general double ","N/A","no internal doorset required",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards in Primary","F6.1","multi-purpose sport","C1.1","general","W6.1h","sports","Floor markings to be suitable for sports to be accommodated. Floor sockets to suit the sports hall floor and FF&E provided. ","L2.6j","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement","500 switchable to 300","key on, day dim, abs off","Yes",null,"T2/T5","High","Medium","<=2.0","<=2.0","Ventilation as Tech Annex 2F 6.4.2","None","Where required","None",10,8,8,"No projections, including opening doors, to avoid injury during activity."]
["SPH04","Sports halls, school (4-court)","Sports halls, school (4-court)","SPH04","SPH00","New Build","SL_42_40_82","Sports halls","18m x 33m sports hall for secondary school PE activities, exams and some recreational community use","Individual activities including Athletics (practice only) and gymnastics. Team games including badminton; basketball; Five-A-Side football / futsal; indoor tennis; judo; karate; korfball; mini handball; netball (practice only); short tennis; table tennis and volleyball.","Halls and dining","Large",12.5,-20,"S","standard",15,1.75,null,0,594,331,331,0,348,"N/A","Yes","Disabled access into the space required","Enclosed",null,"7500 / 7500","7500 / 7500","18000 / 18000","For fire only","CTS","Contractor to Specify for approval","DD1.1kv","general double ","N/A","no internal doorset required",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards in Primary","F6.1","multi-purpose sport","C1.1","general","W6.1h","sports","Floor markings to be suitable for sports to be accommodated. Floor sockets to suit the sports hall floor and FF&E provided. ","L2.6j","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement","500 switchable to 300","key on, day dim, abs off","Yes",null,"T2/T5","High","Medium","<=2.0","<=2.0","Ventilation as Tech Annex 2F 6.4.2","None","Where required","None",10,8,8,"No projections, including opening doors, to avoid injury during activity."]
["SPH20","Sports halls, community (multi-court)","Sports halls, community (multi-court)","SPH20","SPH20","New Build","SL_42_40_82","Sports halls","Sports hall for secondary school PE activities and formal community use","Net bay(s) (36m wide). Badminton courts. Basketball court(s). Five-A-Side Football / Futsal court(s). Indoor Cricket. Indoor Tennis. Judo. Karate. Korfball court(s). Mini Handball court(s). Netball practice only. Short Tennis. Sports hall athletics","Halls and dining","Large",12.5,-20,"S","extensive",15,1.75,null,0,"As SoA","As SoA","As SoA",0,"As SoA","N/A","Yes","Disabled access into the space required","Enclosed",null,"7500 / 7500","7500 / 7500","20000 / 20000","Optional","CTS","Contractor to Specify for approval if provided","DD1.1kv","general double ","N/A","no internal doorset required",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards in Primary and SEN","F6.1","multi-purpose sport","C1.1","general","W6.1h","sports","Floor markings to be suitable for sports to be accommodated. Floor sockets to suit the sports hall floor and FF&E provided. ","L2.6j","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement","500 switchable to 300","key on, day dim, abs off","Yes",null,"T2/T5","High","Medium","<=2.0","<=2.0","Ventilation as Tech Annex 2F 6.4.2","None","Where required","None",13,8,8,"No projections, including opening doors, to avoid injury during activity."]
["SPH24","Sports halls, community (4-court)","Sports halls, community (4-court)","SPH24","SPH20","New Build","SL_42_40_82","Sports halls","20m x 34.5m sports hall for secondary school PE activities and formal community use","2 Net bay(s) (36m wide). Badminton 4 courts. Basketball court(s). Five-A-Side Football / Futsal court(s). Indoor Cricket. Indoor Tennis. Judo. Karate. Korfball court(s). Mini Handball court(s). Netball practice only. Short Tennis. Sports hall athletics","Halls and dining","Large",12.5,-20,"S","extensive",15,1.75,null,0,690,386,386,0,405,"N/A","Yes","Disabled access into the space required","Enclosed",null,"7500 / 7500","7500 / 7500","20000 / 20000","Optional","CTS","Contractor to Specify for approval if provided","DD1.1kv","general double ","N/A","no internal doorset required",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards in Primary","F6.1","multi-purpose sport","C1.1","general","W6.1h","sports","Floor markings to be suitable for sports to be accommodated. Floor sockets to suit the sports hall floor and FF&E provided. ","L2.6j","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement","500 switchable to 300","key on, day dim, abs off","Yes",null,"T2/T5","High","Medium","<=2.0","<=2.0","Ventilation as Tech Annex 2F 6.4.2","None","Where required","None",13,8,10,"No projections, including opening doors, to avoid injury during activity."]
["SPH25","Sports halls, community (5-court)","Sports halls, community (5-court)","SPH25","SPH20","New Build","SL_42_40_82","Sports halls","21.35m x 40.6m sports hall for secondary school PE activities and formal community use","Net bay(s) (36m wide). Badminton 5 courts. Basketball court(s). Five-A-Side Football / Futsal court(s). Indoor Cricket. Indoor Tennis. Judo. Karate. Korfball court(s). Mini Handball court(s). Netball practice only. Short Tennis. Sports hall athletics","Halls and dining","Large",12.5,-20,"S","extensive",15,1.75,null,0,867,487,487,0,511,"N/A","Yes","Disabled access into the space required","Enclosed",null,"7500 / 7500","7500 / 7500","20000 / 20000","Optional","CTS","Contractor to Specify for approval if provided","DD1.1kv","general double ","N/A","no internal doorset required",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards in Primary","F6.1","multi-purpose sport","C1.1","general","W6.1h","sports","Floor markings to be suitable for sports to be accommodated. Floor sockets to suit the sports hall floor and FF&E provided. ","L2.6j","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement","500 switchable to 300","key on, day dim, abs off","Yes",null,"T2/T5","High","Medium","<=2.0","<=2.0","Ventilation as Tech Annex 2F 6.4.2","None","Where required","None",13,8,10,"No projections, including opening doors, to avoid injury during activity."]
["SPH27","Sports halls, community (8-court)","Sports halls, community (8-court)","SPH27","SPH20","New Build","SL_42_40_82","Sports halls","30.5m x 40.7m sports hall for secondary school PE activities and formal community use","Net bay(s) (36m wide). Badminton 8 courts. Basketball court(s). Five-A-Side Football / Futsal court(s). Indoor Cricket. Indoor Tennis. Judo. Karate. Korfball court(s). Mini Handball court(s). Netball practice only. Short Tennis. Sports hall athletics","Halls and dining","Large",12.5,-20,"S","extensive",15,1.75,null,0,1380,780,780,0,819,"N/A","Yes","Disabled access into the space required","Enclosed",null,"7500 / 7500","7500 / 7500","20000 / 20000","Optional","CTS","Contractor to Specify for approval if provided","DD1.1kv","general double ","N/A","no internal doorset required",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards in Primary","F6.1","multi-purpose sport","C1.1","general","W6.1h","sports","Floor markings to be suitable for sports to be accommodated. Floor sockets to suit the sports hall floor and FF&E provided. ","L2.6j","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement","500 switchable to 300","key on, day dim, abs off","Yes",null,"T2/T5","High","Medium","<=2.0","<=2.0","Ventilation as Tech Annex 2F 6.4.2","None","Where required","None",13,10,16,"No projections, including opening doors, to avoid injury during activity."]
["SPH28","Sports halls, community (12-court)","Sports halls, community (12-court)","SPH28","SPH20","New Build","SL_42_40_82","Sports halls","34.5m x 37m sports hall for secondary school PE activities and formal community use","Net bay(s) (36m wide). Badminton 12 courts. Basketball court(s). Five-A-Side Football / Futsal court(s). Indoor Cricket. Indoor Tennis. Judo. Karate. Korfball court(s). Mini Handball court(s). Netball practice only. Short Tennis. Sports hall athletics","Halls and dining","Large",12.5,-20,"S","extensive",15,1.75,null,0,1734,982,982,0,1031,"N/A","Yes","Disabled access into the space required","Enclosed",null,"7500 / 7500","7500 / 7500","20000 / 20000","Optional","CTS","Contractor to Specify for approval if provided","DD1.1kv","general double ","N/A","no internal doorset required",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards in Primary","F6.1","multi-purpose sport","C1.1","general","W6.1h","sports","Floor markings to be suitable for sports to be accommodated. Floor sockets to suit the sports hall floor and FF&E provided. ","L2.6j","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement","500 switchable to 300","key on, day dim, abs off","Yes",null,"T2/T5","High","Medium","<=2.0","<=2.0","Ventilation as Tech Annex 2F 6.4.2","None","Where required","None",13,12,16,"No projections, including opening doors, to avoid injury during activity."]
["SPH31","Sports halls, school (multi-court, extg)","Sports halls, school (multi-court, extg)","SPH31","SPH30","Existing","SL_42_40_82","Sports halls","Existing sports hall for secondary school PE activities and some community use","Individual activities including Athletics (practice only) and gymnastics. Team games including badminton; basketball; Five-A-Side football / futsal; indoor tennis; judo; karate; korfball; mini handball; netball (practice only); short tennis; table tennis and volleyball.","Halls and dining","Large",12.5,-20,"S","standard",15,1.75,null,0,544,302,302,0,317,"N/A","Yes","Disabled access into the space required","Enclosed",null,"7500 / 7500","as existing","as existing","As existing","CTS","Contractor to Specify for approval","DD1.1kv","general double ","N/A","no internal doorset required",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards in Primary","F6.1","multi-purpose sport","C1.1","general","W6.1h","sports","Floor markings to be suitable for sports to be accommodated. Floor sockets to suit the sports hall floor and FF&E provided. ","L2.6j","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement","500 switchable to 300","key on, day dim, abs off","Yes",null,"T2/T5","High","Medium","<=2.0","<=2.0","Ventilation as Tech Annex 2F 6.4.2","None","Where required","None",10,8,8,"No projections, including opening doors, to avoid injury during activity."]
["SPH32","Sports halls, community (multi-court, extg)","Sports halls, community (multi-court, extg)","SPH32","SPH30","Existing","SL_42_40_82","Sports halls","Existing sports hall for secondary school PE activities and formal community use","Net bay(s) (36m wide). Badminton courts. Basketball court(s). Five-A-Side Football / Futsal court(s). Indoor Cricket. Indoor Tennis. Judo. Karate. Korfball court(s). Mini Handball court(s). Netball practice only. Short Tennis. Sports hall athletics","Halls and dining","Large",12.5,-20,"S","extensive",15,1.75,null,0,"As SoA","As SoA","As SoA",0,"As SoA","N/A","Yes","Disabled access into the space required","Enclosed",null,"7500 / 7500","as existing","as existing","As existing","CTS","Contractor to Specify for approval","DD1.1kv","general double ","N/A","no internal doorset required",null,"Plain meeting stiles. Must open out from space. All surfaces must be flush with no projecting frames or ironmongery. Fingerguards in Primary","F6.1","multi-purpose sport","C1.1","general","W6.1h","sports","Floor markings to be suitable for sports to be accommodated. Floor sockets to suit the sports hall floor and FF&E provided. ","L2.6j","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement","500 switchable to 300","key on, day dim, abs off","Yes",null,"T2/T5","High","Medium","<=2.0","<=2.0","Ventilation as Tech Annex 2F 6.4.2","None","Where required","None",13,8,8,"No projections, including opening doors, to avoid injury during activity."]
["STH00","Sports equipment stores, internal","Sports equipment stores, internal","STH00","STH00","New Build","SL_90_50_82","Sports equipment stores","Storage for PE and sports equipment, including mats","Storing PE and sports equipment including trampolines, forms, racquets and balls.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","Optional","Full disabled access not required","Enclosed or open to sports hall",null,"2700 / 2400","2700 / 2400","N/A / 3400","Not required","N/A","","DD5.1h","hall store","N/A","no internal doorset required",null,"Dimensions to suit equipment to be stored, particularly trampolines. Pull handles to be flush-fitting non-projecting handles","F2.1","stores","C1.1","general","W4.1","rough"," ","L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,2,"Fire Containment. Separate mat storage required if mats not flame retardant."]
["STH01","Sports equipment stores, internal (sports hall)","Sports equipment stores, internal (sports hall)","STH01","STH00","New Build","SL_90_50_82","Sports equipment stores","Storage for PE and sports equipment, including mats","Storing PE and sports equipment including trampolines, forms, racquets and balls.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","Optional","Full disabled access not required","Enclosed or open to sports hall","off Sports hall","2700 / 2400","2700 / 2400","N/A / 3400","Not required","N/A","","DD5.1h","hall store","N/A","no internal doorset required",null,"Dimensions to suit equipment to be stored, particularly trampolines. Pull handles to be flush-fitting non-projecting handles","F2.1","stores","C1.1","general","W4.1","rough",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,6,"Fire Containment. Separate mat storage required if mats not flame retardant."]
["STH02","Sports equipment stores, internal (community)","Sports equipment stores, internal (community)","STH02","STH00","New Build","SL_90_50_82","Sports equipment stores","Storage for PE and sports equipment, including mats","Storing PE and sports equipment including trampolines, forms, racquets and balls.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","Yes","Full disabled access not required","Enclosed or open to sports hall",null,"2700 / 2400","2700 / 2400","N/A / 3400","Not required","N/A","","DD5.1h","hall store","N/A","no internal doorset required",null,"Dimensions to suit equipment to be stored, particularly trampolines. Pull handles to be flush-fitting non-projecting handles","F2.1","stores","C1.1","general","W4.1","rough",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,2,"Fire Containment. Separate mat storage required if mats not flame retardant."]
["STH03","Sports equipment stores, internal (activity studio)","Sports equipment stores, internal (activity studio)","STH03","STH00","New Build","SL_90_50_82","Sports equipment stores","Storage for PE and sports equipment, including mats","Storing PE and sports equipment including trampolines, forms, racquets and balls.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","Optional","Full disabled access not required","Enclosed or open to studio","off Activity studio","2700 / 2400","2700 / 2400","N/A / 3400","Not required","N/A","","DD5.1h","hall store","N/A","no internal doorset required",null,"Dimensions to suit equipment to be stored, particularly trampolines. Pull handles to be flush-fitting non-projecting handles","F2.1","stores","C1.1","general","W4.1","rough",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,2,"Fire Containment. Separate mat storage required if mats not flame retardant."]
["STH04","Sports equipment stores, internal (off hall)","Sports equipment stores, internal (off hall)","STH04","STH00","New Build","SL_90_50_82","Sports equipment stores","Storage for PE and sports equipment, including mats","Storing PE and sports equipment including trampolines, forms, racquets and balls.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled access not required","Enclosed or open to hall","off Assembly hall","2700 / 2400","2700 / 2400","N/A / 3400","Not required","N/A","","DD5.1h","hall store","N/A","no internal doorset required",null,"Dimensions to suit equipment to be stored, particularly trampolines. Pull handles to be flush-fitting non-projecting handles","F2.1","stores","C1.1","general","W4.1","rough",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,2,"Fire Containment. Separate mat storage required if mats not flame retardant."]
["STH05","Sports equipment stores, external","Sports equipment stores, external","STH05","STH05","New Build","SL_90_50_82","Sports equipment stores","Store for external PE and sports activities","Storing equipment for outdoor sports including goals, nets, bats, racquets, balls.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,8,"-","-",0,{"$error":"#VALUE!"},"N/A","Optional","Disabled access not required","Enclosed","adjacent to Outdoor PE spaces","2400 / N/A","2200 / N/A","N/A / 1700","Double doors","N/A","Contractor to Specify for approval","N/A","no internal doorset required","N/A","no internal doorset required",null,"Dimensions to suit equipment to be stored, particularly trampolines. Pull handles to be flush-fitting non-projecting handles","F2.1","stores","C1.1","general","W4.1","rough"," ","L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","None","None",0,null,0,"CTS if Fire Containment."]
["STH10","Furniture stores","Furniture stores","STH10","STH10","New Build","SL_90_50_32","Furniture stores","Storage for chairs and tables used in hall","Storage for chairs for assemblies, exams and performances, as well as dining (with tables if required) in an adjacent hall.","Storage (non-teaching)","Storage",2,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","Optional","Disabled access not required","Enclosed",null,"2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","DD1.1a","general double ","N/A","no internal doorset required",null,"Dimensions to suit equipment to be stored, particularly folding dining tables","F2.1","stores","C1.1","general","W1.1h","general","Flooring suitable for heavy movable FF&E on castors ","L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","None","None",0,null,2,"CTS if Fire Containment."]
["STH11","Furniture stores (chair/ table, off hall)","Furniture stores (chair/ table, off hall)","STH11","STH10","New Build","SL_90_50_32","Furniture stores","Storage for chairs and tables used in hall","Storage for chairs for assemblies, exams and performances, as well as dining (with tables if required) in an adjacent hall.","Storage (non-teaching)","Storage",2,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","Optional","Disabled access not required","Enclosed","off Assembly hall","2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","DD1.1a","general double ","N/A","no internal doorset required",null,"Dimensions to suit equipment to be stored, particularly folding dining tables","F2.1","stores","C1.1","general","W1.1h","general","Flooring suitable for heavy movable FF&E on castors ","L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","None","None",0,null,4,"CTS if Fire Containment."]
["STH12","Furniture stores (chair, off hall)","Furniture stores (chair, off hall)","STH12","STH10","New Build","SL_90_50_32","Furniture stores","Storage for chairs and tables used in hall","Storage for chairs for assemblies, exams and performances, as well as dining (with tables if required) in an adjacent hall.","Storage (non-teaching)","Storage",2,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","Optional","Disabled access not required","Enclosed","off Assembly hall","2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","DD1.1a","general double ","N/A","no internal doorset required",null,"Dimensions to suit equipment to be stored, particularly folding dining tables","F2.1","stores","C1.1","general","W1.1h","general","Flooring suitable for heavy movable FF&E on castors ","L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","None","None",0,null,4,"CTS if Fire Containment."]
["STH15","Dining furniture stores, and servery","Dining furniture stores, and servery","STH15","STH15","New Build","SL_90_50_22","Dining furniture stores","Storage for dining furniture and space in front of servery for pupils to queue and collect food","Storage for chairs and tables for dining in an adjacent hall.","Storage (non-teaching)","Storage",2,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","Optional","Disabled access into the space required","Enclosed","off Assembly hall","2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","DD1.1a","general double ","N/A","no internal doorset required",null,"Dimensions to suit equipment to be stored, particularly folding dining tables","F4.2h","dining","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L2.6h","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",200,"key on, day dim, abs off","No",null,"T3","High","High","<=1.0","<=1.5",null,"None","To suit equipment","Where required",0,null,4,"CTS if Fire Containment."]
["STH20","Retractable seating storage (off hall)","Retractable seating storage (off hall)","STH20","STH20","New Build","SL_90_50_73","Retractable seating storage","storage of retractable bleacher seating in hall","Storage for retractable bleacher seating in an adjacent hall. Space required when bleacher seating is fully retracted","Storage (non-teaching)","Storage",2,4,"-","-",0,0,null,0,16,"-","-",0,{"$error":"#VALUE!"},"N/A","Optional","Disabled access not required","Semi-enclosed","off Assembly hall with bleachers","3300 / N/A","CTS","N/A / 1200","Not required","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,"Dimensions to suit retractable seating to be stored","F6.2h","multi-purpose hall","N/A","not applicable","W2.1h","science","Floor finish to match adjacent hall where required","N/A","Not applicable","Not applicable","Not applicable","Not applicable","-","n/a","No",null,"N/A","N/A","N/A","N/A","N/A",null,"None","None","None",0,null,4,"Appropriate barriers to edge"]
["STN00","Coats and bags stores","Coats and bags stores","STN00","STN00","New Build","SL_90_50_19","Coats and bags stores","Space for lockers or coat hooks and shelving for bags, typically off circulation areas, for pupils","Storing pupils personal belongings (coats, bags, books, PE equipment etc).","Storage (non-teaching)","Storage",2,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access to at least 25% of coat hooks required","Open plan",null,"2400 / N/A","2200 / N/A","N/A / 600","Not required","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F2.1","stores","C1.1","general","W1.1","general"," ","L4.4o","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",100,"man on, man off","No",null,"T3","Average","High","<=1.5","<=2.0",null,"None","None","None",0,null,2,"Allow sufficient space for safe access."]
["STN01","Coats and bags stores (coat hooks)","Coats and bags stores (coat hooks)","STN01","STN00","New Build","SL_90_50_19","Coats and bags stores","Coat hooks and shelving for bags off circulation areas for pupils","Storing pupils personal belongings (coats, bags, books, PE equipment etc).","Storage (non-teaching)","Storage",2,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access to at least 25% of coat hooks required","Open plan",null,"2400 / N/A","2200 / N/A","N/A / 600","Not required","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F2.1","stores","C1.1","general","W1.1","general"," ","L4.4o","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",100,"man on, man off","No",null,"T3","Average","High","<=1.5","<=2.0",null,"None","None","None",0,null,2,"Allow sufficient space for safe access."]
["STN02","Coats and bags stores (lockers)","Coats and bags stores (lockers)","STN02","STN00","New Build","SL_90_50_19","Coats and bags stores","Space for lockers, and access to lockers, off circulation area","Storing pupils personal belongings (coats, bags, books, PE equipment etc).","Storage (non-teaching)","Storage",2,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access to at least 25% of lockers required","Open plan","off Corridor","2400 / N/A","2200 / N/A","N/A / 600","Not required","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F2.1","stores","C1.1","general","W1.1","general"," ","L4.4o","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",100,"man on, man off","No",null,"T3","Average","High","<=1.5","<=2.0",null,"None","None","None",0,null,4,"Allow sufficient space for safe access."]
["STN03","Coats and bags stores (community lockers)","Coats and bags stores (community lockers)","STN03","STN00","New Build","SL_90_50_19","Coats and bags stores","Space for lockers, and access to lockers, off circulation areas, for community use outside school core hours","Storing pupils personal belongings (coats, bags, books, PE equipment etc).","Storage (non-teaching)","Storage",2,4,"-","-",0,0,null,0,4,"-","-",0,{"$error":"#VALUE!"},"N/A","Yes","Disabled access to at least 25% of lockers required","Open plan","off Corridor","2400 / N/A","2200 / N/A","N/A / 600","Not required","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F2.1","stores","C1.1","general","W1.1","general",null,"L4.4o","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",100,"man on, man off","No",null,"T3","Average","High","<=1.5","<=2.0",null,"None","None","None",0,null,2,"Allow sufficient space for safe access."]
["STN05","Equipment stores, room (nursery mobility/ buggies)","Equipment stores, appliance store","STN05","STN05","New Build","SL_90_50_27","Equipment stores","Store room for wheelchairs/ other appliances and buggies","Storing wheelchair, mobility equipment or buggies appliance used by pupils","Storage (non-teaching)","Storage",2,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","Yes","Disabled access into the space required","Enclosed or semi-enclosed","off Corridor","2400 / N/A","2200 / N/A","N/A / 1200","Not required","N/A","","DD1.1a","general double ","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general","A means to protect walls from wheelchair damage to be provided","L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T3","N/A","N/A","N/A","N/A",null,"None","Minimal. To recharge appliances","None",0,null,10,"Allow sufficient space for safe access."]
["STN06","Equipment stores, room (physiotherapy)",null,null,"STN05","New Build","SL_90_50_27","Equipment stores","Store room for physiotherapy equipment","Storing wheelchair, mobility equipment or buggies appliance used by pupils","Storage (non-teaching)","Storage",2,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","Yes","Disabled access into the space required","Enclosed or semi-enclosed","off Corridor","2400 / N/A","2200 / N/A","N/A / 1200","Not required","N/A","","DD1.1a","general double ","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general","A means to protect walls from wheelchair damage to be provided","L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T3","N/A","N/A","N/A","N/A",null,"None","Minimal. To recharge appliances","None",0,null,10,"Allow sufficient space for safe access."]
["STN11","Cloakrooms, early years (50% circ)","Cloakrooms, early years (50% circ)","STN11","STN11","New Build","SL_90_20_14","Cloakrooms","Space for coat hooks and bench for bags to side of circulation area for pupils, acting a draught lobby","Storing pupils personal belongings (coats, bags, books, PE equipment etc).","Storage (non-teaching)","Storage",2,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access to at least 25% of coat hooks required","Enclosed",null,"2400 / N/A","2200 / N/A","N/A / 1700","Entrance doors","N/A","Contractor to Specify for approval","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F2.1","stores","C1.1","general","W1.1","general",null,"L4.4o","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",100,"man on, man off","No",null,"T3","Average","High","<=1.5","<=2.0",null,"None","None","None",0,null,2,"Allow sufficient space for safe access."]
["STN12","Cloakrooms, SEN (50% circ)",null,null,"STN11","New Build","SL_90_20_14","Cloakrooms","Space for coat hooks and bench for bags to side of circulation area for pupils, acting a draught lobby","Storing pupils personal belongings (coats, bags, books, PE equipment etc).","Storage (non-teaching)","Storage",2,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access to at least 25% of coat hooks required","Enclosed",null,"2400 / N/A","2200 / N/A","N/A / 1700","Entrance doors","N/A","Contractor to Specify for approval","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F2.1","stores","C1.1","general","W1.1","general",null,"L4.4o","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",100,"man on, man off","No",null,"T3","Average","High","<=1.5","<=2.0",null,"None","None","None",0,null,2,"Allow sufficient space for safe access."]
["STN15","Cloakrooms, secure room",null,null,"STN15","New Build","SL_90_20_14","Cloakrooms","Secure room for coats and bags to be dropped off by pupils, adjacent to pupil entrance","Storing pupils personal belongings (coats, bags, books, PE equipment etc).","Storage (non-teaching)","Storage",2,4,"-","-",0,0,null,0,12,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access to at least 25% of coat hooks required","Enclosed",null,"2400 / N/A","2200 / N/A","N/A / 1700","Entrance doors","N/A","Contractor to Specify for approval","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F2.1","stores","C1.1","general","W1.1","general",null,"L4.4o","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",100,"man on, man off","No",null,"T3","Average","High","<=1.5","<=2.0",null,"None","None","None",0,null,2,"Allow sufficient space for safe access."]
["STN20","General storerooms (off corridor)","General storerooms (off corridor)","STN20","STN20","New Build","SL_90_50_35","General storerooms","Store room for general materials or admin resources, typically opening off corridor","Storing teaching resources including books, files and digital equipment.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,5,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled access not required","Enclosed","off Corridor","2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","D4.1a","store room","N/A","no internal doorset required",null,null,"F2.1","stores","C1.1","general","W1.1","general"," ","L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,2,"CTS if Fire Containment."]
["STN22","General storerooms (central stock)","General storerooms (central stock)","STN22","STN20","New Build","SL_90_50_35","General storerooms","Storage of stock and stationery","Storing bulk items of paper or stock","Storage (non-teaching)","Storage",2,4,"-","-",0,0,null,0,8,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled access not required","Enclosed",null,"2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","D4.1a","store room","N/A","no internal doorset required",null,null,"F2.1","stores","C1.1","general","W1.1","general",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,4,"Staff-only access. Fire Containment."]
["STN23","General storerooms (linen)","General storerooms (linen)","STN23","STN20","New Build","SL_90_50_35","General storerooms","Storage for linen in residential areas","Storing items linen used in residential accommodation","Storage (non-teaching)","Storage",2,4,"-","-",0,0,null,0,4,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled access not required","Enclosed",null,"2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","D4.1a","store room","N/A","no internal doorset required",null,null,"F2.1","stores","C1.1","general","W1.1","general",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,4,"Staff-only access. Fire Containment."]
["STN25","General storerooms (community)","General storerooms (community)","STN25","STN20","New Build","SL_90_50_35","General storerooms","Storage for community use outside school core hours","Storing items used and provided by community users","Storage (non-teaching)","Storage",2,4,"-","-",0,0,null,0,4,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled access not required","Enclosed",null,"2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","D4.1a","store room","N/A","no internal doorset required",null,null,"F2.1","stores","C1.1","general","W1.1","general",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,4,"Staff-only access. Fire Containment."]
["STN31","Cleaners' stores","Cleaners' stores","STN31","STN31","New Build","SL_90_50_16","Cleaners' stores","Cleaners' store with sink","Filling and emptying buckets. Storing cleaning materials and equipment.","Storage (non-teaching)","Storage",2,4,"-","-",0,0,null,0,1.5,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled access not required","Enclosed",null,"2400 / N/A","2200 / N/A","N/A / 750","Not required","N/A","","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room. ","F3.4","chemical resistant non-slip","C1.2","humid areas","W2.2h","humid areas and toilets","Flooring suitable for heavy movable FF&E on castors ","L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A","Extract as Tech Annex 2F 6.3","None","Minimal","Hot and cold water to sink listed in School-specific SoA and ADS",0,null,6,"Staff-only access. Fire Containment."]
["STN32","Equipment stores, maintenance","Equipment stores, maintenance","STN32","STN32","New Build","SL_90_50_27","Equipment stores","General storage of maintenance equipment and resources such as floor cleaners","Filling and emptying buckets. Storing maintenance materials and equipment.","Storage (non-teaching)","Storage",2,4,"-","-",0,0,null,0,8,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled access not required","Enclosed",null,"2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","DD1.1a","general double ","N/A","no internal doorset required",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W1.1","general",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,2,"Staff-only access. Fire Containment."]
["STN50","Secure storerooms","Secure storerooms","STN50","STN50","New Build","SL_90_50_77","Secure storerooms","Secure storage of exam papers, archives or medical equipment and drugs","Storing examination papers, archived documents or other confidential items securely.","Storage (non-teaching)","Storage",2,4,"-","-",0,0,null,0,8,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled access not required","Securely enclosed",null,"2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room. Secure locks and ironmongery. 5-lever mortice locks or key pad required","F2.1","stores","C1.1","general","W1.1","general"," ","L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,2,"Staff-only access. Fire Containment. To suit examination board requirements (Joint Council for Qualifications (JCQ) or equivalent)."]
["STN51","Secure storerooms (medical)","Secure storerooms (medical)","STN51","STN50","New Build","SL_90_50_77","Secure storerooms","Secure storage of medical equipment and drugs","Storing medical items","Storage (non-teaching)","Storage",2,4,"-","SEN",0,0,null,0,3,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled access not required","Securely enclosed",null,"2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room. Secure locks and ironmongery. 5-lever mortice locks or key pad required","F2.1","stores","C1.1","general","W1.1","general",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,2,"Staff-only access. Fire Containment."]
["STN52","Gas storage spaces (oxygen cylinders)","Gas storage spaces (oxygen cylinders)","STN52","STN52","New Build","SL_55_20_34","Gas storage spaces","Secure storage of oxygen cylinders","Storing oxygen cylinders","Storage (non-teaching)","Storage",2,4,"-","SEN",0,0,null,0,3,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled and trolley access into the space required","Enclosed",null,"2400 / N/A","2200 / N/A","N/A / CTS","Not required","N/A","","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room. ","F1.1","general","C1.1","general","W1.1","general",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0]
["STN53","Chemicals stores, pool","Chemicals stores, pool","STN53","STN53","New Build","SL_90_50_13","Chemicals stores","Secure store room for chemicals used in hydrotherapy/warm water pool.","Storing chemicals used in hydrotherapy or warm water pool","Storage (non-teaching)","Storage",2,4,"-","SEN",0,0,null,0,5,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed",null,"2400 / N/A","2200 / N/A","N/A / CTS","Required","N/A","Contractor to Specify for approval","D5.1h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room. ","F3.4","chemical resistant non-slip","C3.2","humid areas","W3.2","humid areas and toilets","Floor finish capable of withstanding acid and alkali.","L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0]
["STN55","Equipment stores, room (appliances/ wheelchairs)","Equipment stores, appliance store (wheelchairs)","STN55","STN05","New Build","SL_90_50_27","Equipment stores","Store room for wheelchairs or other appliances","Storing wheelchair or appliance used by pupils","Storage (non-teaching)","Storage",2,4,"-","SEN",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled access required","Enclosed or semi-enclosed","off Corridor","2400 / N/A","2200 / N/A","N/A / 1200","Not required","N/A","","DD1.1a","general double ","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general","A means to protect walls from wheelchair damage to be provided","L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T3","N/A","N/A","N/A","N/A",null,"None","Minimal. To recharge appliances","None",0,null,2]
["STT00","Classroom stores, room (off classroom)","Classroom stores, room (off classroom)","STT00","STT00","New Build","SL_90_50_18","Classroom stores","Store room opening off a room for teaching resources or materials","Storing teaching resources including books, files and digital equipment.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed","off Classroom","2400 / N/A","2200 / N/A","N/A / 900","Not required","N/A","","D4.1a","store room","N/A","no internal doorset required",null,"Door to open outwards if store opens off teaching space.","F1.1","general","C1.1","general","W1.1","general",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,2]
["STT01","Classroom stores, room (off nursery)","Classroom stores, room (off nursery)","STT01","STT00","New Build","SL_90_50_18","Classroom stores","Store room for teaching resources and materials available to staff","Storing teaching resources and equipment.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,4,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed","off Nursery playroom","2400 / N/A","2200 / N/A","N/A / 900","Not required","N/A","","D4.1a","store room","N/A","no internal doorset required",null,"Door to open outwards if store opens off teaching space.","F1.1","general","C1.1","general","W1.1","general",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","None","None",0,null,2]
["STT02","Classroom stores, room (off reception)","Classroom stores, room (off reception)","STT02","STT00","New Build","SL_90_50_18","Classroom stores","Store room for teaching resources and materials available to staff","Storing teaching resources and equipment.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,3,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed","off Reception classroom","2400 / N/A","2200 / N/A","N/A / 900","Not required","N/A","","D4.1a","store room","N/A","no internal doorset required",null,"Door to open outwards if store opens off teaching space.","F1.1","general","C1.1","general","W1.1","general",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","None","None",0,null,2]
["STT03","Classroom stores, room (off infants and juniors)","Classroom stores, room (off infants and juniors)","STT03","STT00","New Build","SL_90_50_18","Classroom stores","Store room for teaching resources and materials available to staff","Storing teaching resources and equipment.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed","off Infants or Junior classrooms","2400 / N/A","2200 / N/A","N/A / 900","Not required","N/A","","D4.1a","store room","N/A","no internal doorset required",null,"Door to open outwards if store opens off teaching space.","F1.1","general","C1.1","general","W1.1","general",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","None","None",0,null,4]
["STT08","Equipment stores, drama","Equipment stores, drama","STT08","STT08","New Build","SL_90_50_27","Equipment stores","Store room for drama teaching resources, opening off drama studio","Storing drama teaching resources including costumes, props and some flats.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed","off Drama studio (and Assembly hall)","2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","DD1.1a","general double ","N/A","no internal doorset required",null,"Door to open outwards if store opens off teaching space.","F2.1","stores","C1.1","general","W1.1","general"," ","L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,2,"CTS if Fire Containment."]
["STT09","Classroom stores, bay (off classroom)","Classroom stores, bay (off classroom)","STT09","STT09","New Build","SL_90_50_18","Classroom stores","Storage bay opening off a classroom for teaching resources and materials available to staff","Storing teaching resources and equipment.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Semi-enclosed","off Classroom","2400 / N/A","2200 / N/A","N/A / 900","Not required","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,"Curtain or similar across doorway","F1.1","general","C1.1","general","W1.1","general"," ","L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","None","None",0,null,2]
["STT10","Teaching resources stores","Teaching resources stores","STT10","STT10","New Build","SL_90_50_87","Teaching resources stores","Store room for general teaching or ICT resources","Storing teaching resources including books, files and digital equipment.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,5,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled access not required","Enclosed","off Corridor","2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","D4.1a","store room","N/A","no internal doorset required",null,"Door to open outwards if store opens off teaching space.","F2.1","stores","C1.1","general","W1.1","general",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,4]
["STT13","Teaching resources stores (IT/ GT off corridor)","Teaching resources stores (IT/ GT off corridor)","STT13","STT10","New Build","SL_90_50_87","Teaching resources stores","Store room for general teaching or ICT resources","Storing teaching resources including books, files and digital equipment.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,5,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled access not required","Enclosed","off Corridor","2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","D4.1a","store room","N/A","no internal doorset required",null,"Door to open outwards if store opens off teaching space.","F2.1","stores","C1.1","general","W1.1","general",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,4]
["STT15","Teaching resources stores (specialist)","Teaching resources stores (specialist)","STT15","STT10","New Build","SL_90_50_87","Teaching resources stores","Store room opening off a teaching space for specialist teaching resources or work in progress","Storing teaching resources and materials relevant to the teaching space (e.g. art, graphics or music) and/or work in progress. Storing teaching resources including books, files and equipment.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,5,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed","off Primary practical room","2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","D4.1a","store room","N/A","no internal doorset required",null,"Door to open outwards if store opens off teaching space.","F2.1","stores","C1.1","general","W1.1","general"," ","L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,2,"CTS if Fire Containment."]
["STT16","Teaching resources stores (off art room)","Teaching resources stores (off art room)","STT16","STT10","New Build","SL_90_50_87","Teaching resources stores","Store room for art teaching resources or work in progress","Storing teaching resources and materials relevant to the teaching space (e.g. art, graphics or music) and/or work in progress. Storing teaching resources including books, files and equipment.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,5,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed","off Art room","2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","D4.1a","store room","N/A","no internal doorset required",null,"Door to open outwards if store opens off teaching space.","F2.1","stores","C1.1","general","W1.1","general",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,2]
["STT17","Teaching resources stores (music)","Teaching resources stores (music)","STT17","STT10","New Build","SL_90_50_87","Teaching resources stores","Store room for music teaching resources or instruments","Storing teaching resources including books, files and digital equipment.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled access not required","Enclosed","in Music practice suite","2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","D4.1a","store room","N/A","no internal doorset required",null,"Door to open outwards if store opens off teaching space.","F2.1","stores","C1.1","general","W1.1","general",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,4]
["STT18","Teaching resources stores (off DT studio)","Teaching resources stores (off DT studio)","STT18","STT10","New Build","SL_90_50_87","Teaching resources stores","Store room opening off a teaching space for specialist teaching resources or work in progress","Storing teaching resources and materials relevant to the teaching space (e.g. art, graphics or music) and/or work in progress. Storing teaching resources including books, files and equipment.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,5,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed","off DT studio","2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","D4.1a","store room","N/A","no internal doorset required",null,"Door to open outwards if store opens off teaching space.","F2.1","stores","C1.1","general","W1.1","general",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,4]
["STT21","Science prep rooms (central)","Science prep rooms (central)","STT21","STT20","New Build","SL_25_80_75","Science preparation rooms","Technician's preparation/ store room for all labs or studios in suite","Administrative tasks requiring ICT. Preparation of materials for practical activities. Stocktaking. Storing and cleaning equipment.","Storage (teaching)","Light practical (science)",2.5,4,"K","-",4,3.7,0,50,"As SoA","As SoA","As SoA","As SoA","As SoA","N/A","None","Disabled and trolley access into the space required","Enclosed",null,"3300 / 2700 (2700 / 2400 if <27m2)","2700 / 2400","7800 / 7000","Not required","N/A","","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L1.1c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, abs off","Yes",null,"T5","Low","Medium","<=1.0","<=1.0","Ventilation as Tech Annex 2F 7.7","Gas taps at preparation benching, minimum total one gas taps per technician","To suit equipment","Cold water to wet serviced bollards or similar listed under FF&E, hot and cold to belfast or hand wash sink; chemically resistance drainage.",10,2,4,"Fire Containment. Gas cylinders to be safely clamped. Radioactive cupboard should be fixed to a wall or bench 2m away from occupied areas"]
["STT22","Science prep rooms (satellite)","Science prep rooms (satellite)","STT22","STT20","New Build","SL_25_80_75","Science preparation rooms","Technician's preparation/ store room for some labs or studios ","Administrative tasks requiring ICT. Preparation of materials for practical activities. Stocktaking. Storing and cleaning equipment.","Storage (teaching)","Light practical (science)",2.5,4,"K","-",4,3.7,0,50,"As SoA","As SoA","As SoA","As SoA","As SoA","N/A","None","Disabled and trolley access into the space required","Enclosed",null,"2700 / 2400 (3300 / 2700 if >27m2)","2700 / 2400","7800 / 7000","Not required","N/A","","D1.1av","general","D1.1av","general",null,null,"F3.4","chemical resistant non-slip","C1.1","general","W2.1h","science","Flooring suitable for heavy movable FF&E on castors ","L1.1c","Required in 80% of spaces with L1 code","Required in 80% of spaces with L1 code","Required in remaining spaces with L1 code","Required in remaining spaces with L1 code",500,"man on, abs off","Yes",null,"T5","Low","Medium","<=1.0","<=1.0","Ventilation as Tech Annex 2F 7.7","Gas taps at preparation benching, minimum total one gas taps per technician","To suit equipment","Cold water to wet serviced bollards or similar listed under FF&E, hot and cold to belfast or hand wash sink; chemically resistance drainage.",9,2,4,"Fire Containment. Gas cylinders to be safely clamped. Radioactive cupboard should be fixed to a wall or bench 2m away from occupied areas"]
["STT23","Chemicals stores, science","Chemicals stores, science","STT23","STT23","New Build","SL_90_50_13","Chemicals stores","Chemical store associated with science prep room","Storing chemicals, some hazardous.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,7,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed","off Science prep room","2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","D5.2h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room. ","F3.4","chemical resistant non-slip","C1.1","general","W2.1h","humid areas and toilets","Flooring suitable for heavy movable FF&E on castors. Floor should be bunded and impervious to chemicals. ","L5.5p","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T3","N/A","N/A","N/A","N/A","Ventilation as Tech Annex 2F 7.7","None","None","None",0,null,6,"Staff only access. Fire Containment. Fire resistant cupboards for highly flammable liquids and most hazardous chemicals provided as Group 3 FF&E items"]
["STT25","Teaching resources stores, science",null,null,"STT23","New Build","SL_90_50_87","Teaching resources stores","Store room opening off a teaching space for science resources or work in progress","Storing science equipment and materials including chemicals, some hazardous.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,7,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed","off Science laboratories","2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","D5.2h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room. ","F3.4","chemical resistant non-slip","C1.1","general","W2.1h","humid areas and toilets","Flooring suitable for heavy movable FF&E on castors. Floor should be bunded and impervious to chemicals. ","L5.5p","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T3","N/A","N/A","N/A","N/A","Ventilation as Tech Annex 2F 7.7","None","None","None",0,null,6,"Staff only access. Fire Containment. Fire resistant cupboards for highly flammable liquids and most hazardous chemicals provided as Group 3 FF&E items"]
["STT26","Teaching resources stores, pool",null,null,"STT23","New Build","SL_90_50_87","Teaching resources stores","Store room opening off a teaching space for science resources or work in progress","Storing teaching resources and materials","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,"As SoA","-","-",0,{"$error":"#VALUE!"},"N/A","None","Full disabled access required","Enclosed","off pool","2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","D5.2h","strong, no vision panel","N/A","no internal doorset required",null,"Door should be unlockable from inside the room. ","F3.4","chemical resistant non-slip","C1.1","general","W2.1h","humid areas and toilets","Flooring suitable for heavy movable FF&E on castors. Floor should be bunded and impervious to chemicals. ","L5.5p","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T3","N/A","N/A","N/A","N/A","Ventilation as Tech Annex 2F 7.7","None","None","None",0,null,6,"Staff only access. Fire Containment. "]
["STT32","DT prep rooms","DT prep rooms","STT32","STT32","New Build","SL_25_80_85","Design technology preparation rooms","Technician's preparation/store room for all resistant materials rooms","Maintaining tools and equipment. Some administrative work requiring ICT. Storing and preparing resistant materials (wood, metal, plastics) and components for pupils' use.","Storage (teaching)","Heavy practical (workshop)",3.5,4,"I","-",22,3.7,null,1,"As SoA","As SoA","As SoA",1,"As SoA","N/A","None","Disabled access into the space required","Enclosed","adjacent to Workshop(s)","3300 / 2700","2700 / 2400","7800 / 4350","Double doors","N/A","Contractor to Specify for approval","D5.1av","strong, with vision panel","D5.1av","strong, with vision panel",null,null,"F5.4","heavy practical","C1.1","general","W4.1","rough","Flooring suitable for heavy movable FF&E on castors ","L4.1c","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",500,"man on, abs off","Yes",null,"T5","High","High","<=1.0","<=1.0","Specialist dust extraction to serve adjacent workshops. Extract ventilation based on Tech Annex 2F 7.5 and 7.6.","None","To suit equipment","Hot and cold water to sink listed in School-specific SoA and ADS",3,null,2,"Staff-only access. Fire Containment."]
["STT33","Teaching resources stores (off DT workshop)","Teaching resources stores (off DT workshop)","STT33","STT10","New Build","SL_90_50_87","Teaching resources stores","Store room for teaching resources or materials for resistant materials room","Storing resistant materials (wood, metal, plastics) and components for pupils' use.","Storage (teaching)","Storage",2,4,"-","SEN",0,0,null,0,7,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled and trolley access into the space required","Enclosed","off Workshop","2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","D4.1a","store room","N/A","no internal doorset required",null,null,"F2.1","stores","C1.1","general","W1.1","general",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0]
["STT34","Food prep rooms","Food prep rooms","STT34","STT34","New Build","SL_25_80_30","Food preparation rooms","Technician's preparation/store room for all food rooms","Laundry of food room linen. Preparing food ingredients for lessons. Storing cooking equipment and ingredients.","Storage (teaching)","Heavy practical (clean)",1.5,4,"-","-",0,0,null,0,10,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access into the space required","Enclosed","off Food room","3300 / 2700","2400 / N/A","N/A / 1700","Not required","N/A","","D5.2av","strong, with vision panel","D5.2av","strong, with vision panel",null,null,"F3.4h","hygienic non-slip","C1.2","humid areas","W3.2","humid","Flooring suitable for heavy movable FF&E on castors ","L4.1p","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",500,"man on, abs off","No",null,"T5","Average","Medium","<=1.0","<=1.2",null,"None","Dado on 2 walls","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",0,null,2,"Staff-only access. CTS if Fire Containment."]
["STT35","Food stores, off food room","Food stores, off food room","STT35","STT35","New Build","SL_90_50_29","Food stores","Store room opening off a food room for food, teaching resources or materials","Storing dry food and cooking equipment.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,5,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed","off Food room","2400 / N/A","2200 / N/A","N/A / 1700","Not required","N/A","","D4.2a","food store","N/A","no internal doorset required",null,"Door to open outwards if store opens off teaching space.","F3.4h","hygienic non-slip","C1.2","humid areas","W3.2","humid",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,4,"CTS if Fire Containment."]
["STT41","Teaching resources stores (off LRC)","Teaching resources stores (off LRC)","STT41","STT10","New Build","SL_90_50_87","Teaching resources stores","Store room for teaching resources or materials","Storing teaching resources including books, files and digital equipment.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,3,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed","off LRC","2400 / N/A","2200 / N/A","N/A / 900","Not required","N/A","","D4.1a","store room","N/A","no internal doorset required",null,"Door to open outwards if store opens off teaching space.","F2.1","stores","C1.1","general","W1.1","general",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,4]
["STT42","Classroom stores, room (off SEN room)","Classroom stores, room (off SEN room)","STT42","STT00","New Build","SL_90_50_18","Classroom stores","Store room for teaching resources or materials","Storing teaching resources including books, files and digital equipment.","Storage (teaching)","Storage",2,4,"-","-",0,0,null,0,5,"-","-",0,{"$error":"#VALUE!"},"N/A","None","Disabled access not required","Enclosed","off SEN resource space","2400 / N/A","2200 / N/A","N/A / 900","Not required","N/A","","D4.1a","store room","N/A","no internal doorset required",null,"Door to open outwards if store opens off teaching space.","F1.1","general","C1.1","general","W1.1","general",null,"L5.5l","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No",null,"T1","N/A","N/A","N/A","N/A",null,"None","Minimal","None",0,null,4]
["SUP01","Faith spaces (chapel)","Faith spaces (chapel)","SUP01","SUP00","New Build","SL_25_90_30","Faith spaces","Chapel or similar for small group prayer and reflection","Individual/small group prayer and reflection. Private counselling.","Learning resources","General",1.5,4,"A","-",2,1.1000000000000001,null,0,"As SoA","As SoA","As SoA",0,"As SoA","N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400 (3300 / 2700 if >27m2)","2400 / N/A","N/A / 3400","Optional","CTS","Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general"," ","L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","No",null,"T5","Low","Low","0.8 - 1.2","0.8 - 1.2",null,"None","Where required","None",0,null,2]
["SUP02","Faith spaces (prayer room)","Faith spaces (prayer room)","SUP02","SUP00","New Build","SL_25_90_30","Faith spaces","Prayer room or similar for small group prayer and reflection","Individual/small group prayer and reflection. Private counselling.","Learning resources","General",1.5,4,"A","-",2,1.1000000000000001,null,0,"As SoA","As SoA","As SoA",0,"As SoA","N/A","None","Disabled access into the space required","Enclosed",null,"2700 / 2400 (3300 / 2700 if >27m2)","2400 / N/A","N/A / 3400","Optional","CTS","Contractor to Specify for approval if provided","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L2.6i","No requirement","Required in 65% of spaces with L2 code","Required in remaining spaces with L2 code","No requirement",300,"key on, day dim, abs off","No",null,"T5","Low","Low","0.8 - 1.2","0.8 - 1.2",null,"None","Where required","None",0,null,2]
["SUP05","Staff workrooms (sacristy)","Staff workrooms (sacristy)","SUP05","OFF33","New Build","SL_90_20_86","Staff workrooms","Storage and changing area adjacent to chapel","Administrative tasks (including use of ICT) and filing. Storage.","Learning resources","General",1.5,4,"B","-",2,1.6,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access into the space required","Enclosed",null,"2700 / 2400","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F1.1","general","C1.1","general","W1.1","general",null,"L3.1k","No requirement","Required in 50% of spaces with L3 code","No requirement","No requirement",300,"man on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.0",null,"None","To suit ICT","None",0,null,2]
["TOC01","Changing rooms, with showers (pupils)","Changing rooms, with showers (pupils)","TOC01","TOC01","New Build","SL_90_20_13","Changing rooms","Wet changing and shower cubicles for male or female pupils","Changing and showering for PE.","Non-net","Non-net",null,null,"A","-",2,1.1000000000000001,null,0,"As SoA","As SoA","As SoA",0,"As SoA","11-19","Yes","Disabled access not required unless accessible changing to be part of the facility","Enclosed","near to indoor PE facilities","3300 / 2700 (2700 / 2400 if <27m2)","2400 / N/A","7800 / CTS","Required","CTS","Contractor to Specify for approval","D3.2cv","toilets","N/A","no internal doorset required",null,null,"F7.3h","wet area","C2.2/ 2.3","humid/ wet ","W3.2/ 3.3","humid/ wet","Flooring in barefoot areas shall be barefoot slip resistance category B Ceiling type C3 and wall type W3w in shower areas. Floor finish in shower areas to provide drainage ","L4.4o","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",100,"pres on, abs off","No","Water / moisture grade luminaires. IP rating for wet areas","T6","High","High","<=1.5","<=2.0","Locally controlled mechanical ventilation shall be provided as specified in Tech Annex 2F 6.3","None","Hand dryer","Hot and cold drinking water to all sinks, equipment and appliances",0]
["TOC02","Accessible (and staff) changing rooms","Accessible (and staff) changing rooms","TOC02","TOC02","New Build","SL_35_80_01","Accessible changing rooms","Wet changing and shower cubicle for male or female staff, or for disabled or community users","Changing and showering for staff member or disabled pupil or visitor, for PE.","Non-net","Non-net",null,null,"T","-",0.5,3,null,0,6,2,2,0,3,"11-19","Yes","Full disabled access required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Not required","N/A","","D2.2d","strong","N/A","no internal doorset required",null,"Ergonomic handle and Access control system to be agreed with school. If door leaf opens inwards it shall be openable outwards in an emergency","F7.3h","wet area","C2.3","wet areas","W3.3","wet areas","Flooring in barefoot areas shall be barefoot slip resistance category B Ceiling type C3 and wall type W3w in shower areas. Floor finish in shower areas to provide drainage ","L4.4o","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",100,"pres on, abs off","No","Water / moisture grade luminaires. IP rating for wet areas","T6","High","High","<=1.5","<=2.0","Locally controlled mechanical ventilation shall be provided as specified in Tech Annex 2F 6.3","None","Hand dryer","Hot and cold drinking water to all sinks, equipment and appliances",0,null,null,"Emergency call system"]
["TOC03","Changing rooms, ablutions and shoe space","Changing rooms, ablutions and shoe space","TOC03","TOC03","New Build","SL_90_20_13","Changing rooms","Changing and washing for pupils, adjacent to a prayer space","Changing and washing","Non-net","Non-net",null,null,"A","-",2,1.1000000000000001,null,0,"As SoA","As SoA","As SoA",0,"As SoA","N/A","None","Disabled access into the space required","Enclosed","off Faith space","2400 / N/A","2400 / N/A","N/A / 1700","Not required","CTS","","D1.1av","general","N/A","no internal doorset required",null,null,"F7.3h","wet area","C2.2","humid areas","W3.2","humid areas",null,"L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off","No",null,"T5","Low","Medium","<=1.0","<=1.0",null,"None","Minimal","Hot and cold drinking water to all sinks, equipment and appliances",0,null,2]
["TOC04","Hygiene rooms","Hygiene rooms","TOC04","TOC04","New Build","SL_35_80_39","Hygiene rooms","Hygiene room for disabled pupils' wash-down, showering and toileting using a ceiling-mounted hoist, with wc, wash-hand basin, shower and a shower-bed","Assisted shower. Peninsular WC able to be accessed from either side. Room for changing pupils, with bed against wall.","Non-net","Non-net",null,null,"T","-",0.5,3,null,0,12,4,4,0,5,"CTS","None","Full disabled access required","Enclosed",null,"2700 / N/A","2700 / 2400","N/A / 2700","Not required","N/A","","D2.2d","strong","CTS","Contractor to specify",null,"Ergonomic handle and Access control system to be agreed with school. If door leaf opens inwards it shall be openable outwards in an emergency","F7.3h","wet area","C2.3","wet areas","W3.3","wet areas","Flooring in barefoot areas shall be barefoot slip resistance category B Ceiling type C3 and wall type W3w in shower areas. Floor finish in shower areas to provide drainage ","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off","No","Water / moisture grade luminaires if shower bed provided. Avoid direct downlighting over changing bed","T6","Average","High","<=1.5","<=2.0","Mechanical ventilation shall be provided as specified in Tech Annex 2F 7.8.1.","None","Hand dryer","Hot and cold drinking water to all sinks, equipment and appliances in Annex 2A Table 1",0,null,4,"Emergency call system"]
["TOC05","Hygiene rooms (small 1 door)","Hygiene rooms (small 1 door)","TOC05","TOC04","New Build","SL_35_80_39","Hygiene rooms","Hygiene room for disabled pupils’ wash-down and toileting, using a ceiling-mounted hoist, with wc and wash-hand basin, and space for shower-bed","Assisted shower. Peninsular WC able to be accessed from either side. Room for changing pupils, with bed against wall.","Non-net","Non-net",null,null,"T","-",0.5,3,null,0,8,3,3,0,4,"CTS","None","Full disabled access required","Enclosed",null,"2700 / 2400","2700 / 2400","N/A / 2700","Not required","N/A","","D2.2d","strong","N/A","no internal doorset required",null,"Ergonomic handle and Access control system to be agreed with school. If door leaf opens inwards it shall be openable outwards in an emergency","F7.3h","wet area","C2.3","wet areas","W3.3","wet areas","Flooring in barefoot areas shall be barefoot slip resistance category B Ceiling type C3 and wall type W3w in shower areas. Floor finish in shower areas to provide drainage ","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off","No","Water / moisture grade luminaires if shower bed provided. Avoid direct downlighting over changing bed","T6","Average","High","<=1.5","<=2.0","Mechanical ventilation shall be provided as specified in Tech Annex 2F 7.8.1.","None","Hand dryer","Hot and cold drinking water to all sinks, equipment and appliances in Annex 2A Table 1",0,null,4,"Emergency call system"]
["TOC06","Hygiene rooms, small (2 doors)","Hygiene rooms, small (2 doors)","TOC06","TOC04","New Build","SL_35_80_39","Hygiene rooms","Hygiene room for disabled pupils wash-down and toileting, using a ceiling-mounted hoist, with wc and wash-hand basin, and space for shower-bed; accessed from both nursery and main school","Room for changing pupils, with bed against wall, and two doors: one to nursery playroom (where applicable) and one to rest of school.","Non-net","Non-net",null,null,"T","-",0.5,3,null,0,9,3,3,0,4,"CTS","None","Full disabled access required","Enclosed",null,"2700 / 2400","2700 / 2400","N/A / 2700","Not required","N/A","","D2.2d","strong","D2.2d","strong",null,"2 doors: one to nursery playroom (where applicable) and one to rest of school. Ergonomic handle and Access control system to be agreed with school. If door leaf opens inwards it shall be openable outwards in an emergency","F7.3h","wet area","C2.3","wet areas","W3.3","wet areas","Flooring in barefoot areas shall be barefoot slip resistance category B Ceiling type C3 and wall type W3w in shower areas. Floor finish in shower areas to provide drainage ","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off","No","Water / moisture grade luminaires if shower bed provided. Avoid direct downlighting over changing bed","T6","Average","High","<=1.5","<=2.0","Mechanical ventilation shall be provided as specified in Tech Annex 2F 7.8.1.","None","Hand dryer","Hot and cold drinking water to all sinks, equipment and appliances in Annex 2A Table 1",0,null,4,"Emergency call system"]
["TOC10","Toilets, suite","Toilets, suite","TOC10","TOC10","New Build","SL_35_80_89","Toilets","Staff toilet cubicles and hand-wash/ dry area","Suite of toilet cubicles and hand-wash/ dry area, for staff","Non-net","Non-net",null,null,"T","-",0.5,3,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Full disabled access not required","Enclosed",null,"2700 / 2400","2200 / N/A","N/A / CTS","Not required","N/A","","D3.2cv","toilets","N/A","no internal doorset required",null,null,"F7.3h","wet area","C2.2","humid areas","W2.2h","humid areas and toilets","Tiling or similar above wash-hand basin as a minimum","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off","No",null,"T3","Average","High","<=1.5","<=2.0","Locally controlled mechanical ventilation shall be provided as specified in Tech Annex 2F 6.3","None","Hand dryer","Hot and cold drinking water to all sinks, equipment and appliances in Annex 2A Table 1",0]
["TOC12","Toilets, suite (staff)","Toilets, suite (staff)","TOC12","TOC10","New Build","SL_35_80_89","Toilets","Staff toilet cubicles and hand-wash/ dry area","Suite of toilet cubicles and hand-wash/ dry area, for staff","Non-net","Non-net",null,null,"T","-",0.5,3,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Full disabled access not required","Enclosed",null,"2700 / 2400","2200 / N/A","N/A / CTS","Not required","N/A","","D3.2cv","toilets","N/A","no internal doorset required",null,null,"F7.3h","wet area","C2.2","humid areas","W2.2h","humid areas and toilets","Tiling or similar above wash-hand basin as a minimum","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off","No",null,"T3","Average","High","<=1.5","<=2.0","Locally controlled mechanical ventilation shall be provided as specified in Tech Annex 2F 6.3","None","Hand dryer","Hot and cold drinking water to all sinks, equipment and appliances in Annex 2A Table 1",0]
["TOC13","Toilets, suite (pupils)","Toilets, suite (pupils)","TOC13","TOC10","New Build","SL_35_80_89","Toilets","Pupils' toilet cubicles and hand-wash/ dry area","Suite of toilet cubicles and hand-wash/ dry area, for mainstream pupils","Non-net","Non-net",null,null,"T","-",0.5,3,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Full disabled access not required","Enclosed",null,"2700 / 2400","2200 / N/A","N/A / CTS","Not required","N/A","","D3.2cv","toilets","N/A","no internal doorset required",null,null,"F7.3h","wet area","C2.2","humid areas","W2.2h","humid areas and toilets","Tiling or similar above wash-hand basin as a minimum","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off","No",null,"T3","Average","High","<=1.5","<=2.0","Locally controlled mechanical ventilation shall be provided as specified in Tech Annex 2F 6.3","None","Hand dryer","Hot and cold drinking water to all sinks, equipment and appliances in Annex 2A Table 1",0]
["TOC14","Toilets, suite (pupils, other)","Toilets, suite (pupils, other)","TOC14","TOC10","New Build","SL_35_80_89","Toilets","Pupils' toilet cubicles and hand-wash/ dry area","Suite of toilet cubicles and hand-wash/ dry area, for mainstream pupils","Non-net","Non-net",null,null,"T","-",0.5,3,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Full disabled access not required","Enclosed",null,"2700 / 2400","2200 / N/A","N/A / CTS","Not required","N/A","","D3.2cv","toilets","N/A","no internal doorset required",null,null,"F7.3h","wet area","C2.2","humid areas","W2.2h","humid areas and toilets","Tiling or similar above wash-hand basin as a minimum","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off","No",null,"T3","Average","High","<=1.5","<=2.0","Locally controlled mechanical ventilation shall be provided as specified in Tech Annex 2F 6.3","None","Hand dryer","Hot and cold drinking water to all sinks, equipment and appliances in Annex 2A Table 1",0]
["TOC15","Toilets, individual (pupil)","Toilets, individual (pupil)","TOC15","TOC15","New Build","SL_35_80_89","Toilets","Individual pupils toilet, sink and hand-wash/ dry in one space","Toilet and wash hand basin for mainstream pupils","Non-net","Non-net",null,null,"T","-",0.5,3,null,0,2,1,1,0,2,"CTS","None","Disabled access not required","Enclosed",null,"2400 / N/A","2200 / N/A","N/A / 800","Not required","N/A","","D3.2b","toilets","N/A","no internal doorset required",null,"Door leaf shall open inwards but be openable outwards in an emergency","F7.3h","wet area","C2.2","humid areas","W2.2h","humid areas and toilets","Tiling or similar above wash-hand basin as a minimum","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off","No",null,"T3","Average","High","<=1.5","<=2.0","A locally controlled extract system shall be provided as specified in Tech Annex 2F 6.3","None","Hand dryer","Hot and cold drinking water to all sinks, equipment and appliances in Annex 2A Table 1",0]
["TOC16","Toilets, individual (staff)","Toilets, individual (staff)","TOC16","TOC15","New Build","SL_35_80_89","Toilets","Individual staff toilet, sink and hand-wash/ dry in one space","Toilet and wash hand basin for staff or visitors","Non-net","Non-net",null,null,"T","-",0.5,3,null,0,2,1,1,0,2,"N/A","None","Disabled access not required","Enclosed",null,"2400 / N/A","2200 / N/A","N/A / 800","Not required","N/A","","D3.2b","toilets","N/A","no internal doorset required",null,null,"F7.3h","wet area","C2.2","humid areas","W2.2h","humid areas and toilets","Tiling or similar above wash-hand basin as a minimum","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off","No",null,"T3","Average","High","<=1.5","<=2.0","A locally controlled extract system shall be provided as specified in Tech Annex 2F 6.3","None","Hand dryer","Hot and cold drinking water to all sinks, equipment and appliances in Annex 2A Table 1",0]
["TOC21","Accessible (and staff) toilets","Accessible (and staff) toilets","TOC21","TOC21","New Build","SL_35_80_03","Accessible toilets","Accessible toilets suitable for disabled pupils as well as any staff or visitors","Unisex toilet and wash hand basin for non-ambulant pupils/adults, or ambulant staff or visitors.","Non-net","Non-net",null,null,"T","-",0.5,3,null,0,3.8,1,1,0,2,"N/A","Optional","Full disabled access required","Enclosed",null,"2400 / N/A","2200 / N/A","N/A / 2300","Not required","N/A","","D2.2d","strong","N/A","no internal doorset required",null,"Ergonomic handle and Access control system to be agreed with school. If door leaf opens inwards it shall be openable outwards in an emergency","F7.3h","wet area","C2.2","humid areas","W2.2h","humid areas and toilets","Tiling or similar above wash-hand basin as a minimum","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off","No",null,"T3","Average","High","<=1.5","<=2.0","A locally controlled extract system shall be provided as specified in Tech Annex 2F 6.3","None","Hand dryer","Hot and cold drinking water to all sinks, equipment and appliances in Annex 2A Table 1",0]
["TOC22","Accessible toilets (pupils)",null,null,"TOC21","New Build","SL_35_80_03","Accessible toilets","Accessible toilets suitable for disabled pupils (counting toward number of pupil toilets)","Unisex toilet and wash hand basin for non-ambulant pupils","Non-net","Non-net",null,null,"T","-",0.5,3,null,0,3.8,1,1,0,2,"N/A","Optional","Full disabled access required","Enclosed",null,"2400 / N/A","2200 / N/A","N/A / 2300","Not required","N/A","","D2.2d","strong","N/A","no internal doorset required",null,"Ergonomic handle and Access control system to be agreed with school. If door leaf opens inwards it shall be openable outwards in an emergency","F7.3h","wet area","C2.2","humid areas","W2.2h","humid areas and toilets","Tiling or similar above wash-hand basin as a minimum","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off","No",null,"T3","Average","High","<=1.5","<=2.0","A locally controlled extract system shall be provided as specified in Tech Annex 2F 6.3","None","Hand dryer","Hot and cold drinking water to all sinks, equipment and appliances in Annex 2A Table 1",0]
["TOC30","Supervisable toilets","Supervisable toilets","TOC30","TOC30","New Build","SL_35_80_85","Supervisable toilets","Pupils' toilets and hand-wash/ dry area that are easily supervisable","Toilet cubicles with shared hand washing and drying facilities, with low walls to allow supervision by staff","Non-net","Non-net",null,null,"T","-",0.5,3,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access not required","Semi-enclosed","off playroom or classroom","2700 / 2400","2200 / N/A","N/A / CTS","Not required","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,"Low level cubicles screens and doors to allow adult supervision","F7.3h","wet area","C1.1","general","W2.2h","humid areas and toilets","Tiling or similar above wash-hand basin as a minimum","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off","No",null,"T5","Average","High","<=1.5","<=2.0","A locally controlled extract system shall be provided as specified in Tech Annex 2F 6.3","None","Hand dryer","Hot and cold drinking water to all sinks, equipment and appliances in Annex 2A Table 1",0]
["TOC31","Supervisable toilets (early years)","Supervisable toilets (early years)","TOC31","TOC30","New Build","SL_35_80_85","Supervisable toilets","Pupils' toilets and hand-wash/ dry area for early years, easily supervisable","Toilet cubicles with shared hand washing and drying facilities, with low walls to allow supervision by staff","Non-net","Non-net",null,null,"T","-",0.5,3,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access not required","Semi-enclosed","off playroom or classroom","2700 / 2400","2200 / N/A","N/A / CTS","Not required","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,"Low level cubicles screens and doors to allow adult supervision","F7.3h","wet area","C1.1","general","W2.2h","humid areas and toilets","Tiling or similar above wash-hand basin as a minimum","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off","No",null,"T5","Average","High","<=1.5","<=2.0","A locally controlled extract system shall be provided as specified in Tech Annex 2F 6.3","None","Hand dryer","Hot and cold drinking water to all sinks, equipment and appliances in Annex 2A Table 1",0]
["TOC32","Supervisable toilets (SEN)","Supervisable toilets (SEN)","TOC32","TOC30","New Build","SL_35_80_85","Supervisable toilets","Pupils' toilets and hand-wash/ dry area for SEN pupils, easily supervisable","Toilet cubicles with shared hand washing and drying facilities, with low walls to allow supervision by staff","Non-net","Non-net",null,null,"T","-",0.5,3,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Full disabled access required","Semi-enclosed","off SEN classroom","2700 / 2400","2200 / N/A","N/A / CTS","Not required","N/A","","N/A","no internal doorset required","N/A","no internal doorset required",null,null,"F7.3h","wet area","C1.1","general","W2.2h","humid areas and toilets","Tiling or similar above wash-hand basin as a minimum","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off","No",null,"T5","Average","High","<=1.5","<=2.0","A locally controlled extract system shall be provided as specified in Tech Annex 2F 6.3","None","Hand dryer","Hot and cold drinking water to all sinks, equipment and appliances in Annex 2A Table 1",0]
["TOC51","Changing rooms, with showers (ambulant)","Changing rooms, with showers (pupils)","TOC51","TOC51","New Build","SL_90_20_13","Changing rooms","Wet changing and shower cubicle(s) for male or female pupil(s) with special needs","Changing and showering for PE","Non-net","Non-net",null,null,"C","SEN",4,1.7,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","Yes","Full disabled access required","Enclosed",null,"2700 / N/A","2200 / N/A","7800 / CTS","Required","CTS","Contractor to Specify for approval","D3.2cv","toilets","N/A","no internal doorset required",null,"Access control system to be agreed with school","F7.3h","wet area","C2.2/ 2.3","humid/ wet ","W3.2/ 3.3","humid/ wet","Flooring in barefoot areas shall be barefoot slip resistance category B Ceiling type C3 and wall type W3w in shower areas. Floor finish in shower areas to provide drainage ","L4.4o","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",100,"pres on, abs off","No","Water / moisture grade luminaires. IP rating for wet areas","T6","High","High","<=1.5","<=2.0","Locally controlled mechanical ventilation shall be provided as specified in Tech Annex 2F 6.3","None","Hand dryer","Hot and cold drinking water to all sinks, equipment and appliances",0]
["TOC52","Changing cubicles, with showers (ambulant)","Changing rooms, with showers (pupils)","TOC51","TOC51","New Build","SL_90_20_13","Changing rooms","Wet changing and shower in individual cubicle(s) for male or female pupil(s) with special needs","Changing and showering for PE","Non-net","Non-net",null,null,"C","SEN",4,1.7,null,0,"As SoA","As SoA","As SoA",0,"As SoA","CTS","Yes","Full disabled access required","Enclosed",null,"2700 / N/A","2200 / N/A","7800 / CTS","Required","CTS","Contractor to Specify for approval","D3.2cv","toilets","N/A","no internal doorset required",null,"Access control system to be agreed with school","F7.3h","wet area","C2.2/ 2.3","humid/ wet ","W3.2/ 3.3","humid/ wet","Flooring in barefoot areas shall be barefoot slip resistance category B Ceiling type C3 and wall type W3w in shower areas. Floor finish in shower areas to provide drainage ","L4.4o","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",100,"pres on, abs off","No","Water / moisture grade luminaires. IP rating for wet areas","T6","High","High","<=1.5","<=2.0","Locally controlled mechanical ventilation shall be provided as specified in Tech Annex 2F 6.3","None","Hand dryer","Hot and cold drinking water to all sinks, equipment and appliances",0]
["TOC53","Hygiene rooms, non-ambulant","Hygiene rooms, non-ambulant","TOC53","TOC53","New Build","SL_35_80_39","Hygiene rooms","Hygiene room for disabled pupils' wash-down, showering and toileting using a ceiling-mounted hoist, with wc, wash-hand basin, and sluice, and space for a shower-bed","Room for changing pupils and washing down, with bed against wall","Non-net","Non-net",null,null,"T","SEN",0.5,3,null,0,15,5,5,0,6,"CTS","None","Full disabled access required","Enclosed",null,"2700 / N/A","2700 / 2400","N/A / CTS","Not required","N/A","","D2.2d","strong","N/A","no internal doorset required",null,"Ergonomic handle. If door to open out, to have horizontal rail to enable closing. ","F7.3h","wet area","C2.3","wet areas","W3.3","wet areas","Flooring in barefoot areas shall be barefoot slip resistance category B Ceiling type C3 and wall type W3w in shower areas. Floor finish in shower areas to provide drainage ","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off","No","Water / moisture grade luminaires if shower bed provided. Avoid direct downlighting over changing bed","T7","Average","High","<=1.5","<=2.0","Mechanical ventilation shall be provided as specified in Tech Annex 2F 7.8.1.6","None","Hand dryer","Hot and cold drinking water to all sinks, equipment and appliances in Annex 2A Table 1",0,null,4,"Emergency call system"]
["TOC54","Hygiene rooms, non-ambulant (peninsular)","Hygiene rooms, non-ambulant (peninsular)","TOC54","TOC53","New Build","SL_35_80_39","Hygiene rooms","Hygiene room for disabled pupils' wash-down, showering and toileting using a ceiling-mounted hoist, with wc, wash-hand basin, shower and sluice, and space for a shower-bed with access each side","Room for changing pupils and washing down, with peninsular bed to allow carer each side","Non-net","Non-net",null,null,"T","SEN",0.5,3,null,0,20,7,7,0,8,"CTS","None","Full disabled access required","Enclosed",null,"2700 / 2400","2700 / 2400","N/A / CTS","Not required","N/A","","D2.2d","strong","N/A","no internal doorset required",null,"Ergonomic handle. If door to open out, to have horizontal rail to enable closing. ","F7.3h","wet area","C2.3","wet areas","W3.3","wet areas","Flooring in barefoot areas shall be barefoot slip resistance category B Ceiling type C3 and wall type W3w in shower areas. Floor finish in shower areas to provide drainage ","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"pres on, abs off","No","Water / moisture grade luminaires if shower bed provided. Avoid direct downlighting over changing bed","T7","Average","High","<=1.5","<=2.0","Mechanical ventilation shall be provided as specified in Tech Annex 2F 7.8.1.6","None","Hand dryer","Hot and cold drinking water to all sinks, equipment and appliances in Annex 2A Table 1",0,null,4,"Emergency call system"]
["TOC60","Changing rooms, ambulant for pool (pupils)","Changing rooms, ambulant for pool (pupils)","TOC60","TOC60","New Build","SL_90_20_13","Changing rooms","Wet changing and showering for pupils needing additional support","Changing and showering for hydrotherapy or warm water pool","Non-net","Non-net",null,null,null,"SEN",7,4,null,0,15,2,2,0,3,"CTS","Optional","Full disabled access required","Enclosed",null,"2700 / N/A","2400 / N/A","7800 / CTS","Not required","N/A","","D2.2d","no internal doorset required","N/A","no internal doorset required",null,"Curtain or doorset at entrance to be agreed with school","F7.3h","wet area","C2.3","general","W3.3","wet areas","Flooring in barefoot areas shall be barefoot slip resistance category B Ceiling type C3 and wall type W3w in shower areas. Floor finish in shower areas to provide drainage ","L4.4o","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",100,"pres on, abs off","No","Water / moisture grade luminaires. IP rating for wet areas","T8","Average","High","<=1.5","<=2.0","Locally controlled mechanical ventilation shall be provided as specified in Tech Annex 2F 6.3","None","Hand dryer","Hot and cold drinking water to all sinks, equipment and appliances",0]
["TOC65","Changing rooms, non-ambulant for pool (pupils)","Changing rooms, non-ambulant for pool (pupils)","TOC65","TOC65","New Build","SL_90_20_13","Changing rooms","Wet changing and showering for disabled pupils using a ceiling-mounted hoist with wc, wash-hand basin, shower and a shower-bed","Changing and showering for hydrotherapy or warm water pool","Non-net","Non-net",null,null,null,"SEN",9,5,null,0,20,2,2,0,3,"CTS","Optional","Full disabled access required","Enclosed","off Hydrotherapy pool","2700 / N/A","2700 / 2400","7800 / CTS","Not required","N/A","","D2.2d","no internal doorset required","N/A","no internal doorset required",null,"Curtain or doorset at entrance to be agreed with school","F7.3h","wet area","C2.3","general","W3.3","wet areas","Flooring in barefoot areas shall be barefoot slip resistance category B Ceiling type C3 and wall type W3w in shower areas. Floor finish in shower areas to provide drainage ","L4.4o","No requirement","No requirement","Required in upper floors and where possible elsewhere","Not applicable",100,"pres on, abs off","No","Water / moisture grade luminaires. IP rating for wet areas","T8","Average","High","<=1.5","<=2.0","Locally controlled mechanical ventilation shall be provided as specified in Tech Annex 2F 6.3","None","Hand dryer","Hot and cold drinking water to all sinks, equipment and appliances",0]
["-",0,0,"-",null,null,null,"-",null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","no internal doorset required"]
["BED01","Bedrooms (staff)","Bedrooms","BED00","BED00","New Build","SL_45_10_09","Bedrooms","Residential school bedroom for overnight staff","Sleeping, changing, privacy and belongings","Residential","N/A",null,null,null,"-",3,6,null,null,"As SoA","As SoA","As SoA",0,"As SoA","N/A","None","Disabled access into the space required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Not required",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1a","private","N/A","no internal doorset required",null,"Access system to be agreed with school","F1.1","general","C2.1","normal","W1.1","general","Flooring to be cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","None","None",2,null,2]
["BED05","First aid posts, overnight sick room","First aid posts, overnight sick room","BED05","BED05","New Build","SL_35_10_30","First aid posts","Residential school sick room for pupils staying overnight","Sleeping, changing, privacy and belongings; pupil overnight room for sickness observation","Residential","N/A",null,null,null,"-",6,6,null,null,12,1,1,0,2,"N/A","None","Disabled access into the space required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Not required",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1a","private","N/A","no internal doorset required",null,"Access system to be agreed with school","F1.1","general","C2.1","normal","W1.1","general","Flooring to be cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","Minimal","Hot and cold drinking water to all sinks and equipment listed in Annex 3: FF&E, with labelled drinking water to sink",2,null,2]
["BED10","Bedrooms (pupil)","Bedrooms (pupil)","BED10","BED00","New Build","SL_45_10_09","Bedrooms","Residential school bedroom for mainstream pupil(s)","Sleeping, changing, privacy and belongings","Residential","N/A",null,null,null,"-",3,6,null,null,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Full disabled access not required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Not required",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1a","private","N/A","no internal doorset required",null,"Access system to be agreed with school","F1.1","general","C2.1","normal","W1.1","general","Flooring to be cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","None","None",1,null,2]
["BED11","Bedrooms (1-bed, pupil)","Bedrooms (1-bed, pupil)","BED11","BED00","New Build","SL_45_10_09","Bedrooms","Residential school single bedroom for a mainstream pupil","Sleeping, changing, privacy and belongings","Residential","N/A",null,null,null,"-",3,6,null,null,9,1,1,0,2,"CTS","None","Full disabled access not required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Not required",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1a","private","N/A","no internal doorset required",null,"Access system to be agreed with school","F1.1","general","C2.1","normal","W1.1","general","Flooring to be cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","None","None",1,null,2]
["BED12","Bedrooms (2-bed, pupil)","Bedrooms (2-bed, pupil)","BED12","BED00","New Build","SL_45_10_09","Bedrooms","Residential school twin bedroom for mainstream pupils","Sleeping, changing, privacy and belongings","Residential","N/A",null,null,null,"-",3,6,null,null,15,2,2,0,3,"CTS","None","Full disabled access not required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Not required",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1a","private","N/A","no internal doorset required",null,"Access system to be agreed with school","F1.1","general","C2.1","normal","W1.1","general","Flooring to be cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","None","None",2,null,4]
["BED13","Bedrooms (3-bed, pupil)","Bedrooms (3-bed, pupil)","BED13","BED00","New Build","SL_45_10_09","Bedrooms","Residential school triple bedroom for mainstream pupils","Sleeping, changing, privacy and belongings","Residential","N/A",null,null,null,"-",3,6,null,null,15,3,3,0,4,"CTS","None","Full disabled access not required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Not required",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1a","private","N/A","no internal doorset required",null,"Access system to be agreed with school","F1.1","general","C2.1","normal","W1.1","general","Flooring to be cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","None","None",3,null,6]
["BED14","Bedrooms (4-bed, pupil)","Bedrooms (4-bed, pupil)","BED14","BED00","New Build","SL_45_10_09","Bedrooms","Residential school quadruple bedroom for mainstream pupils","Sleeping, changing, privacy and belongings","Residential","N/A",null,null,null,"-",3,6,null,null,21,4,4,0,5,"CTS","None","Full disabled access not required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Not required",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1a","private","N/A","no internal doorset required",null,"Access system to be agreed with school","F1.1","general","C2.1","normal","W1.1","general","Flooring to be cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","None","None",4,null,8]
["BED20","Bedrooms (accessible)",null,null,"BED00","New Build","SL_45_10_09","Bedrooms","Residential school bedroom for a mainstream pupil with disabilities","Sleeping, changing, privacy and belongings","Residential","N/A",null,null,null,"-",3,6,null,null,27,"As SoA","As SoA",0,"As SoA","N/A","None","Disabled access into the space required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Not required",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1a","private","N/A","no internal doorset required",null,"Access system to be agreed with school","F1.1","general","C2.1","normal","W1.1","general","Flooring to be cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","None","None",2,null,2]
["BED60","Bedrooms (ambulant pupil)","Bedrooms (ambulant pupil)","BED60","BED00","New Build","SL_45_10_09","Bedrooms","Residential special school bedroom for predominantly ambulant pupil(s)","Sleeping, changing, privacy and belongings","Residential","N/A",null,null,null,"-",3,6,null,null,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access into the space required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Not required",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1a","private","N/A","no internal doorset required",null,"Handles ergonomic to suit limited dexterity and to be at the correct height to promote independence. Access system to be agreed with school.  Hinge protection.","F1.1","general","C2.1","normal","W1.1","general","Flooring suitable for wheelchairs; Readily cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","None","None",1,null,2,"Any SEN specific safety and security requirements to be confirmed with school. "]
["BED61","Bedrooms (1-bed, ambulant pupil)","Bedrooms (1-bed, ambulant pupil)","BED61","BED00","New Build","SL_45_10_09","Bedrooms","Residential special school single bedroom for a predominantly ambulant pupil","Sleeping, changing, privacy and belongings","Residential","N/A",null,null,null,"-",5,6,null,null,12,1,1,0,2,"CTS","None","Disabled access into the space required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Not required",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1a","private","N/A","no internal doorset required",null,"Handles ergonomic to suit limited dexterity and to be at the correct height to promote independence. Access system to be agreed with school.  Hinge protection.","F1.1","general","C2.1","normal","W1.1","general","Flooring suitable for wheelchairs; Readily cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","None","None",1,null,2,"Any SEN specific safety and security requirements to be confirmed with school. "]
["BED62","Bedrooms (2-bed, ambulant pupil)","Bedrooms (2-bed, ambulant pupil)","BED62","BED00","New Build","SL_45_10_09","Bedrooms","Residential special school twin bedroom for predominantly ambulant pupils","Sleeping, changing, privacy and belongings","Residential","N/A",null,null,null,"-",5,6,null,null,18,2,2,0,3,"CTS","None","Disabled access into the space required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Not required",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1a","private","N/A","no internal doorset required",null,"Handles ergonomic to suit limited dexterity and to be at the correct height to promote independence. Access system to be agreed with school.  Hinge protection.","F1.1","general","C2.1","normal","W1.1","general","Flooring suitable for wheelchairs; Readily cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","None","None",2,null,4,"Any SEN specific safety and security requirements to be confirmed with school. "]
["BED63","Bedrooms (3-bed, ambulant pupil)","Bedrooms (3-bed, ambulant pupil)","BED63","BED00","New Build","SL_45_10_09","Bedrooms","Residential special school triple bedroom for predominantly ambulant pupils","Sleeping, changing, privacy and belongings","Residential","N/A",null,null,null,"-",5,6,null,null,24,3,3,0,4,"CTS","None","Disabled access into the space required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Not required",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1a","private","N/A","no internal doorset required",null,"Handles ergonomic to suit limited dexterity and to be at the correct height to promote independence. Access system to be agreed with school.  Hinge protection.","F1.1","general","C2.1","normal","W1.1","general","Flooring suitable for wheelchairs; Readily cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","None","None",3,null,6,"Any SEN specific safety and security requirements to be confirmed with school. "]
["BED64","Bedrooms (4-bed, ambulant pupil)","Bedrooms (4-bed, ambulant pupil)","BED64","BED00","New Build","SL_45_10_09","Bedrooms","Residential special school quadruple bedroom for predominantly ambulant pupils","Sleeping, changing, privacy and belongings","Residential","N/A",null,null,null,"-",5,6,null,null,30,4,4,0,5,"CTS","None","Disabled access into the space required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Not required",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1a","private","N/A","no internal doorset required",null,"Handles ergonomic to suit limited dexterity and to be at the correct height to promote independence. Access system to be agreed with school.  Hinge protection.","F1.1","general","C2.1","normal","W1.1","general","Flooring suitable for wheelchairs; Readily cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","None","None",4,null,8,"Any SEN specific safety and security requirements to be confirmed with school. "]
["BED65","Bedrooms (non-ambulant pupil)","Bedrooms (non-ambulant pupil)","BED65","BED65","New Build","SL_45_10_09","Bedrooms","Residential special school bedroom for predominantly non-ambulant pupil(s)","Sleeping, changing, privacy and belongings","Residential","N/A",null,null,null,"-",6,9,null,null,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Full disabled access required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Not required",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1a","private","N/A","no internal doorset required",null,"Handles ergonomic to suit limited dexterity and to be at the correct height to promote independence. Access system to be agreed with school.  Hinge protection.","F1.1","general","C2.1","normal","W1.1","general","Flooring suitable for wheelchairs; Readily cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T7","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","None","None",1,null,2,"Any SEN specific safety and security requirements to be confirmed with school. "]
["TOC41","Bathrooms, ensuite (staff)","Bathrooms, ensuite (staff)","TOC41","TOC40","New Build","SL_35_80_08","Bathrooms","Residential school bathroom with shower off staff bedroom","Showering or bathing, toileting, personal hygiene","Residential","Non-net",null,null,"T","-",0.5,3,null,null,3,1,1,0,2,"N/A","None","Disabled access not required","Enclosed","off Bedroom (staff)","2400 / N/A","2400 / N/A","N/A / CTS","Not required","N/A","","D3.2b","toilets","N/A","no internal doorset required",null,"If door leaf opens inwards it shall be openable outwards in an emergency","F7.3h","wet area","C2.3","wet areas","W3.3","wet areas","Flooring in barefoot areas shall be barefoot slip resistance category B. Tiling or similar full height around shower area and above wash-hand basin as a minimum.","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No","Mirror light","T6","N/A","N/A","N/A","N/A","A locally controlled extract system shall be provided as specified in Tech Annex 2F 6.3","None","Shaver socket and optional hand drier","WC, whb & shower. Cold, with hot and cold with single mixer extended lever spray tap to handwash basin. Shower control and fixed head outlet, with thermostatic mixer valve to max temperature 43 degrees. Water to whb to be pre-mixed max temperature 43 degrees. Towel and soap dispensers to be agreed with school.  Mirror above wash hand basin.",0,null,0]
["TOC40","Bathrooms","Bathrooms","TOC40","TOC40","New Build","SL_35_80_08","Bathrooms","Residential school bathroom, with shower or bath for pupil or overnight staff use","Showering or bathing, toileting, personal hygiene","Residential","Non-net",null,null,"T","-",0.5,3,null,null,3,1,1,0,2,"CTS","None","Disabled access not required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Not required","N/A","","D3.2b","toilets","N/A","no internal doorset required",null,"If door leaf opens inwards it shall be openable outwards in an emergency","F7.3h","wet area","C2.3","wet areas","W3.3","wet areas","Flooring in barefoot areas shall be barefoot slip resistance category B. Tiling or similar full height around shower area and above wash-hand basin as a minimum.","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No","Mirror light","T6","N/A","N/A","N/A","N/A","A locally controlled extract system shall be provided as specified in Tech Annex 2F 6.3","None","Shaver socket and optional hand drier","Shower, hot and cold. Shower control and fixed head outlet, with thermostatic mixer valve to max temperature 43 degrees. Water to whb to be pre-mixed max temperature 43 degrees. Towel and soap dispensers to be agreed with school.  ",0,null,0,"Emergency call system; to be agreed with the school"]
["TOC42","Bathrooms (with shower, pupil)","Bathrooms (with shower, pupil)","TOC42","TOC40","New Build","SL_35_80_08","Bathrooms","Residential school bathroom with shower, for pupils, off corridor for shared use","Showering or bathing, toileting, personal hygiene","Residential","Non-net",null,null,"T","-",0.5,3,null,null,3,1,1,0,2,"CTS","None","Disabled access not required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Not required","N/A","","D3.2b","toilets","N/A","no internal doorset required",null,"If door leaf opens inwards it shall be openable outwards in an emergency","F7.3h","wet area","C2.3","wet areas","W3.3","wet areas","Flooring in barefoot areas shall be barefoot slip resistance category B. Tiling or similar full height around shower area and above wash-hand basin as a minimum.","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No","Mirror light","T6","N/A","N/A","N/A","N/A","A locally controlled extract system shall be provided as specified in Tech Annex 2F 6.3","None","Shaver socket and optional hand drier","WC, whb & shower. Cold, with hot and cold with single mixer extended lever spray tap to handwash basin. Shower control and fixed head outlet, with thermostatic mixer valve to max temperature 43 degrees. Water to whb to be pre-mixed max temperature 43 degrees. Towel and soap dispensers to be agreed with school.  Mirror above wash hand basin.",0,null,0,"Emergency call system; to be agreed with the school"]
["TOC43","Bathrooms (with bath, pupil)","Bathrooms (with bath, pupil)","TOC43","TOC40","New Build","SL_35_80_08","Bathrooms","Residential school bathroom with bath, for pupils, off corridor for shared use","Showering or bathing, toileting, personal hygiene","Residential","Non-net",null,null,"T","-",0.5,3,null,null,3.5,1,1,0,2,"CTS","None","Disabled access not required","Enclosed","off Bedroom (pupil) if required in SSB","2400 / N/A","2400 / N/A","N/A / CTS","Not required","N/A","","D3.2b","toilets","N/A","no internal doorset required",null,"If door leaf opens inwards it shall be openable outwards in an emergency","F7.3h","wet area","C2.3","wet areas","W3.3","wet areas","Flooring in barefoot areas shall be barefoot slip resistance category B. Tiling or similar full height around shower area and above wash-hand basin as a minimum.","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No","Mirror light","T6","N/A","N/A","N/A","N/A","A locally controlled extract system shall be provided as specified in Tech Annex 2F 6.3","None","Shaver socket and optional hand drier","WC, whb & bath. Cold, with hot and cold with single mixer extended lever spray tap to handwash basin and bath. Water to whb to be pre-mixed max temperature 43 degrees. Towel and soap dispensers to be agreed with school.  Mirror above wash hand basin.",0,null,0,"Emergency call system; to be agreed with the school"]
["TOC44","Bathrooms (ensuite, pupil)","Bathrooms (ensuite, pupil)","TOC44","TOC40","New Build","SL_35_80_08","Bathrooms","Residential school bathroom with shower, for pupils, off bedroom","Showering or bathing, toileting, personal hygiene","Residential","Non-net",null,null,"T","-",0.5,3,null,null,3,1,1,0,2,"CTS","None","Disabled access not required","Enclosed","off Bedroom (pupil)","2400 / N/A","2400 / N/A","N/A / CTS","Not required","N/A","","D3.2b","toilets","N/A","no internal doorset required",null,"If door leaf opens inwards it shall be openable outwards in an emergency","F7.3h","wet area","C2.3","wet areas","W3.3","wet areas","Flooring in barefoot areas shall be barefoot slip resistance category B. Tiling or similar full height around shower area and above wash-hand basin as a minimum.","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No","Mirror light","T6","N/A","N/A","N/A","N/A","A locally controlled extract system shall be provided as specified in Tech Annex 2F 6.3","None","Shaver socket and optional hand drier","WC, whb & shower. Cold, with hot and cold with single mixer extended lever spray tap to handwash basin. Shower control and fixed head outlet, with thermostatic mixer valve to max temperature 43 degrees. Water to whb to be pre-mixed max temperature 43 degrees. Towel and soap dispensers to be agreed with school.  Mirror above wash hand basin.",0,null,0,"Emergency call system; to be agreed with the school"]
["TOC45","Bathrooms, accessible (ensuite, pupil)","Bathrooms, accessible (ensuite, pupil)","TOC45","TOC45","New Build","SL_35_80_08","Bathrooms","Residential school bathroom with shower, for pupils with accessibility needs, off accessible bedroom","Showering or bathing, toileting, personal hygiene","Residential","Non-net",null,null,"T","-",0.5,3,null,null,5,2,2,0,3,"CTS","None","Full disabled access required","Enclosed","off Bedroom (pupil)","2400 / N/A","2400 / N/A","N/A / CTS","Not required","N/A","","D2.2d","toilets","N/A","no internal doorset required",null,"Ergonomic handle and Access control system to be agreed with school. If door leaf opens inwards it shall be openable outwards in an emergency","F7.3h","wet area","C2.3","wet areas","W3.3","wet areas","Flooring in barefoot areas shall be barefoot slip resistance category B. Tiling or similar full height around shower area and above wash-hand basin as a minimum.","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No","Mirror light","T6","N/A","N/A","N/A","N/A","A locally controlled extract system shall be provided as specified in Tech Annex 2F 6.3","None","Shaver socket and optional hand drier","WC, whb & shower. Cold, with hot and cold with single mixer extended lever spray tap to handwash basin. Shower control and fixed head outlet, with thermostatic mixer valve to max temperature 43 degrees. Water to whb to be pre-mixed max temperature 43 degrees. Towel and soap dispensers to be agreed with school.  Mirror above wash hand basin.",0,null,0,"Emergency call system; to be agreed with the school"]
["TOC71","Bathrooms (toilet, ambulant pupil)","Bathrooms (toilet, ambulant pupil)","TOC71","TOC40","New Build","SL_35_80_08","Bathrooms","Residential special school individual pupils toilet, sink and hand-wash/ dry in one space","Showering or bathing, toileting, personal hygiene","Residential","Non-net",null,null,"T","SEN",0.5,3,null,null,4,1,1,0,2,"CTS","None","Disabled access not required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Not required","N/A","","D3.2n","toilets","N/A","no internal doorset required",null,"If door leaf opens inwards it shall be openable outwards in an emergency","F7.3h","wet area","C2.3","wet areas","W3.3","wet areas","Flooring in barefoot areas shall be barefoot slip resistance category B. Tiling or similar full height around shower area and above wash-hand basin as a minimum.","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No","Mirror light","T6","N/A","N/A","N/A","N/A","A locally controlled extract system shall be provided as specified in Tech Annex 2F 6.3","None","Shaver socket and optional hand drier","Hot and cold drinking water to all sinks, equipment and appliances in Annex 2A Table 1",0,null,0,"Emergency call system; to be agreed with the school. Any SEN specific safety and security requirements to be confirmed with school. "]
["TOC72","Bathrooms (with shower, ambulant pupil)","Bathrooms (with shower, ambulant pupil)","TOC72","TOC40","New Build","SL_35_80_08","Bathrooms","Residential special school bathroom with shower, for pupils, off corridor for shared use","Showering or bathing, toileting, personal hygiene","Residential","Non-net",null,null,"T","SEN",0.5,3,null,null,5,2,2,0,3,"CTS","None","Disabled access not required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Not required","N/A","","D3.2n","toilets","N/A","no internal doorset required",null,"If door leaf opens inwards it shall be openable outwards in an emergency","F7.3h","wet area","C2.3","wet areas","W3.3","wet areas","Flooring in barefoot areas shall be barefoot slip resistance category B. Tiling or similar full height around shower area and above wash-hand basin as a minimum.","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No","Mirror light","T6","N/A","N/A","N/A","N/A","A locally controlled extract system shall be provided as specified in Tech Annex 2F 6.3","None","Shaver socket and optional hand drier","Whb & shower. Cold, with hot and cold handwash. Hot and cold with single mixer extended lever spray tap to handwash basin. Shower control and fixed head outlet, with thermostatic mixer valve to max temperature 43 degrees. Water to whb to be pre-mixed max temperature 43 degrees. Towel and soap dispensers to be agreed with school. Mirror above wash hand basin.",0,null,0,"Emergency call system; to be agreed with the school. Any SEN specific safety and security requirements to be confirmed with school. "]
["TOC73","Bathrooms (with bath, ambulant pupil)","Bathrooms (with bath, ambulant pupil)","TOC73","TOC40","New Build","SL_35_80_08","Bathrooms","Residential special school bathroom with bath, for pupils, off corridor for shared use","Showering or bathing, toileting, personal hygiene","Residential","Non-net",null,null,"T","SEN",0.5,3,null,null,6,2,2,0,3,"CTS","None","Disabled access not required","Enclosed","off Bedroom (pupil) if required in SSB","2400 / N/A","2400 / N/A","N/A / CTS","Not required","N/A","","D3.2n","toilets","N/A","no internal doorset required",null,"If door leaf opens inwards it shall be openable outwards in an emergency","F7.3h","wet area","C2.3","wet areas","W3.3","wet areas","Flooring in barefoot areas shall be barefoot slip resistance category B. Tiling or similar full height around shower area and above wash-hand basin as a minimum.","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No","Mirror light","T6","N/A","N/A","N/A","N/A","A locally controlled extract system shall be provided as specified in Tech Annex 2F 6.3","None","Shaver socket and optional hand drier","WC, whb & bath. Cold, with hot and cold with single mixer extended lever spray tap to handwash basin and bath. Water to whb to be pre-mixed max temperature 43 degrees. Towel and soap dispensers to be agreed with school.  Mirror above wash hand basin.",0,null,0,"Emergency call system; to be agreed with the school. Any SEN specific safety and security requirements to be confirmed with school. "]
["TOC74","Bathrooms, ensuite (ambulant pupil)","Bathrooms, ensuite (ambulant pupil)","TOC74","TOC40","New Build","SL_35_80_08","Bathrooms","Residential special school bathroom with shower, for predominantly ambulant pupil(s), off bedroom","Showering or bathing, toileting, personal hygiene","Residential","Non-net",null,null,"T","SEN",0.5,3,null,null,6,2,2,0,3,"CTS","None","Disabled access not required","Enclosed","off Bedroom (ambulant pupil)","2400 / N/A","2400 / N/A","N/A / CTS","Not required","N/A","","D3.2n","toilets","N/A","no internal doorset required",null,"If door leaf opens inwards it shall be openable outwards in an emergency","F7.3h","wet area","C2.3","wet areas","W3.3","wet areas","Flooring in barefoot areas shall be barefoot slip resistance category B. Tiling or similar full height around shower area and above wash-hand basin as a minimum.","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No","Mirror light","T6","N/A","N/A","N/A","N/A","A locally controlled extract system shall be provided as specified in Tech Annex 2F 6.3","None","Shaver socket and optional hand drier","WC, whb & shower. Cold, with hot and cold handwash. Hot and cold with single mixer extended lever spray tap to handwash basin. Shower control and fixed head outlet, with thermostatic mixer valve to max temperature 43 degrees. Water to whb to be pre-mixed max temperature 43 degrees. Towel and soap dispensers to be agreed with school.  Lockable sheet dispensing toilet paper holders. Mirror above wash hand basin.",0,null,0,"Emergency call system; to be agreed with the school. Any SEN specific safety and security requirements to be confirmed with school. "]
["TOC75","Bathrooms (non-ambulant, ensuite)","Bathrooms (non-ambulant, ensuite)","TOC75","TOC75","New Build","SL_35_80_08","Bathrooms","Residential special school bathroom with bath, for predominantly non-ambulant pupil(s), off bedroom","Showering or bathing, toileting, personal hygiene","Residential","Non-net",null,null,"T","SEN",0.5,3,null,null,9,3,3,0,4,"CTS","None","Full disabled access required","Enclosed","off Bedroom (non-ambulant pupil)","2400 / N/A","2400 / N/A","N/A / CTS","Not required","N/A","","D3.2n","toilets","N/A","no internal doorset required",null,"Ergonomic handle and Access control system to be agreed with school. If door leaf opens inwards it shall be openable outwards in an emergency","F7.3h","wet area","C2.3","wet areas","W3.3","wet areas","Flooring in barefoot areas shall be barefoot slip resistance category B. Tiling or similar full height around shower area and above wash-hand basin as a minimum.","L5.4o","No requirement","No requirement","Not applicable","Not applicable",100,"man on, man off","No","Mirror light","T7","N/A","N/A","N/A","N/A","A locally controlled extract system shall be provided as specified in Tech Annex 2F 6.3","None","Shaver socket and optional hand drier","WC, whb & bath. Cold, with hot and cold with single mixer extended lever spray tap to handwash basin and bath. Water to whb to be pre-mixed max temperature 43 degrees. Towel and soap dispensers to be agreed with school.  Mirror above wash hand basin.",0,null,0,"Emergency call system; to be agreed with the school. Any SEN specific safety and security requirements to be confirmed with school. "]
[0,0,0,0,null,null,null,"-",null,null,null,null,null,null,null,null,null,null,null,null,null,0]
["LIV00","Kitchen-dining rooms (staff)","Kitchen-dining rooms (staff)","LIV00","LIV00","New Build","SL_45_10_44","Kitchen-dining rooms","Kitchen, living and dining room for overnight staff in residential accommodation","Food preparation, dining, relaxation, study and social interaction","Residential","N/A",null,null,"B","-",2,1.6,null,null,"As SoA","As SoA","As SoA",0,"As SoA","N/A","None","Disabled access into the space required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Optional",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1av","general","N/A","no internal doorset required",null,"Access system to be agreed with school.","F1.1","general","C2.1","normal","W1.1","general","Flooring to be cleanable and not hold smells","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","To suit equipment","Hot and cold drinking water to all sinks, equipment and appliances",6,null,6]
["LIV01","Kitchen-dining rooms (pupil)","Kitchen-dining rooms (pupil)","LIV01","LIV00","New Build","SL_45_10_44","Kitchen-dining rooms","Kitchen, living and dining room for overnight staff in residential accommodation","Food preparation, dining, relaxation, study and social interaction","Residential","N/A",null,null,"B","-",2,1.6,null,null,"As SoA","As SoA","As SoA",0,"As SoA","N/A","None","Disabled access into the space required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Optional",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1av","general","N/A","no internal doorset required",null,"Access system to be agreed with school.","F1.1","general","C2.1","normal","W1.1","general","Flooring to be cleanable and not hold smells","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","To suit equipment","Hot and cold drinking water to all sinks, equipment and appliances",6,null,6]
["LIV70","Kitchen-dining rooms (special)","Kitchen-dining rooms (special)","LIV70","LIV70","New Build","SL_45_10_44","Kitchen-dining rooms","Kitchen, living and dining room for pupils with SEN in residential accommodation, respite or for life skills","Food preparation, dining, relaxation, study and social interaction","Residential","N/A",null,null,"B","-",2,1.6,null,null,"As SoA","As SoA","As SoA",0,"As SoA","N/A","None","Disabled access into the space required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Optional",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1av","general","N/A","no internal doorset required",null,"Handles ergonomic to suit limited dexterity and to be at the correct height to promote independence. Access system to be agreed with school.  Hinge protection.","F1.1","general","C2.1","normal","W1.1","general","Flooring to be cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","To suit equipment","Hot and cold drinking water to all sinks, equipment and appliances",6,null,6]
["LIV10","Communal living (and dining) rooms","Communal living (and dining) rooms","LIV10","LIV10","New Build","SL_45_10_14","Communal living rooms","Living and dining room for mainstream pupils in residential accommodation, or for life skills","Dining, relaxation, study and social interaction","Residential","N/A",null,null,"B","-",2,1.6,null,null,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access into the space required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Optional",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1av","general","N/A","no internal doorset required",null,"Access system to be agreed with school.","F1.1","general","C2.1","normal","W1.1","general","Flooring to be cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","To suit equipment","None",6,null,6]
["LIV12","Communal living rooms (pupil dining)","Communal living rooms (pupil dining)","LIV12","LIV10","New Build","SL_45_10_14","Communal living rooms","Dining room for mainstream pupils in residential accommodation, or for life skills","Dining, relaxation, study and social interaction","Residential","N/A",null,null,"B","-",2,1.6,null,null,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access into the space required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Optional",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1av","general","N/A","no internal doorset required",null,"Access system to be agreed with school.","F1.1","general","C2.1","normal","W1.1","general","Flooring to be cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","To suit equipment","None",6,null,6]
["LIV13","Communal living (and games) rooms","Communal living (and games) rooms","LIV13","LIV10","New Build","SL_45_10_14","Communal living rooms","Living and games room for mainstream pupils in residential accommodation, or for life skills","Informal eating, relaxation, recreation and social interaction, indoor games such as pool or computer games","Residential","N/A",null,null,"B","-",2,1.6,null,null,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access into the space required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Optional",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1av","general","N/A","no internal doorset required",null,"Access system to be agreed with school.","F1.1","general","C2.1","normal","W1.1","general","Flooring to be cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","To suit equipment","None",6,null,6]
["LIV14","Communal living (and study) rooms","Communal living (and study) rooms","LIV14","LIV10","New Build","SL_45_10_14","Communal living rooms","Living and study room for mainstream pupils in residential accommodation, or for life skills","Informal eating, relaxation, recreation and social interaction, group or private study","Residential","N/A",null,null,"B","-",2,1.6,null,null,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Disabled access into the space required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Optional",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1av","general","N/A","no internal doorset required",null,"Handles ergonomic to suit limited dexterity and to be at the correct height to promote independence. Access system to be agreed with school.","F1.1","general","C2.1","normal","W1.1","general","Flooring to be cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","To suit equipment","None",6,null,6]
["LIV61","Communal living (and dining) rooms (special)","Communal living (and dining) rooms (special)","LIV61","LIV60","New Build","SL_45_10_14","Communal living rooms","Living and dining room for pupils with SEN in residential accommodation, respite or for life skills","Dining, relaxation, study and social interaction","Residential","N/A",null,null,"G","SEN",10,2.9,null,null,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Full disabled access required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Optional",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1av","general","N/A","no internal doorset required",null,"Handles ergonomic to suit limited dexterity and to be at the correct height to promote independence. Access system to be agreed with school.  Hinge protection.","F1.1","general","C2.1","normal","W1.1","general","Flooring suitable for wheelchairs; Readily cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","To suit equipment","None",6,null,6,"Any SEN specific safety and security requirements to be confirmed with school. "]
["LIV62","Communal living rooms (pupil dining, special)","Communal living rooms (pupil dining, special)","LIV62","LIV60","New Build","SL_45_10_14","Communal living rooms","Dining room for pupils with SEN in residential accommodation, respite or for life skills","Dining, relaxation, study and social interaction","Residential","N/A",null,null,"G","SEN",10,2.9,null,null,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Full disabled access required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Optional",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1av","general","N/A","no internal doorset required",null,"Handles ergonomic to suit limited dexterity and to be at the correct height to promote independence. Access system to be agreed with school.  Hinge protection.","F1.1","general","C2.1","normal","W1.1","general","Flooring suitable for wheelchairs; Readily cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","To suit equipment","None",6,null,6,"Any SEN specific safety and security requirements to be confirmed with school. "]
["LIV63","Communal living (and games) rooms (special)","Communal living (and games) rooms (special)","LIV63","LIV60","New Build","SL_45_10_14","Communal living rooms","Living and games room for pupils with SEN in residential accommodation, respite or for life skills","Informal eating, relaxation, recreation and social interaction, indoor games such as pool or computer games","Residential","N/A",null,null,"G","SEN",10,2.9,null,null,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Full disabled access required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Optional",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1av","general","N/A","no internal doorset required",null,"Handles ergonomic to suit limited dexterity and to be at the correct height to promote independence. Access system to be agreed with school.  Hinge protection.","F1.1","general","C2.1","normal","W1.1","general","Flooring suitable for wheelchairs; Readily cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","To suit equipment","None",6,null,6,"Any SEN specific safety and security requirements to be confirmed with school. "]
["LIV64","Communal living (and study) rooms (special)","Communal living (and study) rooms (special)","LIV64","LIV60","New Build","SL_45_10_14","Communal living rooms","Living and study room for pupils with SEN in residential accommodation, respite or for life skills","Informal eating, relaxation, recreation and social interaction, group or private study","Residential","N/A",null,null,"G","SEN",10,2.9,null,null,"As SoA","As SoA","As SoA",0,"As SoA","CTS","None","Full disabled access required","Enclosed",null,"2400 / N/A","2400 / N/A","N/A / CTS","Optional",1050,"Lockable openable windows and vents to be provided, in line with residential standards. ","D1.1av","general","N/A","no internal doorset required",null,"Handles ergonomic to suit limited dexterity and to be at the correct height to promote independence. Access system to be agreed with school.  Hinge protection.","F1.1","general","C2.1","normal","W1.1","general","Flooring suitable for wheelchairs; Readily cleanable and not hold smells; If carpet, must be suitable to sit on.","L4.5f","No requirement","No requirement","Daylight required to residential standards","No requirement",200,"man on, man off","Yes","Task luminaire (fixed or portable) required. Manual dimming to main lighting required.","T2/T6","N/A","N/A","N/A","N/A","Natural vent (opening windows) with trickle vent required. TM59 recommendations to be followed.","None","To suit equipment","None",6,null,6,"Any SEN specific safety and security requirements to be confirmed with school. "]

{"sheet":"ADS Template","index":12,"n_rows":267,"n_cols":23,"rows_kept":267,"cut":false,"hidden":true,"merged":[[3,0,3,4],[5,10,5,12],[5,16,5,18],[5,20,5,22],[6,10,6,12],[6,16,6,18],[6,20,6,22],[8,10,8,12],[8,16,8,22],[9,16,10,22],[1,6,1,7],[2,16,3,18],[2,20,3,22],[14,6,15,7],[20,10,20,12],[20,16,20,18],[20,20,20,22],[22,10,22,12],[23,10,23,12],[23,16,23,18],[23,20,23,22],[11,3,11,4],[11,6,11,7],[11,10,11,12],[11,16,11,18],[11,20,11,22],[12,6,13,7],[32,10,32,12],[32,16,32,18],[32,20,32,22],[34,2,34,3],[34,10,34,12],[34,16,34,18],[34,20,34,22],[28,6,28,7],[28,10,28,12],[28,16,28,18],[28,20,28,22],[30,10,30,12],[30,16,30,18],[30,20,30,22],[43,10,43,12],[43,16,43,18],[43,20,43,22],[48,2,49,2],[48,3,49,4],[48,6,49,6],[48,10,49,12],[48,16,49,18],[48,20,49,22],[77,10,77,12],[78,2,78,4],[98,10,98,12],[98,16,98,18],[98,20,98,22],[100,16,101,18],[100,20,101,22],[52,16,53,18],[52,20,53,22],[54,10,54,12],[55,2,55,4],[75,16,76,18],[75,20,76,22],[133,20,133,22],[138,10,138,12],[139,16,139,18],[139,20,139,22],[102,10,102,12],[117,16,118,18],[117,20,118,22],[119,10,119,12],[123,16,124,18],[123,20,124,22],[141,4,142,4],[144,2,144,4],[155,2,155,4],[155,6,155,7],[158,6,159,7],[158,10,158,12],[125,10,125,12],[133,10,133,12],[133,16,133,18],[164,16,164,18],[164,20,164,22],[165,2,165,4],[165,6,165,7],[166,6,166,7],[167,6,168,7],[158,16,158,18],[158,20,158,22],[160,10,160,12],[160,16,160,18],[160,20,160,22],[162,3,162,4],[162,6,162,7],[162,10,162,12],[162,16,162,18],[162,20,162,22],[175,2,175,4],[176,2,176,4],[178,16,178,18],[178,20,178,22],[179,2,180,3],[181,2,182,3],[170,2,170,4],[170,6,172,6],[171,2,171,4],[172,2,172,4],[173,2,173,4],[174,2,174,4],[174,6,174,7],[194,2,194,4],[194,6,196,6],[196,2,196,4],[202,3,202,4],[202,6,202,7],[202,10,202,12],[183,2,183,4],[188,2,189,3],[188,10,188,12],[189,10,189,12],[190,6,190,7],[191,2,191,4],[205,20,205,22],[206,3,206,4],[206,10,206,12],[206,16,206,18],[206,20,206,22],[202,16,202,18],[202,20,202,22],[203,10,203,12],[204,3,204,4],[204,10,204,12],[204,16,204,18],[204,20,204,22],[207,10,207,12],[208,10,208,12],[209,10,209,12],[210,10,210,12],[211,10,211,12],[212,10,212,12],[205,3,205,4],[205,10,205,12],[205,16,205,18],[220,10,220,12],[222,6,222,7],[222,10,222,12],[222,16,222,18],[222,20,222,22],[224,10,224,12],[224,16,224,18],[224,20,224,22],[214,10,214,12],[215,10,215,12],[216,10,216,12],[217,10,217,12],[218,10,218,12],[219,10,219,12],[229,6,229,7],[229,10,229,12],[229,16,229,18],[229,20,229,22],[231,10,231,12],[233,3,233,4],[233,10,233,12],[233,16,233,18],[233,20,233,22],[238,6,239,7],[265,3,265,4],[265,6,265,7],[265,10,265,12],[265,16,265,18],[265,20,265,22],[235,10,235,12],[235,16,235,18],[235,20,235,22],[237,10,237,12],[237,16,237,18],[237,20,237,22]]}
[]
["AREA DATA SHEETS",null,null,null,null,null,"notes & information for client",null,null,null,null,"Area data for:",null,null,null,null,null,null,null,"compliance checks"]
["for spaces in: ",null,null,null,null,null,{"$f":"MAX(MAX($G$1:$H2),MAX($F3:F3))+1","v":1},null,null,null,null,{"$f":"MAX(MAX($J$1:$N2),MAX($J3:K3))+1","v":1},null,null,null,null,"Contractor's Interim Bid Proposal",null,null,null,"Contractor's Final Bid Proposal"]
["[name of school]",null,null,null,null,null,{"$f":"MAX(MAX($G$1:$H3),MAX($F4:F4))+1","v":2},null,null,null,null,{"$f":"MAX(MAX($J$1:$N3),MAX($J4:K4))+1","v":2}]
["Key Data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"identify if new/ remodel or refurb/ redec'n"]
[null,null,"reference code",null,"name of individual space",null,"Contractor to amend to individual space name in SoA",null,null,null,{"$f":"MAX(MAX($J$1:$N5),MAX($J6:J6))+1","v":3}]
[null,null,null,null,"ref code for individual space",null,"Contractor to amend to individual space code if in SoA",null,null,null,{"$f":"MAX(MAX($J$1:$N6),MAX($J7:J7))+1","v":4},null,null,null,null,null,"code on drawing",null,null,null,"code on drawing"]
[null,"1. Function"]
[null,null,"Summary description",null,null,null,"brief description of space",null,null,null,{"$f":"MAX(MAX($J$1:$N8),MAX($J9:J9))+1","v":5},null,null,null,null,null,"NOTE: if value is left blank, the proposal is deemed to be as the requirement, unless Contractor to Specify (CTS). 'Note ref.' must be provided where differences are proposed, referencing supporting information."]
[null,null,"Required Area",null,null,null,{"$f":"MAX(MAX($G$1:$H9),MAX($F10:F10))+1","v":3},null,null,null,{"$f":"MAX(MAX($J$1:$N9),MAX($J10:J10))+1","v":6},"m2",null,null,null,null,"List any changes to activities described below (or leave blank if there are no changes)"]
[]
[null,null,"Activities description","Range of activities or uses to be accommodated",null,null,"This text box describes the activities that should be able to take place in the space, which in turn will influence the choice of F&E and many of the requirements below, including the area.",null,null,null,{"$f":"MAX(MAX($J$1:$N11),MAX($J12:J12))+1","v":7}]
[null,null,null,null,null,null,"maximum (not average) teaching group, or maximum group including meeting area in staff and admin spaces, as SoA"]
[null,null,null,null,"Maximum group size/ Net capacity workplaces",null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N13),MAX($J14:J14))+1","v":8},"/",{"$f":"MAX(MAX($J$1:$N13),MAX($J14:L14))+1","v":9}]
[null,null,null,null,"number of staff",null,"staff or adults over and above pupils in teaching spaces, staff workstations in staff and admin spaces",null,null,null,{"$f":"MAX(MAX($J$1:$N14),MAX($J15:J15))+1","v":10}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Actual area provided (m2)"]
[null,null,null,null,"Area Guidelines Category",null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N16),MAX($J17:J17))+1","v":11},null,null,null,null,null,"actual area",null,"note ref.",null,"actual area",null,"note ref."]
[null,null,null,null,"Area Guidelines Zone",null,{"$f":"MAX(MAX($G$1:$H17),MAX($F18:F18))+1","v":4},null,null,null,{"$f":"MAX(MAX($J$1:$N17),MAX($J18:J18))+1","v":12}]
[null,null,null,null,"Net capacity category",null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N18),MAX($J19:J19))+1","v":13}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"identify if available for community use during or after school day"]
[null,null,"Community use",null,"Third Party Use",null,"community use during or outside core school day",null,null,null,{"$f":"MAX(MAX($J$1:$N20),MAX($J21:J21))+1","v":14}]
[null,null,"FM issues"]
[null,null,"Availability Priority Category",null,null,null,"As SoA",null,null,null,{"$f":"MAX(MAX($J$1:$N22),MAX($J23:J23))+1","v":15}]
[null,null,"Consequential Unavailability",null,null,null,"As SoA",null,null,null,{"$f":"MAX(MAX($J$1:$N23),MAX($J24:J24))+1","v":16}]
[]
[]
["Location and Space"]
[null,"2. Location and access",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"actual location",null,null,null,"actual location"]
[null,null,"Location",null,null,null,"school to identify where this space should be located",null,null,null,{"$f":"MAX(MAX($J$1:$N28),MAX($J29:J29))+1","v":17}]
[]
[null,null,"Access requirements",null,null,null,"disabled access options",null,null,null,{"$f":"MAX(MAX($J$1:$N30),MAX($J31:J31))+1","v":18}]
[null,"3. Organisation",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"actual enclosure/ adjacency",null,null,null,"actual enclosure/ adjacency"]
[null,null,"Enclosure requirements",null,null,null,"enclosed/ semi-enclosed/ open plan",null,null,null,{"$f":"MAX(MAX($J$1:$N32),MAX($J33:J33))+1","v":19}]
[]
[null,null,"Adjacency requirements",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N34),MAX($J35:J35))+1","v":20}]
[null,"4. Space",null,null,null,null,null,null,null,null,"If new / remodel",null,"If refurb / redec'n"]
[null,null,"Minimum area (m2)",null,null,null,"As SoA",null,null,null,{"$f":"MAX(MAX($J$1:$N36),MAX($J37:J37))+1","v":21},null,{"$f":"MAX(MAX($J$1:$N36),MAX($J37:L37))+1","v":22},null,null,null,"actual dims",null,"note ref.",null,"actual dims",null,"note ref."]
[]
[null,null,"Minimum ceiling height",null,null,null,{"$f":"MAX(MAX($G$1:$H38),MAX($F39:F39))+1","v":5},null,null,null,{"$f":"MAX(MAX($J$1:$N38),MAX($J39:J39))+1","v":23},null,{"$f":"MAX(MAX($J$1:$N38),MAX($J39:L39))+1","v":24}]
[null,null,"Space depth (mm)",null,"where required",null,{"$f":"MAX(MAX($G$1:$H39),MAX($F40:F40))+1","v":6},null,null,null,{"$f":"MAX(MAX($J$1:$N39),MAX($J40:J40))+1","v":25}]
[]
[]
["Fabric and environment"]
[null,"5. External door(s)",null,null,"if required or preferred",null,"i.e. direct access via external door",null,null,null,{"$f":"MAX(MAX($J$1:$N43),MAX($J44:J44))+1","v":26}]
[]
[null,"6. Windows and internal doorsets",null,null,null,null,null,null,null,null,"If new / remodel",null,"If refurb / redec'n",null,null,null,"actual dimension",null,null,null,"actual dimension"]
[null,null,"Window sill height (mm)",null,null,null,{"$f":"MAX(MAX($G$1:$H46),MAX($F47:F47))+1","v":7},null,null,null,{"$f":"MAX(MAX($J$1:$N46),MAX($J47:J47))+1","v":27},null,{"$f":"MAX(MAX($J$1:$N46),MAX($J47:L47))+1","v":28}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"description of window solution"]
[null,null,"Specific external door or window requirements","ironmongery, access, locks, integral or external blinds (for blinds see FF&E below)",null,null,"(requirement for external door identified in Access to outdoors above)",null,null,null,{"$f":"MAX(MAX($J$1:$N48),MAX($J49:J49))+1","v":29}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"If new / remodel",null,"If refurb / redec'n",null,null,null,"description of entrance doorset solution"]
[null,null,"Doorset from circulation",null," including atria",null,"see tech annexe doorsets",null,null,null,{"$f":"MAX(MAX($J$1:$N52),MAX($J53:J53))+1","v":30},null,{"$f":"MAX(MAX($J$1:$N52),MAX($J53:L53))+1","v":31}]
[]
[null,null,"Description",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N54),MAX($J55:J55))+1","v":32},null,null,null,null,null,"value",null,"note ref.",null,"value",null,"note ref."]
[null,null,"Acoustic airborne sound insulation rating for door into space from: corridor or non-teaching area",null,null,null,{"$f":"MAX(MAX($G$1:$H55),MAX($F56:F56))+1","v":8},null,null,null,{"$f":"MAX(MAX($J$1:$N55),MAX($J56:J56))+1","v":33},null,{"$f":"MAX(MAX($J$1:$N55),MAX($J56:L56))+1","v":34}]
[null,null,"Door leaf width",null,null,null,"mm",null,null,null,{"$f":"MAX(MAX($J$1:$N56),MAX($J57:J57))+1","v":35},null,{"$f":"MAX(MAX($J$1:$N56),MAX($J57:L57))+1","v":36}]
[null,null,"Minimum clear opening width",null,null,null,"effective clear width in mm",null,null,null,{"$f":"MAX(MAX($J$1:$N57),MAX($J58:J58))+1","v":37},null,{"$f":"MAX(MAX($J$1:$N57),MAX($J58:L58))+1","v":38}]
[null,null,"Minimum clear opening height",null,null,null,"effective clear height in mm",null,null,null,{"$f":"MAX(MAX($J$1:$N58),MAX($J59:J59))+1","v":39},null,{"$f":"MAX(MAX($J$1:$N58),MAX($J59:L59))+1","v":40}]
[null,null,"Minimum mechanical durability",null,null,null,{"$f":"MAX(MAX($G$1:$H59),MAX($F60:F60))+1","v":9},null,null,null,{"$f":"MAX(MAX($J$1:$N59),MAX($J60:J60))+1","v":41},null,{"$f":"MAX(MAX($J$1:$N59),MAX($J60:L60))+1","v":42}]
[null,null,"Minimum mechanical strength",null,null,null,"BS EN1192:2000",null,null,null,{"$f":"MAX(MAX($J$1:$N60),MAX($J61:J61))+1","v":43},null,{"$f":"MAX(MAX($J$1:$N60),MAX($J61:L61))+1","v":44}]
[null,null,"Minimum fire and smoke resistance (value of \"##\") ",null,null,null,{"$f":"MAX(MAX($G$1:$H61),MAX($F62:F62))+1","v":10},null,null,null,{"$f":"MAX(MAX($J$1:$N61),MAX($J62:J62))+1","v":45},null,{"$f":"MAX(MAX($J$1:$N61),MAX($J62:L62))+1","v":46}]
[null,null,"Minimum security rating",null,null,null,{"$f":"MAX(MAX($G$1:$H62),MAX($F63:F63))+1","v":11},null,null,null,{"$f":"MAX(MAX($J$1:$N62),MAX($J63:J63))+1","v":47},null,{"$f":"MAX(MAX($J$1:$N62),MAX($J63:L63))+1","v":48}]
[null,null,"Minimum hygrothermal performance",null,null,null,"class defined in BS EN1192:2000 and BS EN1294:2000",null,null,null,{"$f":"MAX(MAX($J$1:$N63),MAX($J64:J64))+1","v":49},null,{"$f":"MAX(MAX($J$1:$N63),MAX($J64:L64))+1","v":50}]
[null,null,"Vision panels",null,null,null,"min height and width as FOS",null,null,null,{"$f":"MAX(MAX($J$1:$N64),MAX($J65:J65))+1","v":51},null,{"$f":"MAX(MAX($J$1:$N64),MAX($J65:L65))+1","v":52}]
[]
[null,null,"Ironmongery hardware:","Closer",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N66),MAX($J67:J67))+1","v":53},null,{"$f":"MAX(MAX($J$1:$N66),MAX($J67:L67))+1","v":54}]
[null,null,null,"Electromagnetic hold open device",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N67),MAX($J68:J68))+1","v":55},null,{"$f":"MAX(MAX($J$1:$N67),MAX($J68:L68))+1","v":56}]
[null,null,null,"Hinges",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N68),MAX($J69:J69))+1","v":57},null,{"$f":"MAX(MAX($J$1:$N68),MAX($J69:L69))+1","v":58}]
[null,null,null,"Cylinder/ lock",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N69),MAX($J70:J70))+1","v":59},null,{"$f":"MAX(MAX($J$1:$N69),MAX($J70:L70))+1","v":60}]
[null,null,null,"Lever handle",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N70),MAX($J71:J71))+1","v":61},null,{"$f":"MAX(MAX($J$1:$N70),MAX($J71:L71))+1","v":62}]
[null,null,null,"Vertical pull handle",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N71),MAX($J72:J72))+1","v":63},null,{"$f":"MAX(MAX($J$1:$N71),MAX($J72:L72))+1","v":64}]
[null,null,null,"Staff-only access control system",null,null,{"$f":"MAX(MAX($G$1:$H72),MAX($F73:F73))+1","v":12},null,null,null,{"$f":"MAX(MAX($J$1:$N72),MAX($J73:J73))+1","v":65},null,{"$f":"MAX(MAX($J$1:$N72),MAX($J73:L73))+1","v":66}]
[null,null,null,"Door protection",null,null,"kick plate height (mm)",null,null,null,{"$f":"MAX(MAX($J$1:$N73),MAX($J74:J74))+1","v":67},null,{"$f":"MAX(MAX($J$1:$N73),MAX($J74:L74))+1","v":68}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"description of interlinking doorset solution"]
[null,null,"Doorset to adjacent space of similar type",null,null,null,"see tech annexe doorsets",null,null,null,{"$f":"MAX(MAX($J$1:$N75),MAX($J76:J76))+1","v":69},null,{"$f":"MAX(MAX($J$1:$N75),MAX($J76:L76))+1","v":70}]
[]
[null,null,"Description",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N77),MAX($J78:J78))+1","v":71},null,null,null,null,null,"value",null,"note ref.",null,"value",null,"note ref."]
[null,null,"Acoustic airborne sound insulation rating for door into space from: teaching space (eg. of same type)",null,null,null,{"$f":"MAX(MAX($G$1:$H78),MAX($F79:F79))+1","v":13},null,null,null,{"$f":"MAX(MAX($J$1:$N78),MAX($J79:J79))+1","v":72},null,{"$f":"MAX(MAX($J$1:$N78),MAX($J79:L79))+1","v":73}]
[null,null,"Door leaf width",null,null,null,"mm",null,null,null,{"$f":"MAX(MAX($J$1:$N79),MAX($J80:J80))+1","v":74},null,{"$f":"MAX(MAX($J$1:$N79),MAX($J80:L80))+1","v":75}]
[null,null,"Minimum clear opening width",null,null,null,"effective clear width in mm",null,null,null,{"$f":"MAX(MAX($J$1:$N80),MAX($J81:J81))+1","v":76},null,{"$f":"MAX(MAX($J$1:$N80),MAX($J81:L81))+1","v":77}]
[null,null,"Minimum clear opening height",null,null,null,"effective clear height in mm",null,null,null,{"$f":"MAX(MAX($J$1:$N81),MAX($J82:J82))+1","v":78},null,{"$f":"MAX(MAX($J$1:$N81),MAX($J82:L82))+1","v":79}]
[null,null,"Minimum mechanical durability",null,null,null,{"$f":"MAX(MAX($G$1:$H82),MAX($F83:F83))+1","v":14},null,null,null,{"$f":"MAX(MAX($J$1:$N82),MAX($J83:J83))+1","v":80},null,{"$f":"MAX(MAX($J$1:$N82),MAX($J83:L83))+1","v":81}]
[null,null,"Minimum mechanical strength",null,null,null,"BS EN1192:2000",null,null,null,{"$f":"MAX(MAX($J$1:$N83),MAX($J84:J84))+1","v":82},null,{"$f":"MAX(MAX($J$1:$N83),MAX($J84:L84))+1","v":83}]
[null,null,"Minimum fire and smoke resistance (value of \"##\") ",null,null,null,{"$f":"MAX(MAX($G$1:$H84),MAX($F85:F85))+1","v":15},null,null,null,{"$f":"MAX(MAX($J$1:$N84),MAX($J85:J85))+1","v":84},null,{"$f":"MAX(MAX($J$1:$N84),MAX($J85:L85))+1","v":85}]
[null,null,"Minimum security rating",null,null,null,{"$f":"MAX(MAX($G$1:$H85),MAX($F86:F86))+1","v":16},null,null,null,{"$f":"MAX(MAX($J$1:$N85),MAX($J86:J86))+1","v":86},null,{"$f":"MAX(MAX($J$1:$N85),MAX($J86:L86))+1","v":87}]
[null,null,"Minimum hygrothermal performance",null,null,null,"class defined in BS EN1192:2000 and BS EN1294:2000",null,null,null,{"$f":"MAX(MAX($J$1:$N86),MAX($J87:J87))+1","v":88},null,{"$f":"MAX(MAX($J$1:$N86),MAX($J87:L87))+1","v":89}]
[null,null,"Vision panels",null,null,null,"min height and width as FOS",null,null,null,{"$f":"MAX(MAX($J$1:$N87),MAX($J88:J88))+1","v":90},null,{"$f":"MAX(MAX($J$1:$N87),MAX($J88:L88))+1","v":91}]
[]
[null,null,"Ironmongery hardware:","Closer",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N89),MAX($J90:J90))+1","v":92},null,{"$f":"MAX(MAX($J$1:$N89),MAX($J90:L90))+1","v":93}]
[null,null,null,"Electromagnetic hold open device",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N90),MAX($J91:J91))+1","v":94},null,{"$f":"MAX(MAX($J$1:$N90),MAX($J91:L91))+1","v":95}]
[null,null,null,"Hinges",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N91),MAX($J92:J92))+1","v":96},null,{"$f":"MAX(MAX($J$1:$N91),MAX($J92:L92))+1","v":97}]
[null,null,null,"Cylinder/ lock",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N92),MAX($J93:J93))+1","v":98},null,{"$f":"MAX(MAX($J$1:$N92),MAX($J93:L93))+1","v":99}]
[null,null,null,"Lever handle",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N93),MAX($J94:J94))+1","v":100},null,{"$f":"MAX(MAX($J$1:$N93),MAX($J94:L94))+1","v":101}]
[null,null,null,"Vertical pull handle",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N94),MAX($J95:J95))+1","v":102},null,{"$f":"MAX(MAX($J$1:$N94),MAX($J95:L95))+1","v":103}]
[null,null,null,"Staff-only access control system",null,null,{"$f":"MAX(MAX($G$1:$H95),MAX($F96:F96))+1","v":17},null,null,null,{"$f":"MAX(MAX($J$1:$N95),MAX($J96:J96))+1","v":104},null,{"$f":"MAX(MAX($J$1:$N95),MAX($J96:L96))+1","v":105}]
[null,null,null,"Door protection",null,null,"kick plate height (mm)",null,null,null,{"$f":"MAX(MAX($J$1:$N96),MAX($J97:J97))+1","v":106},null,{"$f":"MAX(MAX($J$1:$N96),MAX($J97:L97))+1","v":107}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"specific doorset requirements met and additions"]
[null,null,"Specific doorset requirements",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N98),MAX($J99:J99))+1","v":108}]
[null,"7. Finishes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"description of floor finish solution"]
[null,null,"Floor finish",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N100),MAX($J101:J101))+1","v":109},null,{"$f":"MAX(MAX($J$1:$N100),MAX($J101:L101))+1","v":110}]
[]
[null,null,"Description",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N102),MAX($J103:J103))+1","v":111},null,null,null,null,null,"value",null,"note ref.",null,"value",null,"note ref."]
[null,null,"BS EN 14041:2004 Essential characteristics",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N103),MAX($J104:J104))+1","v":112},null,{"$f":"MAX(MAX($J$1:$N103),MAX($J104:L104))+1","v":113}]
[null,null,"BS EN ISO 10874:2012 durability classification",null,null,null,"European Flooring Use classification ",null,null,null,{"$f":"MAX(MAX($J$1:$N104),MAX($J105:J105))+1","v":114},null,{"$f":"MAX(MAX($J$1:$N104),MAX($J105:L105))+1","v":115}]
[null,null,"BS EN 14904: 2006 Sports floor elasticity",null,null,null,"Area elastic (A3) or point elastic (P3)",null,null,null,{"$f":"MAX(MAX($J$1:$N105),MAX($J106:J106))+1","v":116},null,{"$f":"MAX(MAX($J$1:$N105),MAX($J106:L106))+1","v":117}]
[null,null,"Minimum reflectance ",null,null,null,"0.3 for all habitable rooms",null,null,null,{"$f":"MAX(MAX($J$1:$N106),MAX($J107:J107))+1","v":118},null,{"$f":"MAX(MAX($J$1:$N106),MAX($J107:L107))+1","v":119}]
[null,null,"Minimum Required Life  (years)",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N107),MAX($J108:J108))+1","v":120},null,{"$f":"MAX(MAX($J$1:$N107),MAX($J108:L108))+1","v":121}]
[null,null,"Slip Resistance",null,null,null,"(Ramp test rating, or R value)",null,null,null,{"$f":"MAX(MAX($J$1:$N108),MAX($J109:J109))+1","v":122},null,{"$f":"MAX(MAX($J$1:$N108),MAX($J109:L109))+1","v":123}]
[null,null,"Slip Resistance Value (SRV)",null,null,null,"and surface roughness",null,null,null,{"$f":"MAX(MAX($J$1:$N109),MAX($J110:J110))+1","v":124},null,{"$f":"MAX(MAX($J$1:$N109),MAX($J110:L110))+1","v":125}]
[null,null,"Water Resistance",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N110),MAX($J111:J111))+1","v":126},null,{"$f":"MAX(MAX($J$1:$N110),MAX($J111:L111))+1","v":127}]
[null,null,"Fire Performance",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N111),MAX($J112:J112))+1","v":128},null,{"$f":"MAX(MAX($J$1:$N111),MAX($J112:L112))+1","v":129}]
[null,null,"Hygiene Performance",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N112),MAX($J113:J113))+1","v":130},null,{"$f":"MAX(MAX($J$1:$N112),MAX($J113:L113))+1","v":131}]
[null,null,"BS EN 14041:2004 Electrostatic rating",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N113),MAX($J114:J114))+1","v":132},null,{"$f":"MAX(MAX($J$1:$N113),MAX($J114:L114))+1","v":133}]
[null,null,"Chemical Resistance",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N114),MAX($J115:J115))+1","v":134},null,{"$f":"MAX(MAX($J$1:$N114),MAX($J115:L115))+1","v":135}]
[null,null,"Heat Resistance",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N115),MAX($J116:J116))+1","v":136},null,{"$f":"MAX(MAX($J$1:$N115),MAX($J116:L116))+1","v":137}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"description of ceiling/ soffit finish solution"]
[null,null,"Ceiling finish",null,"or soffit finish",null,"see technical annexe - ceiling finish",null,null,null,{"$f":"MAX(MAX($J$1:$N117),MAX($J118:J118))+1","v":138},null,{"$f":"MAX(MAX($J$1:$N117),MAX($J118:L118))+1","v":139}]
[]
[null,null,"Description",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N119),MAX($J120:J120))+1","v":140},null,null,null,null,null,"value",null,"note ref.",null,"value",null,"note ref."]
[null,null,"Minimum reflectance ",null,null,null,"0.7 for all habitable rooms",null,null,null,{"$f":"MAX(MAX($J$1:$N120),MAX($J121:J121))+1","v":141},null,{"$f":"MAX(MAX($J$1:$N120),MAX($J121:L121))+1","v":142}]
[null,null,"Hygrothermal performance",null,null,null,"generally as wall finish below",null,null,null,{"$f":"MAX(MAX($J$1:$N121),MAX($J122:J122))+1","v":143},null,{"$f":"MAX(MAX($J$1:$N121),MAX($J122:L122))+1","v":144}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"description of wall finish solution"]
[null,null,"Wall finish",null,null,null,"see technical annexe - wall finish",null,null,null,{"$f":"MAX(MAX($J$1:$N123),MAX($J124:J124))+1","v":145},null,{"$f":"MAX(MAX($J$1:$N123),MAX($J124:L124))+1","v":146}]
[]
[null,null,"Description",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N125),MAX($J126:J126))+1","v":147},null,null,null,null,null,"value",null,"note ref.",null,"value",null,"note ref."]
[null,null,"Minimum reflectance ",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N126),MAX($J127:J127))+1","v":148},null,{"$f":"MAX(MAX($J$1:$N126),MAX($J127:L127))+1","v":149}]
[null,null,"Impervious ",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N127),MAX($J128:J128))+1","v":150},null,{"$f":"MAX(MAX($J$1:$N127),MAX($J128:L128))+1","v":151}]
[null,null,"Jointless",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N128),MAX($J129:J129))+1","v":152},null,{"$f":"MAX(MAX($J$1:$N128),MAX($J129:L129))+1","v":153}]
[null,null,"Smooth",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N129),MAX($J130:J130))+1","v":154},null,{"$f":"MAX(MAX($J$1:$N129),MAX($J130:L130))+1","v":155}]
[null,null,"Hygrothermal performance",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N130),MAX($J131:J131))+1","v":156},null,{"$f":"MAX(MAX($J$1:$N130),MAX($J131:L131))+1","v":157}]
[null,null,"Acoustic wall finish and absorbent panels",null,null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N131),MAX($J132:K132))+1","v":158}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"specific finishes requirements met and additions"]
[null,null,"Specific finishes requirements",null,"incl part-covering, colour or pattern",null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N133),MAX($J134:J134))+1","v":159}]
[]
[]
[null,"8. Environmental requirements",null,null,null,null,null,null,null,null,"If new build",null,"If refurbishment",null,null,null,"identify if daylight provided",null,null,null,"identify if daylight provided"]
[null,null,"Daylight and lighting requirements",null,null,null,"see technical annexe lighting ",null,null,null,{"$f":"MAX(MAX($J$1:$N137),MAX($J138:J138))+1","v":160},null,{"$f":"MAX(MAX($J$1:$N137),MAX($J138:L138))+1","v":161},null,null,null,null,null,"Yes/ No",null,null,null,"Yes/ No"]
[null,null,"Daylighting",null,null,null,null,null,null,null,null,null,null,null,null,null,"lighting system solution"]
[null,null,"Direct daylighting requirement",null,null,null,"required, preferred or not required",null,null,null,{"$f":"MAX(MAX($J$1:$N139),MAX($J140:J140))+1","v":162},null,{"$f":"MAX(MAX($J$1:$N139),MAX($J140:L140))+1","v":163}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"value",null,"note ref.",null,"value",null,"note ref."]
[null,null,"For new build:                                   Daylight Autonomy",null,"Required in 80% of spaces where daylight required (above)",null,"Percentage of regularly used area that has an illuminance of 300 lux for half of core hours",null,null,null,{"$f":"MAX(MAX($J$1:$N141),MAX($J142:J142))+1","v":164},null,{"$f":"MAX(MAX($J$1:$N141),MAX($J142:L142))+1","v":165}]
[null,null,"Usable daylight Index, UDI-a ",null,null,null,{"$f":"MAX(MAX($G$1:$H142),MAX($F143:F143))+1","v":18},null,null,null,{"$f":"MAX(MAX($J$1:$N142),MAX($J143:J143))+1","v":166},null,{"$f":"MAX(MAX($J$1:$N142),MAX($J143:L143))+1","v":167}]
[null,null,"For refurbishment:","Minimum uniformity of daylight ",null,null,"(under diffuse sky) where daylight provided",null,null,null,{"$f":"MAX(MAX($J$1:$N143),MAX($J144:J144))+1","v":168},null,{"$f":"MAX(MAX($J$1:$N143),MAX($J144:L144))+1","v":169}]
[]
[null,null,"Lighting system",null,null,null,null,null,null,null,null,null,null,null,null,null,"value",null,"note ref.",null,"value",null,"note ref."]
[null,null,"Minimum horizontal/ task illuminance (lux)",null,null,null,"maintained average",null,null,null,{"$f":"MAX(MAX($J$1:$N146),MAX($J147:J147))+1","v":170},null,{"$f":"MAX(MAX($J$1:$N146),MAX($J147:L147))+1","v":171}]
[null,null,"Maximum horizontal illuminance (lux)",null,null,null,"maintained average",null,null,null,{"$f":"MAX(MAX($J$1:$N147),MAX($J148:J148))+1","v":172},null,{"$f":"MAX(MAX($J$1:$N147),MAX($J148:L148))+1","v":173}]
[null,null,"Minimum ceiling luminance",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N148),MAX($J149:J149))+1","v":174},null,{"$f":"MAX(MAX($J$1:$N148),MAX($J149:L149))+1","v":175}]
[null,null,"Minimum cylindrical illuminance (lux)",null,null,null,"at head height in teaching and learning spaces",null,null,null,{"$f":"MAX(MAX($J$1:$N149),MAX($J150:J150))+1","v":176},null,{"$f":"MAX(MAX($J$1:$N149),MAX($J150:L150))+1","v":177}]
[null,null,"Max. CIBSE limiting glare index",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N150),MAX($J151:J151))+1","v":178},null,{"$f":"MAX(MAX($J$1:$N150),MAX($J151:L151))+1","v":179}]
[null,null,"Modelling Index",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N151),MAX($J152:J152))+1","v":180},null,{"$f":"MAX(MAX($J$1:$N151),MAX($J152:L152))+1","v":181}]
[null,null,"Minimum uniformity of artificial lighting",null,null,null,"at task position",null,null,null,{"$f":"MAX(MAX($J$1:$N152),MAX($J153:J153))+1","v":182},null,{"$f":"MAX(MAX($J$1:$N152),MAX($J153:L153))+1","v":183}]
[null,null,"Min. colour rendering (Ra)",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N153),MAX($J154:J154))+1","v":184},null,{"$f":"MAX(MAX($J$1:$N153),MAX($J154:L154))+1","v":185}]
[null,null,"Maximum lighting energy units (W/m2.100 lux)",null,null,null,"Contractor to Specify using suggested figures in technical annexe",null,null,null,{"$f":"MAX(MAX($J$1:$N154),MAX($J155:J155))+1","v":186},{"$f":"MAX(MAX($J$1:$N154),MAX($J155:K155))+1","v":187},{"$f":"MAX(MAX($J$1:$N154),MAX($J155:L155))+1","v":188}]
[null,null,"Minimum initial efficacy - Luminaire lumens / circuit watt with allowance for control factors as in Approved Documents in support of Part L ",null,null,null,"(excluding track-mounted and emergency lighting) or higher if Part L changes in 2013.  Contractor to Specify using suggested figures in technical annexe",null,null,null,{"$f":"MAX(MAX($J$1:$N155),MAX($J156:J156))+1","v":189},{"$f":"MAX(MAX($J$1:$N155),MAX($J156:K156))+1","v":190},{"$f":"MAX(MAX($J$1:$N155),MAX($J156:L156))+1","v":191}]
[null,null,"Lighting Energy Numerical Index (LENI) ",null,null,null,"Contractor to specify (CTS) in new build (kWh/m2)",null,null,null,{"$f":"MAX(MAX($J$1:$N156),MAX($J157:J157))+1","v":192},null,{"$f":"MAX(MAX($J$1:$N156),MAX($J157:L157))+1","v":193}]
[]
[null,null,"Lighting controls",null,null,null,"d-daylight linking, sw - central manual switching, occ - occupancy, dim - dimming to 10 lux",null,null,null,{"$f":"MAX(MAX($J$1:$N158),MAX($J159:J159))+1","v":194}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"identify any emergency lighting",null,null,null,"identify any emergency lighting"]
[null,null,"Emergency lighting",null,null,null,"If community use or high risk areas",null,null,null,{"$f":"MAX(MAX($J$1:$N160),MAX($J161:J161))+1","v":195}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"specific lighting requirements met and additions"]
[null,null,"Specific lighting requirements","over and above those already required",null,null,"notes, including specialist and task lighting  (all occupied spaces shall allow for data screens to be used in a variety of positions without glare)",null,null,null,{"$f":"MAX(MAX($J$1:$N162),MAX($J163:J163))+1","v":196}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"thermal comfort solution"]
[null,null,"Temperature and thermal comfort",null,null,null,"see technical annexe - temperature T",null,null,null,{"$f":"MAX(MAX($J$1:$N164),MAX($J165:J165))+1","v":197},null,{"$f":"MAX(MAX($J$1:$N164),MAX($J165:L165))+1","v":198}]
[null,null,"Normal maintained air temperature (1m above floor level at centre of room) (oC)",null,null,null,"to be achieved by heating system in less than 20 minutes after closing any external doors",null,null,null,{"$f":"MAX(MAX($J$1:$N165),MAX($J166:J166))+1","v":199},null,{"$f":"MAX(MAX($J$1:$N165),MAX($J166:L166))+1","v":200}]
[null,null,"Type of ventilation",null,null,null,"Contractor to specify (CTS): nat vent, mech vent or hybrid",null,null,null,null,{"$f":"MAX(MAX($J$1:$N166),MAX($J167:K167))+1","v":201}]
[null,null,"Minimum maintained air temperature (oC)",null,null,null,"provided by heating system in heating season, during maximum occupancy (1m above floor level)",null,null,null,{"$f":"MAX(MAX($J$1:$N167),MAX($J168:J168))+1","v":202},null,{"$f":"MAX(MAX($J$1:$N167),MAX($J168:L168))+1","v":203}]
[null,null,"Maximum maintained air temperature (oC)",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N168),MAX($J169:J169))+1","v":204},null,{"$f":"MAX(MAX($J$1:$N168),MAX($J169:L169))+1","v":205}]
[null,null,"CIBSE summertime overheating criteria:",null,null,null,null,null,null,null,null,null,null,null,null,null,"value",null,"note ref.",null,"value",null,"note ref."]
[null,null,"1. Maximum hours of exceedence",null,null,null,"For new build only. 2 out of 3 of the CIBSE summertime overheating criteria must be met ",null,null,null,{"$f":"MAX(MAX($J$1:$N170),MAX($J171:J171))+1","v":206},null,{"$f":"MAX(MAX($J$1:$N170),MAX($J171:L171))+1","v":207}]
[null,null,"2. maximum daily weighted exceedence",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N171),MAX($J172:J172))+1","v":208},null,{"$f":"MAX(MAX($J$1:$N171),MAX($J172:L172))+1","v":209}]
[null,null,"3. Upper limit temperature: maximum ΔT",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N172),MAX($J173:J173))+1","v":210},null,{"$f":"MAX(MAX($J$1:$N172),MAX($J173:L173))+1","v":211}]
[null,null,"Maximum hours when air temperature in the space is above 28oC",null,null,null,"In refurbishment and naturally ventilated spaces only",null,null,null,{"$f":"MAX(MAX($J$1:$N173),MAX($J174:J174))+1","v":212},null,{"$f":"MAX(MAX($J$1:$N173),MAX($J174:L174))+1","v":213}]
[null,null,"Maximum difference between internal air temperature and external air temperature  - oC",null,null,null,"In refurbishment, when external temperature > 20°C, when the spaces are occupied for more than 30 minutes",null,null,null,{"$f":"MAX(MAX($J$1:$N174),MAX($J175:J175))+1","v":214},null,{"$f":"MAX(MAX($J$1:$N174),MAX($J175:L175))+1","v":215}]
[null,null,"Maximum hours outside heating season when air temperature in the space is above 25oC  (oC)",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N175),MAX($J176:J176))+1","v":216},null,{"$f":"MAX(MAX($J$1:$N175),MAX($J176:L176))+1","v":217}]
[null,null,"Minimum air temperature of air delivered at 1.4m above floor level in occupied zone  (oC)",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N176),MAX($J177:J177))+1","v":218},null,{"$f":"MAX(MAX($J$1:$N176),MAX($J177:L177))+1","v":219}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ventilation system solution"]
[null,null,"Ventilation",null,null,null,"see technical annexe - ventilation  V",null,null,null,{"$f":"MAX(MAX($J$1:$N178),MAX($J179:J179))+1","v":220},null,{"$f":"MAX(MAX($J$1:$N178),MAX($J179:L179))+1","v":221}]
[null,null,"Operational target for maximum average daily concentration of carbon dioxide (ppm) ",null,"for mechanical ventilation",null,"parts per million (ppm)",null,null,null,{"$f":"MAX(MAX($J$1:$N179),MAX($J180:J180))+1","v":222},null,{"$f":"MAX(MAX($J$1:$N179),MAX($J180:L180))+1","v":223}]
[null,null,null,null,"for natural ventilation",null,"parts per million (ppm)",null,null,null,{"$f":"MAX(MAX($J$1:$N180),MAX($J181:J181))+1","v":224},null,{"$f":"MAX(MAX($J$1:$N180),MAX($J181:L181))+1","v":225}]
[null,null,"Maximum carbon dioxide concentration not to be exceeded for more than 20 minutes each day (ppm) ",null,"for mechanical ventilation",null,"parts per million (ppm)",null,null,null,{"$f":"MAX(MAX($J$1:$N181),MAX($J182:J182))+1","v":226},null,{"$f":"MAX(MAX($J$1:$N181),MAX($J182:L182))+1","v":227}]
[null,null,null,null,"for natural ventilation",null,"parts per million (ppm)",null,null,null,{"$f":"MAX(MAX($J$1:$N182),MAX($J183:J183))+1","v":228},null,{"$f":"MAX(MAX($J$1:$N182),MAX($J183:L183))+1","v":229}]
[null,null,"Minimum rate of ventilation when occupied",null,null,null,"litres per second per person",null,null,null,{"$f":"MAX(MAX($J$1:$N183),MAX($J184:J184))+1","v":230},null,{"$f":"MAX(MAX($J$1:$N183),MAX($J184:L184))+1","v":231}]
[null,null,"Maximum winter time cold air inlet velocity (m/s)",null,null,null,"meters per second during occupation",null,null,null,{"$f":"MAX(MAX($J$1:$N184),MAX($J185:J185))+1","v":232},null,{"$f":"MAX(MAX($J$1:$N184),MAX($J185:L185))+1","v":233}]
[null,null,"Minimum capability rate of ventilation",null,null,null,"in air changes per hour (ach) or litres per second per person (l/s/p) ",null,null,null,{"$f":"MAX(MAX($J$1:$N185),MAX($J186:J186))+1","v":234},null,{"$f":"MAX(MAX($J$1:$N185),MAX($J186:L186))+1","v":235}]
[]
[null,null,"Acoustics",null,null,null,"see technical annexe - acoustics  A",null,null,null,{"$f":"MAX(MAX($J$1:$N187),MAX($J188:J188))+1","v":236},null,{"$f":"MAX(MAX($J$1:$N187),MAX($J188:L188))+1","v":237},null,null,null,"value",null,"note ref.",null,"value",null,"note ref."]
[null,null,"Room classification (for airborne sound insulation)",null,"Activity noise level",null,"(Source room) Low/Average/High/Very High",null,null,null,{"$f":"MAX(MAX($J$1:$N188),MAX($J189:J189))+1","v":238}]
[null,null,null,null,"Noise tolerance",null,"(Receiving room) Low/Medium/High",null,null,null,{"$f":"MAX(MAX($J$1:$N189),MAX($J190:J190))+1","v":239}]
[null,null,"Minimum Dw (dB) (between spaces of same type)",null,null,null,"Contractor to specify (CTS) with reference to Acoustic Performance Standards for PSBP",null,null,null,null,{"$f":"MAX(MAX($J$1:$N190),MAX($J191:K191))+1","v":240}]
[null,null,"Maximum indoor ambient noise level for ventilation to achieve 1500ppm Carbon Dioxide concentration ",null,null,null,"and for Nat Vent when nat vent paths are shut - see note 4 (tech annexe)",null,null,null,{"$f":"MAX(MAX($J$1:$N191),MAX($J192:J192))+1","v":241},null,{"$f":"MAX(MAX($J$1:$N191),MAX($J192:L192))+1","v":242}]
[null,null,"Maximum impact sound pressure from above  ",null,null,null,"sound pressure level L’w ",null,null,null,{"$f":"MAX(MAX($J$1:$N192),MAX($J193:J193))+1","v":243},null,{"$f":"MAX(MAX($J$1:$N192),MAX($J193:L193))+1","v":244}]
[null,null,"Either:",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N193),MAX($J194:J194))+1","v":245},null,{"$f":"MAX(MAX($J$1:$N193),MAX($J194:L194))+1","v":246}]
[null,null,"Minimum composite Rw (dB) of corridor** wall, glazing and ventilators in walls with ventilators ",null,null,null,"Contractor to identify which measure is being used and mark other as N/A",null,null,null,{"$f":"MAX(MAX($J$1:$N194),MAX($J195:J195))+1","v":247},null,{"$f":"MAX(MAX($J$1:$N194),MAX($J195:L195))+1","v":248}]
[null,null,"Or:",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N195),MAX($J196:J196))+1","v":249},null,{"$f":"MAX(MAX($J$1:$N195),MAX($J196:L196))+1","v":250}]
[null,null,"Minimum composite Rw (dB) of corridor** wall and glazing without ventilators ",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N196),MAX($J197:J197))+1","v":251},null,{"$f":"MAX(MAX($J$1:$N196),MAX($J197:L197))+1","v":252}]
[null,null,"Minimum Dn,e,w – 10logN dB for ventilators in walls",null,null,null,"Dn,e,w – 10logN3 (dB) where applicable",null,null,null,{"$f":"MAX(MAX($J$1:$N197),MAX($J198:J198))+1","v":253},null,{"$f":"MAX(MAX($J$1:$N197),MAX($J198:L198))+1","v":254}]
[]
[null,null,"Reverberation",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N199),MAX($J200:J200))+1","v":255},null,{"$f":"MAX(MAX($J$1:$N199),MAX($J200:L200))+1","v":256},null,null,null,"actual reverberation time"]
[null,null,"Maximum reverberation time",null,null,null,"seconds",null,null,null,{"$f":"MAX(MAX($J$1:$N200),MAX($J201:J201))+1","v":257},null,{"$f":"MAX(MAX($J$1:$N200),MAX($J201:L201))+1","v":258}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"specific environmental requirements met and additions"]
[null,null,"Specific environmental requirements","(extraction units and fume cupboards covered under fittings, dim out covered under lighting)",null,null,"requirements not covered in environmental headings above, including special exhaust ventilation, surface temp of heat emitters, minimum STI in open plan areas and intermittent ventilation (as Part L Table 6.1a) ",null,null,null,{"$f":"MAX(MAX($J$1:$N202),MAX($J203:J203))+1","v":259}]
[null,"9. Building services",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"description of building services solutions"]
[null,null,"Gas supply","As described",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N204),MAX($J205:J205))+1","v":260}]
[null,null,"Specific electrical services requirements","Including specialist power",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N205),MAX($J206:J206))+1","v":261}]
[null,null,"Specific wet services requirements","(water supply, drainage, sanitary ware and fixtures)",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N206),MAX($J207:J207))+1","v":262}]
[null,null,"Power sockets",null,null,null,null,null,null,null,null,null,null,null,null,null,"value",null,"note ref.",null,"value",null,"note ref."]
[null,null,null,"Trunking at dado level",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N208),MAX($J209:J209))+1","v":263}]
[null,null,null,"Double Power Socket Total",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N209),MAX($J210:J210))+1","v":264}]
[null,null,null,"Single Power Socket Total",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N210),MAX($J211:J211))+1","v":265}]
[null,null,null,"Additional Power (Double Socket)",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N211),MAX($J212:J212))+1","v":266}]
[null,null,null,"Cleaner's Power (single socket)",null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N212),MAX($J213:J213))+1","v":267}]
[null,null,"Communication and ICT infrastructure"]
[null,null,null,"Voice over Internet Protocol (VoIP)",null,null,"Telephone system using data sockets",null,null,null,{"$f":"MAX(MAX($J$1:$N214),MAX($J215:J215))+1","v":268}]
[null,null,null,"Wifi AP Data Point",null,null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N215),MAX($J216:J216))+1","v":269}]
[null,null,null,"Data Points Total",null,null,"As specified in FOS",null,null,null,{"$f":"MAX(MAX($J$1:$N216),MAX($J217:J217))+1","v":270}]
[null,null,null,"Additional Data",null,null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N217),MAX($J218:J218))+1","v":271}]
[null,null,null,"TV Signal point - IPTV",null,null,"Central controller or receiver box",null,null,null,{"$f":"MAX(MAX($J$1:$N218),MAX($J219:J219))+1","v":272}]
[null,null,null,"Projector AV faceplate",null,null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N219),MAX($J220:J220))+1","v":273}]
[null,null,null,"PA and alarms",null,null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N220),MAX($J221:J221))+1","v":274}]
[null,"10. Safety and security",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"specific safety and security requirements met and additions"]
[null,null,"Specific requirements",null,null,null,"school to add additional requirements if necessary, including space between F&E",null,null,null,{"$f":"MAX(MAX($J$1:$N222),MAX($J223:J223))+1","v":275}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"identify if sprinklers provided"]
[null,null,"Sprinklers, where supplied",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N224),MAX($J225:J225))+1","v":276}]
[]
[]
[null,"11. Fittings, furniture and equipment"]
[null,"Signage",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"specific signage requirements met and additions"]
[null,null,"Specific signage requirements",null,null,null,"Not including doorset signage (covered below)",null,null,null,{"$f":"MAX(MAX($J$1:$N229),MAX($J230:J230))+1","v":277}]
[]
[null,null,"Nameplate",null,"at entry to space",null,"Description on or adjacent to entrance or door ",null,null,null,{"$f":"MAX(MAX($J$1:$N231),MAX($J232:J232))+1","v":278},null,null,null,null,null,null,null,"Yes/ No",null,null,null,"Yes/ No"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"identify any fire fighting equipment provided"]
[null,null,"Fire fighting equipment","including fire extinguisher and holder",null,null,"Contractor to specify particular appliances where provided",null,null,null,{"$f":"MAX(MAX($J$1:$N233),MAX($J234:J234))+1","v":279}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"identify any first aid equipment provided"]
[null,null,"First aid equipment",null,null,null,null,null,null,null,{"$f":"MAX(MAX($J$1:$N235),MAX($J236:J236))+1","v":280}]
[null,"Curtains and blinds",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"specific curtain and blind requirements met and additions"]
[null,null,"Specific curtain and blinds requirements",null,null,null,"To internal and external windows and doors only",null,null,null,{"$f":"MAX(MAX($J$1:$N237),MAX($J238:J238))+1","v":281}]
["ICT equipment",null,null,null,null,null,"Contractor to Specify (CTS) ICT below, based on ICT Solution Summary and discussion with school"]
[null,"Fixed ICT equipment",null,null,null,null,null,null,null,null,"group",null,"quantity",null,null,null,null,null,null,null,"group",null,"quantity"]
[null,null,"Projector",null,"Separate",null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N240),MAX($J241:J241))+1","v":282},null,{"$f":"MAX(MAX($J$1:$N240),MAX($J241:L241))+1","v":283}]
[null,null,"",null,"Wall Mounted",null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N241),MAX($J242:J242))+1","v":284},null,{"$f":"MAX(MAX($J$1:$N241),MAX($J242:L242))+1","v":285}]
[null,null,"",null,"Ceiling Mounted",null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N242),MAX($J243:J243))+1","v":286},null,{"$f":"MAX(MAX($J$1:$N242),MAX($J243:L243))+1","v":287}]
[null,null,"",null,"Theatre",null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N243),MAX($J244:J244))+1","v":288},null,{"$f":"MAX(MAX($J$1:$N243),MAX($J244:L244))+1","v":289}]
[null,null,"Interactive Whiteboard",null,"",null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N244),MAX($J245:J245))+1","v":290},null,{"$f":"MAX(MAX($J$1:$N244),MAX($J245:L245))+1","v":291}]
[null,null,"Integrated IWB and projector",null,"",null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N245),MAX($J246:J246))+1","v":292},null,{"$f":"MAX(MAX($J$1:$N245),MAX($J246:L246))+1","v":293}]
[null,null,"Speakers",null,"",null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N246),MAX($J247:J247))+1","v":294},null,{"$f":"MAX(MAX($J$1:$N246),MAX($J247:L247))+1","v":295}]
[null,null,"Digital Display",null,"",null,"(Plasma or LCD)",null,null,null,{"$f":"MAX(MAX($J$1:$N247),MAX($J248:J248))+1","v":296},null,{"$f":"MAX(MAX($J$1:$N247),MAX($J248:L248))+1","v":297}]
[null,null,"Electric Screen",null,"",null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N248),MAX($J249:J249))+1","v":298},null,{"$f":"MAX(MAX($J$1:$N248),MAX($J249:L249))+1","v":299}]
[null,null,"Sound Field",null,"",null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N249),MAX($J250:J250))+1","v":300},null,{"$f":"MAX(MAX($J$1:$N249),MAX($J250:L250))+1","v":301}]
[null,"Loose ICT equipment"]
[null,null,"Projector - Mobile",null,"",null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N251),MAX($J252:J252))+1","v":302},null,{"$f":"MAX(MAX($J$1:$N251),MAX($J252:L252))+1","v":303}]
[null,null,"Teacher Laptop/Desktop",null,"",null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N252),MAX($J253:J253))+1","v":304},null,{"$f":"MAX(MAX($J$1:$N252),MAX($J253:L253))+1","v":305}]
[null,null,"Computer",null,"Desktop",null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N253),MAX($J254:J254))+1","v":306},null,{"$f":"MAX(MAX($J$1:$N253),MAX($J254:L254))+1","v":307}]
[null,null,"",null,"Laptop",null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N254),MAX($J255:J255))+1","v":308},null,{"$f":"MAX(MAX($J$1:$N254),MAX($J255:L255))+1","v":309}]
[null,null,"",null,"Netbook",null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N255),MAX($J256:J256))+1","v":310},null,{"$f":"MAX(MAX($J$1:$N255),MAX($J256:L256))+1","v":311}]
[null,null,"",null,"Tablet",null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N256),MAX($J257:J257))+1","v":312},null,{"$f":"MAX(MAX($J$1:$N256),MAX($J257:L257))+1","v":313}]
[null,null,"Printer",null,"Multi-function Device",null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N257),MAX($J258:J258))+1","v":314},null,{"$f":"MAX(MAX($J$1:$N257),MAX($J258:L258))+1","v":315}]
[null,null,"",null,"Workgroup",null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N258),MAX($J259:J259))+1","v":316},null,{"$f":"MAX(MAX($J$1:$N258),MAX($J259:L259))+1","v":317}]
[null,null,"",null,"Large Form Factor",null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N259),MAX($J260:J260))+1","v":318},null,{"$f":"MAX(MAX($J$1:$N259),MAX($J260:L260))+1","v":319}]
[null,null,"Laptop Trolley",null,"",null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N260),MAX($J261:J261))+1","v":320},null,{"$f":"MAX(MAX($J$1:$N260),MAX($J261:L261))+1","v":321}]
[null,null,"Networked Peripheral",null,"Scanner",null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N261),MAX($J262:J262))+1","v":322},null,{"$f":"MAX(MAX($J$1:$N261),MAX($J262:L262))+1","v":323}]
[null,null,"",null,"VC Unit",null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N262),MAX($J263:J263))+1","v":324},null,{"$f":"MAX(MAX($J$1:$N262),MAX($J263:L263))+1","v":325}]
[null,null,"",null,"Visualiser",null,"",null,null,null,{"$f":"MAX(MAX($J$1:$N263),MAX($J264:J264))+1","v":326},null,{"$f":"MAX(MAX($J$1:$N263),MAX($J264:L264))+1","v":327}]
["FF&E",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"specific FF&E requirements met and additions"]
[null,null,"Specific FF&E requirements","incl. extraction units and fume cupboards.\n\nFF&E should comply to requirements in FF&E matrix for reference number listed below.",null,null,{"$f":"MAX(MAX($G$1:$H265),MAX($F266:F266))+1","v":19},null,null,null,{"$f":"MAX(MAX($J$1:$N265),MAX($J266:J266))+1","v":328}]
[null,"Fittings",null,null,null,null,null,null,null,null,"group",null,"quantity",null,null,null,"group",null,"quantity",null,"group",null,"quantity"]

{"sheet":"LOCK WORKBOOK","index":13,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}