**RA 2335 Form 5: Public Display Authority (PDA) Form**

In accordance with (iaw) RA 2335 - Flying Displays, Display Flying, Display Parachuting, Role Demonstrations and Flypasts, paragraph 85, an Military Aviation Authority (MAA) Form 5, and its associated Annexes, **should** be completed by Aviation Duty Holder (ADH) / Accountable Manager (Military Flying) (AM(AF)) for military Aircrew that will conduct Display Flying. It can also be used for Role Demonstrations when deemed appropriate.

A copy of the signed Form 5, along with its associated Annexes, **should** be sent to the MAA via email: DSA-MAA-Display-Forms@mod.gov.uk. A copy of the PDA **should** be carried by the display pilot and made available to Flying Display Directors (FDD).

The Aircrew detailed in the table below are authorised to conduct the public Display Sequence(s) / Role Demonstration detailed in Annex A and B to this document, iaw RA 2335:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Aircrew Full Name | Rank | Service Number | Aircraft Type and Mark | PDA Valid from | PDA Valid to |
|   |   |   |   |   |   |
|   |   |   |   |   |   |
|   |   |   |   |   |   |
|   |   |   |   |   |   |

**RA 2335 Form 5: Public Display Authority (PDA) Form**

**Annex A**

ADH / AM(MF) **should** provide a signed PDF document that includes the following minimum detail:

1. **The Occasion for the PDA.** This can be for a single occasion, a specific period or for an entire Flying Display Season.
2. **Display Team Name.** Details of the Display Team Name.
3. **Display Sequence Names and Descriptions.** This section **should** include details of all Display Sequences approved ie full, flat and rolling Displays.An individual ribbon diagram for each Display Sequence **should** be provided at Annex B.
4. **Display Duration.** The Display duration **should** be provided for each approved Display Sequence.
5. **Display Sequence Minimum Heights.** The minimum heights **should** be provided, in height above ground level (AGL), for each approved Display Sequence when conducting:
	1. Aerobatic Manoeuvres.
	2. Non-Aerobatic Manoeuvres.
	3. Wings level passes (<20° Angle of Bank).
6. **Display Sequence Maximum Speed.** The maximum speed **should** be provided for each approved Display Sequence.
7. **Weather Minima.** Details of the weather minima, including cloud base and visibility, **should** be provided for each approved Display Sequence.
8. **Permitted Modifications to Display Sequences and Approved Basic Manoeuvres.** The details of any permitted Display Sequence modifications **should** be included. This section can be omitted if it is not applicable.
9. **Contact Details.** Contact details of key display team members **should** be provided.

|  |  |
| --- | --- |
| **Display Supervisor / Approving Officer:** | **ADH / AM(MF):** |
| **Name:**   | **Name:**   |
| **Rank:**   | **Rank:**   |
| **Appointment:**   | **Appointment:**   |
| **Date:**   | **Date:**   |
| **Signature:**   | **Signature:**   |

**RA 2335 Form 5: Public Display Authority (PDA) Form**

**Annex B**

ADH / AM(MF) **should** provide detailed ribbon diagrams for each approved Display Sequence as detailed in Annex A Para 1.c.